## FUEL PRICE ADJUSTMENT:

|  |  |  |
| --- | --- | --- |
| (11-15-05) (Rev. 2-18-14) | 109-8 | SP1 G43 |

Revise the *2012* *Standard Specifications* as follows:

**Page 1-83, Article 109-8, Fuel Price Adjustments,** add the following:

The base index price for DIESEL #2 FUEL is **$ [number]** per gallon. Where any of the following are included as pay items in the contract, they will be eligible for fuel price adjustment.

The pay items and the fuel factor used in calculating adjustments to be made will be as follows:

|  |  |  |
| --- | --- | --- |
| **Description** | **Units** | **Fuel Usage Factor Diesel** |
| Unclassified Excavation | Gal/CY | 0.29 |
| Borrow Excavation | Gal/CY | 0.29 |
| Class IV Subgrade Stabilization | Gal/Ton | 0.55 |
| Aggregate Base Course | Gal/Ton | 0.55 |
| Sub-Ballast | Gal/Ton | 0.55 |
| Asphalt Concrete Base Course, Type \_\_\_\_ | Gal/Ton | 2.90 |
| Asphalt Concrete Intermediate Course, Type \_\_\_\_ | Gal/Ton | 2.90 |
| Asphalt Concrete Surface Course, Type \_\_\_\_ | Gal/Ton | 2.90 |
| Open-Graded Asphalt Friction Course | Gal/Ton | 2.90 |
| Permeable Asphalt Drainage Course, Type \_\_\_\_ | Gal/Ton | 2.90 |
| Sand Asphalt Surface Course, Type \_\_\_\_ | Gal/Ton | 2.90 |
| Aggregate for Cement Treated Base Course | Gal/Ton | 0.55 |
| Portland Cement for Cement Treated Base Course | Gal/Ton | 0.55 |
| \_\_" Portland Cement Concrete Pavement | Gal/SY |  0.245 |
| Concrete Shoulders Adjacent to \_\_" Pavement | Gal/SY |  0.245 |