**LUMP SUM GRADING:**

|  |  |  |
| --- | --- | --- |
| (8-17-10) | 226 | SP2 R16 |

Lump sum grading shall be performed in accordance with Section 226 Comprehensive Grading of the *2012* *Standard Specifications* except as follows:

Delete all references to [Fill-in from choices below]\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Section 200, Clearing and Grubbing.

Section 225, Unclassified Excavation.

Section 230, Borrow Excavation.

Section 250, Removal of Existing Asphalt Pavement.

Section 250, Removal of Existing Concrete Pavement.

Section 250, Breaking of Existing Asphalt Pavement.

Section 250, Breaking of Existing Concrete Pavement.

Section 500, Fine Grading.

Section 560, Shoulder Borrow.

INSTRUCTIONS

This provision should be used only when *Item 0063 Lump Sum Grading* is included in estimate. In addition, one or more of the following Items will also be included in estimate:

0001 - Clearing and Grubbing

0022 - Unclassified Excavation

0106 - Borrow Excavation

0156 - Removal of Existing Asphalt Pavement

0163 - Removal of Existing Concrete Pavement

0177 - Breaking of Existing Asphalt Pavement

0185 - Breaking of Existing Concrete Pavement

1011 - Fine Grading

1231 - Shoulder Borrow

Does NOT apply to *Item 0043 Lump Sum Grading*.