**PIPE INSTALLATION:**

|  |  |  |
| --- | --- | --- |
| (11-20-12) (Rev. 8-18-15) | 300 | SP3 R01 |

Revise the *2012* *Standard Specifications* as follows:

**Page 3-1, Article 300-2, Materials,** line 15, in the materials table, replace“Flowable Fill” and “Geotextiles” with the following:

| **Item** | **Section** |
| --- | --- |
| Flowable Fill, Excavatable | 1000-6 |
| Grout, Type 2  Geotextiles, Type 4 | 1003  1056 |

**Page 3-1, Article 300-2, Materials,** lines 23-24, replace sentence with the following:

Provide foundation conditioning geotextile and geotextile to wrap pipe joints in accordance with Section 1056 for Type 4 geotextile.

**Page 3-3, Subarticle 300-6(A), Rigid Pipe,** line 2, in the first paragraph, replace “an approved non-shrink grout.” with “grout.” and line 4, in the second paragraph, replace “filtration geotextile” with “geotextile”.

**Page 3-3, Article 300-7, Backfilling,** lines 37-38, in the first and second sentences of the fifth paragraph, replace “Excavatable flowable fill” with “Flowable fill”.