**REINFORCED CONCRETE TAPERED INLET:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 11-20-12) | 300 | SP3 R05 |

**Description**

Construct tapered inlets in accordance with the details in the plans, Section 310 of the *2012* *Standard Specifications*, and as directed by the Engineer.

**Measurement and Payment**

*\_\_\_" x \_\_\_" Reinforced Concrete Pipe Tapered Inlet, Class III* will be measured and paid as each, for the actual number incorporated into the completed and accepted work. Such price and payment will be full compensation for all materials, labor, equipment, and other incidentals necessary to complete the work.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| \_\_\_" x \_\_\_" Reinforced Concrete Pipe Tapered Inlet, Class III | Each |