**FLOWABLE FILL:**

|  |  |  |
| --- | --- | --- |
| (9-17-02) (Rev 1-17-12) | 300, 340, 450, 1000, 1530, 1540, 1550 | SP3 R30 |

**Description**

This work consists of all work necessary to place flowable fill in accordance with these provisions, the plans, and as directed.

**Materials**

Refer to Division 10 of the *2012* *Standard Specifications*.

|  |  |
| --- | --- |
| **Item** | **Section** |
| Flowable Fill | 1000-6 |

**Construction Methods**

Discharge flowable fill material directly from the truck into the space to be filled, or by other approved methods. The mix may be placed full depth or in lifts as site conditions dictate. The Contractor shall provide a method to plug the ends of the existing pipe in order to contain the flowable fill.

**Measurement and Payment**

At locations where flowable fill is called for on the plans and a pay item for flowable fill is included in the contract, *Flowable Fill* will be measured in cubic yards and paid as the actual number of cubic yards that have been satisfactorily placed and accepted. Such price and payment will be full compensation for all work covered by this provision including, but not limited to, the mix design, furnishing, hauling, placing and containing the flowable fill.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Flowable Fill | Cubic Yard |