**ASPHALT CONCRETE SURFACE COURSE COMPACTION:**

|  |  |
| --- | --- |
| (7-1-95) (Rev. 8-21-12) | SP6 R49R |

Compact the asphalt surface course on this project in accordance with Subarticle 610-9 of the *2012 Standard Specifications* and the following provision:

Perform the first rolling with a steel wheel roller followed by rolling with a self-propelled pneumatic tired roller with the final rolling by a steel wheel roller.