**REPAIR OF EXISTING PAVEMENT:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 5-20-14) | 610 | SP6 R58R |

**Description**

The Contractor's attention is directed to the fact that the existing pavement shall be removed and repaired prior to resurfacing in the areas indicated in the contract.

**Materials**

Refer to Division 6 of the *2012* *Standard Specifications*.

|  |  |
| --- | --- |
| **Item** | **Section** |
| Asphalt Concrete Base Course, Type \_\_ | 610 |

**Construction Methods**

The repair of the existing pavement includes, but is not limited to, the cutting of the existing pavement to a neat vertical joint and uniform line; the removal and disposal of pavement, base, and subgrade material as approved or directed by the Engineer; the coating of the area to be repaired with a tack coat; and conditioning of the surface on which the base course material is to be placed.

Do not excavate below the plane of the bottom of existing pavement, unless otherwise directed by the Engineer. Replace material excavated below existing pavement with Asphalt Concrete Base Course, Type \_\_ in layers not to exceed 5 inch compacted.

Machine place the Asphalt Concrete Base Course, Type \_\_ in two equal layers. Perform compaction of the base course material at transverse joint by the use of mechanical hand tamps or other equipment approved by the Engineer in order to achieve required density.

Construct the pavement repair so the surface of the complete repair matches the surface of existing pavement.

Schedule operations so all areas where pavement has been removed will be repaired and all lanes of traffic restored on the same day of the pavement removal. The Contractor will be restricted to repairing one side of the existing pavement at a time unless otherwise permitted by the Engineer.

**Measurement and Payment**

*Asphalt Concrete Base Course, Type \_\_* will be measured and paid in accordance with Article 610-16 of the *2012* *Standard Specification*s.

Furnished asphalt binder for the mix will be paid in accordance with Article 620-4 of the *2012* *Standard Specifications*.

If it becomes necessary to excavate below existing pavement, measurement and payment for all labor, equipment, and incidentals necessary to complete the excavation shall be made in accordance with Article 104-7 of the *2012* *Standard Specifications*.