**PAVING INTERSECTIONS:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 8-21-12) | 610 | SP6 R67BR |

Condition, prime, and surface all unpaved intersections back from the edge of the pavement on the main line of the project a minimum distance of 50 feet. The pavement placed in the intersections shall be of the same material and thickness placed on the mainline of the project.

Resurface all paved intersections back to the ends of the radii, or as directed by the Engineer.

Widen the pavement on curves as directed by the Engineer.