**ADJUSTMENT OF MANHOLES:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 8-21-12) | 858 | SP8 R95R |

The Contractor's attention is directed to Section 858-3 of the *2012* *Standard Specifications*.

The use of cast iron or steel fittings in the adjustment of manholes will not be permitted on this project except where it is considered by the Engineer to be in the best interest of the Department to allow rings to be used. When rings are permitted for the adjustment of manholes, the rings shall have satisfactory bearing on the existing manhole frames and 50 percent of the circumference shall be tack welded at four equally spaced locations as directed by the Engineer. If the existing covers do not fit the rings, furnish and install new covers at no additional expense to the Department.