**ADJUSTMENT TO MANHOLES:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 8-21-12) | 858 | SP8 R96R |

The Contractor's attention is directed to Section 858-3 of the *2012* *Standard Specifications*.

Make adjustments to manholes on this project by using rings or rapid set (grout, mortar, or concrete) as approved by the Engineer.