**SANITARY SEWER:**

|  |  |  |
| --- | --- | --- |
| (11-19-13) | 1520 | SP15 R20 |

Revise the *2012* *Standard Specifications* as follows:

**Page 15-11, Article 1520-3(A)(2) Testing, line 5,** replace the second paragraph with the following:

Test all 24" and smaller gravity sewer lines for leakage using infiltration, exfiltration, or air test. Perform visual inspection on gravity sewer lines larger than 24". Perform line and grade testing and deflection testing on all gravity sewer lines.