**GROUT REFERENCES FOR UTILITY MANHOLES:**

|  |  |  |
| --- | --- | --- |
| (8-18-15) | 1525 | SP15 R40 |

Revise the *2012* *Standard Specifications* as follows:

**Page 15-13, Article 1525-2, Materials,** line 9,in the materials table, add the following:

| **Item** | **Section** |
| --- | --- |
| Grout, Type 2 | 1003 |

**Page 15-13, Article 1525-2, Materials,** lines 20-21, replace the third paragraph after the materials table with the following:

Use Type 2 grout with properties that meet Table 1003-2 in the *Grout Production and Delivery* provision except provide grout with a plastic consistency in accordance with ASTM C1107.

**Page 15-14, Subarticle 1525-3(B), Installation of Precast Units,** line 22, in the second sentence of the first paragraph, replace “non-shrink grout.” with “grout.”