{"text_format":"1","workbook":"xlsx","n_sheets":17,"sheets":["Summary - Statewide","Items - Statewide","BExRepositorySheet","Items - Div 1","Items - Div 2","Items - Div 3","Items - Div 4","Items - Div 5","Items - Div 6","Items - Div 7","Items - Div 8","Items - Div 9","Items - Div 10","Items - Div 11","Items - Div 12","Items - Div 13","Items - Div 14"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary - Statewide","index":0,"n_rows":1036,"n_cols":24,"rows_kept":1036,"cut":false,"hidden":false,"merged":[[0,0,0,23]]}
["NORTH CAROLINA DEPARTMENT OF TRANSPORATION - 2014 BID AVERAGES"]
["LET DATE","RPN","TIP","CONTR ","PROJECT","CAT ","COUNTY","VENDOR NAME","$TOTAL","JOB","FED WRK ","PROJ LGTH (MI/ KM)"," LN / CVT FILL DPTH","CVT CODE OVR/UND RET WLL X-SECT","BOX LTH /WLL HT","BOX SPAN","BRG SUP STR","SUB STR"," SPAN","BRG WTH","BRG LTH","AREA","DIV","LOC"]
["1/21/2014","1","R-3307","C202848","C202848-EC","1","CARTERET","CONTI ENTPR INC",2031222.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C202848-RW","1","CARTERET","CONTI ENTPR INC",20100188.690000001,"RW1","I000",3.1120000000000001,4,"N220",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C202848-SG","1","CARTERET","CONTI ENTPR INC",240266.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C202848-SI","1","CARTERET","CONTI ENTPR INC",230178.34,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C202848-ST","1","CARTERET","CONTI ENTPR INC",365750,"WL1","X081",null,null,"W001",11,null,"","",null,null,null,"COAST","2","63+00.00 -L-"]
["","","","","","2","CARTERET","CONTI ENTPR INC",1144325,"WL2","Y007",null,null,"W001",13.4,null,"","",null,null,null,"COAST","2","145+49.89 -L-"]
["","","","","","3","CARTERET","CONTI ENTPR INC",38317136.469999999,"BR01","X081",0.64300000000000002,null,"15",null,80.583299999999994,"878","I",29,78,3395,"COAST","2","46+21.50 -L-"]
["","","","","","4","CARTERET","CONTI ENTPR INC",3638331.5,"BR02","X081",null,null,"15",null,74.583299999999994,"745","A",9,61,585,"COAST","2","16+05.50 -L-"]
["","","","","C202848-TC","1","CARTERET","CONTI ENTPR INC",370375,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","","","","Result",66437774,"","",3.7549999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","2","R-2633BA","C203199","C203199-EC","1","BRUNSWICK","BARNHILL CONT CO",2831040.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203199-RW","1","BRUNSWICK","BARNHILL CONT CO",49438785,"RW1","I000",4.4509999999999996,4,"N210",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203199-SG","1","BRUNSWICK","BARNHILL CONT CO",1086760.25,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203199-SI","1","BRUNSWICK","BARNHILL CONT CO",650743.56999999995,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203199-ST","1","BRUNSWICK","BARNHILL CONT CO",166291,"CV01","Y007",null,3.12,"C001",79,12,"","",null,null,null,"COAST","3"," 52+09.00 -Y7-"]
["","","","","","2","BRUNSWICK","BARNHILL CONT CO",480920,"WL1","Y007",null,null,"W000",19.23,null,"","A",null,null,null,"COAST","3","14+17.83 -EY7A-"]
["","","","","","3","BRUNSWICK","BARNHILL CONT CO",476548,"WL2","Y007",null,null,"W000",18.420000000000002,null,"","A",null,null,null,"COAST","3","14+73.17 -EY7A-"]
["","","","","","4","BRUNSWICK","BARNHILL CONT CO",5849514.3799999999,"BR01","X131",null,null,"12",null,45.25,"585","Q",3,42,502.25,"COAST","3","147+38.89 -L- LT"]
["","","","","","5","BRUNSWICK","BARNHILL CONT CO",6036871.7800000003,"BR02","X131",9.8000000000000004E-2,null,"12",null,45.25,"585","Q",3,42,515.25,"COAST","3","147+38.89 -L- RT"]
["","","","","","6","BRUNSWICK","BARNHILL CONT CO",945257.84,"BR03","X281",null,null,"11",null,55.25,"864","A",2,52,209.84899999999999,"COAST","3","182+99.94 -L-"]
["","","","","","7","BRUNSWICK","BARNHILL CONT CO",1085084.17,"BR04","X181",null,null,"12",null,67.25,"863","A",1,64,97.75,"COAST","3","38+50.27 -Y7-"]
["","","","","","8","BRUNSWICK","BARNHILL CONT CO",2077864.29,"BR05","X081",null,null,"15",null,45.25,"854","A",4,42,326,"COAST","3","265+53.58 -L- LT"]
["","","","","","9","BRUNSWICK","BARNHILL CONT CO",1924052.41,"BR05","X081",6.2E-2,null,"15",null,45.25,"854","A",4,42,326,"COAST","3","265+53.58 -L- LT"]
["","","","","","10","BRUNSWICK","BARNHILL CONT CO",837393.07,"BR07","X271",null,null,"11",null,51.25,"563","B",1,48,145,"COAST","3","281+51.83 -L- LT"]
["","","","","","11","BRUNSWICK","BARNHILL CONT CO",778620.57,"BR08","X271",2.7E-2,null,"11",null,45.25,"563","B",1,42,145,"COAST","3","281+51.83 -L- RT"]
["","","","","","12","BRUNSWICK","BARNHILL CONT CO",2113119.9,"BR09","X081",null,null,"15",null,59.25,"854","A",4,56,328,"COAST","3"," 48+79.00 -Y8-"]
["","","","","C203199-TC","1","BRUNSWICK","BARNHILL CONT CO",184687.47,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203199-UT","1","BRUNSWICK","BARNHILL CONT CO",2532594.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","","2","BRUNSWICK","BARNHILL CONT CO",143000,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","","3","BRUNSWICK","BARNHILL CONT CO",27300,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","","4","BRUNSWICK","BARNHILL CONT CO",16750,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","","","","Result",79683198.700000003,"","",4.6379999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","3","U-2810C","C203291","C203291-EC","1","CUMBERLAND","HIGHLAND PAVING CO LLC",296518.75,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203291-RW","1","CUMBERLAND","HIGHLAND PAVING CO LLC",8392884.5,"RW1","I000",2.1619999999999999,4,"D330",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203291-SG","1","CUMBERLAND","HIGHLAND PAVING CO LLC",461365.75,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203291-SI","1","CUMBERLAND","HIGHLAND PAVING CO LLC",77684.14,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203291-TC","1","CUMBERLAND","HIGHLAND PAVING CO LLC",213853.75,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203291-UT","2","CUMBERLAND","HIGHLAND PAVING CO LLC",2620884.2599999998,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",12063191.15,"","",2.1619999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","4","K-3800","C203304","C203304-EC","1","BEAUFORT","BARNHILL CONT CO",206005.25,"RW1","Y021",null,1,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203304-LI","1","BEAUFORT","BARNHILL CONT CO",266432.15000000002,"RW1","Y021",null,1,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203304-RA","1","BEAUFORT","BARNHILL CONT CO",1252583.3500000001,"RW1","Y021",null,1,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203304-RW","1","BEAUFORT","BARNHILL CONT CO",2444791.6,"RW1","Y021",0.374,1,"M701",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203304-SI","1","BEAUFORT","BARNHILL CONT CO",36255.9,"RW1","Y021",null,1,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203304-TC","1","BEAUFORT","BARNHILL CONT CO",41088.199999999997,"RW1","Y021",null,1,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203304-UT","1","BEAUFORT","BARNHILL CONT CO",91958,"RW1","Y021",null,1,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","","","","Result",4339114.45,"","",0.374,null,"",null,null,"","",null,null,null,"","",""]
["","5","B-5111","C203300","C203300-EC","1","PITT","S T WOOTEN CORP",32359.95,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203300-RW","1","PITT","S T WOOTEN CORP",189561.68,"RW1","I000",3.9E-2,2,"B810",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203300-SI","1","PITT","S T WOOTEN CORP",1960,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203300-ST","1","PITT","S T WOOTEN CORP",420195.05,"BR01","X081",3.2500000000000001E-2,null,"15",null,30,"721","A",3,27.833300000000001,171.5,"COAST","2","20+67.50 -L-"]
["","","","","C203300-TC","1","PITT","S T WOOTEN CORP",4659.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","C203300-UT","1","PITT","S T WOOTEN CORP",47605.09,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
["","","","","","","","Result",696341.52,"","",7.1499999999999994E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","6","B-5143","C203302","C203302-EC","1","DUPLIN","FSC II LLC DBA FRED SMITH CO",36665,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
["","","","","C203302-RW","1","DUPLIN","FSC II LLC DBA FRED SMITH CO",226795.5,"RW1","I000",0.123,2,"B810",null,null,"","",null,null,null,"PDMT","3",""]
["","","","","C203302-SI","1","DUPLIN","FSC II LLC DBA FRED SMITH CO",2886.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
["","","","","C203302-ST","1","DUPLIN","FSC II LLC DBA FRED SMITH CO",418482,"BR01","X080",1.4E-2,null,"15",null,30,"722","A",1,28.83,72.25,"PDMT","3","17+27.00 -L-"]
["","","","","C203302-TC","1","DUPLIN","FSC II LLC DBA FRED SMITH CO",4207,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
["","","","","C203302-UT","1","DUPLIN","FSC II LLC DBA FRED SMITH CO",64091,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
["","","","","","","","Result",753127,"","",0.13700000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203480","C203480A-RW","1","BRUNSWICK","BARNHILL CONT CO",2441628.56,"RW1","",7.83,4,"R000",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203480B-RW","1","NEW HANOVER","BARNHILL CONT CO",1861228.36,"RW1","",3.83,4,"R000",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203480C-RW","1","PENDER","BARNHILL CONT CO",2613450.8199999998,"RW1","",9.61,3,"R000",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203480D-RW","1","BRUNSWICK","BARNHILL CONT CO",2171599.35,"RW1","",15.34,4,"R000",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203480E-RW","1","NEW HANOVER","BARNHILL CONT CO",2183013.31,"RW1","",9.61,4,"R000",null,null,"","",null,null,null,"COAST","3",""]
["","","","","","","","Result",11270920.4,"","",46.22,null,"",null,null,"","",null,null,null,"","",""]
["","8","","C203476","C203476-RW","1","JOHNSTON","FSC II LLC DBA FRED SMITH CO",1980323.37,"RW1","",12.105,2,"R000",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","","","","Result",1980323.37,"","",12.105,null,"",null,null,"","",null,null,null,"","",""]
["","9","B-4666","C203294","C203294-EC","1","WARREN","FSC II LLC DBA FRED SMITH CO",23099.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203294-RW","1","WARREN","FSC II LLC DBA FRED SMITH CO",163761,"RW1","I000",4.3999999999999997E-2,2,"B810",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203294-SI","1","WARREN","FSC II LLC DBA FRED SMITH CO",2240,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203294-ST","1","WARREN","FSC II LLC DBA FRED SMITH CO",540486,"BR01","X080",3.2000000000000001E-2,null,"15",null,30,"721","A",4,27.832999999999998,168.03,"PDMT","5","16+02.50 -L-"]
["","","","","C203294-TC","1","WARREN","FSC II LLC DBA FRED SMITH CO",4928,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",734514.5,"","",7.5999999999999998E-2,null,"",null,null,"","",null,null,null,"","",""]
["","10","B-4478","C203293","C203293-EC","1","COLUMBUS","SMITH-ROWE LLC",30788,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203293-RW","1","COLUMBUS","SMITH-ROWE LLC",276544,"RW1","I000",7.0000000000000007E-2,2,"B810",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203293-SI","1","COLUMBUS","SMITH-ROWE LLC",3456,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203293-ST","1","COLUMBUS","SMITH-ROWE LLC",449472.42,"BR01","X080",2.5000000000000001E-2,null,"15",null,33,"721","A",3,30.833300000000001,132.5,"COAST","6","17+68.00 -L-"]
["","","","","C203293-TC","1","COLUMBUS","SMITH-ROWE LLC",4024,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",764284.42,"","",9.5000000000000001E-2,null,"",null,null,"","",null,null,null,"","",""]
["","11","R-5512","C203435","C203435-RW","1","CUMBERLAND","BARNHILL CONT CO",6786916.0199999996,"RW1","I000",8.2899999999999991,6,"R000",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",6786916.0199999996,"","",8.2899999999999991,null,"",null,null,"","",null,null,null,"","",""]
["","12","B-4400","C203292","C203292-EC","1","ALAMANCE","RE BURNS & SONS CO INC",51640.4,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203292-RW","1","ALAMANCE","RE BURNS & SONS CO INC",187851,"RW1","I000",0.10199999999999999,2,"B810",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203292-SI","1","ALAMANCE","RE BURNS & SONS CO INC",10475.93,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203292-ST","1","ALAMANCE","RE BURNS & SONS CO INC",584914.5,"BR01","X081",2.9000000000000001E-2,null,"15",null,33,"722","Q",3,30.833300000000001,152.5,"PDMT","7","16+88.00 -L-"]
["","","","","C203292-TC","1","ALAMANCE","RE BURNS & SONS CO INC",2558.79,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",837440.62,"","",0.13100000000000001,null,"",null,null,null,null,null,null,null,"","",""]
["","13","","C203475","C203475A-RW","1","ROCKINGHAM","BLYTHE CONST INC",240456.45,"RW1","",1.123,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203475B-RW","1","ROCKINGHAM","BLYTHE CONST INC",1679734.28,"RW1","",19.151,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",1920190.73,"","",20.274000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","14","R-3421C","C202962","C202962-EC","1","RICHMOND","W C ENGLISH INC",5478150,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C202962-RW","1","RICHMOND","W C ENGLISH INC",36782595.990000002,"RW1","I000",3.7240000000000002,4,"RH10",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C202962-SI","1","RICHMOND","W C ENGLISH INC",840467.4,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C202962-ST","1","RICHMOND","W C ENGLISH INC",702907.8,"CV01","X728",null,7.15,"C002",424.58,9,"","",null,null,null,"PDMT","8","509+83.00 -L-"]
["","","","","","2","RICHMOND","W C ENGLISH INC",682136,"WL1","Y007",null,null,"M711",12.3,null,"","",null,null,null,"PDMT","8","545+93.58 -L-"]
["","","","","","3","RICHMOND","W C ENGLISH INC",647860.81999999995,"BR01","X281",null,null,"61",null,33.25,"863","A",2,30,212,"PDMT","8","378+94.34 -L-"]
["","","","","","4","RICHMOND","W C ENGLISH INC",2271058.4700000002,"BR02","X231",null,null,"61",null,77.25,"666","A",2,74,256,"PDMT","8","395+64.54 -L-"]
["","","","","","5","RICHMOND","W C ENGLISH INC",1561759.37,"BR03","X231",null,null,"61",null,55.25,"666","A",2,52,265,"PDMT","8","456+99.33 -L-"]
["","","","","C202962-TC","1","RICHMOND","W C ENGLISH INC",873793.11,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",49840728.960000001,"","",3.7240000000000002,null,"",null,null,null,null,null,null,null,"","",""]
["","15","B-4731","C203297","C203297-EC","1","CHATHAM","APAC - ATLANTIC INC THOMPSON ARTHUR DI",31658.36,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203297-RW","1","CHATHAM","APAC - ATLANTIC INC THOMPSON ARTHUR DI",297790.09999999998,"RW1","I000",0.10100000000000001,2,"B810",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203297-SI","1","CHATHAM","APAC - ATLANTIC INC THOMPSON ARTHUR DI",3540.65,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203297-ST","1","CHATHAM","APAC - ATLANTIC INC THOMPSON ARTHUR DI",485521.37,"BR01","X081",2.4E-2,null,"15",null,33,"722","Q",3,30.5,127.58329999999999,"PDMT","8","16+13.50-L-"]
["","","","","C203297-TC","1","CHATHAM","APAC - ATLANTIC INC THOMPSON ARTHUR DI",4819,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",823329.48,"","",0.125,null,"",null,null,"","",null,null,null,"","",""]
["","17","B-4720","C203296","C203296-EC","1","CABARRUS","TCB BUILDERS LLC",20100,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203296-RW","1","CABARRUS","TCB BUILDERS LLC",157219.04999999999,"RW1","I000",5.8000000000000003E-2,2,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203296-ST","1","CABARRUS","TCB BUILDERS LLC",352878.2,"BR01","X080",1.7999999999999999E-2,null,"15",null,33,"729","A",1,30.5,92.25,"PDMT","10","21+77.00 -L-"]
["","","","","C203296-TC","1","CABARRUS","TCB BUILDERS LLC",3193,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",533390.25,"","",7.5999999999999998E-2,null,null,null,null,null,null,null,null,null,"","",""]
["","18","R-3101","C203386","C203386-EC","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",1899138.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203386-RW","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",12637201.6,"RW1","I000",9.6479999999999997,2,"D300",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203386-SG","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",33796.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203386-SI","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",181957.1,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203386-ST","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",148126.25,"CV01","Y007",null,7.57,"C002",87.75,7,"","",null,null,null,"MTN","11","405+28.06 -L-"]
["","","","","","2","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",106136.25,"CV02","Y007",null,10.49,"C101",97.5,6,"","",null,null,null,"MTN","11","442+13.60 -L-"]
["","","","","","3","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",27376.25,"CV03","Y007",null,12.46,"C201",15.08,4,"","",null,null,null,"MTN","11","52+41.45 -L-"]
["","","","","","4","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",270160,"WL1","Y007",null,null,"W000",7.68,null,"","",null,null,null,"MTN","11","27+90.00 -L-"]
["","","","","","5","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",125000,"WL2","Y007",null,null,"W000",7.35,null,"","",null,null,null,"MTN","11","36+80.00 -L-"]
["","","","","","6","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",49320,"WL3","Y007",null,null,"W005",5.5,null,"","",null,null,null,"MTN","11","56+15.00 -L-"]
["","","","","","7","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",144720,"WL4","Y007",null,null,"W000",10.26,null,"","",null,null,null,"MTN","11","14+00.00 -Y5-"]
["","","","","","8","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",29700,"WL5","Y007",null,null,"W005",5.5,null,"","",null,null,null,"MTN","11","183+20.00 -L-"]
["","","","","","9","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",545155,"BR01","X080",1.7000000000000001E-2,null,"15",null,45,"722","A",2,42.833300000000001,87.739599999999996,"MTN","11","71+53.83-L-"]
["","","","","","10","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",534378.35,"BR02","X081",1.9E-2,null,"5",null,46.25,"754","A",1,44,100,"MTN","11","393+57.38-L-"]
["","","","","C203386-TC","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",752074.85,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203386-UT","1","ALLEGHANY","JAMES R VANNOY & SONS CONST CO",261793,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",17746033.399999999,"","",9.6839999999999993,null,"",null,null,null,null,null,null,null,"","",""]
["","19","B-4705","C203295","C203295-EC","1","ASHE","JAMES R VANNOY & SONS CONST CO",58056.33,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","C203295-RW","1","ASHE","JAMES R VANNOY & SONS CONST CO",120939.59,"RW1","I000",0.06,2,"B810",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","C203295-ST","1","ASHE","JAMES R VANNOY & SONS CONST CO",171946.06,"CV01","X028",5.9999999999999995E-4,5.73,"C003",47.25,9,"","",null,null,null,"V MTN","11","13+61.50 -L-"]
["","","","","C203295-TC","1","ASHE","JAMES R VANNOY & SONS CONST CO",21717.48,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","","","","Result",372659.46,"","",6.0600000000000001E-2,null,null,null,null,"","",null,null,null,"","",""]
["","20","B-4846","C203298","C203298-EC","1","WILKES","COUNTRY BOY LANDSCAPING INC",10894.24,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203298-RW","1","WILKES","COUNTRY BOY LANDSCAPING INC",214741.6,"RW1","I000",6.0999999999999999E-2,2,"B810",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203298-SI","1","WILKES","COUNTRY BOY LANDSCAPING INC",2073.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203298-ST","1","WILKES","COUNTRY BOY LANDSCAPING INC",415327.24,"BR01","X081",1.6E-2,null,"15",null,30,"729","A",1,27.83,82.32,"MTN","11","14+35.00 -L-"]
["","","","","C203298-TC","1","WILKES","COUNTRY BOY LANDSCAPING INC",9852.2000000000007,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",652888.88,"","",7.6999999999999999E-2,null,"",null,null,"","",null,null,null,"","",""]
["","21","B-5138","C203301","C203301-EC","1","CALDWELL","MILLER ENG CO INC",55778,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203301-RW","1","CALDWELL","MILLER ENG CO INC",166971.04999999999,"RW1","I000",2.9000000000000001E-2,2,"B810",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203301-SI","1","CALDWELL","MILLER ENG CO INC",4330,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203301-ST","1","CALDWELL","MILLER ENG CO INC",288500.65000000002,"CV01","X028",8.9999999999999993E-3,5.52,"C003",73.75,12,"","",null,null,null,"MTN","11","21+69.00 -L-"]
["","","","","C203301-TC","1","CALDWELL","MILLER ENG CO INC",6460,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203301-UT","1","CALDWELL","MILLER ENG CO INC",49892,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",571931.69999999995,"","",3.7999999999999999E-2,null,"",null,null,"","",null,null,null,"","",""]
["","22","B-5146","C203303","C203303-EC","1","WILKES","DEVERE CONST CO INC",65414.25,"RW1","I000",null,3,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203303-RW","1","WILKES","DEVERE CONST CO INC",300155,"RW1","I000",9.6000000000000002E-2,3,"B812",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203303-SG","1","WILKES","DEVERE CONST CO INC",45964,"RW1","I000",null,3,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203303-SI","1","WILKES","DEVERE CONST CO INC",2109.6799999999998,"RW1","I000",null,3,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203303-ST","1","WILKES","DEVERE CONST CO INC",523310,"BR01","X081",1.9E-2,null,"15",null,27,"733","A",1,24.833300000000001,102.6,"MTN","11","15+16.00-L-"]
["","","","","C203303-TC","1","WILKES","DEVERE CONST CO INC",35120.25,"RW1","I000",null,3,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",972073.18,"","",0.115,null,"",null,null,null,null,null,null,null,"","",""]
["","23","B-5101","C203299","C203299-EC","1","CATAWBA","DEVERE CONST CO INC",43750,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203299-RW","1","CATAWBA","DEVERE CONST CO INC",254660,"RW1","I000",0.10299999999999999,2,"B811",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203299-SI","1","CATAWBA","DEVERE CONST CO INC",5425.2,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203299-ST","1","CATAWBA","DEVERE CONST CO INC",588155.25,"BR01","X080",2.5100000000000001E-2,null,"15",null,36,"722","Q",3,33.5,132.583,"PDMT","12","16+83.50 -L-"]
["","","","","C203299-TC","1","CATAWBA","DEVERE CONST CO INC",2903.36,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",894893.81,"","",0.12809999999999999,null,null,null,null,null,null,null,null,null,"","",""]
["","25","","C203478","C203478A-RW","1","BURKE","MAYMEAD INC",1445420.7,"RW1","",5.77,5,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203478B-RW","1","BURKE","MAYMEAD INC",1436485.36,"RW1","",13.27,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",2881906.06,"","",19.04,null,"",null,null,"","",null,null,null,"","",""]
["","26","","C203481","C203481A-RW","1","MCDOWELL","MAYMEAD INC",2262600.16,"RW1","",16.73,5,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203481B-RW","1","MCDOWELL","MAYMEAD INC",1163969.3,"RW1","",5.75,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",3426569.46,"","",22.48,null,"",null,null,"","",null,null,null,"","",""]
["","27","","C203482","C203482A-RW","1","MITCHELL","ROGERS GROUP INC",1118701.68,"RW1","",5.17,4,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203482B-RW","1","MITCHELL","ROGERS GROUP INC",710848.48,"RW1","",5.04,3,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1829550.16,"","",10.210000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","28","","C203479","C203479A-RW","1","RUTHERFORD","HARRISON CONST CO DIV O",1163989.04,"RW1","",7.09,5,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203479B-RW","1","RUTHERFORD","HARRISON CONST CO DIV O",1915714.64,"RW1","",15,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",3079703.68,"","",22.09,null,"",null,null,"","",null,null,null,"","",""]
["","29","R-5527A","C203449","C203449-RW","1","CHEROKEE","SIMPSON CONST CO INC",2520623.35,"RW1","",4.7E-2,2,"B801",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",2520623.35,"","",4.7E-2,null,"",null,null,"","",null,null,null,"","",""]
["","30","","C203381","C203381-RW","1","DARE","DSC DREDGE LLC",7905189,"RW1","",null,null,"M713",null,null,"","",null,null,null,"COAST","1",""]
["","","","","","","","Result",7905189,"","",null,null,"",null,null,"","",null,null,null,"","",""]
["2/18/2014","1","B-4827","C203350","C203350-EC","1","VANCE","HURLEY GROUP LLC",71445,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203350-RW","1","VANCE","HURLEY GROUP LLC",222429.75,"RW1","I000",9.6000000000000002E-2,2,"B810",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203350-SI","1","VANCE","HURLEY GROUP LLC",3024,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203350-ST","1","VANCE","HURLEY GROUP LLC",555871.73,"BR01","X080",2.7E-2,null,"15",null,33,"721","Q",3,30.833300000000001,142.5,"PDMT","5","14+83.00 -L-"]
["","","","","C203350-TC","1","VANCE","HURLEY GROUP LLC",12834.95,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",865605.43,"","",0.123,null,"",null,null,null,null,null,null,null,"","",""]
["","2","B-4991","C202573","C202573-RW","1","WAKE","DEVERE CONST CO INC",1626458.25,"RW1","I000",0.23300000000000001,2,"B801",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C202573-ST","1","WAKE","DEVERE CONST CO INC",10125,"WL1","",null,null,"W005",3.72,null,"","",null,null,null,"PDMT","5","10+00.00 -L-"]
["","","","","","2","WAKE","DEVERE CONST CO INC",1419753.71,"BR01","X081",6.3E-2,null,"15",null,40.916699999999999,"854","Q",4,33,330,"PDMT","5","18+75.00 -L-"]
["","","","","C202573-TC","1","WAKE","DEVERE CONST CO INC",52612.45,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C202573-UT","2","WAKE","DEVERE CONST CO INC",818650,"RW1","NPAR",null,null,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",3927599.41,"","",0.29599999999999999,null,null,null,null,null,null,null,null,null,"","",""]
["","3","I-5205B","C203453","C203453-RW","1","GRANVILLE","AMERICAN CONT & SERVICES INC",1844010.49,"RW1","I000",0.17,4,"M720",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",1844010.49,"","",0.17,null,"",null,null,"","",null,null,null,"","",""]
["","4","B-4475","C203348","C203348-EC","1","COLUMBUS","SMITH-ROWE LLC",18584.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203348-RW","1","COLUMBUS","SMITH-ROWE LLC",194225,"RW1","I000",4.2999999999999997E-2,2,"B810",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203348-SI","1","COLUMBUS","SMITH-ROWE LLC",4113.6000000000004,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203348-ST","1","COLUMBUS","SMITH-ROWE LLC",304009.27,"BR01","X080",1.7000000000000001E-2,null,"15",null,33,"718","A",2,30.833300000000001,90,"COAST","6","15+66.00 -L-"]
["","","","","C203348-TC","1","COLUMBUS","SMITH-ROWE LLC",3284.36,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",524216.73,"","",0.06,null,"",null,null,null,null,null,null,null,"","",""]
["","5","B-5132","C203354","C203354-EC","1","HOKE","SMITH-ROWE LLC",18373,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203354-RW","1","HOKE","SMITH-ROWE LLC",185973,"RW1","I000",6.2E-2,2,"B810",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203354-SI","1","HOKE","SMITH-ROWE LLC",3016.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203354-ST","1","HOKE","SMITH-ROWE LLC",419885.1,"BR01","X080",2.3E-2,null,"15",null,33,"721","A",3,30.832999999999998,122.5,"PDMT","8","13+85.00 -L-"]
["","","","","C203354-TC","1","HOKE","SMITH-ROWE LLC",3226,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203354-UT","1","HOKE","SMITH-ROWE LLC",51605,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",682078.7,"","",8.5000000000000006E-2,null,null,null,null,null,null,null,null,null,"","",""]
["","6","B-5137","C203355","C203355-EC","1","STANLY","SMITH-ROWE LLC",18255.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203355-RW","1","STANLY","SMITH-ROWE LLC",219773,"RW1","I000",7.9000000000000001E-2,2,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203355-ST","1","STANLY","SMITH-ROWE LLC",404667.3,"BR01","X080",1.5599999999999999E-2,null,"15",null,36,"729","A",1,33.5,82.604200000000006,"PDMT","10","15+14.00 -L-"]
["","","","","C203355-TC","1","STANLY","SMITH-ROWE LLC",6174.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",648870.05000000005,"","",9.4600000000000004E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","7","","C203507","C203507A-RW","1","STANLY","J T RUSSELL & SONS INC",606740.52,"RW1","",1.56,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203507B-RW","1","STANLY","J T RUSSELL & SONS INC",396430.52,"RW1","",1.94,5,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203507C-RW","1","STANLY","J T RUSSELL & SONS INC",809982.08,"RW1","",6.27,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203507D-RW","1","STANLY","J T RUSSELL & SONS INC",70828.28,"RW1","",0.75,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203507E-RW","1","STANLY","J T RUSSELL & SONS INC",210779.46,"RW1","",1.36,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203507F-RW","1","STANLY","J T RUSSELL & SONS INC",19629.11,"RW1","",0.1,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",2114389.9700000002,"","",11.98,null,"",null,null,"","",null,null,null,"","",""]
["","8","B-4701","C203349","C203349-EC","1","ALLEGHANY","SMITH-ROWE LLC",31463.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203349-RW","1","ALLEGHANY","SMITH-ROWE LLC",198176,"RW1","I000",6.7000000000000004E-2,2,"B810",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203349-SI","1","ALLEGHANY","SMITH-ROWE LLC",4021.12,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C203349-ST","1","ALLEGHANY","SMITH-ROWE LLC",571379.06000000006,"BR01","X081",2.5600000000000001E-2,null,"15",null,29.25,"736","Q",3,26,135,"MTN","11","11+97.50 -L-"]
["","","","","C203349-TC","1","ALLEGHANY","SMITH-ROWE LLC",2998.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",808037.68,"","",9.2600000000000002E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","10","B-5110","C203353","C203353-EC","1","ALEXANDER","DEVERE CONST CO INC",41587.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203353-RW","1","ALEXANDER","DEVERE CONST CO INC",201692.05,"RW1","I000",8.8999999999999996E-2,2,"B810",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203353-SI","1","ALEXANDER","DEVERE CONST CO INC",3516.45,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203353-ST","1","ALEXANDER","DEVERE CONST CO INC",130391,"CV01","X028",6.0000000000000001E-3,3.5,"C003",40.5,10,"","",null,null,null,"MTN","12","13+44.00 -L-"]
["","","","","C203353-TC","1","ALEXANDER","DEVERE CONST CO INC",3065.8,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203353-UT","1","ALEXANDER","DEVERE CONST CO INC",39580,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",419832.8,"","",9.5000000000000001E-2,null,null,null,null,"","",null,null,null,"","",""]
["","11","B-5155","C203356","C203356-EC","1","LINCOLN","COUNTRY BOY LANDSCAPING INC",35361.86,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203356-RW","1","LINCOLN","COUNTRY BOY LANDSCAPING INC",264448.34999999998,"RW1","I000",0.125,2,"C002",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203356-ST","1","LINCOLN","COUNTRY BOY LANDSCAPING INC",410622.17,"CV01","X028",8.0000000000000002E-3,8.3000000000000007,"C101",70.75,42,"","",null,null,null,"PDMT","12","14+34.00 -L-"]
["","","","","C203356-TC","1","LINCOLN","COUNTRY BOY LANDSCAPING INC",7456.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",717888.88,"","",0.13300000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","12","I-5606","C203384","C203384-RW","1","IREDELL","MAYMEAD INC",8762940.6099999994,"RW1","I000",7.2,4,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",8762940.6099999994,"","",7.2,null,"",null,null,"","",null,null,null,"","",""]
["","13","B-4984","C203351","C203351-EC","1","MADISON","BUCKEYE BRG LLC",66587.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203351-RW","1","MADISON","BUCKEYE BRG LLC",291028.5,"RW1","I000",3.9E-2,2,"B812",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203351-SI","1","MADISON","BUCKEYE BRG LLC",739.2,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203351-ST","1","MADISON","BUCKEYE BRG LLC",72450,"WL1","Y007",null,null,"W000",7.63,null,"","",null,null,null,"V MTN","13","13+01.30-L-"]
["","","","","","2","MADISON","BUCKEYE BRG LLC",552456.15,"BR01","X080",1.2999999999999999E-2,null,"15",null,30,"722","A",1,27.5,72.593800000000002,"V MTN","13","13+01.30 -L-"]
["","","","","C203351-TC","1","MADISON","BUCKEYE BRG LLC",76813.66,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1060075.01,"","",5.1999999999999998E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","14","","C203506","C203506A-RW","1","BUNCOMBE","HARRISON CONST CO DIV O",2541187.0299999998,"RW1","",9.2100000000000009,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203506B-RW","1","BUNCOMBE","HARRISON CONST CO DIV O",1874518.34,"RW1","",14.99,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",4415705.37,"","",24.2,null,"",null,null,"","",null,null,null,"","",""]
["","15","","C203504","C203504A-RW","1","MADISON","HARRISON CONST CO DIV O",1276191.72,"RW1","",4.1100000000000003,5,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203504B-RW","1","MADISON","HARRISON CONST CO DIV O",1175175.3600000001,"RW1","",8.36,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",2451367.08,"","",12.47,null,"",null,null,"","",null,null,null,"","",""]
["","16","","C203505","C203505A-RW","1","YANCEY","MAYMEAD INC",850877.32,"RW1","",6.4,4,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203505B-RW","1","YANCEY","MAYMEAD INC",738853.76,"RW1","",4.7699999999999996,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1589731.08,"","",11.17,null,"",null,null,"","",null,null,null,"","",""]
["","17","B-3346","C203347","C203347-EC","1","HENDERSON","DEVERE CONST CO INC",52285,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203347-RW","1","HENDERSON","DEVERE CONST CO INC",487871,"RW1","I000",7.8E-2,2,"B801",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203347-SI","1","HENDERSON","DEVERE CONST CO INC",3118,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203347-ST","1","HENDERSON","DEVERE CONST CO INC",136875,"WL1","Y007",null,null,"W000",13.64,null,"","",null,null,null,"V MTN","14","12+71.50 -L-"]
["","","","","","2","HENDERSON","DEVERE CONST CO INC",305404.75,"BR01","X080",8.9999999999999993E-3,null,"15",null,27,"718","B",1,24.75,47.281300000000002,"V MTN","14","12+71.50 -L-"]
["","","","","","3","HENDERSON","DEVERE CONST CO INC",35000,"BR02","X001",6.9999999999999999E-4,null,"0",null,7,"98","A",1,5.5,35.666699999999999,"V MTN","14","BR 440042"]
["","","","","C203347-TC","1","HENDERSON","DEVERE CONST CO INC",4395.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",1024949.25,"","",8.77E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","18","B-4988","C203352","C203352-EC","1","HENDERSON","NHM CONSTR LLC",43707.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203352-RW","1","HENDERSON","NHM CONSTR LLC",120234.44,"RW1","I000",4.4999999999999998E-2,2,"C002",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203352-SI","1","HENDERSON","NHM CONSTR LLC",1824,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203352-ST","1","HENDERSON","NHM CONSTR LLC",213978.1,"CV01","X028",5.8999999999999999E-3,3.74,"C002",76.75,8,"","",null,null,null,"V MTN","14","15+84.00 -L-"]
["","","","","C203352-TC","1","HENDERSON","NHM CONSTR LLC",4210,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",383954.04,"","",5.0900000000000001E-2,null,"",null,null,"","",null,null,null,"","",""]
["3/18/2014","1","R-5505","C203422","C203422-RW","1","NORTHAMPTON","ROSE BROS PAVING CO INC",2720296,"RW1","I000",14.5,2,"R000",null,null,"","",null,null,null,"PDMT","1",""]
["","","","","","","","Result",2720296,"","",14.5,null,"",null,null,"","",null,null,null,"","",""]
["","2","B-4785","C203366","C203366-EC","1","PERSON","FSC II LLC DBA FRED SMITH CO",21422.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203366-RW","1","PERSON","FSC II LLC DBA FRED SMITH CO",177373.5,"RW1","I000",6.3E-2,2,"C002",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203366-SI","1","PERSON","FSC II LLC DBA FRED SMITH CO",2492,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203366-ST","1","PERSON","FSC II LLC DBA FRED SMITH CO",573000,"CV01","X024",0.01,3.06,"15",63,48,"","",null,null,null,"PDMT","5","13+71.41 -L-"]
["","","","","C203366-TC","1","PERSON","FSC II LLC DBA FRED SMITH CO",8857,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",783145,"","",7.2999999999999995E-2,null,"",null,null,"","",null,null,null,"","",""]
["","3","","C203512","C203512-RW","1","DURHAM","PALMETTO INFRASTR INC",1250683.3500000001,"RW1","",3.4000000000000002E-2,2,"M720",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",1250683.3500000001,"","",3.4000000000000002E-2,null,"",null,null,"","",null,null,null,"","",""]
["","4","R-5526","C203456","C203456-RW","1","HARNETT","FSC II LLC DBA FRED SMITH CO",2304342.65,"RW1","I000",1.2090000000000001,2,"N200",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203456-SG","1","HARNETT","FSC II LLC DBA FRED SMITH CO",18900,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203456-ST","1","HARNETT","FSC II LLC DBA FRED SMITH CO",124259.6,"CV01","Y007",4.0000000000000001E-3,3,"C002",50.42,10,"","",null,null,null,"PDMT","6","58+98 -L-"]
["","","","","","","","Result",2447502.25,"","",1.2130000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","5","B-4758","C203363","C203363-EC","1","GUILFORD","SMITH-ROWE LLC",37005,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203363-RW","1","GUILFORD","SMITH-ROWE LLC",219448,"RW1","I000",6.9000000000000006E-2,2,"B810",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203363-SI","1","GUILFORD","SMITH-ROWE LLC",4201,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203363-ST","1","GUILFORD","SMITH-ROWE LLC",549005.36,"BR01","X080",2.1299999999999999E-2,null,"15",null,30,"722","Q",3,27.833300000000001,112.5,"PDMT","7","16+64.29 -L-"]
["","","","","C203363-TC","1","GUILFORD","SMITH-ROWE LLC",2874,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",812533.36,"","",9.0300000000000005E-2,null,"",null,null,"","",null,null,null,"","",""]
["","6","B-5131","C203367","C203367-EC","1","SCOTLAND","SMITH-ROWE LLC",23289,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203367-RW","1","SCOTLAND","SMITH-ROWE LLC",155386,"RW1","I000",5.0999999999999997E-2,2,"C002",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203367-SI","1","SCOTLAND","SMITH-ROWE LLC",2729,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203367-ST","1","SCOTLAND","SMITH-ROWE LLC",322217.92,"BR01","X080",1.4999999999999999E-2,null,"15",null,33,"718","A",2,30.5,77.375,"PDMT","8","17+45.00 -L-"]
["","","","","C203367-TC","1","SCOTLAND","SMITH-ROWE LLC",3658.36,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203367-UT","1","SCOTLAND","SMITH-ROWE LLC",39940,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",547220.28,"","",6.6000000000000003E-2,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203522","C203522A-RW","1","HOKE","HUDSON PAVING INC",1002707.19,"RW1","",9.0530000000000008,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203522B-RW","1","HOKE","HUDSON PAVING INC",736332.12,"RW1","",5.89,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203522C-RW","1","SCOTLAND","HUDSON PAVING INC",808208.09,"RW1","",7.76,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",2547247.4,"","",22.702999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","8","","C203523","C203523A-RW","1","LEE","RILEY PAVING INC",428974.2,"RW1","",3.31,5,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203523B-RW","1","LEE","RILEY PAVING INC",768406.8,"RW1","",7.2880000000000003,5,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",1197381,"","",10.598000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","9","","C203524","C203524A-RW","1","MONTGOMERY","J T RUSSELL & SONS INC",218526.05,"RW1","",1.51,1,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203524B-RW","1","MONTGOMERY","J T RUSSELL & SONS INC",901791.1,"RW1","",8.74,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",1120317.1499999999,"","",10.25,null,"",null,null,"","",null,null,null,"","",""]
["","10","","C203525","C203525A-RW","1","MOORE","S T WOOTEN CORP",1574998.25,"RW1","",10.789,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203525B-RW","1","MOORE","S T WOOTEN CORP",1296461,"RW1","",12.39,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",2871459.25,"","",23.178999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C203526","C203526A-RW","1","RANDOLPH","BLYTHE CONST INC",463589.97,"RW1","",2.3079999999999998,3,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203526B-RW","1","RANDOLPH","BLYTHE CONST INC",3001973.1,"RW1","",23.417000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",3465563.07,"","",25.725000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","12","","C203521","C203521-RW","1","CHATHAM","S T WOOTEN CORP",1209922.21,"RW1","",11.214,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",1209922.21,"","",11.214,null,"",null,null,"","",null,null,null,"","",""]
["","13","","C203527","C203527-RW","1","RICHMOND","HUDSON PAVING INC",738950.95,"RW1","",8.5299999999999994,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",738950.95,"","",8.5299999999999994,null,"",null,null,"","",null,null,null,"","",""]
["","14","B-4740","C203362","C203362-EC","1","DAVIDSON","DANE CONST INC",53277.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203362-RW","1","DAVIDSON","DANE CONST INC",334885.59999999998,"RW1","I000",0.153,2,"B810",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203362-SI","1","DAVIDSON","DANE CONST INC",3290.78,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203362-ST","1","DAVIDSON","DANE CONST INC",450267.41,"BR01","X080",1.9900000000000001E-2,null,"15",null,33,"733","A",1,30.833300000000001,105,"PDMT","9","14+66.00 -L-"]
["","","","","C203362-TC","1","DAVIDSON","DANE CONST INC",3130.95,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",844852.24,"","",0.1729,null,"",null,null,"","",null,null,null,"","",""]
["","15","B-4651","C203426","C203426-EC","1","UNION","BLYTHE CONST INC",77175.27,"RW1","I000",null,3,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203426-RW","1","UNION","BLYTHE CONST INC",562248.69999999995,"RW1","I000",0.13400000000000001,3,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203426-ST","1","UNION","BLYTHE CONST INC",893524,"BR01","X080",2.5999999999999999E-2,null,"15",null,51,"121","I",3,43.041699999999999,142.25,"PDMT","10","17+73.00 -L-"]
["","","","","C203426-UT","1","UNION","BLYTHE CONST INC",56820.1,"RW1","I000",null,3,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",1589768.07,"","",0.16,null,"",null,null,"","",null,null,null,"","",""]
["","16","B-4779","C203284","C203284-EC","1","MECKLENBURG","DEVERE CONST CO INC",114163.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203284-RW","1","MECKLENBURG","DEVERE CONST CO INC",1669995,"RW1","I000",0.17699999999999999,4,"B813",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203284-SI","1","MECKLENBURG","DEVERE CONST CO INC",13735.9,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203284-ST","1","MECKLENBURG","DEVERE CONST CO INC",1131917.05,"BR01","X080",2.9000000000000001E-2,null,"15",null,57,"722","Q",3,46,155,"PDMT","10","20+20.50 -L-"]
["","","","","","2","MECKLENBURG","DEVERE CONST CO INC",972199,"BR02","X080",null,null,"15",null,45,"722","Q",3,34,155,"PDMT","10","20+47.50 -L-"]
["","","","","C203284-TC","1","MECKLENBURG","DEVERE CONST CO INC",257719.3,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203284-UT","1","MECKLENBURG","DEVERE CONST CO INC",325,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","2","MECKLENBURG","DEVERE CONST CO INC",233782.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",4393837.25,"","",0.20599999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","17","B-5134","C203368","C203368-EC","1","UNION","DELLINGER INC",29294.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203368-RW","1","UNION","DELLINGER INC",368006.5,"RW1","I000",7.5999999999999998E-2,2,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203368-SI","1","UNION","DELLINGER INC",850,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203368-ST","1","UNION","DELLINGER INC",624042,"BR01","X080",1.9E-2,null,"15",null,36,"733","A",1,33.833300000000001,102.604,"PDMT","10","15+09.00 -L-"]
["","","","","C203368-TC","1","UNION","DELLINGER INC",16087.2,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",1038280.2,"","",9.5000000000000001E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","18","I-4928","C203357","C203357-EC","1","GASTON","SLOAN CONST A DIV OF REEVES",837783.25,"RW1","Y222",null,1,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203357-LI","1","GASTON","SLOAN CONST A DIV OF REEVES",1285810.05,"RW1","Y222",null,1,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203357-RW","1","GASTON","SLOAN CONST A DIV OF REEVES",14441433.380000001,"RW1","Y222",2.2440000000000002,1,"M720",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203357-SG","1","GASTON","SLOAN CONST A DIV OF REEVES",1590375.11,"RW1","Y222",null,1,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203357-SI","1","GASTON","SLOAN CONST A DIV OF REEVES",395857.38,"RW1","Y222",null,1,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203357-ST","1","GASTON","SLOAN CONST A DIV OF REEVES",329175.40000000002,"CV01","Y007",null,41.17,"C202",92.42,6,"","",null,null,null,"PDMT","12","153+40.68 -L-"]
["","","","","C203357-TC","1","GASTON","SLOAN CONST A DIV OF REEVES",404101.25,"RW1","Y222",null,1,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203357-UT","1","GASTON","SLOAN CONST A DIV OF REEVES",447722.5,"RW1","Y222",null,1,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",19732258.32,"","",2.2440000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","19","B-5167","C203369","C203369-EC","1","BUNCOMBE","NHM CONSTR LLC",89290,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203369-RW","1","BUNCOMBE","NHM CONSTR LLC",391494,"RW1","I000",8.5000000000000006E-2,2,"C002",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203369-SI","1","BUNCOMBE","NHM CONSTR LLC",1888.42,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203369-ST","1","BUNCOMBE","NHM CONSTR LLC",220050,"CV01","Y007",5.0000000000000001E-3,4.4000000000000004,"C002",45.92,12,"","",null,null,null,"MTN","13","16+00.00 -L-"]
["","","","","C203369-TC","1","BUNCOMBE","NHM CONSTR LLC",63503.17,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",766225.59,"","",0.09,null,"",null,null,"","",null,null,null,"","",""]
["","20","I-5501","C203530","C203200-EC","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",215852.5,"RW1","I000",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203200-LI","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",519393.5,"RW1","I000",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203200-RW","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",6215153.7699999996,"RW1","I000",0.435,5,"M720",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203200-SG","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",596175.94999999995,"RW1","I000",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203200-SI","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",326192.05,"RW1","I000",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203200-ST","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",102604.5,"WL1","Y007",null,null,"0",6.25,null,"","",null,null,null,"MTN","13","10+00.00 -WALL1-"]
["","","","","","2","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",302455.05,"BR01","X281",5.7000000000000002E-2,null,"11",null,83.082999999999998,"854","I",4,80,303,"MTN","13","25 + 83.78 -L-"]
["","","","","C203200-TC","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",291809.7,"RW1","I000",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203200-UT","1","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",9000,"RW1","I000",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","2","BUNCOMBE","YOUNG & MCQUEEN GRADING CO INC",196900,"RW1","NPAR",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",8775537.0199999996,"","",0.49199999999999999,null,"",null,null,null,null,null,null,null,"","",""]
["","21","B-4762","C203364","C203364-EC","1","HAYWOOD","NHM CONSTR LLC",22115,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203364-RW","1","HAYWOOD","NHM CONSTR LLC",196136.3,"RW1","I000",8.0000000000000002E-3,2,"B801",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203364-ST","1","HAYWOOD","NHM CONSTR LLC",407168.25,"BR01","X080",1.4E-2,null,"15",null,27,"722","A",1,24.833300000000001,72.25,"V MTN","14","10+58.00 -L-"]
["","","","","C203364-TC","1","HAYWOOD","NHM CONSTR LLC",26159.599999999999,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",651579.15,"","",2.1999999999999999E-2,null,"",null,null,"","",null,null,null,"","",""]
["","22","B-4763","C203365","C203365-EC","1","HAYWOOD","SIMPSON CONST CO INC",119421.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203365-RW","1","HAYWOOD","SIMPSON CONST CO INC",544830.69999999995,"RW1","I000",0.16800000000000001,2,"C002",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203365-SI","1","HAYWOOD","SIMPSON CONST CO INC",3042,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203365-ST","1","HAYWOOD","SIMPSON CONST CO INC",336425.25,"CV01","X028",1.0999999999999999E-2,3.69,"C002",94,14,"","",null,null,null,"V MTN","14","15+16.00 -L-"]
["","","","","C203365-TC","1","HAYWOOD","SIMPSON CONST CO INC",21503.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",1025222.7,"","",0.17899999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","23","K-5002","C203202","C203202-EC","1","HAYWOOD","BUCHANAN AND SONS INC",360161.15,"RW1","Y022",null,1,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203202-LI","1","HAYWOOD","BUCHANAN AND SONS INC",231880,"RW1","Y022",null,1,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203202-RA","1","HAYWOOD","BUCHANAN AND SONS INC",3551008.7,"RW1","Y022",null,1,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203202-RW","1","HAYWOOD","BUCHANAN AND SONS INC",1901154.88,"RW1","Y022",0.26500000000000001,1,"M701",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203202-SI","1","HAYWOOD","BUCHANAN AND SONS INC",28315.1,"RW1","Y022",null,1,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203202-TC","1","HAYWOOD","BUCHANAN AND SONS INC",79196.2,"RW1","Y022",null,1,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",6151716.0300000003,"","",0.26500000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","24","R-5527B","C203454","C203454-RW","1","CHEROKEE","ADAMS CONT",4365362.32,"RW1","",0.47399999999999998,2,"N240",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",4365362.32,"","",0.47399999999999998,null,"",null,null,"","",null,null,null,"","",""]
["4/3/2014","1","I-5110","C203433","C203433B-RW","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",48355000,"RW1","I000",1.62,4,"M713",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203433C-RW","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",12750000,"RW1","I000",null,4,"M713",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",61105000,"","",1.62,null,"",null,null,"","",null,null,null,"","",""]
["","","R-2413A","C203433","C203433A-RW","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",115445000,"RW1","",7.78,4,"M713",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",115445000,"","",7.78,null,"",null,null,"","",null,null,null,"","",""]
["","2","I-3802A","C203328","C203328-RW","1","CABARRUS","BLYTHE CONST INC",186687000,"RW1","I000",7.9,8,"M713",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",186687000,"","",7.9,null,"",null,null,"","",null,null,null,"","",""]
["4/15/2014","1","B-4748","C203390","C203390-EC","1","FRANKLIN","DANE CONST INC",51337.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203390-RW","1","FRANKLIN","DANE CONST INC",339209.5,"RW1","I000",0.114,2,"B810",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203390-SI","1","FRANKLIN","DANE CONST INC",5120,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203390-ST","1","FRANKLIN","DANE CONST INC",439555.08,"BR01","X081",1.9E-2,null,"15",null,34.583300000000001,"754","A",1,32,100,"PDMT","5","14+12.00 -L-"]
["","","","","C203390-TC","1","FRANKLIN","DANE CONST INC",3968.65,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",839190.73,"","",0.13300000000000001,null,"",null,null,null,null,null,null,null,"","",""]
["","2","","C203542","C203542A-RW","1","WARREN","S T WOOTEN CORP",170910.45,"RW1","I000",1.1499999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203542B-RW","1","FRANKLIN","S T WOOTEN CORP",696353.75,"RW1","I000",6.7,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203542C-RW","1","WARREN","S T WOOTEN CORP",1691964.6,"RW1","I000",17.899999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203542D-RW","1","WARREN","S T WOOTEN CORP",722555.1,"RW1","I000",11.58,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",3281783.9,"","",37.33,null,"",null,null,"","",null,null,null,"","",""]
["","3","","C203543","C203543A-RW","1","VANCE","S T WOOTEN CORP",1580073.26,"RW1","I000",15.9,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203543B-RW","1","VANCE","S T WOOTEN CORP",787740.82,"RW1","I000",9.1,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",2367814.08,"","",25,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C203511","C203511A-RW","1","ANSON","BARNHILL CONT CO",1069182.8500000001,"RW1","",4.0999999999999996,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203511B-RW","1","ANSON","BARNHILL CONT CO",985639.76,"RW1","",3.7,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203511C-RW","1","ANSON","BARNHILL CONT CO",407515.82,"RW1","",2.7,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203511D-RW","1","ANSON","BARNHILL CONT CO",206291.56,"RW1","",1.9,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203511E-RW","1","ANSON","BARNHILL CONT CO",421645.14,"RW1","",3.2,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203511F-RW","1","ANSON","BARNHILL CONT CO",194405.35,"RW1","",1.3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",3284680.48,"","",16.899999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C203541","C203541A-RW","1","CABARRUS","BLYTHE CONST INC",535811.27,"RW1","",3.15,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541B-RW","1","CABARRUS","BLYTHE CONST INC",773761.35,"RW1","",2.5499999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541C-RW","1","CABARRUS","BLYTHE CONST INC",450677.3,"RW1","",1.86,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541D-RW","1","CABARRUS","BLYTHE CONST INC",527464.94999999995,"RW1","",3.15,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541E-RW","1","CABARRUS","BLYTHE CONST INC",69347.399999999994,"RW1","",0.4,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541F-RW","1","CABARRUS","BLYTHE CONST INC",222159.25,"RW1","",1.54,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541G-RW","1","CABARRUS","BLYTHE CONST INC",65911.05,"RW1","",0.42,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541H-RW","1","CABARRUS","BLYTHE CONST INC",170252.25,"RW1","",0.75,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541I-RW","1","CABARRUS","BLYTHE CONST INC",68777.100000000006,"RW1","",0.37,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541J-RW","1","CABARRUS","BLYTHE CONST INC",446940.4,"RW1","",1.53,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541K-RW","1","CABARRUS","BLYTHE CONST INC",16531.599999999999,"RW1","",1.1000000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203541L-RW","1","CABARRUS","BLYTHE CONST INC",41844.6,"RW1","",3.2,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",3389478.52,"","",20.02,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C203531","C203531A-RW","1","UNION","BLYTHE CONST INC",548334.36,"RW1","",2.1,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531B-RW","1","UNION","BLYTHE CONST INC",486489.34,"RW1","",1.9,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531C-RW","1","UNION","BLYTHE CONST INC",333330.40999999997,"RW1","",1.3,5,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531D-RW","1","UNION","BLYTHE CONST INC",288757.17,"RW1","",1.1000000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531E-RW","1","UNION","BLYTHE CONST INC",439045.67,"RW1","",1.7,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531F-RW","1","UNION","BLYTHE CONST INC",944310.05,"RW1","",3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531G-RW","1","UNION","BLYTHE CONST INC",317456.98,"RW1","",1.9,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531H-RW","1","UNION","BLYTHE CONST INC",523502.24,"RW1","",2.8,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531I-RW","1","UNION","BLYTHE CONST INC",384724.35,"RW1","",2.62,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531J-RW","1","UNION","BLYTHE CONST INC",206001.94,"RW1","",0.6,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531K-RW","1","UNION","BLYTHE CONST INC",146016,"RW1","",0.7,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531L-RW","1","UNION","BLYTHE CONST INC",279956.09999999998,"RW1","",1.5,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203531M-RW","1","UNION","BLYTHE CONST INC",732098.93,"RW1","",3.55,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",5630023.54,"","",24.77,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203508","C203508-EC","1","SURRY","SMITH-ROWE LLC",61883.75,"RW1","",null,3,"",null,null,"","",null,null,null,"PDMT","11",""]
["","","","","C203508-RW","1","SURRY","SMITH-ROWE LLC",792221.62,"RW1","",0.186,3,"",null,null,"","",null,null,null,"PDMT","11",""]
["","","","","C203508-SI","1","SURRY","SMITH-ROWE LLC",12525,"RW1","",null,3,"R000",null,null,"","",null,null,null,"PDMT","11",""]
["","","","","C203508-ST","1","SURRY","SMITH-ROWE LLC",167176.79999999999,"WL1","Y007",null,null,"W000",12.21,null,"","",null,null,null,"PDMT","11","15+67.28 -L- EB1"]
["","","","","","2","SURRY","SMITH-ROWE LLC",180958.56,"WL2","Y007",null,null,"W000",13.76,null,"","",null,null,null,"PDMT","11","15+67.28 -L- EB2"]
["","","","","","3","SURRY","SMITH-ROWE LLC",133133.84,"WL3","Y007",null,null,"W000",12.26,null,"","",null,null,null,"PDMT","11","14+62.76 -L1- EB1"]
["","","","","","4","SURRY","SMITH-ROWE LLC",147988.79999999999,"WL4","Y007",null,null,"W000",13.5,null,"","",null,null,null,"PDMT","11","14+62.76 -L1- EB2"]
["","","","","","5","SURRY","SMITH-ROWE LLC",878245.78,"BR01","X281",2.8000000000000001E-2,null,"11",null,53.583300000000001,"845","D",2,40,150,"PDMT","11","15+67.28 -L-"]
["","","","","","6","SURRY","SMITH-ROWE LLC",599265.13,"BR02","X281",0.03,null,"11",null,33.25,"845","D",2,30.5,157,"PDMT","11","14+62.76 -L1-"]
["","","","","C203508-TC","1","SURRY","SMITH-ROWE LLC",166483.6,"RW1","",null,3,"",null,null,"","",null,null,null,"PDMT","11",""]
["","","","","","","","Result",3139882.88,"","",0.24399999999999999,null,"",null,null,null,null,null,null,null,"","",""]
["","11","B-4288","C202778","C202778-EC","1","TRANSYLVANIA","NHM CONSTR LLC",67754,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C202778-RW","1","TRANSYLVANIA","NHM CONSTR LLC",270888.3,"RW1","I000",9.7000000000000003E-2,2,"B801",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C202778-SI","1","TRANSYLVANIA","NHM CONSTR LLC",4693,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C202778-ST","1","TRANSYLVANIA","NHM CONSTR LLC",282494,"BR01","X080",1.2E-2,null,"15",null,30,"722","A",1,27.5,62.25,"V MTN","14","12+81.00 -L2-"]
["","","","","C202778-TC","1","TRANSYLVANIA","NHM CONSTR LLC",41966.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",667795.9,"","",0.109,null,"",null,null,null,null,null,null,null,"","",""]
["","12","","C203509","C203509-RW","1","SURRY","SMITH-ROWE LLC",10342293.98,"RW1","",0.96,2,"M713",null,null,"","",null,null,null,"PDMT","11",""]
["","","","","","","","Result",10342293.98,"","",0.96,null,"",null,null,"","",null,null,null,"","",""]
["","13","","C203510","C203510-RW","1","BURKE","RE BURNS & SONS CO INC",7473172,"RW1","",0.83,2,"M713",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",7473172,"","",0.83,null,"",null,null,"","",null,null,null,"","",""]
["5/20/2014","1","B-5141","C203396","C203396-EC","1","BERTIE","S T WOOTEN CORP",104035,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203396-RW","1","BERTIE","S T WOOTEN CORP",938394.75,"RW1","I000",0.13100000000000001,2,"B812",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203396-SI","1","BERTIE","S T WOOTEN CORP",8298.9,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203396-ST","1","BERTIE","S T WOOTEN CORP",871661.19,"BR01","X081",2.1000000000000001E-2,null,"15",null,43.25,"845","A",2,40,110,"COAST","1","15+67.00 -L-"]
["","","","","C203396-TC","1","BERTIE","S T WOOTEN CORP",28335.8,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203396-UT","1","BERTIE","S T WOOTEN CORP",69954,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","","","","Result",2020679.64,"","",0.152,null,"",null,null,null,null,null,null,null,"","",""]
["","2","B-4591","C203395","C203395-EC","1","PENDER","S T WOOTEN CORP",142783.78,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203395-RW","1","PENDER","S T WOOTEN CORP",1050925,"RW1","I000",0.40300000000000002,2,"B810",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203395-SI","1","PENDER","S T WOOTEN CORP",12110.2,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","C203395-ST","1","PENDER","S T WOOTEN CORP",818039.7,"BR01","X081",1.7000000000000001E-2,null,"15",null,34.583300000000001,"836","A",2,32,90,"COAST","3","23+25.00 -L-"]
["","","","","C203395-TC","1","PENDER","S T WOOTEN CORP",5852.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
["","","","","","","","Result",2029711.18,"","",0.42,null,null,null,null,null,null,null,null,null,"","",""]
["","3","U-3609A","C202603","C202603-RW","1","WAYNE","FSC II LLC DBA FRED SMITH CO",2586106,"RW1","I000",1.081,4,"D345",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","C202603-ST","1","WAYNE","FSC II LLC DBA FRED SMITH CO",182394,"CV01","Y007",null,2.99,"C102",93.25,6,"","",null,null,null,"PDMT","4","33+65.00 -L-"]
["","","","","","","","Result",2768500,"","",1.081,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C203553","C203553A-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",1275661.93,"RW1","",5.0999999999999996,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203553B-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",1470808.59,"RW1","",9.9320000000000004,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",2746470.52,"","",15.032,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C203554","C203554A-RW","1","WAKE","FSC II LLC DBA FRED SMITH CO",877346.45,"RW1","",2.952,3,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203554B-RW","1","WAKE","FSC II LLC DBA FRED SMITH CO",3931393.59,"RW1","",16.84,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",4808740.04,"","",19.792000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C203555","C203555A-RW","1","WAKE","FSC II LLC DBA FRED SMITH CO",981346.62,"RW1","",3.83,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203555B-RW","1","WAKE","FSC II LLC DBA FRED SMITH CO",3825250.56,"RW1","",3.83,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",4806597.18,"","",7.66,null,"",null,null,"","",null,null,null,"","",""]
["","7","W-5114","C203415","C203415-EC","1","GUILFORD","YATES CONST CO INC",193876.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203415-LI","1","GUILFORD","YATES CONST CO INC",25000,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203415-RW","1","GUILFORD","YATES CONST CO INC",1464294.32,"RW1","I000",0.52100000000000002,2,"D300",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203415-SI","1","GUILFORD","YATES CONST CO INC",23525.1,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203415-TC","1","GUILFORD","YATES CONST CO INC",113111.22,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",1819807.14,"","",0.52100000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","8","B-5164","C203397","C203397-EC","1","MOORE","TCB BUILDERS LLC",25825.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203397-RW","1","MOORE","TCB BUILDERS LLC",138285.75,"RW1","I000",5.1999999999999998E-2,2,"B810",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203397-SI","1","MOORE","TCB BUILDERS LLC",3001,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203397-ST","1","MOORE","TCB BUILDERS LLC",411919.1,"BR01","X080",2.1999999999999999E-2,null,"15",null,30,"722","A",2,27.833300000000001,117.375,"PDMT","8","15+64.50 -L-"]
["","","","","C203397-TC","1","MOORE","TCB BUILDERS LLC",4076.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",583107.85,"","",7.3999999999999996E-2,null,"",null,null,null,null,null,null,null,"","",""]
["","9","","C203557","C203557A-RW","1","MECKLENBURG","FEREBEE CORP",133268.64000000001,"RW1","",0.56499999999999995,3,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557B-RW","1","MECKLENBURG","FEREBEE CORP",56571.46,"RW1","",0.38600000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557C-RW","1","MECKLENBURG","FEREBEE CORP",138317.84,"RW1","",1.0229999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557D-RW","1","MECKLENBURG","FEREBEE CORP",287825.34000000003,"RW1","",1.671,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557E-RW","1","MECKLENBURG","FEREBEE CORP",84683.89,"RW1","",0.23200000000000001,4,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557F-RW","1","MECKLENBURG","FEREBEE CORP",111570.17,"RW1","",0.54300000000000004,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557G-RW","1","MECKLENBURG","FEREBEE CORP",89066.21,"RW1","",0.441,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557H-RW","1","MECKLENBURG","FEREBEE CORP",150694.03,"RW1","",1.0469999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557I-RW","1","MECKLENBURG","FEREBEE CORP",205847.62,"RW1","",1.4019999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557J-RW","1","MECKLENBURG","FEREBEE CORP",77266.47,"RW1","",0.41,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557K-RW","1","MECKLENBURG","FEREBEE CORP",166050.5,"RW1","",0.51200000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557L-RW","1","MECKLENBURG","FEREBEE CORP",160197.18,"RW1","",1.054,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557M-RW","1","MECKLENBURG","FEREBEE CORP",205471.39,"RW1","",1.0009999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557N-RW","1","MECKLENBURG","FEREBEE CORP",278775.90000000002,"RW1","",0.81799999999999995,4,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557O-RW","1","MECKLENBURG","FEREBEE CORP",128150.56,"RW1","",0.51800000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557P-RW","1","MECKLENBURG","FEREBEE CORP",191746.19,"RW1","",1.1379999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557Q-RW","1","MECKLENBURG","FEREBEE CORP",167246.12,"RW1","",1.1339999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557R-RW","1","MECKLENBURG","FEREBEE CORP",113703.05,"RW1","",0.35599999999999998,3,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203557S-RW","1","MECKLENBURG","FEREBEE CORP",91684.81,"RW1","",0.39800000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",2838137.37,"","",14.648999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","10","","C203556","C203556A-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",220430.28,"RW1","",0.68,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556B-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",105244.88,"RW1","",0.64300000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556C-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",304533.23,"RW1","",1.234,3,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556D-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",481356.34,"RW1","",1.6839999999999999,3,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556E-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",344470.06,"RW1","",2.1589999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556F-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",20668.849999999999,"RW1","",0.183,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556G-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",185787.85,"RW1","",1.157,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556H-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",461497.4,"RW1","",3.17,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556I-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",233096.3,"RW1","",0.98099999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556J-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",198462.98,"RW1","",1.196,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556K-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",195718.37,"RW1","",1.1539999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556L-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",53203.64,"RW1","",0.30499999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203556M-RW","1","MECKLENBURG","J T RUSSELL & SONS INC",129473.07,"RW1","",0.82,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",2933943.25,"","",15.366,null,"",null,null,"","",null,null,null,"","",""]
["","13","R-2707AB","C203547","C203027-ECC","1","CLEVELAND","ES WAGNER CO LLC ",662880.24,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203027-RWC","1","CLEVELAND","ES WAGNER CO LLC ",4084234.26,"RW1","I000",1.6559999999999999,4,"G401",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203027-SIC","1","CLEVELAND","ES WAGNER CO LLC ",2140.16,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203027-STC","4","CLEVELAND","ES WAGNER CO LLC ",1236538.98,"BR01","X081",4.8300000000000003E-2,null,"15",null,41.25,"854","E",3,38,255,"MTN","12","157+75.50 -L- WBL"]
["","","","","","5","CLEVELAND","ES WAGNER CO LLC ",962983.03,"BR02","X081",null,null,"15",null,41.25,"854","E",3,38,255,"MTN","12","157+75.50 -L- EBL"]
["","","","","","6","CLEVELAND","ES WAGNER CO LLC ",671145.36,"BR03","X281",null,null,"11",null,43.25,"864","A",2,40,181.34,"MTN","12","203+50.35 -L-"]
["","","","","C203027-TCC","1","CLEVELAND","ES WAGNER CO LLC ",7800.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203027-UTC","1","CLEVELAND","ES WAGNER CO LLC ",67683.67,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","2","CLEVELAND","ES WAGNER CO LLC ",244799.63,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","3","CLEVELAND","ES WAGNER CO LLC ",40591.07,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","4","CLEVELAND","ES WAGNER CO LLC ",112632.7,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",8093429.5999999996,"","",1.7042999999999999,null,"",null,null,null,null,null,null,null,"","",""]
["","","R-2707B","C203547","C203201-ECC","1","CLEVELAND","ES WAGNER CO LLC ",2083821.2,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203201-RWC","1","CLEVELAND","ES WAGNER CO LLC ",10962636.369999999,"RW1","I000",3.2,4,"G401",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203201-SIC","1","CLEVELAND","ES WAGNER CO LLC ",33545.18,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203201-STC","1","CLEVELAND","ES WAGNER CO LLC ",733535.77,"CV01","X028",5.0000000000000001E-3,27.63,"C002",347,10,"","",null,null,null,"MTN","12","222+20.43 -L-"]
["","","","","","2","CLEVELAND","ES WAGNER CO LLC ",556000,"WL1","Y007",null,null,"W000",9.09,null,"","",null,null,null,"MTN","12","252+73.29 -L- EB1"]
["","","","","","3","CLEVELAND","ES WAGNER CO LLC ",394000,"WL2","Y007",null,null,"W000",25.61,null,"","",null,null,null,"MTN","12","252+73.29 -L- EB2"]
["","","","","","7","CLEVELAND","ES WAGNER CO LLC ",803647.78,"BR01","X281",2.8299999999999999E-2,null,"11",null,49.25,"854","I",2,46,149.25,"MTN","12","247+90.66 -L- LT"]
["","","","","","8","CLEVELAND","ES WAGNER CO LLC ",858677.73,"BR02","X281",null,null,"11",null,49.25,"854","I",2,46,163,"MTN","12","247+90.66 -L- RT"]
["","","","","","9","CLEVELAND","ES WAGNER CO LLC ",1019561.17,"BR03","X171",3.1300000000000001E-2,null,"12",null,44.916699999999999,"579","A",1,41.666699999999999,165,"MTN","12","252+73.29 -L-LT"]
["","","","","","10","CLEVELAND","ES WAGNER CO LLC ",1295940.33,"BR04","X171",null,null,"12",null,49.25,"579","A",1,46,185,"MTN","12","252+73.29 -L- RT"]
["","","","","","11","CLEVELAND","ES WAGNER CO LLC ",2035993.39,"BR05","X081",8.1100000000000005E-2,null,"15",null,41.25,"854","Q",5,38,428.29,"MTN","12","340+70.00 -L- LT"]
["","","","","","12","CLEVELAND","ES WAGNER CO LLC ",2068853.54,"BR06","X081",null,null,"15",null,41.25,"854","Q",5,38,431.76,"MTN","12","340+70.00 -L- RT"]
["","","","","","13","CLEVELAND","ES WAGNER CO LLC ",1146163.6499999999,"BR07","X281",null,null,"11",null,59.25,"872","I",2,56,230.25,"MTN","12","354+83.22 -L-"]
["","","","","C203201-TCC","1","CLEVELAND","ES WAGNER CO LLC ",65762.559999999998,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203201-UTC","1","CLEVELAND","ES WAGNER CO LLC ",916843.12,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","2","CLEVELAND","ES WAGNER CO LLC ",46639.69,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","3","CLEVELAND","ES WAGNER CO LLC ",7452.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",25029073.98,"","",3.3456999999999999,null,null,null,null,null,null,null,null,null,"","",""]
["","14","","C203544","C203544-RW","1","MONTGOMERY","SMITH-ROWE LLC",8819994.4900000002,"RW1","",0.93,2,"M713",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",8819994.4900000002,"","",0.93,null,"",null,null,"","",null,null,null,"","",""]
["","15","","C203546","C203546-RW","1","ASHE","JAMES R VANNOY & SONS CONST CO",4553549.72,"RW1","",0.372,2,"M713",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","","","","Result",4553549.72,"","",0.372,null,"",null,null,"","",null,null,null,"","",""]
["","16","","C203528","C203528-RW","1","ALEXANDER","RE BURNS & SONS CO INC",4364855,"RW1","",0.39,2,"M713",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",4364855,"","",0.39,null,"",null,null,"","",null,null,null,"","",""]
["6/17/2014","1","U-2525B","C203399","C203399-EC","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",8938877.5,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203399-LI","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",352310,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203399-RW","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",61956798.100000001,"RW1","",4.4740000000000002,4,"N210",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203399-SG","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1483472.5,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203399-SI","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",2680390.16,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203399-ST","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",548038.6,"CV01","Y007",null,30,"C002",249.5,9,"","",null,null,null,"PDMT","7","48+65.00 -L-"]
["","","","","","2","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",196302.5,"CV02","Y007",null,7.6,"C002",184,7,"","",null,null,null,"PDMT","7","114+55.00 -L-"]
["","","","","","3","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",174045.4,"CV03","Y007",null,8.6,"C002",156.66999999999999,7,"","",null,null,null,"PDMT","7","218+00.00 -L-"]
["","","","","","4","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",452585.68,"CV04","Y007",null,24.2,"C002",273.42,8,"","",null,null,null,"PDMT","7","241+96.00 -L-"]
["","","","","","5","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",160000,"WL1","Y007",null,null,"W000",13.97,null,"","",null,null,null,"PDMT","7","10+73.00 -Y9-"]
["","","","","","6","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",187200,"WL2","Y007",null,null,"W000",15,null,"","",null,null,null,"PDMT","7","10+49.00 -Y9-"]
["","","","","","7","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1851591.73,"BR01","X581",7.8700000000000006E-2,null,"14",null,45.5,"754","Q",5,42.25,415.58330000000001,"PDMT","7","14+99.25 -L-"]
["","","","","","8","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",815700.1,"BR01","X231",3.0499999999999999E-2,null,"11",null,45.25,"542","Q",3,42,160.87,"PDMT","7","26+21.64 -L- LT"]
["","","","","","9","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",493044.8,"BR03","X231",3.1600000000000003E-2,null,"11",null,51.166699999999999,"542","Q",3,48,166.76560000000001,"PDMT","7","26+21.65 -L- RT"]
["","","","","","10","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",631607.67000000004,"BR04","X481",3.5799999999999998E-2,null,"16",null,45.666699999999999,"854","Q",2,42.416699999999999,189.25,"PDMT","7","129+37.56 -L- LT"]
["","","","","","11","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",667868.71,"BR05","X481",3.5799999999999998E-2,null,"16",null,45.666699999999999,"854","Q",2,42.416699999999999,189.25,"PDMT","7","129+37.56 -L- RT"]
["","","","","","12","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",7489202.3899999997,"BR06","X431",0.26889999999999997,null,"16",null,45.25,"690","Q",7,42,1420,"PDMT","7","144+90.00 -L-"]
["","","","","","13","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",8539834.4499999993,"BR07","X431",0.26889999999999997,null,"16",null,45.25,"690","Q",8,42,1601.25,"PDMT","7","144+60.63 -L-"]
["","","","","","14","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",392222.71999999997,"BR08","X281",2.0799999999999999E-2,null,"11",null,45.25,"872","A",1,42,110,"PDMT","7","174+72.46 -L- LT"]
["","","","","","15","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",403319.86,"BR08","X281",2.0799999999999999E-2,null,"11",null,45.25,"872","A",1,42,110,"PDMT","7","174+72.46 -L- RT"]
["","","","","","16","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1920403.35,"BR10","X231",5.1200000000000002E-2,null,"11",null,57.25,"654","D",2,54,270.25,"PDMT","7","268+22.89 -L-"]
["","","","","","17","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",678927.07,"BR11","X781",3.4599999999999999E-2,null,"11",null,51.25,"854","D",2,48,182.5,"PDMT","7","80+74.41 -L-"]
["","","","","","18","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",762201.47,"BR12","X781",3.6200000000000003E-2,null,"11",null,53.583300000000001,"854","I",2,40,191,"PDMT","7","228+23.81 -L-"]
["","","","","","19","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1542849.2,"BR13","X981",5.1799999999999999E-2,null,"11",null,48.083300000000001,"873","D",2,40,273.5,"PDMT","7","26+17.64 -Y22- LT"]
["","","","","","20","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1005568.95,"BR14","X981",5.1799999999999999E-2,null,"11",null,36.083300000000001,"873","D",2,28,273.5,"PDMT","7","26+17.64 -Y22- RT"]
["","","","","C203399-TC","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1014794.52,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203399-UT","1","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",1540806,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","2","GUILFORD","FLATIRON CONSTR INC- BLYTHE DEV",4803457.7,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",111683421.13,"","",5.4913999999999996,null,"",null,null,null,null,null,null,null,"","",""]
["","2","R-3620","C203413","C203413-EC","1","WASHINGTON","BARNHILL CONT CO",1284015.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203413-RW","1","WASHINGTON","BARNHILL CONT CO",6626645.2300000004,"RW1","I000",3.3330000000000002,4,"N200",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203413-SG","1","WASHINGTON","BARNHILL CONT CO",268693.40000000002,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203413-SI","1","WASHINGTON","BARNHILL CONT CO",131380.94,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203413-ST","1","WASHINGTON","BARNHILL CONT CO",173745,"CV01","X728",null,5.5,"C001",72.5,12,"","",null,null,null,"COAST","1","148+73.00 -L-"]
["","","","","C203413-TC","1","WASHINGTON","BARNHILL CONT CO",90364.25,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","C203413-UT","1","WASHINGTON","BARNHILL CONT CO",40062.78,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","1",""]
["","","","","","","","Result",8614907.0999999996,"","",3.3330000000000002,null,null,null,null,"","",null,null,null,"","",""]
["","3","U-3331","C203458","C203458-RW","1","NASH","BARNHILL CONT CO",4166849.7,"RW1","I000",1.0609999999999999,2,"D343",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","","2","NASH","BARNHILL CONT CO",512886.98,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","C203458-SG","1","NASH","BARNHILL CONT CO",258013,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","C203458-SI","1","NASH","BARNHILL CONT CO",51864.09,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","C203458-ST","1","NASH","BARNHILL CONT CO",2915743.61,"BR01","X080",4.8000000000000001E-2,null,"15",null,78,"721","Q",5,64.25,253.17699999999999,"PDMT","4","32+18.50 -L-"]
["","","","","C203458-TC","1","NASH","BARNHILL CONT CO",209551.05,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
["","","","","","","","Result",8114908.4299999997,"","",1.109,null,"",null,null,null,null,null,null,null,"","",""]
["","4","U-4432","C203360","C203360-EC","1","WAKE","S T WOOTEN CORP",287326.59999999998,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203360-RW","1","WAKE","S T WOOTEN CORP",4410462.97,"RW1","I000",0.90700000000000003,4,"N220",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203360-SG","1","WAKE","S T WOOTEN CORP",268933.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203360-SI","1","WAKE","S T WOOTEN CORP",72405.289999999994,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203360-ST","1","WAKE","S T WOOTEN CORP",2174399.9700000002,"BR01","X181",3.4299999999999997E-2,null,"12",null,87.083299999999994,"854","E",3,73.5,181.3125,"PDMT","5","28+17.07 -L-"]
["","","","","C203360-TC","1","WAKE","S T WOOTEN CORP",239943.55,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203360-UT","2","WAKE","S T WOOTEN CORP",386406.35,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",7839878.2300000004,"","",0.94130000000000003,null,null,null,null,null,null,null,null,null,"","",""]
["","5","X-0002CC","C203361","C203361-EC","1","CUMBERLAND","BARNHILL CONT CO",439912.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203361-LI","1","CUMBERLAND","BARNHILL CONT CO",1822010.25,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203361-RW","1","CUMBERLAND","BARNHILL CONT CO",27605761.579999998,"RW1","I000",6.8259999999999996,4,"P501",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203361-SG","1","CUMBERLAND","BARNHILL CONT CO",209450,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203361-SI","1","CUMBERLAND","BARNHILL CONT CO",1871025.97,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203361-TC","1","CUMBERLAND","BARNHILL CONT CO",35557,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",31983717.300000001,"","",6.8259999999999996,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C203569","C203569A-RW","1","CUMBERLAND","BARNHILL CONT CO",2907375.01,"RW1","",8.49,6,"R000",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203569B-RW","1","HARNETT","BARNHILL CONT CO",316845.05,"RW1","",1.1299999999999999,5,"R000",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203569C-RW","1","CUMBERLAND","BARNHILL CONT CO",3021915.5,"RW1","",25.87,2,"R000",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203569D-RW","1","HARNETT","BARNHILL CONT CO",1929132.21,"RW1","",16.27,2,"R000",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","","","","Result",8175267.7699999996,"","",51.76,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203548","C203548A-RW","1","ROBESON","BARNHILL CONT CO",2215898.52,"RW1","",18.8,2,"R000",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203548B-RW","1","ROBESON","BARNHILL CONT CO",2487327.75,"RW1","",25.79,2,"R000",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",4703226.2699999996,"","",44.59,null,"",null,null,"","",null,null,null,"","",""]
["","8","R-2612B","C203412","C203412-EC","1","GUILFORD","BRANCH HIGHWAYS INC",942119,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203412-LI","1","GUILFORD","BRANCH HIGHWAYS INC",10000,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203412-RW","1","GUILFORD","BRANCH HIGHWAYS INC",9400628.4499999993,"RW1","I000",0.71299999999999997,4,"I604",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203412-SI","1","GUILFORD","BRANCH HIGHWAYS INC",235083.1,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203412-ST","1","GUILFORD","BRANCH HIGHWAYS INC",507068,"CV01","X028",5.1000000000000004E-3,42.2,"C002",223,12,"","",null,null,null,"PDMT","7","43+86.48 -Y-"]
["","","","","","2","GUILFORD","BRANCH HIGHWAYS INC",575304,"CV02","Y007",5.1000000000000004E-3,22.56,"C002",335.5,12,"","",null,null,null,"PDMT","7","14+77.40 -YLPD-"]
["","","","","","3","GUILFORD","BRANCH HIGHWAYS INC",1483354.56,"BR01","X281",5.9799999999999999E-2,null,"11",null,56.083300000000001,"875","D",3,53.5,315.5,"PDMT","7","60+37.13 -L-"]
["","","","","C203412-TC","1","GUILFORD","BRANCH HIGHWAYS INC",354502.74,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203412-UT","2","GUILFORD","BRANCH HIGHWAYS INC",20438,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",13528497.85,"","",0.78300000000000003,null,"",null,null,null,null,null,null,null,"","",""]
["","9","B-4608","C203410","C203410-EC","1","RANDOLPH","RE BURNS & SONS CO INC",45420,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203410-RW","1","RANDOLPH","RE BURNS & SONS CO INC",356049.5,"RW1","I000",0.191,2,"B812",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203410-SI","1","RANDOLPH","RE BURNS & SONS CO INC",3479,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203410-ST","1","RANDOLPH","RE BURNS & SONS CO INC",658553.69999999995,"BR01","X081",2.7E-2,null,"15",null,33,"733","Q",2,30.5,142.458,"PDMT","8","16+29.00 -L-"]
["","","","","C203410-TC","1","RANDOLPH","RE BURNS & SONS CO INC",3032.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",1066534.95,"","",0.218,null,null,null,null,null,null,null,null,null,"","",""]
["","10","","C203570","C203570A-RW","1","CHATHAM","S T WOOTEN CORP",2324689.44,"RW1","",4.7960000000000003,4,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203570B-RW","1","CHATHAM","S T WOOTEN CORP",1416217.82,"RW1","",10.641999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",3740907.26,"","",15.438000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C203572","C203572A-RW","1","LEE","RILEY PAVING INC",1434370.15,"RW1","",5.0369999999999999,4,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203572B-RW","1","LEE","RILEY PAVING INC",765574.95,"RW1","",8.2590000000000003,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",2199945.1,"","",13.295999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","12","","C203571","C203571A-RW","1","SCOTLAND","BARNHILL CONT CO",1720131.94,"RW1","",14.4,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203571B-RW","1","HOKE","BARNHILL CONT CO",504330.5,"RW1","",3.8570000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203571C-RW","1","SCOTLAND","BARNHILL CONT CO",325307.28999999998,"RW1","",3.26,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",2549769.73,"","",21.516999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","13","","C203560","C203560A-RW","1","DAVIDSON","BLYTHE CONST INC",1750772.29,"RW1","",10.957000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203560B-RW","1","ROWAN","BLYTHE CONST INC",58272.68,"RW1","",0.192,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203560C-RW","1","DAVIDSON","BLYTHE CONST INC",3056794.21,"RW1","",27.8,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",4865839.18,"","",38.948999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","14","","C203568","C203568A-RW","1","FORSYTH","APAC - ATLANTIC INC THOMPSON ARTHUR DI",2495891.11,"RW1","",13.018000000000001,6,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203568B-RW","1","FORSYTH","APAC - ATLANTIC INC THOMPSON ARTHUR DI",1680737.83,"RW1","",9.51,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",4176628.94,"","",22.527999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","17","B-4983","C203411","C203411-EC","1","BURKE","NHM CONSTR LLC",52605,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203411-RW","1","BURKE","NHM CONSTR LLC",530428.85,"RW1","I000",0.11899999999999999,2,"B812",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203411-SG","1","BURKE","NHM CONSTR LLC",109930,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203411-SI","1","BURKE","NHM CONSTR LLC",4441.6499999999996,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203411-ST","1","BURKE","NHM CONSTR LLC",812690.8,"BR01","X271",2.5999999999999999E-2,null,"12",null,40.083300000000001,"845","E",3,32,135.83330000000001,"MTN","13","13+52.95 -L-"]
["","","","","C203411-TC","1","BURKE","NHM CONSTR LLC",14339.65,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",1524435.95,"","",0.14499999999999999,null,"",null,null,null,null,null,null,null,"","",""]
["","18","R-4047","C203393","C203393-EC","1","HAYWOOD","NHM CONSTR LLC",778194.35,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203393-LI","1","HAYWOOD","NHM CONSTR LLC",154335.6,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203393-RW","1","HAYWOOD","NHM CONSTR LLC",10003894.039999999,"RW1","I000",0.77700000000000002,4,"M720",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203393-SG","1","HAYWOOD","NHM CONSTR LLC",753634.2,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203393-SI","1","HAYWOOD","NHM CONSTR LLC",426306.3,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203393-ST","1","HAYWOOD","NHM CONSTR LLC",159109.5,"CV01","Y007",null,11.86,"C001",111.58,12,"","",null,null,null,"V MTN","14","11+41.87 -Y4-"]
["","","","","","2","HAYWOOD","NHM CONSTR LLC",666080,"WL1","Y007",null,null,"W000",13.18,null,"","",null,null,null,"V MTN","14","12+00.00 -Y4-"]
["","","","","","3","HAYWOOD","NHM CONSTR LLC",3907819.8,"BR01","X631",null,null,"26",null,22,"578","Q",4,20,279.25,"V MTN","14","42+60.93 -L-"]
["","","","","C203393-TC","1","HAYWOOD","NHM CONSTR LLC",325343.8,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203393-UT","1","HAYWOOD","NHM CONSTR LLC",1657691.76,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","2","HAYWOOD","NHM CONSTR LLC",34193.83,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",18866603.18,"","",0.77700000000000002,null,null,null,null,null,null,null,null,null,"","",""]
["","19","","C203559","C203559-RW","1","WILKES","JAMES R VANNOY & SONS CONST CO",9671481.6199999992,"RW1","",0.75900000000000001,2,"M720",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",9671481.6199999992,"","",0.75900000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","20","","C203545","C203545-RW","1","HAYWOOD","NHM CONSTR LLC",5347000,"RW1","",0.66700000000000004,2,"M720",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",5347000,"","",0.66700000000000004,null,"",null,null,"","",null,null,null,"","",""]
["7/15/2014","1","B-4251","C203407","C203407-EC","1","ROBESON","SMITH-ROWE LLC",19283.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203407-RW","1","ROBESON","SMITH-ROWE LLC",254642.88,"RW1","I000",0.112,2,"B810",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203407-SI","1","ROBESON","SMITH-ROWE LLC",4492,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203407-ST","1","ROBESON","SMITH-ROWE LLC",421239.26,"BR01","X081",2.1299999999999999E-2,null,"15",null,33,"721","A",3,30.833300000000001,112.5,"COAST","6","15+08.00 -L-"]
["","","","","C203407-TC","1","ROBESON","SMITH-ROWE LLC",4436,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203407-UT","1","ROBESON","SMITH-ROWE LLC",54876.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",758969.89,"","",0.1333,null,"",null,null,null,null,null,null,null,"","",""]
["","2","B-4639","C203408","C203408-EC","1","SCOTLAND","SANFORD CONTR INC",91757.28,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203408-RW","1","SCOTLAND","SANFORD CONTR INC",761997.38,"RW1","I000",0.17299999999999999,2,"B812",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203408-SI","1","SCOTLAND","SANFORD CONTR INC",10601,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203408-ST","1","SCOTLAND","SANFORD CONTR INC",919121.54,"BR01","X081",3.4299999999999997E-2,null,"15",null,35.25,"836","A",3,32,181.083,"PDMT","8","20+03.00 -L-"]
["","","","","C203408-TC","1","SCOTLAND","SANFORD CONTR INC",23272.799999999999,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",1806750,"","",0.20730000000000001,null,"",null,null,null,null,null,null,null,"","",""]
["","3","","C203577","C203577A-RW","1","MONTGOMERY","RILEY PAVING INC",448921.62,"RW1","",2.11,3,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203577B-RW","1","MOORE","RILEY PAVING INC",918457.8,"RW1","",4.83,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203577C-RW","1","MONTGOMERY","RILEY PAVING INC",332094.46000000002,"RW1","",3.51,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203577D-RW","1","MOORE","RILEY PAVING INC",1325466.7,"RW1","",12.246,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",3024940.58,"","",22.696000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C203578","C203578A-RW","1","RICHMOND","HUDSON PAVING INC",1119899.17,"RW1","",8.9499999999999993,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203578B-RW","1","RICHMOND","HUDSON PAVING INC",526189.49,"RW1","",6.18,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",1646088.66,"","",15.13,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C203574","C203574A-RW","1","ROWAN","J T RUSSELL & SONS INC",1444705.75,"RW1","",2.1520000000000001,4,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203574B-RW","1","ROWAN","J T RUSSELL & SONS INC",2000665.49,"RW1","",17.167999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",3445371.24,"","",19.32,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C203576","C203576A-RW","1","STOKES","APAC - ATLANTIC INC THOMPSON ARTHUR DI",802452.98,"RW1","",7.6779999999999999,3,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203576B-RW","1","STOKES","APAC - ATLANTIC INC THOMPSON ARTHUR DI",1457106.52,"RW1","",14.227,3,"R000",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",2259559.5,"","",21.905000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203579","C203579A-RW","1","LINCOLN","BLYTHE CONST INC",1079647.5,"RW1","",5.0599999999999996,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203579B-RW","1","LINCOLN","BLYTHE CONST INC",1896683.5,"RW1","",14.65,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",2976331,"","",19.71,null,"",null,null,"","",null,null,null,"","",""]
["","8","B-4554","C203409","C203409-EC","1","JACKSON","NHM CONSTR LLC",139150,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203409-RW","1","JACKSON","NHM CONSTR LLC",1610689.7,"RW1","I000",0.36199999999999999,4,"B813",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203409-SI","1","JACKSON","NHM CONSTR LLC",16764.95,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203409-ST","1","JACKSON","NHM CONSTR LLC",4444965.08,"BR01","X071",5.8999999999999997E-2,null,"17",null,86.583299999999994,"560","Q",3,84,313,"V MTN","14","27+11.72 -L-"]
["","","","","C203409-TC","1","JACKSON","NHM CONSTR LLC",241137.4,"RW1","I000",null,4,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",6452707.1299999999,"","",0.42099999999999999,null,"",null,null,null,null,null,null,null,"","",""]
["","9","R-5525","C203598","C203437-RW","1","WATAUGA","JW HAMPTON CO",3189302,"RW1","I000",0.46600000000000003,2,"N240",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","","2","WATAUGA","JW HAMPTON CO",275479,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","C203437-ST","1","WATAUGA","JW HAMPTON CO",756547.35,"BR01","X080",1.9400000000000001E-2,null,"15",null,64.333299999999994,"721","A",2,60.333300000000001,102.375,"V MTN","11","11+00.19 -L-"]
["","","","","","","","Result",4221328.3499999996,"","",0.4854,null,"",null,null,null,null,null,null,null,"","",""]
["","10","","C203573","C203573-RW","1","MITCHELL","DANE CONST INC",11373160,"RW1","",0.86099999999999999,2,"M713",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",11373160,"","",0.86099999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C203529","C203529-RW","1","JACKSON","SIMPSON CONST CO INC",5472099,"RW1","",0.38500000000000001,2,"M713",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",5472099,"","",0.38500000000000001,null,"",null,null,"","",null,null,null,"","",""]
["8/19/2014","1","U-2519CB","C203398","C203398-EC","1","CUMBERLAND","CONTI ENTPR INC",6050692.5,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203398-LI","1","CUMBERLAND","CONTI ENTPR INC",767431.75,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203398-RW","1","CUMBERLAND","CONTI ENTPR INC",52450742.640000001,"RW1","",5.5919999999999996,4,"N210",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203398-SG","1","CUMBERLAND","CONTI ENTPR INC",694206.5,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203398-SI","1","CUMBERLAND","CONTI ENTPR INC",1064753.55,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203398-ST","1","CUMBERLAND","CONTI ENTPR INC",513500,"WL1","Y007",null,null,"W000",9.93,null,"","",null,null,null,"COAST","6","10+23.00 -RPC2-"]
["","","","","","2","CUMBERLAND","CONTI ENTPR INC",955500,"WL2","Y007",null,null,"W000",14.52,null,"","",null,null,null,"COAST","6","22+50.00 -TT5-"]
["","","","","","3","CUMBERLAND","CONTI ENTPR INC",425750,"WL3","Y007",null,null,"W000",12.78,null,"","",null,null,null,"COAST","6","969+51.52 -L- EB1"]
["","","","","","4","CUMBERLAND","CONTI ENTPR INC",455000,"WL4","Y007",null,null,"W000",13.91,null,"","",null,null,null,"COAST","6","969+51.52 -L- EB2"]
["","","","","","5","CUMBERLAND","CONTI ENTPR INC",146250,"WL5","Y007",null,null,"W000",12,null,"","",null,null,null,"COAST","6","57+20 -Y1- LT"]
["","","","","","6","CUMBERLAND","CONTI ENTPR INC",165750,"WL6","Y007",null,null,"W000",13.46,null,"","",null,null,null,"COAST","6","57+20 -Y1- RT"]
["","","","","","7","CUMBERLAND","CONTI ENTPR INC",32417.75,"WL7","Y007",null,null,"W000",22.75,null,"","",null,null,null,"COAST","6","21+10.00 -TT5-"]
["","","","","","8","CUMBERLAND","CONTI ENTPR INC",694277.5,"WL8","Y007",null,null,"W000",18.89,null,"","",null,null,null,"COAST","6","6+66.02 -RPA2-"]
["","","","","","9","CUMBERLAND","CONTI ENTPR INC",385307,"WL9","Y007",null,null,"W000",19.489999999999998,null,"","",null,null,null,"COAST","6","971+71.64 -L-"]
["","","","","","10","CUMBERLAND","CONTI ENTPR INC",268750.5,"WL10","Y007",null,null,"W000",27.22,null,"","",null,null,null,"COAST","6","969+32.37 -L-"]
["","","","","","11","CUMBERLAND","CONTI ENTPR INC",30029,"WL11","Y007",null,null,"W000",25.02,null,"","",null,null,null,"COAST","6","23+00.00 -Y2"]
["","","","","","12","CUMBERLAND","CONTI ENTPR INC",986250,"WL12","Y007",null,null,"W000",15.03,null,"","",null,null,null,"COAST","6","794+89.54 -L-"]
["","","","","","13","CUMBERLAND","CONTI ENTPR INC",861000,"WL13","Y007",null,null,"W000",21.06,null,"","",null,null,null,"COAST","6","969+50.59 -L-"]
["","","","","","14","CUMBERLAND","CONTI ENTPR INC",738375,"WL14","Y007",null,null,"W000",20.51,null,"","",null,null,null,"COAST","6","32+80.83 -L-"]
["","","","","","15","CUMBERLAND","CONTI ENTPR INC",357000,"WL15","Y007",null,null,"W000",23.8,null,"","",null,null,null,"COAST","6","46+61.41 -L-"]
["","","","","","16","CUMBERLAND","CONTI ENTPR INC",994875,"WL16","Y007",null,null,"W000",20.25,null,"","",null,null,null,"COAST","6","52+17.03 -L-"]
["","","","","","17","CUMBERLAND","CONTI ENTPR INC",512250,"WL17","Y007",null,null,"W000",22.77,null,"","",null,null,null,"COAST","6","71+03.27 -L-"]
["","","","","","18","CUMBERLAND","CONTI ENTPR INC",805910,"BR01","X281",3.3300000000000003E-2,null,"11",null,51.25,"854","I",2,48,175.8802,"COAST","6","765+27.44 -L-LT"]
["","","","","","19","CUMBERLAND","CONTI ENTPR INC",786359,"BR02","X281",null,null,"11",null,51.25,"854","I",2,48,170.9271,"COAST","6","765+27.44 -L-RT"]
["","","","","","20","CUMBERLAND","CONTI ENTPR INC",4552958,"BR03","X081",null,null,"15",null,45.25,"864","E",10,42,995.79169999999999,"COAST","6","826+15.00 -L- LT"]
["","","","","","21","CUMBERLAND","CONTI ENTPR INC",3899598.7,"BR04","X081",0.1905,null,"15",null,45.25,"864","E",10,42,1005.7083,"COAST","6","826+15.00 -L- RT"]
["","","","","","22","CUMBERLAND","CONTI ENTPR INC",4162747.5,"BR05","X081",null,null,"15",null,45.25,"864","E",8,42,840.10940000000005,"COAST","6","898+20.00 -L- LT"]
["","","","","","23","CUMBERLAND","CONTI ENTPR INC",3367383.75,"BR06","X081",0.16,null,"15",null,45.25,"864","E",8,42,844.9375,"COAST","6","898+20.00 -L- RT"]
["","","","","","24","CUMBERLAND","CONTI ENTPR INC",1491290.59,"BR07","X271",3.9199999999999999E-2,null,"11",null,45.25,"570","A",1,42,207,"COAST","6","969+51.52 -L-LT"]
["","","","","","25","CUMBERLAND","CONTI ENTPR INC",2058789.49,"BR08","X271",null,null,"11",null,63.25,"570","A",1,60,207,"COAST","6","969+51.52 -L-RT"]
["","","","","","26","CUMBERLAND","CONTI ENTPR INC",4072581.68,"BR09","X031",0.13009999999999999,null,"16",null,44.583300000000001,"662","D",5,41.333300000000001,686.6875,"COAST","6","94+24.58 -L- LT"]
["","","","","","27","CUMBERLAND","CONTI ENTPR INC",3557221.84,"BR09","X031",0.13469999999999999,null,"16",null,44.583300000000001,"662","D",5,41.333300000000001,711.27599999999995,"COAST","6","94+24.58 -L- RT"]
["","","","","","28","CUMBERLAND","CONTI ENTPR INC",2807200.47,"BR11","X271",null,null,"11",null,106.58329999999999,"656","I",2,93,236.25,"COAST","6","943+21.58 -L- RT"]
["","","","","","29","CUMBERLAND","CONTI ENTPR INC",3257450.75,"BR12","X271",null,null,"11",null,89.583299999999994,"648","I",2,76,277.75,"COAST","6","991+28.13 -L-"]
["","","","","","30","CUMBERLAND","CONTI ENTPR INC",10724523.300000001,"BR13","X731",0.30299999999999999,null,"71",null,40.666699999999999,"690","D",10,37.416699999999999,1600,"COAST","6","57+07.00 -RP1DB-"]
["","","","","","31","CUMBERLAND","CONTI ENTPR INC",3846269.48,"BR14","X731",0.1424,null,"71",null,50.5,"662","D",6,47.25,751.6875,"COAST","6","94+43.84 -COL1-"]
["","","","","","32","CUMBERLAND","CONTI ENTPR INC",563202,"BR15","X281",null,null,"11",null,32.770800000000001,"845","I",3,29.520800000000001,142.95830000000001,"COAST","6","42+10.23 -RP1B-"]
["","","","","","33","CUMBERLAND","CONTI ENTPR INC",4049731.86,"BR16","X071",null,null,"15",null,32.770800000000001,"658","N",6,29.520800000000001,787.40629999999999,"COAST","6","45+07.87 -RP1C-"]
["","","","","","34","CUMBERLAND","CONTI ENTPR INC",690248.9,"BR17","X780",null,null,"11",null,51,"733","A",1,43.041699999999999,101.25,"COAST","6","21+10.60 -PXROAD-"]
["","","","","C203398-TC","1","CUMBERLAND","CONTI ENTPR INC",826998,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203398-UT","2","CUMBERLAND","CONTI ENTPR INC",406947,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",125477521,"","",6.7252000000000001,null,"",null,null,null,null,null,null,null,"","",""]
["","2","B-5117","C203459","C203459-EC","1","BLADEN","S & C CONST LLC",78989.350000000006,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203459-RW","1","BLADEN","S & C CONST LLC",1090931.75,"RW1","I000",0.36799999999999999,2,"B801",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203459-SI","1","BLADEN","S & C CONST LLC",11512.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203459-ST","1","BLADEN","S & C CONST LLC",456738.87,"BR01","X080",0.02,null,"15",null,36,"721","A",3,33.833300000000001,107.58329999999999,"COAST","6","26+16.00 -L-"]
["","","","","C203459-TC","1","BLADEN","S & C CONST LLC",99099.1,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",1737271.67,"","",0.38800000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","3","","C203596","C203596A-RW","1","ALEXANDER","MAYMEAD INC",527968.6,"RW1","",3.22,2,"R000",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203596B-RW","1","ALEXANDER","MAYMEAD INC",882282.8,"RW1","",6.09,2,"R000",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",1410251.4,"","",9.31,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C203597","C203597A-RW","1","CATAWBA","MAYMEAD INC",1662671.33,"RW1","",4.7,5,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203597B-RW","1","CATAWBA","MAYMEAD INC",3620715.38,"RW1","",25.14,5,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",5283386.71,"","",29.84,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C203586","C203586A-RW","1","IREDELL","MAYMEAD INC",2789773,"RW1","",18.72,6,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203586B-RW","1","IREDELL","MAYMEAD INC",3291949.69,"RW1","",27.366,6,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",6081722.6900000004,"","",46.085999999999999,null,"",null,null,"","",null,null,null,"","",""]
["8/26/2014","1","","C203602","C203602A-RW","1","FRANKLIN","CAROLINA SUNROCK LLC",1206909.7,"RW1","I000",10.5,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203602B-RW","1","WAKE","CAROLINA SUNROCK LLC",1055362.0900000001,"RW1","I000",4.66,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",2262271.79,"","",15.16,null,"",null,null,"","",null,null,null,"","",""]
["","2","","C203603","C203603A-RW","1","PERSON","ADAMS CONST CO",3766815.11,"RW1","",18.48,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203603B-RW","1","PERSON","ADAMS CONST CO",1474517.94,"RW1","",11.55,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",5241333.05,"","",30.03,null,"",null,null,"","",null,null,null,"","",""]
["","3","","C203608","C203608A-RW","1","RANDOLPH","APAC - ATLANTIC INC THOMPSON ARTHUR DI",1939380.45,"RW1","",3.3370000000000002,5,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203608B-RW","1","RANDOLPH","APAC - ATLANTIC INC THOMPSON ARTHUR DI",2778060.7999999998,"RW1","",24.143999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",4717441.25,"","",27.481000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C203605","C203605A-RW","1","BURKE","MAYMEAD INC",1130496.49,"RW1","",4.4000000000000004,5,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203605B-RW","1","BURKE","MAYMEAD INC",1242867.74,"RW1","",9.9600000000000009,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",2373364.23,"","",14.36,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C203607","C203607A-RW","1","MCDOWELL","MAYMEAD INC",664083.73,"RW1","",3.97,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203607B-RW","1","MCDOWELL","MAYMEAD INC",1355606.26,"RW1","",7.76,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",2019689.99,"","",11.73,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C203606","C203606A-RW","1","MITCHELL","MAYMEAD INC",1171125.25,"RW1","",2.81,5,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203606B-RW","1","MITCHELL","MAYMEAD INC",455165.7,"RW1","",3.32,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1626290.95,"","",6.13,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203604","C203604A-RW","1","RUTHERFORD","HARRISON CONST CO DIV O",1101260.8899999999,"RW1","",8.64,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203604B-RW","1","RUTHERFORD","HARRISON CONST CO DIV O",1595847.27,"RW1","",10.95,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",2697108.16,"","",19.59,null,"",null,null,"","",null,null,null,"","",""]
["9/16/2014","1","P-5204","C203489","C203489-EC","1","GUILFORD","TRIANGLE GRADING & PAVING INC",650119.94999999995,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203489-RW","1","GUILFORD","TRIANGLE GRADING & PAVING INC",4479359.7,"RW1","I000",0.47399999999999998,2,"M720",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203489-SI","1","GUILFORD","TRIANGLE GRADING & PAVING INC",23913.05,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203489-ST","1","GUILFORD","TRIANGLE GRADING & PAVING INC",1283827.77,"BR01","X131",2.8000000000000001E-2,null,"17",null,37.666699999999999,"660","A",1,35.5,149.6875,"PDMT","7","24+59.04 -L-"]
["","","","","C203489-TC","1","GUILFORD","TRIANGLE GRADING & PAVING INC",180101.38,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203489-UT","2","GUILFORD","TRIANGLE GRADING & PAVING INC",461614.3,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",7078936.1500000004,"","",0.502,null,"",null,null,null,null,null,null,null,"","",""]
["","2","I-5608","C203488","C203488-RW","1","BUNCOMBE","ROGERS GROUP INC",4980161.5999999996,"RW1","I000",5.3,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",4980161.5999999996,"","",5.3,null,"",null,null,"","",null,null,null,"","",""]
["10/21/2014","2","U-2579B","C203484","C203484-EC","1","FORSYTH","DRAGADOS USA INC",10647312.67,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203484-RW","1","FORSYTH","DRAGADOS USA INC",97702209.890000001,"RW1","I000",3.843,6,"N211",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203484-SG","1","FORSYTH","DRAGADOS USA INC",1630402.45,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203484-SI","1","FORSYTH","DRAGADOS USA INC",1611286.45,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203484-ST","1","FORSYTH","DRAGADOS USA INC",831040.87,"CV01","X028",4.0000000000000001E-3,54.75,"C002",368.58,10,"","",null,null,null,"PDMT","9","559+74.00 -L-"]
["","","","","","2","FORSYTH","DRAGADOS USA INC",1882015.75,"CV02","X028",7.1000000000000004E-3,40.299999999999997,"C003",598.5,10,"","",null,null,null,"PDMT","9","616+45.00 -L-"]
["","","","","","3","FORSYTH","DRAGADOS USA INC",1105495.92,"CV03","X028",7.1000000000000004E-3,25.12,"C003",330.25,12,"","",null,null,null,"PDMT","9","667+15.00 -L-"]
["","","","","","4","FORSYTH","DRAGADOS USA INC",397131.65,"CV04","X928",null,31.61,"C002",336.75,7,"","",null,null,null,"PDMT","9","23+11.00-Y1-"]
["","","","","","5","FORSYTH","DRAGADOS USA INC",102839.18,"CV05","X928",null,9.98,"C203",48.08,8,"","",null,null,null,"PDMT","9","45+65.43 -Y4-"]
["","","","","","6","FORSYTH","DRAGADOS USA INC",373452.64,"WL1","Y007",null,null,"W000",20.57,null,"","",null,null,null,"PDMT","9","22+74.08 -Y3-"]
["","","","","","7","FORSYTH","DRAGADOS USA INC",65501,"WL2","Y007",null,null,"W000",8.98,null,"","",null,null,null,"PDMT","9","46+65.34 -Y4WB-"]
["","","","","","8","FORSYTH","DRAGADOS USA INC",844173,"WL3","Y007",null,null,"W000",15.79,null,"","",null,null,null,"PDMT","9","50+50.00 -Y4WB-"]
["","","","","","9","FORSYTH","DRAGADOS USA INC",786192,"WL4","Y007",null,null,"W000",14.73,null,"","",null,null,null,"PDMT","9","557+97.95 -L- NWL1"]
["","","","","","10","FORSYTH","DRAGADOS USA INC",905498,"WL5","Y007",null,null,"W000",17.62,null,"","",null,null,null,"PDMT","9","585+81.40 -L- NWL2"]
["","","","","","11","FORSYTH","DRAGADOS USA INC",875864,"WL6","Y007",null,null,"W000",19.25,null,"","",null,null,null,"PDMT","9","11+18.96 -Y4CD- NWL3"]
["","","","","","12","FORSYTH","DRAGADOS USA INC",85998,"WL7","Y007",null,null,"W000",12.2,null,"","",null,null,null,"PDMT","9","19+26.04 -Y4RPA-"]
["","","","","","13","FORSYTH","DRAGADOS USA INC",831050,"WL8","Y007",null,null,"W000",16.28,null,"","",null,null,null,"PDMT","9","29+60.86 -Y4RPC-"]
["","","","","","14","FORSYTH","DRAGADOS USA INC",483802,"WL9","Y007",null,null,"W000",13.33,null,"","",null,null,null,"PDMT","9","130+26.37 -Y4EB-"]
["","","","","","15","FORSYTH","DRAGADOS USA INC",444268,"WL10","Y007",null,null,"W000",17.11,null,"","",null,null,null,"PDMT","9","26+02.53 -Y4RPD-"]
["","","","","","16","FORSYTH","DRAGADOS USA INC",664356,"WL11","Y007",null,null,"W000",21.57,null,"","",null,null,null,"PDMT","9","69+87.45 -Y4RPBD-"]
["","","","","","17","FORSYTH","DRAGADOS USA INC",554576,"WL12","Y007",null,null,"W000",19.39,null,"","",null,null,null,"PDMT","9","12+16.27 -Y4RPD-"]
["","","","","","18","FORSYTH","DRAGADOS USA INC",1934187.69,"BR01","X281",null,null,"11",null,107.25,"873","I",2,104,233.75,"PDMT","9","482+13.14 -L-"]
["","","","","","19","FORSYTH","DRAGADOS USA INC",721873.19,"BR02","X281",null,null,"11",null,37.75,"873","I",2,34.5,229,"PDMT","9","516+31.30 -L-"]
["","","","","","20","FORSYTH","DRAGADOS USA INC",1608861.15,"BR03","X081",4.2599999999999999E-2,null,"15",null,63.25,"854","Q",3,60,225,"PDMT","9","556+85.00 -L-LT"]
["","","","","","21","FORSYTH","DRAGADOS USA INC",1671751.13,"BR04","X081",null,null,"15",null,63.25,"854","Q",3,60,225,"PDMT","9","556+85.00 -L-RT"]
["","","","","","22","FORSYTH","DRAGADOS USA INC",1897986.23,"BR05","X581",null,null,"14",null,75.25,"873","I",3,72,280.47919999999999,"PDMT","9","584+36.24 -L-LT"]
["","","","","","23","FORSYTH","DRAGADOS USA INC",2057615.31,"BR06","X581",5.3999999999999999E-2,null,"14",null,75.25,"873","I",3,72,285.6823,"PDMT","9","584+36.24 -L-RT"]
["","","","","","24","FORSYTH","DRAGADOS USA INC",2709558.61,"BR07","X081",null,null,"15",null,41.25,"854","Q",5,38,384.40629999999999,"PDMT","9","17+10.00 -Y4RPA"]
["","","","","","25","FORSYTH","DRAGADOS USA INC",1268732.48,"BR08","X081",null,null,"15",null,33.25,"864","Q",3,30,309.54689999999999,"PDMT","9","33+15.67 -Y4CD-"]
["","","","","","26","FORSYTH","DRAGADOS USA INC",2476808.59,"BR09","X081",null,null,"15",null,63.25,"863","Q",3,60,308.75220000000002,"PDMT","9","628+65.50 -L- LT"]
["","","","","","27","FORSYTH","DRAGADOS USA INC",1965788.21,"BR10","X081",5.8500000000000003E-2,null,"15",null,63.25,"863","Q",3,60,308.75220000000002,"PDMT","9","628+65.50 -L- RT"]
["","","","","","28","FORSYTH","DRAGADOS USA INC",1383654.9,"BR11","X081",null,null,"15",null,41.25,"854","Q",3,38,264.16669999999999,"PDMT","9","26+60.00 -Y4RPBD-"]
["","","","","","29","FORSYTH","DRAGADOS USA INC",1037617.05,"BR12","X781",null,null,"68",null,53.833300000000001,"864","D",2,50.583300000000001,216.5,"PDMT","9","46+87.16 -Y4CD-"]
["","","","","","30","FORSYTH","DRAGADOS USA INC",1117768.3600000001,"BR13","X281",4.1000000000000002E-2,null,"11",null,63.833300000000001,"864","D",2,60.583300000000001,216.5,"PDMT","9","642+81.42 -L- LT"]
["","","","","","31","FORSYTH","DRAGADOS USA INC",1257969.97,"BR14","X281",null,null,"64",null,75.916700000000006,"864","D",2,72.666700000000006,216.5,"PDMT","9","642+81.42 -L- RT"]
["","","","","","32","FORSYTH","DRAGADOS USA INC",2102926.14,"BR15","X231",null,null,"64",null,43.25,"670","D",2,40,280,"PDMT","9","44+08.64 -Y4RPBD-"]
["","","","","","33","FORSYTH","DRAGADOS USA INC",1312105.56,"BR16","X781",null,null,"11",null,43.25,"772","I",3,40,306.25,"PDMT","9","52+94.28 -Y4RPBD-"]
["","","","","","34","FORSYTH","DRAGADOS USA INC",477986.2,"BR17","X982",null,null,"1",null,38.416699999999999,"772","A",1,35.833300000000001,119.25,"PDMT","9","23+59.12 -Y5-"]
["","","","","","35","FORSYTH","DRAGADOS USA INC",1412152.49,"BR18","X981",null,null,"1",null,38.083300000000001,"873","D",4,35.5,413.54169999999999,"PDMT","9","28+50.16 -Y5-"]
["","","","","C203484-TC","1","FORSYTH","DRAGADOS USA INC",1464527.19,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203484-UT","1","FORSYTH","DRAGADOS USA INC",608965.02,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","2","FORSYTH","DRAGADOS USA INC",686649.06,"RW1","NPAR",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",153999950,"","",4.0572999999999997,null,"",null,null,null,null,null,null,null,"","",""]
["","3","B-5325","C203500","C203500-EC","1","FRANKLIN","S T WOOTEN CORP",100565,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203500-RW","1","FRANKLIN","S T WOOTEN CORP",565697.1,"RW1","I000",0.24,2,"B801",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203500-SI","1","FRANKLIN","S T WOOTEN CORP",7695,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203500-ST","1","FRANKLIN","S T WOOTEN CORP",737368.61,"BR01","X081",2.5000000000000001E-2,null,"15",null,36,"739","Q",3,33.67,132.5,"PDMT","5","17+86.40 -L-"]
["","","","","C203500-TC","1","FRANKLIN","S T WOOTEN CORP",45295.38,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203500-UT","1","FRANKLIN","S T WOOTEN CORP",150806,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",1607427.09,"","",0.26500000000000001,null,"",null,null,null,null,null,null,null,"","",""]
["","4","","C203611","C203611A-RW","1","ALAMANCE","RILEY PAVING INC",204015.02,"RW1","",0.84899999999999998,3,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203611B-RW","1","ALAMANCE","RILEY PAVING INC",1372832.86,"RW1","",12.058,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203611C-RW","1","GUILFORD","RILEY PAVING INC",41438.04,"RW1","",0.21299999999999999,3,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",1618285.92,"","",13.12,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C203610","C203610A-RW","1","ROCKINGHAM","BLYTHE CONST INC",1051598.3,"RW1","",7.05,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","C203610B-RW","1","ROCKINGHAM","BLYTHE CONST INC",1793618.45,"RW1","",17.071000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
["","","","","","","","Result",2845216.75,"","",24.120999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","6","I-3803BA","C203485","C203485-SG","1","CABARRUS","ALS OF NORTH CAROLINA INC",875245.58,"RW1","",7.5,null,"M705",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",875245.58,"","",7.5,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C203612","C203612A-RW","1","BUNCOMBE","HARRISON CONST CO DIV O",1909286.73,"RW1","",5.53,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C203612B-RW","1","BUNCOMBE","HARRISON CONST CO DIV O",1607992.12,"RW1","",11.11,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",3517278.85,"","",16.64,null,"",null,null,"","",null,null,null,"","",""]
["","8","","C203613","C203613A-RW","1","MADISON","HARRISON CONST CO DIV O",1228683.25,"RW1","",7,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203613B-RW","1","MADISON","HARRISON CONST CO DIV O",114186.3,"RW1","",0.53,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1342869.55,"","",7.53,null,"",null,null,"","",null,null,null,"","",""]
["","9","","C203614","C203614A-RW","1","YANCEY","ROGERS GROUP INC",707352.13,"RW1","",4.99,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203614B-RW","1","YANCEY","ROGERS GROUP INC",73043.69,"RW1","",0.53,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",780395.82,"","",5.52,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C203600","C203600-RW","1","CHEROKEE","HARRISON CONST CO DIV O",2999995.05,"RW1","",5,4,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",2999995.05,"","",5,null,"",null,null,"","",null,null,null,"","",""]
["11/18/2014","1","R-2519B","C203358","C203358-EC","1","YANCEY","WRIGHT BROS CONST CO IN",6846651.8399999999,"RW1","",null,4,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203358-RW","1","YANCEY","WRIGHT BROS CONST CO IN",45378512.420000002,"RW1","",7.71,4,"D320",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203358-SI","1","YANCEY","WRIGHT BROS CONST CO IN",305008.73,"RW1","",null,4,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C203358-ST","1","YANCEY","WRIGHT BROS CONST CO IN",640900.31999999995,"CV01","Y007",1.2999999999999999E-2,12,"C204",100,12,"","",null,null,null,"V MTN","13","44+11.92 -L-"]
["","","","","","2","YANCEY","WRIGHT BROS CONST CO IN",389020.44,"CV02","Y007",null,10,"C202",100,6,"","",null,null,null,"V MTN","13","134+80.45 -L-"]
["","","","","","3","YANCEY","WRIGHT BROS CONST CO IN",83396.09,"CV03","Y007",null,6.3,"C201",55.67,7,"","",null,null,null,"V MTN","13","155+44.57 -L-"]
["","","","","","4","YANCEY","WRIGHT BROS CONST CO IN",225379.56,"CV04","Y007",5.0000000000000001E-3,10,"C203",90,8,"","",null,null,null,"V MTN","13","319+76.16 -L-"]
["","","","","","5","YANCEY","WRIGHT BROS CONST CO IN",298842.90999999997,"CV05","Y007",4.0000000000000001E-3,10,"C002",100,8,"","",null,null,null,"V MTN","13","323+58.66 -L-"]
["","","","","","6","YANCEY","WRIGHT BROS CONST CO IN",78869.48,"CV06","Y007",null,10,"C202",100,7,"","",null,null,null,"V MTN","13","327+50.47 -L-"]
["","","","","","7","YANCEY","WRIGHT BROS CONST CO IN",96298.29,"CV07","Y007",null,20.100000000000001,"C202",65,7,"","",null,null,null,"V MTN","13","345+98.42 -L-"]
["","","","","","8","YANCEY","WRIGHT BROS CONST CO IN",83254.399999999994,"CV08","Y007",null,6.6,"C001",82.75,8,"","",null,null,null,"V MTN","13","14+90.30 -Y17-"]
["","","","","","9","YANCEY","WRIGHT BROS CONST CO IN",60832.78,"CV09","Y007",null,6.1,"C001",68,6,"","",null,null,null,"V MTN","13","11+07.96 -Y34-"]
["","","","","","10","YANCEY","WRIGHT BROS CONST CO IN",482219,"WL1","Y007",null,null,"W000",7.44,null,"","",null,null,null,"V MTN","13","78+50.00 -L-"]
["","","","","","11","YANCEY","WRIGHT BROS CONST CO IN",190767,"WL2","Y007",null,null,"W000",5.75,null,"","",null,null,null,"V MTN","13","125+50.00 -L-"]
["","","","","","12","YANCEY","WRIGHT BROS CONST CO IN",430200,"WL3","Y007",null,null,"W000",8.89,null,"","",null,null,null,"V MTN","13","198+00.00 -L-"]
["","","","","","13","YANCEY","WRIGHT BROS CONST CO IN",200307,"WL4","Y007",null,null,"W000",3.33,null,"","",null,null,null,"V MTN","13","226+50.00 -L-"]
["","","","","","14","YANCEY","WRIGHT BROS CONST CO IN",160704,"WL1","Y007",null,null,"W000",9.98,null,"","",null,null,null,"V MTN","13","246 + 23.60 -L-"]
["","","","","","15","YANCEY","WRIGHT BROS CONST CO IN",175113.75,"WL2","Y007",null,null,"W000",122.93,null,"","",null,null,null,"V MTN","13","248 + 44.30 -L-"]
["","","","","","16","YANCEY","WRIGHT BROS CONST CO IN",154119,"WL7","Y007",null,null,"W000",6,null,"","",null,null,null,"V MTN","13","274+00.00 -L-"]
["","","","","","17","YANCEY","WRIGHT BROS CONST CO IN",371884.64,"WL8","Y007",null,null,"W000",13.45,null,"","",null,null,null,"V MTN","13","306+00.00 -L-"]
["","","","","","18","YANCEY","WRIGHT BROS CONST CO IN",219464.75,"WL9","Y007",null,null,"W000",4.55,null,"","",null,null,null,"V MTN","13","78+50.00 -L-"]
["","","","","","19","YANCEY","WRIGHT BROS CONST CO IN",716739.07,"BR01","X081",2.53E-2,null,"11",null,39.25,"700","A",1,36,133.54169999999999,"V MTN","13","24+11.31 -L- LT"]
["","","","","","20","YANCEY","WRIGHT BROS CONST CO IN",793703.94,"BR02","X081",null,null,"11",null,39.25,"700","A",1,36,133.54169999999999,"V MTN","13","24+11.31 -L- RT"]
["","","","","","21","YANCEY","WRIGHT BROS CONST CO IN",1477356.1,"BR03","X081",5.9700000000000003E-2,null,"45",null,39.25,"700","Q",3,36,315,"V MTN","13","122+22.50 -L- LT"]
["","","","","","22","YANCEY","WRIGHT BROS CONST CO IN",1264186.53,"BR04","X081",null,null,"15",null,39.25,"700","Q",3,36,315,"V MTN","13","122+22.50 -L- RT"]
["","","","","","23","YANCEY","WRIGHT BROS CONST CO IN",1309480.56,"BR05","X031",3.5000000000000003E-2,null,"15",null,39.25,"580","A",1,36,185,"V MTN","13","247+87.50 -L- LT"]
["","","","","","24","YANCEY","WRIGHT BROS CONST CO IN",1384488.16,"BR06","X031",null,null,"15",null,39.25,"580","A",1,36,185,"V MTN","13","247+87.50 -L- RT"]
["","","","","C203358-TC","1","YANCEY","WRIGHT BROS CONST CO IN",1002182.9,"RW1","",null,4,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",64819883.659999996,"","",7.8520000000000003,null,"",null,null,"","",null,null,null,"","",""]
["","2","U-0071","C203394","C203394-EC","1","DURHAM","DRAGADOS USA INC",6663811.0700000003,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203394-LI","1","DURHAM","DRAGADOS USA INC",812206.25,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203394-RW","1","DURHAM","DRAGADOS USA INC",75461211.900000006,"RW1","",3.7890000000000001,6,"N210",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203394-SG","1","DURHAM","DRAGADOS USA INC",1439941.25,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203394-SI","1","DURHAM","DRAGADOS USA INC",2985513.99,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203394-ST","1","DURHAM","DRAGADOS USA INC",308854.5,"CV01","Y007",null,25.13,"15",363.75,8,"","",null,null,null,"PDMT","5","95+48.49 -L-"]
["","","","","","2","DURHAM","DRAGADOS USA INC",375328.5,"CV02","Y007",null,72.14,"15",457,6,"","",null,null,null,"PDMT","5","133+41.46 -L-"]
["","","","","","3","DURHAM","DRAGADOS USA INC",344861,"CV03","Y007",null,19.5,"15",349,8,"","",null,null,null,"PDMT","5","34+45.00 -Y3-"]
["","","","","","4","DURHAM","DRAGADOS USA INC",194783.5,"CV04","Y007",null,20.53,"15",236.25,8,"","",null,null,null,"PDMT","5","19+07.28 -Y4-"]
["","","","","","5","DURHAM","DRAGADOS USA INC",506495.43,"WL1","Y007",null,null,"W000",7.83,null,"","",null,null,null,"PDMT","5","14+25 -L-"]
["","","","","","6","DURHAM","DRAGADOS USA INC",663186.15,"WL2","Y007",null,null,"W000",4.8,null,"","",null,null,null,"PDMT","5","25+28.00 -L-"]
["","","","","","7","DURHAM","DRAGADOS USA INC",379980.52,"WL3","Y007",null,null,"W000",9.26,null,"","",null,null,null,"PDMT","5","38+35.00 -L-"]
["","","","","","8","DURHAM","DRAGADOS USA INC",211534.4,"WL4","Y007",null,null,"W000",22,null,"","",null,null,null,"PDMT","5","31+71.32 -Y1-"]
["","","","","","9","DURHAM","DRAGADOS USA INC",748832.58,"WL5","Y007",null,null,"W000",16.61,null,"","",null,null,null,"PDMT","5","36+35.00 -L-"]
["","","","","","10","DURHAM","DRAGADOS USA INC",620996.49,"WL6","Y007",null,null,"W000",11.48,null,"","",null,null,null,"PDMT","5","45+11.77 -L-"]
["","","","","","11","DURHAM","DRAGADOS USA INC",208782.8,"WL7","Y007",null,null,"W000",22.82,null,"","",null,null,null,"PDMT","5","32+26.41 -Y1-"]
["","","","","","12","DURHAM","DRAGADOS USA INC",917564.73,"WL8","Y007",null,null,"W000",17.059999999999999,null,"","",null,null,null,"PDMT","5","44+39.73 -L-"]
["","","","","","13","DURHAM","DRAGADOS USA INC",50700,"WL9","Y007",null,null,"W005",2.5,null,"","",null,null,null,"PDMT","5","21+35.00 -Y1-"]
["","","","","","14","DURHAM","DRAGADOS USA INC",63552.1,"WL10","Y007",null,null,"W000",5.26,null,"","",null,null,null,"PDMT","5","24+00.00 -Y1-"]
["","","","","","15","DURHAM","DRAGADOS USA INC",271229.40000000002,"WL11","Y007",null,null,"W000",19.86,null,"","",null,null,null,"PDMT","5","14+80.00 -Y7RPC-"]
["","","","","","16","DURHAM","DRAGADOS USA INC",88475.4,"WL12","Y007",null,null,"W000",11.83,null,"","",null,null,null,"PDMT","5","21+14.89 -Y2-"]
["","","","","","17","DURHAM","DRAGADOS USA INC",119554,"WL13","Y007",null,null,"W000",14.14,null,"","",null,null,null,"PDMT","5","107+94.68 -WBL-"]
["","","","","","18","DURHAM","DRAGADOS USA INC",365217,"WL14","Y007",null,null,"W000",19.87,null,"","",null,null,null,"PDMT","5","107+85.36 -L-"]
["","","","","","19","DURHAM","DRAGADOS USA INC",418072.5,"WL15","Y007",null,null,"W000",21.04,null,"","",null,null,null,"PDMT","5","52+84.32 -DFWB-"]
["","","","","","20","DURHAM","DRAGADOS USA INC",144844,"WL16","Y007",null,null,"W000",14.07,null,"","",null,null,null,"PDMT","5","46+46.95 -DFEB-"]
["","","","","","21","DURHAM","DRAGADOS USA INC",398677.5,"WL17","Y007",null,null,"W000",24.22,null,"","",null,null,null,"PDMT","5","157+72.04 -LDFEB-"]
["","","","","","22","DURHAM","DRAGADOS USA INC",757785,"WL18","Y007",null,null,"W000",14.02,null,"","",null,null,null,"PDMT","5","58+19.81 -DFWB-"]
["","","","","","23","DURHAM","DRAGADOS USA INC",382953,"WL19","Y007",null,null,"W000",14.11,null,"","",null,null,null,"PDMT","5","16+70.77 -US70FLY-"]
["","","","","","24","DURHAM","DRAGADOS USA INC",2408126.59,"BR01","X271",2.52E-2,null,"11",null,149.25,"550","A",1,146,133,"PDMT","5","44+08.60 -L-"]
["","","","","","25","DURHAM","DRAGADOS USA INC",3565524.69,"BR21","X671",null,null,"21",null,17,"590","Q",4,15,410.02600000000001,"PDMT","5","64+55.50 -L-"]
["","","","","","26","DURHAM","DRAGADOS USA INC",3494812.28,"BR22","X671",null,null,"21",null,18,"590","Q",4,16,410.02600000000001,"PDMT","5","64+74.69 -L-"]
["","","","","","27","DURHAM","DRAGADOS USA INC",3025286.7,"BR23","X671",null,null,"21",null,16,"536","Q",8,8.25,440,"PDMT","5","65+21.79 -L-"]
["","","","","","28","DURHAM","DRAGADOS USA INC",1521397.99,"BR03","X771",null,null,"11",null,49.583300000000001,"666","Q",2,36,270,"PDMT","5","85+26.52 -L-"]
["","","","","","29","DURHAM","DRAGADOS USA INC",1758868.86,"BR04","X771",null,null,"11",null,53.25,"660","Q",2,50,270,"PDMT","5","107+45.55 -L-"]
["","","","","","30","DURHAM","DRAGADOS USA INC",3125425.27,"BR05","X771",null,null,"11",null,41.25,"670","P",4,38,547,"PDMT","5","105+29.00 -L-"]
["","","","","","31","DURHAM","DRAGADOS USA INC",1212730.73,"BR06","X271",2.5899999999999999E-2,null,"11",null,75.25,"554","A",1,72,137,"PDMT","5","125+91.57-L-WBL"]
["","","","","","32","DURHAM","DRAGADOS USA INC",1277133.28,"BR07","X271",null,null,"11",null,75.25,"554","A",1,72,137,"PDMT","5","125+91.57-L-EBL"]
["","","","","","33","DURHAM","DRAGADOS USA INC",4018862.31,"BR08","X571",7.5399999999999995E-2,null,"14",null,76.75,"664","Q",3,73.5,398,"PDMT","5","17+97.57 -DFLW-"]
["","","","","","34","DURHAM","DRAGADOS USA INC",4027763.04,"BR09","X571",null,null,"14",null,76.75,"664","Q",3,73.5,398,"PDMT","5","138+40.45 -LDFEB-"]
["","","","","","35","DURHAM","DRAGADOS USA INC",2747914.2,"BR10","X271",null,null,"11",null,386,"754","Q",1,142.79169999999999,215.97919999999999,"PDMT","5","157+33.78 -LDFEB-"]
["","","","","","36","DURHAM","DRAGADOS USA INC",4957749.21,"BR11","X771",null,null,"11",null,41.25,"664","P",6,38,916,"PDMT","5","23+29.61 -DFFLY-"]
["","","","","","37","DURHAM","DRAGADOS USA INC",319864.46000000002,"BR12","X271",null,null,"11",null,15.416700000000001,"592","Q",3,13.792,152.31800000000001,"PDMT","5","36+69.26 -DFWB- WID"]
["","","","","","38","DURHAM","DRAGADOS USA INC",1052282.52,"BR14","X271",null,null,"11",null,60,"592","I",3,57.375,173.8802,"PDMT","5","34+62.88 -DFEB- WID"]
["","","","","","39","DURHAM","DRAGADOS USA INC",1226856.18,"BR16","X171",null,null,"12",null,16.958400000000001,"592","Q",3,15.333299999999999,339.9896,"PDMT","5","24+70.18 -DFWB- WID"]
["","","","","","40","DURHAM","DRAGADOS USA INC",64691.59,"BR13","X271",2.8799999999999999E-2,null,"11",null,57.5,"596","I",3,54.833300000000001,152.3177,"PDMT","5","36+69.26 -DFWB- P&R"]
["","","","","","41","DURHAM","DRAGADOS USA INC",62816.66,"BR15","X271",null,null,"11",null,50.291699999999999,"596","I",3,47.625,173.8802,"PDMT","5","34+62.88 -DFEB- P&R"]
["","","","","","42","DURHAM","DRAGADOS USA INC",239413.99,"BR17","X271",6.4399999999999999E-2,null,"11",null,57.916699999999999,"596","I",3,55.041699999999999,339.9896,"PDMT","5","24+70.18 -DFWB- P&R"]
["","","","","","43","DURHAM","DRAGADOS USA INC",258178.27,"BR18","X271",null,null,"12",null,49.5,"596","I",3,47,320.41669999999999,"PDMT","5","23+44.51 -DFEB- P&R"]
["","","","","C203394-TC","1","DURHAM","DRAGADOS USA INC",3408911.1,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203394-UT","1","DURHAM","DRAGADOS USA INC",1168586.52,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","2","DURHAM","DRAGADOS USA INC",1101358.6000000001,"RW1","NPAR",null,6,"",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",141949500,"","",4.0087000000000002,null,"",null,null,null,null,null,null,null,"","",""]
["","3","","C203618","C203618A-RW","1","DURHAM","CAROLINA SUNROCK LLC",3184732.4,"RW1","",10.391,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","C203618B-RW","1","DURHAM","CAROLINA SUNROCK LLC",2804252.75,"RW1","",14.888999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
["","","","","","","","Result",5988985.1500000004,"","",25.28,null,"",null,null,"","",null,null,null,"","",""]
["","4","U-3465","C203497","C203497-EC","1","HARNETT","FSC II LLC DBA FRED SMITH CO",1011834,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203497-RW","1","HARNETT","FSC II LLC DBA FRED SMITH CO",17032887.5,"RW1","I000",3.8050000000000002,4,"G410",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203497-SG","1","HARNETT","FSC II LLC DBA FRED SMITH CO",231698.15,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203497-SI","1","HARNETT","FSC II LLC DBA FRED SMITH CO",95804.25,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203497-TC","1","HARNETT","FSC II LLC DBA FRED SMITH CO",475304.8,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","C203497-UT","1","HARNETT","FSC II LLC DBA FRED SMITH CO",1737000,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","","","","Result",20584528.699999999,"","",3.8050000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","5","R-5523","C203599","C203599-RW","1","HARNETT","HIGHLAND PAVING CO LLC",1917813.9,"RW1","I000",0.43099999999999999,2,"N200",null,null,"","",null,null,null,"PDMT","6",""]
["","","","","","","","Result",1917813.9,"","",0.43099999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","6","R-0623","C203494","C203494-EC","1","MONTGOMERY","J T RUSSELL & SONS INC",5301876.0999999996,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203494-RW","1","MONTGOMERY","J T RUSSELL & SONS INC",30022070.59,"RW1","",6.5220000000000002,4,"N210",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203494-SG","1","MONTGOMERY","J T RUSSELL & SONS INC",239946.25,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203494-SI","1","MONTGOMERY","J T RUSSELL & SONS INC",249110.83,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203494-ST","1","MONTGOMERY","J T RUSSELL & SONS INC",251839.53,"CV01","X028",3.8999999999999998E-3,11.76,"C002",182.5,8,"","",null,null,null,"PDMT","8","53+95.00 -L-"]
["","","","","","2","MONTGOMERY","J T RUSSELL & SONS INC",359609.16,"CV02","X028",4.3E-3,16.899999999999999,"C002",183,10,"","",null,null,null,"PDMT","8","77+04.00 -L-"]
["","","","","","3","MONTGOMERY","J T RUSSELL & SONS INC",261140.91,"CV03","X028",2.5999999999999999E-3,29.38,"C001",256,10,"","",null,null,null,"PDMT","8","188+02.00 -L-"]
["","","","","","4","MONTGOMERY","J T RUSSELL & SONS INC",417823.11,"CV04","X028",5.7000000000000002E-3,14.64,"C002",203.5,12,"","",null,null,null,"PDMT","8","204+38.00 -L-"]
["","","","","","5","MONTGOMERY","J T RUSSELL & SONS INC",259931.7,"CV05","X028",4.4999999999999997E-3,9.6199999999999992,"C002",150,11,"","",null,null,null,"PDMT","8","283+62.00 -L-"]
["","","","","","6","MONTGOMERY","J T RUSSELL & SONS INC",1032715.34,"BR01","X081",4.8300000000000003E-2,null,"15",null,40.5,"854","Q",3,37.25,255,"PDMT","8","123+82.50 -L- WBL"]
["","","","","","7","MONTGOMERY","J T RUSSELL & SONS INC",1014567.32,"BR02","X081",null,null,"15",null,40.333300000000001,"854","Q",3,37.083300000000001,255,"PDMT","8","123+82.50 -L- EBL"]
["","","","","","8","MONTGOMERY","J T RUSSELL & SONS INC",1364639.46,"BR03","X081",5.9700000000000003E-2,null,"15",null,39.25,"872","Q",3,36,315,"PDMT","8","339+48.56 -L- WBL"]
["","","","","","9","MONTGOMERY","J T RUSSELL & SONS INC",1508986.22,"BR04","X081",null,null,"15",null,39.25,"872","Q",3,36,315,"PDMT","8","339+48.56 -L- EBL"]
["","","","","C203494-TC","1","MONTGOMERY","J T RUSSELL & SONS INC",454209.97,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","C203494-UT","1","MONTGOMERY","J T RUSSELL & SONS INC",2328056.16,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","8",""]
["","","","","","","","Result",45066522.649999999,"","",6.6509999999999998,null,"",null,null,null,null,null,null,null,"","",""]
["","7","B-4511","C203493","C203493-EC","1","FORSYTH","SMITH-ROWE LLC",38723,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203493-RW","1","FORSYTH","SMITH-ROWE LLC",442458.6,"RW1","I000",0.17199999999999999,2,"B810",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203493-SI","1","FORSYTH","SMITH-ROWE LLC",7536.48,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203493-ST","1","FORSYTH","SMITH-ROWE LLC",419987.41,"BR01","X080",1.7399999999999999E-2,null,"15",null,39,"733","A",1,36.5,92.25,"PDMT","9","18+66.50 -L-"]
["","","","","C203493-TC","1","FORSYTH","SMITH-ROWE LLC",3000.92,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",911706.41,"","",0.18940000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","8","R-5115","C203495","C203495-EC","1","MACON","WATSON CONT INC",65455.5,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203495-RW","1","MACON","WATSON CONT INC",420235.5,"RW1","",0.14799999999999999,2,"M720",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203495-SI","1","MACON","WATSON CONT INC",19152,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203495-TC","1","MACON","WATSON CONT INC",7323,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203495-UT","1","MACON","WATSON CONT INC",47769,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",559935,"","",0.14799999999999999,null,"",null,null,"","",null,null,null,"","",""]
["12/16/2014","2","R-4903","C203503","C203503-EC","1","BLADEN","BARNHILL CONT CO",1174108,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203503-RW","1","BLADEN","BARNHILL CONT CO",8559043.1600000001,"RW1","I000",1.0880000000000001,2,"I604",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203503-SG","1","BLADEN","BARNHILL CONT CO",48492.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203503-SI","1","BLADEN","BARNHILL CONT CO",154902.14000000001,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203503-ST","1","BLADEN","BARNHILL CONT CO",604145.72,"BR01","X081",0.02,null,"15",null,55.25,"836","A",3,52,105,"COAST","6","67+16.50 -L-"]
["","","","","","2","BLADEN","BARNHILL CONT CO",981664.03,"BR02","X231",null,null,"11",null,49.25,"570","A",1,46,157.5,"COAST","6","46+73.19 -L- LT"]
["","","","","","3","BLADEN","BARNHILL CONT CO",981391.33,"BR03","X231",null,null,"11",null,49.25,"570","A",1,46,157.4948,"COAST","6","46+73.19 -L- RT"]
["","","","","C203503-TC","1","BLADEN","BARNHILL CONT CO",213493.86,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","C203503-UT","1","BLADEN","BARNHILL CONT CO",547980.99,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
["","","","","","","","Result",13265221.98,"","",1.1080000000000001,null,"",null,null,null,null,null,null,null,"","",""]
["","3","B-4741","C203499","C203499-EC","1","DAVIDSON","DANE CONST INC",63794.45,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203499-RW","1","DAVIDSON","DANE CONST INC",966779,"RW1","I000",0.249,2,"B801",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203499-SI","1","DAVIDSON","DANE CONST INC",7096.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","C203499-ST","1","DAVIDSON","DANE CONST INC",1265537.3500000001,"BR01","X080",5.3999999999999999E-2,null,"15",null,33,"733","Q",4,30.5,282.625,"PDMT","9","20+92.00 -L-"]
["","","","","C203499-TC","1","DAVIDSON","DANE CONST INC",30586.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
["","","","","","","","Result",2333793.9,"","",0.30299999999999999,null,"",null,null,null,null,null,null,null,"","",""]
["","4","I-5321","C203502","C203502-RW","1","BUNCOMBE","HARRISON CONST CO DIV O",4662807.3,"RW1","I000",7.47,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",4662807.3,"","",7.47,null,"",null,null,"","",null,null,null,"","",""]
["","5","I-5512","C203620","C203601-RW","1","HAYWOOD","LANFORD BROS CO INC",6948501.46,"RW1","",0.67400000000000004,4,"M720",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",6948501.46,"","",0.67400000000000004,null,"",null,null,"","",null,null,null,"","",""]
[" ",null,null,"","","","","Overall Result",1811149524.1199999,"","",1306.9304999999999,null,"",null,null,null,null,null,null,null,"","",""]

{"sheet":"Items - Statewide","index":1,"n_rows":2788,"n_cols":7,"rows_kept":2788,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - STATEWIDE"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",156,420352.19788461499,65574942.869999997]
["0000400000-N","CONST SURVEYING","","",55,175671.281090909,9661920.4600000009]
["0000700000-N","FIELD OFFICE","","",4,134899.34,539597.36]
["0000900000-N","GENERIC MISC ITEM (LS)","ALT LUMP SUM BID","FOR BRG 100012",1,665000,665000]
["","","","FOR BRG 560001",1,550000,550000]
["","","","FOR BRG 560076",1,715000,715000]
["","","","FOR BRG 560231",1,415000,415000]
["","","","FOR BRG 600005",1,817115,817115]
["","","","FOR BRG 760056",1,808901.19,808901.19]
["","","","FOR BRG 800172",1,328250,328250]
["","","","FOR BRG 820006",1,978338.42,978338.42]
["","","CONST TAXIWAY BRG","",1,12750000,12750000]
["","","CNTRL OF VIBRATION","",1,41500,41500]
["","","DESIGN & CONST OF","BRGS",8,3844603.9550000001,30756831.640000001]
["","","","CLVT  430020",1,327000,327000]
["","","","CLVT  430273",1,614000,614000]
["","","","CLVT  430305",1,470000,470000]
["","","","CLVT  430309",1,390000,390000]
["","","","CLVT  430310",1,458000,458000]
["","","","CLVT  430314",1,369000,369000]
["","","","CLVT  430315",1,507000,507000]
["","","","CLVT  430317",1,410000,410000]
["","","","CLVT  430372",1,504000,504000]
["","","","CLVT  490055",1,512000,512000]
["","","","OF CLVT 610228",1,613870.69999999995,613870.69999999995]
["","","DESIGN & CONST OF","CLVT  430102",1,411000,411000]
["","","DESIGN & CONST","I-5110",1,48355000,48355000]
["","","","R-2413A & R-2413B",1,115445000,115445000]
["","","","",1,186687000,186687000]
["","","INSPECT BLDG: COMPLETE GENERAL","CONST & ALL SYST INDICATED",1,600000,600000]
["","","SCALE BLDG & SCALE BOOTH: COMPLETE","GEN CONST & ALL SYST  INDICATED",1,900000,900000]
["","","TEMP GUARD BLDG","",1,35000,35000]
["","","TEMP SPRUNG STR AT","YADKIN RD DETR",1,75000,75000]
["0000910000-N","GENERIC MISC ITEM (HR)","EXPLORATORY EXCAV","STD",750,202.5,151875]
["","","EXPLORATORY EXCAV-","VACUUM",250,250,62500]
["0000915000-N","GENERIC MISC ITEM (EA)","END BENTS STR 010071","",2,29600,59200]
["","","END BENTS STR 010079","",2,26000,52000]
["","","END BENTS STR 010081","",2,31000,62000]
["","","END BENTS STR 010246","",2,29000,58000]
["","","END BENTS STR 020031","",2,20885.759999999998,41771.519999999997]
["","","END BENTS STR 020046","",2,48953.43,97906.86]
["","","END BENTS STR 020057","",2,20857.990000000002,41715.980000000003]
["","","END BENTS STR 040060","",2,18130.810000000001,36261.620000000003]
["","","END BENTS STR 040061","",2,55051.4,110102.8]
["","","END BENTS STR 040066","",2,64490.51,128981.02]
["","","END BENTS STR 040187","",2,21328.33,42656.66]
["","","END BENTS STR 040350","",2,59360.26,118720.52]
["","","END BENTS STR 040371","",2,22593.19,45186.38]
["","","END BENTS STR 100371","",2,85000,170000]
["","","END BENTS STR 100676","",2,45000,90000]
["","","END BENTS STR 100677","",2,45000,90000]
["","","END BENTS STR 110014","",2,90000,180000]
["","","END BENTS STR 110015","",2,98000,196000]
["","","END BENTS STR 110034","",2,80000,160000]
["","","END BENTS STR 110035","",2,78000,156000]
["","","END BENTS STR 110060","",2,83000,166000]
["","","END BENTS STR 130077","",2,19932.689999999999,39865.379999999997]
["","","END BENTS STR 130164","",2,40139.99,80279.98]
["","","END BENTS STR 430326","",2,46290,92580]
["","","END BENTS STR 430334","",2,80437.5,160875]
["","","END BENTS STR 460023","",2,14007.68,28015.360000000001]
["","","END BENTS STR 460024","",2,13338.84,26677.68]
["","","END BENTS STR 460025","",2,13338.84,26677.68]
["","","END BENTS STR 460098","",2,13954.68,27909.360000000001]
["","","END BENTS STR 480282","",2,27500,55000]
["","","END BENTS STR 490103","",2,53595,107190]
["","","END BENTS STR 490164","",2,57111.5,114223]
["","","END BENTS STR 490182","",2,58790,117580]
["","","END BENTS STR 490337","",2,87745,175490]
["","","END BENTS STR 580005","",2,118000,236000]
["","","END BENTS STR 580021","",2,89000,178000]
["","","END BENTS STR 580022","",2,70000,140000]
["","","END BENTS STR 600031","",2,45000,90000]
["","","END BENTS STR 600042","",2,45000,90000]
["","","END BENTS STR 600163","",2,85000,170000]
["","","END BENTS STR 610030","",2,14502.4,29004.799999999999]
["","","END BENTS STR 610157","",2,21868.9,43737.8]
["","","END BENTS STR 610232","",2,24568,49136]
["","","END BENTS STR 760093","",2,13447.82,26895.64]
["","","END BENTS STR 760110","",2,13408.45,26816.9]
["","","END BENTS STR 800094","",2,120000,240000]
["","","END BENTS STR 800174","",2,23000,46000]
["","","END BENTS STR 800195","",2,98000,196000]
["","","END BENTS STR 820011","",2,17996.689999999999,35993.379999999997]
["","","END BENTS STR 850019","",2,15011.88,30023.759999999998]
["","","END BENTS STR 850034","",2,18301.93,36603.86]
["","","END BENTS STR 850094","",2,34574.22,69148.44]
["","","END BENTS STR 850143","",2,15011.88,30023.759999999998]
["","","END BENTS STR 850202","",2,72582.399999999994,145164.79999999999]
["","","END BENTS STR 850203","",2,47007.61,94015.22]
["","","END BENTS STR 850213","",2,42160.08,84320.16]
["","","END BENTS STR 850257","",2,95450.79,190901.58]
["","","END BENTS STR 850322","",2,26154.04,52308.08]
["","","END BENTS STR 960106","",2,25029.06,50058.12]
["","","END BENTS STR 960143","",2,17681.900000000001,35363.800000000003]
["","","END BENTS STR 960144","",2,17350.48,34700.959999999999]
["","","END BENTS STR 960187","",2,17053.47,34106.94]
["","","END BENTS STR 960405","",2,17877.02,35754.04]
["","","END BENTS STR 980091","",2,28520.82,57041.64]
["","","END BENTS STR 980092","",2,53745.52,107491.04]
["","","END BENTS STR 980109","",2,15011.88,30023.759999999998]
["","","INTERIOR BENT CAP STR","010079",2,23000,46000]
["","","","010081",1,32280,32280]
["","","","040060",1,26847.16,26847.16]
["","","","100012",null,null,0]
["","","","130077",1,27766.39,27766.39]
["","","","480282",2,20000,40000]
["","","","610157",1,16838.25,16838.25]
["","","","850019",2,13975.44,27950.880000000001]
["","","","850034",1,18710.490000000002,18710.490000000002]
["","","","850094",2,15947.39,31894.78]
["","","","850143",1,14256.92,14256.92]
["","","","850203",1,13015.16,13015.16]
["","","","960106",2,28823.040000000001,57646.080000000002]
["","","","960143",1,27961.65,27961.65]
["","","","960144",2,24713.07,49426.14]
["","","","960405",2,26801.69,53603.38]
["","","","980109",2,13975.44,27950.880000000001]
["","","RIGHT OF WAY ACQUISIT","",172,4140.1627906980002,712108]
["0000930000-E","GENERIC MISC ITEM (LF)","AVE FOUND LGTH  END","BENT1 STR 010071",19,1,19]
["","","","BENT1 STR 010079",37,1,37]
["","","","BENT1 STR 010081",30,1,30]
["","","","BENT1 STR 010246",20,1,20]
["","","","BENT1 STR 020031",12,2827.07,33924.839999999997]
["","","","BENT1 STR 020046",12,2664.51,31974.12]
["","","","BENT1 STR 020057",11,3952.04,43472.44]
["","","","BENT1 STR 040060",14,466.66,6533.24]
["","","","BENT1 STR 040061",14,1,14]
["","","","BENT1 STR 040066",11,1,11]
["","","","BENT1 STR 040187",15,488.25,7323.75]
["","","","BENT1 STR 040350",13,539.99,7019.87]
["","","","BENT1 STR 040371",36,439.28,15814.08]
["","","","BENT1 STR 100371",10,9,90]
["","","","BENT1 STR 100676",48,325,15600]
["","","","BENT1 STR 100677",14,4250,59500]
["","","","BENT1 STR 110014",11,1,11]
["","","","BENT1 STR 110015",17,1,17]
["","","","BENT1 STR 110034",25,1,25]
["","","","BENT1 STR 110035",66,1,66]
["","","","BENT1 STR 110060",23,1,23]
["","","","BENT1 STR 130077",46,377.49,17364.54]
["","","","BENT1 STR 130164",16,829.99,13279.84]
["","","","BENT1 STR 430326",40,1151.5,46060]
["","","","BENT1 STR 430334",18,1569,28242]
["","","","BENT1 STR 460023",65,209.52,13618.8]
["","","","BENT1 STR 460024",62,219.66,13618.92]
["","","","BENT1 STR 460025",66,206.34,13618.44]
["","","","BENT1 STR 460098",65,223.42,14522.3]
["","","","BENT1 STR 480282",19,1,19]
["","","","BENT1 STR 490103",10,4151,41510]
["","","","BENT1 STR 490164",11,3129,34419]
["","","","BENT1 STR 490182",11,4137.5,45512.5]
["","","","BENT1 STR 490337",47,387.5,18212.5]
["","","","BENT1 STR 580005",11,1,11]
["","","","BENT1 STR 580021",41,1,41]
["","","","BENT1 STR 580022",58,1,58]
["","","","BENT1 STR 600031",13,5065,65845]
["","","","BENT1 STR 600042",22,2725,59950]
["","","","BENT1 STR 600163",22,380,8360]
["","","","BENT1 STR 610030",14,366.68,5133.5200000000004]
["","","","BENT1 STR 610157",16,320.85000000000002,5133.6000000000004]
["","","","BENT1 STR 610232",15,342.24,5133.6000000000004]
["","","","BENT1 STR 760093",18,326.99,5885.82]
["","","","BENT1 STR 760110",16,367.87,5885.92]
["","","","BENT1 STR 800094",20,1,20]
["","","","BENT1 STR 800174",35,1,35]
["","","","BENT1 STR 800195",11,1,11]
["","","","BENT1 STR 820011",95,281.39,26732.05]
["","","","BENT1 STR 850019",32,258.3,8265.6]
["","","","BENT1 STR 850034",21,395.09,8296.89]
["","","","BENT1 STR 850094",36,321.44,11571.84]
["","","","BENT1 STR 850143",30,249.53,7485.9]
["","","","BENT1 STR 850202",39,231.93,9045.27]
["","","","BENT1 STR 850203",12,1,12]
["","","","BENT1 STR 850213",40,226.13,9045.2000000000007]
["","","","BENT1 STR 850257",14,1,14]
["","","","BENT1 STR 850322",15,343.11,5146.6499999999996]
["","","","BENT1 STR 960106",15,423.9,6358.5]
["","","","BENT1 STR 960143",44,245.39,10797.16]
["","","","BENT1 STR 960144",24,325.83,7819.92]
["","","","BENT1 STR 960187",14,451.95,6327.3]
["","","","BENT1 STR 960405",23,318.58999999999997,7327.57]
["","","","BENT1 STR 980091",12,363.9,4366.8]
["","","","BENT1 STR 980092",21,282.20999999999998,5926.41]
["","","","BENT1 STR 980109",13,365.9,4756.7]
["","","","BENT2 STR 010071",14,1,14]
["","","","BENT2 STR 010079",36,1,36]
["","","","BENT2 STR 010081",45,1,45]
["","","","BENT2 STR 010246",16,1,16]
["","","","BENT2 STR 020031",16,2153.62,34457.919999999998]
["","","","BENT2 STR 020046",11,2900.62,31906.82]
["","","","BENT2 STR 020057",27,1423.62,38437.74]
["","","","BENT2 STR 040060",13,557.19000000000005,7243.47]
["","","","BENT2 STR 040061",15,2372.9,35593.5]
["","","","BENT2 STR 040066",11,1,11]
["","","","BENT2 STR 040187",24,299.64,7191.36]
["","","","BENT2 STR 040350",10,1,10]
["","","","BENT2 STR 040371",37,439.2,16250.4]
["","","","BENT2 STR 100371",12,5200,62400]
["","","","BENT2 STR 100676",41,330,13530]
["","","","BENT2 STR 100677",13,5065,65845]
["","","","BENT2 STR 110014",10,1,10]
["","","","BENT2 STR 110015",10,1,10]
["","","","BENT2 STR 110034",24,1,24]
["","","","BENT2 STR 110035",50,1,50]
["","","","BENT2 STR 110060",15,1,15]
["","","","BENT2 STR 130077",41,396.86,16271.26]
["","","","BENT2 STR 130164",19,3550.24,67454.559999999998]
["","","","BENT2 STR 430326",16,1525,24400]
["","","","BENT2 STR 430334",24,232,5568]
["","","","BENT2 STR 460023",65,209.52,13618.8]
["","","","BENT2 STR 460024",60,214.44,12866.4]
["","","","BENT2 STR 460025",67,214.49,14370.83]
["","","","BENT2 STR 460098",65,223.42,14522.3]
["","","","BENT2 STR 480282",24,1,24]
["","","","BENT2 STR 490103",10,4151,41510]
["","","","BENT2 STR 490164",20,427.5,8550]
["","","","BENT2 STR 490182",10,3891,38910]
["","","","BENT2 STR 490337",55,356.5,19607.5]
["","","","BENT2 STR 580005",10,1,10]
["","","","BENT2 STR 580021",48,1,48]
["","","","BENT2 STR 580022",71,1,71]
["","","","BENT2 STR 600031",15,4170,62550]
["","","","BENT2 STR 600042",18,3330,59940]
["","","","BENT2 STR 600163",18,420,7560]
["","","","BENT2 STR 610030",15,342.24,5133.6000000000004]
["","","","BENT2 STR 610157",15,342.24,5133.6000000000004]
["","","","BENT2 STR 610232",15,342.24,5133.6000000000004]
["","","","BENT2 STR 760093",15,342.24,5133.6000000000004]
["","","","BENT2 STR 760110",15,342.24,5133.6000000000004]
["","","","BENT2 STR 800094",22,1,22]
["","","","BENT2 STR 800174",27,1,27]
["","","","BENT2 STR 800195",30,1,30]
["","","","BENT2 STR 820011",95,281.49,26741.55]
["","","","BENT2 STR 850019",29,258.13,7485.77]
["","","","BENT2 STR 850034",18,460.94,8296.92]
["","","","BENT2 STR 850094",32,327.5,10480]
["","","","BENT2 STR 850143",32,258.3,8265.6]
["","","","BENT2 STR 850202",39,231.93,9045.27]
["","","","BENT2 STR 850203",13,365.9,4756.7]
["","","","BENT2 STR 850213",43,228.49,9825.07]
["","","","BENT2 STR 850257",13,1,13]
["","","","BENT2 STR 850322",18,329.24,5926.32]
["","","","BENT2 STR 960106",14,440.62,6168.68]
["","","","BENT2 STR 960143",21,370.77,7786.17]
["","","","BENT2 STR 960144",39,268.91000000000003,10487.49]
["","","","BENT2 STR 960187",17,403.01,6851.17]
["","","","BENT2 STR 960405",26,294.66000000000003,7661.16]
["","","","BENT2 STR 980091",11,396.99,4366.8900000000003]
["","","","BENT2 STR 980092",26,257.93,6706.18]
["","","","BENT2 STR 980109",30,249.53,7485.9]
["","","AVE FOUND LGTH AT INTE-","RIOR BENT 1 STR 010079",52,3700,192400]
["","","","RIOR BENT 1 STR 010081",57,4260,242820]
["","","","RIOR BENT 1 STR 040060",24,2202.44,52858.559999999998]
["","","","RIOR BENT 1 STR 130077",56,1444.22,80876.320000000007]
["","","","RIOR BENT 1 STR 480282",34,4200,142800]
["","","","RIOR BENT 1 STR 610157",25,2000,50000]
["","","","RIOR BENT 1 STR 850019",40,1967.75,78710]
["","","","RIOR BENT 1 STR 850034",27,3607.23,97395.21]
["","","","RIOR BENT 1 STR 850094",43,2601.41,111860.63]
["","","","RIOR BENT 1 STR 850143",42,2096.9899999999998,88073.58]
["","","","RIOR BENT 1 STR 850203",23,5166.2,118822.6]
["","","","RIOR BENT 1 STR 960106",27,3080.43,83171.61]
["","","","RIOR BENT 1 STR 960143",56,1504.34,84243.04]
["","","","RIOR BENT 1 STR 960144",54,1328.96,71763.839999999997]
["","","","RIOR BENT 1 STR 960405",44,1525.51,67122.44]
["","","","RIOR BENT 1 STR 980109",44,1908.54,83975.76]
["","","","RIOR BENT 2 STR 010079",52,3700,192400]
["","","","RIOR BENT 2 STR 480282",34,4200,142800]
["","","","RIOR BENT 2 STR 850019",40,1967.75,78710]
["","","","RIOR BENT 2 STR 850094",43,2601.41,111860.63]
["","","","RIOR BENT 2 STR 960106",27,3116.47,84144.69]
["","","","RIOR BENT 2 STR 960144",54,2190.0700000000002,118263.78]
["","","","RIOR BENT 2 STR 960405",44,1534.04,67497.759999999995]
["","","","RIOR BENT 2 STR 980109",44,1908.54,83975.76]
["","","BRG LGTH STR","020031",105,2644.4,277662]
["","","","020046",55,1457.9,80184.5]
["","","","020057",65,1883.81,122447.65]
["","","","040060",105,1843.99,193618.95]
["","","","040061",55,2230.41,122672.55]
["","","","040066",90,2469.25,222232.5]
["","","","040187",70,1704.23,119296.1]
["","","","040350",40,1466.38,58655.199999999997]
["","","","040371",35,1554.79,54417.65]
["","","","130077",135,2484.63,335425.05]
["","","","130164",70,1655.22,115865.4]
["","","","960106",135,1985.59,268054.65000000002]
["","","","960143",95,1889.12,179466.4]
["","","","960144",145,1916.16,277843.20000000001]
["","","","960187",70,1700.63,119044.1]
["","","","960405",140,1525.75,213605]
["","","BRG LGTH STR 010071","",70,2500,175000]
["","","BRG LGTH STR 010079","",130,2300,299000]
["","","BRG LGTH STR 010081","",100,2400,240000]
["","","BRG LGTH STR 010246","",70,2400,168000]
["","","BRG LGTH STR 100371","",70,2375,166250]
["","","BRG LGTH STR 100676","",50,1560,78000]
["","","BRG LGTH STR 100677","",50,1560,78000]
["","","BRG LGTH STR 110014","",40,2200,88000]
["","","BRG LGTH STR 110015","",55,2200,121000]
["","","BRG LGTH STR 110034","",70,2400,168000]
["","","BRG LGTH STR 110035","",40,2000,80000]
["","","BRG LGTH STR 110060","",40,2100,84000]
["","","BRG LGTH STR 430326","",50,2894,144700]
["","","BRG LGTH STR 430334","",40,1567.5,62700]
["","","BRG LGTH STR 460023","",60,1886.47,113188.2]
["","","BRG LGTH STR 460024","",55,1678.75,92331.25]
["","","BRG LGTH STR 460025","",55,1678.75,92331.25]
["","","BRG LGTH STR 460098","",65,1836.92,119399.8]
["","","BRG LGTH STR 480282","",190,2500,475000]
["","","BRG LGTH STR 490103","",30,1802,54060]
["","","BRG LGTH STR 490164","",55,1865,102575]
["","","BRG LGTH STR 490182","",35,1987.5,69562.5]
["","","BRG LGTH STR 490337","",35,1961,68635]
["","","BRG LGTH STR 580005","",70,2300,161000]
["","","BRG LGTH STR 580021","",55,2300,126500]
["","","BRG LGTH STR 580022","",100,3100,310000]
["","","BRG LGTH STR 600031","",35,1895,66325]
["","","BRG LGTH STR 600042","",115,2900,333500]
["","","BRG LGTH STR 600163","",70,2395,167650]
["","","BRG LGTH STR 610030","",70,1812.86,126900.2]
["","","BRG LGTH STR 610157","",130,3447.46,448169.8]
["","","BRG LGTH STR 610232","",100,2792.16,279216]
["","","BRG LGTH STR 760093","",55,1731.32,95222.6]
["","","BRG LGTH STR 760110","",50,1744.14,87207]
["","","BRG LGTH STR 800094","",55,1940,106700]
["","","BRG LGTH STR 800174","",70,2400,168000]
["","","BRG LGTH STR 800195","",70,2200,154000]
["","","BRG LGTH STR 820011","",60,1853.07,111184.2]
["","","BRG LGTH STR 850019","",140,1586.41,222097.4]
["","","BRG LGTH STR 850034","",130,3561.74,463026.2]
["","","BRG LGTH STR 850094","",190,2816.13,535064.69999999995]
["","","BRG LGTH STR 850143","",120,1934.03,232083.6]
["","","BRG LGTH STR 850202","",70,1657.51,116025.7]
["","","BRG LGTH STR 850203","",100,1448.17,144817]
["","","BRG LGTH STR 850213","",45,1317.28,59277.599999999999]
["","","BRG LGTH STR 850257","",40,1497.42,59896.800000000003]
["","","BRG LGTH STR 850322","",105,2523.27,264943.34999999998]
["","","BRG LGTH STR 980091","",50,1527.51,76375.5]
["","","BRG LGTH STR 980092","",45,1511.46,68015.7]
["","","BRG LGTH STR 980109","",135,1562.88,210988.79999999999]
["0001000000-E","CLEARING & GRUBBING","","",1291,24218.869904718002,31264139.16]
["0005000000-N","GENERIC FERRY ITEM (LS)","CO2 FLOODING SYSTEM","",1,19762,19762]
["","","CRANE SERV & ","LAUNCHING",1,118578,118578]
["","","DELIVERY","",1,158104,158104]
["","","DOORS WINDOWS","",1,39526,39526]
["","","DREDGE BOOM & CUTTR ","HEAD",1,375497,375497]
["","","DREDGE MANEUVERING ","SYSTEM",1,98815,98815]
["","","DREDGE PUMP PIPING","",1,98815,98815]
["","","DREDGE PUMP SKID","",1,750993,750993]
["","","DREDGE RECORDING ","SYSTEM",1,39526,39526]
["","","ELECTRICAL","",1,513837,513837]
["","","ELECTRONICS","",1,189725,189725]
["","","ENGINEERING & NC ","PROGRAMMING",1,988149,988149]
["","","FENDERS","",1,71147,71147]
["","","FIRE SAFETY EQUIP","",1,140712,140712]
["","","GENERATORS","",1,260871,260871]
["","","HULL STL","",1,913049,913049]
["","","HVAC INCLUDING WHEELHOUSE","",1,79052,79052]
["","","HYDRAULIC POWER UNIT","",1,296445,296445]
["","","JOINER","",1,276682,276682]
["","","MACHINERY ALARM ","SYSTEM",1,98815,98815]
["","","MACHINERY ALL EX AS","LISTED SEPARATE",1,750993,750993]
["","","MOBILIZATION","",1,256919,256919]
["","","NAMES & TAGS","",1,2372,2372]
["","","OUTFIT (DECK FITTING ","ONLY)",1,79052,79052]
["","","PAINTING","",1,256128,256128]
["","","PIPING","",1,158104,158104]
["","","POST-DELIVY TRAIN & ","TRIAL RUN",1,79052,79052]
["","","PRE-DELIVY TEST & ","TRIALS",1,79051,79051]
["","","SPUDS & SPUD WELLS","",1,138340,138340]
["","","STABILITY / INCLINING","",1,39526,39526]
["","","STAIRS LADDERS & ","HANDRAILS",1,23715,23715]
["","","SPRSTR & WHEELHOUSE","",1,513837,513837]
["0008000000-E","SUPP CLEAR & GRUBBING","","",62.25,4958.7582329320003,308682.7]
["0015000000-N","SEAL ABANDED WELLS","","",103,1255.4687378640001,129313.28]
["0022000000-E","UNCLAS EXCAV","","",17114550,4.5794709759999996,78375585]
["0029000000-N","REINF BRG APPR **********","(10+0000)","",1,1200,1200]
["","","(122+2250 -L- LT)","",1,40379.39,40379.39]
["","","(122+2250 -L- RT)","",1,43075.45,43075.45]
["","","(123+7225 -L- LT)","",1,45303.3,45303.3]
["","","(123+7225 -L- RT)","",1,45303.3,45303.3]
["","","(125+8560 -L- EB)","",1,52873.89,52873.89]
["","","(126+0804 -L- WB)","",1,52875.19,52875.19]
["","","(129+3756 -L- LT)","",1,22000,22000]
["","","(129+3756 -L- RT)","",1,28000,28000]
["","","(13+5300)","",1,30000,30000]
["","","(13+8500)","",1,6500,6500]
["","","(139+6419 -LDFEB-)","",1,53584.31,53584.31]
["","","(14+1200 -L-)","",1,29540,29540]
["","","(14+9925 -L- LT)","",1,16500,16500]
["","","(144+4179 -L- LT)","",1,23200,23200]
["","","(144+6063 -L- RT)","",1,26000,26000]
["","","(144+9000 -L- LT)","",1,26000,26000]
["","","(145+6797 -L- RT)","",1,23200,23200]
["","","(15+0900)","",1,24000,24000]
["","","(15+6600-L-)","",1,9450,9450]
["","","(15+67-L-)","",1,50000,50000]
["","","(157+7550 -L- EB)","",1,24500,24500]
["","","(157+7550 -L- WB)","",1,24500,24500]
["","","(16+0550-Y2-)","",1,40000,40000]
["","","(16+8314 -Y5-)","",1,42350,42350]
["","","(17+1018-Y4RPA-)","",1,33325.07,33325.07]
["","","(17+27)","",1,12000,12000]
["","","(17+4500-L-)","",1,7400,7400]
["","","(17+6800)","",1,9100,9100]
["","","(18+75)","",1,25000,25000]
["","","(19+1955 -DFLW-)","",1,53584.31,53584.31]
["","","(19+8314 -Y3-)","",1,38000,38000]
["","","(20+0300-L-)","",1,24536.92,24536.92]
["","","(20+2021-Y2-)","",1,24520.42,24520.42]
["","","(20+2050 -L- SBL)","",1,25000,25000]
["","","(20+4750 -L- NBL)","",1,25000,25000]
["","","(20+5261 -Y7-)","",1,39198.269999999997,39198.269999999997]
["","","(20+6720 -L-)","",1,12491.76,12491.76]
["","","(21+6908-Y11- CL)","",1,24000,24000]
["","","(23+2500)","",1,49000,49000]
["","","(23+5425-Y5-)","",1,30113.53,30113.53]
["","","(24+0357 -L- LT)","",1,33221.089999999997,33221.089999999997]
["","","(24+1562 -L- RT)","",1,33245.67,33245.67]
["","","(24+5670 -Y4- CL)","",1,29000,29000]
["","","(247+7914 -L- LT)","",1,25000,25000]
["","","(248+1265 -L- RT)","",1,28000,28000]
["","","(25+5800 -DFFLY-)","",1,20290.97,20290.97]
["","","(26+1600-L-)","",1,12100,12100]
["","","(26+1764 -Y22- LT)","",1,27000,27000]
["","","(26+1764 -Y22- RT)","",1,23000,23000]
["","","(26+2165 -L- LT)","",1,30000,30000]
["","","(26+2165 -L- RT)","",1,1100,1100]
["","","(26+4862-Y4RPBD-)","",1,23124.11,23124.11]
["","","(265+0000 -L- LT)","",1,16600,16600]
["","","(265+0000 -L- RT)","",1,22800,22800]
["","","(27+1172)","",1,85000,85000]
["","","(279+4322 -Y02- EBL)","",1,13000,13000]
["","","(279+4887 -Y02- WBL)","",1,13000,13000]
["","","(28+1707-L-)","",1,54500,54500]
["","","(28+2706 -Y1-)","",1,46000,46000]
["","","(28+7585-Y5-)","",1,25832.639999999999,25832.639999999999]
["","","(281+5183 -L- LT)","",1,11500,11500]
["","","(281+5183 -L- RT)","",1,10800,10800]
["","","(29+7305 -Y9 SBL-)","",1,90000,90000]
["","","(31+6368 -Y7-)","",1,8700,8700]
["","","(33+0710 -Y10-)","",1,63000,63000]
["","","(33+1649-Y4CD-)","",1,22395.83,22395.83]
["","","(339+6919 -L- LT)","",1,51510,51510]
["","","(339+6919 -L- RT)","",1,51510,51510]
["","","(34+0868-Y1-)","",1,65194.06,65194.06]
["","","(34+1049 -Y8 REV-)","",1,27000,27000]
["","","(34+6288 -DFEB-)","",1,10838.89,10838.89]
["","","(340+4708 -L- LT)","",1,27000,27000]
["","","(340+9321 -L- RT)","",1,30000,30000]
["","","(36+6926 -DFWB-)","",1,12897.2,12897.2]
["","","(393+5738-L-)","",1,28000,28000]
["","","(40+4897-Y-)","",1,59000,59000]
["","","(41+9004 -RP1B-)","",1,18000,18000]
["","","(44+1864-Y4RPBD-)","",1,39884.57,39884.57]
["","","(45+0787 -RP1C-)","",1,20650,20650]
["","","(46+2150-L-)","",1,40000,40000]
["","","(46+8344-Y4CD-)","",1,33412.19,33412.19]
["","","(48+79 -Y8-)","",1,9100,9100]
["","","(49+5223 -Y1-)","",1,48000,48000]
["","","(53+2116-Y4RPBD-)","",1,32401.61,32401.61]
["","","(55+9307 -RP1DB-)","",1,26000,26000]
["","","(556+8500-L-LT)","",1,39353.58,39353.58]
["","","(556+8500-L-RT)","",1,39353.58,39353.58]
["","","(584+1777-L-LT)","",1,56961.25,56961.25]
["","","(584+2418-L-RT)","",1,56961.25,56961.25]
["","","(628+5775-L-RT)","",1,51286.93,51286.93]
["","","(628+7447-L-LT)","",1,51286.93,51286.93]
["","","(642+7524-L-LT)","",1,42406.89,42406.89]
["","","(642+8018-L-RT)","",1,52477.65,52477.65]
["","","(67+1650 -L-)","",1,15850,15850]
["","","(71+6063-L-)","",1,19000,19000]
["","","(765+2145 -L- RT)","",1,35000,35000]
["","","(765+3336 -L- LT)","",1,29000,29000]
["","","(826+1499 -L- LT)","",1,28000,28000]
["","","(826+1502 -L- RT)","",1,28000,28000]
["","","(898+0042 -L- RT)","",1,36000,36000]
["","","(898+3937 -L- LT)","",1,36000,36000]
["","","(91+8118 -COL1-)","",1,15000,15000]
["","","(91+8785 -L- RT)","",1,15000,15000]
["","","(91+8869 -L- LT)","",1,15000,15000]
["0030000000-N","BRG APP SUB REG TIER**","(10+5800-L-)","",1,6000,6000]
["","","(11+00-L-)","",1,17000,17000]
["","","(12+00 -L-)","",1,12200,12200]
["","","(12+1950)","",1,36700,36700]
["","","(12+7150-L-)","",1,10000,10000]
["","","(12+8100-L2-)","",1,20000,20000]
["","","(13+0134-L-)","",1,15000,15000]
["","","(14+35)","",1,8100,8100]
["","","(14+6600-L-)","",1,17160,17160]
["","","(14+8343-L-)","",1,8000,8000]
["","","(15+08 -L-)","",1,5000,5000]
["","","(15+1100)","",1,8500,8500]
["","","(15+16-L-)","",1,15000,15000]
["","","(15+6450)","",1,9500,9500]
["","","(16+0250)","",1,10000,10000]
["","","(16+1350)","",1,7000,7000]
["","","(16+2900)","",1,14000,14000]
["","","(16+6429 -L-)","",1,4275,4275]
["","","(16+8350)","",1,10000,10000]
["","","(16+8800 -L-)","",1,7000,7000]
["","","(17+7300 -L-)","",1,10000,10000]
["","","(17+8640 -L-)","",1,7500,7500]
["","","(18+6650 -L-)","",1,10950,10950]
["","","(20+9200)","",1,10000,10000]
["","","(21+77 -L-)","",1,6800,6800]
["","","(24+7018-DFWB-)","",1,12664.61,12664.61]
["","","(32+1850 -L-)","",1,18000,18000]
["0036000000-E","UNDERCUT EXCAV","","",262010,7.9421949539999996,2080934.5]
["0043000000-N","GRADING","","",43,220472.08511627899,9480299.6600000001]
["0050000000-E","SUPP CLEAR & GRUBBING","","",63,883.160634921,55639.12]
["0057000000-E","UNDERCUT EXCAV","","",16540,12.968863362,214505]
["0063000000-N","GRADING","","",21,374907.13761904801,7873049.8899999997]
["0084000000-E","WICK DRNS","","",863000,0.35,302050]
["0098000000-E","PRE-SPLITTING OF ROCK","","",3080,18,55440]
["0106000000-E","BORROW EXCAV","","",12381625,4.7256811189999999,58511611.490000002]
["0127000000-N","EMBM'T SETTLMT GAUGE","","",26,1042.307692308,27100]
["0134000000-E","DRNG DITCH EXCAV","","",335528,4.8885636970000004,1640250]
["0141000000-E","BERM DITCH CONST","","",35040,4.4969320780000004,157572.5]
["0156000000-E","REML OF EXT ASPH PVT","","",661886,2.7056026260000001,1790800.5]
["0163000000-E","REML OF EXT CONC PVT","","",80240,2.2220837489999998,178300]
["0170000000-E","REML OF CONC PVT SLBS","","",4000,65,260000]
["0177000000-E","BREAK OF EXT ASPH PVT","","",120040,2.0631972680000001,247666.2]
["0185000000-E","BREAK OF EXT CONC PVT","","",8400,4.9885714290000003,41904]
["0192000000-N","PROOF ROLLING","","",910.9,194.77538698000001,177420.9]
["0194000000-E","SEL GRAN MATL CL III","","",82230,7.0158093150000003,576910]
["0195000000-E","SEL GRAN MAT'L","","",391730,7.6865506850000003,3011052.5]
["0196000000-E","GEOTEXTILE SOIL STAB","","",653102,1.4524974660000001,948629]
["0199000000-E","TEMP SHORING","","",100198.75,32.434530070999998,3249899.37]
["0220000000-E","ROCK EMBANKMTS","","",4030,44.632754341999998,179870]
["0222000000-E","GEOTEXTILE ROCK EMBANK","","",2370,2.6645569619999998,6315]
["0223000000-E","ROCK PLATING","","",19825,58.114401008999998,1152118]
["0225000000-E","REINF SOIL SLOPES","","",1130,129.621238938,146472]
["0234000000-E","GENERIC GRAD ITEM (CY)","CLAY CORE","",2100,64.209999999999994,134841]
["","","UNDERCUT EXCAV","",1193,29,34597]
["0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR EMBANKMT","STAB",3810,10.706036745,40790]
["","","","STAB 1",69550,13.255930984999999,921950]
["","","","STAB 2",25750,10.397708738,267741]
["","","SOIL NAIL SLOPE STAB","",6000,167.41666666699999,1004500]
["0248000000-N","GENERIC GRAD ITEM (LS)","ENERGY DISSIPATOR ","BASIN",1,3000,3000]
["","","HAZARDOUS SPILL BASIN/","BIORETENTION BASIN",1,4500,4500]
["0255000000-E","GENERC GRAD ITEM(TON)","AGG SHDR BORROW","",48725.16,19.497624430999998,950024.87]
["","","CLEAN SAND","",335,38,12730]
["","","HAULING & DISP OF PETROLEUM ","CONTAMINATED SOIL",2320,147.93103448299999,343200]
["","","HAULING & DISP OF PETROLEUM","CONTAMINATED SOIL",150,65.333333332999999,9800]
["","","HAULING & DISP OF PETROLEUM","CONTAMINATED SOIL",3100,103.238709677,320040]
["","","HAULING & DISP OF PETROLEUM","CONTAMINATED SOIL",380,70.703947368000001,26867.5]
["","","HAULING & DISP OF PETROLEUM","CONTAMINATED SOIL",300,64,19200]
["0257000000-E","GENERIC GRADING ITEM (LF)","HORIZONTAL INCLINOMETER CASING","",270,9,2430]
["","","REM & REPL 2'-6\" CURB & ","GTR",200,50,10000]
["0262000000-N","GENERIC GRADING ITEM (EA)","HAZARDOUS SPILL BASIN/","BIORETENTION BASIN",1,67000,67000]
["","","SOIL NAIL PROOF TESTS","",26,497.11538461499998,12925]
["","","SOIL NAIL VERIFICATION TESTS","",26,507.5,13195]
["","","VW PIEZOMETER","",16,1962.5,31400]
["0264000000-E","GENERIC GRADING ITEM (SMI)","SHDR GRADING","",95.59,3022.901663354,288959.17]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",74074,28.934747144999999,2143312.46]
["0320000000-E","FND CONDIT GEOTEXTILE","","",216169,2.2133044050000001,478447.8]
["0331000000-E","GENERIC DRNG ITEM (CY)","FILTER DIAPHRAGM","",20,64.209999999999994,1284.2]
["0335000000-E","**\" DRNG PIPE","(30\")","",188,50,9400]
["0335100000-E","12\" DRNG PIPE","","",52,30,1560]
["0335200000-E","15\" DRNG PIPE","","",8954,29.729336609000001,266196.47999999998]
["0335300000-E","18\" DRNG PIPE","","",3716,33.337545747999997,123882.32]
["0335400000-E","24\" DRNG PIPE","","",1624,40.628571428999997,65980.800000000003]
["0335500000-E","30\" DRNG PIPE","","",840,54.812857143000002,46042.8]
["0335600000-E","36\" DRNG PIPE","","",464,72.387931034000005,33588]
["0335800000-E","48\" DRNG PIPE","","",56,104.285714286,5840]
["0335850000-E","**\" DRNG PIPE ELB","(15\")","",57,240.52631578899999,13710]
["","","(18\")","",3,175,525]
["","","(24\")","",14,371.42857142899999,5200]
["","","(30\")","",6,350,2100]
["","","(36\")","",2,500,1000]
["0342000000-E","**\" SIDE DRN PIPE","(12\")","",290,27.850827586000001,8076.74]
["","","(30\")","",13892,53.728137056999998,746391.28]
["","","(36\")","",5028,70.229546538999998,353114.16]
["","","(42\")","",4030,77.026808932999998,310418.03999999998]
["","","(48\")","",368,126.875326087,46690.12]
["","","(54\")","",84,371.66,31219.439999999999]
["","","(6\")","",20,25,500]
["","","(60\")","",604,198.4,119833.60000000001]
["0343000000-E","15\" SIDE DRN PIPE","","",77126,33.402752120000002,2576220.66]
["0344000000-E","18\" SIDE DRN PIPE","","",25774,34.746102274000002,895546.04]
["0345000000-E","24\" SIDE DRN PIPE","","",24546,46.237130286000003,1134936.6000000001]
["0348000000-E","**\" SIDE DRN PIPE ELB","(15\")","",370,286.24556756800001,105910.86]
["","","(18\")","",107,373.36691588799999,39950.26]
["","","(24\")","",33,555.11272727300002,18318.72]
["","","(30\")","",15,709.33,10639.95]
["","","(36\")","",4,725.27499999999998,2901.1]
["0350000000-E","***\" RC PIPE CULV CONTR DESIGN","(18\")","",484,21.95,10623.8]
["","","(24\")","",244,103.71,25305.24]
["","","(36\")","",380,78.03,29651.4]
["","","(42\")","",1308,93.45,122232.6]
["","","(48\")","",1276,110.3,140742.79999999999]
["","","(54\")","",356,320,113920]
["","","(60\")","",308,179.73,55356.84]
["0354000000-E","***\" RC PIPE CULV *****","(12\" V)","",1000,29.033000000000001,29033]
["","","(15\" V)","",5532,29.419739696000001,162750]
["","","(18\" V)","",1216,55.450361842,67427.64]
["","","(24\" V)","",926,61.108855292000001,56586.8]
["","","(30\" V)","",2732,89.163469985000006,243594.6]
["","","(36\" V)","",1576,96.188883249,151593.68]
["","","(42\" V)","",308,132.766233766,40892]
["","","(48\" V)","",544,172.676470588,93936]
["","","(54\" V)","",444,183.828378378,81619.8]
["","","(60\" V)","",444,241.52207207199999,107235.8]
["","","(66\" V)","",880,290.72727272700001,255840]
["","","(72\" V)","",324,279.60000000000002,90590.399999999994]
["0360000000-E","12\" RC PIPE CULV III","","",988,27.360728744999999,27032.400000000001]
["0366000000-E","15\" RC PIPE CULV III","","",50228,30.766175440000001,1545323.46]
["0372000000-E","18\" RC PIPE CULV III","","",37406,35.548963268000001,1329744.52]
["0378000000-E","24\" RC PIPE CULV III","","",27782,43.976222014000001,1221747.3999999999]
["0384000000-E","30\" RC PIPE CULV III","","",16016,74.687147851999995,1196189.3600000001]
["0390000000-E","36\" RC PIPE CULV III","","",12680,77.021283912000001,976629.88]
["0396000000-E","42\" RC PIPE CULV III","","",6732,90.015442661999998,605983.96]
["0402000000-E","48\" RC PIPE CULV III","","",3760,114.733680851,431398.64]
["0408000000-E","54\" RC PIPE CULV III","","",2728,158.69281524900001,432914]
["0414000000-E","60\" RC PIPE CULV III","","",1404,225.89558404600001,317157.40000000002]
["0420000000-E","66\" RC PIPE CULV III","","",1468,303.47138964599998,445496]
["0426000000-E","72\" RC PIPE CULV III","","",804,284.93159204,229085]
["0448000000-E","***\" RCP CULV CL IV","(12\")","",436,37.963302751999997,16552]
["","","(48\")","",4936,178.12799027599999,879239.76]
["","","(54\")","",2172,178.99771638999999,388783.04]
["","","(60\")","",3604,228.83207547200001,824710.8]
["","","(66\")","",1556,269.20308483299999,418880]
["","","(72\")","",368,412.17391304300003,151680]
["","","(84\")","",180,499,89820]
["0448200000-E","15\" RCP CULV CL IV","","",95264,36.562876637999999,3483125.88]
["0448300000-E","18\" RCP CULV CL IV","","",23110,39.178251838999998,905409.4]
["0448400000-E","24\" RCP CULV CL IV","","",16274,51.876959567,844245.64]
["0448500000-E","30\" RCP CULV CL IV","","",10350,84.702206763000007,876667.84]
["0448600000-E","36\" RCP CULV CL IV","","",8756,109.211151211,956252.84]
["0448700000-E","42\" RCP CULV CL IV","","",2828,118.309024045,334577.91999999998]
["0453000000-E","**\" PIPE END SECTION","(15\")","",16,731.703125,11707.25]
["","","(18\")","",35,689.43028571399998,24130.06]
["","","(24\")","",13,805,10465]
["","","(30\")","",8,990,7920]
["0542000000-E","**\" PVC PIPE CLVTS","(8\")","",10,500,5000]
["0546000000-E","**\" CAA PIPE CLVT *****\"","(18\" 0064\")","",788,33.502538070999996,26400]
["","","(4\" 0064\")","",56,27,1512]
["","","(54\" 0109\")","",28,216,6048]
["","","(60\" 0105\")","",144,718,103392]
["","","(84\" 0105\")","",192,335,64320]
["0564000000-E","**\" CAA PIPE ELB *****\"","(18\" 0064\")","",14,270,3780]
["0570000000-E","6\" CS PIPE 0064\" SPR BOX","","",8,80,640]
["0576000000-E","**\" CS PIPE CULV *****\"","(12\" 0064\")","",272,40.783235294000001,11093.04]
["","","(120\" 0138\")","",104,525,54600]
["","","(30\" 0138\")","",328,65,21320]
["","","(36\" 0079\")","",1056,97.468106061,102926.32]
["","","(42\" 0109\")","",244,118.573114754,28931.84]
["","","(48\" 0109\")","",36,230.69,8304.84]
["","","(54\" 0109\")","",280,141.82928571400001,39712.199999999997]
["","","(60\" 0138\")","",470,240.359276596,112968.86]
["","","(96\" 0168\")","",80,415,33200]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",10812,38.008479467000001,410947.68]
["0588000000-E","18\" CS PIPE CULV 0064\"","","",4506,47.165454949000001,212527.54]
["0594000000-E","24\" CS PIPE CULV 0064\"","","",3206,63.396768559000002,203250.04]
["0600000000-E","30\" CS PIPE CULV 0079\"","","",2084,70.397907868999994,146709.24]
["0636000000-E","**\" CS ELB *****\" TK","(15\" 0064\")","",88,287.40272727299998,25291.439999999999]
["","","(15\" 0064)","",91,563.27076923100003,51257.64]
["","","(18\" 0064)","",16,646.94000000000005,10351.040000000001]
["","","(18\" 0064\")","",28,346.23642857099998,9694.6200000000008]
["","","(24\" 0064)","",34,938.26,31900.84]
["","","(24\" 0064\")","",12,463.11,5557.32]
["","","(30\" 0079)","",16,1246.19,19939.04]
["","","(30\" 0079\")","",11,636.03636363600003,6996.4]
["","","(30\" 0138\")","",3,900,2700]
["","","(36\" 0079)","",10,1591.8,15918]
["","","(42\" 0109\")","",1,476.47,476.47]
["0654000000-E","***X***\"CSP ARCH CULV *****","(77\" X 52\" 0109\")","",80,205,16400]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\" 0500\")","",44,470,20680]
["","","(18\" 0250\")","",130,430,55900]
["","","(18\" 0500\")","",40,488,19520]
["","","(24\" 0250\")","",124,610,75640]
["","","(24\" 0500\")","",828,348.49724637700001,288555.71999999997]
["","","(30\" 0500\")","",839,347.23713945200001,291331.96000000002]
["","","(36\" 0500\")","",331,456.62365558900001,151142.43]
["","","(42\" 0625\")","",420,533.17371428599995,223932.96]
["","","(48\" 0625\")","",280,686.99285714300004,192358]
["","","(54\" 0750\")","",88,714,62832]
["","","(54\" 0875\")","",133,753.84,100260.72]
["","","(60\" 0875\")","",138,948.57217391300003,130902.96]
["","","(66\" 0875\")","",155,1205.28,186818.4]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\" 0500\")","",16,25,400]
["","","(18\" 0250\")","",50,725,36250]
["","","(18\" 0500\")","",16,25,400]
["","","(24\" 05\")","",76,875,66500]
["","","(24\" 0250\")","",124,710,88040]
["","","(24\" 0500\")","",544,713.72007352900005,388263.72]
["","","(30\" 05\")","",131,1120,146720]
["","","(30\" 0500\")","",342,640.98795321600005,219217.88]
["","","(36\" 05\")","",16,1540,24640]
["","","(36\" 0500\")","",283,953.18879858699995,269752.43]
["","","(42\" 0625\")","",420,1135.2537142860001,476806.56]
["","","(48\" 0625\")","",280,1205.6428571429999,337580]
["","","(54\" 0750\")","",88,775,68200]
["","","(54\" 0875\")","",133,1368.07,181953.31]
["","","(60\" 0875\")","",58,1572.12,91182.96]
["","","(60: 0875\")","",80,775,62000]
["","","(66\" 0875\")","",155,1555.28,241068.4]
["0974000000-E","**\"WLD STL PIPE ***\" B RR","(24\" 0312\")","",56,285,15960]
["","","(36\" 05\")","",130,229.4,29822]
["","","(42\" 0625\")","",56,565,31640]
["0986000000-E","GENERIC PIPE ITEM (LF)","15\" CS SLOTTED DRN 0064\" TK","",96,177.64,17053.439999999999]
["","","15\" DUCTILE IRON PIPE","",1020,80.7,82314]
["","","18\" DUCTILE IRON PIPE","",448,88.8,39782.400000000001]
["","","24\" DUCTILE IRON PIPE","",460,140.5,64630]
["","","24\" WELDED STL PIPE 0500\"","TK GRADE B OPEN CUT",20,117.5,2350]
["","","30\" CCFRPM PIPE","",208,650,135200]
["","","36\" DUCTILE IRON PIPE","",240,355.9,85416]
["","","42\" CCFRPM PIPE","",68,750,51000]
["","","48\" DUCTILE IRON PIPE","",12,697.1,8365.2000000000007]
["","","54\" CCFRPM PIPE","",64,1000,64000]
["","","54\" WELDED STL PIPE ","LINER",244,820.43,200184.92]
["","","8\" DUCTILE IRON PIPE","",548,36,19728]
["","","NCDOT APPROVED PIPE ","LINER",253,1275,322575]
["0992000000-E","GENERIC PIPE ITEM (EA)","15\" DUCTILE IRON PIPE ","ELB",2,1737.5,3475]
["0995000000-E","PIPE REML","","",77628.399999999994,11.727914010999999,910419.2]
["0996000000-N","PIPE CLEAN-OUT","","",5,2518,12590]
["1000000000-E","6\" SLOPE PROTECTION","","",1930,95.160621762000005,183660]
["1011000000-N","FINE GRADING","","",20,865903.34,17318066.800000001]
["1044000000-E","LIME TRTD SOIL (SLURY)","","",714920,2.4448343870000002,1747861]
["1066000000-E","LIME FOR LIME TRTD SOIL","","",7240,206.59908839799999,1495777.4]
["1077000000-E","#57 STONE","","",2932,34.739427012,101856]
["1099500000-E","SHALLOW UNDERCUT","","",54860,9.1805058329999998,503642.55]
["1099700000-E","CL IV SUBGRD STAB","","",102715,24.003446429,2465514]
["1110000000-E","STABILIZER AGG","","",7250,23.724137931000001,172000]
["1111000000-E","CL IV AGG STAB","","",33850,25.757754801000001,871900]
["1115000000-E","GEOTEXTILE FOR PVT STABILIZ","","",673429,2.8163372089999998,1896603.15]
["1121000000-E","AGG BASE CRS","","",1522137,21.737850338000001,33087986.300000001]
["1176000000-E","SOIL CEMT BASE","","",714950,2.211372404,1581020.7]
["1187000000-E","PC FOR SOIL CEMT BASE","","",19764,140.00654978700001,2767089.45]
["1209000000-E","ASPH CURING SEAL","","",214500,2.8992051280000002,621879.5]
["1220000000-E","INCIDENTAL STONE BASE","","",111814,25.443826353999999,2844976]
["1231000000-E","SHDR BORROW","","",264306,3.6123599159999999,954768.4]
["1243000000-E","SHDR CONST","","",6.5,2541.0461538459999,16516.8]
["1245000000-E","SHDR RECONST","","",1551.54,2055.8765742420001,3189774.74]
["1275000000-E","PRIME COAT","","",64729,3.9134636719999998,253314.59]
["1297000000-E","MILL ASP PVT *****\" DTH","(1\")","",973,6.5034943470000002,6327.9]
["","","(1-1/2\")","",2683658,1.0515810400000001,2822083.87]
["","","(1-1/4\")","",41698,1.6602379009999999,69228.600000000006]
["","","(14\")","",3345,11.7,39136.5]
["","","(2\")","",935153,0.68126231800000003,637084.5]
["","","(2-1/2\")","",375219,1.0644255220000001,399392.68]
["","","(25\")","",82200,1.6,131520]
["","","(3\")","",405176,2.1899237619999998,887304.55]
["","","(3/4\")","",96500,0.9,86850]
["","","(4\")","",5865,2,11730]
["","","(5\")","",310,73.03,22639.3]
["","","(5-1/2\")","",170,17,2890]
["","","(5/8\")","",234243,1.203642713,281944.88]
["1308000000-E","MILL ASPH PVT ***** - *****","(0\" TO 1 1/2\")","",20640,1.66,34262.400000000001]
["","","(0\" TO 1\")","",1626,1.95,3170.7]
["","","(0\" TO 1-1/2\")","",427517,1.675059284,716116.32]
["","","(0\" TO 1-1/4\")","",2940,1.75,5145]
["","","(0\" TO 2\")","",21987,2.1247851,46717.65]
["","","(0\" TO 2-1/2\")","",400,8.5,3400]
["","","(0\" TO 3\")","",37428,2.2130811160000001,82831.199999999997]
["","","(0\" TO 4-1/2\")","",50908,2,101816]
["","","(0\" TO 5-1/2\")","",420,12.4,5208]
["","","(1-1/2\" TO 2-1/2\")","",116046,1.0732666360000001,124548.3]
["","","(1-1/2\" TO 3\")","",44064,1.5145034500000001,66735.08]
["","","(1-1/2\" TO 3-1/2\")","",41710,1.52,63399.199999999997]
["","","(2-1/2\" TO 4\")","",400,8.5,3400]
["","","(3\" TO 6\")","",21138,2.7,57072.6]
["1330000000-E","INCIDENTAL MILLING","","",321532,5.6159518799999999,1805708.24]
["1489000000-E","ASP CONC BASE CRS B250B","","",325455,41.908634896000002,13639374.77]
["1491000000-E","ASP CONC BASE CRS B250C","","",539384,36.396470825999998,19631674.02]
["1498000000-E","ASP CNC INTR CRS I190B","","",352958,38.658422674000001,13644799.550000001]
["1503000000-E","ASP CNC INTR CRS I190C","","",598515,35.163915273999997,21046130.75]
["1508000000-E","ASP CNC INTR CRS I190D","","",5760,39.1,225216]
["1519000000-E","ASP CONC SURF CRS S95B","","",1277841,35.328919974999998,45144742.43]
["1520000000-E","ASP CONC SURF CRS S95B LEVEL","","",24010,33.706813828000001,809300.6]
["1523000000-E","ASP CONC SURF CRS S95C","","",862427,35.185074876000002,30344558.57]
["1524000000-E","ASP CONC SURF CRS S95C LEVEL","","",10201,34.177541417999997,348645.1]
["1524200000-E","ASP CONC SURF CRS S95D","","",43990,40.597885882999996,1785901]
["1525000000-E","ASP CONC SURF CRS SF95A","","",516701,38.056602599999998,19663884.620000001]
["1525100000-E","ASP CONC SURF CRS SF95A LEVEL","","",7140,49.339285713999999,352282.5]
["1526000000-E","ASP CONC SURF CRS S475A","","",6345,47.305484634000003,300153.3]
["1527000000-E","ASP CNC SURF CRS SA-1","","",631,58.35,36818.85]
["1575000000-E","ASP FOR PLANT MIX","","",249892.5,594.01671918900001,148440323]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",3463,780.68004620299996,2703495]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",350,72.928571429000002,25525]
["1682000000-E","PERM ASP DRNG CO P-57","","",18000,43,774000]
["1693000000-E","ASPH PLT MIX PVT REP","","",15497,148.82433696800001,2306330.75]
["1704000000-E","PATCHING EXIST PVT","","",152294,92.985168818000005,14161083.300000001]
["1771000000-E","AST MAT CT #6M STONE","","",605197,1.285147002,777767.11]
["1775000000-E","AST MAT CT #78M STONE","","",587798,1.0449387029999999,614212.88]
["1814000000-E","AST STRAIGHT SEAL","","",45310,1.1200000000000001,50747.199999999997]
["1839000000-E","GENERIC PAV ITEM (660)","ASPH SURF TRTMT MAT","COAT 67 STONE",165908,1.1589970350000001,192286.88]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",17733,45.612840466999998,808852.5]
["1839200000-E","APPLIC OF ULTRATHIN HOT MIX ASPH","","",512714,1.800282809,923030.2]
["1840000000-E","MILLED RUMBLE STRIPS","","",1440049,0.18310042200000001,263673.58]
["1847000000-E","******\"PCC PVT THRU LNS","(10\")","",137500,42,5775000]
["","","(12\")","",65610,64.131229994999998,4207650]
["","","(12-1/2\")","",257000,60,15420000]
["","","(8-1/2\")","",232,68,15776]
["1858000000-E","******\"PCC PVT RAMPS","(11-1/2\")","",41250,72,2970000]
["","","(12\")","",2000,68,136000]
["1869000000-E","******\"PCC PVT MISC","(12\")","",2477,69,170913]
["","","(12-1/2\")","",11000,80,880000]
["1880000000-E","GENERIC PAV ITEM (TON)","AGG SHDR BORROW","",4701,21.6,101541.6]
["","","PATCHING EXT PVT","(FULL DEPTH)",1915,129,247035]
["","","","I190C (MILL)",1612,126.05,203192.6]
["","","","S95B(FULL DEPTH)",25,151.94999999999999,3798.75]
["","","","S95B (MILL)",887,150,133050]
["","","PATCHING EXT PVT(MILL)","",2245,127.9,287135.5]
["","","STABILIZER AGG","",500,30,15000]
["1881000000-E","GENERIC PAV ITEM (LF)","MILLED RUMBLE STRIPS","(CONC SHLD)",41100,0.5,20550]
["","","MILLED RUMBLE STRIPS ","(CONCSHDR)",83000,1,83000]
["","","PEDESTRIAN SAFETY ","RAIL",120,52,6240]
["","","SPEED MODULATOR","",65,55,3575]
["1891000000-E","GENERIC PAV ITEM (SY)","6\" JOINTED CONC ","GREENWAY",400,48,19200]
["","","6\" JOINTED CONC W/","WIRE MESH (4X4 W3XW3)",470,54,25380]
["","","DIAMOND GRINDING PCC ","PVT",131000,2.25,294750]
["","","FINE MILLING","",122500,1.3213387759999999,161864]
["","","NONWOVEN GEOTEXTILE ","INTERLAYER",50000,2.2120000000000002,110600]
["","","PVT INTERLAYER","",114591,5.3,607332.30000000005]
["","","REP OF JOINTED CONC","PVT SLAB",3145,250,786250]
["","","","PVT SLABS",8500,215,1827500]
["1892000000-E","GENERIC PAV ITEM (SY) 710","VARIABLE DEPTH CONC SHLD ADJA-","CENT TO 10\" PVT - MIN 7\" TKNESS",50700,34,1723800]
["1902000000-N","SURF TEST CONC PVT","","",4,88875,355500]
["1913000000-E","CONC SHLD ADJ *****\"PVT","(10\")","",22400,34,761600]
["","","(12-1/2\")","",51000,57.5,2932500]
["1924000000-N","FIELD LAB RENTAL PCCP","","",4,57100,228400]
["2000000000-N","RIGHT OF WAY MARKERS","","",3034,156.201384311,473915]
["2020000000-N","CNTRL OF ACCESS MKRS","","",51,145.88235294099999,7440]
["2022000000-E","SUBDRN EXCAV","","",61371.9,19.908696325000001,1221834.52]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",53510,3.6272098669999999,194092]
["2033000000-E","SUBDRN FINE AGG","","",26561.1,52.559831105999997,1396046.93]
["2036000000-E","SUBDRN CRS AGG","","",9003.5,52.012761703999999,468296.9]
["2043000000-E","4\" PERF SUBDRN PIPE","","",25810,7.8,201318]
["2044000000-E","6\" PERF SUBDRN PIPE","","",184444,10.715997809999999,1976501.5]
["2070000000-N","SUBDRN PIPE OUTLET","","",449,344.18195991099998,154537.70000000001]
["2076000000-E","4\" OUTLET PIPE","","",312,22.06,6882.72]
["2077000000-E","6\" OUTLET PIPE","","",2382,29.868337531000002,71146.38]
["2099000000-E","SHDR DRN","","",144400,6.3773545709999997,920890]
["2110000000-E","4\" SHDR DRN PIPE","","",144400,1.657652355,239365]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",7890,9.4129911279999998,74268.5]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",166,308.98192771100003,51291]
["2143000000-E","BLOTTING SAND","","",110,60.338181818000002,6637.2]
["2165000000-E","12\" FUNNEL DRN PIPE","","",24,100,2400]
["2176000000-E","12\" FUNNEL DRN ELBS","","",1,500,500]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",224,704.94419642900004,157907.5]
["2199000000-E","SANDBAG HEADWALLS","","",355,15,5325]
["2209000000-E","ENDWALLS","","",658.64599999999996,890.300707816,586393]
["2220000000-E","REINF ENDWALLS","","",441.8,1023.153779991,452029.34]
["2253000000-E","PIPE COLLARS","","",97.650999999999996,806.80382177299998,78785.2]
["2264000000-E","PIPE PLUGS","","",23.623999999999999,998.67634608900005,23592.73]
["2275000000-E","FLOWABLE FILL","","",1773.05,169.58439412300001,300681.61]
["2286000000-N","MASNRY DRNG STR","","",4673,1245.295775733,5819267.1600000001]
["2297000000-E","MASNRY DRNG STR","","",447.495,1077.7755282180001,482299.16]
["2308000000-E","MASNRY DRNG STR","","",2484.7800000000002,242.29895604399999,602059.6]
["2352000000-N","FRM W/GRT 840***** STD","(84016)","",35,575,20125]
["","","(84020)","",8,600,4800]
["2354000000-N","FRM W/GRT 84022 STD","","",47,507.20425531900003,23838.6]
["2354200000-N","FRM W/GRT 84024 STD","","",12,556.08333333300004,6673]
["2355000000-N","FRM W/GRT 84029 STD","","",4,512.5,2050]
["2363000000-N","FRM W/2GRTS 840***** STD","(84033)","",20,481.25,9625]
["2364000000-N","FRM W/2GRTS 84016 STD","","",281,498.406939502,140052.35]
["2364200000-N","FRM W/2GRTS 84020 STD","","",467,527.61648822300003,246396.9]
["2365000000-N","FRM W/2GRTS 84022 STD","","",1194,579.61586264699997,692061.34]
["2366000000-N","FRM W/2GRTS 84024 STD","","",460,586.93478260899997,269990]
["2367000000-N","FRM W/2GRTS 84029 STD","","",395,495.57073417700002,195750.44]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",179,531.76787709500002,95186.45]
["","","(F)","",538,539.48299256500002,290241.84999999998]
["","","(G)","",545,538.75522935799995,293621.59999999998]
["2396000000-N","FRM W/COVER STD 84054","","",228,395.10666666700001,90084.32]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",90,1387.8488888889999,124906.4]
["2418000000-E","FRM W/GRTS DRIVEWY DI","","",74,220.27027027,16300]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",101,597.66336633699996,60364]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",268,646.33694029900005,173218.3]
["2462000000-E","**\" SLUICE GATE","(18\")","",4,3500,14000]
["","","(24\")","",2,3600,7200]
["","","(30\")","",2,4900,9800]
["","","(36\")","",4,5312.5,21250]
["","","(42\")","",1,7800,7800]
["","","(48\")","",1,9800,9800]
["","","(6\")","",2,2532.5,5065]
["","","(8\")","",4,1000,4000]
["2473000000-N","GENERIC DRNG ITEM (EA)","BICYCL SAFE STL FRM & ","GRT",4,1456.25,5825]
["","","OIL / H2O SEPARATOR","",1,88000,88000]
["","","RETICULINE FRM & GRT","",2,7000,14000]
["","","RETICULINE FRM & GRT","",2,4650,9300]
["","","RIPRAP ENERGY ","DISSIPATOR BASIN",6,2850,17100]
["","","TRASH RACK","",1,1200,1200]
["2474000000-N","GENERIC DRNG ITEM (LS)","LEVEL SPREADER W/ ","VEGETATED TROUGH",1,15000,15000]
["2484000000-E","GENERIC DRNG ITEM (LF)","4\" PERF OR SLOT DRN","PIPE W/ GEOTEXTILE SOCK",18,19,342]
["","","4\" SOLID DRN PIPE","",50,26,1300]
["","","SHDR BERM CURB","",10,58,580]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",1000,18.055,18055]
["","","(8\" X 18\")","",1375,17.943636364,24672.5]
["","","(9\" X 12\")","",1390,12.25,17027.5]
["","","(9\" X 18\")","",1700,20.126470588,34215]
["2538000000-E","**'-**\" CONC CURB & GTR","(2'-0\")","",120,23,2760]
["","","(2'-9\")","",49540,16.160587404000001,800595.5]
["2542000000-E","1'-6\" CONC CURB & GTR","","",104180,13.707508159,1428048.2]
["2549000000-E","2'-6\" CONC CURB & GTR","","",207590,15.693111181000001,3257732.95]
["2556000000-E","SHDR BERM GTR","","",124112,18.667735997000001,2316890.0499999998]
["2570000000-N","MOD CONC FLUME","","",14,1178.5714285710001,16500]
["2577000000-E","CONC EXPRESSWAY GTR","","",25790,19.769183792,509847.25]
["2580000000-E","CONC VALLEY GTR","","",770,22.627402597,17423.099999999999]
["2591000000-E","4\" CONC SIDEWALK","","",56625,28.297799558000001,1602362.9]
["2600000000-N","RETROFIT EXT CURB RMP","","",294,423.350408163,124465.02]
["2605000000-N","CONC CURB RAMP","","",1108,1432.0627978340001,1586725.58]
["2612000000-E","6\" CONC DRIVEWAY","","",12115,53.090004127,643185.4]
["2619000000-E","4\" CONC PAVED DITCH","","",3691,58.675182876999997,216570.1]
["2627000000-E","4\" CONC ISL& COVER","","",3555,36.618846695000002,130180]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",21695,42.536483060999998,922829]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",26929,45.297783058999997,1219824]
["2703000000-E","CONC BARR ******","(III)","",145,350,50750]
["","","(IV)","",2025,56.814888889000002,115050.15]
["","","(T1)","",270,120,32400]
["2710000000-N","CONC BARR TRANS SECTN","","",8,16689.400000000001,133515.20000000001]
["2717000000-E","VAR HT CONC BARR ****","(II)","",540,142.5,76950]
["","","(III)","",2800,117.45,328860]
["","","(T1)","",2221,112.724448447,250361]
["","","(T2)","",397,215.26196473600001,85459]
["2724000000-E","PC REINF BARR SNGL FC","","",38388,68.173778264000006,2617055]
["2738000000-E","GENERIC PAV ITEM (SY)","3' x 6\" CONC PAD","",230,46.5,10695]
["","","7\" CONC TRUCK APRON","",1525,37.032786885,56475]
["","","8\" CONC TRUCK APRON","",864,96,82944]
["2739000000-E","GENERIC PAV ITEM 852 (SY)","REML OF CONC ISLAND","",60,101.1,6066]
["2752000000-E","GENERIC PAV ITEM (LF)","1'-6\" MOD CURB & GTR","",4930,21,103530]
["","","6\" CONC CURB","",1310,21,27510]
["","","DDI BARR","",920,400,368000]
["","","MEDIAN HAZARD PROTECTION","",410,300,123000]
["","","SPEC SHDR BERM","CURB",10,60,600]
["","","SPEC SHDR BERM CURB","",46,49.456521739000003,2275]
["2753000000-E","GENERIC PAV ITEM 846 (LF)","18\" CONC CURB & GTR","",2510,14,35140]
["","","2'-0\" CURB & GTR REM & ","REPL",400,45.7,18280]
["","","2'-6\" CURB & GTR REM & ","REPL",390,47.05,18349.5]
["","","SPEC SHDR BERM GTR","",1963,20.25,39750.75]
["2759000000-N","GENERIC PAV ITEM (EA)","ADJUST MONUMTS","",48,351.85,16888.8]
["","","CONC BARR TRANSITION","",1,13000,13000]
["","","EMERGENCY VEH ","ACCESS",1,5800,5800]
["","","REM & REPL CURB RAMP","",2,1700,3400]
["2800000000-N","ADJ CATCH BASINS","","",28,960.04642857099998,26881.3]
["2815000000-N","ADJ DROP INLETS","","",103,700.74854368900003,72177.100000000006]
["2830000000-N","ADJ MHS","","",1418,572.93538787,812422.38]
["2845000000-N","ADJ METER OR VAL BOX","","",1433,502.83298674100001,720559.67]
["2860000000-N","CONV CB TO JB","","",5,965,4825]
["2875000000-N","CONV CB TO DI","","",5,1500,7500]
["2893000000-N","CONV CB TO JB W/MH","","",3,1735.6666666670001,5207]
["2905000000-N","CONV DI TO JB","","",4,1836.41,7345.64]
["2910000000-N","CONV TRAF BR DI TO TRAF BR JB","","",3,1253.3333333329999,3760]
["2920000000-N","CONV DI TO CB","","",2,961.91,1923.82]
["2938000000-N","CONV DI TO JB W/MH","","",9,1512.52,13612.68]
["2950000000-N","CONV JB TO DI","","",1,800,800]
["2965000000-N","CONV JB TO CB","","",1,850,850]
["2995000000-N","GENERIC DRNG ITEM (EA)","CONV EXT OTCB TO 2GI","",14,750,10500]
["","","CONV EXT TRAF BEAR-ING DROP","INLET TO TRAF BEAR JUNCT BOX",1,1578,1578]
["","","CONV EXT CATCH BASIN TO","TRAF BEARG JUNCT BOX W/ MH",6,1384.1,8304.6]
["3000000000-N","IMPACT ATTEN 350","","",82,13752.804878049001,1127730]
["3030000000-E","STL BM GRDRL","","",525322,14.664067239,7703357.1299999999]
["3045000000-E","SBGR SHOP CRV","","",11030.97,16.193442644000001,178629.38]
["3090000000-N","TRIPLE CORRU GR TERM SECT","","",4,150,600]
["3105000000-N","SBGR TERM SECT","","",64,52.803125000000001,3379.4]
["3150000000-N","ADDIT GRDRL POSTS","","",1131,32.141467728000002,36352]
["3165000000-N","GR ANCH **********","(350 TL-2)","",22,1932.5,42515]
["","","(350 TL-2)","",15,1674.8666666669999,25123]
["","","(TL-2)","",22,1785,39270]
["3180000000-N","GR ANCH **********","(B-77 SHOP CRV)","",2,1875,3750]
["","","(III - SHOP CRV)","",4,1450,5800]
["","","(III SHOP CRV)","",5,1702,8510]
["","","(III-MOD)","",7,2000,14000]
["","","(T-101)","",4,2550,10200]
["","","(W-BEAM)","",5,500,2500]
["3195000000-N","GR ANCH AT-1","","",50,497.19799999999998,24859.9]
["3210000000-N","GR ANCH CAT-1","","",416,454.63180288500001,189126.83]
["3215000000-N","GR ANCH III","","",198,1401.9595959599999,277588]
["3270000000-N","GR ANCH 350","(350 TL-3)","",4,1775,7100]
["","","","",908,1788.4746916300001,1623935.02]
["3285000000-N","GR ANCH M-350","","",102,1605.741176471,163785.60000000001]
["3317000000-N","GR ANCH B-77","","",442,1460.424208145,645507.5]
["3345000000-E","REM & RESET GRDRL","","",85143,4.7771455080000003,406740.5]
["3360000000-E","REM EXT GRDRL","","",252587,1.0672074970000001,269562.74]
["3365000000-E","REM EXT GDRL","","",6330,1,6330]
["3380000000-E","TEMP STL BM GRDRL","","",24700,5.850961538,144518.75]
["3382000000-E","TEMP STL BM GDRAIL SHP CURV","","",600,8.3208333329999995,4992.5]
["3387000000-N","TMP GDRL ANCH UNITS **","(350 TL-2)","",4,1100,4400]
["","","(AT-1)","",7,285.71428571400003,2000]
["","","(B-77 SHOP CRV)","",1,950,950]
["","","(B-77)","",17,923.52941176499996,15700]
["","","(CAT-1)","",22,205.90909090900001,4530]
["","","(III)","",17,852.94117647099995,14500]
["","","(TEMP RETROFIT)","",2,1500,3000]
["","","(W-BEAM)","",4,743.5,2974]
["","","(W-BEAM SHOP CRV)","",1,925,925]
["3389000000-N","TMP GDRL ANCH UNITS **","(350 TL-2)","",10,925,9250]
["","","(M-350)","",1,515,515]
["3389100000-N","TMP GDRL ANCH UNIT350","","",75,915.38666666699999,68654]
["3389200000-E","CABLE GDRL","","",65960,7.0027289269999997,461900]
["3389400000-E","DBL FACED CABLE GDRL","","",61456,7.0129312029999999,430986.7]
["3389500000-N","ADDITIONAL GDRL POSTS","","",136,38.823529411999999,5280]
["3389600000-N","CBL GDRL ANCH UNIT","","",163,1556.812208589,253760.39]
["3420000000-E","GENERIC GRDRL ITEM (LF)","WEATHERING STL BEAM GUARD-","RAIL W/ PAINTED LAPS",150,21.5,3225]
["","","","RAIL W/ PAINTED LAPS SHOP CRV",81.25,21.500061538000001,1746.88]
["3435000000-N","GENERIC GRDRL ITEM(EA)","EXTRA LGTH GRDRL ","POST (8' STL)",20,81,1620]
["","","EXTRA LGTH GRDRL ","POSTS (8' STL)",102,75,7650]
["","","IMPACT ATTENUATR UNIT","350 (TEMP)",1,12000,12000]
["","","IMPACT ATTENUATR UNIT","350 (TEMP)",2,5500,11000]
["","","PAINTED GRDRL ANCH","UNITS 350",1,1160,1160]
["","","TMP IMPACT ATTENUATR ","UNIT 350",2,13500,27000]
["","","WEATHERING SB GRDRL ANCH","UNITS AT-1 W/ PAINTED LAPS",1,1160,1160]
["","","WEATHERING STL ADDITIONAL","GRDRL POSTS",5,22,110]
["3436000000-N","GENERIC GRDRL ITEM (EA) 862","TEMP ADDITIONAL GRDRLPOSTS","",10,52,520]
["3500000000-E","WOVEN WIRE FEN **\" FAB","(48\")","",220,7,1540]
["3503000000-E","WOVEN WIRE FEN 47\"FAB","","",567130,2.330086224,1321461.8]
["3506000000-E","4\" TIMBER POSTS *****LONG","(7'-7\")","",9,15,135]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",36005,15.017345924000001,540699.54]
["3512000000-E","5\" TIMBER POSTS *****LONG","(8'-1\")","",14,30,420]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",8943,25.462636699000001,227712.36]
["3524000000-E","CL FEN **\"FAB VINYL CTD","(48\")","",2450,7,17150]
["3533000000-E","CHN LK FEN **\" FABRIC","(60\")","",4100,6.35,26035]
["","","(72\")","",1040,11.927884615,12405]
["","","(84\")","",110598,14,1548372]
["","","(96\")","",300,8.1,2430]
["3536000000-E","CHN LK FEN 48\" FABRIC","","",13252,4.6328893750000004,61395.05]
["3539000000-E","MET LINE PST **\" CL FEN","(60\")","",360,37.5,13500]
["","","(72\")","",90,50,4500]
["","","(72')","",60,36,2160]
["","","(84\")","",3102,102,316404]
["","","(96\")","",30,45,1350]
["3542000000-E","MET LINE PST 48\" CL FEN","","",1365,33.397069596999998,45587]
["3545000000-E","MET TERM PST **\" CL FEN","(60\")","",50,110,5500]
["","","(72\")","",6,124,744]
["","","(72')","",4,115,460]
["","","(84\")","",204,200,40800]
["","","(96\")","",4,130,520]
["3548000000-E","MET TERM PST 48\" CL FEN","","",112,90.017857143000001,10082]
["3554000000-E","MET GATE PST **\" CL FEN D","(48\")","",4,105,420]
["","","(60\")","",4,135,540]
["3557000000-E","ADDITIONAL BARB WIRE","","",8460,0.215425532,1822.5]
["3559000000-E","** STR& BW FEN W/ POST","(4)","",1425,4.9712280700000004,7084]
["3563000000-E","TEMP **\" WW FEN W/POST","(48\")","",12784,3,38352]
["3564000000-E","SGL GATE **HIGH **WIDE **OPEN","(47\" HIGH 16' WIDE 16' OPEN-ING)","",1,900,900]
["","","(47\" HIGH 8' WIDE 8' ","OPEN- ING)",1,900,900]
["","","(47\" 12' 12')","",6,575,3450]
["","","(47\" 16' 16')","",1,459,459]
["","","(47\" 20' 20')","",9,600,5400]
["3565000000-E","DBL GATE **HIGH **WIDE **OPEN","(47\" 10' 20')","",1,725,725]
["","","(47\" 12' 24')","",2,867,1734]
["","","(47\" 8' 16')","",2,600,1200]
["","","(48\" 6' 12')","",2,820,1640]
["3566000000-E","WOVEN WIRE FEN RESET","","",640,3.5,2240]
["3569000000-E","BARB WIRE FEN RESET","","",830,2.6,2158]
["3572000000-E","CHN LK FEN RESET","","",2000,8.85,17700]
["3574000000-E","GENERIC FENCING ITEM 867 (LF)","4' VINYL FEN RESET","",100,25,2500]
["","","40\" WOOD RAIL FEN ","RESET",100,25,2500]
["","","BARB WIRE FEN RESET (ELEC-","TRIC FEN)",800,6.5,5200]
["","","SPLIT RAIL FEN RESET","",85,20,1700]
["","","WOOD FEN RESET","",350,12,4200]
["3575000000-E","GENERIC FENCING ITEM (LF)","72\" CHN LK FEN W/ SLATS","",718,15.5,11129]
["","","BLACK VINYL COATED CHN LK","FEN 48\" FABRIC",350,12.65,4427.5]
["","","TEMP 4 STR& BARB WIRE","FEN W/ POSTS",10000,2.9,29000]
["","","TEMP 4 STR& BW FEN ","W/POSTS",1150,4.96,5704]
["","","TEMP 72\" CHN LK FENW/ ","POSTS",500,12,6000]
["3578000000-N","GENERIC FENCING ITEM (EA)","DBL CATTLE GATE (47\" HIGH","10' WIDE 20' OPENING)",1,1500,1500]
["","","DBL CATTLE GATE (60\" HIGH","10' WIDE 20' OPENING)",2,1800,3600]
["","","RESET EXT GATE","",2,300,600]
["3595000000-E","RELAPPING GRDRL","","",4770,3.641509434,17370]
["3628000000-E","RIP RAP CL I","","",40508,40.540850943000002,1642228.79]
["3635000000-E","RIP RAP CL II","","",13950,41.435304659000003,578022.5]
["3642000000-E","RIP RAP CL A","","",385,39.892597403000003,15358.65]
["3649000000-E","RIP RAP CL B","","",29541,44.805739142,1323606.3400000001]
["3651000000-E","BOULDERS","","",1733,65.305020196000001,113173.6]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",351580,2.1281377780000001,748210.68]
["3659000000-N","PREFORM SCOUR HOLES","","",78,1433.026923077,111776.1]
["3804000000-E","ABC (SUB-BALLAST)","","",4842,12.646137960000001,61232.6]
["3808000000-E","RR TRK TO BE CONSTRD","","",500,195,97500]
["3832000000-E","RR TRACK TO BE REMD","","",1790,10,17900]
["3848000000-E","RR DET TRACK CONST & REMV","","",1071,295,315945]
["4025000000-E","CONTR FURN ***SIGN","(E)","",355.5,14.276371308,5075.25]
["4048000000-E","REINF CONC FOUNDTN","","",365,745.66246575299999,272166.8]
["4054000000-E","PLN CONC FOUNDTN","","",22,351.70454545500002,7737.5]
["4057000000-E","OVRHD FOOTING","","",2618,778.71329259000004,2038671.4]
["4060000000-E","SUPP BRKAWY STL BM","","",192124,3.3874133369999999,650803.4]
["4066000000-E","SUPP SIMPLE STL BM","","",68993,2.7273172639999999,188165.8]
["4072000000-E","SUPP 3-LB STL U-CHAN","","",64632,5.4736981680000003,353776.06]
["4078000000-E","SUPP 2-LB STL U-CHAN","","",109,37.279816513999997,4063.5]
["4079000000-N","SUPP BARR SMALL","","",9,180.83333333300001,1627.5]
["4080000000-N","SUPP BARR LARGE","","",24,400,9600]
["4082000000-E","SUPP WOOD","","",4544,6.8540492960000003,31144.799999999999]
["4082100000-N","SUPP OVRHD SIGN STR**","(-DFEB- STA 1+40)","",1,54000,54000]
["","","(-DFEB- STA 20+50)","",1,66000,66000]
["","","(-DFEB- STA 36+00)","",1,95000,95000]
["","","(-DFEB- STA 59+00)","",1,24000,24000]
["","","(-DFLW- STA 45+70)","",1,82400,82400]
["","","(-DFLW- STA 59+00)","",1,34500,34500]
["","","(-DFLW- STA 69+00)","",1,72000,72000]
["","","(-DFWB- STA 26+85)","",1,22500,22500]
["","","(-DFWB- STA 38+05)","",1,32000,32000]
["","","(-L- STA 114+02)","",1,25300,25300]
["","","(-L- STA 124+15)","",1,71400,71400]
["","","(-L- STA 127+40)","",1,66500,66500]
["","","(-L- STA 136+85)","",1,68000,68000]
["","","(-L- STA 14+31)","",1,50000,50000]
["","","(-L- STA 142+20)","",1,67500,67500]
["","","(-L- STA 27+51)","",1,75000,75000]
["","","(-L- STA 28+93)","",1,23500,23500]
["","","(-L- STA 60+14)","",1,62500,62500]
["","","(-L- STA 62+33)","",1,30000,30000]
["","","(-L- STA 82+00)","",1,55000,55000]
["","","(-L- STA 84+58)","",1,77000,77000]
["","","(-L- STA 90+98)","",1,31500,31500]
["","","(-LDFEB- STA 188+92)","",1,29000,29000]
["","","(-Y1- STA 30+48)","",1,56000,56000]
["","","(-Y1- STA 35+42)","",1,85000,85000]
["","","(-Y2- STA 22+15)","",1,63000,63000]
["","","(-Y3- STA 41+34)","",1,110000,110000]
["","","(-Y3- STA 53+60)","",1,115000,115000]
["","","(10+00 -RP1D-)","",1,42275,42275]
["","","(100+00 -Y13-)","",1,58000,58000]
["","","(101+80 -L-)","",1,25370,25370]
["","","(107+50 -L-)","",1,29300,29300]
["","","(107+60 -L-)","",1,45750,45750]
["","","(11+00 -Y9NBL)","",1,43477,43477]
["","","(119+44 -L-)","",1,56600,56600]
["","","(12+04 -LP2D-)","",1,42250,42250]
["","","(12+40 -LPB-)","",1,68075,68075]
["","","(12+50-Y2L2-)","",1,47268,47268]
["","","(123+00 -L-)","",1,20000,20000]
["","","(127+50 -Y13-)","",1,45000,45000]
["","","(13+40 -Y2-)","",1,34700,34700]
["","","(131+30 -COL1-)","",1,64000,64000]
["","","(135+50 -L-)","",1,45000,45000]
["","","(135+90 -L-)","",1,29300,29300]
["","","(14+84 -Y12-)","",1,66300,66300]
["","","(16+50 -Y12-)","",1,64075,64075]
["","","(182+30 -L-)","",1,31350,31350]
["","","(187+50 -L-)","",1,44000,44000]
["","","(19+00 -Y5- EBL)","",1,54063.25,54063.25]
["","","(20+00-Y2L2-)","",1,36764,36764]
["","","(22+00 -L- NBL)","",1,58750,58750]
["","","(24+20 -RP1BD-)","",1,63500,63500]
["","","(241+60 -L-)","",1,55000,55000]
["","","(251+50 -L-)","",1,60000,60000]
["","","(28+00 -L-)","",1,40000,40000]
["","","(29+00 -I13CD-)","",1,27000,27000]
["","","(29+20 -COL2-)","",1,40275,40275]
["","","(29+70 -L- NBL)","",1,23500,23500]
["","","(30+00 -Y13RPC-)","",1,37000,37000]
["","","(30+95 -Y1-)","",1,22350,22350]
["","","(32+00 -Y1-)","",1,30400,30400]
["","","(33+16 -COL2-)","",1,44025,44025]
["","","(33+40 -L- SBL)","",1,52000,52000]
["","","(33+40 -RP1BD-)","",1,26400,26400]
["","","(36+50 -Y13-)","",1,50000,50000]
["","","(36+60 -L-)","",1,64000,64000]
["","","(37+30 -Y5- WBL)","",1,67939.75,67939.75]
["","","(37+90 -RP1BD-)","",1,26330,26330]
["","","(38+00 -Y9NBL)","",1,46132,46132]
["","","(39+00 -L-)","",1,64000,64000]
["","","(42+15 -RP1BD-)","",1,57775,57775]
["","","(425+00 -L-)","",1,76117,76117]
["","","(435+00 -L-)","",1,43677,43677]
["","","(451+25 -L-)","",1,76117,76117]
["","","(46+50 -CDR-)","",1,54350,54350]
["","","(464+00 -L-)","",1,58463,58463]
["","","(47+00 -L-)","",1,28000,28000]
["","","(476+90 -L-)","",1,42517,42517]
["","","(48+50 -Y13-)","",1,40000,40000]
["","","(51+15 -CDR-)","",1,76100,76100]
["","","(63+00 -L-)","",1,64000,64000]
["","","(64+60 -L-)","",1,52500,52500]
["","","(65+00 -Y13-)","",1,43000,43000]
["","","(69+00 -L-)","",1,42000,42000]
["","","(7+00 -Y12-RPC)","",1,44700,44700]
["","","(73+50 -L1-)","",1,46270,46270]
["","","(77+50 -Y13-)","",1,49000,49000]
["","","(8+00 -Y13-)","",1,44000,44000]
["","","(81+10 -L-)","",1,25270,25270]
["","","(81+25 -COL1-)","",1,110000,110000]
["","","(89+20 -L-)","",1,25270,25270]
["","","(90+75 -Y13-)","",1,54000,54000]
["","","(94+25 -L-)","",1,50000,50000]
["","","(97+40 -L-)","",1,48450,48450]
["","","(976+60 -L-)","",1,47000,47000]
["","","(A - 28+00 -Y1RPA-)","",1,38000,38000]
["","","(A AT 75' W OF EXT STR)","",1,50000,50000]
["","","(AC AT 50' W OF EXT ","STR)",1,46000,46000]
["","","(AD @ 500' S EXT OVR","HD ASSEM 'PP')",1,20000,20000]
["","","(AT 74 W EXIT)","",1,31850,31850]
["","","(B - 502+50 -L-)","",1,49000,49000]
["","","(B ON RAMP TO I-85 SB & ","I-785 NB)",1,45000,45000]
["","","(C - 531+00 -L-)","",1,104000,104000]
["","","(C AT 50' E OF EXT STR)","",1,49000,49000]
["","","(D - 586+50 -L-)","",1,75000,75000]
["","","(D AT 50' E OF EXT STR)","",1,59000,59000]
["","","(E - 595+00 -L-)","",1,52000,52000]
["","","(E AT 100' E OF EXT STR)","",1,97000,97000]
["","","(F - 610+00 -L-)","",1,75000,75000]
["","","(F AT 400'W OF EXT STR)","",1,95000,95000]
["","","(G -31+50 -Y4RPBD-)","",1,44000,44000]
["","","(G AT 100' W OF EXT ","STR)",1,90000,90000]
["","","(H - 92+50 -Y4-)","",1,40000,40000]
["","","(I - 89+50 -Y4-)","",1,48500,48500]
["","","(J - 43+00 -Y4CD-)","",1,48000,48000]
["","","(K - 42+00 -Y4-)","",1,38500,38500]
["","","(L - 72+00 -Y4-)","",1,53000,53000]
["","","(M - 113+00 -Y4-)","",1,42000,42000]
["","","(N - 322' FRM S MAIN ST ","EXIT)",1,39500,39500]
["","","(N OF 74 E EXIT)","",1,31850,31850]
["","","(O - 19+50 -Y4-)","",1,28500,28500]
["","","(P - 144' FROM LINVILLE ","RD EXIT)",1,40000,40000]
["","","(Q - 280' +/-FROM ROUTE ","MARKERS)",1,28000,28000]
["","","(R - 36+50 -Y1-)","",1,83000,83000]
["4096000000-N","SIGN ERECT D","","",279,83.157921146999996,23201.06]
["4102000000-N","SIGN ERECT E","","",2993,55.408128968,165836.53]
["4108000000-N","SIGN ERECT F","","",437,73.278260869999997,32022.6]
["4109000000-N","SIGN ERECT *** (OVRHD)","(A)","",85,618.381176471,52562.400000000001]
["","","(B)","",36,270.444444444,9736]
["4110000000-N","SIGN ERECT ** (GRD MTD)","(A)","",243,361.19341563799998,87770]
["","","(B)","",107,272.00186915900002,29104.2]
["4114000000-N","SIGN ERECT MILEMKERS","","",195,42.435897435999998,8275]
["4115000000-N","SIGN ERECT OVRLY (OVRHD)","","",16,242.1875,3875]
["4116000000-N","SIGN ERECT OVERLAY (GRD MTD)","","",22,352.04545454499998,7745]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(A)","",23,418.704347826,9630.2000000000007]
["","","(B)","",7,440.71428571400003,3085]
["","","(D)","",37,128.78378378400001,4765]
["","","(E)","",40,87.125,3485]
["","","(LOGO TRAILBLAZER)","",1,100,100]
["4116200000-N","SIGN ERECT REPOSIT OVRHD","","",5,3492,17460]
["4138000000-N","DISP SUPP STL BM","","",33,302.33030302999998,9976.9]
["4141000000-N","DISP SUPP WOOD","","",4,3,12]
["4143000000-N","DISP SUPP OVRHD ST","","",2,2000,4000]
["4149000000-N","DISP SIGN SYST OVRHD","","",15,2317.3333333330002,34760]
["4152000000-N","DISP SIGN SYST STL BM","","",64,349.69375000000002,22380.400000000001]
["4155000000-N","DISP SIGN SYST U-CHAN","","",1601,1.9173891320000001,3069.74]
["4157000000-N","STOCKPILE SIGN SYST WOOD","","",2,30,60]
["4158000000-N","DISP SIGN SYST WOOD","","",158,4.4202531650000001,698.4]
["4192000000-N","DISP SUPP U-CHAN","","",41,1.8780487800000001,77]
["4234000000-N","DISP SIGN A OR B (OVRHD)","","",74,227.14189189199999,16808.5]
["4236000000-N","DISP SIGN A B OR C (GRD MTD)","","",22,117.727272727,2590]
["4238000000-N","DISP SIGN D E F","","",20,24.164999999999999,483.3]
["4251000000-N","DISP LIGHT SYSTEM","","",21,514.42857142900004,10803]
["4263000000-N","DISP WALKWAY","","",21,514.42857142900004,10803]
["4360000000-N","GENERIC SIGNING ITEM (EA)","DISP OF SIGN ON SPAN WIRE","",2,525.20000000000005,1050.4000000000001]
["","","DISP OF SIGN SYSTM ON ","SPAN WIRE",1,220,220]
["","","DMS ACCESS LADDER","",1,4100,4100]
["","","DMS PEDESTAL STR","",1,43000,43000]
["4370000000-N","GENERIC SIGNING ITEM (LS)","DISP OF FLASHER SYSTEM","",1,1500,1500]
["","","INSTALL DMS & EQUIP ","CBNT",1,11000,11000]
["","","REM EXT DMS","",1,3000,3000]
["4399000000-N","TEMP TRAF CNTRL","","",1,21500,21500]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",59684,5.1026662089999997,304547.53000000003]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",24556,12.576027855,308816.94]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",16162,7.0295198609999998,113611.1]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",131828.1,4.0499728810000004,533900.23]
["4415000000-N","FLASHING ARROW BOARD","","",100,3076.0108,307601.08]
["4420000000-N","PORT CHANGE MSG SIGN","","",115,8588.5286956519994,987680.8]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",991,41.649041371999999,41274.199999999997]
["4430000000-N","DRUMS","","",16653,48.155638623999998,801935.85]
["4435000000-N","CONES","","",2860,21.058178322,60226.39]
["4445000000-E","BARRICADES (III)","","",22933,27.124057908000001,622036.02]
["4450000000-N","FLAGGER","","",21076,22.195862593000001,467800]
["4455000000-N","FLAGGER","","",7813,188.45808268299999,1472423]
["4457000000-N","TEMP TRAF CNTRL","","",63,43671.584603174997,2751309.83]
["4465000000-N","TEMP CRASH CUSHIONS","","",113,4925.3938053100001,556569.5]
["4470000000-N","RESET CRASH CUSHION","","",92,1357.1086956520001,124854]
["4480000000-N","TMA","","",92,12488.847826087,1148974]
["4485000000-E","PORT CONC BARR","","",95116,29.574086379000001,2812968.8]
["4490000000-E","PORT CONC BARR(ANCH)","","",31045,35.172105008999999,1091918]
["4500000000-E","RESET PORT CONC BARR","","",76217,6.3470971040000004,483756.7]
["4505000000-E","RESET PORT CONC BARRANCH","","",2050,8.2195121950000001,16850]
["4507000000-E","H2O FILLED BARR","","",10140,47.525936883999996,481913]
["4508000000-E","RESET H2O FILLED BARR","","",2368,5,11840]
["4510000000-N","LAW ENFORCEMT","","",20882,41.484112154000002,866271.23]
["4516000000-N","SKINNY DRUM","","",2684,33.756371088000002,90602.1]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",425,37.818823528999999,16073]
["4575000000-E","MOVABLE CONC BARR","","",1750,63.94,111895]
["4580000000-E","RESET MOVBLE CONC BARR","","",1200,10,12000]
["4585000000-N","TRANSF & TRNPRT VEH","","",1,326000,326000]
["4589000000-N","GENERIC TRAF CNTRL ITEM (LS)","FLAGGERS","",1,400000,400000]
["","","TEMP MEDIAN ","CROSSOVERS",1,125000,125000]
["4600000000-N","GENERIC TRAF CNTRL ITEM (EA)","TEMP PORT TRAF","SGL SYSTEM",6,16000,96000]
["","","TEMP TRAF SGL SYS","",2,24000,48000]
["","","TEMP TRAF SGL SYSTEM","",1,25000,25000]
["4650000000-N","TEMP RAISED PVT MRKS","","",22006,5.9507507039999998,130952.22]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",7043574,0.475524065,3349388.94]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",6698616,0.58867527100000006,3943309.59]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",440,6,2640]
["4688000000-E","THERMO PVT MKG LINES6\"90 MILS","","",1107154,0.82815646200000004,916896.74]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",195202,0.96721734400000003,188802.76]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",106791,1.774079089,189455.68]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",45101,2.2061000860000002,99497.32]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",91896,2.1789214979999998,200234.17]
["4702000000-E","12\"WIDE THERMO 120 MIL","","",14916,2.762473183,41205.050000000003]
["4705000000-E","THERMO LINES 16\" 120MILS","","",5290,5.6853497160000002,30075.5]
["4710000000-E","24\"WIDE THERMO 120 MIL","","",68741,8.0745144819999997,555050.19999999995]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",2271,80.412197269999993,182616.1]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",9018,105.115472389,947931.33]
["4726000000-E","HIP THERMO PVT MKG LINE 4\" 90 MILS","","",100,4.55,455]
["4770000000-E","4\" COLD APPL PLSTIC LINES **","(II)","",16705,2.7836504039999999,46500.88]
["","","(III)","",11628,3.0757774339999999,35765.14]
["","","(IV)","",42099,1.8175175180000001,76515.67]
["4775000000-E","6\" COLD APPL PLSTIC LINES **","(II)","",11136,2.6000359199999998,28954]
["","","(IV)","",43956,2.65,116483.4]
["4780000000-E","8\" COLD APPL PLSTIC LINES **","(II)","",606,7.4194059409999999,4496.16]
["","","(III)","",85,6,510]
["4785000000-E","12\" COLD PLSTIC LINES **","(II)","",1872,9.043269231,16929]
["4795000000-E","24\" COLD APPL PLSTIC LINE **","(IV)","",18,20,360]
["4800000000-N","COLD APP PLAS CHAR *","(II)","",67,284.65671641799997,19072]
["4805000000-N","COLD APPL PLASTIC SYM **","(II)","",46,264.130434783,12150]
["","","(III)","",2,262.5,525]
["","","(IV)","",5,325,1625]
["4810000000-E","PAINT PVT MKG 4\"","","",25832595,0.128682291,3324197.5]
["4815000000-E","PAINT PVT MKG 6\"","","",1135471,0.23507156100000001,266916.94]
["4820000000-E","PAINT PVT MKG 8\"","","",198323,0.51748823899999996,102629.82]
["4825000000-E","PAINT PVT MKG 12\"","","",41091,0.85226935299999995,35020.6]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",2228,2.8476211849999999,6344.5]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",53174,3.158525595,167951.44]
["4840000000-N","PAINT PVT MKG CHAR","","",822,34.318978102000003,28210.2]
["4845000000-N","PAINT PVT MKG SYMBOL","","",6347,34.285805893000003,217612.01]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",1660201,0.83757617900000003,1390544.81]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",1041171,1.148894283,1196195.4099999999]
["","","(STD GLASS BEADS)","",3690,5,18450]
["4847110000-E","POLYUREA LINES (8\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",13625,2.1436513760000002,29207.25]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",54753,2.6951399920000001,147567]
["4850000000-E","LINE REML 4\" WIDE","","",348324,0.70988975799999998,247271.64]
["4855000000-E","LINE REML 6\" WIDE","","",58030,0.625096502,36274.35]
["4860000000-E","LINE REML 8\" WIDE","","",6539,1.2344242240000001,8071.9]
["4865000000-E","LINE REML 12\" WIDE","","",45,2.1,94.5]
["4870000000-E","LINE REML 24\" WIDE","","",2445,3.091615542,7559]
["4875000000-N","REML OF SYMBL & CHAR","","",256,48.852148436999997,12506.15]
["4880000000-E","CURING COMP REML LINE","","",825,1.65,1361.25]
["4890000000-E","GENERIC PVT MKG ITEM (LF)","TEMP RUMBLE STRIPS","",6828,3.4,23215.200000000001]
["4892000000-N","GENERIC PVT MKG ITEM (EA) 1205","INTERSTATE SHIELD THERMO-","PLASTIC SYMBOL (90 MILS)",2,750,1500]
["4900000000-N","PERM RAISED PVT MARKERS","","",41304,4.6298377879999997,191230.82]
["4905000000-N","SNOWPLB PVT MRKER","","",72823,26.198425772,1907847.96]
["4915000000-E","7' U-CHANNEL POSTS","","",79,33.270253165,2628.35]
["4935000000-N","FLEX DELINATR (CRYSTL)","","",744,54.230510752999997,40347.5]
["4940000000-N","FLEX DELINATR (YELLW)","","",350,62.066285714000003,21723.200000000001]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",30,39.991666666999997,1199.75]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",30,39.991666666999997,1199.75]
["4955000000-N","OBJECT MKR (END OF RD)","","",91,108.607142857,9883.25]
["5000000000-E","***' HIGH MOUNT STD","(60')","",6,14000,84000]
["5005000000-E","80' HIGH MOUNT STD","","",12,14659.166666667001,175910]
["5010000000-E","100' HIGH MOUNT STD","","",27,17205.011111111002,464535.3]
["5015000000-E","120' HIGH MOUNT STD","","",38,20149.736842105001,765690]
["5020000000-N","PORT DRIVE UNIT","","",7,3827.2142857140002,26790.5]
["5025000000-E","HIGH MOUNT FOUNDS","","",668.4,685.44823458999997,458153.6]
["5030000000-N","HM LUMINAIRE ************","(400W HPS)","",64,808.75,51760]
["","","(750W HPS)","",370,821.39351351400001,303915.59999999998]
["5050000000-N","LIT STD MTLT ************","(35' SA 15' ARM)","",25,2350,58750]
["","","(45' SA 15' ARM)","",12,2475,29700]
["","","(45' TA 15' ARM)","",3,2797,8391]
["5070000000-N","STD FOUNDAT ***********","(R1)","",33,1013.193939394,33435.4]
["","","(R2)","",4,972.8,3891.2]
["","","(R1)","",72,986.11111111100001,71000]
["","","(R2)","",9,1097.777777778,9880]
["5080000000-N","LITE STD LUM ************","(RDW 250W HPS MC3)","",12,565,6780]
["5090000000-N","LITE STD LUM RDW 400W HPS","","",6,412.1,2472.6]
["5120000000-N","SERVICE POLE ************","(30' CL 4)","",5,1762,8810]
["","","(30' CL 4)","",6,790.76666666699998,4744.6000000000004]
["","","(30FT CL 4)","",3,770,2310]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",1100,26.029545455000001,28632.5]
["5145000000-N","LITE CNTRL RW************","(240/480 V)","",4,9191.7749999999996,36767.1]
["","","(240/480 VOLT)","",9,10853.333333332999,97680]
["5155000000-E","ELECT DUCT BD SIZE *****","(2\")","",3686,6.3203879540000001,23296.95]
["","","(3\")","",1592,8.0495163319999996,12814.83]
["","","(4\")","",682,11.954178885999999,8152.75]
["","","(6\")","",435,19.390804597999999,8435]
["","","(TS2)","",2185,5.6,12236]
["","","(TS3)","",775,5.9,4572.5]
["","","(TS4)","",135,8.8000000000000007,1188]
["5160000000-E","ELECT DUCT JA SIZE *****","(2\")","",581,9.5,5519.5]
["","","(3\")","",1006,16.154821074000001,16251.75]
["","","(4\")","",1353,16.497043606999998,22320.5]
["","","(6\")","",361,17.912742382000001,6466.5]
["","","(TS3)","",795,14.5,11527.5]
["","","(TS4)","",1715,15,25725]
["","","(TS6)","",670,23,15410]
["5170000000-E","**-#8 W/G FEEDER CIRCUIT","(-2)","",560,2.4500000000000002,1372]
["","","(2)","",3380,4.0382100589999999,13649.15]
["5175000000-E","**-#6 W/G FEEDER CIRCUIT","(-2)","",1245,2.4,2988]
["","","(2\")","",170,3,510]
["","","(2)","",2041,4.4954189119999999,9175.15]
["5180000000-E","**-#4 W/G FEEDER CIRCUIT","(-2)","",1015,3.3,3349.5]
["","","(2\")","",560,4,2240]
["","","(2)","",2029,5.1078117299999999,10363.75]
["5185000000-E","**-#2 W/G FEEDER CIRCUIT","(-2)","",1865,5.5,10257.5]
["","","(2\")","",390,5.5,2145]
["","","(2)","",5412,7.3949186989999998,40021.300000000003]
["","","(4)","",770,8.0500000000000007,6198.5]
["5190000000-E","************ FEEDER CIR","(2 1 W/G)","",780,8.5,6630]
["","","(2-1 W/G)","",1086,9,9774]
["","","(4 - 1 W/G )","",1275,10.6,13515]
["","","(4 - 2/0 W/G )","",1335,12.9,17221.5]
["5205000000-E","**-#8 W/G FEEDR N *****\"","(2 1 1/2)","",5450,10.75,58587.5]
["","","(2 1-1/2\")","",10555,15.992790146999999,168803.9]
["","","(2 15\")","",4477,10.26,45934.02]
["","","(2 15)","",7909,6.9185990640000004,54719.199999999997]
["","","(2 TS15)","",6029,5.9,35571.1]
["5210000000-E","**-#6 W/G FEEDR N *****\"","(2 1-1/2\")","",1230,11.1,13653]
["","","(2 15\")","",1880,11.14,20943.2]
["","","(2 15)","",5277,7.4630661360000001,39382.6]
["","","(2 TS15)","",3343,6.65,22230.95]
["5215000000-E","**-#4 W/G FEEDER N *****\"","(2 15\")","",225,12.51,2814.75]
["","","(2 15)","",16625,8.0060451130000008,133100.5]
["","","(2 TS15)","",7848,7.7,60429.599999999999]
["5220000000-E","**-#2 W/G FEEDER N *****\"","(2 15)","",8115,9.8673444240000006,80073.5]
["","","(2 TS15)","",20789,9.4,195416.6]
["","","(4 2)","",8210,10,82100]
["5225000000-E","**-#1 W/G FEEDER CIR ****","(2 2)","",4395,12,52740]
["","","(2 TS2)","",4662,13,60606]
["","","(4 2)","",6825,10.85,74051.25]
["5230000000-E","************ FEEDER N **","(4 - 2/0 W/G 3\")","",3215,16.149999999999999,51922.25]
["5240000000-N","ELEC JB ************","(JB18)","",66,555,36630]
["","","(JB36)","",30,1440,43200]
["","","(PC18)","",118,331.97288135600002,39172.800000000003]
["","","(PC30)","",43,586.11395348799999,25202.9]
["","","(PC36)","",18,764.55555555599994,13762]
["5252000000-N","UNDERPASS LUMINARIES*","(100W HPS PM)","",6,570,3420]
["","","(WM 80W MAX LED)","",6,585,3510]
["5253000000-N","UNDERPASS CIRCUITRY *************","(HOLLOWAY STREET UPL-1)","",1,3280,3280]
["","","(HOLLOWAY STREET UPL-2)","",1,3280,3280]
["","","(RAMSEY ST UPL-1)","",1,4000,4000]
["5255000000-N","PORT LIGHTING","","",26,48758.693461538001,1267726.03]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","ELECTRICAL CONDUIT SYSTEM AT","ANGIER AVENUE ECS-3",1,2735,2735]
["","","RAMP B PIT ELECTRICAL WORK","",1,7575,7575]
["","","RAMP B STATIC SCALE PLATFORM","",1,110915,110915]
["","","RAMP B STATIC SCALE SYSTEM","",1,40915,40915]
["","","RAMP C PIT ELECTRICAL WORK","",1,7575,7575]
["","","RAMP C STATIC SCALE PLATFORM","",1,110915,110915]
["","","RAMP C STATIC SCALE SYSTEM","",1,40915,40915]
["5262000000-E","GENERIC LIGHTING ITEM (CY)","HIGH MOUNT FOUNDS","",21,910,19110]
["5265000000-E","GENERIC LIGHTING ITEM (LF)","146 W/G FEEDER CKT THHN/THWN WIRE","IN 2\" RGS CONDUIT",192,72.209999999999994,13864.32]
["","","166 W/G FEEDER CKT THHN/THWN WIRE","IN 2\" RGS CONDUIT",251,59.07,14826.57]
["","","","IN 3\" PVC CONDUIT",140,68.77,9627.7999999999993]
["","","","IN 3\" RGS CONDUIT",60,107.74,6464.4]
["","","28 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",1276,21.33,27217.08]
["","","","IN 1 1/4\" RGS CONDUIT",415,25.78,10698.7]
["","","28 26 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",4766,18.57,88504.62]
["","","286 W/G FEEDER CKT THHN/THWN WIRE","IN 3\" PVC CONDUIT",97,83.9,8138.3]
["","","","IN 3\" RGS CONDUIT",29,245.39,7116.31]
["","","326 W/G FEEDER CKT THHN/THWN WIRE","IN 3\" PVC CONDUIT",97,89.96,8726.1200000000008]
["","","","IN 3\" RGS CONDUIT",29,130.9,3796.1]
["","","46 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" RGS CONDUIT",101,49.73,5022.7299999999996]
["","","48 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",6075,17.34,105340.5]
["","","48 26 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",2656,22.04,58538.239999999998]
["","","66 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" RGS CONDUIT",82,49.39,4049.98]
["","","68 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",5593,19.309999999999999,108000.83]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","(100') HIGH MOUNT LUMINAIRE - LED","",72,1475,106200]
["","","(120') HIGH MOUNT LUMINAIRE - LED","",24,1740,41760]
["","","(80') HIGH MOUNT LUMINAIRE - LED","",24,1500,36000]
["","","1 POLE 120VAC EQUIP DIS- CONNECT","",8,303,2424]
["","","15KVA POWER TRANSFORMER","",1,3290,3290]
["","","2 POLE 240VAC EQUIP DIS-CONNECT","",1,570,570]
["","","BOLLARD LGT STD","",8,1000,8000]
["","","DAVIT STYLE LGT STD MH 35' SA 6'","",19,2270,43130]
["","","DAVIT STYLE LGT STD MH 35' SA 6'","",36,1900,68400]
["","","ELECTRICAL JUNCT BOXES PC18","",13,432,5616]
["","","ELECTRICAL JUNCT BOXES PG36","",1,1133,1133]
["","","EQUIP DISCONNECT","",1,698.69,698.69]
["","","HIGH MOUNT LUMINAIRE - LED","",42,2236.4285714289999,93930]
["","","INSTALL LED LUMINAIRE","(ROADWAY)",19,1270.9000000000001,24147.1]
["","","","(TUNNEL)",652,1875.9,1223086.8]
["","","LIGHT CNTRL EQUIP TYPE","RA 120/240V",1,4500,4500]
["","","","WS 120/208V",1,10050,10050]
["","","LIGHT CNTRL EQUIP RA 120/240","",1,6850,6850]
["","","LIGHT CNTRL EQUIP TU","(TUNNEL 104)",1,14026,14026]
["","","","(TUNNEL 17)",1,14026,14026]
["","","LIGHT STD JUNCT BOX","",28,594.04999999999995,16633.400000000001]
["","","LIGHT STD MLTS 35'MH 6'SA","",15,2425,36375]
["","","LIGHT CNTRL EQUIP TU","(TUNNEL 15)",1,14026,14026]
["","","PACKAGED DIESEL GENERATOR","SET (FOR TUNNEL 104)",1,116312,116312]
["","","","SET (FOR TUNNELS 15 & 17)",1,152520,152520]
["","","PACKAGED EQUIP ENCLOSURE","(FOR TUNNEL 104 LIGHTING SYSTM)",1,256564,256564]
["","","PACKAGED EQUIP ENCLOSURE","(FOR TUNNELS 15 & 17 LIGHT SYS)",1,261189,261189]
["","","POST TOP LIGHT STD","",29,1464.965517241,42484]
["","","PT LUMINAIRES LED V","",29,1841.586206897,53406]
["","","RDW LUMINAIRES LED III","",55,879.54545454499998,48375]
["","","RELOC CNTRL SYSTEM","",1,5600,5600]
["","","RELOC HIGH MOUNT STD","",2,5500,11000]
["","","RELOC LIGHT STD","",8,800,6400]
["","","REM LIGHT STD","",14,305,4270]
["","","REM LUMINAIRE (ROADWAY)","",19,717.22,13627.18]
["","","REM LUMINAIRE(TUNNEL)","",584,161.32,94210.880000000005]
["","","REPL LUMINAIRE (HIGH MAST)","",8,750,6000]
["","","REPL LUMINAIRE (SINGLE ARM)","",8,260,2080]
["","","ROADWAY LIGHT STD LUMI- NAIRE-LED","",15,1065,15975]
["","","ROADWAY LIGHT STD LUMIN- AIRE - LED","",25,1050,26250]
["","","SPARE LED LUMINAIRE (TUNNEL)","",30,1037.7,31131]
["","","STD FOUND B1","",8,250,2000]
["","","STD FOUND R1S","",29,737.93103448299996,21400]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",40,467.06324999999998,18682.53]
["5325000000-E","**\" H2O LINE","(1\")","",1318,7,9226]
["","","(14\")","",150,61.2,9180]
["","","(18\")","",407,81.599999999999994,33211.199999999997]
["","","(3/4\")","",41,20,820]
["5325200000-E","2\" H2O LINE","","",5744,23.186055014000001,133180.70000000001]
["5325300000-E","3\" H2O LINE","","",563,19.033747779999999,10716]
["5325400000-E","4\" H2O LINE","","",569,45.953778559,26147.7]
["5325600000-E","6\" H2O LINE","","",24572,38.805687775000003,953533.36]
["5325800000-E","8\" H2O LINE","","",24083,40.595670804999997,977665.54]
["5326000000-E","10\" H2O LINE","","",9970,52.048635908000001,518924.9]
["5326200000-E","12\" H2O LINE","","",58565,59.891289337000003,3507533.36]
["5326600000-E","16\" H2O LINE","","",22808,104.097347422,2374252.2999999998]
["5327000000-E","20\" H2O LINE","","",2610,95.589731800999999,249489.2]
["5327400000-E","24\" H2O LINE","","",1180,271.35593220300001,320200]
["5328000000-E","30\" H2O LINE","","",7789,259.02439337499999,2017541]
["5534000000-E","**\" VALVE","(1\")","",2,640,1280]
["","","(1-1/2\")","",1,700,700]
["","","(2\")","",1,935,935]
["","","(3\")","",2,850,1700]
["","","(3/4\")","",6,693.33333333300004,4160]
["5536000000-E","2\" VALVE","","",33,662.64121212099997,21867.16]
["5538000000-E","4\" VALVE","","",5,761,3805]
["5540000000-E","6\" VALVE","","",85,1036.6544705880001,88115.63]
["5546000000-E","8\" VALVE","","",64,1673.7085937500001,107117.35]
["5552000000-E","10\" VALVE","","",22,2129.1454545450001,46841.2]
["5558000000-E","12\" VALVE","","",120,2367.0397499999999,284044.77]
["5558600000-E","16\" VALVE","","",37,5887.5008108109996,217837.53]
["5559000000-E","20\" VALVE","","",3,5413.3333333330002,16240]
["5559400000-E","24\" VALVE","","",2,10500,21000]
["5560000000-E","30\" VALVE","","",12,19500,234000]
["5571600000-E","6\" TAPPING VALVE","","",6,2555.4699999999998,15332.82]
["5571800000-E","8\" TAPPING VALVE","","",2,10158.89,20317.78]
["5572200000-E","12\" TAPPING VALVE","","",3,12333.333333332999,37000]
["5572600000-E","16\" TAPPING VALVE","","",3,12605.58,37816.74]
["5589100000-E","1\" AIR RELEASE VALVE","","",14,2578.8435714289999,36103.81]
["5589200000-E","2\" AIR RELEASE VALVE","","",18,4159.3805555560002,74868.850000000006]
["5606000000-E","2\" BLOW OFF","","",23,1977.7808695650001,45488.959999999999]
["5606600000-E","6\" BLOW OFF","","",2,18000,36000]
["5643000000-E","**\" H2O METER","(1\")","",1,7100,7100]
["","","(5/8\")","",90,1020.17,91815.3]
["5643100000-E","3/4\" H2O METER","","",1,1385.45,1385.45]
["5643150000-E","1-1/2\" H2O METER","","",2,5150,10300]
["5643200000-E","2\" H2O METER","","",1,6825,6825]
["5648000000-N","RELOC H2O METER","","",223,928.5332287,207062.91]
["5649000000-N","RECONNECT H2O METER","","",44,963.282045455,42384.41]
["5653100000-E","RELC **\" DCV BACKFLOW PREVNT A","(3/4\")","",1,2000,2000]
["5653810000-E","RELC 8\" DCV BACKFLOW PREVNT A","","",2,5000,10000]
["5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1-1/2\")","",1,5800,5800]
["5656200000-E","2\" RPZ BACKFLOW PREVNT ASMBLY","","",1,3675,3675]
["5656410000-E","RELC 4\" RPZ BACKFLOW PREVNT A","","",1,3600,3600]
["5656610000-E","RELC 6\" RPZ BACKFLOW PREVNT A","","",1,4200,4200]
["5666000000-E","FIRE HYDRANT","","",82,4065.0240243899998,333331.96999999997]
["5672000000-N","RELOC FIRE HYDRANT","","",92,2851.0531521739999,262296.89]
["5678600000-E","8\" LINE STOP","","",1,7522,7522]
["5679000000-E","12\" LINE STOP","","",2,12500,25000]
["5684400000-E","6\" LINE STOP W/ BYPASS","","",1,6800,6800]
["5684600000-E","8\" LINE STOP W/ BYPASS","","",1,8500,8500]
["5691000000-E","**\" SANIT GRAV SEWER","(15\")","",848,94,79712]
["5691100000-E","4\" SANIT GRAV SEWER","","",495,16.375757576000002,8106]
["5691200000-E","6\" SANIT GRAV SEWER","","",936,43.108974359000001,40350]
["5691300000-E","8\" SANIT GRAV SEWER","","",20649,74.975929585000003,1548177.97]
["5691400000-E","10\" SANIT GRAV SEWER","","",3342,104.16995810900001,348136]
["5691500000-E","12\" SANIT GRAV SEWER","","",2649,76.940732351999998,203816]
["5691600000-E","16\" SANIT GRAV SEWER","","",1438,97.136244783999999,139681.92000000001]
["5691700000-E","18\" SANIT GRAV SEWER","","",1713,138.797431407,237760]
["5691900000-E","24\" SANIT GRAV SEWER","","",1554,149.4,232167.6]
["5692000000-E","30\" SANIT GRAV SEWER","","",632,229.131803797,144811.29999999999]
["5709000000-E","**\" FORCE MAIN SEWER","(3\")","",17482,26,454532]
["","","(30\")","",949,425,403325]
["","","(54\")","",236,2350,554600]
["5709100000-E","2\" FORCE MAIN SEWER","","",747,20.399999999999999,15238.8]
["5709200000-E","4\" FORCE MAIN SEWER","","",2870,30.108013936999999,86410]
["5709300000-E","6\" FORCE MAIN SEWER","","",9710,30.116158598999998,292427.90000000002]
["5709400000-E","8\" FORCE MAIN SEWER","","",1196,88.821070234000004,106230]
["5709600000-E","12\" FORCE MAIN SEWER","","",476,245,116620]
["5768000000-N","SANIT SEWER CLEAN-OUT","","",82,1710.49304878,140260.43]
["5774000000-E","**' DIA UTILITY MH","(7')","",2,2500,5000]
["5775000000-E","4' DIA UTILITY MH","","",132,2442.843787879,322455.38]
["5776000000-E","5' DIA UTILITY MH","","",40,3947.3440000000001,157893.76000000001]
["5777000000-E","6' DIA UTILITY MH","","",4,3232.8,12931.2]
["5780000000-E","UTILITY MH WALL **' DIA","(7')","",12.2,225,2745]
["5781000000-E","UTILITY MH WALL 4' DIA","","",356.91,279.00325011899997,99579.05]
["5782000000-E","UTILITY MH WALL 5' DIA","","",313.75,216.80541832700001,68022.7]
["5783000000-E","UTILITY MH WALL 6' DIA","","",16,322.2,5155.2]
["5800000000-E","ABAND 6\" UTILITY PIPE","","",15317,2.838595025,43478.76]
["5801000000-E","ABAND 8\" UTILITY PIPE","","",27861,6.9895308849999997,194735.32]
["5802000000-E","ABAND 10\" UTILITY PIPE","","",3214,9.6074611080000007,30878.38]
["5804000000-E","ABAND 12\" UTILITY PIPE","","",26283,11.010548644,289390.25]
["5810000000-E","ABAND 16\" UTILITY PIPE","","",19602,15.001986022000001,294068.93]
["5811000000-E","ABAND 18\" UTILITY PIPE","","",2003,18.116030953999999,36286.410000000003]
["5812000000-E","ABAND 20\" UTILITY PIPE","","",3364,20.170986920000001,67855.199999999997]
["5813000000-E","ABAND 24\" UTILITY PIPE","","",1333,6.3,8397.9]
["5814000000-E","ABAND 30\" UTILITY PIPE","","",5551,28.072959826999998,155833]
["5815000000-N","REM H2O METER","","",50,252.9828,12649.14]
["5815500000-N","REM FIRE HYDRANT","","",23,681.29391304299998,15669.76]
["5816000000-N","ABAND UTILITY MH","","",75,809.15773333300001,60686.83]
["5828000000-N","REM UTILITY MH","","",62,991.59693548400003,61479.01]
["5835000000-E","**\" ENCASEMT PIPE","(10\")","",173,60.67,10495.91]
["","","(18\")","",50,85,4250]
["","","(42\")","",1100,262.5,288750]
["","","(48\")","",1107,543.49593495900001,601650]
["","","(60\")","",230,460,105800]
["","","(72\")","",94,820,77080]
["5835400000-E","6\" ENCASEMT PIPE","","",464,63.265086207000003,29355]
["5835600000-E","12\" ENCASEMT PIPE","","",1504,70.845545212999994,106551.7]
["5835700000-E","16\" ENCASEMT PIPE","","",4449,68.170995728999998,303292.76]
["5835800000-E","18\" ENCASEMT PIPE","","",112,84,9408]
["5836000000-E","24\" ENCASEMT PIPE","","",8003,73.911803074000005,591516.16000000003]
["5836200000-E","30\" ENCASEMT PIPE","","",3290,256.841477204,845008.46]
["5836400000-E","36\" ENCASEMT PIPE","","",1053,313.172839506,329771]
["5871000000-E","**\" TRENCHLESS INSTALL (IN SOIL)","(42\")","",275,325,89375]
["","","(48\")","",162,181.481481481,29400]
["5871010000-E","**\" TRENCHLESS INSTALL (NOT IN SOIL)","(42\")","",275,725,199375]
["","","(48\")","",162,712.5,115425]
["5871200000-E","3\" TRENCHLESS INSTALL (IN SOIL)","","",425,72.5,30812.5]
["5871210000-E","3\" TRENCHLESS INSTALL (NOT IN SOIL)","","",425,172,73100]
["5871400000-E","6\" TRENCHLESS INSTALL (IN SOIL)","","",1503,53.047238856,79730]
["5871410000-E","6\" TRENCHLESS INSTALL (NOT IN SOIL)","","",273,41.989010989000001,11463]
["5871500000-E","8\" TRENCHLESS INSTALL (IN SOIL)","","",648,112.75462963,73065]
["5871510000-E","8\" TRENCHLESS INSTALL (NOT IN SOIL)","","",347,151.61383285299999,52610]
["5871700000-E","12\" TRENCHLESS INSTALL (IN SOIL)","","",876,173.07847032000001,151616.74]
["5871710000-E","12\" TRENCHLESS INSTALL (NOT IN SOIL)","","",632,331.949588608,209792.14]
["5871800000-E","14\" TRENCHLESS INSTALL (IN SOIL)","","",75,357,26775]
["5871810000-E","14\" TRENCHLESS INSTALL (NOT IN SOIL)","","",75,357,26775]
["5871900000-E","16\" TRENCHLESS INSTALL (IN SOIL)","","",762,214.109120735,163151.15]
["5871910000-E","16\" TRENCHLESS INSTALL (NOT IN SOIL)","","",542,676.83274907700002,366843.35]
["5872000000-E","18\" TRENCHLESS INSTALL (IN SOIL)","","",203.5,459,93406.5]
["5872010000-E","18\" TRENCHLESS INSTALL (NOT IN SOIL)","","",203.5,459,93406.5]
["5872200000-E","24\" TRENCHLESS INSTALL (IN SOIL)","","",1599,276.567767355,442231.86]
["5872210000-E","24\" TRENCHLESS INSTALL (NOT IN SOIL)","","",1597,486.89471509100002,777570.86]
["5872300000-E","30\" TRENCHLESS INSTALL (IN SOIL)","","",425,155,65875]
["5872310000-E","30\" TRENCHLESS INSTALL (NOT IN SOIL)","","",425,155,65875]
["5872400000-E","36\" TRENCHLESS INSTALL (IN SOIL)","","",372.5,194.91140939600001,72604.5]
["5872410000-E","36\" TRENCHLESS INSTALL (NOT IN SOIL)","","",372.5,724.02013422799996,269697.5]
["5879200000-E","2\" GAS LINE","","",120,17,2040]
["5879600000-E","6\" GAS LINE","","",1390,62.35,86666.5]
["5882000000-N","GENERIC UTILITY ITEM (EA)","12\" ANTI-CAVITATION PRESSURE","REDUCING VALVE",2,28500,57000]
["","","12\" CHECK VALVE & MH","",1,19000,19000]
["","","12\" INSERT VALVE","",1,11000,11000]
["","","12\" NITRILE PIPE GASKET","",8,53.92,431.36]
["","","16\" NITRILE PIPE GASKET","",3,95.54,286.62]
["","","3\" PLUG VALVE","",4,1700,6800]
["","","8\" INSERT VALVE","",1,7500,7500]
["","","8\" NITRILE PIPE GASKET","",16,50.42,806.72]
["","","ABAND H2O METER VAULT","",3,1500,4500]
["","","ABAND/REM SEWER LIFT STA","",1,25000,25000]
["","","ADJUST H2O VAULT LID","",2,2022.25,4044.5]
["","","CONNECTIN DETAIL NO 2","",6,56500,339000]
["","","CONNECTIN DETAIL NO 4","",14,4750,66500]
["","","FORCE MAIN FLUSHING CONNECTION","",2,10400,20800]
["","","RELOC 4\" H2O METER","",1,7000,7000]
["","","RELOC H2O METER W/ NEW VAULT","",2,3060,6120]
["","","ROTAT TOP FOR EXT MH","CONCENTRIC TOP",3,1500,4500]
["","","","(ECCENTRIC TOP)",3,1500,4500]
["","","ROTAT TOP FOR EXT MH","",1,1350,1350]
["","","STL H-PILE PIER","",7,6161.1,43127.7]
["","","YARD HYDRANT","",1,495,495]
["5888000000-E","GENERIC UTILITY ITEM(LF)","10\" ENCASEMT PIPE","",170,100,17000]
["","","3/4\"PVC H2O PIPE SCH 80","",455,8.1999999999999993,3731]
["","","42\" DUMMY ENCASEMT PIPE","",550,260,143000]
["","","54\" DUMMY ENCASEMT PIPE","",280,390,109200]
["","","ANCH SEWER MAIN TO PROPOSED CLVT","",52,135,7020]
["5890000000-N","GENERIC UTILITY ITEM (EA) 1510","REM BLOWOFF ASSEM","",1,1800,1800]
["5894000000-E","GENERIC UTILITY ITEM (CY)","EXCAVATABLE FLOWABLE FILL","",40.5,200,8100]
["","","SEL MATERIAL CL VI","57 STONE",250,60,15000]
["5912000000-N","GENERIC UTILITY ITEM(LS)","4\" H2O METER ASSEM","",1,20000,20000]
["","","NBOUND SEWER PUMP STA","",1,72000,72000]
["","","REM EXT 4\" H2O METER","ASSEM",1,5500,5500]
["","","REM LIFT STA","",1,3060,3060]
["","","SBOUND SEWER PUMP STA","",1,124000,124000]
["","","SUPP 8\" H2O MAIN & 36\" SEWER MAIN","",1,10000,10000]
["6000000000-E","TEMP SILT FEN","","",1791688,1.764168628,3160839.76]
["6006000000-E","EROS CONTRL STONE CL A","","",91850,39.233857376000003,3603629.8]
["6009000000-E","EROS CONTRL STONE CL B","","",375008,39.219800243999998,14707738.85]
["6012000000-E","SEDIMT CNTRL STONE","","",327955,34.958030370000003,11464660.85]
["6015000000-E","TEMP MULCHING","","",5885.93,664.20011111199995,3909435.36]
["6018000000-E","SEED FOR TEMP SEEDING","","",357930,1.7595102389999999,629781.5]
["6021000000-E","FERT FOR TEMP SEEDING","","",1561.7,682.32024716700005,1065579.53]
["6024000000-E","TEMP SLOPE DRNS","","",239365,9.4005692140000008,2250167.25]
["6029000000-E","SAFETY FEN","","",270035,1.314384802,354929.9]
["6030000000-E","SILT EXCAV","","",1184700,3.5339224279999999,4186637.9]
["6036000000-E","MATTING FOR EROS CNTRL","","",3977351,1.2306413490000001,4894692.5999999996]
["6037000000-E","COIR FIBER MAT","","",80762,4.4577173669999999,360014.17]
["6038000000-E","PERM SOIL REINF MAT","","",170846,5.0683425419999999,865906.05]
["6042000000-E","1/4\" HARDWARE CLOTH","","",255663,3.3243889420000001,849923.25]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",5640,3.9740248230000002,22413.5]
["6045000000-E","**\" TEMP PIPE","(15\")","",170,53.409705881999997,9079.65]
["","","(18\")","",1070,28.102803737999999,30070]
["","","(24\")","",1470,37.665816327000002,55368.75]
["","","(30\")","",55,70,3850]
["","","(36\")","",480,53.828125,25837.5]
["","","(54\")","",175,120,21000]
["","","(72\")","",100,208.87,20887]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",1815,73.464628098999995,133338.29999999999]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",7105,22.555531316,160257.04999999999]
["6069000000-E","STILLING BASINS","","",8020,18.094389026999998,145117]
["6070000000-N","SPEC STILLING BASINS","","",599,423.74353923199999,253822.38]
["6071010000-E","WATTLE","","",128667,4.6471894889999996,597939.93000000005]
["6071012000-E","COIR FIBER WATTLE","","",152355,7.8316021789999999,1193183.75]
["6071013000-E","WATTLE BARR","","",2600,9.019230769,23450]
["6071014000-E","COIR FIBR WATTLE BARR","","",1370,14.701313869,20140.8]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",154021,6.401783848,986009.15]
["6071030000-E","COIR FIBER BAFFLE","","",232280,4.7818268899999996,1110722.75]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",932,809.74396995699999,754681.38]
["","","(2\")","",105,1090.364761905,114488.3]
["","","(2-1/2\")","",24,1204.2974999999999,28903.14]
["","","(3\")","",10,1312.4290000000001,13124.29]
["","","(4\")","",3,1562.21,4686.63]
["","","(6\")","",1,1850,1850]
["6078000000-E","SEL UNDERGRTH REML","","",5,5000,25000]
["6084000000-E","SEEDING & MULCHING","","",5340.56,1545.250990533,8252505.6299999999]
["6087000000-E","MOWING","","",2483.77,79.218188479999995,196759.76]
["6090000000-E","SEED FOR REP SEEDING","","",65678,4.3000989680000004,282421.90000000002]
["6093000000-E","FERT FOR REP SEEDING","","",225.76,862.25163890900001,194661.93]
["6096000000-E","SEED FOR SUPP SEEDING","","",113420,3.4022504850000002,385883.25]
["6102000000-E","SODDING","","",2830,6.5,18395]
["6105000000-E","H2O","","",6,250,1500]
["6108000000-E","FERTILIZER TOPDRESSING","","",3367.55,837.477501448,2820247.36]
["6111000000-E","IMPERVIOUS DIKE","","",10997,35.358679639999998,388839.4]
["6114500000-N","SPECIZED H& MOWING","","",3163,47.785298767,151144.9]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",4398,163.43022055500001,718766.11]
["6118000000-N","ROOTWADS","","",2,1250,2500]
["6120000000-E","CLVT DIVERSION CHANNEL","","",16150,14.408916409,232704]
["6123000000-E","REFORESTA","","",132.19999999999999,1236.870574887,163514.29]
["6126000000-E","STREAMBANK REFORESTA","","",12.15,6018.1563786010001,73120.600000000006]
["6129000000-E","WETL& REFORESTA","","",0.34,5000,1700]
["6132000000-N","GENERIC EROS CNTRL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",45,202.777777778,9125]
["","","","DEVICE CLEANOUT",249,68.859437751000002,17146]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",92,124.805434783,11482.1]
["","","LOGS","",6,800,4800]
["6133000000-N","GENERIC EROS CNTRL ITEM (LS)","CONST SURVEYING FOR MITIGATION","",1,26000,26000]
["","","DIVERSION PUMPING FOR MITIGATION","",1,30000,30000]
["","","DIVERSION PUMPING FOR MITIGA- TION","",1,8000,8000]
["","","GRADING FOR MITIGATION","",2,229112.5,458225]
["","","REML OF EROS CNTRL DEVICES","",1,26500,26500]
["","","SURVEYING FOR MITIGATION","",1,4300,4300]
["6135000000-E","GENERIC EROS CNTRL ITEM (ACR)","COMPOST BLANKET","",57,5776.3157894739998,329250]
["","","DISKING","",1.84,889.13043478300006,1636]
["","","RIPPING","",1.84,889.13043478300006,1636]
["","","SEEDING & MULCHING BLUEGRASS","FESCUE MIX REST AREA LAWN",3,1325,3975]
["","","SEEDING & MULCHING; CENTIPEDE","TURF SEEDING 1 LB/1000SF",4.3,2625,11287.5]
["","","WETL& GRASS PLANTNG","",1.5,3000,4500]
["6138000000-E","GENERIC EROS CNTRL ITEM (CY)","IMPERVIOUS SEL MATERIAL","",175,10,1750]
["6150000000-E","GENERIC EROS CNTRL ITEM (TON)","AERIAL FERTILIZER TOPDRESSING","",75,10,750]
["6640000000-N","GENERIC PLANTING ITEM (EA) 1670","ABELIA X KALEIDOSCOPE; KALEI-","DOSCOPE ABELIA 12-15\" 3 CONT",18,40,720]
["","","CORNUS FLORIDA; FLOWERING","DOGWOOD 7-8' 1 1/2\" CAL B&B",21,212.5,4462.5]
["","","GLEDITSIA TRACANTHOS INERMIS; THORNLESS","HONEYLOCUST 12-14' 3\" CAL",7,247,1729]
["","","HEMEROCALLIS 'BUTTER-ED POPCORN' BUTTER-","ED POP-CORN DAYLILY 1 CONT",87,6,522]
["","","ILEX CORNUTA 'CARISSA';","CARISSA HOLLY 18-24\" 3 CONT",29,18,522]
["","","LAGERSTROEMIA 'ARAPAHO';","ARAPAHO CRAPE MYRTLE 6-7' B&B",6,187.5,1125]
["","","LIRIOPE MUSCARII 'BIG BLUE';","BIG BLUE LIRIOPE 1 CONTAINER",85,4.5,382.5]
["","","MAGNOLIA GRANDI-FLORA 'LITTLE GEM","LITTLE GEM MAG-NOLIA 8-10' B&B",21,250,5250]
["","","MYRICA CERIFICA; WAX MYRTLE","4\" 15 CONTAINER",31,96,2976]
["","","QUERCUS VIRGINIANA; LIVE OAK 8-10 2 1/2\"","CALIPER 30 CONTAINER",13,286,3718]
["","","ROSA 'RADTKO'; RED DBL","KNOCKOUT ROSE 18-24\" 3 CONT",4,23,92]
["","","SCHIZACHYRIUM SCOPARIUM;","LITTLE BLUESTEM 1 CONTAINER",43,26,1118]
["","","SPIRAEA JAPONICA 'GOLDMOUND'; GOLD-","MOUND SPIRAEA 12-15\" 3 CONT",11,16,176]
["","","TAXODIUM DISTICHUM; BALD","CYPRESS 6-8' 2\" CALIPER 15CONT",29,108,3132]
["6645000000-N","GENERIC PLANTING ITEM (EA)","BOULDERS","",30,105,3150]
["","","STEPPING STONE","",5,40,200]
["6650000000-E","MULCH FOR PLANTING","","",315,37.047619048000001,11670]
["6655000000-E","H2O FOR PLANTING","","",29,287.06896551699998,8325]
["6665000000-E","POSTEMERGENT HERBICIDAL TRTMT","","",2845,0.181458699,516.25]
["6670000000-E","PREEMERGENT HERBICIDAL TRTMT","","",2845,0.29569420000000002,841.25]
["6674000000-N","GENERIC PLANTING ITEM (LS)","BOULDER H2O FEATURE","",1,51000,51000]
["","","LANDSCAPE PLANTING (NBL)","",1,12600,12600]
["","","LANDSCAPE PLANTING (SBL)","",1,64600,64600]
["","","SPEC SIDEWALK CLVT","",1,4100,4100]
["","","STREAMBANK BUFFER REFOREST-","ATION PLANTING",1,8000,8000]
["6675000000-E","GENERIC PLANTING ITEM (SY)","SODDING","",2600,4.5,11700]
["6676000000-E","GENERIC PLANTING ITEM (SF)","PAVERS","",2130,12,25560]
["","","SEGMTED RET WALL","",350,75,26250]
["6677000000-E","GENERIC PLANTING ITEM (TON)","RIVER STONE","",11,227.27272727299999,2500]
["6680000000-E","GENERIC PLANTING ITEM (CY)","12 MONTH AGED HARDWOOD MULCH","",190,50,9500]
["6690000000-E","GENERIC PLANTING ITEM (LF)","LANDSCAPE METAL EDGING","",184,6,1104]
["","","TREE PROTECTION FEN","",300,1.3,390]
["","","WORMSTYLE FENCING","",1350,26,35100]
["6890000000-E","CONC STEPS","","",6,720,4320]
["6895000000-E","HANDRAIL ON STEPS","","",28,200,5600]
["6900000000-E","TOPSOIL","","",700,25.428571429000002,17800]
["6905000000-N","PICNIC TABLE TERRZO &STL","","",7,4124.5714285710001,28872]
["6910000000-N","PICNIC SHELTER 1 TABLE","","",3,15173,45519]
["6915000000-N","OUTDOOR PARK STOVE","","",2,2550,5100]
["6945000000-E","3/4\"POST YARD HYDRNT","","",3,525,1575]
["6970000000-N","GENERIC REST AREA ITEM (EA)","BICYLE PARKING BOLLARD","",2,832.5,1665]
["","","DEPRESSED CURB HANDICAP","ACCESS 28' X 6'",1,1420,1420]
["","","","ACCESS 60' X 8'",1,3145,3145]
["","","FLAGPOLE","",3,3350,10050]
["","","FLAGPOLE & SIGN LIGHTING","",4,2150,8600]
["","","PICNIC SHELTER SINGLE PICNIC","TABLE STONE VENEER BASE",5,25000,125000]
["","","PLACEMT OF BOULDERS","",8,230,1840]
["","","RECYCLING CONTAINER","",20,869,17380]
["","","SITTING BENCH","",7,1750,12250]
["","","TAPERED ALUMINUM FLAG POLE","",1,2836.05,2836.05]
["","","WASTE CONTAINER","",20,826.5,16530]
["","","WHEEL STOPS @ H/C PARKING","",8,73,584]
["6975000000-N","GENERIC REST AREA ITEM (LS)","(NBL) REST AREA - SOLAR H2O","HEATING SYSTEM",1,20000,20000]
["","","(SBL) REST AREA - SOLAR H2O","HEATING SYSTEM",1,20000,20000]
["","","ELECTRICAL INSTALL FOR","(NBL) REST AREA BLDG",1,60100,60100]
["","","","(SBL) REST AREA BLDG",1,90500,90500]
["","","","(SBL) STORAGE BLDG",1,5650,5650]
["","","","REST AREA BLDG",1,101926,101926]
["","","","STORAGE BLDG",1,4995,4995]
["","","GENERAL CONST OF","REST AREA BLDG",1,541504,541504]
["","","","STORAGE BLDG",1,53245,53245]
["","","GENERAL CONST OF (SBL)","REST AREA BLDG",1,520000,520000]
["","","","STORAGE BLDG",1,37750,37750]
["","","GENERAL RENOVATION OF (NBL)","REST AREA BLDG",1,410000,410000]
["","","IRRIGATION SYSTEM","",1,59415.93,59415.93]
["","","LANDSCAPE GRADING","",1,2341.71,2341.71]
["","","LANDSCAPE GRADING (NBL)","",1,1700,1700]
["","","LANDSCAPE GRADING (SBL)","",1,12650,12650]
["","","MECHANICAL INSTALL FOR","(NBL) REST AREA BLDG",1,30600,30600]
["","","","(SBL) REST AREA BLDG",1,48500,48500]
["","","","REST AREA BLDG",1,123543,123543]
["","","PLUMBING INSTALL OF (NBL)","REST AREA BLDG",1,143300,143300]
["","","PLUMBING INSTALL OF (SBL)","REST AREA BLDG",1,192900,192900]
["","","PLUMBING INSTALL OF REST","AREA BLDG",1,99678,99678]
["","","RAINH2O COLLECTION SYSTEM","",1,33260.22,33260.22]
["","","REST AREA SOLAR H2O HEATING","SYSTEM",1,16100,16100]
["","","SITE DEMOLITION (NBL)","",1,15000,15000]
["","","SPEC REST AREA SIGNAGE","",1,35500,35500]
["","","STORMH2O DRNG SYSTEM (NBL)","",1,16600,16600]
["","","STORMH2O DRNG SYSTEM (SBL)","",1,24500,24500]
["6980000000-E","GENERIC REST AREA ITEM (LF)","3\" PVC UTILITY SLEEVE","",140,12,1680]
["","","6' WOOD FEN","",18,70,1260]
["","","LANDSCAPE METAL EDGING","",1790,4.5,8055]
["","","STONE SEATWALL","",470,275,129250]
["6982000000-E","GENERIC REST AREA ITEM (SF)","COMPOSITE DECKING","",864,12.21,10549.44]
["7000000000-E","PEDEST SIG HEAD (**************)","(16\" 1 SECTION W/ COUNTDOWN &","PUSHBUTTON INDICATOR LIGHT)",32,995,31840]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",68,798.71470588199998,54312.6]
["7060000000-E","SGL CABLE","","",121431,2.3622522259999998,286850.65000000002]
["7120000000-E","VEH SGL HD (12\" 3 SECT)","","",665,722.62042105299997,480542.58]
["7132000000-E","VEH SGL HD (12\" 4 SECT)","","",77,870.17792207800005,67003.7]
["7144000000-E","VEH SGL HD (12\" 5 SECT)","","",43,1082.7116279070001,46556.6]
["7204000000-N","LOUVER","","",2,206,412]
["7216000000-N","MODIFY EXT VEHIC SIGNL HD","","",2,220,440]
["7252000000-E","MESSENGER CABLE (1/4\")","","",30609,2.2550690969999998,69025.41]
["7264000000-E","MESSENGER CABLE (3/8\")","","",28639,2.5294790319999998,72441.75]
["7276000000-E","BORE & JACK (***********)","(1 6\")","",270,80.760000000000005,21805.200000000001]
["7279000000-E","TRACER WIRE","","",140181,0.492242815,69003.09]
["7288000000-E","PAVED TRENCH (*********)","(1 2\")","",275,8.4545454549999999,2325]
["7300000000-E","UNPAVED TRENCH (******)","(1 1\")","",370,6,2220]
["","","(1 2\")","",34881,5.418064276,188987.5]
["","","(1 5\")","",250,10.3,2575]
["","","(1-2\")","",690,5.5,3795]
["","","(2 2\")","",19021,7.045339362,134009.4]
["","","(21-1/2\")","",1815,8.75,15881.25]
["","","(2-2\")","",80,7,560]
["","","(3-2\")","",25,8,200]
["","","(4 1-1/4\")","",34810,5.9450359089999996,206946.7]
["","","(4 2\")","",85,7.1676470590000001,609.25]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",14385,3.547897115,51036.5]
["7301000000-E","DIRECT DRILL (***********)","(1 2\")","",12886,11.187667235999999,144164.28]
["","","(2 1-1/2\")","",1585,19,30115]
["","","(2 125\")","",300,27,8100]
["","","(2 2\")","",17434,15.513675002999999,270465.40999999997]
["","","(3 2\")","",1185,22.635443037999998,26823]
["","","(4 1-1/4\")","",2590,15.815714286,40962.699999999997]
["","","(4 2\")","",45,72.75,3273.75]
["","","(5 2\")","",110,32.75,3602.5]
["","","(7 2\")","",90,37.5,3375]
["7312000000-N","JUNCT BOX (***************)","(SPEC OVERSIZED)","",7,1146.19,8023.33]
["","","(SPEC SIZED)","",11,1224.46,13469.06]
["","","(SPEC-SIZED)","",8,707,5656]
["7324000000-N","JUNCT BOX (STD SIZE)","","",629,261.27340222599997,164340.97]
["7348000000-N","JUNCT BOX (OVER-SIZED HVY-DUTY)","","",307,539.052149837,165489.01]
["7360000000-N","WOOD POLE","","",242,763.75,184827.5]
["7372000000-N","GUY ASSEM","","",322,328.07211180100001,105639.22]
["7384000000-E","***\" RISER W/ **************","(1-1/2\" WEATHERHEAD)","",7,466.42857142899999,3265]
["","","(1-1/4\" WEATHERHEAD)","",3,235.49,706.47]
["7396000000-E","1/2\" RISER W/ WEATHERHEAD","","",3,175,525]
["7408000000-E","1\" RISER W/ WEATHERHEAD","","",30,327.66666666700002,9830]
["7420000000-E","2\" RISER W/ WEATHERHEAD","","",186,399.35521505399998,74280.070000000007]
["7432000000-E","2\" RISER W/ TUBING","","",35,395.25714285700002,13834]
["7444000000-E","INDUCTVE LOOP SAWCUT","","",227849,5.3182184250000004,1211750.75]
["7456000000-E","LEAD-IN CABLE(********)","(14-12)","",17808,1.3,23150.400000000001]
["","","(14-2)","",235575,1.1820016980000001,278450.05]
["7481000000-N","SITE SURVEY","","",9,384.82222222199999,3463.4]
["7481240000-N","CAMERA W/O INT LOOP EMUL PORCESS","","",30,2331.8333333330002,69955]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",9,7118.6888888889998,64068.2]
["7481280000-N","RELOC CAMERA SENSOR UNIT","","",6,585,3510]
["7484000000-N","MICROWAVE VEH DETECTOR","","",5,1680,8400]
["7485000000-N","WRLESS MAGN SENSOR DET SYS","","",1,13500,13500]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",32150,1.7028678070000001,54747.199999999997]
["","","(144)","",97023,2.279764283,221189.57]
["","","(24)","",8020,1.95,15639]
["","","(36)","",8200,12.85,105370]
["","","(72)","",38471,1.9453700190000001,74840.33]
["7528000000-E","DROP CABLE","","",13989,1.389773393,19441.54]
["7540000000-N","SPLICE ENCLOSURE","","",50,1933.8456000000001,96692.28]
["7541000000-N","MOD SPLICE ENCLOSURE","","",9,1665.5822222219999,14990.24]
["7552000000-N","INTERCONNECT CENTER","","",53,1114.455660377,59066.15]
["7564000000-N","FIBER-OPTIC TRANS DROP/REP","","",14,1796.6571428570001,25153.200000000001]
["7564100000-N","FIBER-OPTIC TRANS SELF HEAL","","",4,1990,7960]
["7566000000-N","DELINEATOR MARKER","","",243,83.870164609,20380.45]
["7575140000-N","FIBER-OPTIC SPLICE CBNT (BASE MTD)","","",2,2825,5650]
["7575142000-N","900MHZ RADIO","","",26,3407.4223076919998,88592.98]
["7575142060-N","MOD RADIO INSTALL","","",10,828.11,8281.1]
["7575142200-N","NEW ELECTRICL SERVICE","","",18,1900.42,34207.56]
["7575160000-E","REM EXT COMM CABLE","","",52251,0.94825974599999996,49547.519999999997]
["7575180000-N","CABLE TRANSFER","","",9,151.66666666699999,1365]
["7576000000-N","METAL STRAIN SGL POLE","","",91,7163.8351648349999,651909]
["7588000000-N","SGNL MAST ARM W/ METAL POLE","","",30,11552.863333333,346585.9]
["7590000000-N","DBL MAST ARM W/ METAL POLE","","",9,16065.866666667,144592.79999999999]
["7613000000-N","SOIL TEST","","",160,818.68600000000004,130989.75999999999]
["7614100000-E","DRILLED PIER FOUND","","",1055,728.68024644499997,768757.66]
["7630000000-N","METAL STRAIN POLE DESIGN","","",8,50,400]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",39,86.076923077000004,3357]
["7636000000-N","SIGN FOR SGLS","","",161,372.15745341600001,59917.35]
["7642100000-N","I POST W/ FOUND","","",12,930.83333333300004,11170]
["7642200000-N","II PED W/ FOUND","","",76,1252.1052631580001,95160]
["7648000000-N","RELOC EXT SIGN","","",5,187.95,939.75]
["7684000000-N","SGL CBNT FOUND","","",52,965.35615384599998,50198.52]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",2,307.60000000000002,615.20000000000005]
["7744000000-N","DETECTOR CARD (170)","","",78,120,9360]
["7756000000-N","CONTLR W/ CBNT 2070L BASE MTD","","",52,11633.577307692,604946.02]
["7768000000-N","CONTLR W/ CBNT 2070L POLE MTD","","",6,11175,67050]
["7780000000-N","DETECTOR CARD (2070L)","","",299,104.364080268,31204.86]
["7901000000-N","CBNT BASE EXTENDER","","",52,371.29076923100001,19307.12]
["7948000000-N","TRAF SGL REML","","",7,1371.414285714,9599.9]
["7960000000-N","METAL POLE FOUND REMVL","","",16,700.625,11210]
["7972000000-N","METAL POLE REML","","",20,312.35000000000002,6247]
["7980000000-N","GENERIC SGL ITEM (EA)","10KVA SINGLE PHASE TRANSFORMER","",6,1390.89,8345.34]
["","","5/8\" X 10' GROUNDING ELECTRODE","",216,115.066851852,24854.44]
["","","6\" X 6\" WOOD PEDESTAL","",2,624,1248]
["","","AVI ANTENNA","",6,2500,15000]
["","","AVI READER","",6,4165,24990]
["","","BACK FILL JUNCT BOX","",5,450,2250]
["","","BASE MOUNTED EQUIP CBNT","",3,2500,7500]
["","","CARD CAGES","",1,2476.9,2476.9]
["","","CCTV CBNT","",10,3819.7,38197]
["","","CCTV CAMERA ASSEM","",10,4862.8,48628]
["","","CCTV CAMERA ASSEM","(FIXED MOUNT)",3,1700,5100]
["","","","",25,4115.4480000000003,102886.2]
["","","CCTV CAMERA LOWERING SYSTEM","",8,6580.9224999999997,52647.38]
["","","CCTV EQUIP REML","",2,1135,2270]
["","","CCTV EXTENSION POLE","",2,2899.73,5799.46]
["","","CCTV FIELD EQUIP CBNT","",5,4012.11,20060.55]
["","","CCTV METAL POLE","",12,4007.375,48088.5]
["","","CCTV METAL POLE (50')","",2,11476.67,22953.34]
["","","CCTV METAL POLE (70')","",2,14369.26,28738.52]
["","","CCTV METAL POLE 50'","",1,7780,7780]
["","","CCTV METAL POLE 70'","",1,17400,17400]
["","","CCTV METAL POLE REML","",2,915,1830]
["","","CCTV WOOD POLE","",12,1432.0833333329999,17185]
["","","CENTRAL MEDIA CONVR","",6,410,2460]
["","","CENTRAL MEDIA CONVR","",1,1250,1250]
["","","CENTRAL VIDEO CODEC UNIT","",13,2007.8269230769999,26101.75]
["","","COMMUNICATIONS RACK","",1,2764.95,2764.95]
["","","COMPUTER WORKSTA (INSTALL)","",4,3335,13340]
["","","DIGITAL HARDWARE VIDEO DECODER","",6,2102.0100000000002,12612.06]
["","","DIGITAL HARDWARE VIDEO ENCODER","",14,2366.5757142860002,33132.06]
["","","DMS","",13,73612.969230768998,956968.6]
["","","DMS ACCESS LADDER","",15,5065.8059999999996,75987.09]
["","","DMS OVRHD ASSEM","",1,56788.63,56788.63]
["","","DMS PEDESTAL ASSEM","",2,52912.63,105825.26]
["","","DMS PEDESTAL STR","",5,38995.71,194978.55]
["","","DMS PEDESTAL STR (A)","",4,45700,182800]
["","","DMS PEDESTAL STR (B)","",1,54500,54500]
["","","DMS PEDESTAL STR(A)","",1,45000,45000]
["","","DMS PEDESTAL STR(B)","",1,48000,48000]
["","","DMS PEDESTAL STR","",1,22930,22930]
["","","DROP CABLE ASSEM","",1,1015,1015]
["","","DYNAMIC MESSAG SIGN","",3,69600.67,208802.01]
["","","ENCLOSED COMMUNICATIONS RACK","",3,3780,11340]
["","","EQUIP CBNT BASE EXTEND-ER","",2,807.93,1615.86]
["","","EQUIP CBNT DISCONNECT","",38,517.28578947400001,19656.86]
["","","EQUIP CBNT FOUND","",5,1184.8040000000001,5924.02]
["","","ETHERNET EDGE SWITCH","",21,1455.585238095,30567.29]
["","","FIELD EQUIP CBNT","",20,3972,79440]
["","","FIELD ETHERNET SWITCH","",16,1123.0325,17968.52]
["","","FIELD VIDEO CODEC UNIT","",8,2500,20000]
["","","FIELD VIDEO ENCODER","",2,2215,4430]
["","","FURN CCTV ASSEM","",1,2791.3,2791.3]
["","","FURN DIGITAL HARDWARE ","VIDEODECODER",2,1919.02,3838.04]
["","","FURN DIGITAL HARDWARE ","VIDEOENCODER",2,1919.02,3838.04]
["","","FURN ETHERNET EDGE SWITCH","",1,930.43,930.43]
["","","HUB CBNT","",1,11899.91,11899.91]
["","","HUB SPLICE CENTER","",1,24836.959999999999,24836.959999999999]
["","","INDUSTRIAL ETHERNET SWITCH","",2,1723,3446]
["","","INTERCONNECT CENTER","(144-FIBER)",1,3153.51,3153.51]
["","","INTERCONNECT CENTER (12-FIBER)","",7,1010.69,7074.83]
["","","INTERCONNECT CENTER (72-FIBER)","",1,2265.5100000000002,2265.5100000000002]
["","","JUNCT BOX (OVER-SIZD)","",27,707,19089]
["","","JUNCT BOX (SPEC OVER-","SIZED HEAVY-DUTY)",7,2100,14700]
["","","LANE CNTRL SGL","",4,5000,20000]
["","","MANAGED ETHERNET CORE SWITCH","MODIFICATIONS",1,19565.22,19565.22]
["","","MANAGED ETHERNET ROUTING SWITCH","",1,28695.65,28695.65]
["","","MANAGED ETHERNET SWITCH","",1,49350,49350]
["","","METAL POLE W/ HINGED MAST ARM","",5,8145,40725]
["","","METAL POLE W/ HINGED MAST ARM DESIGN","",5,3030,15150]
["","","METAL POLE W/ MONOTUBE","GANTRY STR",2,21530,43060]
["","","","GANTRY STR DESIGN",2,1010,2020]
["","","METER BASE/DISCONNECT","COMBINATION PANEL",2,738,1476]
["","","METER BASE/ DISCONNECT COMBIN-","ATION PANEL",8,500,4000]
["","","METER BASE/ DISCONNECT COMBINA-","TION PANEL",3,1204.3699999999999,3613.11]
["","","METER BASE/ DISCONNECT COMBINA-","TION PANEL",9,700,6300]
["","","MICROWAVE VEH DETECTION","SYSTEM-MULTIPLE ZONES",1,5750,5750]
["","","MICROWAVE VEH DETECTION SYSTEM","",2,9450,18900]
["","","MICROWAVE VEH DETECTOR-","SINGLE ZONE",2,1520,3040]
["","","MODIFY EXT ELECTRICAL","SERVICE EQUIP",3,755.76,2267.2800000000002]
["","","MODIFY NETWORK MANAGEMT SOFTWARE","",1,1250,1250]
["","","MVD METAL POLE","",1,2025,2025]
["","","MVD POLE FOUND REML","",2,680,1360]
["","","MVD RELOCD TO NEW CCTV METAL POLE","",1,1385,1385]
["","","MVD RELOCD TO NEW METAL MVD POLE","",1,1385,1385]
["","","NEW ELECTRICAL SERVICE (OVER- HEAD)","",1,950,950]
["","","NEW ELECTRICAL SERVICE (UNDER-","GROUND)",1,885,885]
["","","OPTICALLY ACTIVATED TRAF","SGL PRIORITY CNTRL SYSTEM",1,17200,17200]
["","","OVER-HEIGHT VEH DETECTION SYSTEM","",2,14650,29300]
["","","PATCH PANEL (ETHERNET)","",12,720,8640]
["","","PIEZOELECTRIC AXLE SENSOR","",6,1670,10020]
["","","PIEZOELECTRIC QUARTZ SENSOR SET","",6,7325,43950]
["","","POLE MOUNTED EQUIP CBNT","",5,1515,7575]
["","","PORT CCTV","",1,37853.26,37853.26]
["","","PORT CCTV CAMERA LOWERING TOOL","",1,1613.65,1613.65]
["","","PORT CCTV LOWERING TOOL","",2,1700.21,3400.42]
["","","POWDER COAT FOR SINGLE MAST","ARM POLE (COLOR BLACK)",4,910,3640]
["","","PRINTER (INSTALL)","",1,2930,2930]
["","","PROTECTIVE BLACK COATING FOR","METAL STRAIN POLE ASSEM",4,760,3040]
["","","","PEDESTRIAN SGL PEDESTAL",16,62,992]
["","","","SINGLE MAST ARM ASSEM",6,1600,9600]
["","","PROTECTIVE HUNTER GREEN COAT-","ING FOR DUAL MAST ARM ASSEM",2,1596.8,3193.6]
["","","","ING FOR SGL MST ARM ASSEM",15,1313.5,19702.5]
["","","RECTANGULAR RAPID FLASHING","BEACON ASSEM",4,5840,23360]
["","","SERVER (INSTALL)","",2,2525,5050]
["","","SERVICE DISCONNECT","",4,335,1340]
["","","SGL EQUIP CBNT DISCONNECT","",1,1150,1150]
["","","SOLAR POWER ASSEM","",2,12194.81,24389.62]
["","","SPLICE CENTER (36-FIBER)","",1,2930,2930]
["","","STL PEDESTAL POLE","",3,9270,27810]
["","","STRAIN POLE ASSEM W/","PROTECTIVE COATING",4,1044,4176]
["","","UPS","",7,986.09428571399997,6902.66]
["","","VEH SGL HEAD","(12\" 2-SECTION RED-GREEN)",6,2600,15600]
["","","VIDEO ETHERNET DECODER","",4,825,3300]
["","","VIDEO ETHERNET ENCODER","",8,800,6400]
["","","WALL-MOUNTED COMMUNICATIONS RACK","",1,3780,3780]
["","","WOOD PEDESTAL","",12,226.66666666699999,2720]
["7985000000-N","GENERIC SGL ITEM (LS)","ADVANCE LOCATION WIM ELECTRON-ICS","",1,139400,139400]
["","","ALPR SYSTEM","",1,78800,78800]
["","","CCTV SOFTWARE","",1,7080,7080]
["","","CENTRAL CNTRL SOFTWARE","",1,14650,14650]
["","","COMPLIANCE LOCATION WIM ELEC- TRONICS","",1,139400,139400]
["","","DMS","",1,91600,91600]
["","","DMS (REM & REINSTALL)","",1,121290.76,121290.76]
["","","INTEGRATION & CONFIGURATION","",3,5391.2666666670002,16173.8]
["","","NETWORK MANAGEMT SOFTWARE","",1,10355,10355]
["","","OPEN/CLOSED DMS PANEL","",1,8335,8335]
["","","SCALE HOUSE WIM ELECTRONICS","",1,139400,139400]
["","","SYSTEM WARRANTY","",1,36400,36400]
["","","TRAINING","",1,8335,8335]
["7990000000-E","GENERIC SGL ITEM (LF)","4 AWG SOLID BARE COPPER","GROUNDING CONDUCTOR",80,2.0299999999999998,162.4]
["","","4 SOLID BARE COPPER GROUNDINGCONDUCTOR","",20,410,8200]
["","","4 SOLID BARE GROUNDING CON- DUCTOR","",1380,3.4675362320000001,4785.2]
["","","6 AWG 3-WIRE COPPER FEEDER CONDUCTORS","",200,5,1000]
["","","3-WIRE COPPER FEEDER CONDUCTORS","",1820,3.0626373629999999,5574]
["","","3-WIRE COPPER FEEDER CONDUC- TORS","",1895,1.75,3316.25]
["","","3-WIRE COPPER FEEDER CONDUCT- ORS","",1430,3.18,4547.3999999999996]
["","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",265,9.2377358489999999,2448]
["","","3-WIRE FEEDER CONDUCTORS","",3178,4.12,13093.36]
["","","4-WIRE COPPER FEEDER CONDUCTORS","",340,3.65,1241]
["","","4-WIRE COPPER FEEDER CONDUC- TORS","",1630,15,24450]
["","","4-WIRE COPPER FEEDER CONDUCT -ORS","",1820,4.68,8517.6]
["","","4-WIRE COPPER FEEDER CONDUCT- ORS","",600,9,5400]
["","","4-WIRE FEEDER CONDUCTORS","",785,10.130000000000001,7952.05]
["","","BACK PULL FIBER OPTIC CABLE","",1800,2.8055555559999998,5050]
["","","DROP CABLE (6 FIBER)","",1819,10.1,18371.900000000001]
["","","ETHERNET CABLE","",1455,0.6104811,888.25]
["","","FOUR-WIRE COPPER FEEDER CON- DUCTORS","",2536,12.55,31826.799999999999]
["","","LEAD-IN CABLE","",228,3.05,695.4]
["","","TWO-WAY CONC DUCTBANK (ACP)","",1760,47,82720]
["","","UNDERGROUND CONDUIT (1 2\")","",3214,5.2743777219999997,16951.849999999999]
["","","UNDERGROUND CONDUIT (2 2\")","",29109,6.6396341339999996,193273.11]
["","","UNDERGROUND CONDUIT (3 2\")","",1917,10.1,19361.7]
["","","UNDERGROUND CONDUIT (4 2\")","",85,18.2,1547]
["7992000000-E","GENERIC SGL ITEM (CY)","DMS FOUND","",24,775.04,18600.96]
["","","DMS OVRHD FOOTINGS","",8,1010,8080]
["","","ITS OVRHD FOOTING","",40,725,29000]
["","","ITS OVRHD FOOTINGS","",16,800,12800]
["","","OVRHD FOOTINGS","",16,910,14560]
["","","OVRHD SIGN ASSEM","FOOTINGS",16,789.79,12636.64]
["8007000000-N","CM&R TEMP STR ***********","(13+0130-L-)","",1,165000,165000]
["","","(15+1600-L-)","",1,135000,135000]
["","","(15+6700-L-)","",1,181200,181200]
["","","(20+0300-L-)","",1,266160,266160]
["","","(34+6288-DFEB- WID)","",1,739747.67,739747.67]
["8017000000-N","CM&R TEMP ACCESS ****","(10+5800-L-)","",1,66400,66400]
["","","(11+9750-L-)","",1,21100,21100]
["","","(122+2250-L-LT)","",1,62869.31,62869.31]
["","","(14+8300-L-)","",1,15000,15000]
["","","(15+0900 -L-)","",1,8000,8000]
["","","(20+0300-L-)","",1,1.07,1.07]
["","","(20+2050-L-)","",1,25000,25000]
["","","(20+4750-L-)","",1,25000,25000]
["","","(20+9200-L-)","",1,27000,27000]
["","","(265+5358-L-)","",1,625000,625000]
["","","(27+1172-L-)","",1,175000,175000]
["","","(32+1850-L-)","",1,67000,67000]
["","","(339+4856-L-EBL)","",1,45900,45900]
["","","(339+4856-L-WBL)","",1,45900,45900]
["","","(45+0787 -RP1C-)","",1,600000,600000]
["","","(46+2150-L-)","",1,4456070.0199999996,4456070.0199999996]
["","","(48+7900-Y8-)","",1,625000,625000]
["","","(57+0700 -RP1DB-)","",1,5000,5000]
["","","(826+1500 -L- LT)","",1,700000,700000]
["","","(898+2000 -L- LT)","",1,800000,800000]
["","","(94+2458 -L- LT)","",1,900000,900000]
["8021000000-N","REMV EXIST STR **********","(13+0130-L-)","",1,25000,25000]
["","","(13+5295 -L-)","",1,112000,112000]
["","","(14+1200-L-)","",1,50000,50000]
["","","(14+3500 -L-)","",1,30000,30000]
["","","(14+6600-L-)","",1,30000,30000]
["","","(15+1600-L-)","",1,30000,30000]
["","","(16+0000-L-)","",1,12000,12000]
["","","(16+0250-L-)","",1,70000,70000]
["","","(16+8350-L-)","",1,25000,25000]
["","","(17+8640-L-)","",1,60000,60000]
["","","(18+7500-L-)","",1,25000,25000]
["","","(27+1172-L-)","",1,570500,570500]
["","","(30+00 -Y7- RAMP C)","",1,58004.71,58004.71]
["","","(46+2150-L-)","",1,800000,800000]
["8035000000-N","REMV EXIST STR **********","(10+5800-L-)","",1,12000,12000]
["","","(11+9750-L-)","",1,32500,32500]
["","","(12+8100-L2-)","",1,10000,10000]
["","","(122+2250-L-LT)","",1,134124.97,134124.97]
["","","(13+6150-L-)","",1,8069.39,8069.39]
["","","(13+8500-L-)","",1,35800,35800]
["","","(14+8300-L-)","",1,40000,40000]
["","","(14-6276-L1-)","",1,103500,103500]
["","","(15+0800-L-)","",1,49000,49000]
["","","(15+0900 -L-)","",1,22000,22000]
["","","(15+1400-L-)","",1,39500,39500]
["","","(15+1600-L-)","",1,66000,66000]
["","","(15+6450-L-)","",1,48000,48000]
["","","(15+6600 -L-)","",1,33500,33500]
["","","(15+6700-L-)","",1,150000,150000]
["","","(15+6728-L-)","",1,133500,133500]
["","","(16+1350 -L-)","",1,14350,14350]
["","","(16+2900-L-)","",1,20000,20000]
["","","(16+6429-L-)","",1,45225,45225]
["","","(16+8800-L-)","",1,22790,22790]
["","","(17+2700 -L-)","",1,95000,95000]
["","","(17+4500-L-)","",1,32000,32000]
["","","(17+6800 -L-)","",1,46482,46482]
["","","(17+7300-L-)","",1,30000,30000]
["","","(18+6650 -L-)","",1,32500,32500]
["","","(20+2050-L-)","",1,60000,60000]
["","","(20+4750-L-)","",1,60000,60000]
["","","(20+9200-L-)","",1,75000,75000]
["","","(21+7700-L-)","",1,36000,36000]
["","","(23+2500-L-)","",1,75000,75000]
["","","(24+1131-L-RT)","",1,63872.18,63872.18]
["","","(24+7018-DFWB- WID)","",1,31390.92,31390.92]
["","","(247+8750-L-LT)","",1,14577.88,14577.88]
["","","(247+8750-L-RT)","",1,42568.55,42568.55]
["","","(26+1600-L-)","",1,34100,34100]
["","","(26+1764-Y22-LT)","",1,200000,200000]
["","","(26+2165-L-RT)","",1,25000,25000]
["","","(27+6050-L-)","",1,35000,35000]
["","","(28+5089-RRDET-)","",1,98508.06,98508.06]
["","","(32+1850-L-)","",1,60000,60000]
["","","(339+4856-L-EBL)","",1,132600,132600]
["","","(34+6288-DFEB- WID)","",1,15995.46,15995.46]
["","","(36+6926-DFWB- WID)","",1,15995.46,15995.46]
["","","(393+5738-L-)","",1,35000,35000]
["","","(42+6093-L-)","",1,22000,22000]
["","","(67+1650 -L-)","",1,41500,41500]
["","","(71+5383-L-)","",1,25000,25000]
["8042000000-N","REMV EXIST STRS *********","(44+0860-L-)","",1,79050.3,79050.3]
["","","(64+7469-L-)","",1,83839,83839]
["8049000000-N","REMV EXIST STR **********","(13+4400-L-)","",1,10000,10000]
["","","(13+7141-L-)","",1,85000,85000]
["","","(20+0300-L-)","",1,76810,76810]
["","","(21+6900-L-)","",1,35000,35000]
["8056000000-N","REMV EXIST STR **********","(14+3400-L-)","",1,21000,21000]
["","","(15-8400-L-)","",1,35000,35000]
["","","(23+1100-Y1-)","",1,10000,10000]
["","","(28+1707-L-)","",1,285000,285000]
["","","(34+4500-Y3-)","",1,11000,11000]
["","","(442+1360-L-)","",1,10000,10000]
["","","(509+8300-L-)","",1,11000,11000]
["","","(53+9500-L-)","",1,10200,10200]
["","","(73+25 -L- LT)","",1,10000,10000]
["","","(77+0400-L-)","",1,10200,10200]
["8063000000-N","PC RCBC @ STA **********","(33+6500-L-)","",1,83300,83300]
["8070000000-E","FOUND EXCAV","","",1135,39.614537445000003,44962.5]
["8084000000-N","FND EXCAV EB** STA****","(01 38+5027-Y7-)","",1,10000,10000]
["","","(02 38+5027-Y7-)","",1,10000,10000]
["","","(252+9428-Y4RPBD-)","",1,6760.19,6760.19]
["","","(ABUT 1 18+8173-RR-)","",1,3000,3000]
["","","(ABUT 1 64+5550-L-)","",1,4870,4870]
["","","(ABUT 1 64+7469-L-)","",1,4870,4870]
["","","(ABUT 2 64+5550-L-)","",1,4870,4870]
["","","(ABUT 2 64+7469-L-)","",1,4870,4870]
["8091000000-N","FND EXCAV B** STA *****","(1 105+2900-L-)","",1,11859.38,11859.38]
["","","(1 14-6276-L1-)","",1,5000,5000]
["","","(1 15+6728-L-)","",1,6500,6500]
["","","(1 17+1000-Y4RPA-)","",1,6760.19,6760.19]
["","","(1 17+3000-L-)","",1,15000,15000]
["","","(1 203+5035-L-)","",1,2700,2700]
["","","(1 228+2381-L-)","",1,3500,3500]
["","","(1 24+7018-DFWB- WID)","",1,8522.52,8522.52]
["","","(1 247+9066-L-LT)","",1,3800,3800]
["","","(1 247+9066-L-RT)","",1,3800,3800]
["","","(1 26+1764-Y22-LT)","",1,65000,65000]
["","","(1 26+1764-Y22-RT)","",1,22000,22000]
["","","(1 268+2289-L-)","",1,55000,55000]
["","","(1 354+8322-L-)","",1,7000,7000]
["","","(1 378+9434-L-)","",1,6000,6000]
["","","(1 456+9933-L-)","",1,14000,14000]
["","","(1 482+1314 -L-)","",1,9804.2099999999991,9804.2099999999991]
["","","(1 516+3130-L-)","",1,5014.2700000000004,5014.2700000000004]
["","","(1 584+3624 -L-LT)","",1,10028.540000000001,10028.540000000001]
["","","(1 584+3624-L-RT)","",1,10028.540000000001,10028.540000000001]
["","","(1 765+2744 -L- LT)","",1,6600,6600]
["","","(1 765+2744 -L- RT)","",1,14000,14000]
["","","(1 80+7441-L-)","",1,3500,3500]
["","","(1 943+2158 -L-)","",1,34000,34000]
["","","(1 991+2318 -L-)","",1,30000,30000]
["","","(1138+4045-LDFEB-)","",1,6989.38,6989.38]
["","","(123+2961-DFFLY-)","",1,4743.75,4743.75]
["","","(128+5016-Y5-)","",1,5014.2700000000004,5014.2700000000004]
["","","(142+1023 -RP1B-)","",1,7200,7200]
["","","(144+0864-Y4RPBD-)","",1,9267.34,9267.34]
["","","(146+8716-Y4CD-)","",1,7521.39,7521.39]
["","","(152+9428-Y4RPBD-)","",1,6760.19,6760.19]
["","","(157+0700 -RP1DB-)","",1,75000,75000]
["","","(160+3713-L-)","",1,13395,13395]
["","","(1642+8142-L-LT)","",1,5014.2700000000004,5014.2700000000004]
["","","(1642+8142-L-RT)","",1,5014.2700000000004,5014.2700000000004]
["","","(17+9757-DFLW-)","",1,6989.38,6989.38]
["","","(2 105+2900-L-)","",1,8522.52,8522.52]
["","","(2 17+3000-L-)","",1,15000,15000]
["","","(2 23+2961-DFFLY-)","",1,4743.75,4743.75]
["","","(2 24+7018-DFWB-WID)","",1,11859.38,11859.38]
["","","(2 584+3624 -L-LT)","",1,10028.540000000001,10028.540000000001]
["","","(2 584+3624-L-RT)","",1,10028.540000000001,10028.540000000001]
["","","(2 628+6550-L-LT)","",1,6760.19,6760.19]
["","","(2 628+6550-L-RT)","",1,6760.19,6760.19]
["","","(228+5016-Y5-)","",1,5014.2700000000004,5014.2700000000004]
["","","(233+1567-Y4CD-)","",1,6760.19,6760.19]
["","","(242+1023 -RP1B-)","",1,7200,7200]
["","","(252+9428-Y4RPBD-)","",1,6760.19,6760.19]
["","","(257+0700 -RP1DB-)","",1,90000,90000]
["","","(260+3713-L-)","",1,12000,12000]
["","","(3 105+2900-L-)","",1,8522.52,8522.52]
["","","(3 14+9925-L-)","",1,18000,18000]
["","","(3 23+2961-DFFLY-)","",1,4743.75,4743.75]
["","","(328+5016-Y5-)","",1,5014.2700000000004,5014.2700000000004]
["","","(357+0700 -RP1DB-)","",1,60000,60000]
["","","(394+2458 -L- LT)","",1,8600,8600]
["","","(394+2458 -L- RT)","",1,8200,8200]
["","","(395+6454-L-)","",1,39000,39000]
["","","(4 14+9925-L-)","",1,12000,12000]
["","","(4 17+1000-Y4RPA-)","",1,6760.19,6760.19]
["","","(4 23+2961-DFFLY-)","",1,4743.75,4743.75]
["","","(457+0700 -RP1DB-)","",1,23000,23000]
["","","(494+2458 -L- RT)","",1,8300,8300]
["","","(494+4384 -COL1-)","",1,16200,16200]
["","","(5 23+2961-DFFLY-)","",1,4743.75,4743.75]
["","","(557+0700 -RP1DB-)","",1,15200,15200]
["","","(594+4384 -COL1-)","",1,16200,16200]
["","","(657+0700 -RP1DB-)","",1,130000,130000]
["","","(757+0700 -RP1DB-)","",1,143000,143000]
["","","(857+0700 -RP1DB-)","",1,143000,143000]
["","","(957+0700 -RP1DB-)","",1,10000,10000]
["8096000000-E","PILE EXCAV IN SOIL","","",925,301.31069189200002,278712.39]
["8097000000-E","PILE EXCAV NOT IN SOIL","","",961,401.12,385476.32]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",1387.9,740.47071114599999,1027699.3]
["","","(5'-0\")","",416,511.57499999999999,212815.2]
["","","(5'-6\")","",440.6,561.87939173899997,247564.06]
["","","(8'-0\")","",199,1050,208950]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",1351.35,749.86865726899998,1013335.01]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",832.55,856.25504774499996,712875.14]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",1622.11,725.10191663900002,1176195.07]
["8105600000-E","**'-**\" DRILL PIER NO SOIL","(4'-6\")","",618,1153.3957605180001,712798.58]
["","","(5'-0\")","",133,1897.5127067670001,252369.19]
["","","(5'-6\")","",85,2603.1559999999999,221268.26]
["","","(8'-0\")","",232,3875,899000]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",904.5,875.28239911599997,791692.93]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",777,1025.0229086229999,796442.8]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",966,1471.3687784680001,1421342.24]
["8108000000-E","**'-**\" DIA DRILLD PIERS","(3'-0\")","",247,525,129675]
["","","(6'-0\")","",2424,700,1696800]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",563.5,299.481188997,168757.65]
["","","(5'-0\")","",204,503.72,102758.88]
["","","(5'-6\")","",72.599999999999994,550.66184572999998,39978.050000000003]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",756.9,180.81514070599999,136858.98000000001]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",504.92,245.787471283,124103.01]
["8111600000-E","PERM STL CASING FOR 4' PIER","","",168.95,281.15442438600002,47501.04]
["8112730000-N","PDA TESTING","","",115,2359.7866956520002,271375.46999999997]
["8113000000-N","SID INSPECTIONS","","",193,638.53906735800001,123238.04]
["8114000000-N","SPT TESTING","","",211,736.60132701400005,155422.88]
["8115000000-N","CSL TESTING","","",156,1879.3561538460001,293179.56]
["8121000000-N","UNCL STR EXCAV STA ***","(10+5800-L-)","",1,10000,10000]
["","","(11+0019-L-)","",1,6000,6000]
["","","(11+9750-L-)","",1,9500,9500]
["","","(12+8100-L2-)","",1,50000,50000]
["","","(122+2250-L-LT)","",1,10396.790000000001,10396.790000000001]
["","","(122+2250-L-RT)","",1,3465.61,3465.61]
["","","(13+0130-L-)","",1,17000,17000]
["","","(13+7141-L-)","",1,99000,99000]
["","","(13+8500-L-)","",1,6700,6700]
["","","(14+1200-L-)","",1,30000,30000]
["","","(14+3400-L-)","",1,33367.17,33367.17]
["","","(14+3500 -L-)","",1,7000,7000]
["","","(14+6600-L-)","",1,6950,6950]
["","","(14+8300-L-)","",1,5000,5000]
["","","(14+9925-L-)","",1,22000,22000]
["","","(15+0800-L-)","",1,10000,10000]
["","","(15+0900 -L-)","",1,15000,15000]
["","","(15+1400-L-)","",1,5700,5700]
["","","(15+1600-L-)","",1,5000,5000]
["","","(15+6450-L-)","",1,19500,19500]
["","","(15+6600 -L-)","",1,2450,2450]
["","","(15+6700-L-)","",1,18000,18000]
["","","(16+0250-L-)","",1,30000,30000]
["","","(16+0550-Y2-)","",1,35000,35000]
["","","(16+1350 -L-)","",1,5000,5000]
["","","(16+2900-L-)","",1,6500,6500]
["","","(16+6429-L-)","",1,3150,3150]
["","","(16+8350-L-)","",1,7500,7500]
["","","(16+8800-L-)","",1,10000,10000]
["","","(17+4500-L-)","",1,2800,2800]
["","","(17+6800 -L-)","",1,8200,8200]
["","","(17+7300-L-)","",1,20000,20000]
["","","(17+8640-L-)","",1,15000,15000]
["","","(18+6650 -L-)","",1,3360,3360]
["","","(18+7500-L)","",1,5000,5000]
["","","(20+0300-L-)","",1,3386,3386]
["","","(20+2050-L-)","",1,25000,25000]
["","","(20+4750-L-)","",1,25000,25000]
["","","(21+7700-L-)","",1,6900,6900]
["","","(23+2500-L-)","",1,30000,30000]
["","","(24+7018-DFWB- WID)","",1,4870,4870]
["","","(247+8750-L-LT)","",1,13862.38,13862.38]
["","","(247+8750-L-RT)","",1,55449.55,55449.55]
["","","(26+1600-L-)","",1,11550,11550]
["","","(26+1764-Y22-LT)","",1,14000,14000]
["","","(26+1764-Y22-RT)","",1,10000,10000]
["","","(268+2289-L-)","",1,14000,14000]
["","","(27+1172-L-)","",1,40250,40250]
["","","(27+6050-L-)","",1,6000,6000]
["","","(28+1707-L-)","",1,25000,25000]
["","","(28+5089-RRDET-)","",1,4870,4870]
["","","(32+1850-L-)","",1,31000,31000]
["","","(339+4856-L-EBL)","",1,30600,30600]
["","","(339+4856-L-WBL)","",1,7650,7650]
["","","(393+5738-L-)","",1,12000,12000]
["","","(44+0860-L-)","",1,4870,4870]
["","","(46+2150-L-)","",1,20000,20000]
["","","(71+5383-L-)","",1,10000,10000]
["8126000000-N","CULV EXCAV @ **********","(11+0796-Y34-)","",1,16455.84,16455.84]
["","","(11+4187-Y4-)","",1,6320,6320]
["","","(114+5500-L-)","",1,14000,14000]
["","","(13+4400-L-)","",1,17500,17500]
["","","(13+6150-L-)","",1,17477.59,17477.59]
["","","(133+4146-L-)","",1,44500,44500]
["","","(134+8045-L-)","",1,75608.19,75608.19]
["","","(14+7740-YLPD-)","",1,16000,16000]
["","","(14+9030-Y17-)","",1,28730.9,28730.9]
["","","(148+7300-L-)","",1,47800,47800]
["","","(15+1600-L-)","",1,15500,15500]
["","","(15-8400-L-)","",1,45000,45000]
["","","(153+4068 -L-)","",1,2550,2550]
["","","(155+4457-L-)","",1,42518.34,42518.34]
["","","(16+0000-L-)","",1,12000,12000]
["","","(188+0200-L-)","",1,30600,30600]
["","","(19+0728-Y4-)","",1,38500,38500]
["","","(204+3800-L-)","",1,35700,35700]
["","","(21+6900-L-)","",1,20000,20000]
["","","(218+0000-L-)","",1,13000,13000]
["","","(222+2043-L-)","",1,105254.37,105254.37]
["","","(23+1100-Y1-)","",1,37872.81,37872.81]
["","","(241+9600-L-)","",1,30000,30000]
["","","(283+6200-L-)","",1,45900,45900]
["","","(319+7616-L-)","",1,55149.760000000002,55149.760000000002]
["","","(323+5866-L-)","",1,41273.230000000003,41273.230000000003]
["","","(327+5047-L-)","",1,11029.95,11029.95]
["","","(33+6500-L-)","",1,35000,35000]
["","","(34+4500-Y3-)","",1,90000,90000]
["","","(345+9842-L-)","",1,16544.919999999998,16544.919999999998]
["","","(405+2806-L-)","",1,20000,20000]
["","","(43+8648-Y-)","",1,18000,18000]
["","","(44+192-L-)","",1,70093.22,70093.22]
["","","(442+1360-L-)","",1,18000,18000]
["","","(48+6500-L-)","",1,23000,23000]
["","","(509+8300-L-)","",1,64000,64000]
["","","(52+0900-Y7-)","",1,25000,25000]
["","","(52+4145-L-)","",1,1500,1500]
["","","(53+9500-L-)","",1,57120,57120]
["","","(559+7400-L-)","",1,31181.85,31181.85]
["","","(58+9800-L-)","",1,17000,17000]
["","","(616+4500-L-)","",1,56127.29,56127.29]
["","","(667+1500-L-)","",1,49890.93,49890.93]
["","","(77+0400-L-)","",1,51000,51000]
["","","(95+4849-L-)","",1,64000,64000]
["","","(STA 45+6543 -Y4-)","",1,12472.74,12472.74]
["8133000000-E","FND CONDIT MAT BOX CULV","","",12951.71,46.510903966000001,602395.74]
["8140000000-E","CHANNEL EXCAV","","",390,25,9750]
["8147000000-E","REINF CONC DECK SLAB","","",1977166.2,24.370353762000001,48184239.740000002]
["8154000000-E","REINF CONC DECK SLABLTWT","","",101104,31.469465105000001,3181688.8]
["8156000000-E","CONC WEARING SURF","","",48198.2,9.8438302679999996,474454.9]
["8161000000-E","GROOVING BRG FLOORS","","",2245938.2999999998,0.33280904500000003,747468.58]
["8175000000-E","CL AA CONC (BRG)","","",9142.2999999999993,603.96789648100003,5521655.7000000002]
["8182000000-E","CL A CONC (BRG)","","",33617.300000000003,757.62943603400004,25469456.039999999]
["8196000000-E","CL A CONC (CULV)","","",25662.6,409.89323957800002,10518926.25]
["8210000000-N","BRG APPR SLAB *********","(10+0000)","",1,30000,30000]
["","","(105+2900-L-)","",1,31848.69,31848.69]
["","","(107+4555-L-)","",1,42537.69,42537.69]
["","","(11+0019-L-)","",1,40000,40000]
["","","(11+9750-L-)","",1,17300,17300]
["","","(12+1950)","",1,74600,74600]
["","","(12+7150-L-)","",1,25000,25000]
["","","(12+8100-L2-)","",1,12000,12000]
["","","(122+2250-L-LT)","",1,43500,43500]
["","","(122+2250-L-RT)","",1,43500,43500]
["","","(123+8250-L-EBL)","",1,30426.6,30426.6]
["","","(123+8250-L-WBL)","",1,30600,30600]
["","","(125+9157-L-EBL)","",1,54954.55,54954.55]
["","","(125+9157-L-WBL)","",1,54656.34,54656.34]
["","","(129+3756-L-LT)","",1,40000,40000]
["","","(129+3756-L-RT)","",1,40000,40000]
["","","(13+0130-L-)","",1,25000,25000]
["","","(13+5295 -L-)","",1,30000,30000]
["","","(13+8500-L-)","",1,16850,16850]
["","","(138+4045-LDFEB-)","",1,32506.52,32506.52]
["","","(14+1200-L-)","",1,15595,15595]
["","","(14+3500 -L-)","",1,26000,26000]
["","","(14+6600-L-)","",1,11675,11675]
["","","(14+8300-L-)","",1,25000,25000]
["","","(14+9925-L-)","",1,40000,40000]
["","","(14-6276-L1-)","",1,21200,21200]
["","","(144+6063-L-)","",1,40000,40000]
["","","(144+9000-L-)","",1,40000,40000]
["","","(147+3889-L-LT)","",1,41000,41000]
["","","(147+3889-L-RT)","",1,41000,41000]
["","","(15+0800-L-)","",1,17400,17400]
["","","(15+0900 -L-)","",1,38000,38000]
["","","(15+1400-L-)","",1,18100,18100]
["","","(15+1600-L-)","",1,25000,25000]
["","","(15+6450-L-)","",1,8300,8300]
["","","(15+6600 -L-)","",1,17500,17500]
["","","(15+6700-L-)","",1,52000,52000]
["","","(15+6728-L-)","",1,32350,32350]
["","","(157+3378-LDFEB-)","",1,177183.93,177183.93]
["","","(157+7550-L-EBL)","",1,31500,31500]
["","","(157+7550-L-WBL)","",1,315400,315400]
["","","(16+0250-L-)","",1,20800,20800]
["","","(16+0550-Y2-)","",1,75000,75000]
["","","(16+1350 -L-)","",1,19000,19000]
["","","(16+2900-L-)","",1,16240,16240]
["","","(16+6429-L-)","",1,31100,31100]
["","","(16+8350-L-)","",1,25000,25000]
["","","(16+8800-L-)","",1,18000,18000]
["","","(17+1000-Y4RPA-)","",1,35486.080000000002,35486.080000000002]
["","","(17+2700 -L-)","",1,22000,22000]
["","","(17+4500-L-)","",1,16900,16900]
["","","(17+6800 -L-)","",1,18000,18000]
["","","(17+7300-L-)","",1,30000,30000]
["","","(17+8640-L-)","",1,25000,25000]
["","","(17+9757-DFLW-)","",1,51151.91,51151.91]
["","","(174+7246-L-LT)","",1,40000,40000]
["","","(174+7246-L-RT)","",1,40000,40000]
["","","(18+6650 -L-)","",1,18600,18600]
["","","(18+7500-L-)","",1,55000,55000]
["","","(182+9994-L-)","",1,46000,46000]
["","","(20+0300-L-)","",1,39220.47,39220.47]
["","","(20+2050-L-)","",1,70000,70000]
["","","(20+4750-L-)","",1,60000,60000]
["","","(20+9200-L-)","",1,11700,11700]
["","","(203+5035-L-)","",1,50000,50000]
["","","(21+0160 -PXROAD-)","",1,45000,45000]
["","","(21+7700-L-)","",1,11325,11325]
["","","(228+2381-L-)","",1,34000,34000]
["","","(23+2500-L-)","",1,50000,50000]
["","","(23+2961-DFFLY-)","",1,31737.599999999999,31737.599999999999]
["","","(23+5912-Y5-)","",1,33126.21,33126.21]
["","","(24+1131-L-LT)","",1,44500,44500]
["","","(24+1131-L-RT)","",1,44500,44500]
["","","(24+5904-L-)","",1,35000,35000]
["","","(24+7018-DFWB- WID)","",1,39529.550000000003,39529.550000000003]
["","","(247+8750-L-LT)","",1,44500,44500]
["","","(247+8750-L-RT)","",1,44500,44500]
["","","(247+9066-L-LT)","",1,39800,39800]
["","","(247+9066-L-RT)","",1,39800,39800]
["","","(252+7329-L-LT)","",1,38000,38000]
["","","(252+7329-L-RT)","",1,40500,40500]
["","","(26+1600-L-)","",1,20075,20075]
["","","(26+1764-Y22-LT)","",1,42000,42000]
["","","(26+1764-Y22-RT)","",1,35000,35000]
["","","(26+2165-L-LT)","",1,40000,40000]
["","","(26+2165-L-RT)","",1,15000,15000]
["","","(26+6000-Y4RPBD-)","",1,34220.639999999999,34220.639999999999]
["","","(265+5358-L-LT)","",1,41000,41000]
["","","(265+5358-L-RT)","",1,53000,53000]
["","","(268+2289-L-)","",1,45000,45000]
["","","(27+1172-L-)","",1,60000,60000]
["","","(27+6050-L-)","",1,17000,17000]
["","","(28+1707-L-)","",1,87500,87500]
["","","(28+5016-Y5-)","",1,32128.11,32128.11]
["","","(281+5183-L-LT)","",1,43000,43000]
["","","(281+5183-L-RT)","",1,40000,40000]
["","","(32+1850-L-)","",1,93000,93000]
["","","(33+1567-Y4CD-)","",1,26963.65,26963.65]
["","","(339+4856-L-EBL)","",1,29580,29580]
["","","(339+4856-L-WBL)","",1,29580,29580]
["","","(34+6288-DFEB- WID)","",1,59318.03,59318.03]
["","","(340+7000-L-LT)","",1,34900,34900]
["","","(340+7000-L-RT)","",1,34900,34900]
["","","(354+8322-L-)","",1,50000,50000]
["","","(36+6926-DFWB- WID)","",1,65612.45,65612.45]
["","","(378+9434-L-)","",1,20000,20000]
["","","(38+5027-Y7-)","",1,63000,63000]
["","","(393+5738-L-)","",1,31000,31000]
["","","(395+6454-L-)","",1,80000,80000]
["","","(42+1023 -RP1B-)","",1,32000,32000]
["","","(44+0860-L-)","",1,98699.73,98699.73]
["","","(44+0864-Y4RPBD-)","",1,36965.050000000003,36965.050000000003]
["","","(45+0787 -RP1C-)","",1,32000,32000]
["","","(456+9933-L-)","",1,34000,34000]
["","","(46+2150-L-)","",1,75000,75000]
["","","(46+7319 -L- LT)","",1,44875,44875]
["","","(46+7319 -L- RT)","",1,44875,44875]
["","","(46+8716-Y4CD-)","",1,42240.69,42240.69]
["","","(48+7900-Y8-)","",1,52000,52000]
["","","(482+1314-L-)","",1,84549.79,84549.79]
["","","(516+3130-L-)","",1,31554.36,31554.36]
["","","(52+9428-Y4RPBD-)","",1,35784.160000000003,35784.160000000003]
["","","(556+8500-L-LT)","",1,50431.63,50431.63]
["","","(556+8500-L-RT)","",1,50431.63,50431.63]
["","","(57+0700 -RP1DB-)","",1,36000,36000]
["","","(584+3624-L-LT)","",1,74083.63,74083.63]
["","","(584+3624-L-RT)","",1,74083.63,74083.63]
["","","(60+3713-L-)","",1,36980,36980]
["","","(628+6550-L-LT)","",1,71803.95,71803.95]
["","","(628+6550-L-RT)","",1,71803.95,71803.95]
["","","(642+8142-L-LT)","",1,57519.9,57519.9]
["","","(642+8142-L-RT)","",1,69636.61,69636.61]
["","","(67+1650 -L-)","",1,47200,47200]
["","","(71+5383-L-)","",1,35000,35000]
["","","(765+2744 -L- LT)","",1,44000,44000]
["","","(765+2744 -L- RT)","",1,44000,44000]
["","","(80+7441-L-)","",1,42000,42000]
["","","(826+1500 -L- LT)","",1,42000,42000]
["","","(826+1500 -L- RT)","",1,42000,42000]
["","","(85+2652-L-)","",1,26302.45,26302.45]
["","","(898+2000 -L- LT)","",1,42000,42000]
["","","(898+2000 -L- RT)","",1,42000,42000]
["","","(94+2458 -L- LT)","",1,39000,39000]
["","","(94+2458 -L- RT)","",1,38000,38000]
["","","(94+4384 -COL1-)","",1,42000,42000]
["","","(943+2158 -L-)","",1,86000,86000]
["","","(969+5152 -L- LT)","",1,42000,42000]
["","","(969+5152 -L- RT)","",1,58000,58000]
["","","(991+2318 -L-)","",1,78000,78000]
["8217000000-E","REINF STL (BRG)","","",7593292,0.90705867500000004,6887561.3799999999]
["8224000000-E","EPXY COAT REINF STL BRG","","",1981390,1.044895811,2070346.11]
["8226000000-E","EPOXY CTD SPIR REINF STL BRG","","",3915,1.98,7751.7]
["8238000000-E","SPIRAL COL REINF STL BRG","","",712232,1.6361249280000001,1165300.53]
["8245000000-E","REINF STL (CLVT)","","",2594692,0.953908325,2475098.2999999998]
["8259000000-E","36\" PRESTR CONC GIRDR","","",2361.5,148.68857082400001,351128.06]
["8262000000-E","45\" PRESTR CONC GIRDR","","",7744.72,166.10134259200001,1286408.3899999999]
["8265000000-E","54\" PRESTR CONC GIRDR","","",48683.87,195.347966996,9510295.0299999993]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",30081.040000000001,241.078332066,7251886.9500000002]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",21370.37,262.13427984600003,5601906.5499999998]
["8280000000-E","STRL STL","","",36504349,1.468593007,53610031.68]
["8294000000-N","PAINTING STR STL","","",1,93000,93000]
["8296000000-N","POLLUTION CNTRL","","",1,10000,10000]
["8333000000-E","16\" PRESTR CONC PILES","","",4928,58.91700487,290343]
["8336000000-E","20\" PRESTR CONC PILES","","",13490,72.899184581,983410]
["8350000000-E","24\" PRESTR CONC PILES","","",2260,112,253120]
["8353000000-E","30\" PRESTR CONC PILES","","",41700,125,5212500]
["8364000000-E","HP12X53 PILES","","",131121.5,51.177890200999997,6710521.7300000004]
["8365000000-E","HP12X53 GALV PILES","","",2095,53.914081146000001,112950]
["8384000000-E","HP14X73 PILES","","",59000,49.555880508000001,2923796.95]
["8384200000-E","HP14X73 GALV PILES","","",21830,57.403504351999999,1253118.5]
["8385200000-E","PP**X**** GALV STL PILE","(24 X 0625)","",20790,140,2910600]
["","","(24\" X 050\")","",1840,145,266800]
["","","(PP 24 x 050)","",775,125,96875]
["8387000000-E","PP18X050 GALV STL PILE","","",1200,122.5,147000]
["8391000000-N","STL PILE POINTS","","",835,146.09159281399999,121986.48]
["8392000000-N","PIPE PILE PLATES","","",24,162,3888]
["8392500000-E","PREDRILLING FOR PILES","","",951,90.669316508999998,86226.52]
["8393000000-N","PILE REDRIVES","","",1372,316.520495627,434266.12]
["8440000000-E","METHOD A H2OPROOFING","","",202,67.5,13635]
["8453000000-E","METHD B DAMPPROOFING","","",217.8,35,7623]
["8475000000-E","TWO BAR METAL RAIL","","",14760.33,100.70533856599999,1486444.03]
["8482000000-E","THREE BAR METAL RAIL","","",2985.49,173.48073850500001,517925.01]
["8503000000-E","CONC BARR RAIL","","",64160.15,62.930793958999999,4037649.18]
["8505000000-E","VERT CONC BARR RAIL","","",5044.3500000000004,88.010439402000003,443955.46]
["8510000000-E","CONC MEDIAN BARR","","",4290.3999999999996,53.932286034000001,231391.08]
["8517000000-E","1'-**\"X***\"CONC PARAPET","(1'-0\" X 2'-0\")","",558,319,178002]
["","","(1'-2 3/4\" X 2'-6\")","",605.01,98.580006941999997,59641.89]
["","","(1'-2\" X 2'-10 1/2\")","",741,72.864372470000006,53992.5]
["","","(1'-2\" X 2'-10\")","",250.52,68.599992017000005,17185.669999999998]
["","","(1'-2\" X 2'-11 1/2\" )","",120,115,13800]
["","","(1'-2\" X 2'-11 1/4\")","",400.51,96.747771591000003,38748.449999999997]
["","","(1'-2\" X 2'-6\")","",3137.14,68.234946480000005,214062.58]
["","","(1'-2\" X 2'-9\")","",150.25,90.32,13570.58]
["","","(1'-2\" X 3'-0\")","",160,91.27,14603.2]
["","","(1'-2\" X 3'-6\")","",180,100.61,18109.8]
["","","(1'-2\" X 3'-8 7/8\")","",130.25,145,18886.25]
["","","(1'-2\" x 2'-6\")","",7735.15,41.817055906999997,323461.2]
["","","(1'-2\" x 3'-7 1/2\")","",609.6,115,70104]
["","","(1'-3 1/2\" X 3'-3 1/2\")","",327.69,90,29492.1]
["","","(16+2900-L-)","",280.26,100,28026]
["","","(2\" X 2'-11 3/4\")","",357.73,257,91936.61]
["8524000000-E","**\" CHN LK FEN","(72\")","",3566.75,106.546435831,380024.5]
["8531000000-E","4\" SLOPE PROTECTION","","",54334.3,57.822026970000003,3141719.36]
["8559000000-E","SURFACE PREP CL II","","",163.4,237.05630355,38735]
["8573000000-E","LATX MOD CONC OVRLY","","",649,711.47149460699995,461745]
["8580000000-E","PLACING LATEX MOD CONC","","",12682,38.155653682000001,483890]
["8590000000-E","RIP RAP CL **","(I)","",505,45.841584158000003,23150]
["","","(I 2'-0\" TK)","",300,20,6000]
["8594000000-E","RIP RAP B","","",1103,41.002937443,45226.239999999998]
["8608000000-E","RIP RAP II (2'-0\")","","",61382,50.357613469999997,3091051.03]
["8622000000-E","GEOTEXTILE FOR DRNG","","",69901,2.455444843,171638.05]
["8650000000-N","POT BEARGS","","",4,230204.1225,920816.49]
["8654000000-N","DISC BEARGS","","",4,128275.3925,513101.57]
["8657000000-N","ELASTOMERIC BEARGS","","",58,55296.573103447998,3207201.24]
["8660000000-E","CONC REPS","","",469.5,28.977614483,13604.99]
["8664000000-E","SHOTCRETE REPS","","",2683.73,738.477626289,1981874.56]
["8678000000-E","EPOXY RESIN INJECTION","","",612.79999999999995,80.786259791000006,49505.82]
["8692000000-N","FOAM JOINT SEALS","","",18,32976.287777778001,593573.18000000005]
["8706000000-N","EXPANSION JOINT SEALS","","",12,393970.14750000002,4727641.7699999996]
["8713000000-N","MODULAR EXP JNT SEAL","","",3,105000,315000]
["8727000000-N","ELEC CONDUIT SYS SGL ******","(129+3756-L-RT)","",1,26000,26000]
["","","(14+9925-L-)","",1,47000,47000]
["","","(144+6063-L-)","",1,150000,150000]
["","","(147+3889-L-RT)","",1,67000,67000]
["","","(174+7246-L-RT)","",1,18000,18000]
["","","(26+2165-L-LT)","",1,20000,20000]
["","","(268+2289-L-)","",1,34000,34000]
["","","(28+1707-L-)","",1,37500,37500]
["","","(38+5027-Y7-)","",1,17200,17200]
["8734000000-N","ELEC CONDUIT SYS ******","(16+0550-Y2-)","",1,50000,50000]
["8741000000-N","STR DRN SYS ************","(122+2250-L-LT)","",1,56773.42,56773.42]
["","","(122+2250-L-RT)","",1,56773.42,56773.42]
["","","(18+8173-RR-)","",1,200000,200000]
["","","(28+5089-RRDET-)","",1,64210.42,64210.42]
["","","(46+2150-L-)","",1,1000000,1000000]
["","","(64+5550-L-)","",1,64210.42,64210.42]
["","","(64+749-L-)","",1,64210.42,64210.42]
["8744000000-N","SOLAR ARRAY SUPPT PLTFORM","","",1,45000,45000]
["8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",3920,194.89272959199999,763979.5]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",9529.35,223.384359899,2128707.75]
["8755000000-E","3'-0\"X 1'-6\"PRESTR SLAB","","",2193.88,131.04490674100001,287496.8]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLAB","","",25010,129.73449420200001,3244659.7]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLAB","","",13001.88,146.66409780699999,1906909]
["8801000000-E","MSE RETAIN WALL NO **","(1 @ EB1)","",5430,45.01,244404.3]
["","","(1 @ END BENT 1)","",6950,80,556000]
["","","(1 @ END BENT 1","STA 14+6276-L1-)",1736,76.69,133133.84]
["","","","STA15+6728-L-)",1953,85.6,167176.79999999999]
["","","(1)","",28304,60.147280950000003,1702408.64]
["","","(1-A)","",5730,51.64,295897.2]
["","","(11)","",1710,51.74,88475.4]
["","","(12)","",2300,51.98,119554]
["","","(13)","",6700,54.51,365217]
["","","(14)","",7650,54.65,418072.5]
["","","(15)","",2800,51.73,144844]
["","","(16)","",7050,56.55,398677.5]
["","","(17)","",14700,51.55,757785]
["","","(2 @ EB2)","",3472,45.01,156274.72]
["","","(2 @ END BENT 2)","",4925,80,394000]
["","","(2 @ END BENT 2","STA 14+6276-L1-)",1912,77.400000000000006,147988.79999999999]
["","","","STA 15+6728-L-)",2216,81.66,180958.56]
["","","(2)","",36014,62.095429555000003,2236304.7999999998]
["","","(3)","",10290,61.932400389000001,637284.4]
["","","(4)","",18180,55.818624862,1014782.6]
["","","(5)","",11110,51.507785779000002,572251.5]
["","","(6)","",9055,60.700889011999998,549646.55000000005]
["","","(7)","",17700,50.859491525000003,900213]
["8802010000-E","SOIL NAIL RET WALLS","","",21881,67.606096613999995,1479289]
["8802014000-E","SOLDIER PILE RET WALLS","","",23659,97.835200134999994,2314683]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",9,972.81777777800005,8755.36]
["8802015110-N","SOIL NAIL PROOF TESTS","","",46,531.25391304300001,24437.68]
["8802030000-E","SEGMTAL GRAV RETAIN WALLS","","",135,75,10125]
["8802031000-E","PRECAST GRAV RET WALLS","","",1359,75.5,102604.5]
["8802040000-E","CIP GRAV RET WALLS","","",1178,110.118845501,129720]
["8804000000-N","GENERIC CLVT ITEM (LS)","PLACEMT OF NATURAL STREAM","BED MATERIAL",2,76850,153700]
["","","PRECAST REINF CONC THREE-SIDED","CLVT @ STA 14+3400 -L-",1,215000,215000]
["","","PRECAST REINF CONC","THREE-SIDE CLVT",1,370000,370000]
["8825000000-E","GENERIC CLVT ITEM (CY)","SEL MATERIAL CL VI","- 57 ST BACKFILL",300,70,21000]
["8839000000-E","GENERIC RET WALL ITEM (LF)","CONC BARR RAIL W/ MOMT SLAB","",500,275.51,137755]
["8847000000-E","GENERIC RET WALL ITEM (SF)","ANCHED RET WALLS","",800,150,120000]
["","","ANCHED SOLDIER PILE WALLS","",7900,89.42,706418]
["","","ARCH CONC SURFACE TRTMT","",675,25,16875]
["","","MSE RET WALL NO 1","",3850,95,365750]
["","","SOUND BARR WALL","",508924,24.150497912999999,12290768]
["","","VISUAL BARR WALL","",79031.27,25.55762738,2019851.75]
["8860000000-N","GENERIC STR ITEM (LS)","APPLICATION OF BRG COATING","",2,25714.29,51428.58]
["","","APPROX 980100 LBS STRL STL","",1,1700000,1700000]
["","","CONDUIT IN PARAPET @","STA18+8173-RR-",1,2000,2000]
["","","DISC BEARGS","",1,40000,40000]
["","","ELECTRICAL CONDUIT SYSTEM","AT STA 12+9050",1,19000,19000]
["","","ELECTRICAL CONDUIT SYSTEM AT","ROWENA AVE",1,3190,3190]
["","","EXPANSION JOINT SEALS","",1,88000,88000]
["","","FOAM JOINT SEALS","",1,47000,47000]
["","","MOD BRG APPROACH FILL","STA 268+2289-L-",1,30000,30000]
["","","PAINTING EXT STR","",1,5000,5000]
["","","PAINTING STRL STL","",1,5000,5000]
["","","PARTIAL REML OF EXT","STR AT BRG 193",1,70000,70000]
["","","POST TENSIONING TENDONS","",2,402500,805000]
["","","REHAB OF EXT STR","",1,30000,30000]
["","","REML OF EXT BARGE AT","STA 45+2400-L-",1,30000,30000]
["","","REML OF EXT STR 42","",1,5000,5000]
["","","ROCKER BEARG ASSEMBLIES","",1,98471.38,98471.38]
["","","SELF-LUBRICATING EXPANSION","BEARG ASSEMBLIES",2,147607.74,295215.48]
["","","SOUND BARR WALL","(BRG MOUNTED)",1,29161,29161]
["","","SOUND BAR WALL(BRG","MOUNTED)",1,125147.16,125147.16]
["","","STATC AXL COMPRESS LOAD TEST ON","30\"SQ PRESTRESS CONC PILE",1,150000,150000]
["","","STL BEARG ASSEMBLIES","",1,174922,174922]
["","","STRL STL","APPROX 1042750 LBS",1,2331834.92,2331834.92]
["","","","APPROX 465500 LBS",1,1036130.78,1036130.78]
["","","","APPROX 714223 LBS",1,1542939.28,1542939.28]
["","","","APPROX 959500 LBS",1,2173356.39,2173356.39]
["","","TEMP SOLDIER PILE RET WALL FOR RR ABUT","(ABUT 1 25+6900-RRDET-)",1,81128.539999999994,81128.539999999994]
["","","","(ABUT 2 25+6900-RRDET-)",1,71235.67,71235.67]
["","","TEMP RAILRD SHORING","(138+4045-LDFEB)",1,39220.339999999997,39220.339999999997]
["","","","(17+9757-DFLW-)",1,42118.85,42118.85]
["","","","(24+7018-DFWB- WID)",1,96180.22,96180.22]
["","","","",1,350000,350000]
["","","TIMBER FENDER BOARDS","AT CHANNEL BENTS",1,20000,20000]
["","","TREATED LUMBER DECK","",1,137439.39000000001,137439.39000000001]
["","","UNDER STR WORK PLATFORM","",1,12842.08,12842.08]
["","","UTILITY HANGER SYST","",1,174000,174000]
["","","VOLUMETRIC MIXER","",2,32105.71,64211.42]
["8867000000-E","GENERIC STR ITEM (LF)","20\" COMPOSITE PILE","",1000,134,134000]
["","","3'-0\" DIA LFD DRILLED PIERS","IN SOIL",239.6,582.28998330599995,139516.68]
["","","","NOT IN SOIL",384,582.29,223599.35999999999]
["","","3'-6\" DIA LFD DRILLED PIERS","IN SOIL",333.2,626.58001200499996,208776.46]
["","","","NOT IN SOIL",140,626.58000000000004,87721.2]
["","","4'-6\" DIA LFD DRILLED PIERS","IN SOIL",103.8,966.61001926799997,100334.12]
["","","","NOT IN SOIL",208,966.61,201054.88]
["","","74\" MOD PRESTR CONC GDRS","",3783.26,290.34999973599997,1098469.54]
["","","78\" POST TENSIONED","PRESTRESSED CONC GIRDERS",6489,575,3731175]
["","","78\" PRESTRESSED CONC","GIRDERS",11639.9,275,3200972.5]
["","","CLASSC CONC BRG RAIL","",1262,200,252400]
["","","CONC BARR RAIL W/","MOMT SLAB",2175,309.19,672488.25]
["","","CONC BARR RAIL W/ MOMT SLAB","",4340,287.31,1246925.3999999999]
["","","CONC PARAPET","",1640.2,35.65,58473.13]
["","","METAL HANDRAIL","W/ FENCING",635,350,222250]
["","","METAL HANDRAIL(ALUMINUM)","",911,120,109320]
["","","SPEC CONC BARR RAIL","",200.5,420,84210]
["","","TEMP STL CASING AS SHORING","(PIER 1 25+6900-RRDET-)",12,644.41999999999996,7733.04]
["","","","(PIER 2 25+6900-RRDET-)",12,644.41999999999996,7733.04]
["","","","(PIER 6 25+6900-RRDET-)",12,644.41999999999996,7733.04]
["","","","(PIER 7 25+6900-RRDET-)",12,644.41999999999996,7733.04]
["","","T101 RAIL","",84.67,325,27517.75]
["8874000000-E","GENERIC STR ITEM (TON)","FOUND CONDITIONING","MATERIAL FOR CONC SLABS",62,54.5,3379]
["8881000000-E","GENERIC STR ITEM (CY)","6000 PSI CONC","",218.7,1250,273375]
["","","CL A CONC (BRG)","",6.8,2750,18700]
["","","CL AA CONC (AS MOD","BY RAILWAY)",943.5,849.93000529899996,801908.96]
["","","CL AA CONC (WEIGH","BRG - STATIC SCALE)",509,795,404655]
["","","CONC SLABS","",17,599.5,10191.5]
["","","LATEX MOD CONC OVERLAY","- VERY EARLY STRENGTH",166.7,800,133360]
["","","LATEX MOD CONC","",111,276.10000000000002,30647.1]
["","","LATEX MOD CONC-VERY","EARLY STRNGTH",252,276.10000000000002,69577.2]
["","","POST TENSIONING ENCASEMT","",17.399999999999999,1600,27840]
["8882000000-E","GENERIC STR ITEM (CF)","CONC FOR DECK REP","",501,38.666307385000003,19371.82]
["8889000000-E","GENERIC STR ITEM (LB)","EPOXY COATED REINFORCING STL","(WEIGH BRG - STATIC SCALE)",35037,0.85,29781.45]
["","","EPOXY COATED REINFORCING STL(BRG)","",608,3,1824]
["","","POLYURETHANE GROUT INJECTION","",12500,14.15,176875]
["","","REINFORCING STL (WEIGH","BRG - STATIC SCALE)",37175,1.1499999999999999,42751.25]
["","","STRL STL FOR GIRDER","REP",42000,0.31,13020]
["8892000000-E","GENERIC STR ITEM (SF)","18\" STL SHEET PILES","",2150,32,68800]
["","","ARCH CONC SURFACE TRTMT","",289,30,8670]
["","","BRG JOINT DEMOLITION","",2623.3,10.712613883,28102.400000000001]
["","","CONC SIMULATED STONE","FORM LINER",3592.2,5,17961]
["","","CONC STAINING","",21230.1,5.3718315030000001,114044.52]
["","","DAMPROOFING (RR STR)","",4716,0.87,4102.92]
["","","EPOXY COATING","",3188,3,9564]
["","","EPOXY PROTECTIVE COATING","",4239,1,4239]
["","","GALVANIZED 18\" STL SHEET PILES","",1693,40,67720]
["","","GROOVING CONC SLABS","",6422,2.5499999999999998,16376.1]
["","","JOINT REP","",470,8.69,4084.3]
["","","PAINTING OF STRL STL","",2879,5.82,16755.78]
["","","TEMP SHORING","",430,42,18060]
["","","H2OPROOFING (RR STR)","",15159,7.5,113692.5]
["8893000000-E","GENERIC STR ITEM (SY)","EPOXY COATING","",21200,52,1102400]
["","","GEOTEXTILE FABRIC-4","",640,2.25,1440]
["","","HYDRO-DEMOLITION","OF BRG DECK",5756,28.3,162894.79999999999]
["","","HYDRO-DEMOLITION OF BRG DECK","",16684,31.763366098999999,529940]
["","","HYDRODEMOLITION OF BRG DECK","",186,315,58590]
["","","MEMBRANE LAYER H2O-","PROOFING FOR DECK",682,120,81840]
["","","ONE-INCH ASPH PLANKING","PROTECTIVE CRS FOR DECK",682,60,40920]
["","","PLACING & FINISHING LATEX","MOD CONC",2263,7.44,16836.72]
["","","PLACING & FINISHING LMC","- VERY EARLY STRENGTH",4888,7.15,34949.199999999997]
["","","PLACING & FINISHING OF LATEX MOD CONC OVR-","LAY - VERY EARLY STRENGTH",4002,45,180090]
["","","SCARIFYING BRG DECK","",22626,10.219550958999999,231227.56]
["","","SHOTCRETE SLOPE PROTECTION","",3850,15.91,61253.5]
["","","TWO-PART MEMBRANE H2O-","PROOFING SYSTEM",35.200000000000003,140,4928]
["8897000000-N","GENERIC STR ITEM (EA)","ANCH BOLT REPLMT","",4,744.02,2976.08]
["","","BEARG REPLMT","",9,632.35,5691.15]
["","","CONC MEDALLION PANEL","",8,1500,12000]
["","","DRNG PIPE CLEANOUT","",3,20000,60000]
["","","GIRDER JACKING","",26,2602.89,67675.14]

{"sheet":"BExRepositorySheet","index":2,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
[7]

{"sheet":"Items - Div 1","index":3,"n_rows":250,"n_cols":7,"rows_kept":250,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 1"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",3,222333.33333333299,667000]
["0000400000-N","CONST SURVEYING","","",2,63650,127300]
["0001000000-E","CLEARING & GRUBBING","","",22,33482.142857143001,750000]
["0005000000-N","GENERIC FERRY ITEM (LS)","CO2 FLOODING SYST","",1,19762,19762]
["","","CRANE SERV & LAUNCH","",1,118578,118578]
["","","DELIVERY","",1,158104,158104]
["","","DOORS WINDOWS","",1,39526,39526]
["","","DREDGE BOOM & CUTTR ","HEAD",1,375497,375497]
["","","DREDGE MANEUVERING ","SYST",1,98815,98815]
["","","DREDGE PUMP PIPING","",1,98815,98815]
["","","DREDGE PUMP SKID","",1,750993,750993]
["","","DREDGE RECORDG SYST","",1,39526,39526]
["","","ELECTRICAL","",1,513837,513837]
["","","ELECTRONICS","",1,189725,189725]
["","","ENGINEERING & NC PROGRAMMING","",1,988149,988149]
["","","FENDERS","",1,71147,71147]
["","","FIRE SAFETY EQUIP","",1,140712,140712]
["","","GENERATORS","",1,260871,260871]
["","","HULL STEEL","",1,913049,913049]
["","","HVAC INCLUD WHLHSE","",1,79052,79052]
["","","HYDRAULIC POWER UNIT","",1,296445,296445]
["","","JOINER","",1,276682,276682]
["","","MACHINERY ALARM SYS","",1,98815,98815]
["","","MACHINERY ALL EXCEPT","LISTED SEPARATE",1,750993,750993]
["","","MOBILIZATION","",1,256919,256919]
["","","NAMES & TAGS","",1,2372,2372]
["","","OUTFIT (DECK FIT ONLY)","",1,79052,79052]
["","","PAINTING","",1,256128,256128]
["","","PIPING","",1,158104,158104]
["","","POST-DELIVERY TRAIN & ","TRIAL RUN",1,79052,79052]
["","","PRE-DELIVERY TESTG & ","TRIALS",1,79051,79051]
["","","SPUDS & SPUD WELLS","",1,138340,138340]
["","","STABILITY / INCLINING","",1,39526,39526]
["","","STAIRS LADDERS & ","HANDRAILS",1,23715,23715]
["","","SUPERSTR & WHLHOUSE","",1,513837,513837]
["0008000000-E","SUPP CLEAR & GRUBBING","","",2,100,200]
["0022000000-E","UNCLAS EXCAV","","",3100,2,6200]
["0029000000-N","REINF BRG APPR **********","(15+67-L-)","",1,50000,50000]
["0036000000-E","UNDERCUT EXCAV","","",7100,8.3000000000000007,58930]
["0050000000-E","SUPP CLEAR & GRUBBING","","",1,3560,3560]
["0057000000-E","UNDERCUT EXCAV","","",700,12.75,8925]
["0063000000-N","GRADING","","",1,133300,133300]
["0106000000-E","BORROW EXCAV","","",286200,3.4700209640000002,993120]
["0134000000-E","DRNG DITCH EXCAV","","",17611,4.216455624,74256]
["0156000000-E","REML OF EXT ASPH PVT","","",10140,5.45,55263]
["0177000000-E","BRKING OF EXT ASPH PVT","","",7180,4.9000000000000004,35182]
["0192000000-N","PROOF ROLLING","","",15,210,3150]
["0195000000-E","SEL GRANULAR MAT'L","","",15150,5.9376237620000003,89955]
["0196000000-E","GEOTEXTILE SOIL STABILI","","",16600,1.6759036140000001,27820]
["0199000000-E","TEMP SHORING","","",202.5,65,13162.5]
["0223000000-E","ROCK PLATING","","",140,74,10360]
["0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",3650,11,40150]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",687,27.554585153000001,18930]
["0320000000-E","FND CONDIT GEOTEXTILE","","",2020,1.653465347,3340]
["0335200000-E","15\" DRNG PIPE","","",216,52,11232]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",4,550,2200]
["0343000000-E","15\" SIDE DRN PIPE","","",632,25.981012658000001,16420]
["0344000000-E","18\" SIDE DRN PIPE","","",164,33.75,5535]
["0372000000-E","18\" RC PIPE CULV III","","",296,27.7,8199.2000000000007]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",596,103.2,61507.199999999997]
["","","(54\")","",228,145.6,33196.800000000003]
["0448200000-E","15\" RCP CULV CL IV","","",288,35.75,10296]
["0448400000-E","24\" RCP CULV CL IV","","",472,36.75,17346]
["0448500000-E","30\" RCP CULV CL IV","","",376,51.1,19213.599999999999]
["0448600000-E","36\" RCP CULV CL IV","","",1224,67.599999999999994,82742.399999999994]
["0448700000-E","42\" RCP CULV CL IV","","",292,81.349999999999994,23754.2]
["0995000000-E","PIPE REMOVAL","","",569,12.303427064999999,7000.65]
["1011000000-N","FINE GRADING","","",1,985000,985000]
["1099500000-E","SHALLOW UNDERCUT","","",1100,6.0909090910000003,6700]
["1099700000-E","CL IV SUBGRD STABILIZ","","",2100,21.238095238,44600]
["1111000000-E","CL IV AGG STABILIZATN","","",8000,20,160000]
["1121000000-E","AGG BASE COURSE","","",28885,28.79262593,831675]
["1220000000-E","INCIDENTAL STONE BASE","","",958,19.528183716000001,18708]
["1275000000-E","PRIME COAT","","",1903,3.8640567520000002,7353.3]
["1297000000-E","MILL ASP PVT *****\" DTH","(2\")","",275700,0.46,126822]
["1330000000-E","INCIDENTAL MILLING","","",480,28.541666667000001,13700]
["1489000000-E","ASP CNC BAS CRS B250B","","",4240,43.397641509000003,184006]
["1498000000-E","ASP CNC INTR CRS I190B","","",8730,38.381901489000001,335074]
["1519000000-E","ASP CNC SURF CRS S95B","","",47101,29.543194411999998,1391514]
["1575000000-E","ASP FOR PLANT MIX","","",3433,613.13078939699994,2104878]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",10,240,2400]
["2020000000-N","CNTRL OF ACCESS MRKR","","",14,135,1890]
["2022000000-E","SUBDRN EXCAV","","",193,3.9067357509999998,754]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",600,1,600]
["2036000000-E","SUBDRN COARSE AGG","","",104,71.346153846000007,7420]
["2044000000-E","6\" PERF SUBDRN PIPE","","",600,12.5,7500]
["2070000000-N","SUBDRN PIPE OUTLET","","",2,232.5,465]
["2077000000-E","6\" OUTLET PIPE","","",12,27.5,330]
["2209000000-E","ENDWALLS","","",46.9,900,42210]
["2220000000-E","REINF ENDWALLS","","",10,1200,12000]
["2253000000-E","PIPE COLLARS","","",2.0249999999999999,1500,3037.5]
["2275000000-E","FLOWABLE FILL","","",2,200,400]
["2286000000-N","MASNRY DRNG STRUCT","","",12,1341.6666666670001,16100]
["2364000000-N","FRM W/2GRTS 84016 STD","","",1,450,450]
["2367000000-N","FRM W/2GRTS 84029 STD","","",11,588.18181818200003,6470]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",1,850,850]
["2556000000-E","SHOULDER BERM GUTTER","","",1375,16.298181818,22410]
["2600000000-N","RETROFIT EXT CURB RMP","","",2,1500,3000]
["2612000000-E","6\" CONC DRIVEWAY","","",140,55.2,7728]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",220,48,10560]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",370,60,22200]
["2830000000-N","ADJ MANHOLES","","",27,400,10800]
["2845000000-N","ADJ METER OR VAL BOX","","",19,350,6650]
["3030000000-E","STL BM GRDRL","","",2937.5,14.181065532,41656.879999999997]
["3105000000-N","SBGR TERM SECT","","",2,50,100]
["3150000000-N","ADDIT GRDRL POSTS","","",15,7.6666666670000003,115]
["3270000000-N","GR ANCHOR TYPE 350","","",12,1991.6666666670001,23900]
["3317000000-N","GR ANCHOR TYPE B-77","","",4,1475,5900]
["3360000000-E","REM EXT GRDRL","","",930,1,930]
["3380000000-E","TEMP STL BM GRDRL","","",512.5,7.5,3843.75]
["3387000000-N","TEMP GDRL ANCH UNIT***","(III)","",4,750,3000]
["3389100000-N","TEMP GDRL ANCH UNT350","","",6,850,5100]
["3503000000-E","WOVEN WIRE FEN 47\"FAB","","",34600,1.99,68854]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",2240,14,31360]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",440,18,7920]
["3557000000-E","ADDITIONL BARBED WIRE","","",3460,0.1,346]
["3565000000-E","DBL GATE **HIGH **WIDE **OPEN","(47\" 8' 16')","",2,600,1200]
["3578000000-N","GENERIC FENC ITEM (EA)","RESET EXT GATE","",1,300,300]
["3628000000-E","RIP RAP CL I","","",241,57,13737]
["3649000000-E","RIP RAP CL B","","",259,56.567567568000001,14651]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",4648,2.2312822720000001,10371]
["4048000000-E","REINF CONC FOUNDTN","","",17,700,11900]
["4060000000-E","SUPP BRKAWAY STL BM","","",10164,2.75,27951]
["4066000000-E","SUPPT SIMPLE STL BM","","",1405,2.2000000000000002,3091]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",125,5.3247999999999998,665.6]
["4082000000-E","SUPPORT WOOD","","",1282,12.800156006,16409.8]
["4096000000-N","SIGN ERECTION TYPE D","","",11,110,1210]
["4102000000-N","SIGN ERECTION TYPE E","","",89,84.775280898999995,7545]
["4108000000-N","SIGN ERECTION TYPE F","","",20,89.75,1795]
["4110000000-N","SIGN ERECTION TYPE *** (GRD MTD)","(A)","",6,275,1650]
["","","(B)","",6,275,1650]
["4116000000-N","SIGN ERECTION OVERLAY (GRD MTD)","","",2,535,1070]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(D)","",3,120,360]
["4141000000-N","DISPOSE SUPPORT WOOD","","",4,3,12]
["4152000000-N","DISP SIGN SYST STL BM","","",4,700,2800]
["4155000000-N","DISP SIGN SYST U-CHAN","","",1,1,1]
["4158000000-N","DISP SIGN SYST WOOD","","",45,1,45]
["4400000000-E","WORK ZONE SIGN (STAT)","","",800,6.5,5200]
["4405000000-E","WORK ZONE SIGN (PORT)","","",432,25.611111111,11064]
["4410000000-E","WORK ZONE SIGN(BARR)","","",277,6.4422382669999996,1784.5]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",1624,4.2,6820.8]
["4415000000-N","FLASH ARROW BOARD","","",2,1400,2800]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",30,80,2400]
["4430000000-N","DRUMS","","",166,57.385542168999997,9526]
["4435000000-N","CONES","","",146,22.671232877000001,3310]
["4445000000-E","BARRICADES (TYPE III)","","",344,29.116279070000001,10016]
["4450000000-N","FLAGGER","","",1712,18.093457944000001,30976]
["4455000000-N","FLAGGER","","",40,200,8000]
["4457000000-N","TEMP TRAFFIC CONTROL","","",1,36000,36000]
["4480000000-N","TMA","","",2,6900,13800]
["4510000000-N","LAW ENFORCEMENT","","",80,30,2400]
["4650000000-N","TEMP RAISED PVT MRKS","","",454,6.3348017619999997,2876]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",193264,0.42954694100000002,83015.960000000006]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",148932,0.534653936,79627.08]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",387,3,1161]
["4705000000-E","THERMO LINES 16\" 120MILS","","",100,5,500]
["4710000000-E","24\"WIDE THERMO 120 MIL","","",602,7.5149501660000002,4524]
["4721000000-E","THERMO PVT MKG CHAR 120","","",8,100,800]
["4725000000-E","THERMO PVT SYM 90MILS","","",20,182.5,3650]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",440,2,880]
["","","(IV)","",632,1.25,790]
["4810000000-E","PAINT PVT MARKINGS 4\"","","",307685,0.146045956,44936.15]
["4820000000-E","PAINT PVT MARKINGS 8\"","","",425,1,425]
["4830000000-E","PAINT PVT MKGS LINE 16\"","","",100,3,300]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",450,3,1350]
["4840000000-N","PAINT PVT MKG CHAR","","",8,35,280]
["4845000000-N","PAINT PVT MKG SYMBOL","","",18,42.5,765]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",800,1,800]
["4900000000-N","PERM RAISED PVT MRKRS","","",392,7.9005102039999997,3097]
["5325600000-E","6\" WATER LINE","","",1440,50.728749999999998,73049.399999999994]
["5540000000-E","6\" VALVE","","",3,1559.526666667,4678.58]
["5649000000-N","RECONNECT H2O METER","","",4,1062.0999999999999,4248.3999999999996]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",1558,3.2197689349999998,5016.3999999999996]
["5871400000-E","6\" TRENCHLESS INSTALL (IN SOIL)","","",432,38,16416]
["5871410000-E","6\" TRENCHLESS INSTALL (NOT IN SOIL)","","",48,1,48]
["6000000000-E","TEMP SILT FENCE","","",90920,1.6621260449999999,151120.5]
["6006000000-E","EROS CNTRL STONE CL A","","",1050,43.714285713999999,45900]
["6009000000-E","EROS CNTRL STONE CL B","","",6915,46.026753435000003,318275]
["6012000000-E","SEDIMENT CNTRL STONE","","",11285,30.53832521,344625]
["6015000000-E","TEMP MULCHING","","",82,409.75609756099999,33600]
["6018000000-E","SEED FOR TEMP SEEDING","","",4900,3.7020408159999998,18140]
["6021000000-E","FERT FOR TEMP SEEDING","","",24.5,953.06122448999997,23350]
["6024000000-E","TEMP SLOPE DRNS","","",5300,8.773584906,46500]
["6029000000-E","SAFETY FENCE","","",15400,1.642207792,25290]
["6030000000-E","SILT EXCAV","","",6430,1.7356143079999999,11160]
["6036000000-E","MAT FOR EROS CONTROL","","",24000,1.608333333,38600]
["6037000000-E","COIR FIBER MAT","","",300,5.5833333329999997,1675]
["6038000000-E","PERM SOIL REINF MAT","","",1550,5,7750]
["6042000000-E","1/4\" HARDWARE CLOTH","","",1080,5.1851851849999999,5600]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",55,10,550]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",125,130,16250]
["6048000000-E","FLOAT TURBIDITY CURTN","","",150,32,4800]
["6069000000-E","STILLING BASINS","","",100,12,1200]
["6070000000-N","SPECIAL STILLING BASINS","","",4,300,1200]
["6071010000-E","WATTLE","","",300,3,900]
["6071012000-E","COIR FIBER WATTLE","","",4950,7.5,37125]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",660,15.878787879000001,10480]
["6071030000-E","COIR FIBER BAFFLE","","",300,4.1500000000000004,1245]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",3,1300,3900]
["6084000000-E","SEEDING & MULCHING","","",82,1430.4878048779999,117300]
["6087000000-E","MOWING","","",41,59.634146340999997,2445]
["6090000000-E","SEED FOR REPAIR SEEDG","","",1050,7,7350]
["6093000000-E","FERT FOR REPAIR SEEDG","","",3.5,1078.5714285710001,3775]
["6096000000-E","SEED FOR SUPP SEEDING","","",2150,3.127325581,6723.75]
["6108000000-E","FERTILIZER TOPDRESSING","","",63.5,633.95669291299998,40256.25]
["6111000000-E","IMPERVIOUS DIKE","","",215,75,16125]
["6114500000-N","SPECIALIZED HAND MOW","","",40,63.75,2550]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",125,220,27500]
["6120000000-E","CLVT DIVERSION CHANNL","","",60,15,900]
["6123000000-E","REFORESTATION","","",5.7,1885.9649122809999,10750]
["7301000000-E","DIRECT DRILL (***********)","(2 125\")","",300,27,8100]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",4,169,676]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",400,6.5,2600]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",500,1,500]
["7980000000-N","GENERIC SIGNAL ITEM(EA)","5/8\" X 10' GROUNDING ","ELECTRODE",8,165,1320]
["","","6\" X 6\" WOOD PEDESTAL","",2,624,1248]
["","","CCTV CAMERA ","ASSEMBLY",2,5914,11828]
["","","DMS","",2,66978,133956]
["","","DMS ACCESS LADDER","",2,4469,8938]
["","","DMS PEDESTAL STR","",2,40272,80544]
["","","EQUIP CBNT DISCONNCT","",2,512,1024]
["","","INDUSTRIAL ETHERNET ","SWITCH",2,1723,3446]
["","","METER BASE/DISCONNT","COMBO PANEL",2,738,1476]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","4 AWG SOLID BARE COPPER","GROUNDING CONDUCTOR",80,2.0299999999999998,162.4]
["","","3-WIRE COPPER FEEDER ","CONDUCTORS",20,8.6999999999999993,174]
["","","4-WIRE COPPER FEEDER ","CONDUCTORS",340,3.65,1241]
["7992000000-E","GENERIC SIGNAL ITEM(CY)","OVERHEAD FOOTINGS","",16,910,14560]
["8007000000-N","CM&R TEMP STR ***********","(15+6700-L-)","",1,181200,181200]
["8035000000-N","REMV EXIST STR **********","(15+6700-L-)","",1,150000,150000]
["8112730000-N","PDA TESTING","","",2,4000,8000]
["8121000000-N","UNCL STR EXCAV STA***","(15+6700-L-)","",1,18000,18000]
["8126000000-N","CULV EXCAV @ *********","(148+7300-L-)","",1,47800,47800]
["8133000000-E","FND CONDIT MAT BOX CULV","","",68,75,5100]
["8147000000-E","REINF CONC DECK SLAB","","",4758,43,204594]
["8161000000-E","GROOVING BRG FLOORS","","",5821,0.64,3725.44]
["8182000000-E","CL A CONC (BRG)","","",72.400000000000006,900,65160]
["8196000000-E","CL A CONC (CULV)","","",110,930,102300]
["8210000000-N","BRG APPR SLAB ***********","(15+6700-L-)","",1,52000,52000]
["8217000000-E","REINF STEEL (BRG)","","",12842,1,12842]
["8245000000-E","REINF STEEL (CLVT)","","",18545,1,18545]
["8262000000-E","45\" PRESTR CONC GIRDR","","",429,155,66495]
["8333000000-E","16\" PRESTR CONC PILES","","",910,46.5,42315]
["8336000000-E","20\" PRESTR CONC PILES","","",390,74,28860]
["8393000000-N","PILE REDRIVES","","",11,50,550]
["8503000000-E","CONC BARRIER RAIL","","",216.67,125,27083.75]
["8608000000-E","RIP RAP II (2'-0\")","","",112,72,8064]
["8622000000-E","GEOTEXTILE FOR DRNG","","",124,3,372]
["8657000000-N","ELASTOMERIC BEARINGS","","",1,2400,2400]

{"sheet":"Items - Div 2","index":4,"n_rows":378,"n_cols":7,"rows_kept":378,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 2"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",3,1417400,4252200]
["0000400000-N","CONST SURVEYING","","",3,318645.83333333302,955937.5]
["0000700000-N","FIELD OFFICE","","",1,275000,275000]
["0015000000-N","SEAL ABANDONED WELLS","","",4,500,2000]
["0029000000-N","REINF BRG APPR **********","(16+0550-Y2-)","",1,40000,40000]
["","","(20+6720 -L-)","",1,12491.76,12491.76]
["","","(46+2150-L-)","",1,40000,40000]
["0036000000-E","UNDERCUT EXCAV","","",19315,15,289725]
["0043000000-N","GRADING","","",2,270905.84000000003,541811.68000000005]
["0050000000-E","SUPP CLEARING & GRUBBING","","",4,3025.25,12101]
["0057000000-E","UNDERCUT EXCAV","","",300,37.869999999999997,11361]
["0063000000-N","GRADING","","",1,2500000,2500000]
["0106000000-E","BORROW EXCAV","","",580000,5,2900000]
["0127000000-N","EMBM'T SETTLEMT GAUGE","","",4,1500,6000]
["0134000000-E","DRNG DITCH EXCAV","","",14776,6.4057931779999997,94652]
["0192000000-N","PROOF ROLLING","","",23,175,4025]
["0195000000-E","SELECT GRANULAR MAT'L","","",33000,3.061242424,101021]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",33300,1.4143243240000001,47097]
["0220000000-E","ROCK EMBANKMENTS","","",2600,57,148200]
["0222000000-E","GEOTEXTILE ROCK EMBNK","","",1200,3.33,3996]
["0241000000-E","GENERIC GRAD ITEM (SY)","GEOTEXTLE FOR EMBKMT","STABIL 1",1750,3.8,6650]
["","","","STABIL 2",850,3.3,2805]
["0255000000-E","GENERIC GRAD ITEM (TON)","CLEAN SAND","",335,38,12730]
["0262000000-N","GENERIC GRAD ITEM (EA)","HAZRDOUS SPILL BASIN/","BIORETENTION BASIN",1,67000,67000]
["","","VW PIEZOMETER","",4,2750,11000]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",2350,33.914382979000003,79698.8]
["0320000000-E","FND CONDIT GEOTEXTILE","","",7316,2.40895298,17623.900000000001]
["0335200000-E","15\" DRNG PIPE","","",778,27.951413882000001,21746.2]
["0342000000-E","**\" SIDE DRN PIPE","(12\")","",152,30.85,4689.2]
["","","(30\")","",24,61.75,1482]
["","","(42\")","",140,69.3,9702]
["0343000000-E","15\" SIDE DRN PIPE","","",1292,28.4,36692.800000000003]
["0344000000-E","18\" SIDE DRN PIPE","","",236,34,8024]
["0345000000-E","24\" SIDE DRN PIPE","","",200,40.25,8050]
["0354000000-E","***\" RC PIPE CULV *****","(12\" V)","",884,28.25,24973]
["","","(15\" V)","",4140,28.613043478000002,118458]
["","","(18\" V)","",60,34.65,2079]
["","","(24\" V)","",442,64.868778281000004,28672]
["","","(30\" V)","",92,64.5,5934]
["","","(42\" V)","",92,97,8924]
["0360000000-E","12\" RC PIPE CULV III","","",156,24.25,3783]
["0366000000-E","15\" RC PIPE CULV III","","",1948,24.760143737,48232.76]
["0372000000-E","18\" RC PIPE CULV III","","",636,24.852830188999999,15806.4]
["0378000000-E","24\" RC PIPE CULV III","","",1916,33.799999999999997,64760.800000000003]
["0384000000-E","30\" RC PIPE CULV III","","",1212,47.25,57267]
["0390000000-E","36\" RC PIPE CULV III","","",436,54.5,23762]
["0396000000-E","42\" RC PIPE CULV III","","",432,66.5,28728]
["0402000000-E","48\" RC PIPE CULV III","","",932,90.5,84346]
["0408000000-E","54\" RC PIPE CULV III","","",552,112.5,62100]
["0414000000-E","60\" RC PIPE CULV III","","",232,186,43152]
["0426000000-E","72\" RC PIPE CULV III","","",420,223.25,93765]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",216,92.75,20034]
["","","(72\")","",192,240,46080]
["0448200000-E","15\" RCP CULV CL IV","","",476,29.8,14184.8]
["0448400000-E","24\" RCP CULV CL IV","","",64,36.5,2336]
["0448600000-E","36\" RCP CULV CL IV","","",300,82,24600]
["0448700000-E","42\" RCP CULV CL IV","","",40,82.5,3300]
["0453000000-E","**\" PIPE END SECTION","(15\")","",1,1045,1045]
["0546000000-E","**\" CAA PIPE CLVT *****\"","(18\" 0064\")","",4,132,528]
["","","(54\" 0109\")","",28,216,6048]
["0995000000-E","PIPE REML","","",1855,7.6586253370000001,14206.75]
["0996000000-N","PIPE CLEAN-OUT","","",1,2390,2390]
["1077000000-E","57 STONE","","",1150,47,54050]
["1111000000-E","CL IV AGG STABIL","","",7000,23.75,166250]
["1121000000-E","AGG BASE COURSE","","",62600,30.146964856,1887200]
["1220000000-E","INCIDENTAL STONE BASE","","",1150,37.931739129999997,43621.5]
["1275000000-E","PRIME COAT","","",1268,6.0587460569999996,7682.49]
["1330000000-E","INCIDENTAL MILLING","","",1300,17.75,23075]
["1489000000-E","ASP CNC BAS CRS B250B","","",7460,56.142091153000003,418820]
["1491000000-E","ASP CNC BAS CRS B250C","","",110,57.35,6308.5]
["1498000000-E","ASP CONC INTR CRS I190B","","",30790,51.463332250999997,1584556]
["1503000000-E","ASP CONC INTR CRS I190C","","",55,57,3135]
["1519000000-E","ASP CNC SURF CRS S95B","","",28330,51.527815037000003,1459783]
["1523000000-E","ASP CNC SURF CRS S95C","","",50,60,3000]
["1525000000-E","ASP CONC SURF CRS SF95A","","",150,102.5,15375]
["1575000000-E","ASP FOR PLANT MIX","","",3530,553.95892351299995,1955475]
["1693000000-E","ASP PLT MIX PVMT REPAIR","","",770,160.51753246800001,123598.5]
["2022000000-E","SUBDRN EXCAV","","",660.8,7.440677966,4916.8]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2900,2.4258620689999999,7035]
["2036000000-E","SUBDRN COARSE AGG","","",487.2,62.784482758999999,30588.6]
["2044000000-E","6\" PERF SUBDRN PIPE","","",2900,9.853448276,28575]
["2070000000-N","SUBDRN PIPE OUTLET","","",8,207.0625,1656.5]
["2077000000-E","6\" OUTLET PIPE","","",48,35,1680]
["2209000000-E","ENDWALLS","","",30,1130,33900]
["2220000000-E","REINF ENDWALLS","","",49.8,1204.4939759040001,59983.8]
["2253000000-E","PIPE COLLARS","","",8.9160000000000004,1209.112830866,10780.45]
["2275000000-E","FLOWABLE FILL","","",4.8499999999999996,222,1076.7]
["2286000000-N","MASNRY DRNG STRUCT","","",157,861.73350318500002,135292.16]
["2297000000-E","MASNRY DRNG STRUCT","","",31.704999999999998,760,24095.8]
["2308000000-E","MASNRY DRNG STRUCT","","",30.96,190,5882.4]
["2364000000-N","FRM W/2GRTS 84016 STD","","",10,490,4900]
["2366000000-N","FRM W/2GRTS 84024 STD","","",3,330,990]
["2367000000-N","FRM W/2GRTS 84029 STD","","",86,360.70023255799998,31020.22]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",8,452.5,3620]
["","","(F)","",19,478.15789473699999,9085]
["","","(G)","",26,492.30769230800001,12800]
["2396000000-N","FRM W/COVER STD 84054","","",5,336.06799999999998,1680.34]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",60,725,43500]
["2473000000-N","GENERIC DRNG ITEM (EA)","RETICULINE FRM AND ","GRATE",2,4650,9300]
["2538000000-E","**'-**\" CONC CURB & GUTR","(2'-9\")","",24700,10,247000]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",12800,14.40078125,184330]
["2556000000-E","SHOULDER BERM GUTTER","","",2232,17.180107527000001,38346]
["2591000000-E","4\" CONC SIDEWALK","","",4250,26.552941176000001,112850]
["2605000000-N","CONC CURB RAMP","","",18,730.36111111100001,13146.5]
["2612000000-E","6\" CONC DRIVEWAY","","",560,37.558928571000003,21033]
["2647000000-E","5\" MONO CONC ISLDS (SURF MTD)","","",1970,44.733502538000003,88125]
["2724000000-E","PC REINF BARR SNGL FC","","",2500,55,137500]
["3000000000-N","IMPACT ATTEN 350","","",2,15500,31000]
["3030000000-E","STL BM GRDRL","","",3750,14.573333333000001,54650]
["3105000000-N","SBGR TERM SECT","","",6,93,558]
["3150000000-N","ADDIT GRDRL POSTS","","",15,19.333333332999999,290]
["3210000000-N","GR ANCHOR CAT-1","","",5,500,2500]
["3215000000-N","GR ANCHOR III","","",10,980,9800]
["3270000000-N","GR ANCHOR 350","","",11,1881.8181818180001,20700]
["3317000000-N","GR ANCHOR B-77","","",2,1350,2700]
["3435000000-N","GENERIC GRDRL ITEM (EA)","EXTRA LGTH GRDRL ","POSTS (8' STL)",102,75,7650]
["3503000000-E","WOVEN WIRE FEN 47\" FAB","","",29810,3,89430]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1911,14.351125065,27425]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",420,29.285714286000001,12300]
["3539000000-E","MET LINE PST **\" CL FEN","(72\")","",60,47,2820]
["3545000000-E","MET TERM PST **\" CL FEN","(72\")","",3,118,354]
["3564000000-E","SGL GATE **HIGH **WIDE **OPEN","(47\" HIGH 16' WIDE 16' OPEN-ING)","",1,900,900]
["","","(47\" HIGH 8'WIDE 8'OPEN- ","ING)",1,900,900]
["3575000000-E","GENERIC FENCING ITEM(LF)","72\" CHAIN LINK FENCE ","WITH SLATS",718,15.5,11129]
["3628000000-E","RIP RAP CL I","","",165,57,9405]
["3649000000-E","RIP RAP CL B","","",761,57.155716163000001,43495.5]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",9931,2.141868895,21270.9]
["3659000000-N","PREFORMED SCOUR HOLE","","",6,2145,12870]
["4048000000-E","REINF CONC FOUNDTN","","",11,622.27272727299999,6845]
["4054000000-E","PLN CONC FOUNDTN","","",2,450,900]
["4060000000-E","SUPPT BRKAWAY STL BM","","",9440,3.6506779659999999,34462.400000000001]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",482,5,2410]
["4080000000-N","SUPPORT BARR LARGE","","",9,900,8100]
["4082000000-E","SUPPORT WOOD","","",3262,4.5171673820000002,14735]
["4096000000-N","SIGN ERECTION D","","",21,93,1953]
["4102000000-N","SIGN ERECTION E","","",136,72.176470588000001,9816]
["4108000000-N","SIGN ERECTION F","","",60,82,4920]
["4109000000-N","SIGN ERECTION *** (OVRHD)","(B)","",2,825,1650]
["4110000000-N","SIGN ERECTION *** (GRD MTD)","(A)","",9,650.55555555599994,5855]
["","","(B)","",10,460,4600]
["4157000000-N","STKPILE SIGN SYST WOOD","","",2,30,60]
["4158000000-N","DISP SIGN SYST WOOD","","",91,5,455]
["4234000000-N","DISP SIGNA OR B(OVRHD)","","",2,150,300]
["4238000000-N","DISP SIGN D E F","","",3,150,450]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",2238,15.360366399,34376.5]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",634,14.140694006,8965.2000000000007]
["4410000000-E","WORK ZONE SIGN (BARR)","","",562,22.527491102999999,12660.45]
["4415000000-N","FLASHING ARROW BOARD","","",3,2631.6666666669998,7895]
["4420000000-N","PORT CHANGE MSG SIGN","","",5,11900,59500]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",20,100,2000]
["4430000000-N","DRUMS","","",640,48.59375,31100]
["4435000000-N","CONES","","",60,18.333333332999999,1100]
["4445000000-E","BARRICADES (III)","","",516,21.706976743999999,11200.8]
["4450000000-N","FLAGGER","","",1440,12,17280]
["4455000000-N","FLAGGER","","",300,145,43500]
["4465000000-N","TEMP CRASH CUSHIONS","","",1,20000,20000]
["4480000000-N","TMA","","",3,5400,16200]
["4485000000-E","PORT CONC BARRIER","","",1300,35,45500]
["4510000000-N","LAW ENFORCEMENT","","",96,50,4800]
["4650000000-N","TEMP RAISED PVMT MRKS","","",700,6.25,4375]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",17453,0.522689509,9122.5]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",25985,0.61968443299999998,16102.5]
["4688000000-E","THERMO PVT MKG LINES6\"90 MILS","","",32707,0.8,26165.599999999999]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",10797,0.92,9933.24]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",1197,2.4260651630000001,2904]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",587,2,1174]
["4705000000-E","THERMO LINES 16\" 120MIL","","",120,8.25,990]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",1106,8.6283905969999992,9543]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",10,78.5,785]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",153,118.37254901999999,18111]
["4770000000-E","4\" COLD APPL PLSTIC LINES **","(IV)","",15000,1.5,22500]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",266030,0.210408601,55975]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",2035,1,2035]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",1500,3,4500]
["4840000000-N","PAINT PVT MKG CHAR","","",16,25,400]
["4845000000-N","PAINT PVT MKG SYMBOL","","",300,25,7500]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",2774,1.75,4854.5]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",15502,1.75,27128.5]
["4850000000-E","LINE REML 4\" WIDE","","",5000,0.6,3000]
["4870000000-E","LINE REML 24\" WIDE","","",200,3,600]
["4875000000-N","REML OF SYMBL & CHAR","","",30,36,1080]
["4900000000-N","PERM RAISED PVMT MKRS","","",224,6.3571428570000004,1424]
["4905000000-N","SNOWPLB PVMT MRKER","","",1301,30,39030]
["4915000000-E","7' U-CHANNEL POSTS","","",15,38,570]
["4955000000-N","OBJECT MKR (END OF RD)","","",15,75,1125]
["5070000000-N","STD FOUNDAT ***********","(R1)","",36,1000,36000]
["5155000000-E","ELECT DUCT BD SIZE *****","(2\")","",60,6.09,365.4]
["","","(3\")","",92,6.74,620.08000000000004]
["","","(4\")","",37,7.25,268.25]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",65,4.24,275.60000000000002]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2)","",65,6.49,421.85]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2 15\")","",4477,10.26,45934.02]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2 15\")","",1880,11.14,20943.2]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2 15\")","",225,12.51,2814.75]
["5270000000-N","GENERIC LIGHT ITEM (EA)","BOLLARD LGT STD","",8,1000,8000]
["","","DAVIT STYLE LGT STD MH 35' SA 6'","",36,1900,68400]
["","","ELECTRICAL JUNCTION BOXES PC18","",13,432,5616]
["","","ELECTRICAL JUNCTION BOXES PG36","",1,1133,1133]
["","","LIGHT CONTROL EQUIP","RA 120/240V",1,4500,4500]
["","","POST TOP LIGHT STD","",14,731,10234]
["","","PT LUMINAIRES LED V","",14,1629,22806]
["","","RDW LUMINAIRES LED III","",36,750,27000]
["","","STD FOUNDATION B1","",8,250,2000]
["","","STD FOUNDATION R1S","",14,650,9100]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",1.5,670,1005]
["5325000000-E","**\" WATER LINE","(1\")","",1318,7,9226]
["5325200000-E","2\" WATER LINE","","",25,24,600]
["5325300000-E","3\" WATER LINE","","",233,12,2796]
["5325600000-E","6\" WATER LINE","","",1692,33.051034279,55922.35]
["5534000000-E","**\" VALVE","(1\")","",2,640,1280]
["","","(2\")","",1,935,935]
["5540000000-E","6\" VALVE","","",5,1098.72,5493.6]
["5643200000-E","2\" WATER METER","","",1,6825,6825]
["5656200000-E","2\" RPZ BACKFLOW PREVNT ASMBLY","","",1,3675,3675]
["5666000000-E","FIRE HYDRANT","","",1,2555,2555]
["5691200000-E","6\" SANIT GRAVITY SEWER","","",750,29,21750]
["5768000000-N","SANIT SEWER CLEAN-OUT","","",9,330,2970]
["5775000000-E","4' DIA UTILITY MANHOLE","","",2,1950,3900]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",329,7.7,2533.3000000000002]
["5871400000-E","6\" TRENCHLESS INSTALL (IN SOIL)","","",256,39,9984]
["5871410000-E","6\" TRENCHLESS INSTALL (NOT IN SOIL)","","",29,1,29]
["5882000000-N","GENERIC UTILITY ITEM (EA)","YARD HYDRANT","",1,495,495]
["6000000000-E","TEMP SILT FENCE","","",80050,1.957089319,156665]
["6006000000-E","EROS CNTRL STONE CL A","","",7170,49.801673639999997,357078]
["6009000000-E","EROS CNTRL STONE CL B","","",13490,49.648813936000003,669762.5]
["6012000000-E","SEDIMENT CNTROL STONE","","",9055,36.471258972999998,330247.25]
["6015000000-E","TEMP MULCH","","",100.5,426.36815920399999,42850]
["6018000000-E","SEED FOR TEMP SEED","","",2750,3.018181818,8300]
["6021000000-E","FERT FOR TEMP SEED","","",12.5,947.5,11843.75]
["6024000000-E","TEMP SLOPE DRNS","","",6700,23.424179104,156942]
["6029000000-E","SAFETY FENCE","","",8850,1.546610169,13687.5]
["6030000000-E","SILT EXCAV","","",16070,0.96617921600000001,15526.5]
["6036000000-E","MAT FOR EROS CONTROL","","",25200,1.2708333329999999,32025]
["6037000000-E","COIR FIBER MAT","","",335,5.0895522389999996,1705]
["6038000000-E","PERM SOIL REINF MAT","","",206,4.8495145629999996,999]
["6042000000-E","1/4\" HARDWARE CLOTH","","",6520,3.9148773010000002,25525]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",275,2.2363636360000001,615]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",25,133,3325]
["6048000000-E","FLOAT TURBIDITY CURTN","","",2525,19.822772276999999,50052.5]
["6070000000-N","SPECIAL STILLING BASINS","","",6,352.41666666700002,2114.5]
["6071012000-E","COIR FIBER WATTLE","","",4600,7.0978260869999996,32650]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1340,6.3395522389999996,8495]
["6071030000-E","COIR FIBER BAFFLE","","",4840,6.4876033059999996,31400]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",9,809.44444444400006,7285]
["","","(2\")","",1,1000,1000]
["6084000000-E","SEED AND MULCH","","",99.5,1568.5929648240001,156075]
["6087000000-E","MOWING","","",54.25,64.055299539000004,3475]
["6090000000-E","SEED FOR REPAIR SEED","","",1450,3.8103448279999999,5525]
["6093000000-E","FERT FOR REPAIR SEED","","",5.75,986.95652173899998,5675]
["6096000000-E","SEED FOR SUPP SEED","","",2950,3.338983051,9850]
["6108000000-E","FERTILIZER TOPDRESSING","","",86.5,960.69364161800002,83100]
["6111000000-E","IMPERVIOUS DIKE","","",50,120,6000]
["6114500000-N","SPECIALIZ HAND MOWING","","",60,49.166666667000001,2950]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",243,45.061728395000003,10950]
["6123000000-E","REFORESTATION","","",0.1,5000,500]
["6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","DISKING","",1.5,1000,1500]
["","","RIPPING","",1.5,1000,1500]
["","","SEED & MULCH; CENTIPEDE","TURF SEED 1 LB/1000SF",4.3,2625,11287.5]
["","","WETLAND GRASS ","PLANTING",1.5,3000,4500]
["6640000000-N","GENERIC PLANTING ITEM (EA) 1670","ABELIA X KALEIDOSCOP; KALEIDOSCOPE ABELIA","12-15\" 3 CONT",18,40,720]
["","","CORNUS FLORIDA; FLOWERING","DOGWOOD 7-8' 1 1/2\" CAL B&B",21,212.5,4462.5]
["","","GLEDITSIA TRIACANTHOS INERMIS; THORNLESS","HONEYLOCUST 12-14' 3\" CAL",7,247,1729]
["","","HEMEROCALLIS 'BUTTER-ED POPCORN' BUTTERED","POPCORN DAYLILY 1 CONT",87,6,522]
["","","ILEX CORNUTA 'CARISSA' CARISSA HOLLY","18-24\" 3 CONT",29,18,522]
["","","LAGERSTROEMIA 'ARAPAHO';","ARAPAHO CRAPE MYRTLE 6-7' B&B",6,187.5,1125]
["","","LIRIOPE MUSCARII 'BIG BLUE';","BIG BLUE LIRIOPE 1 CONTAINER",85,4.5,382.5]
["","","MAGNOLIA GRANDIFLRA 'LITTLE GEM': LITTLE GEM","MAGNOLIA 8-10' B&B",21,250,5250]
["","","MYRICA CERIFICA; WAX MYRTLE","4\" 15 CONTAINER",31,96,2976]
["","","QUERCUS VIRGINIANA; LIVE OAK 8-10 2 1/2\"","CALIPER 30 CONTAINER",13,286,3718]
["","","ROSA 'RADTKO'; RED DOUBLE KNOCKOUT","ROSE 18-24\" 3 CONTAINER",4,23,92]
["","","SCHIZACHYRIUM SCOPARIUM;","LITTLE BLUESTEM 1 CONTAINER",43,26,1118]
["","","SPIRAEA JAPONICA 'GOLDMOUND'; GOLD-","MOUND SPIRAEA 12-15\" 3 CONT",11,16,176]
["","","TAXODIUM DISTICHUM; BALD CLPRESS","6-8' 2\" CALIPER 15CONTAINER",29,108,3132]
["6650000000-E","MULCH FOR PLANTING","","",170,26,4420]
["6655000000-E","WATER FOR PLANTING","","",9,125,1125]
["6665000000-E","POSTEMERGENT HERBICIDAL TRTMENT","","",1545,0.25,386.25]
["6670000000-E","PREEMERGENT HERBICIDAL TRTMENT","","",1545,0.25,386.25]
["6674000000-N","GENERIC PLANTING ITEM (LS)","STREAMBANK BUFFER REFOREST-","ATION PLANTING",1,8000,8000]
["6675000000-E","GENERIC PLANT ITEM (SY)","SODDING","",2600,4.5,11700]
["6677000000-E","GENERIC PLANT ITEM (TON)","RIVER STONE","",4,275,1100]
["6690000000-E","GENERIC PLANT ITEM (LF)","LANDSCAPE METAL ","EDGING",184,6,1104]
["6900000000-E","TOPSOIL","","",600,21,12600]
["6905000000-N","PICNIC TABLE TERRZO &STL","","",4,4218,16872]
["6910000000-N","PICNIC SHELTER 1 TABLE","","",3,15173,45519]
["6970000000-N","GENERIC REST AREA ITEM (EA)","BICYLE PARKING ","",2,832.5,1665]
["","","DEPRESSED CURB HANDICAP","ACCESS 28' X 6'",1,1420,1420]
["","","","ACCESS 60' X 8'",1,3145,3145]
["","","PLACEMENT OF ","BOULDERS",8,230,1840]
["","","RECYCLING CONTAINER","",10,888,8880]
["","","TAPERED ALUMINM FLAG ","POLE",1,2836.05,2836.05]
["","","WASTE CONTAINER","",10,888,8880]
["","","WHEEL STOPS @ H/C ","PARKING",4,61,244]
["6975000000-N","GENERIC REST AREA ITEM (LS)","ELECTRICAL INSTALLATION FOR","REST AREA BUILDING",1,101926,101926]
["","","","STORAGE BLDG",1,4995,4995]
["","","GENERAL CONSTR OF","REST AREA BLDG",1,541504,541504]
["","","","STORAGE BLDG",1,53245,53245]
["","","IRRIGATION SYSTEM","",1,59415.93,59415.93]
["","","LANDSCAPE GRADING","",1,2341.71,2341.71]
["","","MECHL INSTALL FOR","REST AREA BLDG",1,123543,123543]
["","","PLUMB INSTALL OF REST","AREA BUILDING",1,99678,99678]
["","","RAINWATER COLLECTION ","SYSTEM",1,33260.22,33260.22]
["","","REST AREA SOLAR WATER HEATING","SYSTEM",1,16100,16100]
["6980000000-E","GENERIC REST AREA ITEM (LF)","3\" PVC UTILITY SLEEVE","",140,12,1680]
["","","6' WOOD FENCE","",18,70,1260]
["6982000000-E","GENERIC REST AREA ITEM (SF)","COMPOSITE DECKING","",864,12.21,10549.44]
["7060000000-E","SIGNAL CABLE","","",2995,2.5,7487.5]
["7120000000-E","VEH SIGNAL HD (12\" 3 SECT)","","",21,725,15225]
["7132000000-E","VEH SIGNAL HD (12\" 4 SECT)","","",2,830,1660]
["7144000000-E","VEH SIGNAL HD (12\" 5 SECT)","","",1,1000,1000]
["7264000000-E","MESSENGER CABLE (3/8\")","","",1150,4,4600]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",1770,5.5,9735]
["","","(2 2\")","",40,7,280]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",410,4.25,1742.5]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",16,200,3200]
["7420000000-E","2\"RISER WITH WEATHERHD","","",1,500,500]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",4488,6.5,29172]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",9170,0.85,7794.5]
["7575142000-N","900MHZ RADIO","","",2,3500,7000]
["7575142060-N","MOD RADIO INSTALL","","",1,1000,1000]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",8,8200,65600]
["7613000000-N","SOIL TEST","","",8,610,4880]
["7614100000-E","DRILLED PIER FOUND","","",56,805,45080]
["7636000000-N","SIGN FOR SIGNALS","","",7,230,1610]
["7684000000-N","SIGNAL CBNT FOUND","","",2,1200,2400]
["7756000000-N","CONTLR WITH CBNT 2070L BASE MTD","","",2,14000,28000]
["7780000000-N","DETECTOR CARD (2070L)","","",14,100,1400]
["7901000000-N","CBNT BASE EXTENDER","","",2,450,900]
["8017000000-N","CM&R TEMP ACCESS *******","(46+2150-L-)","",1,4456070.0199999996,4456070.0199999996]
["8021000000-N","REMV EXIST STR **********","(46+2150-L-)","",1,800000,800000]
["8035000000-N","REMV EXIST STR **********","(27+6050-L-)","",1,35000,35000]
["8112730000-N","PDA TESTING","","",14,2147.579285714,30066.11]
["8121000000-N","UNCL STR EXCAV STA ****","(16+0550-Y2-)","",1,35000,35000]
["","","(27+6050-L-)","",1,6000,6000]
["","","(46+2150-L-)","",1,20000,20000]
["8147000000-E","REINF CONC DECK SLAB","","",258062,27,6967674]
["8154000000-E","REINF CONC DECK SLABLTWT","","",58826,40,2353040]
["8161000000-E","GROOVING BRG FLOORS","","",282328,0.2,56465.599999999999]
["8175000000-E","CL AA CONC (BRG)","","",7604,600,4562400]
["8182000000-E","CL A CONC (BRG)","","",46,1317.36,60598.559999999998]
["8210000000-N","BRG APPR SLAB ***********","(16+0550-Y2-)","",1,75000,75000]
["","","(27+6050-L-)","",1,17000,17000]
["","","(46+2150-L-)","",1,75000,75000]
["8217000000-E","REINF STEEL (BRG)","","",7872,1.08,8501.76]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",1815942,1.05,1906739.1]
["8262000000-E","45\" PRESTR CONC GIRDR","","",4614.66,160,738345.6]
["8265000000-E","54\" PRESTR CONC GIRDR","","",12151.2,160,1944192]
["8333000000-E","16\" PRESTR CONC PILES","","",1430,54,77220]
["8336000000-E","20\" PRESTR CONC PILES","","",9125,70,638750]
["8353000000-E","30\" PRESTR CONC PILES","","",41700,125,5212500]
["8364000000-E","HP12X53 PILES","","",650,49.13,31934.5]
["8384200000-E","HP14X73 GALV PILES","","",980,68.31,66943.8]
["8392500000-E","PREDRILLING FOR PILES","","",167,45,7515]
["8393000000-N","PILE REDRIVES","","",244,202.94147541000001,49517.72]
["8475000000-E","TWO BAR METAL RAIL","","",6810.79,85,578917.15]
["8505000000-E","VERT CONC BARRIER RAIL","","",230.75,100,23075]
["8510000000-E","CONC MEDIAN BARRIER","","",3443,50,172150]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" x 2'-6\")","",6825.8,35,238903]
["8608000000-E","RIP RAP II (2'-0\")","","",1730,64.942254335000001,112350.1]
["8622000000-E","GEOTEXTILE FOR DRNG","","",1916,4.0430584549999997,7746.5]
["8657000000-N","ELASTOMERIC BEARINGS","","",2,603500,1207000]
["8692000000-N","FOAM JOINT SEALS","","",1,25000,25000]
["8706000000-N","EXPANSION JOINT SEALS","","",1,375000,375000]
["8713000000-N","MOD EXP JOINT SEALS","","",1,100000,100000]
["8734000000-N","ELEC CONDUIT SYS ********","(16+0550-Y2-)","",1,50000,50000]
["8741000000-N","STR DRN SYS ************","(46+2150-L-)","",1,1000000,1000000]
["8744000000-N","SOLAR ARRAY SUPPT PLTFORM","","",1,45000,45000]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",1150,130,149500]
["8847000000-E","GENERIC RET WALL ITEM (SF)","MSE RETAINING WALL NO 1","",3850,95,365750]
["","","SOUND BARRIER WALL","",32695,35,1144325]
["8860000000-N","GENERIC STR ITEM (LS)","POST TENSIONING TENDONS","",1,675000,675000]
["","","REML OF EXI BARGE AT","STA 45+2400-L-",1,30000,30000]
["","","STATIC AXIAL COMPRESS-IVE LOAD TEST ON","30\" SQ PRESTR CONC PILE",1,150000,150000]
["","","TIMBER FENDER BOARDS","AT CHANL BENTS",1,20000,20000]
["8867000000-E","GENERIC STR ITEM (LF)","78\" POST TENSIONED","PRESTR CONC GIRDERS",6489,575,3731175]
["","","78\" PRESTRESSED CONC","GIRDERS",11639.9,275,3200972.5]
["","","CLASSIC CONC BRG RAIL","",1262,200,252400]

{"sheet":"Items - Div 3","index":5,"n_rows":435,"n_cols":7,"rows_kept":435,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 3"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",4,1110000,4440000]
["0000400000-N","CONST SURVEYING","","",3,97033.333333332994,291100]
["0000700000-N","FIELD OFFICE","","",1,40000,40000]
["0001000000-E","CLEARING & GRUBBING","","",140,47285.714285713999,6620000]
["0008000000-E","SUPP CLEAR & GRUBBING","","",5,7000,35000]
["0015000000-N","SEAL ABANDONED WELLS","","",12,1000,12000]
["0022000000-E","UNCLAS EXCAV","","",63600,10,636000]
["0029000000-N","REINF BRG APPR **********","(144+4179 -L- LT)","",1,23200,23200]
["","","(145+6797 -L- RT)","",1,23200,23200]
["","","(17+27)","",1,12000,12000]
["","","(23+2500)","",1,49000,49000]
["","","(265+0000 -L- LT)","",1,16600,16600]
["","","(265+0000 -L- RT)","",1,22800,22800]
["","","(281+5183 -L- LT)","",1,11500,11500]
["","","(281+5183 -L- RT)","",1,10800,10800]
["","","(31+6368 -Y7-)","",1,8700,8700]
["","","(48+79 -Y8-)","",1,9100,9100]
["0036000000-E","UNDERCUT EXCAV","","",18200,5.5329670330000003,100700]
["0043000000-N","GRADING","","",1,65000,65000]
["0050000000-E","SUPP CLEAR & GRUBBING","","",2,500.5,1001]
["0057000000-E","UNDERCUT EXCAV","","",400,22,8800]
["0063000000-N","GRADING","","",1,75000,75000]
["0084000000-E","WICK DRNS","","",863000,0.35,302050]
["0106000000-E","BORROW EXCAV","","",2742379,4.9211079140000002,13495543]
["0127000000-N","EMBM'T SETTLEMT GAUGE","","",15,750,11250]
["0134000000-E","DRNG DITCH EXCAV","","",22600,4,90400]
["0156000000-E","REML OF EXT APSH PVT","","",8000,3,24000]
["0177000000-E","BRKING OF EXT ASPH PVT","","",2000,3,6000]
["0192000000-N","PROOF ROLLING","","",60,180,10800]
["0194000000-E","SEL GRANULR MATL CL III","","",73500,5.1706122450000001,380040]
["0195000000-E","SELECT GRANULAR MAT'L","","",87800,4.862323462,426912]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",136300,1.329603815,181225]
["0199000000-E","TEMP SHORING","","",250,25,6250]
["0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR EMBANKMT","STABIL 1",67800,13.5,915300]
["","","","STABIL 2",24900,10.64,264936]
["0257000000-E","GENERIC GRADING ITEM (LF)","HORIZONTAL INCLINOMETER CASING","",270,9,2430]
["0262000000-N","GENERIC GRADING ITEM (EA)","VW PIEZOMETER","",12,1700,20400]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",3626,37.388306673999999,135570]
["0320000000-E","FND CONDIT GEOTEXTILE","","",8197,2.2546663410000001,18481.5]
["0335200000-E","15\" DRNG PIPE","","",72,45,3240]
["0342000000-E","**\" SIDE DRN PIPE","(30\")","",48,45.5,2184]
["","","(36\")","",224,57.5,12880]
["0343000000-E","15\" SIDE DRN PIPE","","",24,22,528]
["0344000000-E","18\" SIDE DRN PIPE","","",2256,26,58656]
["0345000000-E","24\" SIDE DRN PIPE","","",220,34,7480]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(18\")","",50,350,17500]
["0354000000-E","***\" RC PIPE CULV *****","(30\" V)","",292,57.5,16790]
["","","(36\" V)","",344,73.5,25284]
["0372000000-E","18\" RC PIPE CULV III","","",2364,26,61464]
["0378000000-E","24\" RC PIPE CULV III","","",48,34,1632]
["0384000000-E","30\" RC PIPE CULV III","","",772,46,35512]
["0390000000-E","36\" RC PIPE CULV III","","",4488,58,260304]
["0396000000-E","42\" RC PIPE CULV III","","",792,71,56232]
["0402000000-E","48\" RC PIPE CULV III","","",732,88,64416]
["0408000000-E","54\" RC PIPE CULV III","","",464,147,68208]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",708,96,67968]
["0448200000-E","15\" RCP CULV CL IV","","",836,27.488038278000001,22980]
["0448300000-E","18\" RCP CULV CL IV","","",4552,27.5,125180]
["0448400000-E","24\" RCP CULV CL IV","","",784,37.5,29400]
["0448500000-E","30\" RCP CULV CL IV","","",600,50,30000]
["0448600000-E","36\" RCP CULV CL IV","","",1412,63,88956]
["0448700000-E","42\" RCP CULV CL IV","","",172,77,13244]
["0453000000-E","**\" PIPE END SECTION","(18\")","",4,700,2800]
["0546000000-E","**\" CAA PIPE CLVT *****\"","(18\" 0064\")","",784,33,25872]
["","","(60\" 0105\")","",144,718,103392]
["","","(84\" 0105\")","",192,335,64320]
["0564000000-E","**\" CAA PIPE ELBOW *****\"","(18\" 0064\")","",14,270,3780]
["0995000000-E","PIPE REML","","",2536,10,25360]
["1000000000-E","6\" SLOPE PROTECTION","","",350,100,35000]
["1011000000-N","FINE GRADING","","",1,350000,350000]
["1099500000-E","SHALLOW UNDERCUT","","",2400,8.4833333329999991,20360]
["1099700000-E","CL IV SUBGRD STABIL","","",4750,31.97,151857.5]
["1111000000-E","CL IV AGGREGAT STABIL","","",18750,29,543750]
["1121000000-E","AGGREGATE BASE CRSE","","",196400,29.121181263,5719400]
["1220000000-E","INCIDENTAL STONE BASE","","",7300,30.793972603,224796]
["1245000000-E","SHOULDER RECONST","","",72.28,2955,213587.4]
["1275000000-E","PRIME COAT","","",7414,4.5,33363]
["1297000000-E","MILL ASP PVT *****\" DTH","(1-1/2\")","",318373,0.9,286535.7]
["","","(2\")","",47147,1.7,80149.899999999994]
["","","(2-1/2\")","",113093,1,113093]
["","","(4\")","",5865,2,11730]
["1308000000-E","MILLN APSH PVT ***** - ****","(0\" TO 1-1/2\")","",1173,3.7,4340.1000000000004]
["1330000000-E","INCIDENTAL MILLING","","",2940,15.454421769,45436]
["1489000000-E","ASP CNC BAS CRS B250B","","",14586,47.226107226000003,688840]
["1491000000-E","ASP CNC BAS CRS B250C","","",51400,42.5,2184500]
["1498000000-E","ASP CONC INTR CRS I190B","","",26560,44.716679216999999,1187675]
["1503000000-E","ASP CONC INTR CRS I190C","","",38882,42.335065069000002,1646072]
["1519000000-E","ASP CNC SURF CRS S95B","","",67947,43.764286871000003,2973652]
["1523000000-E","ASP CNC SURF CRS S95C","","",50127,44.389819858000003,2225128.5]
["1525000000-E","ASP CONC SURF CRS SF95A","","",17343,44.985210170999999,780178.5]
["1525100000-E","ASP CONC SURF CRS SF95A LEVEL","","",80,80,6400]
["1575000000-E","ASP FOR PLANT MIX","","",14252,540.53115352199995,7703650]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",1090,75,81750]
["1840000000-E","MILLED RUMBLE STRIPS","","",93100,0.08,7448]
["1880000000-E","GENERIC PAV ITEM (TON)","PATCH EXISTING PAVEMT","(FULL DEPTH)",1915,129,247035]
["","","","I190C (MILL)",1612,126.05,203192.6]
["","","","S95B (FULL DEPTH)",25,151.94999999999999,3798.75]
["","","","S95B (MILL)",887,150,133050]
["","","PATCH EXT PVT (MILL)","",2245,127.9,287135.5]
["2000000000-N","RIGHT OF WAY MARKERS","","",8,150,1200]
["2022000000-E","SUBDRN EXCAV","","",2634.4,24.872456725999999,65524]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",8000,3.8250000000000002,30600]
["2036000000-E","SUBDRN CRS AGGREGATE","","",1350.8,56.741190406000001,76646]
["2044000000-E","6\" PERF SUBDRN PIPE","","",8000,15.05,120400]
["2070000000-N","SUBDRN PIPE OUTLET","","",17,341.17647058799997,5800]
["2077000000-E","6\" OUTLET PIPE","","",102,38.823529411999999,3960]
["2199000000-E","SANDBAG HEADWALLS","","",355,15,5325]
["2209000000-E","ENDWALLS","","",57.2,740,42328]
["2220000000-E","REINF ENDWALLS","","",18.7,1443.5828877009999,26995]
["2253000000-E","PIPE COLLARS","","",1,1000,1000]
["2264000000-E","PIPE PLUGS","","",1,1000,1000]
["2275000000-E","FLOWABLE FILL","","",12,225,2700]
["2286000000-N","MASNRY DRNG STRUCT","","",155,1070.967741935,166000]
["2308000000-E","MASNRY DRNG STRUCT","","",36,200,7200]
["2354000000-N","FRM W/GRATE 84022 STD","","",7,325,2275]
["2364000000-N","FRM W/2GRTS 84016 STD","","",18,485,8730]
["2364200000-N","FRM W/2GRTS 84020 STD","","",34,455,15470]
["2365000000-N","FRM W/2GRTS 84022 STD","","",49,435,21315]
["2367000000-N","FRM W/2GRTS 84029 STD","","",31,498.54838709699999,15455]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",3,540,1620]
["","","(F)","",3,540,1620]
["","","(G)","",11,540,5940]
["2396000000-N","FRM W/COVER STD 84054","","",2,350,700]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",3,1300,3900]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",2,485,970]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",18,485,8730]
["2549000000-E","2'-6\" CONC CURB & GUTTR","","",2400,14,33600]
["2556000000-E","SHOULDER BERM GUTTER","","",15531,14.308157877999999,222220]
["2591000000-E","4\" CONC SIDEWALK","","",100,48.7,4870]
["2605000000-N","CONC CURB RAMP","","",217,1923,417291]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",3060,38.503267974000003,117820]
["2724000000-E","PC REINF BARR SNGL FC","","",128,105,13440]
["2739000000-E","GENERIC PAVING ITEM 852 (SY)","REML OF CONC ISLAND","",60,101.1,6066]
["2753000000-E","GENERIC PAVING ITEM 846 (LF)","2'-0\" CURB & GUTTER REM & REPLACE","",400,45.7,18280]
["","","2'-6\" CURB & GUTTER REM & REPLACE","",390,47.05,18349.5]
["2759000000-N","GENERIC PAVING ITEM (EA)","ADJUST MONUMTS","",48,351.85,16888.8]
["2800000000-N","ADJ CATCH BASINS","","",2,502.65,1005.3]
["2830000000-N","ADJ MANHOLES","","",175,404.28971428599999,70750.7]
["2845000000-N","ADJ METER OR VAL BOX","","",81,351.85,28499.85]
["3000000000-N","IMPACT ATTEN  350","","",3,8300,24900]
["3030000000-E","STL BM GUARDRAIL","","",19187.5,14.983713355000001,287500]
["3045000000-E","SBGR SHOP CURVED","","",525,16,8400]
["3105000000-N","SBGR TERM SECT","","",2,100,200]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",20,28.5,570]
["3195000000-N","GR ANCHOR  AT-1","","",5,400,2000]
["3210000000-N","GR ANCHOR  CAT-1","","",13,450,5850]
["3215000000-N","GR ANCHOR  III","","",8,1387.5,11100]
["3270000000-N","GR ANCHOR  350","","",28,1864.285714286,52200]
["3285000000-N","GR ANCHOR  M-350","","",6,1700,10200]
["3317000000-N","GR ANCHOR  B-77","","",34,1450,49300]
["3360000000-E","REM EXISTING GUARDRAIL","","",525,1,525]
["3380000000-E","TEMP STL BM GUARDRAIL","","",250,10,2500]
["3389100000-N","TEMP GDRL ANCH UNIT350","","",4,1200,4800]
["3389200000-E","CABLE GUIDERAIL","","",22500,7,157500]
["3389500000-N","ADDIT GUIDERAIL POSTS","","",10,55,550]
["3389600000-N","CBL GUIDERAIL ANCH UNIT","","",26,1500,39000]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",50900,2.25,114525]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",3320,14,46480]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",610,25,15250]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",2700,4,10800]
["3542000000-E","MET LINE PST 48\" CL FEN","","",230,20,4600]
["3548000000-E","MET TERM PST 48\" CL FEN","","",20,45,900]
["3557000000-E","ADDITIONAL BARBED WIRE","","",500,1,500]
["3564000000-E","SGL GATE **HIGH **WIDE **OPEN","(47\" 20' 20')","",9,600,5400]
["3572000000-E","CHAIN LINK FENCE RESET","","",1600,10,16000]
["3574000000-E","GENERIC FENCING ITEM 867 (LF)","40\" WOOD RAIL FENCE RESET","",100,25,2500]
["3628000000-E","RIP RAP CL I","","",320,61.4,19648]
["3649000000-E","RIP RAP CL B","","",1006,61.978131212999998,62350]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",9034,2.174507416,19644.5]
["3659000000-N","PREFORMED SCOUR HOLE","","",5,3500,17500]
["4048000000-E","REINF CONC FOUNDTN","","",70,950,66500]
["4054000000-E","PLN CONC FOUNDTN","","",2,450,900]
["4057000000-E","OVERHEAD FOOTING","","",30,1200,36000]
["4060000000-E","SUPP BRKAWAY STL BM","","",32150,3.2,102880]
["4066000000-E","SUPPORTS SIMPLE STL BM","","",13868,2.2000000000000002,30509.599999999999]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",3697,4.1255612660000001,15252.2]
["4078000000-E","SUPPT 2-LB STL U-CHAN","","",40,34.799999999999997,1392]
["4082100000-N","SUPPT OVRHD SIGN STR **","(19+00 -Y5- EBL)","",1,54063.25,54063.25]
["","","(37+30 -Y5- WBL)","",1,67939.75,67939.75]
["4096000000-N","SIGN ERECTION  D","","",15,68.333333332999999,1025]
["4102000000-N","SIGN ERECTION  E","","",92,54.891304347999998,5050]
["4108000000-N","SIGN ERECTION  F","","",32,75,2400]
["4109000000-N","SIGN ERECT  *** (OVRHD)","(A)","",8,575,4600]
["4110000000-N","SIGN ERECT  *** (GRD MTD)","(A)","",25,475,11875]
["","","(B)","",19,375,7125]
["4114000000-N","SIGN ERECTION MILEMKRS","","",40,55,2200]
["4115000000-N","SIGN ERECTION OVERLAY (OVRHD)","","",3,675,2025]
["4116000000-N","SIGN ERECTION OVERLAY (GRD MTD)","","",4,675,2700]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(A)","",1,475,475]
["","","(B)","",5,475,2375]
["4116200000-N","SIGN ERECTION REPOSIT OVRHD","","",4,4240,16960]
["4138000000-N","DISPOSE SUPPORT STL BM","","",2,150,300]
["4152000000-N","DISP SIGN SYST STL BM","","",7,150,1050]
["4155000000-N","DISP SIGN SYST U-CHAN","","",38,1,38]
["4234000000-N","DISP SIGN A OR B(OVRHD)","","",4,175,700]
["4236000000-N","DISPOSE SIGN A B OR C (GRD MTD)","","",2,100,200]
["4238000000-N","DISPOSE SIGN D E F","","",1,1,1]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",1830,4.8719562840000004,8915.68]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",412,22.5,9270]
["4410000000-E","WORK ZONE SIGN (BARR)","","",604,7.8274006619999996,4727.75]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",6533,4.4000000000000004,28745.200000000001]
["4420000000-N","PORT CHANGE MSG SIGN","","",2,5000,10000]
["4430000000-N","DRUMS","","",350,40,14000]
["4435000000-N","CONES","","",100,18,1800]
["4445000000-E","BARRICADES ( III)","","",616,29.090909091,17920]
["4455000000-N","FLAGGER","","",376,170,63920]
["4457000000-N","TEMP TRAFFIC CONTROL","","",1,100000,100000]
["4465000000-N","TEMP CRASH CUSHIONS","","",2,6000,12000]
["4480000000-N","TMA","","",2,3000,6000]
["4485000000-E","PORT CONC BARRIER","","",390,27.9,10881]
["4510000000-N","LAW ENFORCEMT","","",1843,47.55,87634.65]
["4516000000-N","SKINNY DRUM","","",100,36,3600]
["4650000000-N","TEMP RAISED PVT MRKS","","",203,5,1015]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",219321,0.46886891800000002,102832.8]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",296303,0.51905623599999995,153797.92000000001]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",3620,2.2176795579999999,8028]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",3930,2.2999999999999998,9039]
["4705000000-E","THERMO LINES 16\" 120MIL","","",600,2.65,1590]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",5468,5.0133686910000002,27413.1]
["4721000000-E","THERMO PVT MKG CHAR 120","","",80,35.200000000000003,2816]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",624,81.847275640999996,51072.7]
["4726000000-E","HIP THERMO PVT MKG LINE 4\" 90 MILS","","",100,4.55,455]
["4810000000-E","PAINT PVT MARKINGS 4\"","","",1244813,9.0711873999999998E-2,112919.32]
["4820000000-E","PAINT PVT MARKINGS 8\"","","",1770,0.45,796.5]
["4825000000-E","PAINT PVT MARKINGS 12\"","","",6080,1,6080]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",600,1.5,900]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",5258,1.853708634,9746.7999999999993]
["4840000000-N","PAINT PVT MKG CHAR","","",60,25.15,1509]
["4845000000-N","PAINT PVT MKG SYMBOL","","",579,30.15,17456.849999999999]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",12931,0.89614105600000005,11588]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",130847,0.95,124304.65]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMTS)","",3492,2.75,9603]
["4850000000-E","LINE REML 4\" WIDE","","",7100,0.7,4970]
["4900000000-N","PERM RAISED PVT MKERS","","",1817,3.9665382500000002,7207.2]
["4905000000-N","SNOWPLB PVT MRKER","","",5175,21.330019323999998,110382.85]
["5255000000-N","PORTABLE LIGHTING","","",1,100000,100000]
["5325600000-E","6\" WATER LINE","","",639,53.575899843999998,34235]
["5326200000-E","12\" WATER LINE","","",6149,72.5,445802.5]
["5328000000-E","30\" WATER LINE","","",2104,275,578600]
["5540000000-E","6\" VALVE","","",6,1000,6000]
["5558000000-E","12\" VALVE","","",11,2300,25300]
["5560000000-E","30\" VALVE","","",6,27500,165000]
["5589100000-E","1\" AIR RELEASE VALVE","","",1,7000,7000]
["5648000000-N","RELOCATE WATER METER","","",16,550,8800]
["5666000000-E","FIRE HYDRANT","","",1,3750,3750]
["5672000000-N","RELOCATE FIRE HYDRANT","","",8,3750,30000]
["5691300000-E","8\" SANIT GRAVITY SEWER","","",115,100,11500]
["5691400000-E","10\" SANIT GRAV SEWER","","",631,190,119890]
["5709400000-E","8\" FORCE MAIN SEWER","","",395,150,59250]
["5709600000-E","12\" FORCE MAIN SEWER","","",476,245,116620]
["5768000000-N","SANIT SEWER CLEAN-OUT","","",1,1500,1500]
["5775000000-E","4' DIA UTILITY MANHOLE","","",3,4000,12000]
["5776000000-E","5' DIA UTILITY MANHOLE","","",6,6000,36000]
["5781000000-E","UTILITY MH WALL 4' DIA","","",2,125,250]
["5782000000-E","UTILITY MH WALL 5' DIA","","",54,150,8100]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",450,10,4500]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",348,10,3480]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",761,10,7610]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",5720,7.5,42900]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",1817,26,47242]
["5835000000-E","**\" ENCASEMT PIPE","(42\")","",550,325,178750]
["5836000000-E","24\" ENCASEMT PIPE","","",700,110,77000]
["5871400000-E","6\" TRENCHLESS INSTALL (IN SOIL)","","",250,120,30000]
["5871410000-E","6\" TRENCHLESS INSTALL (NOT IN SOIL)","","",106,1,106]
["5882000000-N","GENERIC UTILITY ITEM (EA)","CONNECTION DETAIL  2","",6,56500,339000]
["","","CONNECTION DETAIL  4","",14,4750,66500]
["5888000000-E","GENERIC UTILITY ITEM (LF)","42\" DUMMY ENCASEMT ","PIPE",550,260,143000]
["","","54\" DUMMY ENCASEMT","PIPE",280,390,109200]
["5912000000-N","GENERIC UTILITY ITEM (LS)","4\" WATER METER ASSEM","",1,20000,20000]
["","","REM EXT 4\" H2O METER","ASSEMBLY",1,5500,5500]
["6000000000-E","TEMP SILT FENCE","","",132672,1.4833416239999999,196797.9]
["6006000000-E","EROS CNTRL STONE CL A","","",3340,58.353293413000003,194900]
["6009000000-E","EROS CONTRL STONE CL B","","",7173,62.621734281000002,449185.7]
["6012000000-E","SEDIMT CONTROL STONE","","",7103,55.774179924000002,396164]
["6015000000-E","TEMP MULCHING","","",341.03,408.90484708100001,139448.82]
["6018000000-E","SEED FOR TEMP SEEDING","","",8400,5.8690476189999998,49300]
["6021000000-E","FERT FOR TEMP SEEDING","","",36.25,793.79310344800001,28775]
["6024000000-E","TEMP SLOPE DRNS","","",30250,3.9950413220000001,120850]
["6029000000-E","SAFETY FENCE","","",19400,1.123195876,21790]
["6030000000-E","SILT EXCAV","","",100990,3.0909000889999998,312150]
["6036000000-E","MAT FOR EROS CONTROL","","",107280,1.0896905290000001,116902]
["6037000000-E","COIR FIBER MAT","","",2850,3.0464912279999998,8682.5]
["6038000000-E","PERM SOIL REINF MAT","","",3135,4.2503987240000001,13325]
["6042000000-E","1/4\" HARDWARE CLOTH","","",11708,3.499607106,40973.4]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",1040,2.505576923,2605.8000000000002]
["6045000000-E","**\" TEMP PIPE","(24\")","",100,50,5000]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",50,50,2500]
["6048000000-E","FLOAT TURBIDITY CURTN","","",225,31.333333332999999,7050]
["6069000000-E","STILLING BASINS","","",400,35,14000]
["6070000000-N","SPECIAL STILLING BASINS","","",10,211.94399999999999,2119.44]
["6071010000-E","WATTLE","","",1080,6.0268518520000001,6509]
["6071012000-E","COIR FIBER WATTLE","","",4275,5.3464912279999997,22856.25]
["6071014000-E","COIR FIBER WATTLE BARR","","",250,12.1,3025]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1120,6.7366071429999996,7545]
["6071030000-E","COIR FIBER BAFFLE","","",8345,3.6115937690000002,30138.75]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",33,751.54666666699995,24801.040000000001]
["","","(2\")","",4,1000,4000]
["","","(3\")","",1,1200,1200]
["6084000000-E","SEEDING AND MULCHING","","",370,1640.160135135,606859.25]
["6087000000-E","MOWING","","",124.1,104.230459307,12935]
["6090000000-E","SEED FOR REPAIR SEEDING","","",5408,6.3661057689999998,34427.9]
["6093000000-E","FERT FOR REPAIR SEEDING","","",28.36,802.247884344,22751.75]
["6096000000-E","SEED FOR SUPP SEEDING","","",9750,3.9948717949999999,38950]
["6108000000-E","FERTILIZER TOPDRESSING","","",291,603.52233677000004,175625]
["6111000000-E","IMPERVIOUS DIKE","","",255,100,25500]
["6114500000-N","SPECIALIZED HAND MOW","","",245,50,12250]
["6117000000-N","RESP FOR EROS CONTROL","","",186,10.967741934999999,2040]
["6123000000-E","REFORESTATION","","",5,1000,5000]
["6126000000-E","STRMBNK REFORESTATON","","",0.14000000000000001,10000,1400]
["6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","COMPOST BLANKET","",20,4800,96000]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",4,829.35,3317.4]
["7060000000-E","SIGNAL CABLE","","",2345,1.9106609809999999,4480.5]
["7120000000-E","VEHICLE SIGNAL HD (12\" 3 SECT)","","",8,700,5600]
["7132000000-E","VEHICLE SIGNAL HD (12\" 4 SECT)","","",2,825,1650]
["7252000000-E","MESSENGER CABLE (1/4\")","","",390,1.85,721.5]
["7279000000-E","TRACER WIRE","","",1450,0.55000000000000004,797.5]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",1745,6.73739255,11756.75]
["","","(2 2\")","",185,8.7364864860000004,1616.25]
["","","(21-1/2\")","",1815,8.75,15881.25]
["","","(4 2\")","",10,9.25,92.5]
["7301000000-E","DIRECT DRILL (***********)","(1 2\")","",510,16.782352940999999,8559]
["","","(2 1-1/2\")","",1585,19,30115]
["","","(2 2\")","",180,18.75,3375]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",40,354.38,14175.2]
["7348000000-N","JUNCTION BOX (OVER-SIZED HVY-DUTY)","","",7,547.48571428599996,3832.4]
["7360000000-N","WOOD POLE","","",7,1000,7000]
["7372000000-N","GUY ASSEMBLY","","",2,420,840]
["7384000000-E","***\" RISER WITH **************","(1-1/2\" WEATHERHEAD)","",5,525,2625]
["7420000000-E","2\" RISR WITH WEATHERHD","","",6,379,2274]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",4893,6.3512058040000001,31076.45]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",6405,1.3666666670000001,8753.5]
["7485000000-N","WRLESS MAGN SENSOR DET SYS","","",1,13500,13500]
["7516000000-E","COMMUN CABLE (** FIBER)","(12)","",1550,1.3,2015]
["7552000000-N","INTERCONNECT CENTER","","",2,1340,2680]
["7564000000-N","FIBER-OPTIC TRANS DROP/REP","","",2,2000,4000]
["7566000000-N","DELINEATOR MARKER","","",5,89,445]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",1,12000,12000]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",1,18500,18500]
["7613000000-N","SOIL TEST","","",2,1250,2500]
["7614100000-E","DRILLED PIER FOUND","","",16,700,11200]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",2,52.5,105]
["7642200000-N"," II PED W/ FOUND","","",3,1123,3369]
["7648000000-N","RELOCATE EXISTING SIGN","","",1,139.75,139.75]
["7684000000-N","SIGNAL CABINET FOUND","","",1,800,800]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",2,307.60000000000002,615.20000000000005]
["7756000000-N","CONTLR WITH CBNT 2070L BASE MTD","","",1,14500,14500]
["7780000000-N","DETECTOR CARD( 2070L)","","",9,139.377777778,1254.4000000000001]
["7901000000-N","CABINET BASE EXTENDER","","",1,450,450]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","5/8\" X 10' GROUNDING ","ELECTRODE",60,90,5400]
["","","CCTV CAMERA ASSEM","",8,4600,36800]
["","","CCTV WOOD POLE","",7,1950,13650]
["","","CENTRAL MEDIA CONVTR","",6,410,2460]
["","","DMS","",6,73500,441000]
["","","DMS ACCESS LADDER","",5,5375,26875]
["","","DMS PEDESTAL STR( A)","",4,45700,182800]
["","","DMS PEDESTAL STR( B)","",1,54500,54500]
["","","EQUIP CBNT DISCONNECT","",12,200,2400]
["","","FIELD EQUIPMT CABINET","",8,4200,33600]
["","","METER BASE/DISCONECT ","COMBO PANEL",9,700,6300]
["","","SOLAR POWER ASSEM","",1,13500,13500]
["","","VIDEO ETHERNET ","DECODER",4,825,3300]
["","","VIDEO ETHERNET ","ENCODER",8,800,6400]
["","","WOOD PEDESTAL","",4,150,600]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","INTEGRATION AND ","CONFIGURATION",1,5100,5100]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","4 SOLID BARE GRD CON- ","DUCTOR",520,1.75,910]
["","","3-WIRE COPPER FEEDER ","CONDUC- TORS",1895,1.75,3316.25]
["","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",125,4,500]
["","","4-WIRE COPPER FEEDER ","CONDUC- TORS",1630,15,24450]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","ITS OVERHEAD FOOTING","",40,725,29000]
["8017000000-N","CM&R TEMP ACCESS ******","(265+5358-L-)","",1,625000,625000]
["","","(48+7900-Y8-)","",1,625000,625000]
["8035000000-N","REMV EXIST STR **********","(17+2700 -L-)","",1,95000,95000]
["","","(23+2500-L-)","",1,75000,75000]
["8084000000-N","FND EXCAV EB** STA*******","(01 38+5027-Y7-)","",1,10000,10000]
["","","(02 38+5027-Y7-)","",1,10000,10000]
["8108000000-E","**'-**\" DIA DRILLD PIERS","(6'-0\")","",2424,700,1696800]
["8112730000-N","PDA TESTING","","",8,1775,14200]
["8113000000-N","SID INSPECTIONS","","",8,1200,9600]
["8114000000-N","SPT TESTING","","",16,1500,24000]
["8115000000-N","CSL TESTING","","",4,2200,8800]
["8121000000-N","UNCL STR EXCAV STA *****","(23+2500-L-)","",1,30000,30000]
["8126000000-N","CULV EXCAV @ ************","(52+0900-Y7-)","",1,25000,25000]
["8133000000-E","FND CONDIT MAT BOX CULV","","",97,50,4850]
["8147000000-E","REINF CONC DECK SLAB","","",135340,24.890944288,3368740.4]
["8161000000-E","GROOVING BRG FLOORS","","",139213,0.36278113400000001,50503.85]
["8175000000-E","CL AA CONC (BRG)","","",751.1,785.89095992499995,590282.69999999995]
["8182000000-E","CL A CONC (BRG)","","",2020.5,538.49443207100001,1088028]
["8196000000-E","CL A CONC (CULV)","","",173.3,650,112645]
["8210000000-N","BRG APPR SLAB ***********","(147+3889-L-LT)","",1,41000,41000]
["","","(147+3889-L-RT)","",1,41000,41000]
["","","(17+2700 -L-)","",1,22000,22000]
["","","(182+9994-L-)","",1,46000,46000]
["","","(23+2500-L-)","",1,50000,50000]
["","","(265+5358-L-LT)","",1,41000,41000]
["","","(265+5358-L-RT)","",1,53000,53000]
["","","(281+5183-L-LT)","",1,43000,43000]
["","","(281+5183-L-RT)","",1,40000,40000]
["","","(38+5027-Y7-)","",1,63000,63000]
["","","(48+7900-Y8-)","",1,52000,52000]
["8217000000-E","REINF STEEL (BRG)","","",636377,0.968316658,616214.44999999995]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",122361,0.96664255799999999,118279.35]
["8238000000-E","SPIRL COL REINF STL BRG","","",114806,1.5,172209]
["8245000000-E","REINF STEEL (CLVT)","","",23796,1,23796]
["8259000000-E","36\" PRESTR CONC GIRDR","","",349,140,48860]
["8265000000-E","54\" PRESTR CONC GIRDR","","",6352.55,217,1378503.35]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",1891.37,270,510669.9]
["8280000000-E","STRUCTURAL STEEL","","",4232116,1.6020354830000001,6780000]
["8333000000-E","16\" PRESTR CONC PILES","","",2588,66,170808]
["8336000000-E","20\" PRESTR CONC PILES","","",3975,79.446540881000004,315800]
["8350000000-E","24\" PRESTR CONC PILES","","",2260,112,253120]
["8364000000-E","HP12X53 PILES","","",7445,52.667562122,392110]
["8384000000-E","HP14X73 PILES","","",575,40,23000]
["8391000000-N","STEEL PILE POINTS","","",30,70,2100]
["8392500000-E","PREDRILLING FOR PILES","","",200,150,30000]
["8393000000-N","PILE REDRIVES","","",107,390.18691588799999,41750]
["8475000000-E","TWO BAR METAL RAIL","","",161.66999999999999,175,28292.25]
["8503000000-E","CONC BARRIER RAIL","","",5368.35,69,370416.15]
["8505000000-E","VERT CONC BARRIER RAIL","","",140.25,120,16830]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",176.67,175,30917.25]
["8524000000-E","**\" CHAIN LINK FENCE","(72\")","",2204.19,109,240256.71]
["8531000000-E","4\" SLOPE PROTECTION","","",12556,64.75,813001]
["8608000000-E","RIP RAP II (2'-0\")","","",3772,86.005302227000001,324412]
["8622000000-E","GEOTEXTILE FOR DRNG","","",4182,3.7962099469999999,15875.75]
["8654000000-N","DISC BEARINGS","","",1,75000,75000]
["8657000000-N","ELASTOMERIC BEARINGS","","",3,22166.666666666999,66500]
["8706000000-N","EXPANSION JOINT SEALS","","",1,601000,601000]
["8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(147+3889-L-RT)","",1,67000,67000]
["","","(38+5027-Y7-)","",1,17200,17200]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",700,145,101500]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",5500,87.44,480920]
["","","(2)","",5450,87.44,476548]
["8867000000-E","GENERIC STR ITEM (LF)","20\" COMPOSITE PILE","",1000,134,134000]
["8892000000-E","GENERIC STR ITEM (SF)","GALV 18\" STL SHEET ","PILES",1693,40,67720]

{"sheet":"Items - Div 4","index":6,"n_rows":290,"n_cols":7,"rows_kept":290,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 4"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",3,199000,597000]
["0001000000-E","CLEARING & GRUBBING","","",3,140000,350000]
["0008000000-E","SUPP CLEAR & GRUBBING","","",1,100,100]
["0022000000-E","UNCLAS EXCAV","","",9900,1,9900]
["0030000000-N","BRG APP SUB REG TIER**","(32+1850 -L-)","",1,18000,18000]
["0036000000-E","UNDERCUT EXCAV","","",1000,11.1,11100]
["0043000000-N","GRADING","","",1,540000,540000]
["0050000000-E","SUPP CLEAR & GRUBBING","","",1,1000,1000]
["0057000000-E","UNDERCUT EXCAV","","",200,35,7000]
["0106000000-E","BORROW EXCAV","","",6400,10,64000]
["0134000000-E","DRNG DITCH EXCAV","","",1912,7.8716527200000002,15050.6]
["0156000000-E","REML OF EXT ASPH PVMT","","",8500,3.65,31025]
["0196000000-E","GEOTEXTILE SOIL STABILI","","",3350,1.643283582,5505]
["0199000000-E","TEMP SHORING","","",450,75,33750]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISP OF PETROLEUM","CONTAMINATED SOIL",55,78.5,4317.5]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",1380,16.753623187999999,23120]
["0320000000-E","FND CONDIT GEOTEXTILE","","",4100,1.309756098,5370]
["0335200000-E","15\" DRNG PIPE","","",928,37.393103447999998,34700.800000000003]
["0335300000-E","18\" DRNG PIPE","","",424,40.468867924999998,17158.8]
["0335400000-E","24\" DRNG PIPE","","",568,45.85,26042.799999999999]
["0335500000-E","30\" DRNG PIPE","","",456,56.260526316000004,25654.799999999999]
["0335600000-E","36\" DRNG PIPE","","",28,78,2184]
["0335800000-E","48\" DRNG PIPE","","",16,115,1840]
["0343000000-E","15\" SIDE DRN PIPE","","",36,75,2700]
["0366000000-E","15\" RC PIPE CULV III","","",436,44,19184]
["0378000000-E","24\" RC PIPE CULV III","","",156,45.85,7152.6]
["0402000000-E","48\" RC PIPE CULV III","","",12,115,1380]
["0448000000-E","***\" RCP CULV CL IV","(12\")","",248,44,10912]
["","","(48\")","",28,125,3500]
["0448200000-E","15\" RCP CULV CL IV","","",3920,40.509897959,158798.79999999999]
["0448300000-E","18\" RCP CULV CL IV","","",1552,46.855670103000001,72720]
["0448400000-E","24\" RCP CULV CL IV","","",1640,52.079390244000002,85410.2]
["0448500000-E","30\" RCP CULV CL IV","","",1284,63.529127725999999,81571.399999999994]
["0448600000-E","36\" RCP CULV CL IV","","",432,79.650000000000006,34408.800000000003]
["0654000000-E","***X***\"CSP ARCH CULV **","(77\" X 52\" 0109\")","",80,205,16400]
["0995000000-E","PIPE REML","","",3313,8.4769091460000006,28084]
["1011000000-N","FINE GRADING","","",1,462000,462000]
["1099500000-E","SHALLOW UNDERCUT","","",1250,13.4,16750]
["1099700000-E","CL IV SUBGRD STABILIZ","","",2350,16.268085106000001,38230]
["1121000000-E","AGGR BASE COURSE","","",235,39.042553191000003,9175]
["1220000000-E","INCIDENTAL STONE BASE","","",1270,26.377952755999999,33500]
["1275000000-E","PRIME COAT","","",318,7.6572327040000001,2435]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",26000,1.25,32500]
["","","(2\")","",222432,0.25,55608]
["","","(3\")","",100,45,4500]
["1308000000-E","MILLN ASP PVT ***** - *****","(0\" TO 1-1/2\")","",5100,2.25,11475]
["1330000000-E","INCIDENTAL MILLING","","",8750,5.2174285710000001,45652.5]
["1489000000-E","ASP CNC BAS CRS B250B","","",10000,38.725000000000001,387250]
["1498000000-E","ASP CONC INTR CRS I190B","","",8650,38.542196531999998,333390]
["1519000000-E","ASP CNC SURF CRS S95B","","",39149,28.275051725000001,1106940]
["1575000000-E","ASP FOR PLANT MIX","","",3211,601.60853316700002,1931765]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",310,157.838709677,48930]
["2000000000-N","RIGHT OF WAY MARKERS","","",30,200,6000]
["2022000000-E","SUBDRN EXCAV","","",168,5.8,974.4]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",750,4.5,3375]
["2033000000-E","SUBDRN FINE AGGREGATE","","",126,26,3276]
["2036000000-E","SUBDRN COARSE AGGR","","",126,33.1,4170.6000000000004]
["2044000000-E","6\" PERF SUBDRN PIPE","","",750,11.45,8587.5]
["2070000000-N","SUBDRN PIPE OUTLET","","",2,356,712]
["2077000000-E","6\" OUTLET PIPE","","",12,25.4,304.8]
["2209000000-E","ENDWALLS","","",6,700,4200]
["2220000000-E","REINF ENDWALLS","","",14.8,700,10360]
["2253000000-E","PIPE COLLARS","","",14,655,9170]
["2264000000-E","PIPE PLUGS","","",1,1180,1180]
["2275000000-E","FLOWABLE FILL","","",75,220,16500]
["2286000000-N","MASNRY DRNG STRUCT","","",119,988.23529411799996,117600]
["2308000000-E","MASNRY DRNG STRUCT","","",22.1,217.55656108599999,4808]
["2352000000-N","FRM W/GRATE 840**** STD","(84016)","",5,425,2125]
["2364000000-N","FRM W/2GRTS 84016 STD","","",24,448,10752]
["2365000000-N","FRM W/2GRTS 84022 STD","","",3,435,1305]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",17,507.88235294100002,8634]
["","","(F)","",37,496.10810810800001,18356]
["","","(G)","",29,511.24137931000001,14826]
["2396000000-N","FRM W/COVER STD 84054","","",2,355,710]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",9,706,6354]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",12,706,8472]
["2462000000-E","**\" SLUICE GATE","(6\")","",1,2765,2765]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",120,20,2400]
["2538000000-E","**'-**\" CONC CURB & GUTR","(2'-9\")","",1190,16.850000000000001,20051.5]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",1020,12.25,12495]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",14470,15.170214236,219513]
["2591000000-E","4\" CONC SIDEWALK","","",4960,25.984274194000001,128882]
["2600000000-N","RETROFIT EXT CURB RAMP","","",8,425,3400]
["2605000000-N","CONC CURB RAMP","","",88,784.88636363600006,69070]
["2612000000-E","6\" CONC DRIVEWAY","","",660,39.787878788,26260]
["2619000000-E","4\" CONC PAVED DITCH","","",90,33.9,3051]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",1120,40.75,45640]
["2815000000-N","ADJ DROP INLETS","","",24,350,8400]
["2830000000-N","ADJ MHS","","",43,393.02325581399998,16900]
["2845000000-N","ADJ METER OR VAL BOX","","",79,344.62025316500001,27225]
["2860000000-N","CONVERT CB TO JB","","",1,1275,1275]
["3030000000-E","STL BM GUARDRAIL","","",312.5,15.7,4906.25]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",10,10,100]
["3215000000-N","GR ANCHOR  III","","",2,1475,2950]
["3270000000-N","GR ANCHOR  350","","",2,1875,3750]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",917,4.6500000000000004,4264.05]
["3542000000-E","MET LINE PST 48\" CL FEN","","",79,37.5,2962.5]
["3548000000-E","MET TERM PST 48\" CL FEN","","",14,88,1232]
["3554000000-E","MET GATE PST **\"CL FEN D","(48\")","",4,105,420]
["3565000000-E","DBL GATE **HIGH **WIDE **OPEN","(48\" 6' 12')","",2,820,1640]
["3628000000-E","RIP RAP CL I","","",150,63.36,9504]
["3635000000-E","RIP RAP CL II","","",180,44.2,7956]
["3649000000-E","RIP RAP CL B","","",80,68.875,5510]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",2865,2.530541012,7250]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",1130,3.7759292040000001,4266.8]
["4096000000-N","SIGN ERECTION  D","","",4,80,320]
["4102000000-N","SIGN ERECTION  E","","",37,46.5,1720.5]
["4108000000-N","SIGN ERECTION  F","","",6,46.5,279]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(D)","",4,125,500]
["","","(E)","",17,95,1615]
["4155000000-N","DISP SIGN SYST U-CHAN","","",39,3.4358974359999999,134]
["4158000000-N","DISP SIGN SYST WOOD","","",4,35,140]
["4192000000-N","DISP SUPPT U-CHAN","","",21,2.3333333330000001,49]
["4238000000-N","DISP SIGN D E F","","",1,5,5]
["4400000000-E","WORK ZONE SIGN (STAT)","","",1121,4.3729705619999999,4902.1000000000004]
["4405000000-E","WORK ZONE SIGN (PORT)","","",472,28.711440677999999,13551.8]
["4410000000-E","WORK ZONE SIGN (BARR)","","",202,15.6,3151.2]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",1246,3.78,4709.88]
["4415000000-N","FLASHING ARROW BOARD","","",2,2645,5290]
["4420000000-N","PORT CHANGE MSG SIGN","","",5,5100,25500]
["4430000000-N","DRUMS","","",630,53,33390]
["4435000000-N","CONES","","",75,19.666666667000001,1475]
["4445000000-E","BARRICADES ( III)","","",264,66.890909090999997,17659.2]
["4450000000-N","FLAGGER","","",1800,23,41400]
["4455000000-N","FLAGGER","","",600,150,90000]
["4457000000-N","TEMP TRAFFIC CONTROL","","",1,22250,22250]
["4507000000-E","WATER FILLED BARRIER","","",640,50,32000]
["4510000000-N","LAW ENFORCEMENT","","",536,39.119402985000001,20968]
["4516000000-N","SKINNY DRUM","","",50,40,2000]
["4650000000-N","TEMP RAISED PVMT MRKS","","",395,6.9620253160000001,2750]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",7508,0.70685135899999996,5307.04]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",32435,0.90427778599999997,29330.25]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",992,2.403225806,2384]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",1795,2.63091922,4722.5]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",699,8.0522174540000009,5628.5]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",51,100,5100]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",155,125.741935484,19490]
["4770000000-E","4\" COLD APPL PLSTIC LINES  **","(II)","",1625,3,4875]
["","","(IV)","",1500,2.65,3975]
["4780000000-E","8\" COLD APPL PLSTIC LINES  **","(II)","",84,6,504]
["4810000000-E","PAINT PVMT MKGS 4\"","","",493189,0.12424545200000001,61276.49]
["4820000000-E","PAINT PVMT MKGS 8\"","","",6025,0.39207468899999998,2362.25]
["4830000000-E","PAINT PVT MKGS LINE 16\"","","",50,2,100]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",2866,3.0601884159999999,8770.5]
["4840000000-N","PAINT PVT MKG CHAR","","",80,37.25,2980]
["4845000000-N","PAINT PVT MKG SYMBOL","","",235,39.829787234000001,9360]
["4850000000-E","LINE REML 4\" WIDE","","",9070,1.4035281150000001,12730]
["4860000000-E","LINE REML 8\" WIDE","","",150,2,300]
["4875000000-N","REML OF SYMBL & CHAR","","",4,65,260]
["4900000000-N","PERM RAISED PVMT MKRS","","",225,8,1800]
["5325600000-E","6\" WATER LINE","","",274,61.737226276999998,16916]
["5325800000-E","8\" WATER LINE","","",184,76.400000000000006,14057.6]
["5326200000-E","12\" WATER LINE","","",885,112.86,99881.1]
["5540000000-E","6\" VALVE","","",4,1195,4780]
["5546000000-E","8\" VALVE","","",1,1722,1722]
["5558000000-E","12\" VALVE","","",2,3160,6320]
["5648000000-N","RELOCATE WATER METER","","",19,843.68421052600002,16030]
["5649000000-N","RECONNECT H2O METER","","",4,1455,5820]
["5653100000-E","RELC **\" DCV BACKFLOW PREVNT A","(3/4\")","",1,2000,2000]
["5672000000-N","RELOCATE FIRE HYDRANT","","",9,2844.8888888890001,25604]
["5678600000-E","8\" LINE STOP","","",1,7522,7522]
["5691000000-E","**\" SANIT GRAV SEWER","(15\")","",848,94,79712]
["5691300000-E","8\" SANIT GRAV SEWER","","",588,71.469387755,42024]
["5691400000-E","10\" SANIT GRAV SEWER","","",2381,78.536749264999997,186996]
["5691500000-E","12\" SANIT GRAV SEWER","","",53,146.19999999999999,7748.6]
["5692000000-E","30\" SANIT GRAV SEWER","","",265,271,71815]
["5768000000-N","SANIT SEWER CLEAN-OUT","","",8,2000,16000]
["5775000000-E","4' DIA UTILITY MH","","",16,2705.5,43288]
["5776000000-E","5' DIA UTILITY MH","","",2,3190,6380]
["5781000000-E","UTILITY MH WALL 4' DIA","","",33,415.45454545500002,13710]
["5782000000-E","UTILITY MH WALL 5' DIA","","",13,370,4810]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",1595,5.5500313480000001,8852.2999999999993]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",2278,9.8686918349999999,22480.880000000001]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",910,8.0500000000000007,7325.5]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",300,65,19500]
["5816000000-N","ABANDON UTILITY MH","","",10,655,6550]
["5828000000-N","REM UTILITY MH","","",8,1200,9600]
["5882000000-N","GENERIC UTILITY ITEM (EA)","ROTATE TOP FOR EXT MH","",1,1350,1350]
["5894000000-E","GENERIC UTILITY ITEM (CY)","SELECT MATL CL VI","57 STONE",250,60,15000]
["6000000000-E","TEMP SILT FENCE","","",17285,1.7992479029999999,31100]
["6006000000-E","EROS CNTRL STONE CL A","","",130,49.338461537999997,6414]
["6009000000-E","EROS CNTRL STONE CL B","","",485,41.603092783999998,20177.5]
["6012000000-E","SEDIMENT CNTROL STONE","","",1685,30.79347181,51887]
["6015000000-E","TEMP MULCHING","","",13,434.61538461499998,5650]
["6018000000-E","SEED FOR TEMP SEED","","",850,4,3400]
["6021000000-E","FERT FOR TEMP SEED","","",4,800,3200]
["6024000000-E","TEMP SLOPE DRNS","","",400,11.625,4650]
["6029000000-E","SAFETY FENCE","","",400,1.9,760]
["6030000000-E","SILT EXCAV","","",1130,18.451327434,20850]
["6036000000-E","MAT FOR EROS CONTROL","","",3150,2.223809524,7005]
["6037000000-E","COIR FIBER MAT","","",1230,6.0731707320000003,7470]
["6038000000-E","PERM SOIL REINF MAT","","",1000,3.9,3900]
["6042000000-E","1/4\" HARDWARE CLOTH","","",3855,3.5,13492.5]
["6045000000-E","**\" TEMP PIPE","(15\")","",35,80,2800]
["","","(30\")","",55,70,3850]
["","","(36\")","",125,50.5,6312.5]
["","","(54\")","",175,120,21000]
["6048000000-E","FLOAT TURBIDITY CURTN","","",145,35,5075]
["6070000000-N","SPECIAL STILLING BASINS","","",51,252.94117647100001,12900]
["6071012000-E","COIR FIBER WATTLE","","",330,6.25,2062.5]
["6071014000-E","COIR FIBER WATTLE BARR","","",100,12,1200]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",15,20,300]
["6071030000-E","COIR FIBER BAFFLE","","",400,5,2000]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",1,1200,1200]
["","","(2\")","",1,1200,1200]
["6084000000-E","SEED & MULCHING","","",14,1346.4285714289999,18850]
["6087000000-E","MOWING","","",11,106.818181818,1175]
["6090000000-E","SEED FOR REPAIR SEED","","",200,8.5,1700]
["6093000000-E","FERT FOR REPAIR SEED","","",0.5,800,400]
["6096000000-E","SEED FOR SUPP SEED","","",350,5.5714285710000002,1950]
["6108000000-E","FERTILIZER TOPDRESSING","","",9.75,676.92307692300005,6600]
["6111000000-E","IMPERVIOUS DIKE","","",65,107.384615385,6980]
["6114500000-N","SPECIALIZED HAND MOW","","",18,67.777777778000001,1220]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",75,250,18750]
["6123000000-E","REFORESTATION","","",0.1,5000,500]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",8,760,6080]
["7060000000-E","SIGNAL CABLE","","",8382,2.183488428,18302]
["7120000000-E","VEHICLE SIGNAL HD (12\" 3 SECT)","","",41,733.46341463399995,30072]
["7132000000-E","VEHICLE SIGNAL HD (12\" 4 SECT)","","",6,875.66666666699996,5254]
["7144000000-E","VEHICLE SIGNAL HD (12\" 5 SECT)","","",5,1041.4000000000001,5207]
["7252000000-E","MESSENGER CABLE (1/4\")","","",950,1.5,1425]
["7264000000-E","MESSENGER CABLE (3/8\")","","",2520,1.655357143,4171.5]
["7279000000-E","TRACER WIRE","","",100,0.6,60]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",610,7.5,4575]
["","","(1-2\")","",690,5.5,3795]
["","","(2-2\")","",80,7,560]
["","","(3-2\")","",25,8,200]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",400,1.25,500]
["7301000000-E","DIRECT DRILL (***********)","(1 2\")","",150,17,2550]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",28,159.67857142899999,4471]
["7348000000-N","JUNCTION BOX (OVER-SIZED HVY-DUTY)","","",3,480.33333333299998,1441]
["7360000000-N","WOOD POLE","","",5,770,3850]
["7372000000-N","GUY ASSEMBLY","","",17,332.58823529400001,5654]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",4,336,1344]
["7432000000-E","2\" RISER WITH TUBING","","",1,381,381]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",10180,5.0933693519999999,51850.5]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",12180,1.3492610840000001,16434]
["7481000000-N","SITE SURVEY","","",1,1033,1033]
["7481240000-N","CAMERA W/O INT LOOP EMUL PORCESS","","",4,612,2448]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",1,5981,5981]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",1400,1.45,2030]
["7540000000-N","SPLICE ENCLOSURE","","",1,1000,1000]
["7541000000-N","MOD SPLICE ENCLOSURE","","",2,520,1040]
["7552000000-N","INTERCONNECT CENTER","","",1,982,982]
["7566000000-N","DELINEATOR MARKER","","",2,99,198]
["7575160000-E","REM EXT COMM CABLE","","",1350,0.9,1215]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",12,7582,90984]
["7613000000-N","SOIL TEST","","",12,949.33333333300004,11392]
["7614100000-E","DRILLED PIER FOUND","","",88,831.36363636399994,73160]
["7636000000-N","SIGN FOR SIGNALS","","",9,245.66666666699999,2211]
["7642200000-N"," II PED W/ FOUND","","",7,1383,9681]
["7684000000-N","SIGNAL CABINET FOUND","","",2,631,1262]
["7756000000-N","CONTLR WITH CBNT 2070L BASE MTD","","",3,11190.333333332999,33571]
["7780000000-N","DETECTOR CARD ( 2070L)","","",19,116.05263157900001,2205]
["7901000000-N","CABINET BASE EXTENDER","","",2,273,546]
["7948000000-N","TRAFFIC SIGNAL REML","","",1,2577,2577]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","ETHERNET EDGE SWITCH","",1,2427,2427]
["8017000000-N","CM&R TEMP ACCESS ******","(32+1850-L-)","",1,67000,67000]
["8035000000-N","REMV EXIST STR **********","(32+1850-L-)","",1,60000,60000]
["8063000000-N","PC RCBC @ STA **********","(33+6500-L-)","",1,83300,83300]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",554.5,677,375396.5]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",228,677,154356]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",355.5,200,71100]
["8114000000-N","SPT TESTING","","",1,500,500]
["8115000000-N","CSL TESTING","","",1,1900,1900]
["8121000000-N","UNCL STR EXCAV STA *****","(32+1850-L-)","",1,31000,31000]
["8126000000-N","CULV EXCAV @ ************","(33+6500-L-)","",1,35000,35000]
["8140000000-E","CHANNEL EXCAV","","",390,25,9750]
["8156000000-E","CONC WEARING SURFACE","","",16094,7.5,120705]
["8161000000-E","GROOVING BRIDGE FLOORS","","",18263,0.35,6392.05]
["8175000000-E","CL AA CONC (BRIDGE)","","",134.69999999999999,340,45798]
["8182000000-E","CL A CONC (BRIDGE)","","",263.89999999999998,733,193438.7]
["8196000000-E","CL A CONC (CULV)","","",36.4,1000,36400]
["8210000000-N","BRG APPR SLAB ***********","(32+1850-L-)","",1,93000,93000]
["8217000000-E","REINF STEEL (BRIDGE)","","",81661,1,81661]
["8224000000-E","EPOXY COAT REINF STL BRG","","",4478,1.1499999999999999,5149.7]
["8238000000-E","SPIRL COL REINF STL BRG","","",14386,1.75,25175.5]
["8245000000-E","REINF STEEL (CULVERT)","","",2627,2,5254]
["8364000000-E","HP12X53 PILES","","",275,65,17875]
["8391000000-N","STEEL PILE POINTS","","",22,200,4400]
["8482000000-E","THREE BAR METAL RAIL","","",484.67,148,71731.16]
["8590000000-E","RIP RAP CL **","(I 2'-0\" THICK)","",300,20,6000]
["8622000000-E","GEOTEXTILE FOR DRNG","","",333,5,1665]
["8657000000-N","ELASTOMERIC BEARINGS","","",1,25000,25000]
["8692000000-N","FOAM JOINT SEALS","","",1,24000,24000]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",6500,133,864500]
["8825000000-E","GENERIC CLVT ITEM (CY)","SELECT MATL CL VI 57","STONE BACKFILL",300,70,21000]
["8893000000-E","GENERIC STR ITEM (SY)","GEOTEXTILE FABRIC- 4","",640,2.25,1440]

{"sheet":"Items - Div 5","index":7,"n_rows":835,"n_cols":7,"rows_kept":835,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 5"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",18,503877.17555555602,9069789.1600000001]
["0000400000-N","CONST SURVEYING","","",2,554000,1108000]
["0000900000-N","GENERIC MISC ITEM (LS)","CNTRL OF VIBRATION","",1,41500,41500]
["0000910000-N","GENERIC MISC ITEM (HR)","EXPLORATORY EXCAV- ","STD",750,202.5,151875]
["","","EXPLORATORY EXCAV-","VACUUM",250,250,62500]
["0001000000-E","CLEARING & GRUBBING","","",130,69230.769230769001,9000000]
["0008000000-E","SUPP CLEAR & GRUBBING","","",5,4500,22500]
["0015000000-N","SEAL ABANDONED WELLS","","",4,1066.58,4266.32]
["0022000000-E","UNCLAS EXCAV","","",1498700,3.995579502,5988175]
["0029000000-N","REINF BRG APPR **********","(10+00.00)","",1,1200,1200]
["","","(125+85.60 -L- EB)","",1,52873.89,52873.89]
["","","(126+08.04 -L- WB)","",1,52875.19,52875.19]
["","","(139+64.19 -LDFEB-)","",1,53584.31,53584.31]
["","","(14+12.00 -L-)","",1,29540,29540]
["","","(18+75)","",1,25000,25000]
["","","(19+19.55 -DFLW-)","",1,53584.31,53584.31]
["","","(20+52.61 -Y7-)","",1,39198.269999999997,39198.269999999997]
["","","(25+58.00 -DFFLY-)","",1,20290.97,20290.97]
["","","(28+17.07-L-)","",1,54500,54500]
["","","(34+62.88 -DFEB-)","",1,10838.89,10838.89]
["","","(36+69.26 -DFWB-)","",1,12897.2,12897.2]
["0030000000-N","BRG APP SUB REG TIER**","(14+83.43-L-)","",1,8000,8000]
["","","(16+02.50)","",1,10000,10000]
["","","(17+86.40 -L-)","",1,7500,7500]
["","","(24+70.18-DFWB-)","",1,12664.61,12664.61]
["0036000000-E","UNDERCUT EXCAV","","",8200,10.848780487999999,88960]
["0043000000-N","GRADING","","",4,57000,228000]
["0050000000-E","SUPP CLEARING & GRUBBING","","",7,2172,15204]
["0057000000-E","UNDERCUT EXCAV","","",3730,14.608579088000001,54490]
["0063000000-N","GRADING","","",3,391333.33333333302,1174000]
["0106000000-E","BORROW EXCAV","","",1337703,5.0978749690000003,6819442.6399999997]
["0127000000-N","EMBM'T SETTLEMENT GAUGE","","",2,2500,5000]
["0134000000-E","DRNG DITCH EXCAV","","",61835,2.6066305490000001,161181]
["0141000000-E","BERM DITCH CONST","","",1710,11.95,20434.5]
["0156000000-E","REML OF EXT ASPH PVT","","",80100,2.42,193842]
["0163000000-E","REML OF EXT CONC PVT","","",67450,1.32,89034]
["0177000000-E","BRKING OF EXT ASPH PVT","","",12210,2.88,35164.800000000003]
["0185000000-E","BRKING OF EXT CONC PVT","","",7800,5.18,40404]
["0192000000-N","PROOF ROLLING","","",100,247.49,24749]
["0195000000-E","SELECT GRANULAR MAT'L","","",10660,27.324812383000001,291282.5]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",43420,1.6702095809999999,72520.5]
["0199000000-E","TEMP SHORING","","",22211,20.418216199,453509]
["0220000000-E","ROCK EMBANKMENTS","","",150,85,12750]
["0222000000-E","GEOTEXTILE ROCK EMBNK","","",190,4,760]
["0223000000-E","ROCK PLATING","","",1700,34.64,58888]
["0234000000-E","GENERIC GRAD ITEM (CY)","CLAY CORE","",2100,64.209999999999994,134841]
["","","UNDERCUT EXCAV","",1193,29,34597]
["0241000000-E","GENERIC GRAD ITEM (SY)","GEOTEXTILE FOR EMBKMT","STABIL",160,4,640]
["0255000000-E","GENERIC GRAD ITEM (TON)","AGG SHDR BORROW","",1.5,200,300]
["","","HAULING & DISP OF PETROLUM","CONTAMINATED SOIL",1500,162.16,243240]
["","","HAULING & DISPOSAL OF 'PETROLEUM ","CONTAMINATED SOIL",150,78,11700]
["0264000000-E","GENERIC GRAD ITEM (SMI)","SHDR GRADING","",95.59,3022.901663354,288959.17]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",6274,20.471431303999999,128437.75999999999]
["0320000000-E","FND CONDIT GEOTEXTILE","","",19670,1.832572445,36046.699999999997]
["0331000000-E","GENERIC DRNG ITEM (CY)","FILTER DIAPHRAGM","",20,64.209999999999994,1284.2]
["0335200000-E","15\" DRNG PIPE","","",248,33.709677419000002,8360]
["0335300000-E","18\" DRNG PIPE","","",368,39.684782609000003,14604]
["0335600000-E","36\" DRNG PIPE","","",328,75,24600]
["0342000000-E","**\" SIDE DRN PIPE","(30\")","",280,70.87,19843.599999999999]
["","","(36\")","",144,106.56,15344.64]
["","","(48\")","",32,209.14,6692.48]
["0343000000-E","15\" SIDE DRN PIPE","","",5232,36.25,189660]
["0344000000-E","18\" SIDE DRN PIPE","","",1524,51.313385826999998,78201.600000000006]
["0345000000-E","24\" SIDE DRN PIPE","","",1568,94.78,148615.04000000001]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",26,249.75,6493.5]
["","","(18\")","",6,299.41000000000003,1796.46]
["","","(24\")","",6,412.47,2474.8200000000002]
["","","(30\")","",4,530.01,2120.04]
["0350000000-E","***\" RC PIPE CULV, CONTR DESIGN","(24\")","",244,103.71,25305.24]
["0354000000-E","***\" RC PIPE CULV *****","(18\", V)","",352,85.07,29944.639999999999]
["","","(30\", V)","",1180,113.83,134319.4]
["","","(36\", V)","",416,138.51,57620.160000000003]
["0366000000-E","15\" RC PIPE CULV III","","",3828,41.697805643000002,159619.20000000001]
["0372000000-E","18\" RC PIPE CULV III","","",4284,40.923202613999997,175315]
["0378000000-E","24\" RC PIPE CULV III","","",2608,48.809202454000001,127294.39999999999]
["0384000000-E","30\" RC PIPE CULV III","","",2268,134.37761904800001,304768.44]
["0390000000-E","36\" RC PIPE CULV III","","",640,121.200125,77568.08]
["0396000000-E","42\" RC PIPE CULV III","","",572,138.51,79227.72]
["0402000000-E","48\" RC PIPE CULV III","","",192,178.07,34189.440000000002]
["0408000000-E","54\" RC PIPE CULV III","","",164,330.2,54152.800000000003]
["0414000000-E","60\" RC PIPE CULV III","","",428,311,133108]
["0420000000-E","66\" RC PIPE CULV III","","",520,347.53,180715.6]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",532,232.27,123567.64]
["","","(54\")","",156,255.61,39875.160000000003]
["0448200000-E","15\" RCP CULV CL IV","","",18992,38.243597303999998,726322.4]
["0448300000-E","18\" RCP CULV CL IV","","",2200,43.671090909,96076.4]
["0448400000-E","24\" RCP CULV CL IV","","",1436,60.464066852000002,86826.4]
["0448500000-E","30\" RCP CULV CL IV","","",1692,72.400000000000006,122500.8]
["0448600000-E","36\" RCP CULV CL IV","","",48,187.09,8980.32]
["0453000000-E","**\" PIPE END SECTION","(15\")","",1,825,825]
["0576000000-E","**\" CS PIPE CULV *****\"","(36\", 0.079\")","",140,207.02,28982.799999999999]
["","","(48\", 0.109\")","",36,230.69,8304.84]
["","","(60\", 0.138\")","",314,270.14999999999998,84827.1]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",2450,37.604473468999998,92130.96]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",726,61.400358126999997,44576.66]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",232,200.59,46536.88]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",13,228.349230769,2968.54]
["","","(18\", 0.064\")","",7,357.59714285699999,2503.1799999999998]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(24\", 0.500\")","",228,459.49,104763.72]
["","","(30\", 0.500\")","",178,558.22,99363.16]
["","","(60\", 0.875\")","",58,1272.1199999999999,73782.960000000006]
["","","(66\", 0.875\")","",155,1205.28,186818.4]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(24\", 0.500\")","",228,609.49,138963.72]
["","","(30\", 0.500\")","",178,758.22,134963.16]
["","","(60\", 0.875\")","",58,1572.12,91182.96]
["","","(66\", 0.875\")","",155,1555.28,241068.4]
["0995000000-E","PIPE REML","","",15372,13.250195160000001,203682]
["1000000000-E","6\" SLOPE PROTECTION","","",160,82,13120]
["1011000000-N","FINE GRADING","","",1,2000000,2000000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",195830,2.4,469992]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",1960,195,382200]
["1077000000-E","57 STONE","","",110,37,4070]
["1099500000-E","SHALLOW UNDERCUT","","",5500,9.7763636359999992,53770]
["1099700000-E","CL IV SUBGRD STABIL","","",10950,22.332191780999999,244537.5]
["1110000000-E","STABILIZER AGG","","",1000,29.5,29500]
["1115000000-E","GEOTEXTILE FOR PVT STABILIZ","","",121000,3.71,448910]
["1121000000-E","AGG BAS COURSE","","",206058,15.063331682999999,3103920]
["1176000000-E","SOIL CEMENT BAS","","",130560,2.2999999999999998,300288]
["1187000000-E","PC FOR SOIL CEMENT BAS","","",3591,145,520695]
["1209000000-E","ASPH CURING SEAL","","",48960,3,146880]
["1220000000-E","INCIDENTAL STONE BAS","","",12170,33.932374692000003,412957]
["1245000000-E","SHDR RECONST","","",164.23,2018.8658588559999,331558.34000000003]
["1275000000-E","PRIME COAT","","",4235,3.75,15881.25]
["1297000000-E","MILL ASP PVT *****\" DTH","(1-1/2\")","",1020678,0.78110530499999997,797257]
["","","(2\")","",305476,0.80626988700000002,246296.1]
["","","(2-1/2\")","",137707,0.55903941000000001,76983.64]
["","","(3\")","",8510,4.2538190360000003,36200]
["1308000000-E","MILLN ASPH PVT ***** - ****","(0\" TO 1-1/2\")","",12090,4.115136476,49752]
["","","(0\" TO 2\")","",1777,4.3499999999999996,7729.95]
["","","(1-1/2\" TO 2-1/2\")","",114046,1.05,119748.3]
["","","(1-1/2\" TO 3\")","",10600,1.41,14946]
["1330000000-E","INCIDENTAL MILLING","","",43486,4.533002346,197122.14]
["1489000000-E","ASP CNC BAS CRS B25.0B","","",34529,36.199116685,1249919.3]
["1491000000-E","ASP CNC BAS CRS B25.0C","","",99110,29.135606900999999,2887630]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",63590,35.504233370000001,2257714.2000000002]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",89980,29.568626361,2660585]
["1519000000-E","ASP CNC SURF CRS S9.5B","","",274623,30.292033368999999,8318889.0800000001]
["1523000000-E","ASP CNC SURF CRS S9.5C","","",85593,27.312957834999999,2337798]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",47019,31.985573066000001,1503929.66]
["1525100000-E","ASP CONC SURF CRS SF9.5A LEVEL","","",625,46.04,28775]
["1575000000-E","ASP FOR PLANT MIX","","",37994,616.29981602400005,23415695.210000001]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",10,825,8250]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",1295,136.74517374499999,177085]
["1704000000-E","PATCHING EXIST PVT","","",19335,99.973509179999994,1932987.8]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",140,57,7980]
["1839200000-E","APPLICATION OF ULTRATHIN HOT MIX ASPH","","",3960,3.5,13860]
["1840000000-E","MILLED RUMBLE STRIPS","","",118100,0.33663505500000002,39756.6]
["1847000000-E","******\"PCC PVT THRU LNS","(12\")","",65200,64,4172800]
["1858000000-E","******\"PCC PVT RAMPS","(12\")","",2000,68,136000]
["1869000000-E","******\"PCC PVT MISC","(12\")","",2477,69,170913]
["1881000000-E","GENERIC PAVING ITEM (LF)","PEDESTRIAN SAFTY RAIL","",120,52,6240]
["1891000000-E","GENERIC PAVING ITEM (SY)","6\" JOINTED CONC W/","WIRE MESH (4X4 W3XW3)",470,54,25380]
["1902000000-N","SURF TEST CONC PVT","","",1,50000,50000]
["1924000000-N","FIELD LAB RENTAL, PCCP","","",1,25000,25000]
["2000000000-N","RIGHT OF WAY MARKERS","","",436,164.72477064200001,71820]
["2022000000-E","SUBDRN EXCAV","","",7881.6,15.153471376000001,119433.60000000001]
["2033000000-E","SUBDRN FINE AGG","","",3991.2,39.642212868000001,158220]
["2044000000-E","6\" PERF SUBDRN PIPE","","",23750,8.9705263160000008,213050]
["2070000000-N","SUBDRN PIPE OUTLET","","",50,252,12600]
["2077000000-E","6\" OUTLET PIPE","","",300,18.12,5436]
["2099000000-E","SHDR DRN","","",21300,6,127800]
["2110000000-E","4\" SHDR DRN PIPE","","",21300,2,42600]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",1100,15,16500]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",15,275,4125]
["2143000000-E","BLOTTING SAND","","",20,84.76,1695.2]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",26,1018.25,26474.5]
["2209000000-E","ENDWALLS","","",50.2,846.41434262899998,42490]
["2220000000-E","REINF ENDWALLS","","",45.7,850,38845]
["2253000000-E","PIPE COLLARS","","",10.241,934.913582658,9574.4500000000007]
["2264000000-E","PIPE PLUGS","","",0.5,150,75]
["2275000000-E","FLOWABLE FILL","","",231.3,182.16346735799999,42134.41]
["2286000000-N","MASNRY DRNG STRUCT","","",515,1128.705320388,581283.24]
["2297000000-E","MASNRY DRNG STRUCT","","",42.731000000000002,675.00011701100004,28843.43]
["2308000000-E","MASNRY DRNG STRUCT","","",449.1,203.07281229099999,91200]
["2354000000-N","FRM W/GRATE 840.22 STD","","",19,500,9500]
["2363000000-N","FRM W/2GRTS 840.**** STD","(840.33)","",19,475,9025]
["2364000000-N","FRM W/2GRTS 840.16 STD","","",17,488.23529411800001,8300]
["2364200000-N","FRM W/2GRTS 840.20 STD","","",112,475,53200]
["2365000000-N","FRM W/2GRTS 840.22 STD","","",172,500,86000]
["2366000000-N","FRM W/2GRTS 840.24 STD","","",13,438.076923077,5695]
["2367000000-N","FRM W/2GRTS 840.29 STD","","",16,546.875,8750]
["2374000000-N","FRM-GRT-HD 840.03 **","(E)","",25,515.20000000000005,12880]
["","","(F)","",52,549.42307692300005,28570]
["","","(G)","",57,532.50877192999997,30353]
["2396000000-N","FRM W/COVER STD 840.54","","",40,397.05,15882]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",10,1100,11000]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",4,500,2000]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",9,858.33333333300004,7725]
["2462000000-E","**\" SLUICE GATE","(8\")","",4,1000,4000]
["2484000000-E","GENERIC DRNG ITEM (LF)","4\" PERF OR SLOT DRN PIPE W/","GEOTEXTILE SOCK",18,19,342]
["","","4\" SOLID DRN PIPE","",50,26,1300]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 18\")","",640,18,11520]
["","","(9\" X 18\")","",840,20,16800]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",3330,13.195195195,43940]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",27615,16.196224877999999,447258.75]
["2556000000-E","SHDR BERM GUTTER","","",12263,25.175242600000001,308724]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",4135,25.048065296000001,103573.75]
["2591000000-E","4\" CONC SIDEWALK","","",12250,29.200816326999998,357710]
["2600000000-N","RETROFIT EXT CURB RAMP","","",25,549.4008,13735.02]
["2605000000-N","CONC CURB RAMP","","",156,1126.7307692310001,175770]
["2612000000-E","6\" CONC DRIVEWAY","","",1220,48.885245902000001,59640]
["2619000000-E","4\" CONC PAVED DITCH","","",1010,59,59590]
["2627000000-E","4\" CONC ISLAND COVER","","",45,100,4500]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",185,67,12395]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",4070,52.830466829999999,215020]
["2703000000-E","CONC BARR  ******","(IV)","",160,81.349999999999994,13016]
["2710000000-N","CONC BARR TRANS SECTN","","",6,20779.2,124675.2]
["2717000000-E","VAR HT CONC BARR *******","(II)","",540,142.5,76950]
["","","(III)","",2800,117.45,328860]
["2724000000-E","PC REINF BARR SNGL FC","","",7400,64.7,478780]
["2738000000-E","GENERIC PAV ITEM (SY)","8\" CONC TRUCK APRON","",864,96,82944]
["2752000000-E","GENERIC PAV ITEM (LF)","MED HAZARD PROTECTN","",410,300,123000]
["2759000000-N","GENERIC PAV ITEM (EA)","REM & REPL CURB RAMPS","",2,1700,3400]
["2815000000-N","ADJ DROP INLETS","","",5,450,2250]
["2830000000-N","ADJ MHS","","",182,429.61637362599998,78190.179999999993]
["2845000000-N","ADJ METER OR VAL BOX","","",357,447.43366946800001,159733.82]
["2893000000-N","CONVERT CB TO JB W/MH","","",1,965,965]
["2905000000-N","CONVERT DI TO JB","","",1,1383.64,1383.64]
["2920000000-N","CONVERT DI TO CB","","",2,961.91,1923.82]
["2938000000-N","CONVERT DI TO JB W/MH","","",9,1512.52,13612.68]
["2995000000-N","GENERIC DRNG ITEM (EA)","CONV EXT CATCH BASIN TO TRAFFIC BEARING","JUNCTION BOX W/ MH",6,1384.1,8304.6]
["3000000000-N","IMPACT ATTEN  350","","",10,10950,109500]
["3030000000-E","STL BM GRDRL","","",43637.5,14.592981954000001,636801.25]
["3045000000-E","SBGR SHOP CURVED","","",137.5,15.272727272999999,2100]
["3105000000-N","SBGR TERM SECT","","",10,81,810]
["3150000000-N","ADDIT GRDRL POSTS","","",88,28.159090909,2478]
["3180000000-N","GR ANCHOR  **********","(III-MOD)","",7,2000,14000]
["3195000000-N","GR ANCHOR  AT-1","","",4,492.5,1970]
["3210000000-N","GR ANCHOR  CAT-1","","",37,402.97297297300003,14910]
["3215000000-N","GR ANCHOR  III","","",28,1448.214285714,40550]
["3270000000-N","GR ANCHOR  350","","",78,1934.871794872,150920]
["3285000000-N","GR ANCHOR  M-350","","",6,1741.6666666670001,10450]
["3317000000-N","GR ANCHOR  B-77","","",52,1304.807692308,67850]
["3345000000-E","REM & RESET GRDRL","","",65,20,1300]
["3360000000-E","REM EXT GRDRL","","",25007,1.0111968650000001,25287]
["3365000000-E","REM EXT GUIDERAIL","","",4850,1,4850]
["3380000000-E","TEMP STL BM GRDRL","","",6550,7,45850]
["3387000000-N","TEMP GDRL ANCH UNIT****","(B-77)","",6,850,5100]
["","","(CAT-1)","",3,300,900]
["","","(III)","",1,900,900]
["","","(W-BEAM)","",1,975,975]
["3389100000-N","TEMP GDRL ANCH UNITS 350","","",4,1000,4000]
["3389200000-E","CABLE GUIDERAIL","","",360,7.5,2700]
["3389400000-E","DBL FACE CBL GUIDERAIL","","",12670,7.25,91857.5]
["3389500000-N","ADDITL GUIDERAIL POSTS","","",40,38,1520]
["3389600000-N","CBL GUIDERAIL ANCH UNIT","","",21,1500,31500]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",23600,2.0499999999999998,48380]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1510,18,27180]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",400,22,8800]
["3533000000-E","CHN LK FENCE **\" FAB","(60\")","",4100,6.35,26035]
["","","(72\")","",340,10.75,3655]
["","","(96\")","",300,8.1,2430]
["3536000000-E","CHN LK FENCE 48\" FAB","","",6100,4.8499999999999996,29585]
["3539000000-E","MET LINE PST **\" CL FEN","(60\")","",360,37.5,13500]
["","","(72\")","",30,56,1680]
["","","(96\")","",30,45,1350]
["3542000000-E","MET LINE PST 48\" CL FEN","","",550,32,17600]
["3545000000-E","MET TERM PST **\" CL FEN","(60\")","",50,110,5500]
["","","(72\")","",3,130,390]
["","","(96\")","",4,130,520]
["3548000000-E","MET TERM PST 48\" CL FEN","","",40,85,3400]
["3554000000-E","MET GATE PST **\"CL FEN D","(60\")","",4,135,540]
["3557000000-E","ADDITIONAL BARBED WIRE","","",500,0.01,5]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 12')","",4,625,2500]
["3574000000-E","GENERIC FENC ITEM867(LF)","4' VINYL FENCE RESET","",100,25,2500]
["","","SPLIT RAIL FENCE RESET","",85,20,1700]
["3575000000-E","GENERIC FENCING ITEM (LF)","BLACK VINYL COATED CHAIN LINK","FENCE, 48\" FAB",350,12.65,4427.5]
["3578000000-N","GENERIC FENCING ITEM (EA)","DOUBLE CATTLE GATE (47\" HIGH,","10' WIDE, 20' OPENING)",1,1500,1500]
["","","DOUBLE CATTLE GATE (60\" HIGH,","10' WIDE, 20' OPENING)",2,1800,3600]
["3595000000-E","RELAPPING GRDRL","","",900,5,4500]
["3628000000-E","RIP RAP, CL I","","",15014,31.169908086,467985]
["3635000000-E","RIP RAP, CL II","","",5294,37.272383830999999,197320]
["3649000000-E","RIP RAP, CL B","","",672,42.215773810000002,28369]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",57870,1.5405736999999999,89153]
["3659000000-N","PREFORM SCOUR HOLES","","",16,891.72249999999997,14267.56]
["3804000000-E","ABC (SUB-BALLAST)","","",2600,0.01,26]
["3808000000-E","RR TRACK TO BE CONSTR","","",500,195,97500]
["3832000000-E","RR TRACK TO BE REMD","","",1790,10,17900]
["3848000000-E","RR DET TRACK CONST & REMV","","",1071,295,315945]
["4048000000-E","REINF CONC FOUNDTN","","",14,850,11900]
["4054000000-E","PLN CONC FOUNDTN","","",4,1,4]
["4057000000-E","OVERHEAD FOOTING","","",665,875,581875]
["4060000000-E","SUPPT, BRKAWAY STL BM","","",9483,3.25,30819.75]
["4066000000-E","SUPPTS, SIMPLE STL BM","","",4960,3.25,16120]
["4072000000-E","SUPPT, 3-LB STL U-CHAN","","",8103,5.9008071080000004,47814.239999999998]
["4078000000-E","SUPPT, 2-LB STL U-CHAN","","",26,35,910]
["4080000000-N","SUPPT, BARR LARGE","","",15,100,1500]
["4082100000-N","SUPPT, OVRHD SIGN STR *","(-DFEB- STA 1+40)","",1,54000,54000]
["","","(-DFEB- STA 20+50)","",1,66000,66000]
["","","(-DFEB- STA 36+00)","",1,95000,95000]
["","","(-DFEB- STA 59+00)","",1,24000,24000]
["","","(-DFLW- STA 45+70)","",1,82400,82400]
["","","(-DFLW- STA 59+00)","",1,34500,34500]
["","","(-DFLW- STA 69+00)","",1,72000,72000]
["","","(-DFWB- STA 26+85)","",1,22500,22500]
["","","(-DFWB- STA 38+05)","",1,32000,32000]
["","","(-L- STA 114+02)","",1,25300,25300]
["","","(-L- STA 124+15)","",1,71400,71400]
["","","(-L- STA 127+40)","",1,66500,66500]
["","","(-L- STA 136+85)","",1,68000,68000]
["","","(-L- STA 14+31)","",1,50000,50000]
["","","(-L- STA 142+20)","",1,67500,67500]
["","","(-L- STA 27+51)","",1,75000,75000]
["","","(-L- STA 28+93)","",1,23500,23500]
["","","(-L- STA 60+14)","",1,62500,62500]
["","","(-L- STA 62+33)","",1,30000,30000]
["","","(-L- STA 82+00)","",1,55000,55000]
["","","(-L- STA 84+58)","",1,77000,77000]
["","","(-L- STA 90+98)","",1,31500,31500]
["","","(-LDFEB- STA 188+92)","",1,29000,29000]
["","","(-Y1- STA 30+48)","",1,56000,56000]
["","","(-Y1- STA 35+42)","",1,85000,85000]
["","","(-Y2- STA 22+15)","",1,63000,63000]
["","","(-Y3- STA 41+34)","",1,110000,110000]
["","","(-Y3- STA 53+60)","",1,115000,115000]
["4096000000-N","SIGN ERECTION,  D","","",28,75.714285713999999,2120]
["4102000000-N","SIGN ERECTION,  E","","",390,49.012820513000001,19115]
["4108000000-N","SIGN ERECTION,  F","","",40,75,3000]
["4109000000-N","SIGN ERECTION,  *** (OVRHD)","(A)","",7,800,5600]
["","","(B)","",8,300,2400]
["4110000000-N","SIGN ERECTION,  *** (GRD MTD)","(A)","",19,375,7125]
["","","(B)","",1,200,200]
["4114000000-N","SIGN ERECTION, MILEMKRS","","",26,50,1300]
["4116000000-N","SIGN ERECTION, OVERLAY (GRD MTD)","","",6,350,2100]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",5,400,2000]
["","","(D)","",1,100,100]
["","","(E)","",11,67.727272726999999,745]
["","","(LOGO TRAILBLAZER)","",1,100,100]
["4138000000-N","DISP SUPPT, STL BM","","",10,250,2500]
["4143000000-N","DISP SUPPT, OVRHD ST","","",1,2000,2000]
["4149000000-N","DISP SIGN SYST OVRHD","","",3,2500,7500]
["4152000000-N","DISP SIGN SYST STL BM","","",10,250,2500]
["4155000000-N","DISP SIGN SYST U-CHAN","","",195,1,195]
["4192000000-N","DISP SUPPT, U-CHAN","","",10,1,10]
["4234000000-N","DISP SIGN,A OR B(OVRHD)","","",12,1,12]
["4251000000-N","DISP LIGHT SYSTEM","","",3,1,3]
["4263000000-N","DISP WALKWAY","","",3,1,3]
["4360000000-N","GENERIC SIGN ITEM (EA)","DMS ACCESS LADDER","",1,4100,4100]
["","","DMS PEDESTAL STR","",1,43000,43000]
["4370000000-N","GENERIC SIGNING ITEM(LS)","INSTALL DMS & EQUIP ","CBNT",1,11000,11000]
["","","REM EXT DMS","",1,3000,3000]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",8384,4.0858158400000004,34255.480000000003]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",3022,17.493845136000001,52866.400000000001]
["4410000000-E","WORK ZONE SIGN (BARR)","","",1735,4.8958213260000001,8494.25]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",21706,3.7123892010000001,80581.119999999995]
["4415000000-N","FLASHING ARROW BOARD","","",21,4611.9047619049998,96850]
["4420000000-N","PORT CHANGE MSG SIGN","","",15,9440,141600]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",194,56.231958763000002,10909]
["4430000000-N","DRUMS","","",1323,50.201058201000002,66416]
["4435000000-N","CONES","","",150,21.066666667,3160]
["4445000000-E","BARRICADES ( III)","","",1984,14.186290323,28145.599999999999]
["4450000000-N","FLAGGER","","",108,22.925925926000001,2476]
["4455000000-N","FLAGGER","","",580,117.068965517,67900]
["4457000000-N","TEMP TRAFFIC CNTRL","","",8,41144.553749999999,329156.43]
["4465000000-N","TEMP CRASH CUSHIONS","","",18,4534.4444444439996,81620]
["4470000000-N","RESET CRASH CUSHION","","",27,938.88888888899999,25350]
["4480000000-N","TMA","","",16,13306.25,212900]
["4485000000-E","PORT CONC BARR","","",39735,40.417138543,1605975]
["4490000000-E","PORT CONC BARR(ANCH)","","",1000,47.2,47200]
["4500000000-E","RESET PORT CONC BARR","","",51000,7.5,382500]
["4505000000-E","RESET PORT CONC BARR,ANCH","","",1000,5,5000]
["4507000000-E","WATER FILLED BARR","","",3080,45.161688312000003,139098]
["4510000000-N","LAW ENFORCEMENT","","",4770,44.514427673,212333.82]
["4516000000-N","SKINNY DRUM","","",345,29.891304347999998,10312.5]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",10,45,450]
["4575000000-E","MOVABLE CONC BARR","","",1750,63.94,111895]
["4580000000-E","RESET MOVBLE CONC BARR","","",1200,10,12000]
["4585000000-N","TRANSF & TRNPRT VEHICL","","",1,326000,326000]
["4650000000-N","TEMP RAISED PVT MRKS","","",5103,4,20412]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",1991176,0.41582629100000001,827983.33]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",1709737,0.55025706299999999,940794.86]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",107955,0.92,99318.6]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",19707,0.97836809300000005,19280.7]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",17379,2.1552016799999998,37455.25]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",18610,1.9677958090000001,36620.68]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",14115,2.9,40933.5]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",6445,2.9164856480000001,18796.75]
["4705000000-E","THERMO LINES 16\" 120MIL","","",300,5.5,1650]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",15250,8.2340996719999993,125570.02]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",442,81.198868778000005,35889.9]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",2238,91.659262734999999,205133.43]
["4770000000-E","4\" COLD APPL PLSTIC LINES  **","(II)","",3028,1.5799207399999999,4784]
["","","(III)","",5478,3.2037495439999999,17550.14]
["","","(IV)","",4022,1.65,6636.3]
["4775000000-E","6\" COLD APPL PLSTIC LINES  **","(II)","",10926,2.4962474829999999,27274]
["","","(IV)","",43956,2.65,116483.4]
["4785000000-E","12\" COLD PLSTIC LINES  **","(II)","",1135,5.5,6242.5]
["4800000000-N","COLD APP PLAS CHAR  *","(II)","",59,300,17700]
["4805000000-N","COLD APPL PLASTIC SYM*","(II)","",21,300,6300]
["","","(III)","",1,200,200]
["","","(IV)","",5,325,1625]
["4810000000-E","PAINT PVT MARKINGS 4\"","","",1835603,0.14700521799999999,269843.21999999997]
["4815000000-E","PAINT PVT MARKINGS 6\"","","",82258,0.35383062999999998,29105.4]
["4820000000-E","PAINT PVT MARKINGS 8\"","","",84056,0.43631233899999999,36674.67]
["4825000000-E","PAINT PVT MARKINGS 12\"","","",885,0.86271186399999999,763.5]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",250,2.0499999999999998,512.5]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",13633,3.0890060880000001,42112.42]
["4840000000-N","PAINT PVT MKG CHAR","","",234,27.307692308,6390]
["4845000000-N","PAINT PVT MKG SYMBOL","","",1956,24.071758690999999,47084.36]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",46381,1.8,83485.8]
["","","(STD GLASS BEADS)","",3690,5,18450]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",9845,3.6,35442]
["4850000000-E","LINE REML 4\" WIDE","","",90827,0.54250476199999997,49274.080000000002]
["4855000000-E","LINE REML 6\" WIDE","","",3704,0.814187365,3015.75]
["4860000000-E","LINE REML 8\" WIDE","","",2341,1.0739000430000001,2514]
["4870000000-E","LINE REML 24\" WIDE","","",733,2.7285129600000002,2000]
["4875000000-N","REML OF SYMBL & CHAR","","",58,32.068965517000002,1860]
["4900000000-N","PERM RAISED PVT MRKRS","","",9029,4.0196588770000004,36293.5]
["4905000000-N","SNOWPLB PVT MRKER","","",12539,27.383313660999999,343359.37]
["4915000000-E","7' U-CHANNEL POSTS","","",13,35,455]
["4955000000-N","OBJECT MKR (END OF RD)","","",13,35,455]
["5005000000-E","80' HIGH MOUNT STD","","",4,15290,61160]
["5010000000-E","100' HIGH MOUNT STD","","",9,18305,164745]
["5015000000-E","120' HIGH MOUNT STD","","",3,21230,63690]
["5020000000-N","PORTABLE DRIVE UNIT","","",1,5175,5175]
["5025000000-E","HIGH MOUNT FOUNDS","","",110,775,85250]
["5120000000-N","SERVICE POLE ************","(30FT, CL 4)","",3,770,2310]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",300,22.4,6720]
["5145000000-N","LITE CNTRL RW************","(240/480 VOLT)","",3,11110,33330]
["5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",1015,5.25,5328.75]
["","","(3\")","",285,5.6,1596]
["","","(4\")","",270,8,2160]
["5160000000-E","ELECT DUCT JA, SIZE *****","(3\")","",130,17.5,2275]
["","","(4\")","",445,17.5,7787.5]
["","","(6\")","",60,25,1500]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",1415,3.2,4528]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",930,3.8,3534]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2)","",745,5,3725]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(2)","",110,7.15,786.5]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2, 1.5)","",4765,6,28590]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",2200,6.9,15180]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",7220,8.1,58482]
["5220000000-E","**-2 W/G FEEDER N *****\"","(2, 1.5)","",635,10.1,6413.5]
["5240000000-N","ELEC JB ************","(PC18)","",32,515,16480]
["","","(PC30)","",6,845,5070]
["","","(PC36)","",5,925,4625]
["5252000000-N","UNDERPASS LUMINARIES *","( WM, 80W MAX LED)","",6,585,3510]
["5253000000-N","UNDERPASS CIRCUITRY***","(HOLLOWAY ST, UPL-1)","",1,3280,3280]
["","","(HOLLOWAY ST, UPL-2)","",1,3280,3280]
["5255000000-N","PORTABLE LIGHTING","","",2,19125.255000000001,38250.51]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","ELECTRICAL CONDUIT SYSTEM AT","ANGIER AVENUE, ECS-3",1,2735,2735]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","(100') HIGH MOUNT LUMINAIRE - LED","",72,1475,106200]
["","","(120') HIGH MOUNT ","LUMINAIRE - LED",24,1740,41760]
["","","(80') HIGH MOUNT ","LUMINAIRE - LED",24,1500,36000]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",23,600.11,13802.53]
["5325200000-E","2\" WATER LINE","","",225,50,11250]
["5325600000-E","6\" WATER LINE","","",1117,30,33510]
["5325800000-E","8\" WATER LINE","","",2249,42.441587372000001,95451.13]
["5326200000-E","12\" WATER LINE","","",3823,84.424190425999996,322753.68]
["5326600000-E","16\" WATER LINE","","",11,109.01,1199.1099999999999]
["5327000000-E","20\" WATER LINE","","",26,574,14924]
["5327400000-E","24\" WATER LINE","","",1120,250,280000]
["5328000000-E","30\" WATER LINE","","",656,211,138416]
["5540000000-E","6\" VALVE","","",1,969.63,969.63]
["5546000000-E","8\" VALVE","","",8,3738.34375,29906.75]
["5558000000-E","12\" VALVE","","",18,2747.2222222219998,49450]
["5558600000-E","16\" VALVE","","",1,7529.93,7529.93]
["5559000000-E","20\" VALVE","","",1,4000,4000]
["5559400000-E","24\" VALVE","","",2,10500,21000]
["5571600000-E","6\" TAPPING VALVE","","",1,3307.82,3307.82]
["5571800000-E","8\" TAPPING VALVE","","",1,3567.78,3567.78]
["5572200000-E","12\" TAPPING VALVE","","",2,8000,16000]
["5589200000-E","2\" AIR RELEASE VALVE","","",2,6130,12260]
["5606000000-E","2\" BLOW OFF","","",3,2964.48,8893.44]
["5648000000-N","RELOCATE WATER METER","","",44,1106.6463636359999,48692.44]
["5649000000-N","RECONNECT H2O METER","","",1,856.99,856.99]
["5666000000-E","FIRE HYDRANT","","",9,6102.2888888890002,54920.6]
["5672000000-N","RELOCATE FIRE HYDRANT","","",16,3124.375,49990]
["5679000000-E","12\" LINE STOP","","",2,12500,25000]
["5691200000-E","6\" SANITARY GRAVITY SEWER","","",186,100,18600]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",6501,70.77,460075.77]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",1562,65.8,102779.6]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",606,80,48480]
["5709300000-E","6\" FORCE MAIN SEWER","","",143,215,30745]
["5709400000-E","8\" FORCE MAIN SEWER","","",351,75,26325]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",2,1000,2000]
["5774000000-E","**' DIA UTILITY MH","(7')","",2,2500,5000]
["5775000000-E","4' DIA UTILITY MH","","",29,2160.0100000000002,62640.29]
["5776000000-E","5' DIA UTILITY MH","","",7,2662.9857142860001,18640.900000000001]
["5780000000-E","UTILITY MH WALL, **' DIA","(7')","",12.2,225,2745]
["5781000000-E","UTILITY MH WALL, 4' DIA","","",120,174.64,20956.8]
["5782000000-E","UTILITY MH WALL, 5' DIA","","",66,215.11,14197.26]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",134,8.25,1105.5]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",12633,5.8760429040000002,74232.05]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",5473,9.9471331989999996,54440.66]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",1169,12.62,14752.78]
["5812000000-E","ABANDON 20\" UTILITY PIPE","","",669,20,13380]
["5815000000-N","REM WATER METER","","",23,251.98,5795.54]
["5815500000-N","REM FIRE HYDRANT","","",11,694.59272727300004,7640.52]
["5816000000-N","ABANDON UTILITY MH","","",16,877.88,14046.08]
["5828000000-N","REM UTILITY MH","","",34,904.47176470600004,30752.04]
["5835000000-E","**\" ENCASEMENT PIPE","(42\")","",550,200,110000]
["","","(48\")","",508,300,152400]
["5835700000-E","16\" ENCASEMENT PIPE","","",1792,50,89600]
["5836000000-E","24\" ENCASEMENT PIPE","","",1621,70,113470]
["5836400000-E","36\" ENCASEMENT PIPE","","",310,160,49600]
["5871000000-E","**\" TRENCHLESS INSTALL (IN SOIL)","(42\")","",275,325,89375]
["","","(48\")","",87,250,21750]
["5871010000-E","**\" TRENCHLESS INSTALL (NOT IN SOIL)","(42\")","",275,725,199375]
["","","(48\")","",87,1150,100050]
["5871700000-E","12\" TRENCHLESS INSTALL (IN SOIL)","","",354,112,39648]
["5871710000-E","12\" TRENCHLESS INSTALL (NOT IN SOIL)","","",354,112,39648]
["5872200000-E","24\" TRENCHLESS INSTALL (IN SOIL)","","",212,110,23320]
["5872210000-E","24\" TRENCHLESS INSTALL (NOT IN SOIL)","","",211,980,206780]
["5872400000-E","36\" TRENCHLESS INSTALL (IN SOIL)","","",36,155,5580]
["5872410000-E","36\" TRENCHLESS INSTALL (NOT IN SOIL)","","",36,980,35280]
["5882000000-N","GENERIC UTILITY ITEM (EA)","12\" CHECK VALVE & MH","",1,19000,19000]
["","","ABANDON/REM SEWER ","LIFT STATION",1,25000,25000]
["6000000000-E","TEMP SILT FENCE","","",190965,1.7658844810000001,337222.13]
["6006000000-E","EROS CNTRL STONE CL A","","",4495,35.964404893999998,161660]
["6009000000-E","EROS CONTRL STONE CL B","","",31110,36.456444873000002,1134160]
["6012000000-E","SEDIMENT CNTRL STONE","","",52325,36.192928809999998,1893795]
["6015000000-E","TEMP MULCHING","","",533.5,444.04873477000001,236900]
["6018000000-E","SEED FOR TEMP SEEDING","","",11640,3.0768900339999998,35815]
["6021000000-E","FERT FOR TEMP SEEDING","","",60.25,870.33195020699998,52437.5]
["6024000000-E","TEMP SLOPE DRNS","","",31580,10.256554782,323902]
["6029000000-E","SAFETY FENCE","","",13000,1.5823076920000001,20570]
["6030000000-E","SILT EXCAV","","",114220,3.5379145510000001,404100.6]
["6036000000-E","MAT FOR EROS CNTRL","","",327590,1.192263195,390573.5]
["6037000000-E","COIR FIBER MAT","","",6350,4.5559055119999998,28930]
["6038000000-E","PERM SOIL REINF MAT","","",21960,5.3654599269999999,117825.5]
["6042000000-E","1/4\" HARDWARE CLOTH","","",45680,3.591889229,164077.5]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",500,83.76,41880]
["6048000000-E","FLOAT TURBIDITY CURTN","","",485,28.865979380999999,14000]
["6069000000-E","STILLING BASINS","","",700,15.11,10577]
["6070000000-N","SPECIAL STILLING BASINS","","",33,384.848484848,12700]
["6071010000-E","WATTLE","","",16835,7.3149985150000001,123148]
["6071012000-E","COIR FIBER WATTLE","","",31235,9.3448855450000003,291887.5]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",20680,10.911629594000001,225652.5]
["6071030000-E","COIR FIBER BAFFLE","","",15600,3.9899038459999998,62242.5]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",44,820.82,36116.080000000002]
["","","(2\")","",18,954.46,17180.28]
["","","(2-1/2\")","",4,1098.8699999999999,4395.4799999999996]
["","","(3\")","",2,1252.2,2504.4]
["","","(4\")","",1,1686.63,1686.63]
["","","(6\")","",1,1850,1850]
["6084000000-E","SEEDING & MULCHING","","",677.73,1830.256134449,1240419.49]
["6087000000-E","MOWING","","",267.45,57.599551318000003,15405]
["6090000000-E","SEED FOR REPAIR SEEDING","","",4000,8.5124999999999993,34050]
["6093000000-E","FERT FOR REPAIR SEEDING","","",14.25,1143.50877193,16295]
["6096000000-E","SEED FOR SUPP SEEDING","","",7425,2.4067340069999998,17870]
["6108000000-E","FERTILIZER TOPDRESSING","","",220,712.47727272700001,156745]
["6111000000-E","IMPERVIOUS DIKE","","",675,17.296296296000001,11675]
["6114500000-N","SPECIALIZED HAND MOW","","",305,48.163934425999997,14690]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",361,127.908587258,46175]
["6120000000-E","CLVT DIVERSION CHANL","","",1000,8.16,8160]
["6123000000-E","REFORESTATION","","",6.7,932.83582089599997,6250]
["6132000000-N","GENERIC EROSION CNTRL ITEM (EA)","FAB INSERT INLET PROTECTION","DEVICE CLEANOUT",120,54.508333333000003,6541]
["","","FAB INSERT INLET PROTECTIONDEVICE","",74,82.190540541000004,6082.1]
["6135000000-E","GENERIC EROSION CNTRL ITEM (ACR)","COMPOST BLANKET","",7,6000,42000]
["7000000000-E","PEDEST SIG HEAD (**************)","(16\", 1 SECT W/ COUNT-DOWN & PUSH BUTTON","INDICATOR LIGHT)",32,995,31840]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",10,970,9700]
["7060000000-E","SIGNAL CABLE","","",32630,2.3105271219999999,75392.5]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",141,682.83687943300004,96280]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",12,843.33333333300004,10120]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",11,1131.8181818180001,12450]
["7216000000-N","MOD EXT VEHIC SIGNL HD","","",2,220,440]
["7252000000-E","MESSENGER CABLE (1/4\")","","",10370,1.1499999999999999,11925.5]
["7264000000-E","MESSENGER CABLE (3/8\")","","",5920,3.0684966220000001,18165.5]
["7279000000-E","TRACER WIRE","","",13600,0.50882352900000005,6920]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",50,12.5,625]
["7300000000-E","UNPAVED TRENCH (*******)","(1, 2\")","",2095,6.3001193320000004,13198.75]
["","","(2, 2\")","",10185,6.25,63656.25]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",5375,2.7955813950000001,15026.25]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",2290,13.572052402000001,31080]
["","","(2, 2\")","",2720,13,35360]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",37,319.45945945900002,11820]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",84,481.42857142899999,40440]
["7360000000-N","WOOD POLE","","",33,805,26565]
["7372000000-N","GUY ASSEMBLY","","",82,315,25830]
["7396000000-E","1/2\" RISER W/ WEATHERHEAD","","",3,175,525]
["7408000000-E","1\" RISER W/ WEATHERHD","","",7,300,2100]
["7420000000-E","2\" RISER W/ WEATHERHD","","",36,400,14400]
["7432000000-E","2\" RISER W/ TUBING","","",17,393.23529411800001,6685]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",72403,5.2389845719999997,379318.2]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",55920,1.154184549,64542]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",11540,1.939514731,22382]
["","","(24)","",8020,1.95,15639]
["","","(72)","",13870,2.15,29820.5]
["7528000000-E","DROP CABLE","","",4600,1.25,5750]
["7540000000-N","SPLICE ENCLOSURE","","",12,1588.75,19065]
["7541000000-N","MOD SPLICE ENCLOSURE","","",1,970,970]
["7552000000-N","INTERCONNECT CENTER","","",11,1590,17490]
["7564100000-N","FIBER-OPTIC TRANS SELF HEAL","","",4,1990,7960]
["7566000000-N","DELINEATOR MARKER","","",50,66.2,3310]
["7575140000-N","FIBER-OPTIC SPLICE CBNT (BAS MTD)","","",2,2825,5650]
["7575142000-N","900MHZ RADIO","","",5,3200,16000]
["7575142200-N","NEW ELECTRICAL SERVICE","","",11,1410,15510]
["7575160000-E","REM EXT COMM CABLE","","",19210,1.1499999999999999,22091.5]
["7575180000-N","CABLE TRANSFER","","",7,95,665]
["7576000000-N","MTL STRAIN SIGNAL POLE","","",13,7895,102635]
["7588000000-N","SGNL MAST ARM W/ MTL POLE","","",2,13200,26400]
["7590000000-N","DBL MAST ARM W/ MTL POLE","","",4,18050,72200]
["7613000000-N","SOIL TEST","","",21,864.047619048,18145]
["7614100000-E","DRILLED PIER FOUND","","",174,971.37931034500002,169020]
["7630000000-N","MTL STRAIN POLE DESIGN","","",8,50,400]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",6,50,300]
["7636000000-N","SIGN FOR SIGNALS","","",57,527.89473684200004,30090]
["7642100000-N"," I POST W/ FOUND","","",2,885,1770]
["7642200000-N"," II PED W/ FOUND","","",22,1137.954545455,25035]
["7684000000-N","SIGNAL CABINET FOUND","","",11,997.27272727299999,10970]
["7744000000-N","DETECTOR CARD ( 170)","","",78,120,9360]
["7756000000-N","CONTLR W/ CBNT, 2070L BAS MTD","","",9,12405.555555556,111650]
["7780000000-N","DETECTOR CARD ( 2070L)","","",19,130,2470]
["7901000000-N","CABINET BAS EXTENDER","","",9,311.11111111100001,2800]
["7948000000-N","TRAFFIC SIGNAL REML","","",3,1240,3720]
["7960000000-N","MTL POLE FOUND REMVL","","",3,680,2040]
["7972000000-N","MTL POLE REML","","",3,220,660]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","CCTV CAMERA ASSEMB","",2,4930,9860]
["","","CCTV CAMERA LOWRING ","SYSTEM",1,7460,7460]
["","","CCTV EQUIPMENT REML","",2,1135,2270]
["","","CCTV MTL POLE 50'","",1,7780,7780]
["","","CCTV MTL POLE 70'","",1,17400,17400]
["","","CCTV MTL POLE REML","",2,915,1830]
["","","DROP CABLE ASSEMBLY","",1,1015,1015]
["","","EQUIPMENT CABINET ","DISCONNECT",2,630,1260]
["","","FIELD EQUIPMT CABINET","",4,4160,16640]
["","","FIELD VIDEO ENCODER","",2,2215,4430]
["","","MVD MTL POLE","",1,2025,2025]
["","","MVD POLE FOUND REML","",2,680,1360]
["","","MVD RELOCATED TO NEW ","CCTV MTL POLE",1,1385,1385]
["","","MVD RELOCATED TO NEW ","MTL MVD POLE",1,1385,1385]
["","","OPTICALLY ACTIVATED TRAFFIC","SIGNAL PRIORITY CNTRL SYSTEM",1,17200,17200]
["","","PORTABLE CCTV ","LOWERING TOOL",1,1645,1645]
["","","RECTANGULAR RAPID FLASHING","BEACON ASSEMBLY",4,5840,23360]
["8007000000-N","CM&R TEMP STR ***********","(34+62.88-DFEB- WID)","",1,739747.67,739747.67]
["8017000000-N","CM&R TEMP ACCESS ******","(14+83.00-L-)","",1,15000,15000]
["8021000000-N","REMV EXIST STR **********","(14+12.00-L-)","",1,50000,50000]
["","","(16+02.50-L-)","",1,70000,70000]
["","","(17+86.40-L-)","",1,60000,60000]
["","","(18+75.00-L-)","",1,25000,25000]
["","","(30+00 -Y7- RAMP C)","",1,58004.71,58004.71]
["8035000000-N","REMV EXIST STR **********","(14+83.00-L-)","",1,40000,40000]
["","","(24+70.18-DFWB- WID)","",1,31390.92,31390.92]
["","","(28+50.89-RRDET-)","",1,98508.06,98508.06]
["","","(34+62.88-DFEB- WID)","",1,15995.46,15995.46]
["","","(36+69.26-DFWB- WID)","",1,15995.46,15995.46]
["8042000000-N","REMV EXIST STRS *********","(44+08.60-L-)","",1,79050.3,79050.3]
["","","(64+74.69-L-)","",1,83839,83839]
["8049000000-N","REMV EXIST STR **********","(13+71.41-L-)","",1,85000,85000]
["8056000000-N","REMV EXIST STR **********","(28+17.07-L-)","",1,285000,285000]
["","","(34+45.00-Y3-)","",1,11000,11000]
["8084000000-N","FND EXCAV EB** STA*******","(ABUT 1, 64+55.50-L-)","",1,4870,4870]
["","","(ABUT 1, 64+74.69-L-)","",1,4870,4870]
["","","(ABUT 2, 64+55.50-L-)","",1,4870,4870]
["","","(ABUT 2, 64+74.69-L-)","",1,4870,4870]
["8091000000-N","FND EXCAV B** STA *******","(1, 105+29.00-L-)","",1,11859.38,11859.38]
["","","(1, 24+70.18-DFWB- WID)","",1,8522.52,8522.52]
["","","(1,138+40.45-LDFEB-)","",1,6989.38,6989.38]
["","","(1,23+29.61-DFFLY-)","",1,4743.75,4743.75]
["","","(17+97.57-DFLW-)","",1,6989.38,6989.38]
["","","(2, 105+29.00-L-)","",1,8522.52,8522.52]
["","","(2, 23+29.61-DFFLY-)","",1,4743.75,4743.75]
["","","(2, 24+70.18-DFWB-WID)","",1,11859.38,11859.38]
["","","(3, 105+29.00-L-)","",1,8522.52,8522.52]
["","","(3, 23+29.61-DFFLY-)","",1,4743.75,4743.75]
["","","(4, 23+29.61-DFFLY-)","",1,4743.75,4743.75]
["","","(5, 23+29.61-DFFLY-)","",1,4743.75,4743.75]
["8096000000-E","PILE EXCAV IN SOIL","","",238,256.08,60947.040000000001]
["8097000000-E","PILE EXCAV NOT IN SOIL","","",362,284.20999999999998,102884.02]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",36,836.43,30111.48]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",464.9,676.96782103700002,314722.34000000003]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",950.7,733.84000210399995,697661.69]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",50,796.58,39829]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",305,905.23016393399996,276095.2]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",704,952.48,670545.92000000004]
["8108000000-E","**'-**\" DIA DRILLD PIERS","(3'-0\")","",247,525,129675]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",39,252,9828]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",418.6,211.20656951699999,88411.07]
["8112730000-N","PDA TESTING","","",3,2628.12,7884.36]
["8113000000-N","SID INSPECTIONS","","",77,514.28571428600003,39600]
["8114000000-N","SPT TESTING","","",114,521.92982456100003,59500]
["8115000000-N","CSL TESTING","","",83,1022.8915662650001,84900]
["8121000000-N","UNCL STR EXCAV STA ****","(13+71.41-L-)","",1,99000,99000]
["","","(14+12.00-L-)","",1,30000,30000]
["","","(14+83.00-L-)","",1,5000,5000]
["","","(16+02.50-L-)","",1,30000,30000]
["","","(17+86.40-L-)","",1,15000,15000]
["","","(18+75.00-L)","",1,5000,5000]
["","","(24+70.18-DFWB- WID)","",1,4870,4870]
["","","(28+17.07-L-)","",1,25000,25000]
["","","(28+50.89-RRDET-)","",1,4870,4870]
["","","(44+08.60-L-)","",1,4870,4870]
["8126000000-N","CULV EXCAV @ ************","(133+41.46-L-)","",1,44500,44500]
["","","(19+07.28-Y4-)","",1,38500,38500]
["","","(34+45.00-Y3-)","",1,90000,90000]
["","","(95+48.49-L-)","",1,64000,64000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",1296,50,64800]
["8147000000-E","REINF CONC DECK SLAB","","",281247,22.960295647999999,6457514.2699999996]
["8156000000-E","CONC WEARING SURFACE","","",4385,14,61390]
["8161000000-E","GROOVING BRIDGE FLOORS","","",393289.2,0.42280581299999997,166284.96]
["8182000000-E","CL A CONC (BRIDGE)","","",5176.6000000000004,650.29059614400001,3366294.3]
["8196000000-E","CL A CONC (CULV)","","",2030.7,357.28098685200001,725530.5]
["8210000000-N","BRG APPR SLAB ***********","(10+00.00)","",1,30000,30000]
["","","(105+29.00-L-)","",1,31848.69,31848.69]
["","","(107+45.55-L-)","",1,42537.69,42537.69]
["","","(125+91.57-L-EBL)","",1,54954.55,54954.55]
["","","(125+91.57-L-WBL)","",1,54656.34,54656.34]
["","","(138+40.45-LDFEB-)","",1,32506.52,32506.52]
["","","(14+12.00-L-)","",1,15595,15595]
["","","(14+83.00-L-)","",1,25000,25000]
["","","(157+33.78-LDFEB-)","",1,177183.93,177183.93]
["","","(16+02.50-L-)","",1,20800,20800]
["","","(17+86.40-L-)","",1,25000,25000]
["","","(17+97.57-DFLW-)","",1,51151.91,51151.91]
["","","(18+75.00-L-)","",1,55000,55000]
["","","(23+29.61-DFFLY-)","",1,31737.599999999999,31737.599999999999]
["","","(24+70.18-DFWB- WID)","",1,39529.550000000003,39529.550000000003]
["","","(28+17.07-L-)","",1,87500,87500]
["","","(34+62.88-DFEB- WID)","",1,59318.03,59318.03]
["","","(36+69.26-DFWB- WID)","",1,65612.45,65612.45]
["","","(44+08.60-L-)","",1,98699.73,98699.73]
["","","(85+26.52-L-)","",1,26302.45,26302.45]
["8217000000-E","REINF STL (BRIDGE)","","",1416148,0.82053669500000004,1162001.3999999999]
["8224000000-E","EPOXY COAT REINF STL BRG","","",31943,0.97,30984.71]
["8226000000-E","EPOXY CTD SPIR REINF STL BRG","","",3915,1.98,7751.7]
["8238000000-E","SPIRAL COL REINF STL BRG","","",134110,1.491173291,199981.25]
["8245000000-E","REINF STL (CULVERT)","","",204497,1,204497]
["8265000000-E","54\" PRESTR CONC GIRDR","","",6426.13,213.79728701400001,1373889.16]
["8280000000-E","STRUCTURAL STL","","",7683965,1.707061393,13117000]
["8296000000-N","POLLUTION CNTRL","","",1,10000,10000]
["8364000000-E","HP12X53 PILES","","",12246,70.744224235999994,866333.77]
["8384000000-E","HP14X73 PILES","","",495,98.12,48569.4]
["8384200000-E","HP14X73 GALV PILES","","",1000,55,55000]
["8387000000-E","PP18X0.50 GALV STL PILE","","",1200,122.5,147000]
["8391000000-N","STL PILE POINTS","","",75,140.44319999999999,10533.24]
["8440000000-E","METHD A WATERPROOFNG","","",202,67.5,13635]
["8475000000-E","TWO BAR MTL RAIL","","",965.62,130.834986848,126336.88]
["8482000000-E","THREE BAR MTL RAIL","","",521,163,84923]
["8503000000-E","CONC BARR RAIL","","",7642.79,62.446559436999998,477265.94]
["8505000000-E","VERT CONC BARR RAIL","","",1149.78,82.436727026,94784.1]
["8510000000-E","CONC MEDIAN BARR","","",182.4,55,10032]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",196.67,111,21830.37]
["","","(1'-2\" X 3'-8 7/8\")","",130.25,145,18886.25]
["","","(1'-3 1/2\" X 3'-3 1/2\")","",327.69,90,29492.1]
["","","(2\" X 2'-11 3/4\")","",357.73,257,91936.61]
["8524000000-E","**\" CHAIN LINK FENCE","(72\")","",682.56,106.639401664,72787.789999999994]
["8531000000-E","4\" SLOPE PROTECTION","","",10180.1,36.879543423000001,375437.44]
["8559000000-E","SURFACE PREP, CL II","","",65,135,8775]
["8573000000-E","LATEX MOD CONC OVERLAY","","",482.3,750,361725]
["8580000000-E","PLACING LATEX MOD CNC","","",8680,35,303800]
["8608000000-E","RIP RAP II (2'-0\")","","",2303,42.363221883999998,97562.5]
["8622000000-E","GEOTEXTILE FOR DRNG","","",2563,2.2508778770000002,5769]
["8650000000-N","POT BEARINGS","","",1,225816.49,225816.49]
["8657000000-N","ELASTOMERIC BEARINGS","","",8,24154.3125,193234.5]
["8660000000-E","CONC REPAIRS","","",469.5,28.977614483,13604.99]
["8664000000-E","SHOTCRETE REPAIRS","","",698.23,350.26002892999998,244562.06]
["8678000000-E","EPOXY RESIN INJECTION","","",612.79999999999995,80.786259791000006,49505.82]
["8692000000-N","FOAM JOINT SEALS","","",4,58991.052499999998,235964.21]
["8706000000-N","EXPANSION JOINT SEALS","","",2,478441.73,956883.46]
["8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(28+17.07-L-)","",1,37500,37500]
["8741000000-N","STR DRN SYS ************","(28+50.89-RRDET-)","",1,64210.42,64210.42]
["","","(64+55.50-L-)","",1,64210.42,64210.42]
["","","(64+74.9-L-)","",1,64210.42,64210.42]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",3910,130.416879795,509930]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",840,172,144480]
["8801000000-E","MSE RETAIN WALL NO **","(1-A)","",5730,51.64,295897.2]
["","","(11)","",1710,51.74,88475.4]
["","","(12)","",2300,51.98,119554]
["","","(13)","",6700,54.51,365217]
["","","(14)","",7650,54.65,418072.5]
["","","(15)","",2800,51.73,144844]
["","","(16)","",7050,56.55,398677.5]
["","","(17)","",14700,51.55,757785]
["","","(2)","",5020,46.39,232877.8]
["","","(3)","",3740,56.56,211534.4]
["","","(4)","",11180,50.07,559782.6]
["","","(5)","",8710,47.25,411547.5]
["","","(6)","",3880,53.81,208782.8]
["","","(7)","",13650,50.74,692601]
["8802010000-E","SOIL NAIL RETAIN WALLS","","",6950,37.700000000000003,262015]
["8802014000-E","SOLDIER PILE RET WALL","","",5150,89.51,460976.5]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",3,500,1500]
["8802015110-N","SOIL NAIL PROOF TESTS","","",16,482.15,7714.4]
["8802030000-E","SEGMENTAL GRAVITY RETAIN WALLS","","",135,75,10125]
["8802040000-E","CIP GRAVITY RET WALLS","","",300,169,50700]
["8804000000-N","GENERIC CULVERT ITEM (LS)","PRECAST REINFORCED CONC","THREE-SIDED CULVERT",1,370000,370000]
["8847000000-E","GENERIC RET WALL ITEM (SF)","SOUND BARR WALL","",17895,21.4,382953]
["8860000000-N","GENERIC STR ITEM (LS)","ELECTRICAL CONDUIT SYSTEM AT","ROWENA AVE.",1,3190,3190]
["","","PAINTING EXT STRUCTURE","",1,5000,5000]
["","","PAINTING STRUCTURAL ","STL",1,5000,5000]
["","","PARTIAL REM OF EXT STR"," AT BRIDGE 193",1,70000,70000]
["","","ROCKER BEARING ","ASSEMBLIES",1,98471.38,98471.38]
["","","SELF-LUBRICATING EXPANSION","BEARING ASSEMBLIES",1,185215.48,185215.48]
["","","SOUND BARR WALL","(BRG MOUNTED)",1,29161,29161]
["","","STL BEARING ASSEMBLS","",1,174922,174922]
["","","STRUCTURAL STL,","APPROX. 1,042,750 LBS",1,2331834.92,2331834.92]
["","","","APPROX. 465,500 LBS",1,1036130.78,1036130.78]
["","","","APPROX. 714,223 LBS",1,1542939.28,1542939.28]
["","","","APPROX. 959,500 LBS",1,2173356.39,2173356.39]
["","","TEMP SOLDIER PILE RET WALL FOR RR ABUT","(ABUT 1, 25+69.00-RRDET)",1,81128.539999999994,81128.539999999994]
["","","","(ABUT 2, 25+69.00-RRDET)",1,71235.67,71235.67]
["","","TEMPORARY RAILROAD SHORING","(138+40.45-LDFEB-)",1,39220.339999999997,39220.339999999997]
["","","","(17+97.57-DFLW)",1,42118.85,42118.85]
["","","","(24+70.18-DFWB- WID)",1,96180.22,96180.22]
["","","TREATED LUMBER DECK","",1,137439.39000000001,137439.39000000001]
["","","UNDER STR WRK PLATFM","",1,12842.08,12842.08]
["","","VOLUMETRIC MIXER","",1,64210.42,64210.42]
["8867000000-E","GENERIC STR ITEM (LF)","3'-0\" DIA LFD DRILL PIERS","IN SOIL",239.6,582.28998330599995,139516.68]
["","","","NOT IN SOIL",384,582.29,223599.35999999999]
["","","3'-6\" DIA LFD DRILL PIERS","IN SOIL",333.2,626.58001200499996,208776.46]
["","","","NOT IN SOIL",140,626.58000000000004,87721.2]
["","","4'-6\" DIA LFD DRILL PIERS","IN SOIL",103.8,966.61001926799997,100334.12]
["","","","NOT IN SOIL",208,966.61,201054.88]
["","","CONC BARR RAIL W/ MOMENT SLAB","",4340,287.31,1246925.3999999999]
["","","CONC PARAPET","",1640.2,35.65,58473.13]
["","","MTL HANDRAIL (ALUMINUM)","",911,120,109320]
["","","TEMP STL CASING AS SHORING","(PIER 1, 25+69.00-RRDET-)",12,644.41999999999996,7733.04]
["","","","(PIER 2, 25+69.00-RRDET-)",12,644.41999999999996,7733.04]
["","","","(PIER 6, 25+69.00-RRDET-)",12,644.41999999999996,7733.04]
["","","","(PIER 7, 25+69.00-RRDET-)",12,644.41999999999996,7733.04]
["8881000000-E","GENERIC STR ITEM (CY)","CL A CONC (BRIDGE)","",6.8,2750,18700]
["","","CL AA CONC (AS MOD","BY RAILWAY)",943.5,849.93000529899996,801908.96]
["","","LATEX MODIFIED CONC","",111,276.10000000000002,30647.1]
["","","LATEX MODIFIED CONC - VERY","EARLY STRENGTH",252,276.10000000000002,69577.2]
["8882000000-E","GENERIC STR ITEM (CF)","CONC FOR DECK REPAIR","",281,10.220000000000001,2871.82]
["8889000000-E","GENERIC STR ITEM (LB)","EPOXY COATED REINFORCING STL(BRG)","",608,3,1824]
["","","STRL STL FOR GIRDER","REPAIR",42000,0.31,13020]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",1934.5,10.966347894,21214.400000000001]
["","","DAMPROOFING (RR STRS)","",4716,0.87,4102.92]
["","","EPOXY COATING","",3188,3,9564]
["","","EPOXY PROTECTIVE COATING","",4239,1,4239]
["","","JOINT REPAIR","",470,8.69,4084.3]
["","","WATERPROOF (RR STRS)","",15159,7.5,113692.5]
["8893000000-E","GENERIC STR ITEM (SY)","HYDRO-DEMOLITION","OF BRIDGE DECK",5756,28.3,162894.79999999999]
["","","HYDRO-DEMOLITION OF ","BRIDGE DECK",8680,38,329840]
["","","PLACING & FINISH LATEX","MODIFIED CONC",2263,7.44,16836.72]
["","","PLACING & FINISHING LMC","- VERY EARLY STRENGTH",4888,7.15,34949.199999999997]
["","","SCARIFYING BRG DECK","",14436,6.4122720979999999,92567.56]
["","","SHOTCRETE SLOPE ","PROTECTION",3850,15.91,61253.5]
["8897000000-N","GENERIC STR ITEM (EA)","ANCHOR BOLT REPLMT","",4,744.02,2976.08]
["","","BEARING REPLACEMENT","",9,632.35,5691.15]
["","","GIRDER JACKING","",26,2602.89,67675.14]

{"sheet":"Items - Div 6","index":8,"n_rows":721,"n_cols":7,"rows_kept":721,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 6"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",14,766961.92857142899,10737467]
["0000400000-N","CONST SURVEYING","","",11,178981.818181818,1968800]
["0000900000-N","GENERIC MISC ITEM (LS)","TEMP GUARD BUILDING","",1,35000,35000]
["","","TEMP SPRUNG STR AT","YADKIN RD DETOUR",1,75000,75000]
["0001000000-E","CLEARING & GRUBBING","","",183,32287.671232877001,5892500]
["0008000000-E","SUPP CLEAR & GRUBBING","","",11,4091.009090909,45001.1]
["0015000000-N","SEAL ABANDONED WELLS","","",11,1681.8181818180001,18500]
["0022000000-E","UNCLAS EXCAV","","",2333450,5.0383166560000001,11756660]
["0029000000-N","REINF BRG APPR **********","(15+66.00-L-)","",1,9450,9450]
["","","(17+68.00)","",1,9100,9100]
["","","(19+83.14 -Y3-)","",1,38000,38000]
["","","(26+16.00-L-)","",1,12100,12100]
["","","(279+43.22 -Y02- EBL)","",1,13000,13000]
["","","(279+48.87 -Y02- WBL)","",1,13000,13000]
["","","(41+90.04 -RP1B-)","",1,18000,18000]
["","","(45+07.87 -RP1C-)","",1,20650,20650]
["","","(49+52.23 -Y1-)","",1,48000,48000]
["","","(55+93.07 -RP1DB-)","",1,26000,26000]
["","","(67+16.50 -L-)","",1,15850,15850]
["","","(765+21.45 -L- RT)","",1,35000,35000]
["","","(765+33.36 -L- LT)","",1,29000,29000]
["","","(826+14.99 -L- LT)","",1,28000,28000]
["","","(826+15.02 -L- RT)","",1,28000,28000]
["","","(898+00.42 -L- RT)","",1,36000,36000]
["","","(898+39.37 -L- LT)","",1,36000,36000]
["","","(91+81.18 -COL1-)","",1,15000,15000]
["","","(91+87.85 -L- RT)","",1,15000,15000]
["","","(91+88.69 -L- LT)","",1,15000,15000]
["0030000000-N","BRG APP SUB REG TIER**","(15+08 -L-)","",1,5000,5000]
["0036000000-E","UNDERCUT EXCAV","","",103575,5.6450398259999996,584685]
["0043000000-N","GRADING","","",5,527326.80000000005,2636634]
["0050000000-E","SUPP CLEAR & GRUBBING","","",5,1,5]
["0057000000-E","UNDERCUT EXCAV","","",1100,9.8181818179999993,10800]
["0106000000-E","BORROW EXCAV","","",706310,2.7599821609999999,1949403]
["0134000000-E","DRNG DITCH EXCAV","","",59525,7.2204787899999996,429799]
["0141000000-E","BERM DITCH CONST","","",6130,6.2120717780000003,38080]
["0156000000-E","REML OF EXT ASPH PVT","","",128450,2.924951343,375710]
["0177000000-E","BRKING OF EXT ASPH PVT","","",7070,1.126237624,7962.5]
["0192000000-N","PROOF ROLLING","","",224,183.92857142899999,41200]
["0195000000-E","SELECT GRANULAR MAT'L","","",121800,2.7216748769999999,331500]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",106475,0.98723174499999999,105115.5]
["0199000000-E","TEMP SHORING","","",13791,23.290841853,321204]
["0223000000-E","ROCK PLATING","","",3100,50.538709677,156670]
["0225000000-E","REINF SOIL SLOPES","","",180,150,27000]
["0255000000-E","GENERIC GRAD ITEM (TON)","AGG SHDR BORROW","",12341,23.128595738000001,285430]
["","","HAULING & DISP OF 'PETROLEUM ","CONTAMINATED SOIL",120,110,13200]
["","","HAULING & DISP OF 'PETROLEUM ","CONTAMINATED SOIL",150,65.333333332999999,9800]
["","","HAULING & DISP OF 'PETROLEUM ","CONTAMINATED SOIL",1600,48,76800]
["0257000000-E","GENERIC GRAD ITEM (LF)","REM & REPLACE 2'-6\" ","CURB & GUTTER",200,50,10000]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",14270,26.394253678999998,376646]
["0320000000-E","FND CONDIT GEOTEXTILE","","",37985,2.3604975650000002,89663.5]
["0335000000-E","**\" DRNG PIPE","(30\")","",188,50,9400]
["0335200000-E","15\" DRNG PIPE","","",4028,22.285501490000001,89766]
["0335300000-E","18\" DRNG PIPE","","",1264,25.938449367,32786.199999999997]
["0335400000-E","24\" DRNG PIPE","","",708,32.389830508000003,22932]
["0335500000-E","30\" DRNG PIPE","","",216,47,10152]
["0335600000-E","36\" DRNG PIPE","","",108,63,6804]
["0335800000-E","48\" DRNG PIPE","","",40,100,4000]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",19,241.578947368,4590]
["","","(18\")","",3,175,525]
["","","(24\")","",12,275,3300]
["","","(30\")","",6,350,2100]
["","","(36\")","",2,500,1000]
["0342000000-E","**\" SIDE DRN PIPE","(30\")","",108,110,11880]
["","","(36\")","",260,120,31200]
["","","(42\")","",20,130,2600]
["0343000000-E","15\" SIDE DRN PIPE","","",1162,41.869191049999998,48652]
["0344000000-E","18\" SIDE DRN PIPE","","",1044,46.574329501999998,48623.6]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",15,400,6000]
["","","(18\")","",9,600,5400]
["","","(24\")","",1,800,800]
["","","(30\")","",2,900,1800]
["0354000000-E","***\" RC PIPE CULV *****","(48\", V)","",208,250,52000]
["","","(66\", V)","",228,350,79800]
["0360000000-E","12\" RC PIPE CULV III","","",100,45,4500]
["0366000000-E","15\" RC PIPE CULV III","","",12872,33.951709135999998,437026.4]
["0372000000-E","18\" RC PIPE CULV III","","",8140,40.835798525999998,332403.40000000002]
["0378000000-E","24\" RC PIPE CULV III","","",5444,44.004371784999996,239559.8]
["0384000000-E","30\" RC PIPE CULV III","","",3984,96.462751003999998,384307.6]
["0390000000-E","36\" RC PIPE CULV III","","",1956,127.09529652400001,248598.39999999999]
["0396000000-E","42\" RC PIPE CULV III","","",2584,87.626006192000006,226425.60000000001]
["0402000000-E","48\" RC PIPE CULV III","","",556,181.985611511,101184]
["0408000000-E","54\" RC PIPE CULV III","","",516,176.76589147300001,91211.199999999997]
["0414000000-E","60\" RC PIPE CULV III","","",108,206.383333333,22289.4]
["0420000000-E","66\" RC PIPE CULV III","","",480,276.875833333,132900.4]
["0426000000-E","72\" RC PIPE CULV III","","",260,400,104000]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",1456,300,436800]
["","","(54\")","",48,340,16320]
["","","(60\")","",580,380,220400]
["","","(66\")","",148,550,81400]
["","","(72\")","",176,600,105600]
["0448200000-E","15\" RCP CULV CL IV","","",27772,34.518471841999997,958647]
["0448300000-E","18\" RCP CULV CL IV","","",6408,40.438826466999998,259132]
["0448400000-E","24\" RCP CULV CL IV","","",7042,47.846464073,336934.8]
["0448500000-E","30\" RCP CULV CL IV","","",3060,136.53045751600001,417783.2]
["0448600000-E","36\" RCP CULV CL IV","","",3848,153.81091476099999,591864.4]
["0448700000-E","42\" RCP CULV CL IV","","",716,173.955586592,124552.2]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",124,40.954838709999997,5078.3999999999996]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",254,48.876377953000002,12414.6]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",132,71.143939394,9391]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",48,100,4800]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(30\", 0.500\")","",48,550,26400]
["","","(36\", 0.500\")","",56,600,33600]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(30\", 0.500\")","",48,1,48]
["","","(36\", 0.500\")","",56,1,56]
["0995000000-E","PIPE REML","","",7137,8.7514361780000005,62459]
["1000000000-E","6\" SLOPE PROTECTION","","",290,100,29000]
["1011000000-N","FINE GRADING","","",6,1000450.2,6002701.2000000002]
["1099500000-E","SHALLOW UNDERCUT","","",3100,6.548387097,20300]
["1099700000-E","CL IV SUBGRD STABIL","","",6300,24.666666667000001,155400]
["1110000000-E","STABILIZER AGG","","",500,15,7500]
["1111000000-E","CL IV AGG STABIL","","",100,19,1900]
["1121000000-E","AGG BASE COURSE","","",467441,17.237160412000001,8057355.5]
["1220000000-E","INCIDENTAL STONE BASE","","",6585,22.757479118999999,149858]
["1231000000-E","SHDR BORROW","","",80900,0.58133498100000003,47030]
["1245000000-E","SHDR RECONST","","",161.15,1646.2593856660001,265294.7]
["1275000000-E","PRIME COAT","","",6935,5.9113193940000004,40995]
["1297000000-E","MILL ASP PVT *****\" DTH","(1-1/2\")","",225087,1.471111837,331128.15000000002]
["","","(3\")","",118241,2.1277822409999998,251591.1]
["1308000000-E","MILLN ASPH PVT ***** - ****","(0\" TO 1-1/2\")","",68404,1.4384209990000001,98393.75]
["","","(0\" TO 2\")","",8213,2.1,17247.3]
["1330000000-E","INCIDENTAL MILLING","","",59717,4.7935453890000002,286256.15000000002]
["1489000000-E","ASP CNC BAS CRS B25.0B","","",85239,39.728463497,3386414.5]
["1491000000-E","ASP CNC BAS CRS B25.0C","","",147750,29.236040609,4319625]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",87618,36.550598051000001,3202490.3]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",193720,28.404139996000001,5502450]
["1519000000-E","ASP CNC SURF CRS S9.5B","","",155092,33.030683723000003,5122794.8]
["1523000000-E","ASP CNC SURF CRS S9.5C","","",199539,30.761551376,6138129.2000000002]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",64991,31.344624639999999,2037118.5]
["1525100000-E","ASP CONC SURF CRS SF9.5A LEVEL","","",58,97,5626]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",1191,44.3,52761.3]
["1527000000-E","ASP CONC SURF CRS SA-1","","",631,58.35,36818.85]
["1575000000-E","ASP FOR PLANT MIX","","",49319,621.37304892600002,30645497.399999999]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",1734,147.14183967700001,255143.95]
["1704000000-E","PATCHING EXIST PVT","","",2098,124.118207817,260400]
["1771000000-E","AST, MAT COAT,6M STONE","","",138642,1.73,239850.66]
["1840000000-E","MILLED RUMBLE STRIPS","","",375589,9.2417242999999996E-2,34710.9]
["1847000000-E","******\"PCC PVT THRU LNS","(12\")","",410,85,34850]
["1880000000-E","GENERIC PAV ITEM (TON)","AGG SHDR BORROW","",4701,21.6,101541.6]
["1881000000-E","GENERIC PAVING ITEM (LF)","SPEED MODULATOR","",65,55,3575]
["1891000000-E","GENERIC PAV ITEM (SY)","PVT INTERLAYER","",114591,5.3,607332.30000000005]
["2020000000-N","CNTROL OF ACCESS MKRS","","",37,150,5550]
["2022000000-E","SUBDRN EXCAV","","",7408.2,7.048095354,52213.7]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",20460,1.5039100679999999,30770]
["2033000000-E","SUBDRN FINE AGG","","",420.8,30.617870721999999,12884]
["2036000000-E","SUBDRN COARSE AGG","","",3440.5,38.581339921999998,132739.1]
["2044000000-E","6\" PERF SUBDRN PIPE","","",22960,7.7073170729999996,176960]
["2070000000-N","SUBDRN PIPE OUTLET","","",50,374.4,18720]
["2077000000-E","6\" OUTLET PIPE","","",300,21.16,6348]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",26,412.5,10725]
["2209000000-E","ENDWALLS","","",50.6,886.66007905100003,44865]
["2220000000-E","REINF ENDWALLS","","",35.9,1017.13091922,36515]
["2253000000-E","PIPE COLLARS","","",8.4540000000000006,891.55784244100005,7537.23]
["2264000000-E","PIPE PLUGS","","",4.5999999999999996,958.69565217399997,4410]
["2275000000-E","FLOWABLE FILL","","",76,200.98684210499999,15275]
["2286000000-N","MASNRY DRNG STRUCT","","",991,1194.0010090820001,1183255]
["2297000000-E","MASNRY DRNG STRUCT","","",116.17100000000001,1220.876380508,141830.43]
["2308000000-E","MASNRY DRNG STRUCT","","",545.4,232.83920058699999,126990.5]
["2352000000-N","FRM W/GRATE 840.**** STD","(840.16)","",30,600,18000]
["","","(840.20)","",7,600,4200]
["2354000000-N","FRM W/GRATE 840.22 STD","","",5,600,3000]
["2354200000-N","FRM W/GRATE 840.24 STD","","",2,500,1000]
["2355000000-N","FRM W/GRATE 840.29 STD","","",1,600,600]
["2364000000-N","FRM W/2GRTS 840.16 STD","","",115,483.82608695699997,55640]
["2364200000-N","FRM W/2GRTS 840.20 STD","","",41,597.56097561000001,24500]
["2365000000-N","FRM W/2GRTS 840.22 STD","","",138,592.02898550700002,81700]
["2366000000-N","FRM W/2GRTS 840.24 STD","","",30,469.66666666700002,14090]
["2367000000-N","FRM W/2GRTS 840.29 STD","","",46,474.67391304300003,21835]
["2374000000-N","FRM-GRT-HD 840.03 **","(E)","",69,540.37681159399995,37286]
["","","(F)","",244,556.67213114799995,135828]
["","","(G)","",238,552.46218487399995,131486]
["2396000000-N","FRM W/COVER STD 840.54","","",26,390.76923076899999,10160]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",7,1440,10080]
["2418000000-E","FRM W/GRTS, DRIVEWY DI","","",30,250,7500]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",44,496.59090909100001,21850]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",57,590.35087719299997,33650]
["2473000000-N","GENERIC DRNG ITEM (EA)","RIPRAP ENERGY DISSI-","PATOR BASIN",6,2850,17100]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",300,13.5,4050]
["","","(8\" X 18\")","",295,15.5,4572.5]
["","","(9\" X 12\")","",1390,12.25,17027.5]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",46830,10.583386718,495620]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",88070,14.083785625000001,1240359]
["2556000000-E","SHDR BERM GUTTER","","",15055,21.216712055999999,319417.59999999998]
["2570000000-N","MOD CONC FLUME","","",6,1466.6666666670001,8800]
["2577000000-E","CONC EXPRESSWAY GUTR","","",14840,16.025471698,237818]
["2580000000-E","CONC VALLEY GUTTER","","",325,30.124615384999998,9790.5]
["2591000000-E","4\" CONC SIDEWALK","","",20140,26.241062562,528495]
["2600000000-N","RETROFIT EXT CURB RAMP","","",44,485,21340]
["2605000000-N","CONC CURB RAMP","","",141,940.53191489400001,132615]
["2612000000-E","6\" CONC DRIVEWAY","","",2560,41.62109375,106550]
["2619000000-E","4\" CONC PAVED DITCH","","",250,51.42,12855]
["2627000000-E","4\" CONC ISLAND COVER","","",570,46,26220]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",5000,34.472000000000001,172360]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",8760,42.127397260000002,369036]
["2703000000-E","CONC BARRIER ******","(T1)","",270,120,32400]
["2724000000-E","PC REINF BARR SNGL FC","","",12810,63.085480093999998,808125]
["2738000000-E","GENERIC PAV ITEM (SY)","7\" CONC TRUCK APRON","",1200,30,36000]
["2752000000-E","GENERIC PAV ITEM (LF)","1'-6\" MOD CURB & GUTR","",4930,21,103530]
["","","6\" CONCRETE CURB","",1310,21,27510]
["","","SPECIAL SHDR BERM ","CURB",11,100,1100]
["2759000000-N","GENERIC PAVING ITEM (EA)","CONC BARR TRANSITION","",1,13000,13000]
["2800000000-N","ADJ CATCH BASINS","","",14,900,12600]
["2815000000-N","ADJ DROP INLETS","","",6,312.5,1875]
["2830000000-N","ADJ MHS","","",148,527.12837837799998,78015]
["2845000000-N","ADJ METER OR VAL BOX","","",91,521.75824175800005,47480]
["2875000000-N","CONVERT CB TO DI","","",5,1500,7500]
["2893000000-N","CONVERT CB TO JB W/MH","","",1,3000,3000]
["2910000000-N","CONVERT TRAF BR DI TO TRAF BR JB","","",2,1500,3000]
["2950000000-N","CONVERT JB TO DI","","",1,800,800]
["2965000000-N","CONVERT JB TO CB","","",1,850,850]
["3000000000-N","IMPACT ATTEN 350","","",39,14846.153846154,579000]
["3030000000-E","STL BM GRDRL","","",68675,14.588842519,1001888.76]
["3045000000-E","SBGR SHOP CURVED","","",417.5,17.251497006000001,7202.5]
["3105000000-N","SBGR TERM SECT","","",2,26,52]
["3150000000-N","ADDIT GRDRL POSTS","","",135,24.229629630000002,3271]
["3180000000-N","GR ANCHOR **********","(W-BEAM)","",5,500,2500]
["3195000000-N","GR ANCHOR AT-1","","",3,533.33333333300004,1600]
["3210000000-N","GR ANCHOR CAT-1","","",84,462.202380952,38825]
["3215000000-N","GR ANCHOR III","","",22,1435.454545455,31580]
["3270000000-N","GR ANCHOR 350","","",129,1740.4651162790001,224520]
["3285000000-N","GR ANCHOR M-350","","",41,1590.975609756,65230]
["3317000000-N","GR ANCHOR B-77","","",138,1442.934782609,199125]
["3360000000-E","REM EXISTING GRDRL","","",2035,1.2653562650000001,2575]
["3380000000-E","TEMP STL BM GRDRL","","",225,7,1575]
["3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",275,7,1925]
["3387000000-N","TEMP GDRL ANCH UNITS**","(B-77)","",2,1000,2000]
["","","(CAT-1)","",1,500,500]
["","","(W-BEAM)","",2,599.5,1199]
["3389100000-N","TEMP GDRL ANCH UNITS 350","","",1,1000,1000]
["3389200000-E","CABLE GUIDERAIL","","",25000,7,175000]
["3389400000-E","DBL FACE CBL GUIDERAIL","","",33956,7,237692]
["3389500000-N","ADDITIL GUIDERAIL POSTS","","",16,34.375,550]
["3389600000-N","CBL GUIDERAIL ANCH UNIT","","",66,1529.4604545449999,100944.39]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",31660,2.66721415,84444]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",2026,16.238647580999999,32899.5]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",450,28.2,12690]
["3533000000-E","CHN LK FENCE **\" FABRIC","(84\")","",110598,14,1548372]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",2130,4.3,9159]
["3539000000-E","MET LINE PST **\" CL FEN","(84\")","",3102,102,316404]
["3542000000-E","MET LINE PST 48\" CL FEN","","",178,33,5874]
["3545000000-E","MET TERM PST **\" CL FEN","(84\")","",204,200,40800]
["3548000000-E","MET TERM PST 48\" CL FEN","","",11,105,1155]
["3574000000-E","GENERIC FENC ITEM867(LF)","WOOD FENCE RESET","",350,12,4200]
["3628000000-E","RIP RAP, CL I","","",2120,51.452830188999997,109080]
["3649000000-E","RIP RAP, CL B","","",2689,40.775381183,109645]
["3651000000-E","BOULDERS","","",350,75,26250]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",24142,1.5651975810000001,37787]
["3659000000-N","PREFORMED SCOUR HOLE","","",9,2000,18000]
["4048000000-E","REINF CONC FOUNDTN","","",136,588.27205882400006,80005]
["4054000000-E","PLN CONC FOUNDTN","","",3,220,660]
["4057000000-E","OVERHEAD FOOTING","","",592,659.54391891900002,390450]
["4060000000-E","SUPPT, BRKAWAY STL BM","","",57140,3.182283864,181835.7]
["4066000000-E","SUPPTS, SIMPLE STL BM","","",29573,2.668591283,78918.25]
["4072000000-E","SUPPT, 3-LB STL U-CHAN","","",11845,5.5374242300000001,65590.789999999994]
["4078000000-E","SUPPT, 2-LB STL U-CHAN","","",38,40.368421052999999,1534]
["4082100000-N","SUPPT, OVRHD SIGN STR *","(10+00 -RP1D-)","",1,42275,42275]
["","","(101+80 -L-)","",1,25370,25370]
["","","(107+60 -L-)","",1,45750,45750]
["","","(12+04 -LP2D-)","",1,42250,42250]
["","","(12+40 -LPB-)","",1,68075,68075]
["","","(13+40 -Y2-)","",1,34700,34700]
["","","(131+30 -COL1-)","",1,64000,64000]
["","","(14+84 -Y12-)","",1,66300,66300]
["","","(16+50 -Y12-)","",1,64075,64075]
["","","(24+20 -RP1BD-)","",1,63500,63500]
["","","(29+20 -COL2-)","",1,40275,40275]
["","","(30+95 -Y1-)","",1,22350,22350]
["","","(32+00 -Y1-)","",1,30400,30400]
["","","(33+16 -COL2-)","",1,44025,44025]
["","","(33+40 -RP1BD-)","",1,26400,26400]
["","","(36+60 -L-)","",1,64000,64000]
["","","(37+90 -RP1BD-)","",1,26330,26330]
["","","(42+15 -RP1BD-)","",1,57775,57775]
["","","(46+50 -CDR-)","",1,54350,54350]
["","","(51+15 -CDR-)","",1,76100,76100]
["","","(63+00 -L-)","",1,64000,64000]
["","","(64+60 -L-)","",1,52500,52500]
["","","(7+00 -Y12-RPC)","",1,44700,44700]
["","","(81+10 -L-)","",1,25270,25270]
["","","(81+25 -COL1-)","",1,110000,110000]
["","","(89+20 -L-)","",1,25270,25270]
["","","(97+40 -L-)","",1,48450,48450]
["","","(976+60 -L-)","",1,47000,47000]
["4096000000-N","SIGN ERECTION, D","","",25,72.2,1805]
["4102000000-N","SIGN ERECTION, E","","",610,50.135245902000001,30582.5]
["4108000000-N","SIGN ERECTION, F","","",76,54.210526315999999,4120]
["4109000000-N","SIGN ERECTION, *** (OVRHD)","(A)","",28,562.5,15750]
["4110000000-N","SIGN ERECT,***(GRD MTD)","(A)","",88,284.65909090899999,25050]
["","","(B)","",31,131.935483871,4090]
["4114000000-N","SIGN ERECTION, MILEMKRS","","",38,26.473684210999998,1006]
["4115000000-N","SIGN ERECTION, OVERLAY (OVRHD)","","",13,142.30769230799999,1850]
["4116000000-N","SIGN ERECTION, OVERLAY (GRD MTD)","","",7,89.285714286000001,625]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",6,370,2220]
["","","(E)","",3,105,315]
["4116200000-N","SIGN ERECTION, REPOSIT OVRHD","","",1,500,500]
["4149000000-N","DISP SIGN SYST OVRHD","","",2,750,1500]
["4152000000-N","DISP SIGN SYST STL BM","","",10,300,3000]
["4155000000-N","DISP SIGN SYST U-CHAN","","",283,1.975265018,559]
["4158000000-N","DISP SIGN SYST WOOD","","",6,1.3333333329999999,8]
["4192000000-N","DISP SUPPT, U-CHAN","","",2,1,2]
["4234000000-N","DISP SIGN,A OR B(OVRHD)","","",4,486.25,1945]
["4236000000-N","DISP SIGN, A, B OR C (GRD MTD)","","",14,150,2100]
["4238000000-N","DISP SIGN, D, E, F","","",6,1,6]
["4370000000-N","GENERIC SIGN ITEM (LS)","DISP OF FLASHER SYST","",1,1500,1500]
["4399000000-N","TEMP TRAFFIC CONTROL","","",1,21500,21500]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",5805,6.6427924200000001,38561.410000000003]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",3257,12.232422475,39841]
["4410000000-E","WORK ZONE SIGNS(BARR)","","",1526,6.6716906949999997,10181]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",10489,3.9244274950000002,41163.32]
["4415000000-N","FLASHING ARROW BOARD","","",9,3455.5555555559999,31100]
["4420000000-N","PORT CHANGE MSG SIGN","","",19,6552.631578947,124500]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",140,33.285714286000001,4660]
["4430000000-N","DRUMS","","",3059,42.075253351000001,128708.2]
["4435000000-N","CONES","","",230,16.652173912999999,3830]
["4445000000-E","BARRICADES ( III)","","",3192,16.827192982,53712.4]
["4450000000-N","FLAGGER","","",900,34.222222221999999,30800]
["4455000000-N","FLAGGER","","",1698,221.23085983499999,375650]
["4457000000-N","TEMP TRAFFIC CONTROL","","",3,45095,135285]
["4465000000-N","TEMP CRASH CUSHIONS","","",10,4620,46200]
["4470000000-N","RESET CRASH CUSHION","","",6,1481.6666666670001,8890]
["4480000000-N","TMA","","",12,13150,157800]
["4485000000-E","PORT CONC BARRIER","","",7500,21.804466667,163533.5]
["4500000000-E","RESET PORT CONC BARR","","",2270,5.4140969160000001,12290]
["4507000000-E","WATER FILLED BARRIER","","",4000,50.625,202500]
["4508000000-E","RESET H2O FILLED BARR","","",1200,5,6000]
["4510000000-N","LAW ENFORCEMENT","","",1382,38.7170767,53507]
["4516000000-N","SKINNY DRUM","","",260,30,7800]
["4520000000-N","TUBULAR MRKERS (FIXED)","","",233,34.858369099000001,8122]
["4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","TEMP MEDIAN CROSSOVERS","",1,125000,125000]
["4650000000-N","TEMP RAISED PVT MRKS","","",2995,5.9600166940000001,17850.25]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",688107,0.497715413,342481.46]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",663528,0.61835331699999996,410294.74]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",440,6,2640]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",298145,0.79250884600000004,236282.55]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",67815,0.98916522900000003,67080.240000000005]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",30450,1.653612479,50352.5]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",6443,2.6416653729999999,17020.25]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",33138,1.9981667569999999,66215.25]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",3370,2.9287833829999999,9870]
["4705000000-E","THERMO LINES 16\" 120MIL","","",1245,6.8112449799999997,8480]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",10381,8.493594066,88172]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",566,62.065371024999997,35129]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",1623,118.34565619200001,192075]
["4770000000-E","4\" COLD APPL PLSTIC LINES **","(III)","",930,3,2790]
["","","(IV)","",3255,2.1616743469999999,7036.25]
["4780000000-E","8\" COLD APPL PLSTIC LINES **","(III)","",85,6,510]
["4805000000-N","COLD APPL PLASTIC SYM **","(III)","",1,325,325]
["4810000000-E","PAINT PVT MARKINGS 4\"","","",3108856,0.128898173,400725.86]
["4815000000-E","PAINT PVT MARKINGS 6\"","","",2300,0.4,920]
["4820000000-E","PAINT PVT MARKINGS 8\"","","",20440,0.75418542099999997,15415.55]
["4825000000-E","PAINT PVT MARKINGS 12\"","","",322,1.6583850929999999,534]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",445,4.3483146069999998,1935]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",8831,3.9505718490000001,34887.5]
["4840000000-N","PAINT PVT MKG CHAR","","",104,40.384615384999996,4200]
["4845000000-N","PAINT PVT MKG SYMBOL","","",977,37.021494371000003,36170]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",3319,3.6303103339999998,12049]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",39090,1.6968124840000001,66328.399999999994]
["4847110000-E","POLYUREA LINES (8\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",350,2.4,840]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",450,3.2,1440]
["4850000000-E","LINE REML 4\" WIDE","","",69100,0.64714833599999999,44717.95]
["4860000000-E","LINE REML 8\" WIDE","","",1910,1.2120418850000001,2315]
["4870000000-E","LINE REML 24\" WIDE","","",878,3.5523918000000001,3119]
["4875000000-N","REML OF SYMBL & CHAR","","",106,58.981132074999998,6252]
["4900000000-N","PERM RAISED PVT MKERS","","",13672,4.3766274139999997,59837.25]
["4905000000-N","SNOWPLB PVT MRKER","","",6926,28.854750216999999,199848]
["4935000000-N","FLEX DELINATR(CRYSTAL)","","",590,56.949152542,33600]
["4940000000-N","FLEX DELINATR (YELLOW)","","",236,69.788135593000007,16470]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",20,35,700]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",20,35,700]
["5005000000-E","80' HIGH MOUNT STD","","",7,14250,99750]
["5010000000-E","100' HIGH MOUNT STD","","",12,16000,192000]
["5015000000-E","120' HIGH MOUNT STD","","",34,20058.823529411999,682000]
["5020000000-N","PORTABLE DRIVE UNIT","","",2,3487.5,6975]
["5025000000-E","HIGH MOUNT FOUNDS","","",488,657.31557377000001,320770]
["5030000000-N","HM LUMINAIRE ************","(400W HPS)","",56,810,45360]
["","","(750W HPS)","",344,818.69767441900001,281632]
["5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",12,2475,29700]
["5070000000-N","STD FOUNDAT ***********","( R1)","",10,740,7400]
["","","( R2)","",2,815,1630]
["5080000000-N","LITE STD LUM ***********","( RDW, 250W HPS, MC3)","",12,565,6780]
["5120000000-N","SERVICE POLE ************","(30' CL 4)","",3,2300,6900]
["","","(30', CL 4)","",5,815,4075]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",575,27.608695652000002,15875]
["5145000000-N","LITE CNTRL RW************","(240/480 V)","",3,8650,25950]
["","","(240/480 VOLT)","",5,11000,55000]
["5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",477,4,1908]
["","","(3\")","",620,5,3100]
["","","(TS2)","",2185,5.6,12236]
["","","(TS3)","",775,5.9,4572.5]
["","","(TS4)","",135,8.8000000000000007,1188]
["5160000000-E","ELECT DUCT JA, SIZE *****","(2\")","",581,9.5,5519.5]
["","","(3\")","",239,11.75,2808.25]
["","","(4\")","",351,15.5,5440.5]
["","","(6\")","",301,16.5,4966.5]
["","","(TS3)","",795,14.5,11527.5]
["","","(TS4)","",1715,15,25725]
["","","(TS6)","",670,23,15410]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(-2)","",560,2.4500000000000002,1372]
["","","(2)","",751,3.25,2440.75]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(-2)","",1245,2.4,2988]
["","","(2)","",643,3.85,2475.5500000000002]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(-2)","",1015,3.3,3349.5]
["","","(2)","",1219,5.0999999999999996,6216.9]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(-2)","",1865,5.5,10257.5]
["","","(2)","",5302,7.4,39234.800000000003]
["5190000000-E","************ FEEDER CIR","(2 1 W/G)","",780,8.5,6630]
["","","(2-1 W/G)","",1086,9,9774]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2, 1.5)","",520,6.5,3380]
["","","(2, TS1.5)","",6029,5.9,35571.1]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",1490,6.25,9312.5]
["","","(2, TS1.5)","",3343,6.65,22230.95]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",5695,7.5,42712.5]
["","","(2, TS1.5)","",7848,7.7,60429.599999999999]
["5220000000-E","**-2 W/G FEEDER N *****\"","(2, 1.5)","",4880,9.5,46360]
["","","(2, TS1.5)","",20789,9.4,195416.6]
["5225000000-E","**-1 W/G FEEDER CIR ****","(2, 2)","",4395,12,52740]
["","","(2, TS2)","",4662,13,60606]
["5240000000-N","ELEC JB ************","(JB18)","",66,555,36630]
["","","(JB36)","",30,1440,43200]
["","","(PC18)","",42,200,8400]
["","","(PC30)","",9,350,3150]
["","","(PC36)","",3,315,945]
["5252000000-N","UNDERPASS LUMINARIES**","(100W HPS, PM)","",6,570,3420]
["5253000000-N","UNDERPASS CIRCUITRY ***","(RAMSEY ST, UPL-1)","",1,4000,4000]
["5255000000-N","PORTABLE LIGHTING","","",2,110225,220450]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",15.5,250,3875]
["5325000000-E","**\" WATER LINE","(3/4\")","",41,20,820]
["5325200000-E","2\" WATER LINE","","",1687,20.487018376000002,34561.599999999999]
["5325400000-E","4\" WATER LINE","","",408,50,20400]
["5325600000-E","6\" WATER LINE","","",4736,26.493443834000001,125472.95]
["5325800000-E","8\" WATER LINE","","",14127,33.544269130000004,473879.89]
["5326200000-E","12\" WATER LINE","","",31415,44.252751232999998,1390200.18]
["5326600000-E","16\" WATER LINE","","",5232,111.308042813,582363.68000000005]
["5328000000-E","30\" WATER LINE","","",1072,235,251920]
["5534000000-E","**\" VALVE","(3/4\")","",2,600,1200]
["5536000000-E","2\" VALVE","","",20,646.28800000000001,12925.76]
["5538000000-E","4\" VALVE","","",4,760,3040]
["5540000000-E","6\" VALVE","","",21,894.98571428599996,18794.7]
["5546000000-E","8\" VALVE","","",33,1328.7769696969999,43849.64]
["5558000000-E","12\" VALVE","","",59,2159.2576271190001,127396.2]
["5558600000-E","16\" VALVE","","",9,5955.1822222219998,53596.639999999999]
["5571600000-E","6\" TAPPING VALVE","","",1,3000,3000]
["5572600000-E","16\" TAPPING VALVE","","",3,12605.58,37816.74]
["5589200000-E","2\" AIR RELEASE VALVE","","",1,2500,2500]
["5606000000-E","2\" BLOW OFF","","",13,2155.9630769229998,28027.52]
["5643000000-E","**\" WATER METER","(5/8\")","",90,1020.17,91815.3]
["5643100000-E","3/4\" WATER METER","","",1,1385.45,1385.45]
["5648000000-N","RELOCATE WATER METER","","",76,1012.551842105,76953.94]
["5649000000-N","RECONNECT H2O METER","","",22,918.18181818200003,20200]
["5653810000-E","RELC 8\" DCV BACKFLOW PREVNT A","","",2,5000,10000]
["5656410000-E","RELC 4\" RPZ BACKFLOW PREVNT A","","",1,3600,3600]
["5656610000-E","RELC 6\" RPZ BACKFLOW PREVNT A","","",1,4200,4200]
["5666000000-E","FIRE HYDRANT","","",45,4290.0168888890003,193050.76]
["5672000000-N","RELOCATE FIRE HYDRANT","","",19,3047.2394736840001,57897.55]
["5684400000-E","6\" LINE STOP W/ BYPASS","","",1,6800,6800]
["5684600000-E","8\" LINE STOP W/ BYPASS","","",1,8500,8500]
["5691100000-E","4\" SANITARY GRAVITY SEWER","","",120,11.3,1356]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",7607,73.458932562000001,558802.1]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",517,93.4,48287.8]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",321,126.52,40612.92]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",42,2441.6292857140002,102548.43]
["5775000000-E","4' DIA UTILITY MH","","",39,2296.4143589740002,89560.16]
["5776000000-E","5' DIA UTILITY MH","","",1,9255.2000000000007,9255.2000000000007]
["5781000000-E","UTILITY MH WALL, 4' DIA","","",138.19999999999999,399.51331403799998,55212.74]
["5782000000-E","UTILITY MH WALL, 5' DIA","","",12.4,485.85,6024.54]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",1468,5,7340]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",5315,6.573249294,34936.82]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",6986,14.54035929,101578.95]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",5534,19.24145103,106482.19]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",1119,36,40284]
["5815000000-N","REM WATER METER","","",15,150,2250]
["5815500000-N","REM FIRE HYDRANT","","",2,1114,2228]
["5816000000-N","ABANDON UTILITY MH","","",18,524.09555555600002,9433.7199999999993]
["5828000000-N","REM UTILITY MH","","",7,1494,10458]
["5835000000-E","**\" ENCASEMENT PIPE","(18\")","",50,85,4250]
["5835400000-E","6\" ENCASEMENT PIPE","","",94,74.148936169999999,6970]
["5835700000-E","16\" ENCASEMENT PIPE","","",718,88.958440111000002,63872.160000000003]
["5836000000-E","24\" ENCASEMENT PIPE","","",142,111.53239436600001,15837.6]
["5836200000-E","30\" ENCASEMENT PIPE","","",442,219.30203619900001,96931.5]
["5871500000-E","8\" TRENCHLESS INSTALL (IN SOIL)","","",300,68,20400]
["5871700000-E","12\" TRENCHLESS INSTALL (IN SOIL)","","",244,208.95,50983.8]
["5871900000-E","16\" TRENCHLESS INSTALL (IN SOIL)","","",315,242.77063492100001,76472.75]
["5871910000-E","16\" TRENCHLESS INSTALL (NOT IN SOIL)","","",95,157.25,14938.75]
["5872200000-E","24\" TRENCHLESS INSTALL (IN SOIL)","","",46,168.41,7746.86]
["5872210000-E","24\" TRENCHLESS INSTALL (NOT IN SOIL)","","",46,168.41,7746.86]
["5882000000-N","GENERIC UTILITY ITEM (EA)","12\" ANTI-CAVITATION PRESSURE","REDUCING VALVE",2,28500,57000]
["","","12\" INSERT VALVE","",1,11000,11000]
["","","12\" NITRILE PIPE GASKET","",8,53.92,431.36]
["","","16\" NITRILE PIPE GASKET","",3,95.54,286.62]
["","","8\" INSERT VALVE","",1,7500,7500]
["","","8\" NITRILE PIPE GASKET","",16,50.42,806.72]
["","","ABAND H2O METER ","VAULT",3,1500,4500]
["","","RELOCATE 4\" WATER ","METER",1,7000,7000]
["","","STEEL H-PILE PIER","",7,6161.1,43127.7]
["5894000000-E","GENERIC UTILITY ITEM (CY)","EXCAVATABLE ","FLOWABLE FILL",40.5,200,8100]
["5912000000-N","GENERIC UTILITY ITEM (LS)","SUPPT 8\" WATER MAIN & ","36\" SEWER MAIN",1,10000,10000]
["6000000000-E","TEMP SILT FENCE","","",338505,2.2683121370000001,767835]
["6006000000-E","EROS CNTRL STONE CL A","","",8970,42.152173912999999,378105]
["6009000000-E","EROS CONTRL STONE CL B","","",23255,42.915760052000003,998006]
["6012000000-E","SEDIMENT CNTROL STONE","","",32320,35.065362004999997,1133312.5]
["6015000000-E","TEMP MULCHING","","",1103.25,866.55336505800005,956025]
["6018000000-E","SEED FOR TEMP SEEDING","","",31500,3.1191746029999998,98254]
["6021000000-E","FERT FOR TEMP SEEDING","","",144.75,1013.937823834,146767.5]
["6024000000-E","TEMP SLOPE DRNS","","",27155,11.704658441999999,317840]
["6029000000-E","SAFETY FENCE","","",18000,1.6033888890000001,28861]
["6030000000-E","SILT EXCAV","","",184700,1.5507958850000001,286432]
["6036000000-E","MAT FOR EROS CONTROL","","",745946,1.385503441,1033510.75]
["6037000000-E","COIR FIBER MAT","","",15730,4.5716783220000003,71912.5]
["6038000000-E","PERM SOIL REINF MAT","","",10630,5.1557855129999997,54806]
["6042000000-E","1/4\" HARDWARE CLOTH","","",51060,3.1804151979999999,162392]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",4270,4.3659718969999997,18642.7]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",275,115.545454545,31775]
["6048000000-E","FLOAT TURBIDITY CURTN","","",465,5,2325]
["6069000000-E","STILLING BASINS","","",260,10.384615385,2700]
["6070000000-N","SPECIAL STILLING BASINS","","",18,497.27777777799997,8951]
["6071010000-E","WATTLE","","",12899,6.1609427090000004,79470]
["6071012000-E","COIR FIBER WATTLE","","",20460,8.9006353859999994,182107]
["6071014000-E","COIR FIBER WATTLE BARR","","",820,18.190000000000001,14915.8]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",20996,5.7851971799999999,121466]
["6071030000-E","COIR FIBER BAFFLE","","",28965,6.0717555670000003,175868.4]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",69,928.985507246,64100]
["","","(2\")","",20,1196.25,23925]
["","","(2-1/2\")","",9,1225,11025]
["","","(3\")","",5,1400,7000]
["","","(4\")","",2,1500,3000]
["6084000000-E","SEEDING & MULCHING","","",795.75,1446.955702168,1151415]
["6087000000-E","MOWING","","",342.3,100.683610868,34464]
["6090000000-E","SEED FOR REPAIR SEEDING","","",11950,4.4000000000000004,52580]
["6093000000-E","FERT FOR REPAIR SEEDING","","",32.25,1016.705426357,32788.75]
["6096000000-E","SEED FOR SUPP SEEDING","","",17050,3.2901906159999998,56097.75]
["6102000000-E","SODDING","","",350,6.5,2275]
["6105000000-E","WATER","","",6,250,1500]
["6108000000-E","FERTILIZER TOPDRESSING","","",506.75,1008.9960532809999,511308.75]
["6111000000-E","IMPERVIOUS DIKE","","",310,35.806451613,11100]
["6114500000-N","SPECIALIZED HAND MOW","","",380,53.552631579,20350]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",875,256.45142857100001,224395]
["6120000000-E","CLVT DIVERSION CHANNEL","","",1000,9.7200000000000006,9720]
["6123000000-E","REFORESTATION","","",23,1086.956521739,25000]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",45,202.777777778,9125]
["","","","DEVICE CLEANOUT",129,82.209302326,10605]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",18,300,5400]
["6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","REML OF EROSION CONTROL DEVICES","",1,26500,26500]
["6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","COMPOST BLANKET","",30,6375,191250]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",24,765.25,18366]
["7060000000-E","SIGNAL CABLE","","",32339,2.537184205,82050]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",177,671.49717514099996,118855]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",9,847.22222222200003,7625]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",11,965,10615]
["7252000000-E","MESSENGER CABLE (1/4\")","","",1725,1.798405797,3102.25]
["7264000000-E","MESSENGER CABLE (3/8\")","","",9399,2.2351845940000001,21008.5]
["7279000000-E","TRACER WIRE","","",7050,0.50709219900000002,3575]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",160,8.5,1360]
["7300000000-E","UNPAVED TRENCH (*******)","(1, 2\")","",7946,4.9432104199999998,39278.75]
["","","(2, 2\")","",181,5.4292817680000001,982.7]
["","","(4, 2\")","",75,6.89,516.75]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",7415,4.2364801080000003,31413.5]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",7335,8.9563735510000004,65695]
["","","(2, 2\")","",983,12.062054934000001,11857]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",184,179.755434783,33075]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",34,328.23529411800001,11160]
["7360000000-N","WOOD POLE","","",21,780,16380]
["7372000000-N","GUY ASSEMBLY","","",37,279.86486486500002,10355]
["7408000000-E","1\" RISER W/ WEATHERHD","","",3,298.33333333299998,895]
["7420000000-E","2\" RISER W/ WEATHERHD","","",34,320.147058824,10885]
["7432000000-E","2\" RISER WITH TUBING","","",6,423.33333333299998,2540]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",76552,4.9687238740000002,380365.75]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",94745,1.108804686,105053.7]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",9000,1.5,13500]
["7528000000-E","DROP CABLE","","",750,1.75,1312.5]
["7540000000-N","SPLICE ENCLOSURE","","",8,1237.5,9900]
["7541000000-N","MOD SPLICE ENCLOSURE","","",2,935,1870]
["7552000000-N","INTERCONNECT CENTER","","",8,619.84375,4958.75]
["7564000000-N","FIBER-OPTIC TRANS DROP/REP","","",8,1948.75,15590]
["7566000000-N","DELINEATOR MARKER","","",14,88,1232]
["7575142000-N","900MHZ RADIO","","",4,3000,12000]
["7575160000-E","REM EXT COMM CABLE","","",2580,0.95348837200000003,2460]
["7575180000-N","CABLE TRANSFER","","",2,350,700]
["7576000000-N","MTL STRAIN SIGNAL POLE","","",42,6597.1428571429997,277080]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",1,10900,10900]
["7613000000-N","SOIL TEST","","",43,729.18604651199996,31355]
["7614100000-E","DRILLED PIER FOUND","","",318,631.320754717,200760]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",1,135,135]
["7636000000-N","SIGN FOR SIGNALS","","",15,216.66666666699999,3250]
["7642100000-N"," I POST W/ FOUND","","",8,850,6800]
["7642200000-N"," II PED W/ FOUND","","",18,1288.3333333329999,23190]
["7648000000-N","RELOCATE EXISTING SIGN","","",4,200,800]
["7684000000-N","SIGNAL CABINET FOUND","","",12,909.16666666699996,10910]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",13,10995.384615385001,142940]
["7780000000-N","DETECTOR CARD (2070L)","","",94,90.319148936000005,8490]
["7901000000-N","CABINET BASE EXTENDER","","",11,384.72727272700001,4232]
["7948000000-N","TRAFFIC SIGNAL REML","","",2,750,1500]
["7960000000-N","MTL POLE FOUND REMVL","","",9,630,5670]
["7972000000-N","METAL POLE REML","","",9,203,1827]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","BACK FILL JUNCT BOX","",5,450,2250]
["","","MICROWAVE VEHICLE DETECTION SYSTEM","",2,9450,18900]
["","","MICROWAVE VEHICLE DETECTOR-","SINGLE ZONE",2,1520,3040]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","BACK PULL FIBER OPTIC ","CABLE",1300,2.692307692,3500]
["","","2-WAY CONC DUCTBANK ","(ACP)",1760,47,82720]
["8017000000-N","CM&R TEMP ACCESS ******","(45+07.87 -RP1C-)","",1,600000,600000]
["","","(57+07.00 -RP1DB-)","",1,5000,5000]
["","","(826+15.00 -L- LT)","",1,700000,700000]
["","","(898+20.00 -L- LT)","",1,800000,800000]
["","","(94+24.58 -L- LT)","",1,900000,900000]
["8035000000-N","REMV EXIST STR **********","(15+08.00-L-)","",1,49000,49000]
["","","(15+66.00 -L-)","",1,33500,33500]
["","","(17+68.00 -L-)","",1,46482,46482]
["","","(26+16.00-L-)","",1,34100,34100]
["","","(67+16.50 -L-)","",1,41500,41500]
["8091000000-N","FND EXCAV B** STA *******","(1, 765+27.44 -L- LT)","",1,6600,6600]
["","","(1, 765+27.44 -L- RT)","",1,14000,14000]
["","","(1, 943+21.58 -L-)","",1,34000,34000]
["","","(1, 991+23.18 -L-)","",1,30000,30000]
["","","(1,42+10.23 -RP1B-)","",1,7200,7200]
["","","(1,57+07.00 -RP1DB-)","",1,75000,75000]
["","","(2,42+10.23 -RP1B-)","",1,7200,7200]
["","","(2,57+07.00 -RP1DB-)","",1,90000,90000]
["","","(3,57+07.00 -RP1DB-)","",1,60000,60000]
["","","(3,94+24.58 -L- LT)","",1,8600,8600]
["","","(3,94+24.58 -L- RT)","",1,8200,8200]
["","","(4,57+07.00 -RP1DB-)","",1,23000,23000]
["","","(4,94+24.58 -L- RT)","",1,8300,8300]
["","","(4,94+43.84 -COL1-)","",1,16200,16200]
["","","(5,57+07.00 -RP1DB-)","",1,15200,15200]
["","","(5,94+43.84 -COL1-)","",1,16200,16200]
["","","(6,57+07.00 -RP1DB-)","",1,130000,130000]
["","","(7,57+07.00 -RP1DB-)","",1,143000,143000]
["","","(8,57+07.00 -RP1DB-)","",1,143000,143000]
["","","(9,57+07.00 -RP1DB-)","",1,10000,10000]
["8112730000-N","PDA TESTING","","",49,2209.6938775509998,108275]
["8121000000-N","UNCL STR EXCAV STA ****","(15+08.00-L-)","",1,10000,10000]
["","","(15+66.00 -L-)","",1,2450,2450]
["","","(17+68.00 -L-)","",1,8200,8200]
["","","(26+16.00-L-)","",1,11550,11550]
["8126000000-N","CULV EXCAV @ ************","(58+98.00-L-)","",1,17000,17000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",85.71,60,5142.6000000000004]
["8147000000-E","REINF CONC DECK SLAB","","",471806,23.268841537,10978379.050000001]
["8156000000-E","CONC WEARING SURFACE","","",4261.2,8,34089.599999999999]
["8161000000-E","GROOVING BRG FLOORS","","",509425.2,0.28762546500000002,146523.66]
["8175000000-E","CL AA CONC (BRG)","","",28.9,900,26010]
["8182000000-E","CL A CONC (BRG)","","",8506.2000000000007,895.60323881399995,7618180.2699999996]
["8196000000-E","CL A CONC (CULV)","","",123,700,86100]
["8210000000-N","BRG APPR SLAB ***********","(15+08.00-L-)","",1,17400,17400]
["","","(15+66.00 -L-)","",1,17500,17500]
["","","(17+68.00 -L-)","",1,18000,18000]
["","","(21+01.60 -PXROAD-)","",1,45000,45000]
["","","(26+16.00-L-)","",1,20075,20075]
["","","(42+10.23 -RP1B-)","",1,32000,32000]
["","","(45+07.87 -RP1C-)","",1,32000,32000]
["","","(46+73.19 -L- LT)","",1,44875,44875]
["","","(46+73.19 -L- RT)","",1,44875,44875]
["","","(57+07.00 -RP1DB-)","",1,36000,36000]
["","","(67+16.50 -L-)","",1,47200,47200]
["","","(765+27.44 -L- LT)","",1,44000,44000]
["","","(765+27.44 -L- RT)","",1,44000,44000]
["","","(826+15.00 -L- LT)","",1,42000,42000]
["","","(826+15.00 -L- RT)","",1,42000,42000]
["","","(898+20.00 -L- LT)","",1,42000,42000]
["","","(898+20.00 -L- RT)","",1,42000,42000]
["","","(94+24.58 -L- LT)","",1,39000,39000]
["","","(94+24.58 -L- RT)","",1,38000,38000]
["","","(94+43.84 -COL1-)","",1,42000,42000]
["","","(943+21.58 -L-)","",1,86000,86000]
["","","(969+51.52 -L- LT)","",1,42000,42000]
["","","(969+51.52 -L- RT)","",1,58000,58000]
["","","(991+23.18 -L-)","",1,78000,78000]
["8217000000-E","REINF STEEL (BRG)","","",1549752,1.0030274969999999,1554443.87]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",1055,1.1499999999999999,1213.25]
["8238000000-E","SPIRL COL REINF STL BRG","","",32038,2.5,80095]
["8245000000-E","REINF STEEL (CULVERT)","","",16017,1,16017]
["8259000000-E","36\" PRESTR CONC GIRDR","","",604.5,164.69000827100001,99555.11]
["8262000000-E","45\" PRESTR CONC GIRDR","","",552.22,150,82833]
["8265000000-E","54\" PRESTR CONC GIRDR","","",2038,200,407600]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",18229.64,230,4192817.2]
["8280000000-E","STRUCTURAL STEEL","","",10900100,1.2854249470000001,14011260.460000001]
["8364000000-E","HP12X53 PILES","","",32590,34.433887695999999,1122200.3999999999]
["8384000000-E","HP14X73 PILES","","",32050,42,1346100]
["8384200000-E","HP14X73 GALV PILES","","",16800,55.340261904999998,929716.4]
["8385200000-E","PP**X**** GALV STL PILE","(24 X 0.625)","",20790,140,2910600]
["8391000000-N","STEEL PILE POINTS","","",17,151.76470588199999,2580]
["8392500000-E","PREDRILLING FOR PILES","","",342,55,18810]
["8393000000-N","PILE REDRIVES","","",678,403.95280236000002,273880]
["8482000000-E","THREE BAR METAL RAIL","","",1076.55,200,215310]
["8503000000-E","CONC BARRIER RAIL","","",19539.02,51.502608113999997,1006310.49]
["8505000000-E","VERT CONC BARRIER RAIL","","",966.25,84.728910737000007,81869.31]
["8531000000-E","4\" SLOPE PROTECTION","","",5469.8,70.271490731,384371]
["8559000000-E","SURFACE PREP, CL II","","",22.4,150,3360]
["8573000000-E","LATEX MOD CNC OVERLY","","",166.7,600,100020]
["8580000000-E","PLACING LATEX MOD CNC","","",4002,45,180090]
["8594000000-E","RIP RAP B","","",703,41.573598861999997,29226.240000000002]
["8608000000-E","RIP RAP II (2'-0\")","","",6042,47.452697782000001,286709.2]
["8622000000-E","GEOTEXTILE FOR DRNG","","",6715,1.758190618,11806.25]
["8650000000-N","POT BEARINGS","","",1,220000,220000]
["8654000000-N","DISC BEARINGS","","",1,320000,320000]
["8657000000-N","ELASTOMERIC BEARINGS","","",6,139725,838350]
["8692000000-N","FOAM JOINT SEALS","","",2,65375,130750]
["8706000000-N","EXPANSION JOINT SEALS","","",1,1200000,1200000]
["8713000000-N","MOD EXP JOINT SEALS","","",1,80000,80000]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",1683,250,420750]
["8755000000-E","3'-0\"X 1'-6\"PRESTR SLABS","","",963.88,119.78000373499999,115453.55]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",3900,128.01658974399999,499264.7]
["8801000000-E","MSE RETAIN WALL NO **","(2)","",14700,65,955500]
["","","(3)","",6550,65,425750]
["","","(4)","",7000,65,455000]
["","","(6)","",2550,65,165750]
["","","(7)","",2250,65,146250]
["8802014000-E","SOLDIER PILE RETAINING WALLS","","",7900,65,513500]
["8847000000-E","GENERIC RET WALL ITEM (SF)","SOUND BARRIER WALL","",177990,25,4449750]
["","","VISUAL BARRIER WALL","",79031.27,25.55762738,2019851.75]
["8860000000-N","GENERIC STR ITEM (LS)","APPROX 980,100 LBS ","STRL STEEL",1,1700000,1700000]
["","","POST TENSIONING ","TENDONS",1,130000,130000]
["8881000000-E","GENERIC STR ITEM (CY)","6,000 PSI CONCRETE","",218.7,1250,273375]
["","","LATEX MOD CONC OVERLAY","- VERY EARLY STRENGTH",166.7,800,133360]
["","","POST TENSIONING ","ENCASEMENT",17.399999999999999,1600,27840]
["8892000000-E","GENERIC STR ITEM (SF)","BRG JOINT DEMOLITION","",688.8,10,6888]
["","","CONCRETE STAINING","",2649,7.98,21139.02]
["","","PAINTING OF STRL STEEL","",2879,5.82,16755.78]
["8893000000-E","GENERIC STR ITEM (SY)","HYDRO-DEMO OF BRG ","DECK",8004,25,200100]
["","","PLACING & FINISH OF LATEX MOD CONC","OVERLAY-VERY EARLY STRNGTH",4002,45,180090]
["","","SCARIFYING BRG DECK","",8004,15,120060]

{"sheet":"Items - Div 7","index":9,"n_rows":637,"n_cols":7,"rows_kept":637,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 7"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",9,758388.88888888899,6825500]
["0000400000-N","CONST SURVEYING","","",4,170926,683704]
["0000900000-N","GENERIC MISC ITEM (LS)","CONST TAXIWAY BRIDGE","",1,12750000,12750000]
["","","DESIGN & CONST","I-5110",1,48355000,48355000]
["","","","R-2413A & R-2413B",1,115445000,115445000]
["0001000000-E","CLEARING & GRUBBING","","",186,10483.870967741999,1950000]
["0008000000-E","SUPP CLEAR & GRUBBING","","",7.25,5913.9310344830001,42876]
["0015000000-N","SEAL ABANDONED WELL","","",12,2275,27300]
["0022000000-E","UNCLAS EXCAV","","",1366500,6.2450493959999998,8533860]
["0029000000-N","REINF BRG APPR **********","(129+37.56 -L- LT)","",1,22000,22000]
["","","(129+37.56 -L- RT)","",1,28000,28000]
["","","(14+99.25 -L- LT)","",1,16500,16500]
["","","(144+60.63 -L- RT)","",1,26000,26000]
["","","(144+90.00 -L- LT)","",1,26000,26000]
["","","(21+69.08-Y11- CL)","",1,24000,24000]
["","","(24+56.70 -Y4- CL)","",1,29000,29000]
["","","(26+17.64 -Y22- LT)","",1,27000,27000]
["","","(26+17.64 -Y22- RT)","",1,23000,23000]
["","","(26+21.65 -L- LT)","",1,30000,30000]
["","","(26+21.65 -L- RT)","",1,1100,1100]
["","","(40+48.97-Y-)","",1,59000,59000]
["0030000000-N","BRG APP SUB REG TIER**","(16+64.29 -L-)","",1,4275,4275]
["","","(16+88.00 -L-)","",1,7000,7000]
["0036000000-E","UNDERCUT EXCAV","","",25750,13.108737864,337550]
["0043000000-N","GRADING","","",2,60125,120250]
["0050000000-E","SUPP CLEAR & GRUBBING","","",3,1533.6666666670001,4601]
["0057000000-E","UNDERCUT EXCAV","","",1650,10.484848485000001,17300]
["0063000000-N","GRADING","","",2,654997,1309994]
["0106000000-E","BORROW EXCAV","","",2983100,5.878012805,17534700]
["0127000000-N","EMBM'T SETTLMT GAUGE","","",2,550,1100]
["0134000000-E","DRNG DITCH EXCAV","","",33860,4.9207028939999997,166615]
["0141000000-E","BERM DITCH CONST","","",2570,4.2,10794]
["0156000000-E","REML OF EXT ASPH PVT","","",56910,3.7975751190000002,216120]
["0163000000-E","REML OF EXT CONC PVT","","",12350,7,86450]
["0177000000-E","BRKING OF EXT ASP PVT","","",5300,2.5,13250]
["0185000000-E","BRKING OF EXT CNC PVT","","",600,2.5,1500]
["0192000000-N","PROOF ROLLING","","",70,115.714285714,8100]
["0195000000-E","SEL GRANULAR MAT'L","","",25350,12.830374752999999,325250]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",52850,1.263859981,66795]
["0199000000-E","TEMP SHORING","","",8445.25,15,126678.75]
["0220000000-E","ROCK EMBANKMENTS","","",280,19,5320]
["0222000000-E","GEOTEXTILE ROCK EMBANK","","",160,1.8,288]
["0223000000-E","ROCK PLATING","","",230,32,7360]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISP OF 'PETROLEUM ","CONTAMINATED SOIL",175,62,10850]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",7154,29.391668996,210268]
["0320000000-E","FND CONDIT GEOTEXTILE","","",23281,1.351690219,31468.7]
["0335200000-E","15\" DRNG PIPE","","",280,32,8960]
["0335300000-E","18\" DRNG PIPE","","",332,33,10956]
["0335400000-E","24\" DRNG PIPE","","",140,42,5880]
["0335500000-E","30\" DRNG PIPE","","",52,63,3276]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",6,495,2970]
["","","(24\")","",2,950,1900]
["0342000000-E","**\" SIDE DRN PIPE","(30\")","",520,61.038461538,31740]
["","","(36\")","",332,70.349397589999995,23356]
["","","(42\")","",196,97.448979592000001,19100]
["0343000000-E","15\" SIDE DRN PIPE","","",15056,39.459883103000003,594108]
["0344000000-E","18\" SIDE DRN PIPE","","",2684,40.327868852000002,108240]
["0345000000-E","24\" SIDE DRN PIPE","","",4068,45.914454276999997,186780]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",133,203.15789473699999,27020]
["","","(18\")","",6,210,1260]
["","","(24\")","",4,265,1060]
["0354000000-E","***\" RC PIPE CULV *****","(18\", V)","",200,50,10000]
["","","(30\", V)","",576,78.368055556000002,45140]
["","","(42\", V)","",216,148,31968]
["","","(48\", V)","",272,125,34000]
["","","(60\", V)","",320,240,76800]
["","","(66\", V)","",652,270,176040]
["0360000000-E","12\" RC PIPE CULV III","","",76,42,3192]
["0366000000-E","15\" RC PIPE CULV III","","",3716,37.24219591,138392]
["0372000000-E","18\" RC PIPE CULV III","","",3572,41.910694288999998,149705]
["0378000000-E","24\" RC PIPE CULV III","","",2252,53.527317940000003,120543.52]
["0384000000-E","30\" RC PIPE CULV III","","",404,73.39009901,29649.599999999999]
["0390000000-E","36\" RC PIPE CULV III","","",712,75,53400]
["0396000000-E","42\" RC PIPE CULV III","","",196,90,17640]
["0402000000-E","48\" RC PIPE CULV III","","",220,110,24200]
["0408000000-E","54\" RC PIPE CULV III","","",232,155,35960]
["0414000000-E","60\" RC PIPE CULV III","","",80,203,16240]
["0420000000-E","66\" RC PIPE CULV III","","",388,290,112520]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",136,110,14960]
["","","(60\")","",260,250,65000]
["0448200000-E","15\" RCP CULV CL IV","","",9792,39.064133986999998,382516]
["0448300000-E","18\" RCP CULV CL IV","","",2468,41.119935169999998,101484]
["0448400000-E","24\" RCP CULV CL IV","","",1548,61.744186046999999,95580]
["0448500000-E","30\" RCP CULV CL IV","","",484,66,31944]
["0448600000-E","36\" RCP CULV CL IV","","",308,76.610389609999999,23596]
["0448700000-E","42\" RCP CULV CL IV","","",664,107.62650602399999,71464]
["0570000000-E","6\" CS PIPE 0.064\"SPR BOX","","",8,80,640]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",212,28.773584906,6100]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",6,248.33333333300001,1490]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(18\", 0.250\")","",130,430,55900]
["","","(24\", 0.250\")","",124,610,75640]
["","","(54\", 0.750\")","",88,714,62832]
["","","(60\", 0.875\")","",80,714,57120]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(18\", 0.250\")","",50,725,36250]
["","","(24\", 0.250\")","",124,710,88040]
["","","(54\", 0.750\")","",88,775,68200]
["","","(60:, 0.875\")","",80,775,62000]
["0995000000-E","PIPE REML","","",8352,16.692169539999998,139413]
["0996000000-N","PIPE CLEAN-OUT","","",1,2000,2000]
["1000000000-E","6\" SLOPE PROTECTION","","",140,300,42000]
["1011000000-N","FINE GRADING","","",2,785295,1570590]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",111600,2.4500000000000002,273420]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",1120,200,224000]
["1077000000-E","57 STONE","","",781,20.358514724999999,15900]
["1099500000-E","SHALLOW UNDERCUT","","",1300,7,9100]
["1099700000-E","CL IV SUBGRD STABILIZ","","",2600,16,41600]
["1110000000-E","STABILIZER AGG","","",1000,20.5,20500]
["1115000000-E","GEOTEXTILE FOR PVT STABILIZ","","",136341,2.2760460899999999,310318.40000000002]
["1121000000-E","AGG BAS COURSE","","",95187,20.020801160000001,1905720]
["1176000000-E","SOIL CEMENT BAS","","",111600,2.2999999999999998,256680]
["1187000000-E","PC FOR SOIL CEMT BAS","","",3070,132,405240]
["1209000000-E","ASPH CURING SEAL","","",33480,2.9,97092]
["1220000000-E","INCIDENTAL STONE BAS","","",18845,23.279331387999999,438699]
["1275000000-E","PRIME COAT","","",24082,2.5617473629999998,61692]
["1297000000-E","MILL ASP PVT *****\" DTH","(1-1/2\")","",75639,1.4114631339999999,106761.66]
["","","(1-1/4\")","",40084,1.5358272630000001,61562.1]
["1308000000-E","MILLN ASPH PVT ***** - ***","(0\" TO 1\")","",1626,1.95,3170.7]
["","","(0\" TO 1-1/2\")","",3749,2.0988236859999998,7868.49]
["","","(0\" TO 1-1/4\")","",2940,1.75,5145]
["","","(1-1/2\" TO 3\")","",30814,1.47,45296.58]
["1330000000-E","INCIDENTAL MILLING","","",21330,7.3006469760000003,155722.79999999999]
["1489000000-E","ASP CONC BAS CRS B25.0B","","",28460,38.402090653999998,1092923.5]
["1491000000-E","ASP CONC BAS CRS B25.0C","","",39110,36.570761953000002,1430282.5]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",21920,38.496806569,843850]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",21260,37.970366886000001,807250]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",42253,37.534991597999998,1585966]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",29940,41.408149633000001,1239760]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",68069,33.373077318999997,2271672]
["1575000000-E","ASP FOR PLANT MIX","","",14366,577.74018515900002,8299815.5]
["1682000000-E","PERM ASPH DRNG CO, P-57","","",18000,43,774000]
["1693000000-E","ASP PLT MIX PVT REPAIR","","",1130,159.292035398,180000]
["1775000000-E","AST, MAT COAT, 78M STONE","","",477460,0.90036501499999999,429888.28]
["1839000000-E","GENERIC PAVING ITEM (660)","ASPH SURFACE TREATMENT, MAT","COAT, 67 STONE",165908,1.1589970350000001,192286.88]
["1840000000-E","MILLED RUMBLE STRIPS","","",52600,0.34125475300000002,17950]
["1847000000-E","******\"PCC PVT THRU LNS","(10\")","",137500,42,5775000]
["1881000000-E","GENERIC PAVING ITEM (LF)","MILLED RUMBLE STRIPS (CONCSHDR)","",83000,1,83000]
["1891000000-E","GENERIC PAVING ITEM (SY)","DIAMOND GRINDING PCC PVT","",131000,2.25,294750]
["1892000000-E","GENERIC PAVING ITEM (SY) 710","VARIABLE DEPTH CONC SHOUL-DER ADJA-","CENT TO 10\" PVT - MIN 7\" THICKNESS",50700,34,1723800]
["1902000000-N","SURF TEST CONC PVT","","",1,150000,150000]
["1913000000-E","CONC SHLD ADJ *****\"PVT","(10\")","",22400,34,761600]
["1924000000-N","FIELD LAB RENTAL, PCCP","","",1,148000,148000]
["2000000000-N","RIGHT OF WAY MKRS","","",480,130.41666666699999,62600]
["2022000000-E","SUBDRN EXCAV","","",17883.8,20.894787461,373678.2]
["2033000000-E","SUBDRN FINE AGG","","",9019.4,40.572211011999997,365937]
["2044000000-E","6\" PERF SUBDRN PIPE","","",53300,10.341463415,551200]
["2070000000-N","SUBDRN PIPE OUTLET","","",107,369.065420561,39490]
["2077000000-E","6\" OUTLET PIPE","","",642,40.140186915999998,25770]
["2099000000-E","SHDR DRN","","",44500,6.1617977530000001,274200]
["2110000000-E","4\" SHDR DRN PIPE","","",44500,1.5682022470000001,69785]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",2490,8.5210843369999996,21217.5]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",54,309.25925925899998,16700]
["2143000000-E","BLOTTING SAND","","",30,33.333333332999999,1000]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",2,1250,2500]
["2209000000-E","ENDWALLS","","",89,989.88764044899995,88100]
["2220000000-E","REINF ENDWALLS","","",48,1150,55200]
["2253000000-E","PIPE COLLARS","","",16.951000000000001,553.42457672099999,9381.1]
["2264000000-E","PIPE PLUGS","","",4,905,3620]
["2275000000-E","FLOWABLE FILL","","",12,541.66666666699996,6500]
["2286000000-N","MASNRY DRNG STRUCT","","",393,1424.3256997460001,559760]
["2297000000-E","MASNRY DRNG STRUCT","","",17,1011.764705882,17200]
["2308000000-E","MASNRY DRNG STRUCT","","",46.99,259.911683337,12213.25]
["2352000000-N","FRM W/GRATE 840.** STD","(840.20)","",1,600,600]
["2354200000-N","FRM W/GRT 840.24 STD","","",2,585,1170]
["2364000000-N","FRM W/2GRTS 840.16 STD","","",17,581.17647058800003,9880]
["2364200000-N","FRM W/2GRTS 840.20 STD","","",114,604.60526315799996,68925]
["2365000000-N","FRM W/2GRTS 840.22 STD","","",155,600.161290323,93025]
["2366000000-N","FRM W/2GRTS 840.24 STD","","",3,625,1875]
["2367000000-N","FRM W/2GRTS 840.29 STD","","",12,553.33333333300004,6640]
["2374000000-N","FRM-GRT-HD 840.03 **","(E)","",13,640.38461538499996,8325]
["","","(F)","",20,650,13000]
["","","(G)","",27,649.07407407400001,17525]
["2396000000-N","FRM W/COVR STD 840.54","","",20,622.5,12450]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",5,600,3000]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",17,738.23529411799996,12550]
["2473000000-N","GENERIC DRNG ITEM (EA)","BICYCLE SAFE STL FRM ","& GRATE",1,1700,1700]
["","","TRASH RACK","",1,1200,1200]
["2474000000-N","GENERIC DRNG ITEM (LS)","LEVEL SPRDER W/ VEGE-","TATE TROUGH",1,15000,15000]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",3700,15,55500]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",11960,15.652173913,187200]
["2556000000-E","SHDR BERM GUTR","","",28973,17.725054361000002,513548]
["2570000000-N","MOD CONC FLUME","","",1,1400,1400]
["2591000000-E","4\" CONC SIDEWALK","","",2500,30,75000]
["2600000000-N","RETROFIT EXT CURB RMP","","",64,397.5,25440]
["2605000000-N","CONC CURB RAMP","","",19,931.57894736799994,17700]
["2612000000-E","6\" CONC DRIVEWAY","","",1200,44.166666667000001,53000]
["2619000000-E","4\" CONC PAVED DITCH","","",125,48,6000]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",3550,42.859154930000003,152150]
["2724000000-E","PC REINF BARR SNGL FC","","",1000,60,60000]
["2752000000-E","GENERIC PAVING ITEM(LF)","SPECIAL SHDR BERM","CURB",10,60,600]
["2815000000-N","ADJ DROP INLETS","","",20,742.3,14846]
["2830000000-N","ADJ MHS","","",140,551.34285714299995,77188]
["2845000000-N","ADJ METER OR VAL BOX","","",160,528.02499999999998,84484]
["2905000000-N","CONVERT DI TO JB","","",1,1200,1200]
["3000000000-N","IMPACT ATTEN  350","","",18,13500,243000]
["3030000000-E","STL BM GRDRL","","",71100,14.391350211000001,1023225]
["3045000000-E","SBGR SHOP CURVED","","",637.5,14.38627451,9171.25]
["3105000000-N","SBGR TERM SECT","","",14,31.8,445.2]
["3150000000-N","ADDIT GRDRL POSTS","","",85,32.362352940999997,2750.8]
["3195000000-N","GR ANCHOR  AT-1","","",1,525,525]
["3210000000-N","GR ANCHOR  CAT-1","","",55,424.90909090899999,23370]
["3215000000-N","GR ANCHOR  III","","",22,1394.545454545,30680]
["3270000000-N","GR ANCHOR  350","","",134,1646.2014925369999,220591]
["3285000000-N","GR ANCHOR  M-350","","",23,1500,34500]
["3317000000-N","GR ANCHOR  B-77","","",53,1500,79500]
["3345000000-E","REM & RESET GRDRL","","",100,5,500]
["3360000000-E","REM EXT GRDRL","","",7485,0.48768203100000002,3650.3]
["3380000000-E","TEMP STL BM GRDRL","","",1887.5,4.2119205300000004,7950]
["3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",50,5,250]
["3387000000-N","TEMP GDRL ANCH UNIT***","(AT-1)","",1,300,300]
["","","(B-77)","",5,1000,5000]
["","","(CAT-1)","",1,315,315]
["3389000000-N","TEMP GDRL ANCH UNIT***","(M-350)","",1,515,515]
["3389100000-N","TEMP GDRL ANCH UNITS 350","","",2,725,1450]
["3389200000-E","CABLE GUIDERAIL","","",18100,7,126700]
["3389500000-N","ADDITIL GUIDERAIL POST","","",30,26,780]
["3389600000-N","CBL GUIDERAIL ANC UNT","","",36,1550,55800]
["3435000000-N","GENERIC GRDRL ITEM(EA)","EXTRA LENGTH GRDRL ","POST (8' STL)",20,81,1620]
["","","TEMP IMPACT ATTENUATOR UNIT,  350","",2,13500,27000]
["3436000000-N","GENERIC GRDRL ITEM (EA) 862","TEMP ADDITIONAL GRDRLPOSTS","",10,52,520]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",74560,2.1679184550000001,161640]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",4810,15.083160082999999,72550]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",1225,20.220408162999998,24770]
["3533000000-E","CHN LK FENCE **\" FABRIC","(72\")","",700,12.5,8750]
["3539000000-E","MET LINE PST **\" CL FEN","(72')","",60,36,2160]
["3545000000-E","MET TERM PST **\" CL FEN","(72')","",4,115,460]
["3557000000-E","ADDITIONAL BARB WIRE","","",1100,0.22727272700000001,250]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 12')","",2,475,950]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 10', 20')","",1,725,725]
["3566000000-E","WOVEN WIRE FENCE RESET","","",640,3.5,2240]
["3569000000-E","BARBED WIRE FENCE RESET","","",830,2.6,2158]
["3572000000-E","CHAIN LINK FENCE RESET","","",400,4.25,1700]
["3628000000-E","RIP RAP, CL I","","",3700,36.200000000000003,133940]
["3642000000-E","RIP RAP, CL A","","",320,39.6875,12700]
["3649000000-E","RIP RAP, CL B","","",4562,52.129767645999998,237816]
["3651000000-E","BOULDERS","","",975,55,53625]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",67246,1.976855129,132935.6]
["3659000000-N","PREFORM SCOUR HOLES","","",17,885.29411764700001,15050]
["4025000000-E","CONTR FURN,  ***SIGN","(E)","",276,14.5,4002]
["4048000000-E","REINF CONC FOUNDTN","","",48,817.1875,39225]
["4054000000-E","PLN CONC FOUNDTN","","",2,475,950]
["4057000000-E","OVERHEAD FOOTING","","",664,668.22289156600004,443700]
["4060000000-E","SUPPT, BRKAWY STL BM","","",32938,3.3128058779999998,109117.2]
["4066000000-E","SUPPT, SIMPLE STL BM","","",2459,2.6,6393.4]
["4072000000-E","SUPPT, 3-LB STL U-CHAN","","",10615,7.2345605280000003,76794.86]
["4082100000-N","SUPPORT, OVRHD SIGN STR ****","(100+00 -Y13-)","",1,58000,58000]
["","","(123+00 -L-)","",1,20000,20000]
["","","(127+50 -Y13-)","",1,45000,45000]
["","","(135+50 -L-)","",1,45000,45000]
["","","(187+50 -L-)","",1,44000,44000]
["","","(241+60 -L-)","",1,55000,55000]
["","","(251+50 -L-)","",1,60000,60000]
["","","(28+00 -L-)","",1,40000,40000]
["","","(29+00 -I13CD-)","",1,27000,27000]
["","","(30+00 -Y13RPC-)","",1,37000,37000]
["","","(36+50 -Y13-)","",1,50000,50000]
["","","(39+00 -L-)","",1,64000,64000]
["","","(47+00 -L-)","",1,28000,28000]
["","","(48+50 -Y13-)","",1,40000,40000]
["","","(65+00 -Y13-)","",1,43000,43000]
["","","(69+00 -L-)","",1,42000,42000]
["","","(73+50 -L1-)","",1,46270,46270]
["","","(77+50 -Y13-)","",1,49000,49000]
["","","(8+00 -Y13-)","",1,44000,44000]
["","","(90+75 -Y13-)","",1,54000,54000]
["","","(94+25 -L-)","",1,50000,50000]
["","","(A AT 75' W OF EXT STR)","",1,50000,50000]
["","","(AC AT 50' W OF EXT ","STR)",1,46000,46000]
["","","(AD AT 500' S OF EXT","OVERHD ASSEM 'PP')",1,20000,20000]
["","","(B ON RAMP TO I-85 SB & ","I-785 NB)",1,45000,45000]
["","","(C AT 50' E OF EXT STR)","",1,49000,49000]
["","","(D AT 50' E OF EXT STR)","",1,59000,59000]
["","","(E AT 100' E OF EXT STR)","",1,97000,97000]
["","","(F AT 400'W OF EXT STR)","",1,95000,95000]
["","","(G @ 100'W OF EXT STR)","",1,90000,90000]
["4096000000-N","SIGN ERECTION,  D","","",48,85.512500000000003,4104.6000000000004]
["4102000000-N","SIGN ERECTION,  E","","",380,60.357894737000002,22936]
["4108000000-N","SIGN ERECTION,  F","","",42,68.523809524000001,2878]
["4109000000-N","SIGN ERECT, *** (OVRHD)","(A)","",28,575,16100]
["","","(B)","",19,160,3040]
["4110000000-N","SIGN ERECTION,  *** (GRD MTD)","(A)","",41,340.60975609799999,13965]
["","","(B)","",24,304.375,7305]
["4114000000-N","SIGN ERECTION, MILEMKR","","",64,32.6875,2092]
["4116000000-N","SIGN ERECTION, OVERLAY (GRD MTD)","","",2,375,750]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",1,250,250]
["4149000000-N","DISP SIGN SYST OVRHD","","",7,2900,20300]
["4152000000-N","DISP SIGN SYST STL BM","","",8,393.75,3150]
["4155000000-N","DISP SIGN SYST U-CHAN","","",251,2.1155378489999999,531]
["4234000000-N","DISP SIGN, A OR B (OVRHD)","","",47,285,13395]
["4236000000-N","DISP SIGN, A, B OR C (GRD MTD)","","",5,57.8,289]
["4238000000-N","DISP SIGN, D, E, F","","",5,1,5]
["4251000000-N","DISP LIGHT SYST","","",18,600,10800]
["4263000000-N","DISP WALKWAY","","",18,600,10800]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",9269,3.453771712,32013.01]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",4717,9.7222811109999991,45860]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",2578,4.415283165,11382.6]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",6509,4.3264449220000003,28160.83]
["4415000000-N","FLASH ARROW BOARD","","",14,2671.4285714289999,37400]
["4420000000-N","PORT CHANGE MSG SIGN","","",14,10928.571428571,153000]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",32,28,896]
["4430000000-N","DRUMS","","",1663,49.343355381999999,82058]
["4435000000-N","CONES","","",424,18.318396226000001,7767]
["4445000000-E","BARRICADES ( III)","","",3129,17.600031958999999,55070.5]
["4450000000-N","FLAGGER","","",944,22,20768]
["4455000000-N","FLAGGER","","",1006,220.477137177,221800]
["4457000000-N","TEMP TRAFFIC CNTRL","","",3,17666.666666666999,53000]
["4465000000-N","TEMP CRASH CUSHIONS","","",17,4661.7647058820003,79250]
["4470000000-N","RESET CRASH CUSHION","","",7,2142.8571428569999,15000]
["4480000000-N","TMA","","",20,12006.25,240125]
["4485000000-E","PORT CONC BARRIER","","",7883,27.152714703000001,214044.85]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",5565,34,189210]
["4500000000-E","RESET PORT CONC BARR","","",4812,4.1296758100000002,19872]
["4510000000-N","LAW ENFORCEMENT","","",440,45.909090909,20200]
["4516000000-N","SKINNY DRUM","","",485,29.603092784000001,14357.5]
["4650000000-N","TEMP RAISED PVT MRKS","","",2277,5.4689503730000002,12452.8]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",293347,0.54865698299999999,160946.88]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",341350,0.70195257099999997,239611.51]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",108584,0.96049141699999996,104294]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",17386,1.282848269,22303.599999999999]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",4141,2.139507365,8859.7000000000007]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",2308,2.7960138649999999,6453.2]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",15539,2.414576228,37520.1]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",3046,7.711950098,23490.6]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",105,85.647619047999996,8993]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",365,129.67123287699999,47330]
["4770000000-E","4\" COLD APPL PLSTIC LINES  **","(II)","",6555,2.9527841339999998,19355.5]
["","","(IV)","",2280,1.6473684209999999,3756]
["4780000000-E","8\" COLD APPL PLSTIC LINES  **","(II)","",112,11.5,1288]
["4785000000-E","12\" COLD PLSTIC LINES  **","(II)","",737,14.5,10686.5]
["4800000000-N","COLD APP PLAS CHAR  *","(II)","",4,280,1120]
["4805000000-N","COLD APPL PLASTIC SYM  **","(II)","",15,285,4275]
["4810000000-E","PAINT PVT MKRGS 4\"","","",2095399,0.150948798,316297.96000000002]
["4815000000-E","PAINT PVT MKRGS 6\"","","",114,0.14298245600000001,16.3]
["4820000000-E","PAINT PVT MKRGS 8\"","","",41182,0.52293477700000002,21535.5]
["4825000000-E","PAINT PVT MKRGS 12\"","","",1740,1.08,1879.2]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",90,2,180]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",3600,3.0429722219999999,10954.7]
["4840000000-N","PAINT PVT MKG CHARACTER","","",84,23.095238094999999,1940]
["4845000000-N","PAINT PVT MKG SYMBOL","","",440,60.937272727,26812.400000000001]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",109493,1.2,131391.6]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",5510,3.1,17081]
["4850000000-E","LINE REML 4\" WIDE","","",53946,0.88665053900000002,47831.25]
["4860000000-E","LINE REML 8\" WIDE","","",1438,1.55,2228.9]
["4870000000-E","LINE REML 24\" WIDE","","",135,2.825185185,381.4]
["4875000000-N","REML OF SYMBL & CHAR","","",28,63.928571429000002,1790]
["4890000000-E","GENERIC PVT MKRG ITEM (LF)","TEMP RUMBLE STRIPS","",6828,3.4,23215.200000000001]
["4900000000-N","PERM RAISED PVT MKRS","","",1841,4.6985334060000001,8650]
["4905000000-N","SNOWPLB PVT MRKER","","",4186,30.468227424999998,127540]
["4915000000-E","7' U-CHANNEL POSTS","","",9,35,315]
["4935000000-N","FLEX DELINTR (CRYSTAL)","","",20,44,880]
["4940000000-N","FLEX DELINTR (YELLOW)","","",20,44,880]
["4955000000-N","OBJECT MKR(END OF RD)","","",21,255,5355]
["5005000000-E","80' HIGH MOUNT STD","","",1,15000,15000]
["5015000000-E","120' HIGH MOUNT STD","","",1,20000,20000]
["5020000000-N","PORTABLE DRIVE UNIT","","",1,3500,3500]
["5025000000-E","HIGH MOUNT FOUNDS","","",28,900,25200]
["5030000000-N","HM LUMINAIRE ************","(400W HPS)","",8,800,6400]
["","","(750W HPS)","",8,850,6800]
["5070000000-N","STD FOUNDAT ***********","( R1)","",6,850,5100]
["","","( R2)","",2,875,1750]
["5120000000-N","SERVICE POLE ************","(30' CL 4)","",1,1150,1150]
["5125000000-E","SERVICE LATERAL ********","(3 1/0 USE)","",100,36,3600]
["5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",200,11.5,2300]
["","","(3\")","",370,12.7,4699]
["","","(6\")","",110,17,1870]
["5160000000-E","ELECT DUCT JA, SIZE *****","(4\")","",180,12.5,2250]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2\")","",170,3,510]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2\")","",560,4,2240]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(2\")","",390,5.5,2145]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2, 1.5)","",190,7,1330]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",520,7.5,3900]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",3710,8.6,31906]
["5220000000-E","**-2 W/G FEEDER N *****\"","(2, 1.5)","",2600,10.5,27300]
["5240000000-N","ELEC JB ************","(PC18)","",16,310,4960]
["","","(PC30)","",3,725,2175]
["5255000000-N","PORTABLE LIGHTING","","",3,58000,174000]
["5270000000-N","GENERIC LIGHT ITEM (EA)","RELOC CNTRL SYST","",1,5600,5600]
["","","RELOC HIGH MOUNT STD","",2,5500,11000]
["","","RELOC LIGHT STD","",8,800,6400]
["","","REM LIGHT STD","",14,305,4270]
["","","REPLACE LUMINAIRE ","(HIGH MAST)",8,750,6000]
["","","REPLACE LUMINAIRE ","(SINGLE ARM)",8,260,2080]
["5325600000-E","6\" H2O LINE","","",165,59,9735]
["5325800000-E","8\" H2O LINE","","",3212,43.631070983999997,140143]
["5326200000-E","12\" H2O LINE","","",4959,114.013309135,565392]
["5326600000-E","16\" H2O LINE","","",6113,121.842466874,744823]
["5328000000-E","30\" H2O LINE","","",3957,265,1048605]
["5540000000-E","6\" VALVE","","",9,1000,9000]
["5546000000-E","8\" VALVE","","",3,1566.6666666670001,4700]
["5552000000-E","10\" VALVE","","",1,1900,1900]
["5558000000-E","12\" VALVE","","",8,2562.5,20500]
["5558600000-E","16\" VALVE","","",10,7950,79500]
["5560000000-E","30\" VALVE","","",6,11500,69000]
["5589200000-E","2\" AIR RELEASE VALVE","","",1,4200,4200]
["5606600000-E","6\" BLOW OFF","","",2,18000,36000]
["5648000000-N","RELOC H2O METER","","",7,1228.5714285710001,8600]
["5666000000-E","FIRE HYDRANT","","",16,2227.5,35640]
["5672000000-N","RELOC FIRE HYDRANT","","",9,3133.3333333330002,28200]
["5691400000-E","10\" SANIT GRAV SEWER","","",330,125,41250]
["5691700000-E","18\" SANIT GRAV SEWER","","",435,220,95700]
["5709000000-E","**\" FORCE MAIN SEWER","(30\")","",949,425,403325]
["","","(54\")","",236,2350,554600]
["5768000000-N","SANIT SEWR CLEAN-OUT","","",4,1000,4000]
["5776000000-E","5' DIA UTIL MH","","",4,4800,19200]
["5782000000-E","UTIL MH WALL, 5' DIA","","",15,330,4950]
["5802000000-E","ABANDON 10\" UTIL PIPE","","",175,4.5,787.5]
["5804000000-E","ABANDON 12\" UTIL PIPE","","",873,4.5999999999999996,4015.8]
["5811000000-E","ABANDON 18\" UTIL PIPE","","",430,9,3870]
["5814000000-E","ABANDON 30\" UTIL PIPE","","",2295,21,48195]
["5815500000-N","REM FIRE HYDRANT","","",1,440,440]
["5816000000-N","ABANDON UTIL MH","","",2,500,1000]
["5835000000-E","**\" ENCASEMENT PIPE","(48\")","",599,750,449250]
["","","(60\")","",230,460,105800]
["","","(72\")","",94,820,77080]
["5835800000-E","18\" ENCASEMENT PIPE","","",112,84,9408]
["5836000000-E","24\" ENCASEMENT PIPE","","",4768,64.185822148,306038]
["5836200000-E","30\" ENCASEMENT PIPE","","",1370,407,557590]
["5836400000-E","36\" ENCASEMENT PIPE","","",353,407,143671]
["5871000000-E","**\" TRENCHLESS INSTALL (IN SOIL)","(48\")","",75,102,7650]
["5871010000-E","**\" TRENCHLESS INSTALL (NOT IN SOIL)","(48\")","",75,205,15375]
["5872200000-E","24\" TRENCHLESS INSTALL (IN SOIL)","","",1293,305,394365]
["5872210000-E","24\" TRENCHLESS INSTALL (NOT IN SOIL)","","",1292,407,525844]
["5872300000-E","30\" TRENCHLESS INSTALL (IN SOIL)","","",425,155,65875]
["5872310000-E","30\" TRENCHLESS INSTALL (NOT IN SOIL)","","",425,155,65875]
["5872400000-E","36\" TRENCHLESS INSTALL (IN SOIL)","","",176.5,193,34064.5]
["5872410000-E","36\" TRENCHLESS INSTALL (NOT IN SOIL)","","",176.5,195,34417.5]
["6000000000-E","TEMP SILT FENCE","","",195980,1.5071576179999999,295372.75]
["6006000000-E","EROS CNTRL STONE CL A","","",8950,32.850279329999999,294010]
["6009000000-E","EROS CNTRL STONE CL B","","",80250,35.488348909999999,2847940]
["6012000000-E","SEDIMENT CNTRL STONE","","",66545,29.651739423999999,1973175]
["6015000000-E","TEMP MULCHING","","",816.3,360.17701825300003,294012.5]
["6018000000-E","SEED FOR TEMP SEEDING","","",26950,2.7181818180000001,73255]
["6021000000-E","FERT FOR TEMP SEEDING","","",109.25,888.94736842099996,97117.5]
["6024000000-E","TEMP SLOPE DRNS","","",38055,8.6956247540000007,330912]
["6029000000-E","SAFETY FENCE","","",51700,1.3543520309999999,70020]
["6030000000-E","SILT EXCAV","","",142530,4.6397074299999996,661297.5]
["6036000000-E","MAT FOR EROS CNTRL","","",271540,1.018970317,276691.20000000001]
["6037000000-E","COIR FIBER MAT","","",10610,4.3180018850000002,45814]
["6038000000-E","PERM SOIL REINF MAT","","",17425,4.5308464849999996,78950]
["6042000000-E","1/4\" HARDWARE CLOTH","","",31735,2.9453757679999999,93471.5]
["6045000000-E","**\" TEMP PIPE","(18\")","",250,35,8750]
["","","(24\")","",50,48,2400]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",250,45,11250]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",1025,18,18450]
["6069000000-E","STILLING BASINS","","",2130,6.8568075119999996,14605]
["6070000000-N","SPECIAL STILLING BASINS","","",126,608.73015872999997,76700]
["6071010000-E","WATTLE","","",1755,6.0128205130000003,10552.5]
["6071012000-E","COIR FIBER WATTLE","","",36700,6.0607084469999997,222428]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",29105,4.9169214910000001,143107]
["6071030000-E","COIR FIBER BAFFLE","","",27420,3.6901075859999999,101182.75]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",95,1102.631578947,104750]
["","","(2\")","",6,1415,8490]
["","","(2-1/2\")","",2,1567.5,3135]
["6078000000-E","SEL UNDERGRTH REML","","",5,5000,25000]
["6084000000-E","SEEDING & MULCHING","","",753.3,1549.0375680340001,1166890]
["6087000000-E","MOWING","","",375.7,83.071599680999995,31210]
["6090000000-E","SEED FOR REPAIR SEED","","",9350,2.7128342249999999,25365]
["6093000000-E","FERT FOR REPAIR SEED","","",32.25,889.72868217099995,28693.75]
["6096000000-E","SEED FOR SUPP SEEDING","","",17925,2.5838214779999999,46315]
["6108000000-E","FERTILIZER TOPDRESSING","","",536,883.34888059699995,473475]
["6111000000-E","IMPERVIOUS DIKE","","",862,23.770301623999998,20490]
["6114500000-N","SPECIALIZED HAND MOW","","",435,59.103448276000002,25710]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",400,181.51499999999999,72606]
["6118000000-N","ROOTWADS","","",2,1250,2500]
["6120000000-E","CLVT DIVERSION CHANL","","",2383,9.5039865720000005,22648]
["6123000000-E","REFORESTATION","","",12.3,1191.4634146339999,14655]
["6126000000-E","STRMBANK REFORESTAT","","",5.34,1150,6141]
["6132000000-N","GENERIC EROSION CNTRL ITEM (EA)","LOGS","",6,800,4800]
["6133000000-N","GENERIC EROSION CNTRL ITEM (LS)","CONST SURVEYING FOR MITIGATION","",1,26000,26000]
["","","DIVERSION PUMPING FOR ","MITIGATION",1,30000,30000]
["","","GRADING FOR MITIGATN","",1,425000,425000]
["6138000000-E","GENERIC EROSION CNTRL ITEM (CY)","IMPERVIOUS SELECT MATERIAL","",175,10,1750]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",10,705,7050]
["7060000000-E","SIGNAL CABLE","","",8750,2.15,18812.5]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",51,665,33915]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",8,825,6600]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",3,1115,3345]
["7252000000-E","MESSENGER CABLE (1/4\")","","",4215,6,25290]
["7279000000-E","TRACER WIRE","","",38000,0.4,15200]
["7288000000-E","PAVED TRENCH (**********)","(1, 2\")","",65,5.230769231,340]
["7300000000-E","UNPAVED TRENCH (******)","(1, 2\")","",6265,5.4166001599999998,33935]
["","","(2, 2\")","",5800,9,52200]
["","","(4, 1-1/4\")","",31200,6,187200]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",300,3,900]
["7301000000-E","DIRECT DRILL (***********)","(2, 2\")","",1500,16,24000]
["","","(4, 1-1/4\")","",1300,16,20800]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",106,295.283018868,31300]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",85,560,47600]
["7360000000-N","WOOD POLE","","",37,950,35150]
["7372000000-N","GUY ASSEMBLY","","",64,375,24000]
["7384000000-E","***\" RISER WITH ***********","(1-1/2\", WEATHERHEAD)","",2,320,640]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",9,325,2925]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",63,439.28571428599997,27675]
["7432000000-E","2\" RISER WITH TUBING","","",2,555,1110]
["7444000000-E","INDUCTIVE LOOP SWCUT","","",15915,5.3319981150000002,84858.75]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",23780,0.96951219499999997,23055]
["7484000000-N","MICROWAVE VEHICLE DETECTOR","","",1,950,950]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(144)","",37500,2.1,78750]
["7528000000-E","DROP CABLE","","",7000,1.45,10150]
["7540000000-N","SPLICE ENCLOSURE","","",7,3000,21000]
["7541000000-N","MOD SPLICE ENCLOSURE","","",1,2400,2400]
["7552000000-N","INTERCONNECT CENTER","","",9,925,8325]
["7566000000-N","DELINEATOR MKR","","",84,72,6048]
["7575142000-N","900MHZ RADIO","","",6,3000,18000]
["7613000000-N","SOIL TEST","","",7,1100,7700]
["7614100000-E","DRILLED PIER FOUND","","",35,840,29400]
["7636000000-N","SIGN FOR SIGNALS","","",9,300,2700]
["7642100000-N"," I POST W/ FOUND","","",2,1300,2600]
["7642200000-N"," II PED W/ FOUND","","",7,1500,10500]
["7684000000-N","SIGNAL CBNT FOUND","","",8,1100,8800]
["7756000000-N","CONTLR WITH CBNT, 2070L BAS MTD","","",8,11500,92000]
["7780000000-N","DETECTOR CARD ( 2070L)","","",34,110,3740]
["7901000000-N","CBNT BAS EXTENDER","","",8,300,2400]
["7980000000-N","GENERIC SIGNAL ITM(EA)","5/8\" X 10' GROUNDING ","ELECTRODE",54,120,6480]
["","","CCTV CAMERA ASSEM","",8,3800,30400]
["","","CCTV EXTENSION POLE","",1,4800,4800]
["","","CCTV METAL POLE","",7,3600,25200]
["","","CENTRAL MEDIA CONVTR","",1,1250,1250]
["","","CENTRAL VIDEO CODEC ","UNIT",8,2650,21200]
["","","DMS","",3,73000,219000]
["","","DMS ACCESS LADDER","",2,4250,8500]
["","","DMS PEDESTAL STR( A)","",1,45000,45000]
["","","DMS PEDESTAL STR( B)","",1,48000,48000]
["","","EQUIP CBNT DISCONNECT","",7,1150,8050]
["","","FIELD EQUIP CBNT","",8,3650,29200]
["","","FIELD ETHERNET SWITCH","",9,1150,10350]
["","","FIELD VIDEO CODEC UNIT","",8,2500,20000]
["","","JUNCTION BOX (SPECIAL OVER-","SIZED, HEAVY-DUTY)",7,2100,14700]
["","","METER BAS/DISCONNECT COMBIN-","ATION PANEL",8,500,4000]
["","","SIGNAL EQUIP CBNT DISCONNECT","",1,1150,1150]
["","","WOOD PEDESTAL","",8,265,2120]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","INTEGRATION & CONFIGURATION","",1,7100,7100]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","4 SOLID BARE COPPER GROUNDINGCONDUCTOR","",20,410,8200]
["","","4 SOLID BARE GROUNDING CONDUCTR","",240,2.2999999999999998,552]
["","","6 AWG 3-WIRE COPPER FEEDER CONDUCTORS","",200,5,1000]
["","","3-WIRE COPPER FEEDER CONDUCTORS","",1800,3,5400]
["","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",50,26,1300]
["","","4-WIRE COPPER FEEDER CONDUCT- ORS","",600,9,5400]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","ITS OVERHEAD FOOTINGS","",16,800,12800]
["8035000000-N","REMV EXIST STR **********","(16+64.29-L-)","",1,45225,45225]
["","","(16+88.00-L-)","",1,22790,22790]
["","","(26+17.64-Y22-LT)","",1,200000,200000]
["","","(26+21.65-L-RT)","",1,25000,25000]
["8091000000-N","FND EXCAV B** STA ******","(1, 228+23.81-L-)","",1,3500,3500]
["","","(1, 26+17.64-Y22-LT)","",1,65000,65000]
["","","(1, 26+17.64-Y22-RT)","",1,22000,22000]
["","","(1, 268+22.89-L-)","",1,55000,55000]
["","","(1, 80+74.41-L-)","",1,3500,3500]
["","","(1,60+37.13-L-)","",1,13395,13395]
["","","(2,60+37.13-L-)","",1,12000,12000]
["","","(3, 14+99.25-L-)","",1,18000,18000]
["","","(4, 14+99.25-L-)","",1,12000,12000]
["8096000000-E","PILE EXCAV IN SOIL","","",83,165,13695]
["8097000000-E","PILE EXCAV NOT IN SOIL","","",67,285,19095]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",304.75,580,176755]
["","","(8'-0\")","",199,1050,208950]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",127.5,933.92941176500005,119076]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",25,650,16250]
["8105600000-E","**'-**\" DRILL PIER NO SOIL","(4'-6\")","",103,1350,139050]
["","","(8'-0\")","",232,3875,899000]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",100.5,991.71343283600004,99667.199999999997]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",50,1250,62500]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",61.4,110,6754]
["8113000000-N","SID INSPECTIONS","","",22,615.68181818200003,13545]
["8114000000-N","SPT TESTING","","",6,920,5520]
["8115000000-N","CSL TESTING","","",20,2405,48100]
["8121000000-N","UNCL STR EXCAV STA****","(14+99.25-L-)","",1,22000,22000]
["","","(16+64.29-L-)","",1,3150,3150]
["","","(16+88.00-L-)","",1,10000,10000]
["","","(26+17.64-Y22-LT)","",1,14000,14000]
["","","(26+17.64-Y22-RT)","",1,10000,10000]
["","","(268+22.89-L-)","",1,14000,14000]
["8126000000-N","CULV EXCAV @ ***********","(114+55.00-L-)","",1,14000,14000]
["","","(14+77.40-YLPD-)","",1,16000,16000]
["","","(218+00.00-L-)","",1,13000,13000]
["","","(241+96.00-L-)","",1,30000,30000]
["","","(43+86.48-Y-)","",1,18000,18000]
["","","(48+65.00-L-)","",1,23000,23000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",2299,37.548499348,86324]
["8147000000-E","REINF CONC DECK SLAB","","",274771,24.28575068,6673020]
["8156000000-E","CONC WEARING SURFAC","","",3069,18.399999999999999,56469.599999999999]
["8161000000-E","GROOVING BRG FLOORS","","",266132,0.28893913500000001,76895.95]
["8182000000-E","CL A CONC (BRIDGE)","","",4351.1000000000004,719.097818942,3128866.52]
["8196000000-E","CL A CONC (CULV)","","",4897.2,373.18590214800003,1827566]
["8210000000-N","BRG APPR SLAB ***********","(129+37.56-L-LT)","",1,40000,40000]
["","","(129+37.56-L-RT)","",1,40000,40000]
["","","(14+99.25-L-)","",1,40000,40000]
["","","(144+60.63-L-)","",1,40000,40000]
["","","(144+90.00-L-)","",1,40000,40000]
["","","(16+64.29-L-)","",1,31100,31100]
["","","(16+88.00-L-)","",1,18000,18000]
["","","(174+72.46-L-LT)","",1,40000,40000]
["","","(174+72.46-L-RT)","",1,40000,40000]
["","","(228+23.81-L-)","",1,34000,34000]
["","","(24+59.04-L-)","",1,35000,35000]
["","","(26+17.64-Y22-LT)","",1,42000,42000]
["","","(26+17.64-Y22-RT)","",1,35000,35000]
["","","(26+21.65-L-LT)","",1,40000,40000]
["","","(26+21.65-L-RT)","",1,15000,15000]
["","","(268+22.89-L-)","",1,45000,45000]
["","","(60+37.13-L-)","",1,36980,36980]
["","","(80+74.41-L-)","",1,42000,42000]
["8217000000-E","REINF STEEL (BRIDGE)","","",974705,0.75655278299999995,737415.78]
["8238000000-E","SPIRAL COL REINF STL BRG","","",85149,1.38139802,117624.66]
["8245000000-E","REINF STEEL (CULVERT)","","",480251,0.88589962300000002,425454.18]
["8265000000-E","54\" PRESTR CONC GIRDR","","",5929.19,175,1037608.25]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",5844.82,217.97444574900001,1274021.3999999999]
["8280000000-E","STRUCTURAL STEEL","","",8014400,1.2957925729999999,10385000]
["8364000000-E","HP12X53 PILES","","",16915.5,52.561408176,889102.5]
["8391000000-N","STEEL PILE POINTS","","",152,129.73684210499999,19720]
["8475000000-E","TWO BAR METAL RAIL","","",1662.8,87.206879962000002,145007.6]
["8482000000-E","THREE BAR METAL RAIL","","",363.67,155,56368.85]
["8503000000-E","CONC BARRIER RAIL","","",9584.15,50,479207.5]
["8505000000-E","VERT CONC BARR RAIL","","",814.58,82.416803752000007,67135.08]
["8517000000-E","1'-**\"X****\"CONC PARAPET","(1'-2\" X 2'-6\")","",1707.8,60.071905375,102590.8]
["8531000000-E","4\" SLOPE PROTECTION","","",7471,73.879801900999993,551956]
["8608000000-E","RIP RAP II (2'-0\")","","",3857,40.159761473000003,154896.20000000001]
["8622000000-E","GEOTEXTILE FOR DRNG","","",4323,2.652729586,11467.75]
["8650000000-N","POT BEARINGS","","",1,425000,425000]
["8657000000-N","ELASTOMERIC BEARINGS","","",5,36700,183500]
["8692000000-N","FOAM JOINT SEALS","","",2,18000,36000]
["8706000000-N","EXPANSION JOINT SEALS","","",1,170000,170000]
["8713000000-N","MODULAR EXP JOINT SEALS","","",1,135000,135000]
["8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(129+37.56-L-RT)","",1,26000,26000]
["","","(14+99.25-L-)","",1,47000,47000]
["","","(144+60.63-L-)","",1,150000,150000]
["","","(174+72.46-L-RT)","",1,18000,18000]
["","","(26+21.65-L-LT)","",1,20000,20000]
["","","(268+22.89-L-)","",1,34000,34000]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLAB","","",1490,137.986577181,205600]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLAB","","",1260,156.9,197694]
["8801000000-E","MSE RETAIN WALL NO **","(1 @ EB1)","",5430,45.01,244404.3]
["","","(1)","",3200,50,160000]
["","","(2 @ EB2)","",3472,45.01,156274.72]
["","","(2)","",3600,52,187200]
["8860000000-N","GENERIC STR ITEM (LS)","MODIFIED BRIDGE APPROACH FILL,","STATION 268+22.89-L-",1,30000,30000]

{"sheet":"Items - Div 8","index":10,"n_rows":569,"n_cols":7,"rows_kept":569,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 8"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",22,284466.5,6258263]
["0000400000-N","CONST SURVEYING","","",4,123598.75,494395]
["0000700000-N","FIELD OFFICE","","",1,138690,138690]
["0000900000-N","GENERIC MISC ITEM (LS)","ALTERNAT LUMP SUM BID","FOR BRG 760056",1,808901.19,808901.19]
["","","","FOR BRG 820006",1,978338.42,978338.42]
["","","DESIGN & CONSTR OF","BRGS",1,3703965.18,3703965.18]
["","","","OF CLVT 610228",1,613870.69999999995,613870.69999999995]
["0000915000-N","GENERIC MISC ITEM (EA)","END BENTS STR 460023","",2,14007.68,28015.360000000001]
["","","END BENTS STR 460024","",2,13338.84,26677.68]
["","","END BENTS STR 460025","",2,13338.84,26677.68]
["","","END BENTS STR 460098","",2,13954.68,27909.360000000001]
["","","END BENTS STR 610030","",2,14502.4,29004.799999999999]
["","","END BENTS STR 610157","",2,21868.9,43737.8]
["","","END BENTS STR 610232","",2,24568,49136]
["","","END BENTS STR 760056","",null,null,0]
["","","END BENTS STR 760093","",2,13447.82,26895.64]
["","","END BENTS STR 760110","",2,13408.45,26816.9]
["","","END BENTS STR 820006","",null,null,0]
["","","END BENTS STR 820011","",2,17996.689999999999,35993.379999999997]
["","","INTERIOR BENT CAPS STR","610157",1,16838.25,16838.25]
["","","RIGHT OF WAY ACQUISIT","",26,4000,104000]
["0000930000-E","GENERIC MISC ITEM (LF)","AVE FOUND LENGTH AT END","BENT 1 STR 460023",65,209.52,13618.8]
["","","","BENT 1 STR 460024",62,219.66,13618.92]
["","","","BENT 1 STR 460025",66,206.34,13618.44]
["","","","BENT 1 STR 460098",65,223.42,14522.3]
["","","","BENT 1 STR 610030",14,366.68,5133.5200000000004]
["","","","BENT 1 STR 610157",16,320.85000000000002,5133.6000000000004]
["","","","BENT 1 STR 610232",15,342.24,5133.6000000000004]
["","","","BENT 1 STR 760093",18,326.99,5885.82]
["","","","BENT 1 STR 760110",16,367.87,5885.92]
["","","","BENT 1 STR 820011",95,281.39,26732.05]
["","","","BENT 2 STR 460023",65,209.52,13618.8]
["","","","BENT 2 STR 460024",60,214.44,12866.4]
["","","","BENT 2 STR 460025",67,214.49,14370.83]
["","","","BENT 2 STR 460098",65,223.42,14522.3]
["","","","BENT 2 STR 610030",15,342.24,5133.6000000000004]
["","","","BENT 2 STR 610157",15,342.24,5133.6000000000004]
["","","","BENT 2 STR 610232",15,342.24,5133.6000000000004]
["","","","BENT 2 STR 760093",15,342.24,5133.6000000000004]
["","","","BENT 2 STR 760110",15,342.24,5133.6000000000004]
["","","","BENT 2 STR 820011",95,281.49,26741.55]
["","","AVE FOUND LENGTH AT INTE-","RIOR BENT 1 STR 610157",25,2000,50000]
["","","BRG LENGTH STR 460023","",60,1886.47,113188.2]
["","","BRG LENGTH STR 460024","",55,1678.75,92331.25]
["","","BRG LENGTH STR 460025","",55,1678.75,92331.25]
["","","BRG LENGTH STR 460098","",65,1836.92,119399.8]
["","","BRG LENGTH STR 610030","",70,1812.86,126900.2]
["","","BRG LENGTH STR 610157","",130,3447.46,448169.8]
["","","BRG LENGTH STR 610232","",100,2792.16,279216]
["","","BRG LENGTH STR 760056","",null,null,0]
["","","BRG LENGTH STR 760093","",55,1731.32,95222.6]
["","","BRG LENGTH STR 760110","",50,1744.14,87207]
["","","BRG LENGTH STR 820006","",null,null,0]
["","","BRG LENGTH STR 820011","",60,1853.07,111184.2]
["0001000000-E","CLEARING & GRUBBING","","",229,17692.554585153001,4051595]
["0008000000-E","SUPP CLEAR & GRUBBING","","",11,6541.909090909,71961]
["0015000000-N","SEAL ABANDONED WELL","","",5,1763,8815]
["0022000000-E","UNCLAS EXCAV","","",3275100,3.6144850540000002,11837800]
["0029000000-N","REINF BRG APPR **********","(123+72.25 -L- LT)","",1,45303.3,45303.3]
["","","(123+72.25 -L- RT)","",1,45303.3,45303.3]
["","","(13+85.00)","",1,6500,6500]
["","","(17+45.00-L-)","",1,7400,7400]
["","","(20+03.00-L-)","",1,24536.92,24536.92]
["","","(29+73.05 -Y9 SBL-)","",1,90000,90000]
["","","(33+07.10 -Y10-)","",1,63000,63000]
["","","(339+69.19 -L- LT)","",1,51510,51510]
["","","(339+69.19 -L- RT)","",1,51510,51510]
["","","(34+10.49 -Y8 REV-)","",1,27000,27000]
["0030000000-N","BRG APP SUB REG TIER**","(15+64.50)","",1,9500,9500]
["","","(16+13.50)","",1,7000,7000]
["","","(16+29.00)","",1,14000,14000]
["0036000000-E","UNDERCUT EXCAV","","",34523,7,241661]
["0043000000-N","GRADING","","",6,104812.756666667,628876.54]
["0050000000-E","SUPP CLEAR & GRUBBING","","",5,1215.5999999999999,6078]
["0057000000-E","UNDERCUT EXCAV","","",1200,11.4375,13725]
["0106000000-E","BORROW EXCAV","","",14319,16.985948739000001,243221.8]
["0127000000-N","EMBM'T SETTLEMENT GAUGE","","",3,1250,3750]
["0134000000-E","DRNG DITCH EXCAV","","",30749,6.9476405740000002,213633]
["0141000000-E","BERM DITCH CONST","","",9300,2.158870968,20077.5]
["0156000000-E","REML OF EXT ASPH PVMT","","",186306,2.5877293269999999,482109.5]
["0177000000-E","BRKING OF EXT ASPH PVT","","",38700,2.368281654,91652.5]
["0192000000-N","PROOF ROLLING","","",141,171.631205674,24200]
["0194000000-E","SEL GRANUL MATL, CL III","","",4100,19.785365853999998,81120]
["0195000000-E","SEL GRANULAR MAT'L","","",49640,10.864423852,539310]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",128700,1.5935508940000001,205090]
["0199000000-E","TEMP SHORING","","",17119,46.594551084000003,797652.12]
["0223000000-E","ROCK PLATING","","",2465,47,115855]
["0241000000-E","GENERIC GRAD ITEM (SY)","SOIL NAIL SLOPE STABIL","",3500,162,567000]
["0255000000-E","GENERIC GRAD ITEM(TON)","AGG SHDR BORROW","",22199.66,16.306460098999999,361997.87]
["0262000000-N","GENERIC GRAD ITEM (EA)","SOIL NAIL PROOF TESTS","",25,500,12500]
["","","SOIL NAIL VERIFICATION ","TESTS",25,500,12500]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",14841,33.946804124000003,503804.52]
["0320000000-E","FND CONDIT GEOTEXTILE","","",27521,2.179510192,59982.3]
["0335200000-E","15\" DRNG PIPE","","",256,41.572968750000001,10642.68]
["0335300000-E","18\" DRNG PIPE","","",16,44,704]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",6,108.333333333,650]
["0342000000-E","**\" SIDE DRN PIPE","(30\")","",5656,48.633125884000002,275068.96000000002]
["","","(36\")","",2216,60.021660650000001,133008]
["","","(42\")","",1460,73.583643835999993,107432.12]
["","","(48\")","",112,92,10304]
["","","(6\")","",20,25,500]
["0343000000-E","15\" SIDE DRN PIPE","","",17006,22.541691168,383344]
["0344000000-E","18\" SIDE DRN PIPE","","",6336,27.181439394000002,172221.6]
["0345000000-E","24\" SIDE DRN PIPE","","",8704,33.325367647,290064]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",57,314.77192982499997,17942]
["","","(18\")","",7,275,1925]
["","","(24\")","",5,705.6,3528]
["","","(30\")","",2,1200,2400]
["0350000000-E","***\" RC PIPE CULV, CONTR DESIGN","(54\")","",356,320,113920]
["0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",1332,31,41292]
["","","(18\", V)","",224,36,8064]
["","","(24\", V)","",76,46,3496]
["","","(30\", V)","",132,61,8052]
["","","(36\", V)","",72,78,5616]
["","","(48\", V)","",64,124,7936]
["0360000000-E","12\" RC PIPE CULV III","","",168,22.889285714,3845.4]
["0366000000-E","15\" RC PIPE CULV III","","",10012,23.62407511,236524.24]
["0372000000-E","18\" RC PIPE CULV III","","",3804,26.982807570999999,102642.6]
["0378000000-E","24\" RC PIPE CULV III","","",5240,35.601526718000002,186552]
["0384000000-E","30\" RC PIPE CULV III","","",2872,48.872562674000001,140362]
["0390000000-E","36\" RC PIPE CULV III","","",2164,62.796025878000002,135890.6]
["0396000000-E","42\" RC PIPE CULV III","","",780,79.138461538000001,61728]
["0402000000-E","48\" RC PIPE CULV III","","",668,97.233532933999996,64952]
["0408000000-E","54\" RC PIPE CULV III","","",600,149,89400]
["0414000000-E","60\" RC PIPE CULV III","","",384,177,67968]
["0420000000-E","66\" RC PIPE CULV III","","",80,242,19360]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",104,103,10712]
["","","(54\")","",1080,178,192240]
["","","(60\")","",700,209.03428571399999,146324]
["","","(66\")","",220,292,64240]
["","","(84\")","",180,499,89820]
["0448200000-E","15\" RCP CULV CL IV","","",5028,22.184367542,111543]
["0448300000-E","18\" RCP CULV CL IV","","",532,32.127819549000002,17092]
["0448400000-E","24\" RCP CULV CL IV","","",328,43.487804877999999,14264]
["0448500000-E","30\" RCP CULV CL IV","","",844,54,45576]
["0448600000-E","36\" RCP CULV CL IV","","",120,67,8040]
["0448700000-E","42\" RCP CULV CL IV","","",216,110,23760]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",1248,28,34944]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",160,32,5120]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",262,36,9432]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",264,48,12672]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",34,289,9826]
["","","(18\", 0.064\")","",1,342.03,342.03]
["","","(24\", 0.064\")","",4,474,1896]
["","","(30\", 0.079\")","",4,579,2316]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(30\", 0.500\")","",104,316,32864]
["0995000000-E","PIPE REML","","",10325,10.718837772000001,110672]
["1000000000-E","6\" SLOPE PROTECTION","","",190,66,12540]
["1011000000-N","FINE GRADING","","",2,500000,1000000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",142490,2.35,334851.5]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",1430,213.18,304847.40000000002]
["1077000000-E","57 STONE","","",31,50,1550]
["1099500000-E","SHALLOW UNDERCUT","","",19300,8.2445595849999993,159120]
["1099700000-E","CL IV SUBGRD STABIL","","",36600,27.06557377,990600]
["1110000000-E","STABILIZER AGG","","",500,35,17500]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",113453,3.2644266790000001,370359]
["1121000000-E","AGG BASE COURSE","","",237800,25.437796467999998,6049108]
["1176000000-E","SOIL CEMENT BASE","","",142490,1.63,232258.7]
["1187000000-E","PC FOR SOIL CEM BASE","","",3920,130.56,511795.20000000001]
["1209000000-E","ASPH CURING SEAL","","",42750,2.15,91912.5]
["1220000000-E","INCIDENTAL STONE BASE","","",13049,29.343397962000001,382902]
["1231000000-E","SHDR BORROW","","",124506,4.9535636839999997,616748.4]
["1243000000-E","SHDR CONST","","",4.1399999999999997,1948.792270531,8068]
["1245000000-E","SHDR RECONST","","",376.18,1421.9702004359999,534916.75]
["1275000000-E","PRIME COAT","","",1952,5.4190573769999997,10578]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",457451,1.050742375,480663.15]
["","","(1-1/4\")","",1614,4.75,7666.5]
["","","(14\")","",3345,11.7,39136.5]
["","","(2\")","",61888,1.616969364,100071]
["","","(2-1/2\")","",103774,1.46,151510.04]
["","","(3\")","",9620,1.8,17316]
["1308000000-E","MILL ASPH PVMT ***** - ***","(0\" TO 1-1/2\")","",24625,1.965744162,48406.45]
["","","(0\" TO 2\")","",720,3.6,2592]
["","","(0\" TO 3\")","",32848,1.4,45987.199999999997]
["","","(0\" TO 4-1/2\")","",50908,2,101816]
["","","(1-1/2\" TO 3\")","",2650,2.4500000000000002,6492.5]
["","","(2-1/2\" TO 4\")","",400,8.5,3400]
["","","(3\" TO 6\")","",21138,2.7,57072.6]
["1330000000-E","INCIDENTAL MILLING","","",52883,6.0044087890000002,317531.15000000002]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",21518,42.874119342,922565.3]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",51812,35.054672662999998,1816252.7]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",24739,36.261530377,897074]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",115795,34.367329331999997,3979564.9]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",93772,39.735159216,3726045.35]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",196039,34.751797345999996,6812707.5999999996]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",153756,40.760663323999999,6267196.5499999998]
["1575000000-E","ASP FOR PLANT MIX","","",37492,534.72858209799995,20048044]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",970,146.64948453599999,142250]
["1704000000-E","PATCHING EXIST PVMT","","",15700,100.51337579600001,1578060]
["1771000000-E","AST, MAT COAT, 6M STONE","","",466555,1.1529539929999999,537916.44999999995]
["1814000000-E","AST, STRAIGHT SEAL","","",45310,1.1200000000000001,50747.199999999997]
["1840000000-E","MILLED RUMBLE STRIPS","","",124840,0.24326145499999999,30368.76]
["1880000000-E","GENERIC PAVING ITEM (TON)","STABILIZER AGG","",500,30,15000]
["2000000000-N","RIGHT OF WAY MKRS","","",561,178.02139037399999,99870]
["2022000000-E","SUBDRN EXCAV","","",7165,26.71653873,191424]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",8300,7.14,59262]
["2033000000-E","SUBDRN FINE AGG","","",2190,46.924657533999998,102765]
["2036000000-E","SUBDRN COARSE AGG","","",1395,71.400000000000006,99603]
["2044000000-E","6\" PERF SUBDRN PIPE","","",21300,13.359154930000001,284550]
["2070000000-N","SUBDRN PIPE OUTLET","","",44,361,15884]
["2077000000-E","6\" OUTLET PIPE","","",264,37.990909090999999,10029.6]
["2099000000-E","SHDR DRN","","",50800,6,304800]
["2110000000-E","4\" SHDR DRN PIPE","","",50800,1.6,81280]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",3200,6.5,20800]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",81,316,25596]
["2143000000-E","BLOTTING SAND","","",10,65,650]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",12,1446.5,17358]
["2209000000-E","ENDWALLS","","",60.4,963.67218543000001,58205.8]
["2220000000-E","REINF ENDWALLS","","",69.099999999999994,1024.461649783,70790.3]
["2253000000-E","PIPE COLLARS","","",4.2450000000000001,1131.3404004710001,4802.54]
["2264000000-E","PIPE PLUGS","","",3.5720000000000001,1034.9384098539999,3696.8]
["2275000000-E","FLOWABLE FILL","","",20.9,330.14832535900001,6900.1]
["2286000000-N","MASNRY DRNG STRUCT","","",604,1170.0654966889999,706719.56]
["2297000000-E","MASNRY DRNG STRUCT","","",71.647999999999996,1304.253014739,93447.12]
["2308000000-E","MASNRY DRNG STRUCT","","",348.44,277.24741705899999,96604.09]
["2354000000-N","FRM W/GRATE 840.22 STD","","",6,467,2802]
["2354200000-N","FRM W/GRATE 840.24 STD","","",3,401,1203]
["2355000000-N","FRM W/GRATE 840.29 STD","","",1,340,340]
["2364000000-N","FRM W/2GRTS 840.16 STD","","",27,455,12285]
["2364200000-N","FRM W/2GRTS 840.20 STD","","",61,460.31147541000001,28079]
["2365000000-N","FRM W/2GRTS 840.22 STD","","",351,463.20512820499999,162585]
["2366000000-N","FRM W/2GRTS 840.24 STD","","",78,467.17948717899998,36440]
["2367000000-N","FRM W/2GRTS 840.29 STD","","",48,474.89583333299998,22795]
["2374000000-N","FRM-GRT-HD 840.03 **","(E)","",2,473,946]
["","","(F)","",6,473,2838]
["","","(G)","",3,473,1419]
["2396000000-N","FRM W/COVR STD 840.54","","",16,405.4375,6487]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",27,561,15147]
["2484000000-E","GENERIC DRNG ITEM (LF)","SHDR BERM CURB","",10,58,580]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",2110,23,48530]
["2556000000-E","SHDR BERM GUTTER","","",19535,16.691425645999999,326067]
["2577000000-E","CONC EXPRESSWY GUTR","","",520,24.48,12729.6]
["2580000000-E","CONC VALLEY GUTTER","","",285,18.36,5232.6000000000004]
["2612000000-E","6\" CONC DRIVEWAY","","",170,61,10370]
["2619000000-E","4\" CONC PAVED DITCH","","",525,61.285714286000001,32175]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",4870,43.490759754000003,211800]
["2710000000-N","CONC BARR TRANS SECT","","",2,4420,8840]
["2717000000-E","VAR HT CONC BARR *****","(T1)","",1261,125,157625]
["","","(T2)","",117,303,35451]
["2752000000-E","GENERIC PAVING ITEM(LF)","SPECL SHDR BERM CURB","",15,25,375]
["2800000000-N","ADJ CATCH BASINS","","",4,489,1956]
["2815000000-N","ADJ DROP INLETS","","",8,629.75,5038]
["2830000000-N","ADJ MANHOLES","","",105,711.89523809499997,74749]
["2845000000-N","ADJ METER OR VAL BOX","","",65,595.4,38701]
["2905000000-N","CONVERT DI TO JB","","",2,2381,4762]
["2995000000-N","GENERIC DRNG ITEM (EA)","CONV EXT TRAF BEARING DROP INLET TO TRAFF","BEARING JUNC-TION BOX",1,1578,1578]
["3030000000-E","STL BM GRDRL","","",42462.5,14.51195761,616214]
["3045000000-E","SBGR SHOP CURVED","","",600,16.079166666999999,9647.5]
["3105000000-N","SBGR TERM SECT","","",4,45.9,183.6]
["3150000000-N","ADDIT GRDRL POSTS","","",243,41.552263373999999,10097.200000000001]
["3165000000-N","GR ANCHOR  **********","(350 TL-2)","",1,1600,1600]
["","","(350, TL-2)","",1,1683,1683]
["3195000000-N","GR ANCHOR  AT-1","","",4,443.625,1774.5]
["3210000000-N","GR ANCHOR  CAT-1","","",49,439.91836734700001,21556]
["3215000000-N","GR ANCHOR  III","","",20,1425,28500]
["3270000000-N","GR ANCHOR  350","(350 TL-3)","",4,1775,7100]
["","","","",116,1848.1120689659999,214381]
["3285000000-N","GR ANCHOR  M-350","","",10,1650.56,16505.599999999999]
["3317000000-N","GR ANCHOR  B-77","","",32,1457.875,46652]
["3360000000-E","REM EXT GRDRL","","",18119,1.0648374629999999,19293.79]
["3380000000-E","TEMP STL BM GRDRL","","",11250,4.4431111110000003,49985]
["3387000000-N","TEMP GDRL ANCH UNIT****","(CAT-1)","",13,105,1365]
["","","(III)","",4,850,3400]
["3389100000-N","TEMP GDRL ANCH UNITS 350","","",25,732.16,18304]
["3389400000-E","DBL FACED CABLE GUIDERAIL","","",14830,6.84,101437.2]
["3389500000-N","ADDITIL GUIDERAIL POSTS","","",40,47,1880]
["3389600000-N","CBL GUIDERAIL ANC UNIT","","",14,1894,26516]
["3435000000-N","GENERIC GRDRL ITEM(EA)","IMPACT ATTENUATR UNIT"," 350 (TEMP)",1,12000,12000]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",120780,2.2247797650000001,268708.90000000002]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",7628,14.939570005,113959.03999999999]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",1853,28.159352402,52179.28]
["3557000000-E","ADDITIONAL BARB WIRE","","",1300,0.376923077,490]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 16', 16')","",1,459,459]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 24')","",2,867,1734]
["3595000000-E","RELAPPING GRDRL","","",3600,3.2,11520]
["3628000000-E","RIP RAP, CL I","","",8087,45.782119451,370240]
["3635000000-E","RIP RAP, CL II","","",208,59.423076923000004,12360]
["3649000000-E","RIP RAP, CL B","","",2611,44.303332056999999,115676]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",50406,2.0430952659999999,102984.26]
["3659000000-N","PREFORM SCOUR HOLES","","",1,2000,2000]
["4048000000-E","REINF CONC FOUNDTN","","",12,1000,12000]
["4054000000-E","PLN CONC FOUNDTN","","",1,474,474]
["4057000000-E","OVERHEAD FOOTING","","",84,1000,84000]
["4060000000-E","SUPPT, BRKAWY STL BM","","",9560,4.1500000000000004,39674]
["4072000000-E","SUPPT, 3-LB STL U-CHAN","","",8658,4.768485793,41285.550000000003]
["4082100000-N","SUPPT, OVRHD SIGN STR*","(11+00 -Y9NBL)","",1,43477,43477]
["","","(38+00 -Y9NBL)","",1,46132,46132]
["","","(425+00 -L-)","",1,76117,76117]
["","","(435+00 -L-)","",1,43677,43677]
["","","(451+25 -L-)","",1,76117,76117]
["","","(464+00 -L-)","",1,58463,58463]
["","","(476+90 -L-)","",1,42517,42517]
["4096000000-N","SIGN ERECTION,  D","","",34,77.441176471000006,2633]
["4102000000-N","SIGN ERECTION,  E","","",341,51.419941348999998,17534.2]
["4108000000-N","SIGN ERECTION,  F","","",72,77.020833332999999,5545.5]
["4110000000-N","SIGN ERECTION,  *** (GRD MTD)","(A)","",7,500,3500]
["","","(B)","",5,394,1970]
["4114000000-N","SIGN ERECTN, MILEMKRS","","",6,58,348]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",4,164.375,657.5]
["4152000000-N","DISP SIGN SYST STL BM","","",4,157,628]
["4155000000-N","DISP SIGN SYST U-CHAN","","",228,2.00877193,458]
["4192000000-N","DISPOSE SUPPT, U-CHAN","","",1,1,1]
["4238000000-N","DISPOSE SIGN, D, E, F","","",3,5.0999999999999996,15.3]
["4360000000-N","GENERIC SIGNING ITEM (EA)","DISP OF SIGN SYSTEM ON SPAN WIRE","",1,220,220]
["4400000000-E","WORK ZONE SIGN (STAT)","","",7587,5.9749110319999996,45331.65]
["4405000000-E","WORK ZONE SIGN (PORT)","","",3058,9.0612164810000007,27709.200000000001]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",2645,9.3224763710000005,24657.95]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",26439,3.5953439989999998,95057.3]
["4415000000-N","FLASH ARROW BOARD","","",8,2328.16,18625.28]
["4420000000-N","PORT CHANGE MSG SIGN","","",11,7369.8909090910001,81068.800000000003]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",98,26.061224490000001,2554]
["4430000000-N","DRUMS","","",1964,51.873727088000003,101880]
["4435000000-N","CONES","","",220,33.681818182000001,7410]
["4445000000-E","BARRICADES ( III)","","",5746,50.37974243,289482]
["4450000000-N","FLAGGER","","",2264,21.473498233000001,48616]
["4455000000-N","FLAGGER","","",270,210.555555556,56850]
["4457000000-N","TEMP TRAFFIC CNTRL","","",13,19576.923076923002,254500]
["4465000000-N","TEMP CRASH CUSHIONS","","",9,6583.3333333330002,59250]
["4470000000-N","RESET CRASH CUSHION","","",10,2216.4,22164]
["4480000000-N","TMA","","",7,10995,76965]
["4485000000-E","PORT CONC BARR","","",5020,21.256573705000001,106708]
["4500000000-E","RESET PORT CONC BARR","","",4470,4.2120134230000001,18827.7]
["4510000000-N","LAW ENFORCEMENT","","",1669,35.158777710999999,58680]
["4516000000-N","SKINNY DRUM","","",210,41.190476189999998,8650]
["4520000000-N","TUBULAR MKRS (FIXED)","","",12,90,1080]
["4650000000-N","TEMP RAISED PVMT MRKS","","",4911,4.5086214619999998,22141.84]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",947531,0.48438226299999998,458967.21]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",626311,0.61580495999999996,385685.42]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",339540,0.802771397,272573]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",45910,0.90130690499999999,41379]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",23069,1.438336295,33180.980000000003]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",2557,2.9276495890000001,7486]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",11040,1.4339673909999999,15831]
["4705000000-E","THERMO LINES 16\" 120MILS","","",1225,5.4693877549999996,6700]
["4710000000-E","24\"WIDE THERMO 120 MIL","","",6660,7.7573678680000002,51664.07]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",202,83.057425742999996,16777.599999999999]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",754,103.02122015899999,77678]
["4770000000-E","4\" COLD APPL PLSTIC LINES  **","(II)","",728,2,1456]
["","","(III)","",5220,2.954980843,15425]
["","","(IV)","",1729,1.848756507,3196.5]
["4780000000-E","8\" COLD APPL PLSTIC LINES  **","(II)","",120,6.5,780]
["4810000000-E","PAINT PVMT MKGS 4\"","","",7379817,0.117490118,867055.57]
["4820000000-E","PAINT PVMT MKGS 8\"","","",24491,0.57910252699999998,14182.8]
["4825000000-E","PAINT PVMT MKGS 12\"","","",1600,0.77,1232]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",50,4,200]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",5744,3.2442200560000001,18634.8]
["4840000000-N","PAINT PVT MKG CHAR","","",38,35.642105262999998,1354.4]
["4845000000-N","PAINT PVT MKG SYMBOL","","",937,33.357203841999997,31255.7]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",2678,1.35,3615.3]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",3799,2.0270071070000002,7700.6]
["4850000000-E","LINE REML 4\" WIDE","","",37176,0.55882101399999995,20774.73]
["4860000000-E","LINE REML 8\" WIDE","","",700,1.02,714]
["4870000000-E","LINE REML 24\" WIDE","","",165,3.06,504.9]
["4900000000-N","PERM RAISED PVMT MKRS","","",5978,5.260833055,31449.26]
["4905000000-N","SNOWPLB PVMT MRKER","","",8190,26.172738706000001,214354.73]
["4915000000-E","7' U-CHANNEL POSTS","","",18,38.375,690.75]
["4935000000-N","FLEX DELINTR (CRYSTAL)","","",44,68,2992]
["4940000000-N","FLEX DELINATR(YELLOW)","","",38,68,2584]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",5,68,340]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",5,68,340]
["4955000000-N","OBJECT MKR (END OF RD)","","",18,97.125,1748.25]
["5255000000-N","PORTABLE LIGHTING","","",2,12000,24000]
["5325000000-E","**\" WATER LINE","(14\")","",150,61.2,9180]
["","","(18\")","",407,81.599999999999994,33211.199999999997]
["5325200000-E","2\" WATER LINE","","",3004,20.399999999999999,61281.599999999999]
["5325400000-E","4\" WATER LINE","","",161,35.700000000000003,5747.7]
["5325600000-E","6\" WATER LINE","","",3303,40.432152588999998,133547.4]
["5325800000-E","8\" WATER LINE","","",1067,56.770121836999998,60573.72]
["5326200000-E","12\" WATER LINE","","",5391,51,274941]
["5326600000-E","16\" WATER LINE","","",6272,66.3,415833.59999999998]
["5327000000-E","20\" WATER LINE","","",2164,91.8,198655.2]
["5536000000-E","2\" VALVE","","",11,663,7293]
["5538000000-E","4\" VALVE","","",1,765,765]
["5540000000-E","6\" VALVE","","",15,1027.3333333329999,15410]
["5546000000-E","8\" VALVE","","",5,1259.2,6296]
["5558000000-E","12\" VALVE","","",11,2244,24684]
["5558600000-E","16\" VALVE","","",7,4386,30702]
["5559000000-E","20\" VALVE","","",2,6120,12240]
["5589100000-E","1\" AIR RELEASE VALVE","","",10,2346,23460]
["5589200000-E","2\" AIR RELEASE VALVE","","",3,3162,9486]
["5606000000-E","2\" BLOW OFF","","",7,1224,8568]
["5648000000-N","RELOCATE WATER METER","","",38,532.10526315799996,20220]
["5649000000-N","RECONNECT H2O METER","","",4,382.5,1530]
["5666000000-E","FIRE HYDRANT","","",7,4080,28560]
["5672000000-N","RELOCATE FIRE HYDRANT","","",9,2550,22950]
["5709100000-E","2\" FORCE MAIN SEWER","","",747,20.399999999999999,15238.8]
["5709300000-E","6\" FORCE MAIN SEWER","","",6532,25.5,166566]
["5709400000-E","8\" FORCE MAIN SEWER","","",450,45.9,20655]
["5775000000-E","4' DIA UTILITY MANHOLE","","",3,2040,6120]
["5781000000-E","UTILITY MH WALL, 4' DIA","","",4.9000000000000004,193.8,949.62]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",794,8.16,6479.04]
["5804000000-E","ABANDN 12\" UTILITY PIPE","","",5492,12.24,67222.080000000002]
["5810000000-E","ABANDN 16\" UTILITY PIPE","","",6690,15.3,102357]
["5812000000-E","ABANDN 20\" UTILITY PIPE","","",2280,17.34,39535.199999999997]
["5816000000-N","ABAND UTILITY MANHOLE","","",3,1428,4284]
["5871400000-E","6\" TRENCHLESS INSTALL (IN SOIL)","","",535,38,20330]
["5871410000-E","6\" TRENCHLESS INSTALL (NOT IN SOIL)","","",60,38,2280]
["5871500000-E","8\" TRENCHLESS INSTALL (IN SOIL)","","",348,151.33620689700001,52665]
["5871510000-E","8\" TRENCHLESS INSTALL (NOT IN SOIL)","","",347,151.61383285299999,52610]
["5871800000-E","14\" TRENCHLESS INSTALL (IN SOIL)","","",75,357,26775]
["5871810000-E","14\" TRENCHLESS INSTALL (NOT IN SOIL)","","",75,357,26775]
["5872000000-E","18\" TRENCHLESS INSTALL (IN SOIL)","","",203.5,459,93406.5]
["5872010000-E","18\" TRENCHLESS INSTALL (NOT IN SOIL)","","",203.5,459,93406.5]
["5882000000-N","GENERIC UTILITY ITEM(EA)","RELOC H2O METER WITH ","NEW VAULT",2,3060,6120]
["5912000000-N","GENERIC UTILITY ITEM(LS)","REM LIFT STATION","",1,3060,3060]
["6000000000-E","TEMP SILT FENCE","","",121402,1.5666204020000001,190190.85]
["6006000000-E","EROS CNTRL STONE CL A","","",26205,42.727994658,1119687.1000000001]
["6009000000-E","EROS CNTRL STONE CL B","","",50660,42.321950256999997,2144030]
["6012000000-E","SEDIMENT CNTRL STONE","","",36685,38.192818590999998,1401103.55]
["6015000000-E","TEMP MULCHING","","",1229.9000000000001,768.61535897199997,945320.03]
["6018000000-E","SEED FOR TEMP SEEDING","","",133200,0.66447447400000004,88508]
["6021000000-E","FERT FOR TEMP SEEDING","","",556.5,484.06788858900001,269383.78000000003]
["6024000000-E","TEMP SLOPE DRNS","","",32150,10.250139968999999,329542]
["6029000000-E","SAFETY FENCE","","",37925,1.188529993,45075]
["6030000000-E","SILT EXCAV","","",179600,3.127621381,561720.80000000005]
["6036000000-E","MAT FOR EROS CNTRL","","",525750,1.2349595819999999,649280]
["6037000000-E","COIR FIBER MAT","","",12670,4.7300710339999998,59930]
["6038000000-E","PERM SOIL REINF MAT","","",54675,5.9455875630000001,325075]
["6042000000-E","1/4\" HARDWARE CLOTH","","",22995,2.672972385,61465]
["6045000000-E","**\" TEMP PIPE","(15\")","",20,50,1000]
["","","(24\")","",465,35,16275]
["","","(36\")","",355,55,19525]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",260,50,13000]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",630,41.194444443999998,25952.5]
["6069000000-E","STILLING BASINS","","",2325,30.645161290000001,71250]
["6070000000-N","SPECIAL STILLING BASINS","","",92,364.89260869600002,33570.120000000003]
["6071010000-E","WATTLE","","",24575,2.744174975,67438.100000000006]
["6071012000-E","COIR FIBER WATTLE","","",26700,8.1481273410000004,217555]
["6071013000-E","WATTLE BARR","","",100,14,1400]
["6071014000-E","COIR FIBR WATTLE BARR","","",200,5,1000]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",28260,6.4998938429999997,183687]
["6071030000-E","COIR FIBER BAFFLE","","",19930,5.3143251380000001,105914.5]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",181,760.56839778999995,137662.88]
["","","(2\")","",16,1100,17600]
["","","(2-1/2\")","",1,1500,1500]
["6084000000-E","SEEDING & MULCHING","","",835.52,1469.236224148,1227576.25]
["6087000000-E","MOWING","","",504.9,76.387403445999993,38568]
["6090000000-E","SEED FOR REPAIR SEED","","",11050,2.8776470590000001,31798]
["6093000000-E","FERT FOR REPAIR SEED","","",30.75,896.07317073199999,27554.25]
["6096000000-E","SEED FOR SUPP SEEDING","","",16175,3.1063060280000001,50244.5]
["6108000000-E","FERTILIZER TOPDRESSING","","",482.75,909.84277576399995,439226.6]
["6111000000-E","IMPERVIOUS DIKE","","",720,50.888888889,36640]
["6114500000-N","SPECIALIZED HAND MOW","","",265,49.905660376999997,13225]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",372,320.02284946200001,119048.5]
["6120000000-E","CLVT DIVERSION CHANL","","",1710,50.368421052999999,86130]
["6123000000-E","REFORESTATION","","",20.100000000000001,1091.5422885569999,21940]
["6126000000-E","STRMBNK REFORESTATN","","",0.25,816,204]
["6129000000-E","WETLAND REFORESTATN","","",0.34,5000,1700]
["6135000000-E","GENERIC EROSION CNTRL ITEM (ACR)","DISKING","",0.34,400,136]
["","","RIPPING","",0.34,400,136]
["7060000000-E","SIGNAL CABLE","","",3475,2.5499999999999998,8861.25]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",21,714,14994]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",5,867,4335]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",1,1224,1224]
["7264000000-E","MESSENGER CABLE (3/8\")","","",500,3.06,1530]
["7300000000-E","UNPAVED TRENCH (*******)","(1, 2\")","",2075,5.0999999999999996,10582.5]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",425,14.28,6069]
["","","(2, 2\")","",235,14.79,3475.65]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",35,204,7140]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",24655,5.0110525250000002,123547.5]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",6400,1.21703125,7789]
["7566000000-N","DELINEATOR MKR","","",2,102,204]
["7575142000-N","900MHZ RADIO","","",2,3570,7140]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",4,6961.5,27846]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",1,8868.9,8868.9]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,13244.7,26489.4]
["7613000000-N","SOIL TEST","","",7,816,5712]
["7614100000-E","DRILLED PIER FOUND","","",42,714,29988]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",3,102,306]
["7636000000-N","SIGN FOR SIGNALS","","",6,306,1836]
["7642200000-N"," II PED W/ FOUND","","",3,1555,4665]
["7684000000-N","SIGNAL CABINET FOUND","","",4,816,3264]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",4,10710,42840]
["7780000000-N","DETECTOR CARD ( 2070L)","","",14,86.7,1213.8]
["7901000000-N","CABINET BASE EXTENDER","","",4,206,824]
["8007000000-N","CM&R TEMP STR ***********","(20+03.00-L-)","",1,266160,266160]
["8017000000-N","CM&R TEMP ACCESS******","(20+03.00-L-)","",1,1.07,1.07]
["","","(339+48.56-L-EBL)","",1,45900,45900]
["","","(339+48.56-L-WBL)","",1,45900,45900]
["8035000000-N","REMV EXIST STR **********","(13+85.00-L-)","",1,35800,35800]
["","","(15+64.50-L-)","",1,48000,48000]
["","","(16+13.50 -L-)","",1,14350,14350]
["","","(16+29.00-L-)","",1,20000,20000]
["","","(17+45.00-L-)","",1,32000,32000]
["","","(339+48.56-L-EBL)","",1,132600,132600]
["8049000000-N","REMV EXIST STR **********","(20+03.00-L-)","",1,76810,76810]
["8056000000-N","REMV EXIST STR **********","(509+83.00-L-)","",1,11000,11000]
["","","(53+95.00-L-)","",1,10200,10200]
["","","(73+25 -L- LT)","",1,10000,10000]
["","","(77+04.00-L-)","",1,10200,10200]
["8091000000-N","FND EXCAV B** STA *****","(1, 378+94.34-L-)","",1,6000,6000]
["","","(1, 456+99.33-L-)","",1,14000,14000]
["","","(395+64.54-L-)","",1,39000,39000]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",108.75,750.97241379299999,81668.25]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",261,1137.3,296835.3]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",102,1420.3921568630001,144880]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",366,1137.5999999999999,416361.6]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",91.5,96.06557377,8790]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",30.2,698.7,21100.74]
["8112730000-N","PDA TESTING","","",9,3300,29700]
["8113000000-N","SID INSPECTIONS","","",10,508,5080]
["8114000000-N","SPT TESTING","","",1,1000,1000]
["8115000000-N","CSL TESTING","","",11,2527.2727272729999,27800]
["8121000000-N","UNCL STR EXCAV STA****","(13+85.00-L-)","",1,6700,6700]
["","","(15+64.50-L-)","",1,19500,19500]
["","","(16+13.50 -L-)","",1,5000,5000]
["","","(16+29.00-L-)","",1,6500,6500]
["","","(17+45.00-L-)","",1,2800,2800]
["","","(20+03.00-L-)","",1,3386,3386]
["","","(339+48.56-L-EBL)","",1,30600,30600]
["","","(339+48.56-L-WBL)","",1,7650,7650]
["8126000000-N","CULV EXCAV @ **********","(188+02.00-L-)","",1,30600,30600]
["","","(204+38.00-L-)","",1,35700,35700]
["","","(283+62.00-L-)","",1,45900,45900]
["","","(509+83.00-L-)","",1,64000,64000]
["","","(53+95.00-L-)","",1,57120,57120]
["","","(77+04.00-L-)","",1,51000,51000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",2343,48.538198889999997,113725]
["8147000000-E","REINF CONC DECK SLAB","","",92859,26.447856751,2455921.5299999998]
["8161000000-E","GROOVING BRG FLOORS","","",91369,0.49833368,45532.25]
["8182000000-E","CL A CONC (BRG)","","",1631.6,875.143184604,1427883.62]
["8196000000-E","CL A CONC (CULV)","","",3369,431.15958741499998,1452576.65]
["8210000000-N","BRG APPR SLAB ***********","(123+82.50-L-EBL)","",1,30426.6,30426.6]
["","","(123+82.50-L-WBL)","",1,30600,30600]
["","","(13+85.00-L-)","",1,16850,16850]
["","","(15+64.50-L-)","",1,8300,8300]
["","","(16+13.50 -L-)","",1,19000,19000]
["","","(16+29.00-L-)","",1,16240,16240]
["","","(17+45.00-L-)","",1,16900,16900]
["","","(20+03.00-L-)","",1,39220.47,39220.47]
["","","(339+48.56-L-EBL)","",1,29580,29580]
["","","(339+48.56-L-WBL)","",1,29580,29580]
["","","(378+94.34-L-)","",1,20000,20000]
["","","(395+64.54-L-)","",1,80000,80000]
["","","(456+99.33-L-)","",1,34000,34000]
["8217000000-E","REINF STEEL (BRG)","","",368309,0.96809130399999999,356556.74]
["8238000000-E","SPIRL COL REINF STL BRG","","",40211,1.7540543630000001,70532.28]
["8245000000-E","REINF STEEL (CLVT)","","",360964,1.028442061,371230.56]
["8259000000-E","36\" PRESTR CONC GIRDR","","",887.5,131.03000563399999,116289.13]
["8265000000-E","54\" PRESTR CONC GIRDR","","",1999.33,188.69999949999999,377273.57]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",836,222,185592]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",2472,275.39999999999998,680788.8]
["8280000000-E","STRUCTURAL STEEL","","",1067000,1.567010309,1672000]
["8364000000-E","HP12X53 PILES","","",9160,48.177658297000001,441307.35]
["8384000000-E","HP14X73 PILES","","",2425,56.1,136042.5]
["8384200000-E","HP14X73 GALV PILES","","",2470,59.861659918999997,147858.29999999999]
["8391000000-N","STEEL PILE POINTS","","",81,232.34567901200001,18820]
["8393000000-N","PILE REDRIVES","","",144,86.265277777999998,12422.2]
["8475000000-E","TWO BAR METAL RAIL","","",634.75,118.924789287,75487.509999999995]
["8503000000-E","CONC BARR RAIL","","",4133.21,67.792284930999998,280199.75]
["8505000000-E","VERT CONC BARR RAIL","","",470.75,78.720361126,37057.61]
["8510000000-E","CONC MEDIAN BARR","","",304.83,61,18594.63]
["8517000000-E","1'-**\"X****\"CONC PARAPET","(1'-2\" X 2'-10\")","",250.52,68.599992017000005,17185.669999999998]
["","","(1'-2\" X 2'-9\")","",150.25,90.32,13570.58]
["","","(16+29.00-L-)","",280.26,100,28026]
["8531000000-E","4\" SLOPE PROTECTION","","",2762,81,223722]
["8608000000-E","RIP RAP II (2'-0\")","","",7512,39.147075346000001,294072.83]
["8622000000-E","GEOTEXTILE FOR DRNG","","",8347,2.1780040729999999,18179.8]
["8657000000-N","ELASTOMERIC BEARINGS","","",8,11888.85,95110.8]
["8692000000-N","FOAM JOINT SEALS","","",1,13000,13000]
["8706000000-N","EXPANSION JOINT SEALS","","",1,108000,108000]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",1540,210,323400]
["8755000000-E","3'-0\"X 1'-6\"PRESTR SLABS","","",825,139.81,115343.25]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",2485,125.09657947700001,310865]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLAB","","",1360,146.76470588199999,199600]
["8847000000-E","GENERIC RET WALL ITEM (SF)","SOUND BARR WALL","",24362,28,682136]
["8860000000-N","GENERIC STR ITEM (LS)","DISC BEARINGS","",1,40000,40000]

{"sheet":"Items - Div 9","index":11,"n_rows":580,"n_cols":7,"rows_kept":580,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 9"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",8,959230,7673840]
["0000400000-N","CONST SURVEYING","","",3,594448.33333333302,1783345]
["0000700000-N","FIELD OFFICE","","",1,85907.36,85907.36]
["0001000000-E","CLEARING & GRUBBING","","",185,5135.1351351350004,950000]
["0008000000-E","SUPP CLEAR & GRUBBING","","",5,4500,22500]
["0015000000-N","SEAL ABANDONED WELLS","","",29,1076.24,31210.959999999999]
["0022000000-E","UNCLAS EXCAV","","",3571000,4.38,15640980]
["0029000000-N","REINF BRG APPR **********","(17+1018-Y4RPA-)","",1,33325.07,33325.07]
["","","(20+2021-Y2-)","",1,24520.42,24520.42]
["","","(23+5425-Y5-)","",1,30113.53,30113.53]
["","","(26+4862-Y4RPBD-)","",1,23124.11,23124.11]
["","","(28+7585-Y5-)","",1,25832.639999999999,25832.639999999999]
["","","(33+1649-Y4CD-)","",1,22395.83,22395.83]
["","","(34+0868-Y1-)","",1,65194.06,65194.06]
["","","(44+1864-Y4RPBD-)","",1,39884.57,39884.57]
["","","(46+8344-Y4CD-)","",1,33412.19,33412.19]
["","","(53+2116-Y4RPBD-)","",1,32401.61,32401.61]
["","","(556+8500-L-LT)","",1,39353.58,39353.58]
["","","(556+8500-L-RT)","",1,39353.58,39353.58]
["","","(584+1777-L-LT)","",1,56961.25,56961.25]
["","","(584+2418-L-RT)","",1,56961.25,56961.25]
["","","(628+5775-L-RT)","",1,51286.93,51286.93]
["","","(628+7447-L-LT)","",1,51286.93,51286.93]
["","","(642+7524-L-LT)","",1,42406.89,42406.89]
["","","(642+8018-L-RT)","",1,52477.65,52477.65]
["0030000000-N","BRG APP SUB REG TIER**","(14+6600-L-)","",1,17160,17160]
["","","(18+6650 -L-)","",1,10950,10950]
["","","(20+9200)","",1,10000,10000]
["0036000000-E","UNDERCUT EXCAV","","",7500,20.29,152175]
["0043000000-N","GRADING","","",1,116450,116450]
["0050000000-E","SUPP CLEARING & GRUBBING","","",3,34,102]
["0057000000-E","UNDERCUT EXCAV","","",1200,9,10800]
["0063000000-N","GRADING","","",2,190085,380170]
["0106000000-E","BORROW EXCAV","","",2937355,4.1685800659999996,12244599.5]
["0134000000-E","DRNG DITCH EXCAV","","",31035,2.9036571609999999,90115]
["0141000000-E","BERM DITCH CONST","","",2860,8.49,24281.4]
["0156000000-E","REML OF EXT ASPH PVMT","","",87000,2.4900000000000002,216630]
["0177000000-E","BRKING OF EXT ASPH PVT","","",18000,2.4900000000000002,44820]
["0192000000-N","PROOF ROLLING","","",120,204.53,24543.599999999999]
["0195000000-E","SEL GRANULAR MAT'L","","",24500,6.8681632649999997,168270]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",49200,1.494410569,73525]
["0199000000-E","TEMP SHORING","","",6000,23.22,139320]
["0220000000-E","ROCK EMBANKMENTS","","",1000,13.6,13600]
["0222000000-E","GEOTEXTILE ROCK EMBNK","","",820,1.55,1271]
["0223000000-E","ROCK PLATING","","",3650,79.173972602999996,288985]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",6936,37.449002307000001,259746.28]
["0320000000-E","FND CONDIT GEOTEXTILE","","",23386,2.3738937830000002,55515.88]
["0335200000-E","15\" DRNG PIPE","","",64,35.625,2280]
["0335300000-E","18\" DRNG PIPE","","",240,30,7200]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",6,150,900]
["0342000000-E","**\" SIDE DRN PIPE","(30\")","",4352,46.21,201105.92000000001]
["","","(36\")","",864,62.87,54319.68]
["","","(42\")","",2172,76.75,166701]
["","","(48\")","",52,138.59,7206.68]
["","","(54\")","",84,371.66,31219.439999999999]
["","","(60\")","",604,198.4,119833.60000000001]
["0343000000-E","15\" SIDE DRN PIPE","","",12456,25.96300578,323395.20000000001]
["0344000000-E","18\" SIDE DRN PIPE","","",6184,27.568952135,170486.39999999999]
["0345000000-E","24\" SIDE DRN PIPE","","",4348,44.57,193790.36]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",72,281.88,20295.36]
["","","(18\")","",20,364.94,7298.8]
["","","(24\")","",7,493.7,3455.9]
["","","(30\")","",7,617.13,4319.91]
["","","(36\")","",2,740.55,1481.1]
["0350000000-E","***\" RC PIPE CULV CONTR DESIGN","(18\")","",484,21.95,10623.8]
["","","(36\")","",380,78.03,29651.4]
["","","(42\")","",1308,93.45,122232.6]
["","","(48\")","",1276,110.3,140742.79999999999]
["","","(60\")","",308,179.73,55356.84]
["0354000000-E","***\" RC PIPE CULV *****","(24\" V)","",408,59.85,24418.799999999999]
["","","(30\" V)","",460,72.52,33359.199999999997]
["","","(36\" V)","",472,90.41,42673.52]
["","","(54\" V)","",368,179.71,66133.279999999999]
["","","(72\" V)","",324,279.60000000000002,90590.399999999994]
["0366000000-E","15\" RC PIPE CULV III","","",4292,23.66,101548.72]
["0372000000-E","18\" RC PIPE CULV III","","",2736,23.896359649000001,65380.44]
["0378000000-E","24\" RC PIPE CULV III","","",1080,46.27,49971.6]
["0384000000-E","30\" RC PIPE CULV III","","",1064,55.29,58828.56]
["0390000000-E","36\" RC PIPE CULV III","","",380,76.38,29024.400000000001]
["0396000000-E","42\" RC PIPE CULV III","","",104,86.88,9035.52]
["0402000000-E","48\" RC PIPE CULV III","","",124,134.84,16720.16]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",528,121.91,64368.480000000003]
["","","(60\")","",1020,190.54,194350.8]
["0448200000-E","15\" RCP CULV CL IV","","",3812,29.012434418000002,110595.4]
["0448300000-E","18\" RCP CULV CL IV","","",1540,29.2,44968]
["0448400000-E","24\" RCP CULV CL IV","","",404,47.08,19020.32]
["0448500000-E","30\" RCP CULV CL IV","","",880,55.14,48523.199999999997]
["0448700000-E","42\" RCP CULV CL IV","","",504,90.58,45652.32]
["0576000000-E","**\" CS PIPE CULV *****\"","(36\" 0079\")","",172,74.22,12765.84]
["","","(42\" 0109\")","",28,115.28,3227.84]
["","","(54\" 0109\")","",260,142.03,36927.800000000003]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",1284,22.531090342999999,28929.919999999998]
["0588000000-E","18\" CS PIPE CULV 0064\"","","",588,41.12,24178.560000000001]
["0594000000-E","24\" CS PIPE CULV 0064\"","","",368,34.24,12600.32]
["0600000000-E","30\" CS PIPE CULV 0079\"","","",164,71.31,11694.84]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\" 0064\")","",12,103.408333333,1240.9000000000001]
["","","(18\" 0064\")","",3,147.16999999999999,441.51]
["","","(24\" 0064\")","",2,222.56,445.12]
["","","(42\" 0109\")","",1,476.47,476.47]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(36\" 0500\")","",227,438.09,99446.43]
["","","(42\" 0625\")","",348,526.79999999999995,183326.4]
["","","(48\" 0625\")","",180,708.8,127584]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(36\" 0500\")","",227,1188.0899999999999,269696.43]
["","","(42\" 0625\")","",348,1166.8,406046.4]
["","","(48\" 0625\")","",180,1248.8,224784]
["0986000000-E","GENERIC PIPE ITEM (LF)","8\" DUCTILE IRON PIPE","",548,36,19728]
["0995000000-E","PIPE REML","","",4969,14.117669551000001,70150.7]
["1000000000-E","6\" SLOPE PROTECTION","","",800,65,52000]
["1011000000-N","FINE GRADING","","",1,3500000,3500000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",130610,2.4,313464]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",1380,198.5,273930]
["1077000000-E","57 STONE","","",505,25,12625]
["1099500000-E","SHALLOW UNDERCUT","","",5400,14.437037037,77960]
["1099700000-E","CL IV SUBGRD STABIL","","",10290,23.577259475000002,242610]
["1110000000-E","STABILIZER AGG","","",1000,24,24000]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",275035,2.4500000000000002,673835.75]
["1121000000-E","AGG BASE COURSE","","",90837,33.278234640000001,3022895]
["1176000000-E","SOIL CEM BASE","","",195910,2.2999999999999998,450593]
["1187000000-E","PC FOR SOIL CEM BASE","","",5486,136.5,748839]
["1209000000-E","ASPH CURING SEAL","","",48980,3.25,159185]
["1220000000-E","INCIDENTAL STONE BASE","","",9733,16.132127813,157014]
["1245000000-E","SHOULDER RECONST","","",186,1834.0836021509999,341139.55]
["1275000000-E","PRIME COAT","","",2240,3.55,7952]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",973,6.5034943470000002,6327.9]
["","","(1-1/2\")","",142300,1.305971609,185839.76]
["","","(3\")","",90593,1.65,149478.45000000001]
["1308000000-E","MILLN ASPH PVMT ***** - *****","(0\" TO 1-1/2\")","",64390,1.219833049,78545.05]
["","","(0\" TO 2\")","",10757,1.2,12908.4]
["","","(1-1/2\" TO 2-1/2\")","",2000,2.4,4800]
["","","(1-1/2\" TO 3-1/2\")","",41710,1.52,63399.199999999997]
["1330000000-E","INCIDENTAL MILLING","","",39230,4.5180869230000003,177244.55]
["1489000000-E","ASP CNC BAS CRS B250B","","",61347,40.763350612000004,2500709.27]
["1491000000-E","ASP CNC BAS CRS B250C","","",71500,42.5,3038750]
["1498000000-E","ASP CONC INTR CRS I190B","","",13870,44.875962508999997,622429.6]
["1503000000-E","ASP CONC INTR CRS I190C","","",40315,43.242974079,1743340.5]
["1519000000-E","ASP CNC SURF CRS S95B","","",126381,35.338405772999998,4466103.0599999996]
["1520000000-E","ASP CONC SURF CRS S95B LEVEL","","",50,48.62,2431]
["1523000000-E","ASP CNC SURF CRS S95C","","",86072,34.576590529000001,2976076.3]
["1525000000-E","ASP CONC SURF CRS SF95A","","",38502,39.018111007000002,1502275.31]
["1575000000-E","ASP FOR PLANT MIX","","",23693,591.09522010700005,14004819.050000001]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",295,117.97220339,34801.800000000003]
["1704000000-E","PATCHING EXIST PVMT","","",795,110.471698113,87825]
["1840000000-E","MILLED RUMBLE STRIPS","","",48100,0.25,12025]
["1847000000-E","******\"PCC PVMT THRU LNS","(12-1/2\")","",257000,60,15420000]
["1869000000-E","******\"PCC PVMT MISC","(12-1/2\")","",11000,80,880000]
["1881000000-E","GENERIC PAVING ITEM (LF)","MILLED RUMBLE STRIPS","(CONC SHLD)",41100,0.5,20550]
["1891000000-E","GENERIC PAVING ITEM(SY)","NONWOVEN GEOTEXTILE ","INTERLAYER",39000,2.2999999999999998,89700]
["1902000000-N","SURF TEST CONC PVMT","","",1,135000,135000]
["1913000000-E","CONC SHLD ADJ ****\"PVMT","(12-1/2\")","",51000,57.5,2932500]
["1924000000-N","FIELD LAB RENTAL PCCP","","",1,40000,40000]
["2000000000-N","RIGHT OF WAY MKRS","","",276,147.373188406,40675]
["2022000000-E","SUBDRN EXCAV","","",2732.8,21.639344262000002,59136]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",12000,5,60000]
["2033000000-E","SUBDRN FINE AGG","","",33.6,30,1008]
["2036000000-E","SUBDRN COARSE AGG","","",2016,55,110880]
["2044000000-E","6\" PERF SUBDRN PIPE","","",12200,12.426229508,151600]
["2070000000-N","SUBDRN PIPE OUTLET","","",25,350,8750]
["2077000000-E","6\" OUTLET PIPE","","",150,29.8,4470]
["2099000000-E","SHOULDER DRN","","",22800,7.8,177840]
["2110000000-E","4\" SHOULDER DRN PIPE","","",22800,1.5,34200]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",840,14,11760]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",10,325,3250]
["2143000000-E","BLOTTING SAND","","",20,59.6,1192]
["2209000000-E","ENDWALLS","","",88.5,781.8,69189.3]
["2220000000-E","REINF ENDWALLS","","",33,777.28,25650.240000000002]
["2253000000-E","PIPE COLLARS","","",13,647.03,8411.39]
["2264000000-E","PIPE PLUGS","","",3,568.57000000000005,1705.71]
["2275000000-E","FLOWABLE FILL","","",20,145.52000000000001,2910.4]
["2286000000-N","MASNRY DRNG STRUCT","","",371,976.45552560600004,362265]
["2297000000-E","MASNRY DRNG STRUCT","","",34,1200,40800]
["2308000000-E","MASNRY DRNG STRUCT","","",242,194,46948]
["2354000000-N","FRM W/GRATE 84022 STD","","",6,743.6,4461.6000000000004]
["2355000000-N","FRM W/GRATE 84029 STD","","",2,555,1110]
["2364000000-N","FRM W/2GRTS 84016 STD","","",1,559.35,559.35]
["2364200000-N","FRM W/2GRTS 84020 STD","","",75,558.14,41860.5]
["2365000000-N","FRM W/2GRTS 84022 STD","","",231,833.14,192455.34]
["2366000000-N","FRM W/2GRTS 84024 STD","","",11,816.27272727299999,8979]
["2367000000-N","FRM W/2GRTS 84029 STD","","",21,549.59619047599995,11541.52]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",5,610.85,3054.25]
["","","(F)","",3,635.15,1905.45]
["","","(G)","",8,635.15,5081.2]
["2396000000-N","FRM W/COVER STD 84054","","",27,462.54,12488.58]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",2,1750,3500]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",1,250,250]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",2420,13.5,32670]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",5260,16.850000000000001,88631]
["2556000000-E","SHOULDER BERM GUTR","","",12235,15.843890478,193850]
["2570000000-N","MOD CONC FLUME","","",6,750,4500]
["2612000000-E","6\" CONC DRIVEWAY","","",150,47.066666667,7060]
["2619000000-E","4\" CONC PAVED DITCH","","",260,45,11700]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",400,55,22000]
["2724000000-E","PC REINF BARR SNGL FC","","",12970,75,972750]
["2815000000-N","ADJ DROP INLETS","","",9,540.67777777799995,4866.1000000000004]
["2830000000-N","ADJ MHS","","",192,490.92447916700002,94257.5]
["2845000000-N","ADJ METER OR VAL BOX","","",205,449.24878048800002,92096]
["2860000000-N","CONV CB TO JB","","",3,750,2250]
["2995000000-N","GENERIC DRNG ITEM (EA)","CONV EXT OTCB TO 2GI","",14,750,10500]
["3000000000-N","IMPACT ATTEN TYPE 350","","",1,13250,13250]
["3030000000-E","STL BM GUARDRAIL","","",99212.5,14.101486707999999,1399043.75]
["3045000000-E","SBGR SHOP CURVED","","",262.5,14.597638095000001,3831.88]
["3105000000-N","SBGR TERM SECT","","",16,30,480]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",25,5.4,135]
["3180000000-N","GR ANCHOR TYPE **********","(III - SHOP CURVED)","",4,1450,5800]
["3195000000-N","GR ANCHOR TYPE AT-1","","",2,450,900]
["3210000000-N","GR ANCHOR TYPE CAT-1","","",44,410,18040]
["3215000000-N","GR ANCHOR TYPE III","","",16,1412.5,22600]
["3270000000-N","GR ANCHOR TYPE 350","","",83,1637.048192771,135875]
["3285000000-N","GR ANCHOR TYPE M-350","","",2,1600,3200]
["3317000000-N","GR ANCHOR TYPE B-77","","",68,1500,102000]
["3360000000-E","REM EXT GUARDRAIL","","",37191,1.5686052999999998E-2,583.38]
["3503000000-E","WOVEN WIRE FEN 47\" FAB","","",57800,1.85,106930]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",3670,14,51380]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",840,18,15120]
["3557000000-E","ADDITIONAL BARBED WIRE","","",500,0.1,50]
["3628000000-E","RIP RAP CL I","","",3100,56.25,174375]
["3635000000-E","RIP RAP CL II","","",1360,56.257352941000001,76510]
["3642000000-E","RIP RAP CL A","","",20,56.07,1121.4000000000001]
["3649000000-E","RIP RAP CL B","","",5991,48.033650475999998,287769.59999999998]
["3651000000-E","BOULDERS","","",135,78.36,10578.6]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",33140,2.9423506339999999,97509.5]
["3659000000-N","PREFORMED SCOUR HOLE","","",13,1088.956153846,14156.43]
["4048000000-E","REINF CONC FOUNDTN","","",10,650,6500]
["4057000000-E","OVERHEAD FOOTING","","",406,750,304500]
["4060000000-E","SUPPT BRKAWAY STL BM","","",3151,3.55,11186.05]
["4066000000-E","SUPPTS SIMPLE STL BM","","",4261,3,12783]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",3549,4.9732544379999997,17650.080000000002]
["4082100000-N","SUPPT OVRHD SIGN STR**","(A - 28+00 -Y1RPA-)","",1,38000,38000]
["","","(B - 502+50 -L-)","",1,49000,49000]
["","","(C - 531+00 -L-)","",1,104000,104000]
["","","(D - 586+50 -L-)","",1,75000,75000]
["","","(E - 595+00 -L-)","",1,52000,52000]
["","","(F - 610+00 -L-)","",1,75000,75000]
["","","(G -31+50 -Y4RPBD-)","",1,44000,44000]
["","","(H - 92+50 -Y4-)","",1,40000,40000]
["","","(I - 89+50 -Y4-)","",1,48500,48500]
["","","(J - 43+00 -Y4CD-)","",1,48000,48000]
["","","(K - 42+00 -Y4-)","",1,38500,38500]
["","","(L - 72+00 -Y4-)","",1,53000,53000]
["","","(M - 113+00 -Y4-)","",1,42000,42000]
["","","(N - 322' FRM S MAIN ST ","EXIT)",1,39500,39500]
["","","(O - 19+50 -Y4-)","",1,28500,28500]
["","","(P - 144' FROM LINVILLE ","RD EXIT)",1,40000,40000]
["","","(Q - 280' +/- FROM ROUTE ","MKRS)",1,28000,28000]
["","","(R - 36+50 -Y1-)","",1,83000,83000]
["4096000000-N","SIGN ERECTION TYPE D","","",15,95.333333332999999,1430]
["4102000000-N","SIGN ERECTION TYPE E","","",126,49.960317459999999,6295]
["4108000000-N","SIGN ERECTION TYPE F","","",10,100,1000]
["4110000000-N","SIGN ERECTION TYPE *** (GRD MTD)","(A)","",8,350,2800]
["","","(B)","",2,200,400]
["4114000000-N","SIGN ERECTION MILEMKRS","","",16,50,800]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(D)","",1,100,100]
["4143000000-N","DISPOSE SUPPT OVRHD ST","","",1,2000,2000]
["4152000000-N","DISP SIGN SYST STL BM","","",8,500,4000]
["4155000000-N","DISP SIGN SYST U-CHAN","","",77,1,77]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",3245,3.8029368259999998,12340.53]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",1243,7.8405711990000002,9745.83]
["4410000000-E","WORK ZONE SIGN (BARR)","","",1515,4.9536303630000003,7504.75]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",10894,3.809409767,41499.71]
["4415000000-N","FLASHING ARROW BOARD","","",4,2348,9392]
["4420000000-N","PORT CHANGE MSG SIGN","","",14,8448,118272]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",379,28.8,10915.2]
["4430000000-N","DRUMS","","",980,39.844081633000002,39047.199999999997]
["4435000000-N","CONES","","",80,15.53125,1242.5]
["4445000000-E","BARRICADES (TYPE III)","","",1560,15.925641025999999,24844]
["4450000000-N","FLAGGER","","",2224,40,88960]
["4455000000-N","FLAGGER","","",228,75,17100]
["4457000000-N","TEMP TRAFFIC CNTRL","","",4,36983.75,147935]
["4465000000-N","TEMP CRASH CUSHIONS","","",10,4000,40000]
["4470000000-N","RESET CRASH CUSHION","","",8,1200,9600]
["4480000000-N","TMA","","",4,18000,72000]
["4485000000-E","PORT CONC BARR","","",2908,18,52344]
["4490000000-E","PORT CONC BARR(ANCH)","","",23400,35,819000]
["4500000000-E","RESET PORT CONC BARR","","",6375,4,25500]
["4510000000-N","LAW ENFORCEM","","",972,37.294238683000003,36250]
["4520000000-N","TUBULAR MKRS (FIXED)","","",120,33.799999999999997,4056]
["4650000000-N","TEMP RAISED PVMT MRKS","","",416,6.360576923,2646]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",1036797,0.43817401099999997,454297.5]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",1131701,0.56573850299999995,640246.82999999996]
["4688000000-E","THERMO PVT MKG LINES6\"90 MILS","","",9692,0.89766198900000005,8700.14]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",2723,0.99598971700000005,2712.08]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",9081,1.516177734,13768.41]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",2913,2.1832303469999998,6359.75]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",1947,1.8598715969999999,3621.17]
["4705000000-E","THERMO LINES 16\" 120MILS","","",750,9,6750]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",6826,9.1522414300000001,62473.2]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",218,95.477064220000003,20814]
["4725000000-E","THERMO PVT SYMB 90MIL","","",690,102.510144928,70732]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(IV)","",282,3.25,916.5]
["4810000000-E","PAINT PVMT MKGS 4\"","","",273604,0.26545584100000003,72629.78]
["4815000000-E","PAINT PVMT MKGS 6\"","","",309927,0.26466051699999998,82025.440000000002]
["4820000000-E","PAINT PVMT MKGS 8\"","","",1570,1.015605096,1594.5]
["4825000000-E","PAINT PVMT MKGS 12\"","","",9304,0.6,5582.4]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",300,4.5,1350]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",2302,4.5955690699999998,10579]
["4840000000-N","PAINT PVT MKG CHARACTER","","",72,42.916666667000001,3090]
["4845000000-N","PAINT PVT MKG SYMBOL","","",63,25,1575]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",38235,0.8559966,32729.03]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",174105,1.17,203702.85]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",5570,2.2999999999999998,12811]
["4850000000-E","LINE REML 4\" WIDE","","",8896,0.9,8006.4]
["4900000000-N","PERM RAISED PVMT MKRS","","",156,6,936]
["4905000000-N","SNOWPLB PVMT MRKER","","",5222,25.084569130999999,130991.62]
["4915000000-E","7' U-CHANNEL POSTS","","",24,24.9,597.6]
["4935000000-N","FLEX DELINAT (CRYSTAL)","","",90,31.95,2875.5]
["4940000000-N","FLEX DELINATR (YELLOW)","","",56,31.95,1789.2]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",5,31.95,159.75]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",5,31.95,159.75]
["4955000000-N","OBJECT MKR (END OF RD)","","",24,50,1200]
["5255000000-N","PORTABLE LIGHTING","","",3,60841.84,182525.52]
["5325600000-E","6\" WATER LINE","","",1423,40.36,57432.28]
["5325800000-E","8\" WATER LINE","","",1125,33.04,37170]
["5326200000-E","12\" WATER LINE","","",2520,49.63,125067.6]
["5326600000-E","16\" WATER LINE","","",1637,85.5,139963.5]
["5327000000-E","20\" WATER LINE","","",420,85.5,35910]
["5540000000-E","6\" VALVE","","",3,872.67,2618.0100000000002]
["5546000000-E","8\" VALVE","","",3,1229.72,3689.16]
["5558000000-E","12\" VALVE","","",2,1962,3924]
["5558600000-E","16\" VALVE","","",2,5143,10286]
["5571600000-E","6\" TAPPING VALVE","","",3,2250,6750]
["5589100000-E","1\" AIR RELEASE VALVE","","",3,1881.27,5643.81]
["5648000000-N","RELOCATE WATER METER","","",3,816.97,2450.91]
["5672000000-N","RELOCATE FIRE HYDRANT","","",8,1905.88,15247.04]
["5691300000-E","8\" SANIT GRAV SEWER","","",1165,36,41940]
["5691600000-E","16\" SANIT GRAV SEWER","","",511,99,50589]
["5691700000-E","18\" SANIT GRAV SEWER","","",724,135,97740]
["5691900000-E","24\" SANIT GRAV SEWER","","",1554,149.4,232167.6]
["5692000000-E","30\" SANIT GRAV SEWER","","",367,198.9,72996.3]
["5775000000-E","4' DIA UTILITY MH","","",13,1944.01,25272.13]
["5776000000-E","5' DIA UTILITY MH","","",11,2365.36,26018.959999999999]
["5777000000-E","6' DIA UTILITY MH","","",4,3232.8,12931.2]
["5781000000-E","UTILITY MH WALL 4' DIA","","",40,135,5400]
["5782000000-E","UTILITY MH WALL 5' DIA","","",133,193.6,25748.799999999999]
["5783000000-E","UTILITY MH WALL 6' DIA","","",16,322.2,5155.2]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",1423,5.27,7499.21]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",100,7.7,770]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",900,3.83,3447]
["5811000000-E","ABANDON 18\" UTILITY PIPE","","",1003,17.97,18023.91]
["5812000000-E","ABANDON 20\" UTILITY PIPE","","",415,36,14940]
["5813000000-E","ABANDON 24\" UTILITY PIPE","","",1333,6.3,8397.9]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",20,30.6,612]
["5815000000-N","REM WATER METER","","",8,171,1368]
["5815500000-N","REM FIRE HYDRANT","","",7,477,3339]
["5816000000-N","ABANDON UTILITY MH","","",7,790.09,5530.63]
["5828000000-N","REM UTILITY MH","","",13,820.69,10668.97]
["5835700000-E","16\" ENCASEMENT PIPE","","",810,66.31,53711.1]
["5836000000-E","24\" ENCASEMENT PIPE","","",300,73.3,21990]
["5836200000-E","30\" ENCASEMENT PIPE","","",810,68.400000000000006,55404]
["5888000000-E","GENERIC UTILITY ITEM (LF)","ANCHOR SEWER MAIN TO ","PROPOSED CLVT",52,135,7020]
["5890000000-N","GENERIC UTIL ITM(EA)1510","REM BLOWOFF ASSEM","",1,1800,1800]
["6000000000-E","TEMP SILT FENCE","","",293696,1.3419999929999999,394140.03]
["6006000000-E","EROS CNTRL STONE CL A","","",6120,39.219771242,240025]
["6009000000-E","EROS CONTRL STONE CL B","","",84610,41.900907693999997,3545235.8]
["6012000000-E","SEDIMENT CNTRL STONE","","",52815,41.574352930000003,2195749.4500000002]
["6015000000-E","TEMP MULCHING","","",511.9,758.56612619700002,388310]
["6018000000-E","SEED FOR TEMP SEEDING","","",83300,1.66487395,138684]
["6021000000-E","FERT FOR TEMP SEEDING","","",364.5,570.64471879300004,208000]
["6024000000-E","TEMP SLOPE DRNS","","",26400,8.5738636360000005,226350]
["6029000000-E","SAFETY FENCE","","",66080,1.0110472150000001,66810]
["6030000000-E","SILT EXCAV","","",170290,3.9305772509999999,669338]
["6036000000-E","MAT FOR EROS CNTRL","","",621100,1.087489937,675440]
["6037000000-E","COIR FIBER MAT","","",4105,4.4920828259999999,18440]
["6038000000-E","PERM SOIL REINF MAT","","",10880,4.6858455880000003,50982]
["6042000000-E","1/4\" HARDWARE CLOTH","","",17570,2.1683409220000001,38097.75]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",125,22.5,2812.5]
["6048000000-E","FLOAT TURBIDITY CURTN","","",445,20.056292135,8925.0499999999993]
["6069000000-E","STILLING BASINS","","",2000,13.6,27200]
["6070000000-N","SPECIAL STILLING BASINS","","",40,289.54500000000002,11581.8]
["6071010000-E","WATTLE","","",4745,4.1054267649999998,19480.25]
["6071012000-E","COIR FIBER WATTLE","","",15600,7.6,118560]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",11585,4.7188174360000001,54667.5]
["6071030000-E","COIR FIBER BAFFLE","","",50500,4.0607920789999996,205070]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",137,722.98423357700005,99048.84]
["","","(2\")","",12,859.01,10308.120000000001]
["","","(2-1/2\")","",2,900,1800]
["6084000000-E","SEEDING & MULCHING","","",612.4,1348.6691704770001,825925]
["6087000000-E","MOWING","","",306.2,66.101241019,20240.2]
["6090000000-E","SEED FOR REPAIR SEEDING","","",7350,1.944557823,14292.5]
["6093000000-E","FERT FOR REPAIR SEEDING","","",29.5,597.93423728799996,17639.060000000001]
["6096000000-E","SEED FOR SUPP SEEDING","","",14675,2.8597103920000002,41966.25]
["6108000000-E","FERTILIZER TOPDRESSING","","",438.75,707.46438746399997,310400]
["6111000000-E","IMPERVIOUS DIKE","","",1500,38.4,57600]
["6114500000-N","SPECIALIZED HAND MOW","","",545,47.839449541,26072.5]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",204,76.647058823999998,15636]
["6120000000-E","CLVT DIVERSION CHANNEL","","",7000,10.08,70560]
["6123000000-E","REFORESTATION","","",10,807.5,8075]
["6126000000-E","STRMBNK REFORESTATN","","",1,760,760]
["7060000000-E","SIGNAL CABLE","","",1750,3.43,6002.5]
["7120000000-E","VEHICLE SIGNAL HD (12\" 3 SECT)","","",13,703.26,9142.3799999999992]
["7252000000-E","MESSENGER CABLE (1/4\")","","",12699,2.04,25905.96]
["7264000000-E","MESSENGER CABLE (3/8\")","","",1200,2.36,2832]
["7276000000-E","BORE & JACK (***********)","(1 6\")","",270,80.760000000000005,21805.200000000001]
["7279000000-E","TRACER WIRE","","",33556,0.54,18120.240000000002]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",1225,4.93,6039.25]
["7301000000-E","DIRECT DRILL (***********)","(1 2\")","",386,12.23,4720.78]
["","","(2 2\")","",10001,14.86,148614.85999999999]
["7312000000-N","JUNCTION BOX (***********)","(SPECIAL SIZED)","",11,1224.46,13469.06]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",27,467.01,12609.27]
["7348000000-N","JUNCTION BOX (OVER-SIZED HVY-DUTY)","","",45,785.83,35362.35]
["7360000000-N","WOOD POLE","","",88,599.29999999999995,52738.400000000001]
["7372000000-N","GUY ASSEM","","",40,391.3,15652]
["7408000000-E","1\" RISER W/ WEATHERHD","","",2,363.85,727.7]
["7420000000-E","2\" RISER W/ WEATHERHD","","",9,405.33,3647.97]
["7432000000-E","2\" RISER WITH TUBING","","",6,347.83,2086.98]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",1350,5.27,7114.5]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",4300,2.73,11739]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(144)","",26023,2.59,67399.570000000007]
["","","(72)","",24601,1.83,45019.83]
["7528000000-E","DROP CABLE","","",1639,1.36,2229.04]
["7540000000-N","SPLICE ENCLOSURE","","",7,2282.61,15978.27]
["7541000000-N","MOD SPLICE ENCLOSURE","","",2,3994.57,7989.14]
["7552000000-N","INTERCONNECT CENTER","","",5,1059.78,5298.9]
["7566000000-N","DELINEATOR MKR","","",49,92.39,4527.1099999999997]
["7575142000-N","900MHZ RADIO","","",2,5212.24,10424.48]
["7575142200-N","NEW ELECTRICAL SERVICE","","",7,2671.08,18697.560000000001]
["7575160000-E","REM EXT COMM CABLE","","",24611,0.82,20181.02]
["7613000000-N","SOIL TEST","","",4,657.13,2628.52]
["7614100000-E","DRILLED PIER FOUND","","",32,828.83,26522.560000000001]
["7636000000-N","SIGN FOR SIGNALS","","",5,305.11,1525.55]
["7684000000-N","SIGNAL CBNT FOUND","","",2,1238.26,2476.52]
["7756000000-N","CONTLR WITH CBNT 2070L BASE MTD","","",2,11715.76,23431.52]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",6,116.11,696.66]
["7901000000-N","CBNT BASE EXTENDER","","",2,437.31,874.62]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","10KVA SINGLE PHASE ","TRANSFORMER",4,1348.37,5393.48]
["","","5/8\" X 10' GROUNDING ","ELECTRODE",27,256.52,6926.04]
["","","CARD CAGES","",1,2476.9,2476.9]
["","","CCTV CBNT","",5,4104.3999999999996,20522]
["","","CCTV CAMERA ASSEM","",5,4023.37,20116.849999999999]
["","","CCTV CAMERA LOWRING ","SYSTEM",2,7163.59,14327.18]
["","","CCTV EXTENSION POLE","",1,999.46,999.46]
["","","CCTV METAL POLE (50')","",2,11476.67,22953.34]
["","","CCTV METAL POLE (70')","",2,14369.26,28738.52]
["","","COMMUNICATIONS RACK","",1,2764.95,2764.95]
["","","DIGITAL HARDWARE ","VIDEO DECODER",6,2102.0100000000002,12612.06]
["","","DIGITAL HARDWARE ","VIDEO ENCODER",6,2102.0100000000002,12612.06]
["","","DMS","",2,81506.3,163012.6]
["","","DMS ACCESS LADDER","",3,5720.65,17161.95]
["","","DMS OVERHEAD ASSEM","",1,56788.63,56788.63]
["","","DMS PEDESTAL ASSEM","",2,52912.63,105825.26]
["","","EQUIP CBNT BASE ","EXTENDER",2,807.93,1615.86]
["","","EQUIP CBNT DISCONNECT","",7,674.18,4719.26]
["","","EQUIP CBNT FOUND","",2,1709.51,3419.02]
["","","ETHERNET EDGE SWITCH","",7,1206.47,8445.2900000000009]
["","","FURN CCTV ASSEM","",1,2791.3,2791.3]
["","","FURN DIGITAL HARDWAR ","VIDEODECODER",2,1919.02,3838.04]
["","","FURN DIGITAL HARDWAR ","VIDEOENCODER",2,1919.02,3838.04]
["","","FURN ETHERNET EDGE ","SWITCH",1,930.43,930.43]
["","","HUB CBNT","",1,11899.91,11899.91]
["","","HUB SPLICE CENTER","",1,24836.959999999999,24836.959999999999]
["","","MANAGED ETHERNET CORE SWITCH","MODIFICATIONS",1,19565.22,19565.22]
["","","MANAGED ETHERNET ","ROUTING SWITCH",1,28695.65,28695.65]
["","","MOD NETWORK MGMT ","SOFTWARE",1,1250,1250]
["","","PORTABLE CCTV","",1,37853.26,37853.26]
["","","PORTABLE CCTV ","LOWERING TOOL",1,1755.42,1755.42]
["","","SOLAR POWER ASSEM","",1,10889.62,10889.62]
["","","UPS","",1,1892.66,1892.66]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","DMS (REM & REINSTALL)","",1,121290.76,121290.76]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","3-WIRE FEEDER ","CONDUCTORS",3178,4.12,13093.36]
["","","4-WIRE FEEDER ","CONDUCTORS",785,10.130000000000001,7952.05]
["","","UNDERGROUND CONDUIT ","(1 2\")",2655,4.8899999999999997,12982.95]
["","","UNDERGROUND CONDUIT ","(2 2\")",23460,6.17,144748.20000000001]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","OVERHEAD SIGN ASSEM","FOOTINGS",16,789.79,12636.64]
["8017000000-N","CM&R TEMP ACCESS ******","(20+9200-L-)","",1,27000,27000]
["8021000000-N","REMV EXIST STR **********","(14+6600-L-)","",1,30000,30000]
["8035000000-N","REMV EXIST STR **********","(18+6650 -L-)","",1,32500,32500]
["","","(20+9200-L-)","",1,75000,75000]
["8056000000-N","REMV EXIST STR **********","(23+1100-Y1-)","",1,10000,10000]
["8084000000-N","FND EXCAV EB** STA*******","(252+9428-Y4RPBD-)","",1,6760.19,6760.19]
["8091000000-N","FND EXCAV B** STA *******","(1 17+1000-Y4RPA-)","",1,6760.19,6760.19]
["","","(1 482+1314 -L-)","",1,9804.2099999999991,9804.2099999999991]
["","","(1 516+3130-L-)","",1,5014.2700000000004,5014.2700000000004]
["","","(1 584+3624 -L-LT)","",1,10028.540000000001,10028.540000000001]
["","","(1 584+3624-L-RT)","",1,10028.540000000001,10028.540000000001]
["","","(128+5016-Y5-)","",1,5014.2700000000004,5014.2700000000004]
["","","(144+0864-Y4RPBD-)","",1,9267.34,9267.34]
["","","(146+8716-Y4CD-)","",1,7521.39,7521.39]
["","","(152+9428-Y4RPBD-)","",1,6760.19,6760.19]
["","","(1642+8142-L-LT)","",1,5014.2700000000004,5014.2700000000004]
["","","(1642+8142-L-RT)","",1,5014.2700000000004,5014.2700000000004]
["","","(2 584+3624 -L-LT)","",1,10028.540000000001,10028.540000000001]
["","","(2 584+3624-L-RT)","",1,10028.540000000001,10028.540000000001]
["","","(2 628+6550-L-LT)","",1,6760.19,6760.19]
["","","(2 628+6550-L-RT)","",1,6760.19,6760.19]
["","","(228+5016-Y5-)","",1,5014.2700000000004,5014.2700000000004]
["","","(233+1567-Y4CD-)","",1,6760.19,6760.19]
["","","(252+9428-Y4RPBD-)","",1,6760.19,6760.19]
["","","(328+5016-Y5-)","",1,5014.2700000000004,5014.2700000000004]
["","","(4 17+1000-Y4RPA-)","",1,6760.19,6760.19]
["8096000000-E","PILE EXCAV IN SOIL","","",64,100,6400]
["8097000000-E","PILE EXCAV NOT IN SOIL","","",78,100,7800]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",454.8,572.9,260554.92]
["","","(5'-0\")","",260,563.52,146515.20000000001]
["","","(5'-6\")","",74.599999999999994,865.46997319000002,64564.06]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",106.65,950,101317.5]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",437,379.79,165968.23000000001]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",132,570.47,75302.039999999994]
["","","(5'-0\")","",103,1998.73,205869.19]
["","","(5'-6\")","",34,3657.89,124368.26]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",106,981,103986]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",152,3786.16,575496.31999999995]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",292.60000000000002,503.71999316500001,147388.47]
["","","(5'-0\")","",204,503.72,102758.88]
["","","(5'-6\")","",48.6,575.68004115199994,27978.05]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",56.12,260,14591.2]
["8111600000-E","PERM STL CASING FOR 4' PIER","","",104,431.76,44903.040000000001]
["8112730000-N","PDA TESTING","","",12,1900,22800]
["8113000000-N","SID INSPECTIONS","","",6,1000,6000]
["8114000000-N","SPT TESTING","","",1,4000,4000]
["8115000000-N","CSL TESTING","","",8,2425,19400]
["8121000000-N","UNCL STR EXCAV STA ****","(14+6600-L-)","",1,6950,6950]
["","","(18+6650 -L-)","",1,3360,3360]
["8126000000-N","CULV EXCAV @ ************","(23+1100-Y1-)","",1,37872.81,37872.81]
["","","(559+7400-L-)","",1,31181.85,31181.85]
["","","(616+4500-L-)","",1,56127.29,56127.29]
["","","(667+1500-L-)","",1,49890.93,49890.93]
["","","(STA 45+6543 -Y4-)","",1,12472.74,12472.74]
["8133000000-E","FND CONDIT MAT BOX CULV","","",3438,50,171900]
["8147000000-E","REINF CONC DECK SLAB","","",225152,21.89,4928577.28]
["8154000000-E","REINF CONC DECK SLABLTWT","","",42278,19.600000000000001,828648.8]
["8161000000-E","GROOVING BRG FLOORS","","",285922,0.25,71480.5]
["8182000000-E","CL A CONC (BRG)","","",6010.6,744.96639104200005,4477694.99]
["8196000000-E","CL A CONC (CULV)","","",9004,350,3151400]
["8210000000-N","BRG APPR SLAB ***********","(14+6600-L-)","",1,11675,11675]
["","","(17+1000-Y4RPA-)","",1,35486.080000000002,35486.080000000002]
["","","(18+6650 -L-)","",1,18600,18600]
["","","(20+9200-L-)","",1,11700,11700]
["","","(23+5912-Y5-)","",1,33126.21,33126.21]
["","","(26+6000-Y4RPBD-)","",1,34220.639999999999,34220.639999999999]
["","","(28+5016-Y5-)","",1,32128.11,32128.11]
["","","(33+1567-Y4CD-)","",1,26963.65,26963.65]
["","","(44+0864-Y4RPBD-)","",1,36965.050000000003,36965.050000000003]
["","","(46+8716-Y4CD-)","",1,42240.69,42240.69]
["","","(482+1314-L-)","",1,84549.79,84549.79]
["","","(516+3130-L-)","",1,31554.36,31554.36]
["","","(52+9428-Y4RPBD-)","",1,35784.160000000003,35784.160000000003]
["","","(556+8500-L-LT)","",1,50431.63,50431.63]
["","","(556+8500-L-RT)","",1,50431.63,50431.63]
["","","(584+3624-L-LT)","",1,74083.63,74083.63]
["","","(584+3624-L-RT)","",1,74083.63,74083.63]
["","","(628+6550-L-LT)","",1,71803.95,71803.95]
["","","(628+6550-L-RT)","",1,71803.95,71803.95]
["","","(642+8142-L-LT)","",1,57519.9,57519.9]
["","","(642+8142-L-RT)","",1,69636.61,69636.61]
["8217000000-E","REINF STEEL (BRG)","","",1224081,0.91138681200000005,1115611.28]
["8238000000-E","SPIRL COL REINF STL BRG","","",161354,1.74240025,281143.25]
["8245000000-E","REINF STEEL (CLVT)","","",820225,0.79,647977.75]
["8265000000-E","54\" PRESTR CONC GIRDR","","",5829.92,254.28000041199999,1482432.06]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",8411.0300000000007,263.54000045200002,2216642.85]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",11704.64,286.23999969200003,3350336.15]
["8280000000-E","STRUCTURAL STEEL","","",445000,2.387351056,1062371.22]
["8364000000-E","HP12X53 PILES","","",38202,59.765030887999998,2283143.71]
["8384000000-E","HP14X73 PILES","","",5025,72.675343283999993,365193.6]
["8391000000-N","STEEL PILE POINTS","","",247,143.91999999999999,35548.239999999998]
["8392500000-E","PREDRILLING FOR PILES","","",242,123.56,29901.52]
["8475000000-E","TWO BAR METAL RAIL","","",1733.87,116.880377422,202655.38]
["8503000000-E","CONC BARR RAIL","","",8793.23,63.550000398000002,558809.77]
["8505000000-E","VERT CONC BARR RAIL","","",204.79,84,17202.36]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-10 1/2\")","",561,72.5,40672.5]
["","","(1'-2\" X 2'-6\")","",1056,55.61,58724.160000000003]
["","","(1'-2\" X 3'-6\")","",180,100.61,18109.8]
["8531000000-E","4\" SLOPE PROTECTION","","",9157,37.31,341647.67]
["8608000000-E","RIP RAP II (2'-0\")","","",21928,57.019481941000002,1250323.2]
["8622000000-E","GEOTEXTILE FOR DRNG","","",24365,2.2634414120000002,55148.75]
["8654000000-N","DISC BEARINGS","","",1,56101.57,56101.57]
["8657000000-N","ELASTOMERIC BEARINGS","","",4,42874.432500000003,171497.73]
["8692000000-N","FOAM JOINT SEALS","","",1,17508.97,17508.97]
["8706000000-N","EXPANSION JOINT SEALS","","",1,352212.94,352212.94]
["8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",1170,204.35,239089.5]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",4206.3500000000004,210.695198925,886257.75]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",6334,58.96,373452.64]
["8802014000-E","SOLDIER PILE RETAINING WALLS","","",850,77.06,65501]
["8804000000-N","GENERIC CLVT ITEM (LS)","PLACEM OF NATURAL STREAM","BED MATL",1,149700,149700]
["8839000000-E","GENERIC RET WALL ITEM (LF)","CONC BARR RAIL WITH MOMENT SLAB","",500,275.51,137755]
["8847000000-E","GENERIC RET WALL ITEM (SF)","ANCHORED SOLDIER PILE WALLS","",7900,89.42,706418]
["","","SOUND BARR WALL","",255982,22,5631604]
["8860000000-N","GENERIC STR ITEM (LS)","SOUND BARR WALL(BRG","MOUNTED)",1,125147.16,125147.16]
["8892000000-E","GENERIC STR ITEM (SF)","CONC SIMULATED STONE","FORM LINER",3592.2,5,17961]
["","","CONC STAINING","",18581.099999999999,5,92905.5]
["8897000000-N","GENERIC STR ITEM (EA)","CONC MEDALLION PANEL","",8,1500,12000]

{"sheet":"Items - Div 10","index":12,"n_rows":304,"n_cols":7,"rows_kept":304,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 10"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",12,79958.333333332994,959500]
["0000400000-N","CONST SURVEYING","","",3,12666.666666667001,38000]
["0000900000-N","GENERIC MISC ITEM (LS)","DESIGN & CONST","",1,186687000,186687000]
["0001000000-E","CLEARING & GRUBBING","","",0,12500,2500]
["0029000000-N","REINF BRG APPR **********","(15+0900)","",1,24000,24000]
["","","(20+2050 -L- SBL)","",1,25000,25000]
["","","(20+4750 -L- NBL)","",1,25000,25000]
["0030000000-N","BRG APP SUB REG TIER**","(15+1100)","",1,8500,8500]
["","","(17+7300 -L-)","",1,10000,10000]
["","","(21+77 -L-)","",1,6800,6800]
["0036000000-E","UNDERCUT EXCAVATION","","",450,18.444444443999998,8300]
["0043000000-N","GRADING","","",4,186652.5,746610]
["0050000000-E","SUPP CLEAR & GRUBBING","","",5,75.2,376]
["0057000000-E","UNDERCUT EXCAVATION","","",2750,9.0363636360000008,24850]
["0063000000-N","GRADING","","",1,80000,80000]
["0106000000-E","BORROW EXCAVATION","","",19809,15.568456256999999,308395.55]
["0134000000-E","DRNG DITCH EXCAVATION","","",780,7.1794871789999997,5600]
["0195000000-E","SELECT GRANULAR MAT'L","","",2650,9.3962264149999992,24900]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",4800,1.6825000000000001,8076]
["0199000000-E","TEMP SHORING","","",550,60,33000]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",559,32.039355993000001,17910]
["0320000000-E","FND CONDIT GEOTEXTILE","","",1178,2.903225806,3420]
["0335200000-E","15\" DRNG PIPE","","",348,35.517241378999998,12360]
["0335300000-E","18\" DRNG PIPE","","",144,34.833333332999999,5016]
["0366000000-E","15\" RC PIPE CULV III","","",154,45,6930]
["0448000000-E","***\" RCP CULV CL IV","(12\")","",188,30,5640]
["0448200000-E","15\" RCP CULV CL IV","","",740,39.459459459000001,29200]
["0448300000-E","18\" RCP CULV CL IV","","",396,41.881313130999999,16585]
["0448600000-E","36\" RCP CULV CL IV","","",152,75,11400]
["0576000000-E","**\" CS PIPE CULV *****\"","(12\" 0064\")","",36,45,1620]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",32,55,1760]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\" 0064\")","",2,500,1000]
["0995000000-E","PIPE REMOVAL","","",238,21.344537814999999,5080]
["1099500000-E","SHALLOW UNDERCUT","","",1900,7.6315789470000004,14500]
["1099700000-E","CL IV SUBGRD STABIL","","",2270,13.623348018,30925]
["1121000000-E","AGG BASE COURSE","","",536,30,16080]
["1220000000-E","INCIDENTAL STONE BASE","","",10561,21.458157370999999,226619.6]
["1243000000-E","SHOULDER CONST","","",2.36,3580,8448.7999999999993]
["1245000000-E","SHOULDER RECONST","","",166.38,2215.0558961410002,368541]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",247332,1.2497365890000001,309099.84999999998]
["","","(2-1/2\")","",20645,2.8,57806]
["","","(3\")","",1905,7.5665354330000003,14414.25]
["1308000000-E","MILL ASP PVMT ***** - *****","(0\" TO 1-1/2\")","",12531,2.9329742240000001,36753.1]
["","","(0\" TO 2\")","",520,12,6240]
["","","(0\" TO 2-1/2\")","",400,8.5,3400]
["","","(0\" TO 3\")","",1690,5,8450]
["1330000000-E","INCIDENTAL MILLING","","",15786,6.0415114660000002,95371.3]
["1489000000-E","ASP CNC BAS CRS B250B","","",19786,40.259716466,796578.75]
["1491000000-E","ASP CNC BAS CRS B250C","","",773,40.851772316000002,31578.42]
["1498000000-E","ASP CONC INTR CRS I190B","","",38300,28.362984334,1086302.3]
["1503000000-E","ASP CONC INTR CRS I190C","","",283,45.805123674999997,12962.85]
["1519000000-E","ASP CNC SURF CRS S95B","","",79450,29.667849716999999,2357110.66]
["1520000000-E","ASP CONC SURF CRS S95B LEVEL","","",12158,33.421623621999998,406340.1]
["1523000000-E","ASP CNC SURF CRS S95C","","",68303,30.219326970000001,2064070.69]
["1524000000-E","ASP CONC SURF CRS S95C LEVEL","","",7951,34.499761036000002,274307.59999999998]
["1525000000-E","ASP CONC SURF CRS SF95A","","",1141,68.411481156999997,78057.5]
["1575000000-E","ASP FOR PLANT MIX","","",12939.5,608.21032033699998,7869937.4400000004]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",637,109.270015699,69605]
["1704000000-E","PATCHING EXIST PVMT","","",23842,79.566206694000002,1897017.5]
["1891000000-E","GENERIC PAVING ITEM(SY)","6\" JOINTED CONC ","GREENWAY",400,48,19200]
["2022000000-E","SUBDRN EXCAVATION","","",115,8.8695652169999999,1020]
["2033000000-E","SUBDRN FINE AGG","","",94,13.127659574000001,1234]
["2044000000-E","6\" PERF SUBDRN PIPE","","",500,2.8,1400]
["2070000000-N","SUBDRN PIPE OUTLET","","",2,87.5,175]
["2077000000-E","6\" OUTLET PIPE","","",12,4.5,54]
["2165000000-E","12\" FUNNEL DRN PIPE","","",24,100,2400]
["2176000000-E","12\" FUNNEL DRN ELBOWS","","",1,500,500]
["2209000000-E","ENDWALLS","","",5.5,809.09090909099996,4450]
["2264000000-E","PIPE PLUGS","","",1,1000,1000]
["2275000000-E","FLOWABLE FILL","","",12,350,4200]
["2286000000-N","MASNRY DRNG STRUCT","","",33,1546.9696969700001,51050]
["2308000000-E","MASNRY DRNG STRUCT","","",4.7,264.36170212799999,1242.5]
["2364000000-N","FRM W/2GRTS 84016 STD","","",2,500,1000]
["2365000000-N","FRM W/2GRTS 84022 STD","","",5,500,2500]
["2367000000-N","FRM W/2GRTS 84029 STD","","",6,421.66666666700002,2530]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",4,562.5,2250]
["","","(F)","",7,592.85714285699999,4150]
["","","(G)","",6,583.33333333300004,3500]
["2396000000-N","FRM W/COVER STD 84054","","",1,500,500]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",1,1500,1500]
["2462000000-E","**\" SLUICE GATE","(18\")","",1,2000,2000]
["2538000000-E","**'-**\" CONC CURB & GUTR","(2'-0\")","",120,23,2760]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",2050,18.402439024,37725]
["2556000000-E","SHOULDER BERM GUTR","","",195,51.179487178999999,9980]
["2591000000-E","4\" CONC SIDEWALK","","",1440,24,34560]
["2600000000-N","RETROFIT EXT CURB RAMP","","",123,358.61788617899998,44110]
["2605000000-N","CONC CURB RAMP","","",4,950,3800]
["2612000000-E","6\" CONC DRIVEWAY","","",5135,65.428237585000005,335974]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",329,58.474164133999999,19238]
["2800000000-N","ADJ CATCH BASINS","","",5,2000,10000]
["2815000000-N","ADJ DROP INLETS","","",3,1133.3333333329999,3400]
["2830000000-N","ADJ MANHOLES","","",62,460.91935483899999,28577]
["2845000000-N","ADJ METER OR VAL BOX","","",89,560.59550561799995,49893]
["3000000000-N","IMPACT ATTEN 350","","",2,12800,25600]
["3030000000-E","STL BM GUARDRAIL","","",2550,18.116764706000001,46197.75]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",35,21.6,756]
["3165000000-N","GR ANCHOR **********","(350 TL-2)","",4,1600,6400]
["3210000000-N","GR ANCHOR CAT-1","","",1,758.13,758.13]
["3215000000-N","GR ANCHOR III","","",21,1350,28350]
["3270000000-N","GR ANCHOR 350","","",17,1853.8541176470001,31515.52]
["3317000000-N","GR ANCHOR B-77","","",2,1400,2800]
["3360000000-E","REM EXT GUARDRAIL","","",107,2.11,225.77]
["3365000000-E","REM EXT GUIDERAIL","","",1480,1,1480]
["3380000000-E","TEMP STL BM GUARDRAIL","","",125,9,1125]
["3389100000-N","TMP GDRL ANCH UNIT 350","","",1,1000,1000]
["3595000000-E","RELAPPING GUARDRAIL","","",270,5,1350]
["3635000000-E","RIP RAP CL II","","",9,50,450]
["3649000000-E","RIP RAP CL B","","",436,37.002293578,16133]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",6400,2.0325000000000002,13008]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",172,5,860]
["4102000000-N","SIGN ERECTION E","","",9,45,405]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(E)","",3,45,135]
["4155000000-N","DISP SIGN SYST U-CHAN","","",8,1,8]
["4192000000-N","DISPOSE SUPPT U-CHAN","","",2,1,2]
["4400000000-E","WORK ZONE SIGN (STAT)","","",2763,4.165530221,11509.36]
["4405000000-E","WORK ZONE SIGN (PORT)","","",591,7.3718274109999999,4356.75]
["4410000000-E","WORK ZONE SIGN (BARR)","","",546,7.5128205130000003,4102]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",11230.1,3.5012982969999999,39319.93]
["4415000000-N","FLASH ARROW BOARD","","",3,3500,10500]
["4420000000-N","PORT CHANGE MSG SIGN","","",2,10000,20000]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",58,87.931034483000005,5100]
["4430000000-N","DRUMS","","",364,66.291208791000003,24130]
["4435000000-N","CONES","","",135,23.703703703999999,3200]
["4445000000-E","BARRICADES ( III)","","",584,14.034246574999999,8196]
["4450000000-N","FLAGGER","","",1400,16.571428570999998,23200]
["4457000000-N","TEMP TRAFFIC CONTROL","","",7,50383.342857142998,352683.4]
["4465000000-N","TEMP CRASH CUSHIONS","","",2,4250,8500]
["4480000000-N","TMA","","",1,10000,10000]
["4485000000-E","PORT CONC BARRIER","","",1070,20,21400]
["4507000000-E","WATER FILLED BARRIER","","",2380,44.25,105315]
["4508000000-E","RESET H2O FILLED BARR","","",1168,5,5840]
["4510000000-N","LAW ENFORCEMENT","","",800,41.5,33200]
["4516000000-N","SKINNY DRUM","","",140,67.142857143000001,9400]
["4650000000-N","TEMP RAISED PVMT MRKS","","",112,8.75,980]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",734018,0.53457200000000005,392385.47]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",763122,0.61919580399999996,472521.94]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",6124,1.9293664269999999,11815.44]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",3206,2.1448970680000001,6876.54]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",5193,2.5808299629999998,13402.25]
["4705000000-E","THERMO LINES 16\" 120MILS","","",350,5.4514285710000001,1908]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",4424,6.5984764919999996,29191.66]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",202,115.658415842,23363]
["4725000000-E","THERMO PVT SYMB 90MIL","","",514,112.692217899,57923.8]
["4770000000-E","4\" COLD APPL PLSTIC LINES **","(II)","",1838,3.8519151250000001,7079.82]
["","","(IV)","",1264,2.4500000000000002,3096.8]
["4775000000-E","6\" COLD APPL PLSTIC LINES **","(II)","",210,8,1680]
["4810000000-E","PAINT PVMT MKGS 4\"","","",1353486,0.11683656100000001,158136.65]
["4820000000-E","PAINT PVMT MKGS 8\"","","",3766,0.61813329800000005,2327.89]
["4825000000-E","PAINT PVMT MKGS 12\"","","",1021,1.422135162,1452]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",100,1.02,102]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",1890,2.6622857139999998,5031.72]
["4840000000-N","PAINT PVT MKG CHAR","","",30,73.413333332999997,2202.4]
["4845000000-N","PAINT PVT MKG SYMBOL","","",184,80.485869565000002,14809.4]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",4603,1.45,6674.35]
["4847110000-E","POLYUREA LINES (8\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",1233,3.25,4007.25]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",2043,1,2043]
["4900000000-N","PERM RAISED PVMT MKRS","","",7854,4.8370078940000001,37989.86]
["5255000000-N","PORT LIGHTING","","",2,7500,15000]
["5326200000-E","12\" WATER LINE","","",539,80,43120]
["5326600000-E","16\" WATER LINE","","",946,135,127710]
["5558000000-E","12\" VALVE","","",2,2050,4100]
["5558600000-E","16\" VALVE","","",2,5250,10500]
["5589200000-E","2\" AIR RELEASE VALVE","","",2,2000,4000]
["5648000000-N","RELOCATE WATER METER","","",2,1500,3000]
["5649000000-N","RECONNECT H2O METER","","",1,1500,1500]
["5672000000-N","RELOCATE FIRE HYDRANT","","",1,3000,3000]
["5804000000-E","ABAND 12\" UTILITY PIPE","","",501,10.1,5060.1000000000004]
["5810000000-E","ABAND 16\" UTILITY PIPE","","",917,15,13755]
["5836000000-E","24\" ENCASEMENT PIPE","","",95,100,9500]
["5872200000-E","24\" TRENCHLESS INSTALL (IN SOIL)","","",48,350,16800]
["5872210000-E","24\" TRENCHLESS INSTALL (NOT IN SOIL)","","",48,775,37200]
["6000000000-E","TEMP SILT FENCE","","",24863,2.0093954869999999,49959.6]
["6006000000-E","EROS CNTRL STONE CL A","","",950,28.568421053000002,27140]
["6009000000-E","EROS CNTRL STONE CL B","","",2235,33.814765100999999,75576]
["6012000000-E","SEDIMENT CNTRL STONE","","",2447,31.554658765999999,77214.25]
["6015000000-E","TEMP MULCHING","","",8.85,759.88700564999999,6725]
["6018000000-E","SEED FOR TEMP SEEDING","","",500,4.8,2400]
["6021000000-E","FERT FOR TEMP SEEDING","","",6.5,1419.2307692310001,9225]
["6024000000-E","TEMP SLOPE DRNS","","",1000,7.8,7800]
["6029000000-E","SAFETY FENCE","","",700,2.0499999999999998,1435]
["6030000000-E","SILT EXCAVATION","","",2060,4.0242718450000003,8290]
["6036000000-E","MAT FOR EROS CONTROL","","",14500,1.2824137929999999,18595]
["6037000000-E","COIR FIBER MAT","","",1075,5.3813953489999999,5785]
["6038000000-E","PERM SOIL REINF MAT","","",400,5,2000]
["6042000000-E","1/4\" HARDWARE CLOTH","","",1630,2.979294479,4856.25]
["6048000000-E","FLOAT TURBIDITY CURTN","","",450,11.52,5184]
["6070000000-N","SPECIAL STILLING BASINS","","",44,272.040909091,11969.8]
["6071010000-E","WATTLE","","",14171,4.2718283819999998,60536.08]
["6071012000-E","COIR FIBER WATTLE","","",275,7.4727272730000003,2055]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",285,24.475614035,6975.55]
["6071030000-E","COIR FIBER BAFFLE","","",750,4.858733333,3644.05]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",11,1001.147272727,11012.62]
["6084000000-E","SEEDING & MULCHING","","",8.85,1654.576271186,14643]
["6087000000-E","MOWING","","",4.72,168.220338983,794]
["6090000000-E","SEED FOR REPAIR SEED","","",250,5.24,1310]
["6093000000-E","FERT FOR REPAIR SEED","","",1.25,1645,2056.25]
["6096000000-E","SEED FOR SUPP SEEDING","","",300,4.3333333329999997,1300]
["6108000000-E","FERTILIZER TOPDRESSING","","",6.25,1072,6700]
["6114500000-N","SPECIALIZED HAND MOW","","",60,30.333333332999999,1820]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",85,49.070588235000002,4171]
["7252000000-E","MESSENGER CABLE (1/4\")","","",260,2.52,655.20000000000005]
["7279000000-E","TRACER WIRE","","",34395,0.39,13414.05]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",1150,4.97,5715.5]
["","","(2 2\")","",1660,5.52,9163.2000000000007]
["","","(4 1-1/4\")","",3610,5.47,19746.7]
["7301000000-E","DIRECT DRILL (***********)","(2 2\")","",730,15.63,11409.9]
["","","(4 1-1/4\")","",1290,15.63,20162.7]
["7312000000-N","JUNCTION BOX (***********)","(SPECIAL OVERSIZED)","",7,1146.19,8023.33]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",20,233.8,4676]
["7348000000-N","JUNCTION BOX (OVER-SIZED HVY-DUTY)","","",12,875.08,10500.96]
["7360000000-N","WOOD POLE","","",5,788.34,3941.7]
["7372000000-N","GUY ASSEMBLY","","",2,297.86,595.72]
["7384000000-E","***\" RISER WITH ************","(1-1/4\" WEATHERHEAD)","",3,235.49,706.47]
["7432000000-E","2\" RISER WITH TUBING","","",2,309.45999999999998,618.91999999999996]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",4310,1.42,6120.2]
["","","(144)","",33500,2.2400000000000002,75040]
["7540000000-N","SPLICE ENCLOSURE","","",7,3118.43,21829.01]
["7566000000-N","DELINEATOR MKR","","",6,116.14,696.84]
["7613000000-N","SOIL TEST","","",8,602.73,4821.84]
["7614100000-E","DRILLED PIER FOUND","","",10,813.36,8133.6]
["7980000000-N","GENERIC SIGNAL ITEM(EA)","10KVA SINGLE PHASE ","TRANSFORMER",2,1475.93,2951.86]
["","","5/8\" X 10' GROUNDING ","ELECTRODE",41,80.099999999999994,3284.1]
["","","CCTV CAMERA ASSEMB","",5,5066.87,25334.35]
["","","CCTV CAMERA LOWERG ","SYST",5,6172.04,30860.2]
["","","CCTV FIELD EQUIP CBNT","",5,4012.11,20060.55]
["","","CCTV METAL POLE","",5,4577.7,22888.5]
["","","CENTRAL VIDEO CODEC ","UNIT",5,980.35,4901.75]
["","","DMS ACCESS LADDER","",3,4837.38,14512.14]
["","","DMS PEDESTAL STR","",3,38144.85,114434.55]
["","","DYNAMIC MESSAGE SIGN","",3,69600.67,208802.01]
["","","EQUIP CBNT DISCONNECT","",8,275.45,2203.6]
["","","FIELD ETHERNET SWITCH","",7,1088.3599999999999,7618.52]
["","","INTERCONNECT CENTER","(144-FIBER)",1,3153.51,3153.51]
["","","INTERCONNECT CENTER ","(12-FIBER)",7,1010.69,7074.83]
["","","INTERCONNECT CENTER ","(72-FIBER)",1,2265.5100000000002,2265.5100000000002]
["","","METER BASE/DISCONECT COMBINA-","TION PANEL",3,1204.3699999999999,3613.11]
["","","MOD EXT ELECTRICAL","SERVICE EQUIP",3,755.76,2267.2800000000002]
["","","PORT CCTV CAMERA ","LOWERING TOOL",1,1613.65,1613.65]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","INTEGRAT & CONFIGUR","",1,3973.8,3973.8]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","4 SOLID BARE GROUND","CONDUCTOR",620,5.36,3323.2]
["","","3-WIRE COPPER FEEDER ","CONDUCT- ORS",1430,3.18,4547.3999999999996]
["","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",90,7.2,648]
["","","4-WIRE COPPER FEEDER ","CONDUCTORS",1820,4.68,8517.6]
["","","ETHERNET CABLE","",500,1.49,745]
["7992000000-E","GENERIC SIGNAL ITEM(CY)","DMS FOUNDATION","",24,775.04,18600.96]
["8017000000-N","CM&R TEMP ACCESS ******","(15+0900 -L-)","",1,8000,8000]
["","","(20+2050-L-)","",1,25000,25000]
["","","(20+4750-L-)","",1,25000,25000]
["8035000000-N","REMV EXIST STR **********","(15+0900 -L-)","",1,22000,22000]
["","","(15+1400-L-)","",1,39500,39500]
["","","(17+7300-L-)","",1,30000,30000]
["","","(20+2050-L-)","",1,60000,60000]
["","","(20+4750-L-)","",1,60000,60000]
["","","(21+7700-L-)","",1,36000,36000]
["8091000000-N","FND EXCAV B** STA *******","(1 17+3000-L-)","",1,15000,15000]
["","","(2 17+3000-L-)","",1,15000,15000]
["8096000000-E","PILE EXCAVATION IN SOIL","","",270,429.853148148,116060.35]
["8097000000-E","PILE EXCAV NOT IN SOIL","","",176,418.73465909100003,73697.3]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",345.5,675,233212.5]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",218,675,147150]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",77,180,13860]
["8113000000-N","SID INSPECTIONS","","",8,500,4000]
["8114000000-N","SPT TESTING","","",4,1500,6000]
["8115000000-N","CSL TESTING","","",2,2450,4900]
["8121000000-N","UNCL STR EXCAV STA ****","(15+0900 -L-)","",1,15000,15000]
["","","(15+1400-L-)","",1,5700,5700]
["","","(17+7300-L-)","",1,20000,20000]
["","","(20+2050-L-)","",1,25000,25000]
["","","(20+4750-L-)","",1,25000,25000]
["","","(21+7700-L-)","",1,6900,6900]
["8156000000-E","CONC WEARING SURFACE","","",16742,9.1999163779999993,154025]
["8161000000-E","GROOVING BRG FLOORS","","",20824,0.68622742999999997,14290]
["8175000000-E","CL AA CONC (BRG)","","",132.19999999999999,482.22390317700001,63750]
["8182000000-E","CL A CONC (BRG)","","",744.3,748.89677549400005,557403.87]
["8210000000-N","BRG APPR SLAB ***********","(15+0900 -L-)","",1,38000,38000]
["","","(15+1400-L-)","",1,18100,18100]
["","","(17+7300-L-)","",1,30000,30000]
["","","(20+2050-L-)","",1,70000,70000]
["","","(20+4750-L-)","",1,60000,60000]
["","","(21+7700-L-)","",1,11325,11325]
["8217000000-E","REINF STEEL (BRG)","","",147041,0.87569711800000005,128763.38]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",5611,1.42220638,7980]
["8238000000-E","SPIRAL COL REINF STL BRG","","",12881,1.2805682789999999,16495]
["8364000000-E","HP12X53 PILES","","",1415,46.408833921999999,65668.5]
["8365000000-E","HP12X53 GALV PILES","","",275,55,15125]
["8384000000-E","HP14X73 PILES","","",190,57,10830]
["8391000000-N","STEEL PILE POINTS","","",11,150,1650]
["8475000000-E","TWO BAR METAL RAIL","","",885.57,113.28037309299999,100317.7]
["8482000000-E","THREE BAR METAL RAIL","","",162.80000000000001,180,29304]
["8503000000-E","CONC BARRIER RAIL","","",140.19999999999999,100,14020]
["8505000000-E","VERT CONC BARRIER RAIL","","",200,80,16000]
["8517000000-E","1'-**\"X****\"CONC PARAPET","(1'-2\" X 2'-10 1/2\")","",180,74,13320]
["","","(1'-2\" X 3'-0\")","",160,91.27,14603.2]
["","","(1'-2\" x 3'-7 1/2\")","",609.6,115,70104]
["8608000000-E","RIP RAP II (2'-0\")","","",3141,41.687360712999997,130940]
["8622000000-E","GEOTEXTILE FOR DRNG","","",3586,2.5347880649999999,9089.75]
["8657000000-N","ELASTOMERIC BEARINGS","","",5,7273.6,36368]
["8692000000-N","FOAM JOINT SEALS","","",2,27000,54000]
["8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",1950,193.27692307699999,376890]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",1200,239,286800]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",2380,120,285600]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",5171.88,125,646485]

{"sheet":"Items - Div 11","index":13,"n_rows":528,"n_cols":7,"rows_kept":528,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 11"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",11,239600.27545454499,2635603.0299999998]
["0000400000-N","CONST SURVEYING","","",5,92992.991999999998,464964.96]
["0000900000-N","GENERIC MISC ITEM (LS)","ALTERNATE LS BID","BRGS",3,4445985.82,13337957.460000001]
["0000915000-N","GENERIC MISC ITEM (EA)","END BENTS STR 020031","",2,20885.759999999998,41771.519999999997]
["","","END BENTS STR 020046","",2,48953.43,97906.86]
["","","END BENTS STR 020057","",2,20857.990000000002,41715.980000000003]
["","","END BENTS STR 040060","",2,18130.810000000001,36261.620000000003]
["","","END BENTS STR 040061","",2,55051.4,110102.8]
["","","END BENTS STR 040066","",2,64490.51,128981.02]
["","","END BENTS STR 040187","",2,21328.33,42656.66]
["","","END BENTS STR 040350","",2,59360.26,118720.52]
["","","END BENTS STR 040371","",2,22593.19,45186.38]
["","","END BENTS STR 130077","",2,19932.689999999999,39865.379999999997]
["","","END BENTS STR 130164","",2,40139.99,80279.98]
["","","END BENTS STR 850019","",2,15011.88,30023.759999999998]
["","","END BENTS STR 850034","",2,18301.93,36603.86]
["","","END BENTS STR 850094","",2,34574.22,69148.44]
["","","END BENTS STR 850143","",2,15011.88,30023.759999999998]
["","","END BENTS STR 850202","",2,72582.399999999994,145164.79999999999]
["","","END BENTS STR 850203","",2,47007.61,94015.22]
["","","END BENTS STR 850213","",2,42160.08,84320.16]
["","","END BENTS STR 850257","",2,95450.79,190901.58]
["","","END BENTS STR 850322","",2,26154.04,52308.08]
["","","END BENTS STR 960106","",2,25029.06,50058.12]
["","","END BENTS STR 960143","",2,17681.900000000001,35363.800000000003]
["","","END BENTS STR 960144","",2,17350.48,34700.959999999999]
["","","END BENTS STR 960187","",2,17053.47,34106.94]
["","","END BENTS STR 960405","",2,17877.02,35754.04]
["","","END BENTS STR 980091","",2,28520.82,57041.64]
["","","END BENTS STR 980092","",2,53745.52,107491.04]
["","","END BENTS STR 980109","",2,15011.88,30023.759999999998]
["","","INTERIOR BENT CAPS STR","040060",1,26847.16,26847.16]
["","","","130077",1,27766.39,27766.39]
["","","","850019",2,13975.44,27950.880000000001]
["","","","850034",1,18710.490000000002,18710.490000000002]
["","","","850094",2,15947.39,31894.78]
["","","","850143",1,14256.92,14256.92]
["","","","850203",1,13015.16,13015.16]
["","","","960106",2,28823.040000000001,57646.080000000002]
["","","","960143",1,27961.65,27961.65]
["","","","960144",2,24713.07,49426.14]
["","","","960405",2,26801.69,53603.38]
["","","","980109",2,13975.44,27950.880000000001]
["","","RIGHT OF WAY ","ACQUISITION",56,5010.8571428570003,280608]
["0000930000-E","GENERIC MISC ITEM (LF)","AVE FOUND LGTH AT END","BENT 1 STR 020031",12,2827.07,33924.839999999997]
["","","","BENT 1 STR 020046",12,2664.51,31974.12]
["","","","BENT 1 STR 020057",11,3952.04,43472.44]
["","","","BENT 1 STR 040060",14,466.66,6533.24]
["","","","BENT 1 STR 040061",14,1,14]
["","","","BENT 1 STR 040066",11,1,11]
["","","","BENT 1 STR 040187",15,488.25,7323.75]
["","","","BENT 1 STR 040350",13,539.99,7019.87]
["","","","BENT 1 STR 040371",36,439.28,15814.08]
["","","","BENT 1 STR 130077",46,377.49,17364.54]
["","","","BENT 1 STR 130164",16,829.99,13279.84]
["","","","BENT 1 STR 850019",32,258.3,8265.6]
["","","","BENT 1 STR 850034",21,395.09,8296.89]
["","","","BENT 1 STR 850094",36,321.44,11571.84]
["","","","BENT 1 STR 850143",30,249.53,7485.9]
["","","","BENT 1 STR 850202",39,231.93,9045.27]
["","","","BENT 1 STR 850203",12,1,12]
["","","","BENT 1 STR 850213",40,226.13,9045.2000000000007]
["","","","BENT 1 STR 850257",14,1,14]
["","","","BENT 1 STR 850322",15,343.11,5146.6499999999996]
["","","","BENT 1 STR 960106",15,423.9,6358.5]
["","","","BENT 1 STR 960143",44,245.39,10797.16]
["","","","BENT 1 STR 960144",24,325.83,7819.92]
["","","","BENT 1 STR 960187",14,451.95,6327.3]
["","","","BENT 1 STR 960405",23,318.58999999999997,7327.57]
["","","","BENT 1 STR 980091",12,363.9,4366.8]
["","","","BENT 1 STR 980092",21,282.20999999999998,5926.41]
["","","","BENT 1 STR 980109",13,365.9,4756.7]
["","","","BENT 2 STR 020031",16,2153.62,34457.919999999998]
["","","","BENT 2 STR 020046",11,2900.62,31906.82]
["","","","BENT 2 STR 020057",27,1423.62,38437.74]
["","","","BENT 2 STR 040060",13,557.19000000000005,7243.47]
["","","","BENT 2 STR 040061",15,2372.9,35593.5]
["","","","BENT 2 STR 040066",11,1,11]
["","","","BENT 2 STR 040187",24,299.64,7191.36]
["","","","BENT 2 STR 040350",10,1,10]
["","","","BENT 2 STR 040371",37,439.2,16250.4]
["","","","BENT 2 STR 130077",41,396.86,16271.26]
["","","","BENT 2 STR 130164",19,3550.24,67454.559999999998]
["","","","BENT 2 STR 850019",29,258.13,7485.77]
["","","","BENT 2 STR 850034",18,460.94,8296.92]
["","","","BENT 2 STR 850094",32,327.5,10480]
["","","","BENT 2 STR 850143",32,258.3,8265.6]
["","","","BENT 2 STR 850202",39,231.93,9045.27]
["","","","BENT 2 STR 850203",13,365.9,4756.7]
["","","","BENT 2 STR 850213",43,228.49,9825.07]
["","","","BENT 2 STR 850257",13,1,13]
["","","","BENT 2 STR 850322",18,329.24,5926.32]
["","","","BENT 2 STR 960106",14,440.62,6168.68]
["","","","BENT 2 STR 960143",21,370.77,7786.17]
["","","","BENT 2 STR 960144",39,268.91000000000003,10487.49]
["","","","BENT 2 STR 960187",17,403.01,6851.17]
["","","","BENT 2 STR 960405",26,294.66000000000003,7661.16]
["","","","BENT 2 STR 980091",11,396.99,4366.8900000000003]
["","","","BENT 2 STR 980092",26,257.93,6706.18]
["","","","BENT 2 STR 980109",30,249.53,7485.9]
["","","AVE FOUND LGTH AT INTE-","RIOR BENT 1 STR 040060",24,2202.44,52858.559999999998]
["","","","RIOR BENT 1 STR 130077",56,1444.22,80876.320000000007]
["","","","RIOR BENT 1 STR 850019",40,1967.75,78710]
["","","","RIOR BENT 1 STR 850034",27,3607.23,97395.21]
["","","","RIOR BENT 1 STR 850094",43,2601.41,111860.63]
["","","","RIOR BENT 1 STR 850143",42,2096.9899999999998,88073.58]
["","","","RIOR BENT 1 STR 850203",23,5166.2,118822.6]
["","","","RIOR BENT 1 STR 960106",27,3080.43,83171.61]
["","","","RIOR BENT 1 STR 960143",56,1504.34,84243.04]
["","","","RIOR BENT 1 STR 960144",54,1328.96,71763.839999999997]
["","","","RIOR BENT 1 STR 960405",44,1525.51,67122.44]
["","","","RIOR BENT 1 STR 980109",44,1908.54,83975.76]
["","","","RIOR BENT 2 STR 850019",40,1967.75,78710]
["","","","RIOR BENT 2 STR 850094",43,2601.41,111860.63]
["","","","RIOR BENT 2 STR 960106",27,3116.47,84144.69]
["","","","RIOR BENT 2 STR 960144",54,2190.0700000000002,118263.78]
["","","","RIOR BENT 2 STR 960405",44,1534.04,67497.759999999995]
["","","","RIOR BENT 2 STR 980109",44,1908.54,83975.76]
["","","BRG LGTH STR","020031",105,2644.4,277662]
["","","","020046",55,1457.9,80184.5]
["","","","020057",65,1883.81,122447.65]
["","","","040060",105,1843.99,193618.95]
["","","","040061",55,2230.41,122672.55]
["","","","040066",90,2469.25,222232.5]
["","","","040187",70,1704.23,119296.1]
["","","","040350",40,1466.38,58655.199999999997]
["","","","040371",35,1554.79,54417.65]
["","","","130077",135,2484.63,335425.05]
["","","","130164",70,1655.22,115865.4]
["","","","960106",135,1985.59,268054.65000000002]
["","","","960143",95,1889.12,179466.4]
["","","","960144",145,1916.16,277843.20000000001]
["","","","960187",70,1700.63,119044.1]
["","","","960405",140,1525.75,213605]
["","","BRG LGTH STR 850019","",140,1586.41,222097.4]
["","","BRG LGTH STR 850034","",130,3561.74,463026.2]
["","","BRG LGTH STR 850094","",190,2816.13,535064.69999999995]
["","","BRG LGTH STR 850143","",120,1934.03,232083.6]
["","","BRG LGTH STR 850202","",70,1657.51,116025.7]
["","","BRG LGTH STR 850203","",100,1448.17,144817]
["","","BRG LGTH STR 850213","",45,1317.28,59277.599999999999]
["","","BRG LGTH STR 850257","",40,1497.42,59896.800000000003]
["","","BRG LGTH STR 850322","",105,2523.27,264943.34999999998]
["","","BRG LGTH STR 980091","",50,1527.51,76375.5]
["","","BRG LGTH STR 980092","",45,1511.46,68015.7]
["","","BRG LGTH STR 980109","",135,1562.88,210988.79999999999]
["0022000000-E","UNCLAS EXCAVATION","","",315000,7,2205000]
["0029000000-N","REINF BRG APPR **********","(393+5738-L-)","",1,28000,28000]
["","","(71+6063-L-)","",1,19000,19000]
["0030000000-N","BRG APP SUB REG TIER**","(11+00-L-)","",1,17000,17000]
["","","(12+00 -L-)","",1,12200,12200]
["","","(14+35)","",1,8100,8100]
["","","(15+16-L-)","",1,15000,15000]
["0036000000-E","UNDERCUT EXCAVATION","","",6300,4.6503174600000001,29297]
["0043000000-N","GRADING","","",3,364500,1093500]
["0050000000-E","SUPP CLEAR & GRUBBING","","",12,550.34333333300003,6604.12]
["0057000000-E","UNDERCUT EXCAVATION","","",500,12,6000]
["0063000000-N","GRADING","","",5,349897.17800000001,1749485.89]
["0106000000-E","BORROW EXCAVATION","","",11750,3.2626382980000002,38336]
["0134000000-E","DRNG DITCH EXCAVATION","","",4580,6.7969432310000002,31130]
["0141000000-E","BERM DITCH CONST","","",4420,2.6990950229999999,11930]
["0192000000-N","PROOF ROLLING","","",1.9,1300,2470]
["0195000000-E","SELECT GRANULAR MAT'L","","",6650,30.605563910000001,203527]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",8690,1.8166858459999999,15787]
["0199000000-E","TEMP SHORING","","",10260,41.586549708,426678]
["0241000000-E","GENERIC GRAD ITM (SY)","SOIL NAIL SLOPE STABIL","",2500,175,437500]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISP OF PETROLEUM","CONTAMINATED SOIL",300,64,19200]
["0262000000-N","GENERIC GRAD ITEM (EA)","SOIL NAIL PROOF TESTS","",1,425,425]
["","","SOIL NAIL VERIFICATION ","TESTS",1,695,695]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",1821,24.017188357999999,43735.3]
["0320000000-E","FND CONDIT GEOTEXTILE","","",5746,2.8580577790000001,16422.400000000001]
["0335100000-E","12\" DRNG PIPE","","",52,30,1560]
["0335200000-E","15\" DRNG PIPE","","",1032,37.286821705000001,38480]
["0335300000-E","18\" DRNG PIPE","","",572,38.271538462000002,21891.32]
["0335400000-E","24\" DRNG PIPE","","",208,53.490384615000004,11126]
["0335500000-E","30\" DRNG PIPE","","",116,60,6960]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",10,90,900]
["0342000000-E","**\" SIDE DRN PIPE","(12\")","",124,22,2728]
["0343000000-E","15\" SIDE DRN PIPE","","",88,31.75,2794]
["0366000000-E","15\" RC PIPE CULV III","","",1292,32.691981423999998,42238.04]
["0372000000-E","18\" RC PIPE CULV III","","",4642,33.169426971,153972.48000000001]
["0378000000-E","24\" RC PIPE CULV III","","",3598,45.797932185000001,164780.96]
["0384000000-E","30\" RC PIPE CULV III","","",1252,57.659552716,72189.759999999995]
["0390000000-E","36\" RC PIPE CULV III","","",188,73,13724]
["0396000000-E","42\" RC PIPE CULV III","","",172,94,16168]
["0414000000-E","60\" RC PIPE CULV III","","",172,200,34400]
["0426000000-E","72\" RC PIPE CULV III","","",100,270,27000]
["0448200000-E","15\" RCP CULV CL IV","","",68,41.647058823999998,2832]
["0448400000-E","24\" RCP CULV CL IV","","",160,56.5,9040]
["0453000000-E","**\" PIPE END SECTION","(15\")","",1,500,500]
["","","(18\")","",30,685,20550]
["","","(24\")","",13,805,10465]
["","","(30\")","",8,990,7920]
["0576000000-E","**\" CS PIPE CULV *****\"","(96\" 0168\")","",80,415,33200]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",512,39.507968750000003,20228.080000000002]
["0588000000-E","18\" CS PIPE CULV 0064\"","","",386,44.529637305999998,17188.439999999999]
["0594000000-E","24\" CS PIPE CULV 0064\"","","",236,52.406779661000002,12368]
["0600000000-E","30\" CS PIPE CULV 0079\"","","",456,66.037894737000002,30113.279999999999]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\" 0064\")","",8,315,2520]
["","","(15\" 0064)","",9,278.10000000000002,2502.9]
["","","(18\" 0064\")","",15,358.66,5379.9]
["","","(24\" 0064\")","",4,505,2020]
["","","(30\" 0079\")","",7,668.62857142899998,4680.3999999999996]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\" 0500\")","",44,470,20680]
["","","(18\" 0500\")","",40,488,19520]
["","","(24\" 0500\")","",316,285.03797468400001,90072]
["","","(30\" 0500\")","",393,219,86067]
["","","(36\" 0500\")","",48,377,18096]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\" 0500\")","",16,25,400]
["","","(18\" 0500\")","",16,25,400]
["","","(24\" 05\")","",76,875,66500]
["","","(24\" 0500\")","",32,25,800]
["","","(30\" 05\")","",131,1120,146720]
["","","(36\" 05\")","",16,1540,24640]
["0986000000-E","GENERIC PIPE ITEM (LF)","15\" CS SLOTTED DRN 0064\" THICK","",96,177.64,17053.439999999999]
["","","30\" CCFRPM PIPE","",208,650,135200]
["","","42\" CCFRPM PIPE","",68,750,51000]
["","","54\" CCFRPM PIPE","",64,1000,64000]
["0995000000-E","PIPE REMOVAL","","",3352.4,11.394687387999999,38199.550000000003]
["1077000000-E","57 STONE","","",20,30,600]
["1099500000-E","SHALLOW UNDERCUT","","",2615,8.5443785850000005,22343.55]
["1099700000-E","CL IV SUBGRD STABIL","","",4823,25.701845324000001,123960]
["1121000000-E","AGG BASE COURSE","","",7800,21.421371794999999,167086.70000000001]
["1220000000-E","INCIDENTAL STONE BASE","","",1285,25.420544747000001,32665.4]
["1275000000-E","PRIME COAT","","",427,10,4270]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",5650,1.45,8192.5]
["","","(3\")","",7800,4,31200]
["1308000000-E","MILL ASP PVMT ***** - ****","(0\" TO 3\")","",890,14.6,12994]
["1330000000-E","INCIDENTAL MILLING","","",500,10,5000]
["1489000000-E","ASP CNC BAS CRS B250B","","",1501,67.136275815999994,100771.55]
["1491000000-E","ASP CNC BAS CRS B250C","","",12030,56.032418952999997,674070]
["1498000000-E","ASP CNC INTR CRS I190B","","",2937,58.228345249999997,171016.65]
["1503000000-E","ASP CNC INTR CRS I190C","","",8363,55.007533182000003,460028]
["1519000000-E","ASP CNC SURF CRS S95B","","",3414,58.900571178,201086.55]
["1523000000-E","ASP CNC SURF CRS S95C","","",27144,47.017830828000001,1276252]
["1525000000-E","ASP CONC SURF CRS SF95A","","",570,78.421052631999999,44700]
["1575000000-E","ASP FOR PLANT MIX","","",3016,677.48342175100004,2043290]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",1460,200,292000]
["1840000000-E","MILLED RUMBLE STRIPS","","",830,6.95,5768.5]
["2000000000-N","RIGHT OF WAY MARKERS","","",429,134.51048951000001,57705]
["2022000000-E","SUBDRN EXCAVATION","","",646.79999999999995,14.79576376,9569.9]
["2033000000-E","SUBDRN FINE AGG","","",474.2,48.651476170000002,23070.53]
["2044000000-E","6\" PERF SUBDRN PIPE","","",2800,10.900357143000001,30521]
["2070000000-N","SUBDRN PIPE OUTLET","","",9,199.722222222,1797.5]
["2077000000-E","6\" OUTLET PIPE","","",54,17.342222222,936.48]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",2,1000,2000]
["2209000000-E","ENDWALLS","","",68.5,850,58225]
["2220000000-E","REINF ENDWALLS","","",37.9,1100,41690]
["2253000000-E","PIPE COLLARS","","",0.84599999999999997,1200,1015.2]
["2264000000-E","PIPE PLUGS","","",1.903,1628.9542827119999,3099.9]
["2275000000-E","FLOWABLE FILL","","",210,210,44100]
["2286000000-N","MASNRY DRNG STRUCT","","",160,1077.25,172360]
["2297000000-E","MASNRY DRNG STRUCT","","",17.3,1050,18165]
["2308000000-E","MASNRY DRNG STRUCT","","",35.520000000000003,199.09628378400001,7071.9]
["2364000000-N","FRM W/2GRTS 84016 STD","","",3,650,1950]
["2364200000-N","FRM W/2GRTS 84020 STD","","",4,400,1600]
["2365000000-N","FRM W/2GRTS 84022 STD","","",6,488.33333333299998,2930]
["2366000000-N","FRM W/2GRTS 84024 STD","","",71,745.77464788700001,52950]
["2367000000-N","FRM W/2GRTS 84029 STD","","",5,699,3495]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",1,425,425]
["","","(F)","",18,440,7920]
["","","(G)","",18,440,7920]
["2396000000-N","FRM W/COVER STD 84054","","",4,407.5,1630]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",20,1800,36000]
["2418000000-E","FRM W/GRATES DRIVEWY DI","","",44,200,8800]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",1,550,550]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",160,30,4800]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",6655,16.8,111804]
["2556000000-E","SHOULDER BERM GUTR","","",830,20.626506024000001,17120]
["2577000000-E","CONC EXPRESSWY GUTR","","",3170,20.283911671999999,64300]
["2580000000-E","CONC VALLEY GUTR","","",160,15,2400]
["2591000000-E","4\" CONC SIDEWALK","","",1340,29.3,39262]
["2605000000-N","CONC CURB RAMP","","",3,1428,4284]
["2619000000-E","4\" CONC PAVED DITCH","","",230,71.391304348000006,16420]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",80,85,6800]
["2752000000-E","GENERIC PAVING ITEM(LF)","SPEC SHDR BERM CURB","",20,40,800]
["3030000000-E","STL BM GUARDRAIL","","",12937.5,15.127033816000001,195706]
["3045000000-E","SBGR SHOP CURVED","","",5225,16.235885166999999,84832.5]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",105,24.40952381,2563]
["3165000000-N","GR ANCHOR  **********","(350 TL-2)","",6,1566.6666666670001,9400]
["","","(350 TL-2)","",2,1750,3500]
["3195000000-N","GR ANCHOR  AT-1","","",13,456.923076923,5940]
["3210000000-N","GR ANCHOR  CAT-1","","",6,458.33333333299998,2750]
["3215000000-N","GR ANCHOR  III","","",26,1453.0769230769999,37780]
["3270000000-N","GR ANCHOR  350","","",101,1677.2277227720001,169400]
["3285000000-N","GR ANCHOR  M-350","","",6,1600,9600]
["3317000000-N","GR ANCHOR  B-77","","",4,1450,5800]
["3360000000-E","REM EXISTING GUARDRAIL","","",17546,0.90860595,15942.4]
["3380000000-E","TEMP STL BM GUARDRAIL","","",1850,6,11100]
["3382000000-E","TEMP STL BM GDRAIL SHP CURV","","",125,6.6,825]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(AT-1)","",4,275,1100]
["","","(B-77)","",4,900,3600]
["","","(CAT-1)","",2,425,850]
["","","(III)","",4,1000,4000]
["3389000000-N","TEMP GDRL ANCH UNIT****","(350 TL-2)","",3,900,2700]
["3389100000-N","TEMP GDRL ANCH UNIT350","","",23,1000,23000]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",200,4.33,866]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",15,17.920000000000002,268.8]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",6,26.88,161.28]
["3557000000-E","ADDITIONAL BARB WIRE","","",50,1.1200000000000001,56]
["3559000000-E","** STRAND BW FENCE W/ POSTS","(4)","",200,5.04,1008]
["3563000000-E","TEMP **\" WW FENCE W/POSTS","(48\")","",12784,3,38352]
["3575000000-E","GENERIC FENCING ITEM (LF)","TEMP 4 STRAND BARBED WIRE","FENCE WITH POSTS",10000,2.9,29000]
["","","TEMP 72\" CHAIN LINK FENCEWITH POSTS","",500,12,6000]
["3628000000-E","RIP RAP CL I","","",423,38.352340425999998,16223.04]
["3635000000-E","RIP RAP CL II","","",247,37.429149797999997,9245]
["3642000000-E","RIP RAP CL A","","",10,30,300]
["3649000000-E","RIP RAP CL B","","",1388,31.097795389000002,43163.74]
["3651000000-E","BOULDERS","","",53,82.075471698000001,4350]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",15314,1.948051456,29832.46]
["3659000000-N","PREFORM SCOUR HOLES","","",1,2500,2500]
["4025000000-E","CONTR FURN  ***SIGN","(E)","",79.5,13.5,1073.25]
["4054000000-E","PLN CONC FOUNDTN","","",1,25,25]
["4060000000-E","SUPPT BRKAWY STL BM","","",295,4,1180]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",2860,4.477055944,12804.38]
["4096000000-N","SIGN ERECTION  D","","",6,95,570]
["4102000000-N","SIGN ERECTION  E","","",134,51.611940298999997,6916]
["4108000000-N","SIGN ERECTION  F","","",6,65,390]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(A)","",1,1400,1400]
["","","(D)","",2,95,190]
["","","(E)","",5,65,325]
["4138000000-N","DISP SUPPT STL BM","","",1,375,375]
["4155000000-N","DISP SIGN SYST U-CHAN","","",122,1,122]
["4158000000-N","DISP SIGN SYST WOOD","","",10,1,10]
["4192000000-N","DISP SUPPT U-CHAN","","",3,1,3]
["4400000000-E","WORK ZONE SIGN (STAT)","","",5919,4.6218465960000001,27356.71]
["4405000000-E","WORK ZONE SIGN (PORT)","","",1593,11.781726302999999,18768.29]
["4410000000-E","WORK ZONE SIGN (BARR)","","",1110,5.6182162160000004,6236.22]
["4415000000-N","FLASH ARROW BOARD","","",8,1623.75,12990]
["4420000000-N","PORT CHANGE MSG SIGN","","",6,7658.3333333330002,45950]
["4430000000-N","DRUMS","","",1963,41.384615384999996,81238]
["4435000000-N","CONES","","",524,17.792729007999998,9323.39]
["4445000000-E","BARRICADES ( III)","","",920,17.780869565,16358.4]
["4450000000-N","FLAGGER","","",2980,19.687248321999999,58668]
["4455000000-N","FLAGGER","","",1875,220,412500]
["4465000000-N","TEMP CRASH CUSHIONS","","",13,4315.384615385,56100]
["4470000000-N","RESET CRASH CUSHION","","",26,1157.692307692,30100]
["4480000000-N","TMA","","",8,5508,44064]
["4485000000-E","PORT CONC BARR","","",3154,21.254121749999999,67035.5]
["4490000000-E","PORT CONC BARR(ANCH)","","",410,31,12710]
["4500000000-E","RESET PORT CONC BARR","","",3080,3.3051948050000002,10180]
["4505000000-E","RESET PORT CONC BARRANCH","","",650,9,5850]
["4510000000-N","LAW ENFORCEMENT","","",240,40,9600]
["4516000000-N","SKINNY DRUM","","",539,28.910946197000001,15583]
["4600000000-N","GENERIC TRAFFIC CNTRL ITEM (EA)","TEMP PORTABLE TRAFFIC","SIGNAL SYSTEM",6,16000,96000]
["4650000000-N","TEMP RAISED PVMT MRKS","","",665,5.9924812029999996,3985]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",1212,3.7376237620000001,4530]
["4710000000-E","24\"WIDE THERMO 120 MIL","","",517,7.4429400389999998,3848]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",44,115.909090909,5100]
["4770000000-E","4\" COLD APPL PLSTIC LINES  **","(IV)","",600,2,1200]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",77462,0.32720637200000002,25346.06]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",889,2.1282339709999998,1892]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",668,3.4520958080000002,2306]
["4845000000-N","PAINT PVT MKG SYMBOL","","",14,67.142857143000001,940]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",229592,0.693681836,159263.79999999999]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",16247,0.664864283,10802.05]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",203,3,609]
["4900000000-N","PERM RAISED PVMT MKRS","","",10,75,750]
["4905000000-N","SNOWPLB PVMT MRKER","","",752,28.878989361999999,21717]
["5325200000-E","2\" H2O LINE","","",28,55,1540]
["5325600000-E","6\" H2O LINE","","",86,60,5160]
["5325800000-E","8\" H2O LINE","","",37,79.594594595000004,2945]
["5326000000-E","10\" H2O LINE","","",4851,33,160083]
["5326200000-E","12\" H2O LINE","","",1794,78.75,141277.5]
["5540000000-E","6\" VALVE","","",1,1100,1100]
["5546000000-E","8\" VALVE","","",2,1900,3800]
["5552000000-E","10\" VALVE","","",3,2000,6000]
["5558000000-E","12\" VALVE","","",4,3875,15500]
["5589200000-E","2\" AIR RELEASE VALVE","","",2,3500,7000]
["5648000000-N","RELOCATE H2O METER","","",3,800,2400]
["5649000000-N","RECONNECT H2O METER","","",4,800,3200]
["5672000000-N","RELOCATE FIRE HYDRANT","","",4,1400,5600]
["5691300000-E","8\" SANIT GRAV SEWER","","",1771,32.273574252000003,57156.5]
["5691500000-E","12\" SANIT GRAV SEWER","","",117,200,23400]
["5709200000-E","4\" FORCE MAIN SEWER","","",2870,30.108013936999999,86410]
["5775000000-E","4' DIA UTILITY MH","","",10,3150,31500]
["5776000000-E","5' DIA UTILITY MH","","",6,4800,28800]
["5816000000-N","ABAND UTILITY MH","","",4,700,2800]
["6000000000-E","TEMP SILT FENCE","","",97440,1.579145628,153871.95000000001]
["6006000000-E","EROS CNTRL STONE CL A","","",3545,27.957376586999999,99108.9]
["6009000000-E","EROS CNTRL STONE CL B","","",10980,31.025227687000001,340657]
["6012000000-E","SEDIMENT CNTRL STONE","","",10735,27.775328365,298168.15000000002]
["6015000000-E","TEMP MULCHING","","",170,628.33170588200005,106816.39]
["6018000000-E","SEED FOR TEMP SEEDING","","",7150,1.834895105,13119.5]
["6021000000-E","FERT FOR TEMP SEEDING","","",37,875.27027026999997,32385]
["6024000000-E","TEMP SLOPE DRNS","","",4625,10.339675676000001,47821]
["6029000000-E","SAFETY FENCE","","",12100,1.55768595,18848]
["6030000000-E","SILT EXCAVATION","","",16300,4.1054907979999999,66919.5]
["6036000000-E","MAT FOR EROS CNTRL","","",222605,1.398321017,311273.25]
["6037000000-E","COIR FIBER MAT","","",10697,4.407045901,47142.17]
["6038000000-E","PERM SOIL REINF MAT","","",13650,4.1615934069999998,56805.75]
["6042000000-E","1/4\" HARDWARE CLOTH","","",20895,3.0896075619999999,64557.35]
["6045000000-E","**\" TEMP PIPE","(18\")","",820,26,21320]
["","","(24\")","",250,35,8750]
["6048000000-E","FLOAT TURBIDITY CURTN","","",450,25,11250]
["6070000000-N","SPECIAL STILLING BASINS","","",65,330.885538462,21507.56]
["6071010000-E","WATTLE","","",21375,4.1970011700000001,89710.9]
["6071012000-E","COIR FIBER WATTLE","","",30,20.55,616.5]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",12830,0.66464536200000002,8527.4]
["6071030000-E","COIR FIBER BAFFLE","","",4500,4.3794444439999998,19707.5]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",58,633.62068965499998,36750]
["6084000000-E","SEEDING & MULCHING","","",211.5,1375.675650118,290955.40000000002]
["6087000000-E","MOWING","","",56.7,81.8,4638.0600000000004]
["6090000000-E","SEED FOR REPAIR SEED","","",2900,2.2186206899999998,6434]
["6093000000-E","FERT FOR REPAIR SEED","","",8.75,868.45371428600004,7598.97]
["6096000000-E","SEED FOR SUPP SEEDING","","",4950,1.966414141,9733.75]
["6108000000-E","FERTILIZER TOPDRESSING","","",144.5,732.08761245699998,105786.66]
["6111000000-E","IMPERVIOUS DIKE","","",730,59.685479452000003,43570.400000000001]
["6114500000-N","SPECIALIZED HAND MOW","","",220,14.732727273,3241.2]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",314,91.911401273999999,28860.18]
["6120000000-E","CLVT DIVERSION CHANNL","","",70,20,1400]
["6123000000-E","REFORESTATION","","",2.35,2743.8297872339999,6448]
["6126000000-E","STRMBNK REFORESTATN","","",0.8,3500,2800]
["7060000000-E","SIGNAL CABLE","","",3610,2.3963988920000001,8651]
["7120000000-E","VEHICLE SIGNAL HD (12\" 3 SECT)","","",23,824.13043478300006,18955]
["7132000000-E","VEHICLE SIGNAL HD (12\" 4 SECT)","","",2,925,1850]
["7144000000-E","VEHICLE SIGNAL HD (12\" 5 SECT)","","",1,1200,1200]
["7264000000-E","MESSENGER CABLE (3/8\")","","",1220,3.0975409840000001,3779]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",710,6,4260]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",330,3.4090909090000001,1125]
["7301000000-E","DIRECT DRILL (***********)","(2 2\")","",270,18,4860]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",11,300,3300]
["7360000000-N","WOOD POLE","","",14,780.35714285699999,10925]
["7372000000-N","GUY ASSEMBLY","","",16,226.875,3630]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",2,452.5,905]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",8,427.5,3420]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",1160,6.6137931029999999,7672]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",3460,1.4432080920000001,4993.5]
["7484000000-N","MICROWAVE VEHICLE DETECTOR","","",4,1862.5,7450]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",4,11745,46980]
["7613000000-N","SOIL TEST","","",4,900,3600]
["7614100000-E","DRILLED PIER FOUND","","",30,500,15000]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",4,100,400]
["7636000000-N","SIGN FOR SIGNALS","","",4,295,1180]
["7684000000-N","SIGNAL CABINET FOUND","","",1,900,900]
["7756000000-N","CONTLR WITH CBNT 2070L BASE MTD","","",1,10750,10750]
["7768000000-N","CONTLR WITH CBNT 2070L POLE MTD","","",2,11375,22750]
["7780000000-N","DETECTOR CARD ( 2070L)","","",8,105,840]
["7901000000-N","CABINET BASE EXTENDER","","",1,375,375]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","MICROWAVE VEHICLE DETECTION","SYSTEM-MULTIPLE ZONES",1,5750,5750]
["","","POWDER COAT FOR SINGLE MAST","ARM POLE (COLOR BLACK)",4,910,3640]
["8007000000-N","CM&R TEMP STR ***********","(15+1600-L-)","",1,135000,135000]
["8017000000-N","CM&R TEMP ACCESS ******","(11+9750-L-)","",1,21100,21100]
["8021000000-N","REMV EXIST STR **********","(14+3500 -L-)","",1,30000,30000]
["","","(15+1600-L-)","",1,30000,30000]
["8035000000-N","REMV EXIST STR **********","(11+9750-L-)","",1,32500,32500]
["","","(13+6150-L-)","",1,8069.39,8069.39]
["","","(14-6276-L1-)","",1,103500,103500]
["","","(15+6728-L-)","",1,133500,133500]
["","","(393+5738-L-)","",1,35000,35000]
["","","(71+5383-L-)","",1,25000,25000]
["8049000000-N","REMV EXIST STR **********","(21+6900-L-)","",1,35000,35000]
["8056000000-N","REMV EXIST STR **********","(442+1360-L-)","",1,10000,10000]
["8091000000-N","FND EXCAV B** STA *******","(1 14-6276-L1-)","",1,5000,5000]
["","","(1 15+6728-L-)","",1,6500,6500]
["8096000000-E","PILE EXCAVATION IN SOIL","","",233,291.502145923,67920]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",265,613.20754717,162500]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",32.1,1449.229906542,46520.28]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",51,1449.23,73910.73]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",29,371.62,10776.98]
["8112730000-N","PDA TESTING","","",3,2316.6666666669998,6950]
["8113000000-N","SID INSPECTIONS","","",6,400,2400]
["8114000000-N","SPT TESTING","","",6,700,4200]
["8115000000-N","CSL TESTING","","",1,2450,2450]
["8121000000-N","UNCL STR EXCAV STA ***","(11+0019-L-)","",1,6000,6000]
["","","(11+9750-L-)","",1,9500,9500]
["","","(14+3500 -L-)","",1,7000,7000]
["","","(15+1600-L-)","",1,5000,5000]
["","","(393+5738-L-)","",1,12000,12000]
["","","(71+5383-L-)","",1,10000,10000]
["8126000000-N","CULV EXCAV @ ************","(13+6150-L-)","",1,17477.59,17477.59]
["","","(21+6900-L-)","",1,20000,20000]
["","","(405+2806-L-)","",1,20000,20000]
["","","(442+1360-L-)","",1,18000,18000]
["","","(52+4145-L-)","",1,1500,1500]
["8133000000-E","FND CONDIT MAT BOX CULV","","",489,47.000899795999999,22983.439999999999]
["8147000000-E","REINF CONC DECK SLAB","","",21504,28.422126116000001,611189.4]
["8156000000-E","CONC WEARING SURFACE","","",3647,13.1,47775.7]
["8161000000-E","GROOVING BRG FLOORS","","",24669,1.125288013,27759.73]
["8182000000-E","CL A CONC (BRG)","","",670,783.30528358200002,524814.54]
["8196000000-E","CL A CONC (CULV)","","",780.6,593.320163976,463145.72]
["8210000000-N","BRG APPR SLAB ***********","(11+0019-L-)","",1,40000,40000]
["","","(11+9750-L-)","",1,17300,17300]
["","","(14+3500 -L-)","",1,26000,26000]
["","","(14-6276-L1-)","",1,21200,21200]
["","","(15+1600-L-)","",1,25000,25000]
["","","(15+6728-L-)","",1,32350,32350]
["","","(393+5738-L-)","",1,31000,31000]
["","","(71+5383-L-)","",1,35000,35000]
["8217000000-E","REINF STEEL (BRG)","","",100509,1.136901173,114268.8]
["8238000000-E","SPIRL COL REINF STL BRG","","",4512,1.9325509750000001,8719.67]
["8245000000-E","REINF STEEL (CULVERT)","","",97589,1.1051380790000001,107849.32]
["8259000000-E","36\" PRESTR CONC GIRDR","","",520.5,166.04,86423.82]
["8262000000-E","45\" PRESTR CONC GIRDR","","",1489.05,183.590000336,273374.69]
["8265000000-E","54\" PRESTR CONC GIRDR","","",586.94000000000005,260,152604.4]
["8364000000-E","HP12X53 PILES","","",1575,60.202222222000003,94818.5]
["8384000000-E","HP14X73 PILES","","",2900,50.929431033999997,147695.35]
["8384200000-E","HP14X73 GALV PILES","","",580,92.413793103000003,53600]
["8391000000-N","STEEL PILE POINTS","","",101,164.20792079200001,16585]
["8475000000-E","TWO BAR METAL RAIL","","",573.04999999999995,119.65999476499999,68571.16]
["8503000000-E","CONC BARR RAIL","","",265.74,86.609994732000004,23015.74]
["8505000000-E","VERT CONC BARR RAIL","","",726.95,99.691519361999994,72470.75]
["8517000000-E","1'-**\"X****\"CONC PARAPET","(1'-2 3/4\" X 2'-6\")","",605.01,98.580006941999997,59641.89]
["8531000000-E","4\" SLOPE PROTECTION","","",64,115,7360]
["8608000000-E","RIP RAP II (2'-0\")","","",1799,27.882712617999999,50161]
["8622000000-E","GEOTEXTILE FOR DRNG","","",2004,2.3161377249999999,4641.54]
["8657000000-N","ELASTOMERIC BEARINGS","","",6,7100.54,42603.24]
["8692000000-N","FOAM JOINT SEALS","","",2,10125,20250]
["8706000000-N","EXPANSION JOINT SEALS","","",1,86675,86675]
["8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",800,185,148000]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",900,235,211500]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",2475,134.54545454500001,333000]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",900,190,171000]
["8801000000-E","MSE RETAIN WALL NO **","(1 @ END BENT 1","STA 14+6276-L1-)",1736,76.69,133133.84]
["","","","STA15+6728-L-)",1953,85.6,167176.79999999999]
["","","(1)","",2456,110,270160]
["","","(2 @ END BENT 2","STA 14+6276-L1-)",1912,77.400000000000006,147988.79999999999]
["","","","STA 15+6728-L-)",2216,81.66,180958.56]
["","","(2)","",1250,100,125000]
["8802010000-E","SOIL NAIL RETAINING WALLS","","",1272,110,139920]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",1,1200,1200]
["8802015110-N","SOIL NAIL PROOF TESTS","","",6,600,3600]
["8802040000-E","CIP GRAV RETAINING WALLS","","",878,90,79020]
["8867000000-E","GENERIC STR ITEM (LF)","SPECIAL CNC BARR RAIL","",200.5,420,84210]
["8892000000-E","GENERIC STR ITEM (SF)","18\" STEEL SHEET PILES","",2150,32,68800]
["","","TEMP SHORING","",430,42,18060]

{"sheet":"Items - Div 12","index":14,"n_rows":560,"n_cols":7,"rows_kept":560,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 12"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",11,313056.83363636403,3443625.17]
["0000400000-N","CONST SURVEYING","","",4,146875,587500]
["0000900000-N","GENERIC MISC ITEM (LS)","DESIGN & CONST OF","BRGS",1,1439895,1439895]
["","","INSPECT BLDG: COMPLETEGENERAL","CONST & ALL SYST INDICATED",1,600000,600000]
["","","SCALE BLDG & BOOTH: COMPLETE GEN CONST","& ALL SYST INDICATED",1,900000,900000]
["0000915000-N","GENERIC MISC ITEM (EA)","END BENTS STR 010071","",2,29600,59200]
["","","END BENTS STR 010079","",2,26000,52000]
["","","END BENTS STR 010081","",2,31000,62000]
["","","END BENTS STR 010246","",2,29000,58000]
["","","END BENTS STR 480282","",2,27500,55000]
["","","INTERIOR BENT CAP STR","010079",2,23000,46000]
["","","","010081",1,32280,32280]
["","","","480282",2,20000,40000]
["","","RIGHT OF WAY ","ACQUISITION",10,3200,32000]
["0000930000-E","GENERIC MISC ITEM (LF)","AVE FOUND LGTH AT END","BENT 1 STR 010071",19,1,19]
["","","","BENT 1 STR 010079",37,1,37]
["","","","BENT 1 STR 010081",30,1,30]
["","","","BENT 1 STR 010246",20,1,20]
["","","","BENT 1 STR 480282",19,1,19]
["","","","BENT 2 STR 010071",14,1,14]
["","","","BENT 2 STR 010079",36,1,36]
["","","","BENT 2 STR 010081",45,1,45]
["","","","BENT 2 STR 010246",16,1,16]
["","","","BENT 2 STR 480282",24,1,24]
["","","AVE FOUND LGTH AT INTE-","RIOR BENT 1 STR 010079",52,3700,192400]
["","","","RIOR BENT 1 STR 010081",57,4260,242820]
["","","","RIOR BENT 1 STR 480282",34,4200,142800]
["","","","RIOR BENT 2 STR 010079",52,3700,192400]
["","","","RIOR BENT 2 STR 480282",34,4200,142800]
["","","BRG LGTH STR 010071","",70,2500,175000]
["","","BRG LGTH STR 010079","",130,2300,299000]
["","","BRG LGTH STR 010081","",100,2400,240000]
["","","BRG LGTH STR 010246","",70,2400,168000]
["","","BRG LGTH STR 480282","",190,2500,475000]
["0001000000-E","CLEARING & GRUBBING","","",94,10875.514468085001,1022298.36]
["0008000000-E","SUPP CLEAR & GRUBBING","","",8,5312.5,42500]
["0015000000-N","SEALING ABANDON WELL","","",16,750,12000]
["0022000000-E","UNCLAS EXCAVATION","","",2106900,3.4641036590000001,7298520]
["0029000000-N","REINF BRG APPR **********","(157+7550 -L- EB)","",1,24500,24500]
["","","(157+7550 -L- WB)","",1,24500,24500]
["","","(16+8314 -Y5-)","",1,42350,42350]
["","","(247+7914 -L- LT)","",1,25000,25000]
["","","(248+1265 -L- RT)","",1,28000,28000]
["","","(28+2706 -Y1-)","",1,46000,46000]
["","","(340+4708 -L- LT)","",1,27000,27000]
["","","(340+9321 -L- RT)","",1,30000,30000]
["0030000000-N","BRG APP SUB REG TIER**","(16+8350)","",1,10000,10000]
["0036000000-E","UNDERCUT EXCAVATION","","",16083,5.678014052,91319.5]
["0043000000-N","GRADING","","",3,87333.333333332994,262000]
["0050000000-E","SUPP CLEAR & GRUBBING","","",3,67,201]
["0057000000-E","UNDERCUT EXCAVATION","","",300,17.263333332999999,5179]
["0063000000-N","GRADING","","",1,96000,96000]
["0106000000-E","BORROW EXCAVATION","","",743300,2.495156733,1854650]
["0134000000-E","DRNG DITCH EXCAVATION","","",18549,1.4914227179999999,27664.400000000001]
["0141000000-E","BERM DITCH CONST","","",3290,2.59,8521.1]
["0156000000-E","REML OF EXT ASPH PVT","","",18080,3.1521017699999998,56990]
["0163000000-E","REML OF EXT CONC PVT","","",440,6.4,2816]
["0170000000-E","REML OF CONC PVT SLBS","","",4000,65,260000]
["0177000000-E","BRKING OF EXT ASPH PVT","","",1900,1.64,3116]
["0192000000-N","PROOF ROLLING","","",75,262,19650]
["0194000000-E","SEL GRANULR MATL CL III","","",4500,25,112500]
["0195000000-E","SEL GRANULAR MAT'L","","",5100,24.901960784,127000]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",30750,2.1521951220000002,66180]
["0223000000-E","ROCK PLATING","","",8500,60,510000]
["0255000000-E","GENERIC GRAD ITEM (TON)","AGG SHDR BORROW","",14183,21.314037933000002,302297]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",5351,20.927303307999999,111982]
["0320000000-E","FND CONDIT GEOTEXTILE","","",26726,1.4551043930000001,38889.120000000003]
["0335200000-E","15\" DRNG PIPE","","",32,50,1600]
["0342000000-E","**\" SIDE DRN PIPE","(36\")","",136,94,12784]
["","","(48\")","",20,165,3300]
["0343000000-E","15\" SIDE DRN PIPE","","",3100,40,124000]
["0344000000-E","18\" SIDE DRN PIPE","","",1182,43,50826]
["0345000000-E","24\" SIDE DRN PIPE","","",1124,56,62944]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",59,440,25960]
["","","(18\")","",9,530,4770]
["","","(24\")","",10,700,7000]
["","","(36\")","",2,710,1420]
["0354000000-E","***\" RC PIPE CULV *****","(12\" V)","",116,35,4060]
["","","(18\" V)","",300,45,13500]
["","","(36\" V)","",272,75,20400]
["0360000000-E","12\" RC PIPE CULV III","","",488,24,11712]
["0366000000-E","15\" RC PIPE CULV III","","",8972,29.249219794999998,262424]
["0372000000-E","18\" RC PIPE CULV III","","",4624,34,157216]
["0378000000-E","24\" RC PIPE CULV III","","",2990,43.752267559000003,130819.28]
["0384000000-E","30\" RC PIPE CULV III","","",1056,54.242424241999998,57280]
["0390000000-E","36\" RC PIPE CULV III","","",1004,74.820717130999995,75120]
["0396000000-E","42\" RC PIPE CULV III","","",352,96.022727273000001,33800]
["0402000000-E","48\" RC PIPE CULV III","","",100,123,12300]
["0426000000-E","72\" RC PIPE CULV III","","",24,180,4320]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",580,118,68440]
["","","(54\")","",488,150,73200]
["","","(60\")","",964,185,178340]
["","","(66\")","",1188,230,273240]
["0448200000-E","15\" RCP CULV CL IV","","",1720,33,56760]
["0448300000-E","18\" RCP CULV CL IV","","",376,41,15416]
["0448400000-E","24\" RCP CULV CL IV","","",528,50.409090909,26616]
["0448500000-E","30\" RCP CULV CL IV","","",528,62.606060606,33056]
["0448600000-E","36\" RCP CULV CL IV","","",676,88,59488]
["0546000000-E","**\" CAA PIPE CLVT *****\"","(4\" 0064\")","",56,27,1512]
["0576000000-E","**\" CS PIPE CULV *****\"","(36\" 0079\")","",156,88,13728]
["","","(42\" 0109\")","",216,119,25704]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",422,47.161137441000001,19902]
["0588000000-E","18\" CS PIPE CULV 0064\"","","",820,41.804878049000003,34280]
["0594000000-E","24\" CS PIPE CULV 0064\"","","",256,63,16128]
["0600000000-E","30\" CS PIPE CULV 0079\"","","",128,112,14336]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\" 0064\")","",5,570,2850]
["0974000000-E","**\"WLD STL PIPE ***\" B RR","(24\" 0312\")","",56,285,15960]
["","","(42\" 0625\")","",56,565,31640]
["0986000000-E","GENERIC PIPE ITEM (LF)","NCDOT APPROVED PIPE ","LINER",253,1275,322575]
["0995000000-E","PIPE REML","","",784,15.981186224,12529.25]
["1011000000-N","FINE GRADING","","",2,202500,405000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",29870,2.65,79155.5]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",300,210,63000]
["1077000000-E","57 STONE","","",80,40,3200]
["1099500000-E","SHALLOW UNDERCUT","","",4845,8.0237358099999998,38875]
["1099700000-E","CL IV SUBGRD STABIL","","",8015,16.462258265999999,131945]
["1110000000-E","STABILIZER AGG","","",500,16,8000]
["1115000000-E","GEOTEXTILE FOR PVT STABILIZ","","",4000,2.9,11600]
["1121000000-E","AGG BASE COURSE","","",31029,20.607886171000001,639442.1]
["1176000000-E","SOIL CEM BASE","","",29870,2.5,74675]
["1187000000-E","PC FOR SOIL CEM BASE","","",822,137,112614]
["1209000000-E","ASPH CURING SEAL","","",8970,2.6,23322]
["1220000000-E","INCIDENTAL STONE BASE","","",5250,20.191428570999999,106005]
["1245000000-E","SHDR RECONST","","",186.61,1540.9999464120001,287566]
["1275000000-E","PRIME COAT","","",8190,4.0199999999999996,32923.800000000003]
["1297000000-E","MILL ASP PVT *****\" DTH","(1-1/2\")","",51679,1.6203438530000001,83737.75]
["","","(2\")","",22510,1.25,28137.5]
["","","(3\")","",14450,2.5423875429999998,36737.5]
["","","(3/4\")","",96500,0.9,86850]
["","","(5/8\")","",228910,1.2,274692]
["1330000000-E","INCIDENTAL MILLING","","",20520,6.9411549709999996,142432.5]
["1489000000-E","ASP CNC BAS CRS B250B","","",12288,45.947290039000002,564600.30000000005]
["1491000000-E","ASP CNC BAS CRS B250C","","",17980,41.067741935000001,738398]
["1498000000-E","ASP CONC INTR CRS I190B","","",6800,32.668823529000001,222148]
["1508000000-E","ASP CONC INTR CRS I190D","","",5760,39.1,225216]
["1519000000-E","ASP CNC SURF CRS S95B","","",118826,33.812358658999997,4017787.33]
["1520000000-E","ASP CONC SURF CRS S95B LEVEL","","",11802,33.937425859999998,400529.5]
["1523000000-E","ASP CNC SURF CRS S95C","","",29480,32.992373813,972615.18]
["1524000000-E","ASP CONC SURF CRS S95C LEVEL","","",2250,33.038888888999999,74337.5]
["1524200000-E","ASP CNC SURF CRS S95D","","",43990,40.597885882999996,1785901]
["1525000000-E","ASP CONC SURF CRS SF95A","","",9048,39.672734306000002,358958.9]
["1525100000-E","ASP CONC SURF CRS SF95A LEVEL","","",418,39.5,16511]
["1575000000-E","ASP FOR PLANT MIX","","",12310,610.40503655600003,7514086]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",2995,776.78631051800005,2326475]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",611,123.52700491,75475]
["1704000000-E","PATCHING EXIST PVT","","",20356,89.750049125999993,1826952]
["1775000000-E","AST MAT COAT 78M STNE","","",110338,1.670545052,184324.6]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",9210,47,432870]
["1839200000-E","APPLICATION OF ULTRATHIN HOT MIX ASPH","","",262858,1.65,433715.7]
["1840000000-E","MILLED RUMBLE STRIPS","","",329314,0.143055503,47110.18]
["1858000000-E","******\"PCC PVT RAMPS","(11-1/2\")","",41250,72,2970000]
["1891000000-E","GENERIC PAVING ITEM(SY)","NONWOVEN GEOTEXTIL ","INTERLAYER",11000,1.9,20900]
["1902000000-N","SURF TEST CONC PVT","","",1,20500,20500]
["1924000000-N","FIELD LAB RENTAL PCCP","","",1,15400,15400]
["2000000000-N","RIGHT OF WAY MKRS","","",13,350,4550]
["2022000000-E","SUBDRN EXCAVATION","","",1489.6,17.503759398,26073.599999999999]
["2033000000-E","SUBDRN FINE AGG","","",1058.4000000000001,42.285714286000001,44755.199999999997]
["2044000000-E","6\" PERF SUBDRN PIPE","","",6300,6.063492063,38200]
["2070000000-N","SUBDRN PIPE OUTLET","","",14,254.285714286,3560]
["2077000000-E","6\" OUTLET PIPE","","",84,22.714285713999999,1908]
["2099000000-E","SHDR DRN","","",5000,7.25,36250]
["2110000000-E","4\" SHDR DRN PIPE","","",5000,2.2999999999999998,11500]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",260,15.35,3991]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",6,270,1620]
["2143000000-E","BLOTTING SAND","","",15,70,1050]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",154,625,96250]
["2209000000-E","ENDWALLS","","",70,934.5,65415]
["2220000000-E","REINF ENDWALLS","","",41,900,36900]
["2253000000-E","PIPE COLLARS","","",7,847.14285714300001,5930]
["2264000000-E","PIPE PLUGS","","",2,1327.5,2655]
["2286000000-N","MASNRY DRNG STRUCT","","",280,1293.8571428570001,362280]
["2297000000-E","MASNRY DRNG STRUCT","","",11.8,1110,13098]
["2308000000-E","MASNRY DRNG STRUCT","","",172,198.04651162799999,34064]
["2354000000-N","FRM W/GRATE 84022 STD","","",4,450,1800]
["2364000000-N","FRM W/2GRTS 84016 STD","","",2,595,1190]
["2364200000-N","FRM W/2GRTS 84020 STD","","",12,518.75,6225]
["2365000000-N","FRM W/2GRTS 84022 STD","","",59,633.57627118599999,37381]
["2366000000-N","FRM W/2GRTS 84024 STD","","",2,755,1510]
["2367000000-N","FRM W/2GRTS 84029 STD","","",9,603.33333333300004,5430]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",9,520,4680]
["","","(F)","",5,530,2650]
["","","(G)","",9,530,4770]
["2396000000-N","FRM W/COVER STD 84054","","",5,405.4,2027]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",2,1800,3600]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",5,490,2450]
["2462000000-E","**\" SLUICE GATE","(18\")","",2,4000,8000]
["","","(24\")","",2,3600,7200]
["","","(30\")","",1,4100,4100]
["","","(36\")","",3,5000,15000]
["","","(42\")","",1,7800,7800]
["","","(48\")","",1,9800,9800]
["2473000000-N","GENERIC DRNG ITEM (EA)","OIL / H2O SEPARATOR","",1,88000,88000]
["2535000000-E","**\"X**\" CONC CURB","(9\" X 18\")","",860,20.25,17415]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",1790,18.2,32578]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",5690,22.570070299000001,128423.7]
["2556000000-E","SHDR BERM GUTR","","",2926,21.772966507,63707.7]
["2591000000-E","4\" CONC SIDEWALK","","",230,45.45,10453.5]
["2600000000-N","RETROFIT EXT CURB RAMP","","",28,480,13440]
["2605000000-N","CONC CURB RAMP","","",6,1370,8220]
["2612000000-E","6\" CONC DRIVEWAY","","",60,49.49,2969.4]
["2619000000-E","4\" CONC PAVED DITCH","","",40,36.64,1465.6]
["2627000000-E","4\" CONC ISLAND COVER","","",250,45.45,11362.5]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",2780,35.549999999999997,98829]
["2724000000-E","PC REINF BARR SNGL FC","","",80,126,10080]
["2753000000-E","GENERIC PAVING ITEM 846 (LF)","SPECIAL SHDR BERM GUTR","",1963,20.25,39750.75]
["2815000000-N","ADJ DROP INLETS","","",17,973.52941176499996,16550]
["2830000000-N","ADJ MHS","","",37,895.94594594600005,33150]
["2845000000-N","ADJ METER OR VAL BOX","","",26,805.76923076900005,20950]
["2910000000-N","CONVERT TRAF BR DI TO TRAF BR JB","","",1,760,760]
["3000000000-N","IMPACT ATTEN  350","","",1,13130,13130]
["3030000000-E","STL BM GUARDRAIL","","",120934.5,14.788784342,1788474.24]
["3045000000-E","SBGR SHOP CURVED","","",887.5,14.971830986000001,13287.5]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",245,44.117346939000001,10808.75]
["3165000000-N","GR ANCHOR  **********","(350 TL-2)","",2,1620,3240]
["3195000000-N","GR ANCHOR  AT-1","","",3,600,1800]
["3210000000-N","GR ANCHOR  CAT-1","","",64,486.875,31160]
["3215000000-N","GR ANCHOR  III","","",4,1350,5400]
["3270000000-N","GR ANCHOR  350","","",82,1776.524390244,145675]
["3285000000-N","GR ANCHOR  M-350","","",2,1620,3240]
["3317000000-N","GR ANCHOR  B-77","","",10,1546,15460]
["3360000000-E","REM EXISTING GUARDRAIL","","",110847,1.473206311,163300.5]
["3380000000-E","TEMP STL BM GUARDRAIL","","",775,7.5,5812.5]
["3389100000-N","TEMP GDRL ANCH UNITS 350","","",4,1000,4000]
["3500000000-E","WOVEN WIRE FEN **\" FAB","(48\")","",220,7,1540]
["3503000000-E","WOVEN WIRE FEN 47\" FAB","","",68880,2.0213109760000001,139227.9]
["3506000000-E","4\" TIMBER POSTS ****LONG","(7'-7\")","",9,15,135]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",4384,14.170244069000001,62122.35]
["3512000000-E","5\" TIMBER POSTS ****LONG","(8'-1\")","",14,30,420]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",1015,20.030541872000001,20331]
["3557000000-E","ADDITIONAL BARBED WIRE","","",1050,0.11952380999999999,125.5]
["3559000000-E","** STRD BW FEN W/ POST","(4)","",1225,4.96,6076]
["3575000000-E","GENERIC FENCING ITEM(LF)","TEMP 4 STRAND BW ","FENCE W/POSTS",1150,4.96,5704]
["3578000000-N","GENERIC FENC ITEM (EA)","RESET EXISTING GATE","",1,300,300]
["3628000000-E","RIP RAP CL I","","",4075,44.337423313000002,180675]
["3635000000-E","RIP RAP CL II","","",5032,42.463235294,213675]
["3649000000-E","RIP RAP CL B","","",5753,39.986094211999998,230040]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",33176,2.1608454909999999,71688.210000000006]
["3659000000-N","PREFORMED SCOUR HOLE","","",5,1366.422,6832.11]
["4048000000-E","REINF CONC FOUNDTN","","",8,810,6480]
["4054000000-E","PLN CONC FOUNDTN","","",2,790,1580]
["4057000000-E","OVERHEAD FOOTING","","",84,760,63840]
["4060000000-E","SUPPT BRKAWAY STL BM","","",7812,3.8,29685.599999999999]
["4066000000-E","SUPPTS SIMPLE STL BM","","",1207,3.05,3681.35]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",1256,7.1527468150000004,8983.85]
["4078000000-E","SUPPT 2-LB STL U-CHAN","","",2,21.25,42.5]
["4082100000-N","SUPPT OVRHD SIGN STR**","(107+50 -L-)","",1,29300,29300]
["","","(119+44 -L-)","",1,56600,56600]
["","","(135+90 -L-)","",1,29300,29300]
["","","(182+30 -L-)","",1,31350,31350]
["","","(AT 74 WEST EXIT)","",1,31850,31850]
["","","(NORTH OF 74 EAST EXIT)","",1,31850,31850]
["4096000000-N","SIGN ERECTION  D","","",24,49.579166667000003,1189.9000000000001]
["4102000000-N","SIGN ERECTION  E","","",33,54.528787878999999,1799.45]
["4108000000-N","SIGN ERECTION  F","","",2,202,404]
["4109000000-N","SIGN ERECTN *** (OVRHD)","(A)","",2,2626,5252]
["","","(B)","",2,404,808]
["4110000000-N","SIGN ERECT *** (GRD MTD)","(A)","",12,354,4248]
["","","(B)","",7,177,1239]
["4114000000-N","SIGN ERECTION MILEMKRS","","",2,177,354]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(B)","",2,355,710]
["4138000000-N","DISP SUPPT STL BM","","",2,75.75,151.5]
["4149000000-N","DISP SIGN SYST OVRHD","","",3,1820,5460]
["4152000000-N","DISP SIGN SYST STL BM","","",2,50.5,101]
["4155000000-N","DISP SIGN SYST U-CHAN","","",30,3.673333333,110.2]
["4158000000-N","DISP SIGN SYST WOOD","","",2,20.2,40.4]
["4234000000-N","DISP SIGN A OR B(OVRHD)","","",4,101,404]
["4400000000-E","WORK ZONE SIGN (STAT)","","",3061,3.8301829469999999,11724.19]
["4405000000-E","WORK ZONE SIGN (PORT)","","",1105,8.8831855199999996,9815.92]
["4410000000-E","WORK ZONE SIGN (BARR)","","",787,7.6543837359999998,6024]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",11394,4.750416886,54126.25]
["4415000000-N","FLASHING ARROW BOARD","","",3,2225,6675]
["4420000000-N","PORT CHANGE MSG SIGN","","",2,7975,15950]
["4430000000-N","DRUMS","","",651,47.671274961999998,31034]
["4435000000-N","CONES","","",286,19.263986014,5509.5]
["4445000000-E","BARRICADES ( III)","","",1068,20.298127341000001,21678.400000000001]
["4450000000-N","FLAGGER","","",16,25,400]
["4455000000-N","FLAGGER","","",300,0.01,3]
["4457000000-N","TEMP TRAFFIC CNTRL","","",5,65600,328000]
["4465000000-N","TEMP CRASH CUSHIONS","","",3,5000,15000]
["4480000000-N","TMA","","",3,23740,71220]
["4485000000-E","PORT CONC BARR","","",10000,19.149999999999999,191500]
["4510000000-N","LAW ENFORCEM","","",344,38.982558140000002,13410]
["4516000000-N","SKINNY DRUM","","",50,42.75,2137.5]
["4650000000-N","TEMP RAISED PVT MRKS","","",835,11.098802395,9267.5]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",473380,0.568442224,269089.18]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",493492,0.60952469300000001,300795.56]
["4688000000-E","THERMO PVT MKG LINES6\"90 MILS","","",202323,0.80968179600000001,163817.25]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",27491,0.86402095199999995,23752.799999999999]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",2113,1.5917936580000001,3363.46]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",1175,2.1755319150000001,2556.25]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",9557,1.954222036,18676.5]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",1081,2.8,3026.8]
["4705000000-E","THERMO LINES 16\" 120MILS","","",150,3.75,562.5]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",2108,9.181214421,19354]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",100,71.328000000000003,7132.8]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",260,120.626923077,31363]
["4770000000-E","4\" COLD APPL PLSTIC LINES  **","(II)","",1520,3.1631578949999999,4808]
["4780000000-E","8\" COLD APPL PLSTIC LINES  **","(II)","",112,6.5,728]
["4810000000-E","PAINT PVT MKGS 4\"","","",2079857,0.11207245,233094.67]
["4815000000-E","PAINT PVT MKGS 6\"","","",523928,0.21222687100000001,111191.6]
["4820000000-E","PAINT PVT MKGS 8\"","","",1020,0.55000000000000004,561]
["4825000000-E","PAINT PVT MKGS 12\"","","",17172,1.001677149,17200.8]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",212,3,636]
["4845000000-N","PAINT PVT MKG SYMBOL","","",2,85.9,171.8]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",206914,1.25,258642.5]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",8550,2.75,23512.5]
["4850000000-E","LINE REML 4\" WIDE","","",1000,3.5,3500]
["4855000000-E","LINE REML 6\" WIDE","","",53000,0.6,31800]
["4870000000-E","LINE REML 24\" WIDE","","",24,5,120]
["4900000000-N","PERM RAISED PVT MKRS","","",16,18.125,290]
["4905000000-N","SNOWPLB PVT MRKER","","",7006,25.227897515999999,176746.65]
["5010000000-E","100' HIGH MOUNT STD","","",3,18700,56100]
["5020000000-N","PORTABLE DRIVE UNIT","","",1,3030,3030]
["5070000000-N","STD FOUNDAT ***********","(R1)","",12,865,10380]
["","","(R2)","",3,885,2655]
["5155000000-E","ELECT DUCT BD SIZE *****","(3\")","",165,14.15,2334.75]
["","","(4\")","",245,18.2,4459]
["","","(6\")","",325,20.2,6565]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(4)","",770,8.0500000000000007,6198.5]
["5190000000-E","************ FEEDER CIR","(4 - 1 W/G )","",1275,10.6,13515]
["","","(4 - 2/0 W/G )","",1335,12.9,17221.5]
["5220000000-E","**-2 W/G FEEDER N *****\"","(4 2)","",8210,10,82100]
["5225000000-E","**-1 W/G FEEDER CIR ****","(4 2)","",6825,10.85,74051.25]
["5230000000-E","************ FEEDER N **","(4 - 2/0 W/G 3\")","",3215,16.149999999999999,51922.25]
["5240000000-N","ELEC JB ************","(PC30)","",13,660,8580]
["","","(PC36)","",9,800,7200]
["5255000000-N","PORTABLE LIGHTING","","",2,17500,35000]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","RAMP B PIT ELECTRICAL WORK","",1,7575,7575]
["","","RAMP B STATIC SCALE ","PLATFORM",1,110915,110915]
["","","RAMP B STATIC SCALE ","SYST",1,40915,40915]
["","","RAMP C PIT ELECTRICAL ","WORK",1,7575,7575]
["","","RAMP C STATIC SCALE ","PLATFORM",1,110915,110915]
["","","RAMP C STATIC SCALE ","SYST",1,40915,40915]
["5262000000-E","GENERIC LIGHT ITEM (CY)","HIGH MOUNT FOUNDS","",21,910,19110]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","1 POLE 120VAC EQUIP DIS- CONNECT","",8,303,2424]
["","","15KVA POWER ","TRANSFORMER",1,3290,3290]
["","","2 POLE 240VAC EQUIP ","DIS-CONNECT",1,570,570]
["","","HIGH MOUNT LUMINAIRE - ","LED",18,2185,39330]
["","","LIGHT CNTRL EQUIP ","WS 120/208V",1,10050,10050]
["","","LIGHT STANDARD  MLTS ","35'MH 6'SA",15,2425,36375]
["","","ROADWAY LIGHT STD ","LUMI- NAIRE-LED",15,1065,15975]
["5325600000-E","6\" H2O LINE","","",7120,42.062117978000003,299482.28000000003]
["5325800000-E","8\" H2O LINE","","",80,138.52000000000001,11081.6]
["5326200000-E","12\" H2O LINE","","",1020,80.89,82507.8]
["5326600000-E","16\" H2O LINE","","",2597,139.53,362359.41]
["5540000000-E","6\" VALVE","","",11,1133.1918181819999,12465.11]
["5558000000-E","12\" VALVE","","",3,2290.19,6870.57]
["5558600000-E","16\" VALVE","","",6,4287.16,25722.959999999999]
["5589200000-E","2\" AIR RELEASE VALVE","","",1,6622.85,6622.85]
["5648000000-N","RELOCATE H2O METER","","",7,1314.46,9201.2199999999993]
["5649000000-N","RECONNECT H2O METER","","",1,1011.12,1011.12]
["5666000000-E","FIRE HYDRANT","","",1,5055.6099999999997,5055.6099999999997]
["5672000000-N","RELOCATE FIRE HYDRANT","","",5,3134.48,15672.4]
["5691700000-E","18\" SANIT GRAV SEWER","","",554,80,44320]
["5709300000-E","6\" FORCE MAIN SEWER","","",3035,31.34,95116.9]
["5775000000-E","4' DIA UTILITY MH","","",2,6850,13700]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",11378,2.02,22983.56]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",78,20.22,1577.16]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",4392,12.13,53274.96]
["5811000000-E","ABANDON 18\" UTILITY PIPE","","",570,25.25,14392.5]
["5815000000-N","REMOVE H2O METER","","",4,808.9,3235.6]
["5815500000-N","REMOVE FIRE HYDRANT","","",2,1011.12,2022.24]
["5816000000-N","ABANDON UTILITY MH","","",3,1560,4680]
["5835000000-E","**\" ENCASEMENT PIPE","(10\")","",173,60.67,10495.91]
["5835600000-E","12\" ENCASEMENT PIPE","","",1126,67.75,76286.5]
["5836000000-E","24\" ENCASEMENT PIPE","","",154,108.19,16661.259999999998]
["5836200000-E","30\" ENCASEMENT PIPE","","",668,202.22,135082.96]
["5836400000-E","36\" ENCASEMENT PIPE","","",390,350,136500]
["5871400000-E","6\" TRENCHLESS INSTALL (IN SOIL)","","",30,100,3000]
["5871410000-E","6\" TRENCHLESS INSTALL (NOT IN SOIL)","","",30,300,9000]
["5871700000-E","12\" TRENCHLESS INSTALL (IN SOIL)","","",89,278.06,24747.34]
["5871710000-E","12\" TRENCHLESS INSTALL (NOT IN SOIL)","","",89,278.06,24747.34]
["5872400000-E","36\" TRENCHLESS INSTALL (IN SOIL)","","",160,206,32960]
["5872410000-E","36\" TRENCHLESS INSTALL (NOT IN SOIL)","","",160,1250,200000]
["5879200000-E","2\" GAS LINE","","",120,17,2040]
["5879600000-E","6\" GAS LINE","","",1390,62.35,86666.5]
["5882000000-N","GENERIC UTILITY ITEM (EA)","ADJUST H2O VAULT LID","",2,2022.25,4044.5]
["5888000000-E","GENERIC UTILITY ITEM (LF)","10\" ENCASEMENT PIPE","",170,100,17000]
["6000000000-E","TEMP SILT FENCE","","",65500,1.49670229,98034]
["6006000000-E","EROS CNTRL STONE CL A","","",6225,31.849285140999999,198261.8]
["6009000000-E","EROS CNTRL STONE CL B","","",17700,34.110288136000001,603752.1]
["6012000000-E","SEDIMENT CNTRL STONE","","",15435,28.317926790000001,437087.2]
["6015000000-E","TEMP MULCHING","","",217,783.709769585,170065.02]
["6018000000-E","SEED FOR TEMP SEEDING","","",13450,1.541301115,20730.5]
["6021000000-E","FERT FOR TEMP SEEDING","","",57.75,583.93506493500001,33722.25]
["6024000000-E","TEMP SLOPE DRNS","","",12525,12.126007983999999,151878.25]
["6029000000-E","SAFETY FENCE","","",10900,1.0906422019999999,11888]
["6030000000-E","SILT EXCAVATION","","",76760,3.4840281399999999,267434]
["6036000000-E","MAT FOR EROS CNTRL","","",239900,1.1942684450000001,286505]
["6037000000-E","COIR FIBER MAT","","",9700,3.2848453609999999,31863]
["6038000000-E","PERM SOIL REINF MAT","","",8400,4.0238095239999998,33800]
["6042000000-E","1/4\" HARDWARE CLOTH","","",14420,2.7723647709999999,39977.5]
["6045000000-E","**\" TEMP PIPE","(24\")","",180,50,9000]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",180,55.81,10045.799999999999]
["6069000000-E","STILLING BASINS","","",60,50,3000]
["6070000000-N","SPECIAL STILLING BASINS","","",28,610.69857142900003,17099.560000000001]
["6071010000-E","WATTLE","","",29605,4.4842931940000001,132757.5]
["6071012000-E","COIR FIBER WATTLE","","",150,7.69,1153.5]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",17385,7.3508484330000003,127794.5]
["6071030000-E","COIR FIBER BAFFLE","","",20560,4.1817120619999999,85976]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",111,1018.557837838,113059.92]
["","","(2\")","",14,1181.7785714290001,16544.900000000001]
["","","(2-1/2\")","",6,1174.6099999999999,7047.66]
["","","(3\")","",1,1401.89,1401.89]
["6084000000-E","SEEDING AND MULCHING","","",332.2,1456.703913305,483917.04]
["6087000000-E","MOWING","","",103,75.194174756999999,7745]
["6090000000-E","SEED FOR REPAIR SEED","","",2550,6.9203921570000002,17647]
["6093000000-E","FERT FOR REPAIR SEEDING","","",10,617.75,6177.5]
["6096000000-E","SEED FOR SUPP SEEDING","","",6150,3.2151626019999999,19773.25]
["6108000000-E","FERTILIZER TOPDRESSING","","",183,613.57240437200005,112283.75]
["6111000000-E","IMPERVIOUS DIKE","","",1140,45.631578947000001,52020]
["6114500000-N","SPECIALIZED HAND MOW","","",235,42.52,9992.2000000000007]
["6117000000-N","RESPONSE FOR EROS CNTRL","","",453,86.203487859000006,39050.18]
["6123000000-E","REFORESTATION","","",14,1100,15400]
["7060000000-E","SIGNAL CABLE","","",260,3.8,988]
["7279000000-E","TRACER WIRE","","",7955,0.86,6841.3]
["7301000000-E","DIRECT DRILL (***********)","(1 2\")","",115,19.2,2208]
["","","(2 2\")","",620,38.4,23808]
["","","(4 2\")","",45,72.75,3273.75]
["7312000000-N","JUNCTION BOX (***********)","(SPECIAL-SIZED)","",8,707,5656]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",32,380,12160]
["7360000000-N","WOOD POLE","","",1,707,707]
["7420000000-E","2\" RISER W/ WEATHERHD","","",6,380,2280]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",1858,7.5268568350000002,13984.9]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(36)","",8200,12.85,105370]
["7540000000-N","SPLICE ENCLOSURE","","",8,990,7920]
["7552000000-N","INTERCONNECT CENTER","","",12,1010,12120]
["7566000000-N","DELINEATOR MKR","","",16,160,2560]
["7613000000-N","SOIL TEST","","",9,707,6363]
["7614100000-E","DRILLED PIER FOUND","","",45,1010,45450]
["7901000000-N","CBNT BASE EXTENDER","","",3,835,2505]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","5/8\" X 10' GROUNDING ","ELECTRODE",26,55.55,1444.3]
["","","AVI ANTENNA","",6,2500,15000]
["","","AVI READER","",6,4165,24990]
["","","BASE MTD EQUIP CBNT","",3,2500,7500]
["","","CCTV CBNT","",5,3535,17675]
["","","CCTV CAMERA ASSEM","(FIXED MOUNT)",3,1700,5100]
["","","CCTV WOOD POLE","",5,707,3535]
["","","COMPUTER WRKSTATN ","(INSTALL)",4,3335,13340]
["","","DIGITAL HARDWARE ","VIDEO ENCODER",8,2565,20520]
["","","DMS PEDESTAL  STR","",1,22930,22930]
["","","ENCLOSED COMMUNICATIONS RACK","",3,3780,11340]
["","","EQUIP CBNT FOUND","",3,835,2505]
["","","ETHERNET EDGE SWITCH","",13,1515,19695]
["","","JUNCTION BOX (OVER-","SIZED)",27,707,19089]
["","","LANE CNTRL SIGNAL","",4,5000,20000]
["","","MANAGED ETHERNET ","SWITCH",1,49350,49350]
["","","METAL POLE WITH HINGED MAST ARM","",5,8145,40725]
["","","METAL POLE W/ HINGED MAST ARM DESIGN","",5,3030,15150]
["","","METAL POLE W/ MONOTUBE","GANTRY STR",2,21530,43060]
["","","","GANTRY STR DESIGN",2,1010,2020]
["","","NEW ELECTRICAL SERVICE (OVER- HEAD)","",1,950,950]
["","","NEW ELECTRICAL SERV (UNDER-GROUND)","",1,885,885]
["","","OVER-HEIGHT VEHICLE DETECTION SYST","",2,14650,29300]
["","","PATCH PANEL (ETHERNET)","",12,720,8640]
["","","PIEZOELECTRIC AXLE SENSOR","",6,1670,10020]
["","","PIEZOELECTRIC QUARTZ SENSOR SET","",6,7325,43950]
["","","POLE MTD EQUIP CBNT","",5,1515,7575]
["","","PRINTER (INSTALL)","",1,2930,2930]
["","","SERVER (INSTALL)","",2,2525,5050]
["","","SERVICE DISCONNECT","",4,335,1340]
["","","SPLICE CENTER (36-","FIBER)",1,2930,2930]
["","","STEEL PEDESTAL POLE","",3,9270,27810]
["","","UPS","",6,835,5010]
["","","VEHICLE SIGNAL HEAD","(12\" 2-SECTION RED-GREEN)",6,2600,15600]
["","","WALL-MTD COMMUNICATIONS RACK","",1,3780,3780]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","ADVANCE LOCATION WIM ELECTRON-ICS","",1,139400,139400]
["","","ALPR SYST","",1,78800,78800]
["","","CCTV SOFTWARE","",1,7080,7080]
["","","CENTRAL CNTRL SOFTWARE","",1,14650,14650]
["","","COMPLIANCE LOCATION WIM ELEC- TRONICS","",1,139400,139400]
["","","DMS","",1,91600,91600]
["","","NETWORK MGMT SOFTWARE","",1,10355,10355]
["","","OPEN/CLOSED DMS PANEL","",1,8335,8335]
["","","SCALE HOUSE WIM ELECTRONICS","",1,139400,139400]
["","","SYST WARRANTY","",1,36400,36400]
["","","TRAINING","",1,8335,8335]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","DROP CABLE (6 FIBER)","",1819,10.1,18371.900000000001]
["","","ETHERNET CABLE","",955,0.15,143.25]
["","","FOUR-WIRE COPPER FEEDER CON- DUCTORS","",2536,12.55,31826.799999999999]
["","","LEAD-IN CABLE","",228,3.05,695.4]
["","","UNDERGROUND CONDUIT (1 2\")","",559,7.1,3968.9]
["","","UNDERGROUND CONDUIT (2 2\")","",5649,8.59,48524.91]
["","","UNDERGROUND CONDUIT (3 2\")","",1917,10.1,19361.7]
["","","UNDERGROUND CONDUIT (4 2\")","",85,18.2,1547]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","DMS OVERHEAD FOOTINGS","",8,1010,8080]
["8021000000-N","REMV EXIST STR **********","(16+8350-L-)","",1,25000,25000]
["8049000000-N","REMV EXIST STR **********","(13+4400-L-)","",1,10000,10000]
["8056000000-N","REMV EXIST STR **********","(14+3400-L-)","",1,21000,21000]
["8091000000-N","FND EXCAV B** STA *******","(1 203+5035-L-)","",1,2700,2700]
["","","(1 247+9066-L-LT)","",1,3800,3800]
["","","(1 247+9066-L-RT)","",1,3800,3800]
["","","(1 354+8322-L-)","",1,7000,7000]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",436.35,1150,501802.5]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",118.5,750,88875]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",249,1150,286350]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",46,750,34500]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",153.30000000000001,41.079973907000003,6297.56]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",101.5,100,10150]
["8112730000-N","PDA TESTING","","",4,4100,16400]
["8113000000-N","SID INSPECTIONS","","",25,512.93119999999999,12823.28]
["8114000000-N","SPT TESTING","","",25,532.93119999999999,13323.28]
["8115000000-N","CSL TESTING","","",9,6233.3333333330002,56100]
["8121000000-N","UNCL STR EXCAV STA ****","(14+3400-L-)","",1,33367.17,33367.17]
["","","(16+8350-L-)","",1,7500,7500]
["8126000000-N","CULV EXCAV @ ************","(13+4400-L-)","",1,17500,17500]
["","","(153+4068 -L-)","",1,2550,2550]
["","","(222+2043-L-)","",1,105254.37,105254.37]
["8133000000-E","FND CONDIT MAT BOX CULV","","",834,47.013788968999997,39209.5]
["8147000000-E","REINF CONC DECK SLAB","","",108777.2,26,2828207.2]
["8161000000-E","GROOVING BRG FLOORS","","",111225.9,0.34000003600000001,37816.81]
["8182000000-E","CL A CONC (BRG)","","",2162.6999999999998,696.33097516999999,1505955]
["8196000000-E","CL A CONC (CULV)","","",1917.5,420.42670143399999,806168.2]
["8210000000-N","BRG APPR SLAB ***********","(157+7550-L-EBL)","",1,31500,31500]
["","","(157+7550-L-WBL)","",1,315400,315400]
["","","(16+8350-L-)","",1,25000,25000]
["","","(203+5035-L-)","",1,50000,50000]
["","","(247+9066-L-LT)","",1,39800,39800]
["","","(247+9066-L-RT)","",1,39800,39800]
["","","(252+7329-L-LT)","",1,38000,38000]
["","","(252+7329-L-RT)","",1,40500,40500]
["","","(340+7000-L-LT)","",1,34900,34900]
["","","(340+7000-L-RT)","",1,34900,34900]
["","","(354+8322-L-)","",1,50000,50000]
["8217000000-E","REINF STEEL (BRG)","","",456621,0.87667108999999999,400306.43]
["8238000000-E","SPIRL COL REINF STL BRG","","",52026,1.75409353,91258.47]
["8245000000-E","REINF STEEL (CULVERT)","","",171335,1.008551084,172800.1]
["8265000000-E","54\" PRESTR CONC GIRDR","","",7370.61,184,1356192.24]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",713,205,146165]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",1348.91,220,296760.2]
["8280000000-E","STRUCTURAL STEEL","","",792568,1.324807461,1050000]
["8364000000-E","HP12X53 PILES","","",7880,47.496065989999998,374269]
["8384000000-E","HP14X73 PILES","","",5810,62.11,360859.1]
["8385200000-E","PP**X**** GALV STL PILE","(24\" X 050\")","",1840,145,266800]
["8392000000-N","PIPE PILE PLATES","","",24,162,3888]
["8393000000-N","PILE REDRIVES","","",141,202,28482]
["8475000000-E","TWO BAR METAL RAIL","","",244.9,127,31102.3]
["8503000000-E","CONC BARR RAIL","","",5133.3999999999996,89,456872.6]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-11 1/4\")","",260.51,95,24748.45]
["8524000000-E","**\" CHAIN LINK FENCE","(72\")","",680,98.5,66980]
["8531000000-E","4\" SLOPE PROTECTION","","",4326.3999999999996,69.820000461999996,302069.25]
["8608000000-E","RIP RAP II (2'-0\")","","",5985,41.859649122999997,250530]
["8622000000-E","GEOTEXTILE FOR DRNG","","",6593,1.9032246319999999,12547.96]
["8657000000-N","ELASTOMERIC BEARINGS","","",2,126000,252000]
["8692000000-N","FOAM JOINT SEALS","","",1,25500,25500]
["8706000000-N","EXPANSION JOINT SEALS","","",1,485000,485000]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",720,120,86400]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",840,145,121800]
["8801000000-E","MSE RETAIN WALL NO **","(1 @ END BENT 1)","",6950,80,556000]
["","","(2 @ END BENT 2)","",4925,80,394000]
["8804000000-N","GENERIC CULVERT ITEM (LS)","PLACEM OF NATURAL STREAM","BED MATERIAL",1,4000,4000]
["","","PRECAST REINF CONC THREE-SIDED","CULVERT @ STA 14+3400 -L-",1,215000,215000]
["8860000000-N","GENERIC STR ITEM (LS)","APPLICAT BRG COATING","",1,48928.58,48928.58]
["8881000000-E","GENERIC STR ITEM (CY)","CL AA CONC (WEIGH","BRG - STATIC SCALE)",509,795,404655]
["8889000000-E","GENERIC STR ITEM (LB)","EPOXY COATED REINFORCING STEEL","(WEIGH BRG - STATIC SCALE)",35037,0.85,29781.45]
["","","POLYURETHANE GROUT INJECTION","",12500,14.15,176875]
["","","REINFORCING STEEL (WEIGH","BRG - STATIC SCALE)",37175,1.1499999999999999,42751.25]
["8892000000-E","GENERIC STR ITEM (SF)","GROOVING CONC SLAB","",6422,2.5499999999999998,16376.1]

{"sheet":"Items - Div 13","index":15,"n_rows":591,"n_cols":7,"rows_kept":591,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 13"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",23,214969.36565217399,4944295.41]
["0000400000-N","CONST SURVEYING","","",5,183249.2,916246]
["0000900000-N","GENERIC MISC ITEM (LS)","ALTERNATE LS BID","FOR BRG 100012",1,665000,665000]
["","","","FOR BRG 560001",1,550000,550000]
["","","","FOR BRG 560076",1,715000,715000]
["","","","FOR BRG 560231",1,415000,415000]
["","","","FOR BRG 600005",1,817115,817115]
["","","","FOR BRG 800172",1,328250,328250]
["","","DESIGN & CONST OF","BRGS",2,4369043.5,8738087]
["0000915000-N","GENERIC MISC ITEM (EA)","END BENTS STR 100371","",2,85000,170000]
["","","END BENTS STR 100676","",2,45000,90000]
["","","END BENTS STR 100677","",2,45000,90000]
["","","END BENTS STR 110014","",2,90000,180000]
["","","END BENTS STR 110015","",2,98000,196000]
["","","END BENTS STR 110034","",2,80000,160000]
["","","END BENTS STR 110035","",2,78000,156000]
["","","END BENTS STR 110060","",2,83000,166000]
["","","END BENTS STR 580005","",2,118000,236000]
["","","END BENTS STR 580021","",2,89000,178000]
["","","END BENTS STR 580022","",2,70000,140000]
["","","END BENTS STR 600031","",2,45000,90000]
["","","END BENTS STR 600042","",2,45000,90000]
["","","END BENTS STR 600163","",2,85000,170000]
["","","END BENTS STR 800094","",2,120000,240000]
["","","END BENTS STR 800174","",2,23000,46000]
["","","END BENTS STR 800195","",2,98000,196000]
["","","RIGHT OF WAY ACQUISIT","",46,3119.5652173909998,143500]
["0000930000-E","GENERIC MISC ITEM (LF)","AVE FOUNDATION LGTH AT END","BENT 1 STR 100371",10,9,90]
["","","","BENT 1 STR 100676",48,325,15600]
["","","","BENT 1 STR 100677",14,4250,59500]
["","","","BENT 1 STR 110014",11,1,11]
["","","","BENT 1 STR 110015",17,1,17]
["","","","BENT 1 STR 110034",25,1,25]
["","","","BENT 1 STR 110035",66,1,66]
["","","","BENT 1 STR 110060",23,1,23]
["","","","BENT 1 STR 580005",11,1,11]
["","","","BENT 1 STR 580021",41,1,41]
["","","","BENT 1 STR 580022",58,1,58]
["","","","BENT 1 STR 600031",13,5065,65845]
["","","","BENT 1 STR 600042",22,2725,59950]
["","","","BENT 1 STR 600163",22,380,8360]
["","","","BENT 1 STR 800094",20,1,20]
["","","","BENT 1 STR 800174",35,1,35]
["","","","BENT 1 STR 800195",11,1,11]
["","","","BENT 2 STR 100371",12,5200,62400]
["","","","BENT 2 STR 100676",41,330,13530]
["","","","BENT 2 STR 100677",13,5065,65845]
["","","","BENT 2 STR 110014",10,1,10]
["","","","BENT 2 STR 110015",10,1,10]
["","","","BENT 2 STR 110034",24,1,24]
["","","","BENT 2 STR 110035",50,1,50]
["","","","BENT 2 STR 110060",15,1,15]
["","","","BENT 2 STR 580005",10,1,10]
["","","","BENT 2 STR 580021",48,1,48]
["","","","BENT 2 STR 580022",71,1,71]
["","","","BENT 2 STR 600031",15,4170,62550]
["","","","BENT 2 STR 600042",18,3330,59940]
["","","","BENT 2 STR 600163",18,420,7560]
["","","","BENT 2 STR 800094",22,1,22]
["","","","BENT 2 STR 800174",27,1,27]
["","","","BENT 2 STR 800195",30,1,30]
["","","BRG LGTH STR 100371","",70,2375,166250]
["","","BRG LGTH STR 100676","",50,1560,78000]
["","","BRG LGTH STR 100677","",50,1560,78000]
["","","BRG LGTH STR 110014","",40,2200,88000]
["","","BRG LGTH STR 110015","",55,2200,121000]
["","","BRG LGTH STR 110034","",70,2400,168000]
["","","BRG LGTH STR 110035","",40,2000,80000]
["","","BRG LGTH STR 110060","",40,2100,84000]
["","","BRG LGTH STR 580005","",70,2300,161000]
["","","BRG LGTH STR 580021","",55,2300,126500]
["","","BRG LGTH STR 580022","",100,3100,310000]
["","","BRG LGTH STR 600031","",35,1895,66325]
["","","BRG LGTH STR 600042","",115,2900,333500]
["","","BRG LGTH STR 600163","",70,2395,167650]
["","","BRG LGTH STR 800094","",55,1940,106700]
["","","BRG LGTH STR 800174","",70,2400,168000]
["","","BRG LGTH STR 800195","",70,2200,154000]
["0001000000-E","CLEARING & GRUBBING","","",110,4471.325454545,491845.8]
["0008000000-E","SUPP CLEAR & GRUBBING","","",5,4276.92,21384.6]
["0015000000-N","SEALING ABANDON WELL","","",8,1152.625,9221]
["0022000000-E","UNCLAS EXCAVATION","","",2002500,5.44,10893600]
["0029000000-N","REINF BRG APPR **********","(122+2250 -L- LT)","",1,40379.39,40379.39]
["","","(122+2250 -L- RT)","",1,43075.45,43075.45]
["","","(13+5300)","",1,30000,30000]
["","","(24+0357 -L- LT)","",1,33221.089999999997,33221.089999999997]
["","","(24+1562 -L- RT)","",1,33245.67,33245.67]
["0030000000-N","BRG APP SUB REG TIER**","(13+0134-L-)","",1,15000,15000]
["0036000000-E","UNDERCUT EXCAVATION","","",7489,5.7393510479999996,42982]
["0043000000-N","GRADING","","",3,649033.33333333302,1947100]
["0050000000-E","SUPP CLEAR & GRUBBING","","",4,300.25,1201]
["0057000000-E","UNDERCUT EXCAVATION","","",1685,13.192878338,22230]
["0063000000-N","GRADING","","",1,125000,125000]
["0098000000-E","PRE-SPLITTING OF ROCK","","",3080,18,55440]
["0106000000-E","BORROW EXCAVATION","","",5175,7.5,38812.5]
["0134000000-E","DRNG DITCH EXCAVATION","","",35586,6.155341988,219044]
["0141000000-E","BERM DITCH CONST","","",3960,2.65,10494]
["0156000000-E","REML OF EXT ASPH PVT","","",53900,0.99,53361]
["0177000000-E","BRKING OF EXT ASPH PVT","","",27680,0.38,10518.4]
["0192000000-N","PROOF ROLLING","","",70,181.19,12683.3]
["0195000000-E","SELECT GRANULAR MAT'L","","",4555,38.466520307000003,175215]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",30552,1.801289605,55033]
["0199000000-E","TEMP SHORING","","",19428,41.533096561999997,806905]
["0225000000-E","REINF SOIL SLOPES","","",950,125.76,119472]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETROLEUM"," CONTAMINATED SOIL",2200,150,330000]
["0318000000-E","FND CONDIT MATL MIN STR","","",6365,23.757077768999999,151213.79999999999]
["0320000000-E","FND CONDIT GEOTEXTILE","","",19990,2.6217758880000002,52409.3]
["0335200000-E","15\" DRNG PIPE","","",476,35.378151260999999,16840]
["0335300000-E","18\" DRNG PIPE","","",44,42,1848]
["0335850000-E","**\" DRNG PIPE ELBOW","(15\")","",6,250,1500]
["0342000000-E","**\" SIDE DRN PIPE","(12\")","",14,47.11,659.54]
["","","(30\")","",2904,69.933471073999996,203086.8]
["","","(36\")","",852,82.42,70221.84]
["","","(42\")","",42,116.26,4882.92]
["","","(48\")","",152,126.23,19186.96]
["0343000000-E","15\" SIDE DRN PIPE","","",21010,40.579850546999999,852582.66]
["0344000000-E","18\" SIDE DRN PIPE","","",4104,46.731929825000002,191787.84]
["0345000000-E","24\" SIDE DRN PIPE","","",4250,55.08,234090]
["0348000000-E","**\" SIDE DRN PIPE ELBOW","(15\")","",8,275,2200]
["0354000000-E","***\" RC PIPE CULV *****","(15\" V)","",60,50,3000]
["","","(54\" V)","",76,203.77,15486.52]
["","","(60\" V)","",124,245.45,30435.8]
["0366000000-E","15\" RC PIPE CULV III","","",1806,39.619102990000002,71552.100000000006]
["0372000000-E","18\" RC PIPE CULV III","","",1772,46.577878104,82536]
["0378000000-E","24\" RC PIPE CULV III","","",1726,55.571517960999998,95916.44]
["0384000000-E","30\" RC PIPE CULV III","","",228,67.3,15344.4]
["0390000000-E","36\" RC PIPE CULV III","","",712,83.2,59238.400000000001]
["0396000000-E","42\" RC PIPE CULV III","","",748,102.94,76999.12]
["0402000000-E","48\" RC PIPE CULV III","","",224,123.71,27711.040000000001]
["0408000000-E","54\" RC PIPE CULV III","","",200,159.41,31882]
["0448000000-E","***\" RCP CULV CL IV","(48\")","",52,141.97,7382.44]
["","","(54\")","",172,197.39,33951.08]
["","","(60\")","",80,253.7,20296]
["0448200000-E","15\" RCP CULV CL IV","","",12936,42.337915893999998,547683.28]
["0448300000-E","18\" RCP CULV CL IV","","",1194,52.445561138999999,62620]
["0448400000-E","24\" RCP CULV CL IV","","",1376,63.001686047,86690.32]
["0448500000-E","30\" RCP CULV CL IV","","",558,76.89827957,42909.24]
["0448600000-E","36\" RCP CULV CL IV","","",236,93.97,22176.92]
["0453000000-E","**\" PIPE END SECTION","(15\")","",13,718.25,9337.25]
["","","(18\")","",1,780.06,780.06]
["0576000000-E","**\" CS PIPE CULV *****\"","(12\" 0064\")","",236,40.14,9473.0400000000009]
["","","(36\" 0079\")","",432,79.540000000000006,34361.279999999999]
["","","(54\" 0109\")","",20,139.22,2784.4]
["","","(60\" 0138\")","",116,175.36,20341.759999999998]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",4068,45.326037364999998,184386.32]
["0588000000-E","18\" CS PIPE CULV 0064\"","","",1444,47.923324100000002,69201.279999999999]
["0594000000-E","24\" CS PIPE CULV 0064\"","","",1592,56.37,89741.04]
["0600000000-E","30\" CS PIPE CULV 0079\"","","",1024,71.38,73093.119999999995]
["0636000000-E","**\" CS ELBOW *****\" TK","(15\" 0064)","",82,594.57000000000005,48754.74]
["","","(18\" 0064)","",16,646.94000000000005,10351.040000000001]
["","","(24\" 0064)","",34,938.26,31900.84]
["","","(30\" 0079)","",16,1246.19,19939.04]
["","","(36\" 0079)","",10,1591.8,15918]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(24\" 0500\")","",284,330,93720]
["","","(30\" 0500\")","",116,402.05,46637.8]
["","","(42\" 0625\")","",72,563.98,40606.559999999998]
["","","(48\" 0625\")","",100,647.74,64774]
["","","(54\" 0875\")","",133,753.84,100260.72]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(24\" 0500\")","",284,875,248500]
["","","(30\" 0500\")","",116,725.92,84206.720000000001]
["","","(42\" 0625\")","",72,982.78,70760.160000000003]
["","","(48\" 0625\")","",100,1127.96,112796]
["","","(54\" 0875\")","",133,1368.07,181953.31]
["0986000000-E","GENERIC PIPE ITEM (LF)","24\" WLD STL PIPE 0500\""," B OPEN CUT",20,117.5,2350]
["","","54\" WLD STL PIPE LINER","",244,820.43,200184.92]
["0995000000-E","PIPE REML","","",14741,11.14271759,164254.79999999999]
["0996000000-N","PIPE CLEAN-OUT","","",1,1000,1000]
["1011000000-N","FINE GRADING","","",1,846815.6,846815.6]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",104520,2.65,276978]
["1066000000-E","LIME FOR LIME TRTED SOIL","","",1050,236,247800]
["1077000000-E","57 STONE","","",75,59,4425]
["1099500000-E","SHALLOW UNDERCUT","","",3224,10.037841191,32362]
["1099700000-E","CL IV SUBGRD STABIL","","",6678,19.147050015000001,127864]
["1110000000-E","STABILIZER AGG","","",1000,23.1,23100]
["1115000000-E","GEOTEX FOR PVT STABILI","","",18600,2.8,52080]
["1121000000-E","AGG BASE COURSE","","",95730,16.943069048000002,1621960]
["1176000000-E","SOIL CEMENT BASE","","",104520,2.5499999999999998,266526]
["1187000000-E","PC FOR SOIL CEM BASE","","",2875,162.75,467906.25]
["1209000000-E","ASPHALT CURING SEAL","","",31360,3.3,103488]
["1220000000-E","INCIDENTAL STONE BASE","","",20763,25.406757211999999,527520.5]
["1231000000-E","SHDR BORROW","","",58000,5,290000]
["1245000000-E","SHDR RECONST","","",238.71,3548.95479871,847171]
["1275000000-E","PRIME COAT","","",4635,3.4959546929999998,16203.75]
["1297000000-E","MILL ASP PVT *****\" DTH","(1-1/2\")","",109087,1.708052747,186326.35]
["","","(25\")","",82200,1.6,131520]
["","","(3\")","",89815,2.1587875080000001,193891.5]
["","","(5/8\")","",5333,1.36,7252.88]
["1308000000-E","MILL ASPH PVT ***** - ****","(0\" TO 1 1/2\")","",20640,1.66,34262.400000000001]
["","","(0\" TO 1-1/2\")","",235455,1.6163699220000001,380582.38]
["1330000000-E","INCIDENTAL MILLING","","",52850,5.1354143800000003,271406.65000000002]
["1489000000-E","ASP CNC BAS CRS B250B","","",14856,48.480162897,720221.3]
["1491000000-E","ASP CNC BAS CRS B250C","","",32670,43.619375574000003,1425045]
["1498000000-E","ASP CONC INTR CRS I190B","","",3040,51.674999999999997,157092]
["1503000000-E","ASP CONC INTR CRS I190C","","",78950,43.571057631000002,3439935]
["1519000000-E","ASP CNC SURF CRS S95B","","",179278,40.403943038000001,7243538.0999999996]
["1523000000-E","ASP CNC SURF CRS S95C","","",74905,42.214071156999999,3162045]
["1525000000-E","ASP CONC SURF CRS SF95A","","",114772,40.764926113999998,4678672.0999999996]
["1526000000-E","ASP CONC SURF CRS S475A","","",5154,48,247392]
["1575000000-E","ASP FOR PLANT MIX","","",29250,598.91858632499998,17518368.649999999]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",449,805.679287305,361750]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",205,75,15375]
["1693000000-E","ASPH PLT MIX PVT REPAIR","","",4100,147.46951219499999,604625]
["1704000000-E","PATCHING EXIST PVT","","",70168,93.744171132000005,6577841]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",8383,43.898663962999997,368002.5]
["1839200000-E","APPLICATION OF ULTRATHIN HOT MIX ASPH","","",245896,1.9335593099999999,475454.5]
["1840000000-E","MILLED RUMBLE STRIPS","","",285026,0.14860272399999999,42355.64]
["1891000000-E","GENERIC PAVING ITEM(SY)","FINE MILLING","",122500,1.3213387759999999,161864]
["","","REPAIR JOINTED CONC","PAVEMT SLAB",3145,250,786250]
["","","","PAVEMT SLABS",8500,215,1827500]
["2000000000-N","RIGHT OF WAY MKRS","","",801,161.66666666699999,129495]
["2022000000-E","SUBDRN EXCAVATION","","",11199,26.989920528999999,302260.12]
["2033000000-E","SUBDRN FINE AGG","","",8403,76.588504106000002,643573.19999999995]
["2043000000-E","4\" PERF SUBDRN PIPE","","",25810,7.8,201318]
["2044000000-E","6\" PERF SUBDRN PIPE","","",24180,13.897270471000001,336036]
["2070000000-N","SUBDRN PIPE OUTLET","","",103,388.689320388,40035]
["2076000000-E","4\" OUTLET PIPE","","",312,22.06,6882.72]
["2077000000-E","6\" OUTLET PIPE","","",306,27.632352941000001,8455.5]
["2143000000-E","BLOTTING SAND","","",15,70,1050]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",2,1300,2600]
["2209000000-E","ENDWALLS","","",30.245999999999999,750,22684.5]
["2220000000-E","REINF ENDWALLS","","",32,975,31200]
["2253000000-E","PIPE COLLARS","","",8.75,656.51428571400004,5744.5]
["2264000000-E","PIPE PLUGS","","",0.36799999999999999,970.38043478300006,357.1]
["2275000000-E","FLOWABLE FILL","","",1055,139,146645]
["2286000000-N","MASNRY DRNG STRUCT","","",622,1700.935691318,1057982]
["2297000000-E","MASNRY DRNG STRUCT","","",74.64,810,60458.400000000001]
["2308000000-E","MASNRY DRNG STRUCT","","",471.07,307.55569236000002,144880.26]
["2354200000-N","FRM W/GRATE 84024 STD","","",1,500,500]
["2363000000-N","FRM W/2GRTS 840***** STD","(84033)","",1,600,600]
["2364000000-N","FRM W/2GRTS 84016 STD","","",33,598.78787878799994,19760]
["2364200000-N","FRM W/2GRTS 84020 STD","","",5,590,2950]
["2365000000-N","FRM W/2GRTS 84022 STD","","",3,575,1725]
["2366000000-N","FRM W/2GRTS 84024 STD","","",231,609.02597402599997,140685]
["2367000000-N","FRM W/2GRTS 84029 STD","","",88,605.28409090900004,53265]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",5,577,2885]
["","","(F)","",72,557.29166666699996,40125]
["","","(G)","",53,577.830188679,30625]
["2396000000-N","FRM W/COVER STD 84054","","",72,317.15277777799997,22835]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",8,1400,11200]
["2440000000-N","CONC TRAN SECT FOR CB","","",42,695,29190]
["2451000000-N","CONC TRAN SECT FOR DI","","",26,718.84615384599999,18690]
["2462000000-E","**\" SLUICE GATE","(30\")","",1,5700,5700]
["","","(36\")","",1,6250,6250]
["2473000000-N","GENERIC DRNG ITEM (EA)","BICYCLE SAFE STL FRM ","AND GRATE",3,1375,4125]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",320,16.5,5280]
["","","(8\" X 18\")","",440,19.5,8580]
["2538000000-E","**'-**\" CONC CURB & GUTR","(2'-9\")","",23650,22.56,533544]
["2542000000-E","1'-6\" CONC CURB & GUTR","","",44760,16.77,750625.2]
["2549000000-E","2'-6\" CONC CURB & GUTR","","",7170,18.90111576,135521]
["2556000000-E","SHDR BERM GUTR","","",11786,21.556147123999999,254060.75]
["2577000000-E","CONC EXPRESSWAY GUTR","","",2930,27.721331058000001,81223.5]
["2591000000-E","4\" CONC SIDEWALK","","",2960,32.881891891999999,97330.4]
["2605000000-N","CONC CURB RAMP","","",431,1662.2948491879999,716449.08]
["2612000000-E","6\" CONC DRIVEWAY","","",170,49.017647058999998,8333]
["2619000000-E","4\" CONC PAVED DITCH","","",670,63.55,42578.5]
["2627000000-E","4\" CONC ISLAND COVER","","",2690,32.75,88097.5]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",8080,49.550742573999997,400370]
["2703000000-E","CONC BARRIER  ******","(III)","",145,350,50750]
["2724000000-E","PC REINF BARR SNGL FC","","",400,66.5,26600]
["2752000000-E","GENERIC PAVING ITEM (LF)","DDI BARRIER","",920,400,368000]
["2753000000-E","GENERIC PAV ITEM 846(LF)","18\" CONC CURB & GUTR","",2510,14,35140]
["2759000000-N","GENERIC PAVING ITEM (EA)","EMERGENCY VEHICLE ","ACCESS",1,5800,5800]
["2800000000-N","ADJ CATCH BASINS","","",3,440,1320]
["2815000000-N","ADJ DROP INLETS","","",9,1433.3333333329999,12900]
["2830000000-N","ADJ MANHOLES","","",307,813.82736156399994,249845]
["2845000000-N","ADJ METER OR VAL BOX","","",261,631.59770114900005,164847]
["2860000000-N","CONVERT CB TO JB","","",1,1300,1300]
["3000000000-N","IMPACT ATTEN  350","","",6,14725,88350]
["3030000000-E","STL BM GUARDRAIL","","",30537.5,15.960499386,487393.75]
["3045000000-E","SBGR SHOP CURVED","","",1738.47,17.161998769,29835.62]
["3105000000-N","SBGR TERM SECT","","",6,72.5,435]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",45,21.5,967.5]
["3165000000-N","GR ANCHOR  **********","(350 TL-2)","",3,1725,5175]
["","","(350 TL-2)","",4,1725,6900]
["","","(TL-2)","",22,1785,39270]
["3180000000-N","GR ANCHOR  **********","(B-77 SHOP CURVED)","",2,1875,3750]
["3195000000-N","GR ANCHOR  AT-1","","",8,531.25,4250]
["3210000000-N","GR ANCHOR  CAT-1","","",48,495.83333333299998,23800]
["3215000000-N","GR ANCHOR  III","","",8,1412.5,11300]
["3270000000-N","GR ANCHOR  350","","",98,2007.2448979589999,196710]
["3285000000-N","GR ANCHOR  M-350","","",6,1810,10860]
["3317000000-N","GR ANCHOR  B-77","","",38,1600.131578947,60805]
["3345000000-E","REM & RESET GUARDRAIL","","",84238,4.75,400130.5]
["3360000000-E","REM EXISTING GUARDRAIL","","",28037,1.1093412279999999,31102.6]
["3380000000-E","TEMP STL BM GUARDRAIL","","",900,9.0583333330000002,8152.5]
["3382000000-E","TEMP STL BM GDRAIL SHP CURV","","",100,13.925000000000001,1392.5]
["3387000000-N","TEMP GDRL ANCH UNIT****","(B-77 SHOP CURVED)","",1,950,950]
["","","(CAT-1)","",2,300,600]
["","","(III)","",4,800,3200]
["","","(W-BEAM)","",1,800,800]
["","","(W-BEAM SHOP CURVED)","",1,925,925]
["3389000000-N","TEMP GDRL ANCH UNIT****","(350 TL-2)","",5,870,4350]
["3389100000-N","TEMP GDRL ANCH UNIT350","","",4,1225,4900]
["3503000000-E","WOVEN WIRE FEN 47\" FAB","","",72190,3.1840421110000001,229856]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",4361,16.744060995000002,73020.850000000006]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",1634,34.584332924999998,56510.8]
["3524000000-E","CL FEN **\" FAB VINYL CTD","(48\")","",2450,7,17150]
["3542000000-E","MET LINE PST 48\" CL FEN","","",210,46.25,9712.5]
["3548000000-E","MET TERM PST 48\" CL FEN","","",20,122.5,2450]
["3628000000-E","RIP RAP CL I","","",1889,37.397432504000001,70643.75]
["3635000000-E","RIP RAP CL II","","",1350,35.35,47722.5]
["3642000000-E","RIP RAP CL A","","",35,35.35,1237.25]
["3649000000-E","RIP RAP CL B","","",2635,35.536053131000003,93637.5]
["3651000000-E","BOULDERS","","",220,83.5,18370]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",23911,2.9864183849999999,71408.25]
["3659000000-N","PREFORMED SCOUR HOLE","","",5,1720,8600]
["4048000000-E","REINF CONC FOUNDTN","","",3,817,2451]
["4054000000-E","PLN CONC FOUNDTN","","",2,817,1634]
["4057000000-E","OVERHEAD FOOTING","","",45,1500,67500]
["4060000000-E","SUPPT BRKAWAY STL BM","","",2516,4.95,12454.2]
["4066000000-E","SUPPTS SIMPLE STL BM","","",708,4.0999999999999996,2902.8]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",7079,4.4346673259999996,31393.01]
["4079000000-N","SUPPT BARR SMALL","","",6,192.5,1155]
["4082100000-N","SUPPT OVRHD SIGN STR***","(22+00 -L- NBL)","",1,58750,58750]
["","","(29+70 -L- NBL)","",1,23500,23500]
["","","(33+40 -L- SBL)","",1,52000,52000]
["4096000000-N","SIGN ERECTION  D","","",23,88.111304348000004,2026.56]
["4102000000-N","SIGN ERECTION  E","","",374,60.774598930000003,22729.7]
["4108000000-N","SIGN ERECTION  F","","",55,65.110909090999996,3581.1]
["4109000000-N","SIGN ERECT  *** (OVRHD)","(A)","",7,1.2,8.4]
["4110000000-N","SIGN ERECT  *** (GRD MTD)","(A)","",3,470,1410]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(A)","",8,350,2800]
["","","(D)","",14,133.75,1872.5]
["4138000000-N","DISP SUPPT STL BM","","",16,350,5600]
["4155000000-N","DISP SIGN SYST U-CHAN","","",215,3.0629767440000002,658.54]
["4192000000-N","DISP SUPPT U-CHAN","","",1,5,5]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",2292,5.0022033160000001,11465.05]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",1435,14.519756098,20835.849999999999]
["4410000000-E","WORK ZONE SIGN (BARR)","","",846,6.0471394800000002,5115.88]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",22644,4.8042700050000002,108787.89]
["4415000000-N","FLASHING ARROW BOARD","","",6,3916.6666666669998,23500]
["4420000000-N","PORT CHANGE MSG SIGN","","",4,12250,49000]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",40,46,1840]
["4430000000-N","DRUMS","","",1338,56.434977578000002,75510]
["4435000000-N","CONES","","",121,27.636363635999999,3344]
["4445000000-E","BARRICADES ( III)","","",1762,23.471963678000002,41357.599999999999]
["4450000000-N","FLAGGER","","",1536,25,38400]
["4455000000-N","FLAGGER","","",480,208.75,100200]
["4457000000-N","TEMP TRAF CONTROL","","",16,60681.25,970900]
["4465000000-N","TEMP CRASH CUSHIONS","","",16,5209.375,83350]
["4470000000-N","RESET CRASH CUSHION","","",6,1958.3333333329999,11750]
["4480000000-N","TMA","","",2,13400,26800]
["4485000000-E","PORT CONC BARRIER","","",10405,20.039524267000001,208511.25]
["4490000000-E","PORT CONC BARR(ANCH)","","",50,40,2000]
["4500000000-E","RESET PORT CONC BARR","","",1650,3.7981818180000002,6267]
["4510000000-N","LAW ENFORCEMENT","","",2660,36.293233082999997,96540]
["4516000000-N","SKINNY DRUM","","",216,35.694444443999998,7710]
["4589000000-N","GENERIC TRAF CONTROL ITEM (LS)","FLAGGERS","",1,400000,400000]
["4600000000-N","GENERIC TRAF CNTRL ITEM (EA)","TEMP TRAF SIGNAL SYS","",1,34000,34000]
["","","TEMP TRAF SIGNAL SYS","",1,25000,25000]
["4650000000-N","TEMP RAISED PVT MRKS","","",1525,11.654544262,17773.18]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",318332,0.536834688,170891.66]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",416605,0.57333200500000003,238852.98]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",2471,1.8049129909999999,4459.9399999999996]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",4534,1.937803264,8786]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",200,1.5,300]
["4705000000-E","THERMO LINES 16\" 120MILS","","",450,2.1,945]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",9836,8.8762200080000007,87306.5]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",271,87.656826568,23755]
["4725000000-E","THERMO PVT SYM 90MILS","","",1295,108.285714286,140230]
["4770000000-E","4\" COLD APP PLSTIC LINE**","(IV)","",3468,2.2847981549999998,7923.68]
["4795000000-E","24\" COLD APPL PLSTIC LINE  **","(IV)","",18,20,360]
["4810000000-E","PAINT PVT MKGS 4\"","","",5023761,0.12823121400000001,644202.97]
["4815000000-E","PAINT PVT MKGS 6\"","","",195500,0.212346803,41513.800000000003]
["4820000000-E","PAINT PVT MKGS 8\"","","",4183,0.36647382299999998,1532.96]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",243,3.1481481480000002,765]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",3699,3.9879697219999999,14751.5]
["4840000000-N","PAINT PVT MKG CHAR","","",64,47.78125,3058]
["4845000000-N","PAINT PVT MKG SYMBOL","","",240,54.53125,13087.5]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",1352378,0.84610337499999999,1144251.5900000001]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",314670,0.89148187000000001,280522.59999999998]
["4847110000-E","POLYUREA LINES (8\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",11708,1.952254868,22857]
["4847120000-E","POLYUREA LINES (12\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",21336,2.2346034870000002,47677.5]
["4850000000-E","LINE REML 4\" WIDE","","",13526,1.1411030609999999,15434.56]
["4875000000-N","REML OF SYMBL & CHAR","","",5,121.33,606.65]
["4880000000-E","CURING COMP REML LINES","","",825,1.65,1361.25]
["4892000000-N","GENERIC PVT MKG ITEM (EA) 1205","INTERSTATE SHIELD THERMO-","PLASTIC SYMBOL (90 MILS)",2,750,1500]
["4900000000-N","PERM RAISED PVT MKRS","","",22,23.5,517]
["4905000000-N","SNOWPLB PVT MRKER","","",19447,24.529862703999999,477032.24]
["5000000000-E","***' HIGH MOUNT STD","(60')","",6,14000,84000]
["5020000000-N","PORTABLE DRIVE UNIT","","",1,4000,4000]
["5025000000-E","HIGH MOUNT FOUNDS","","",23.4,670,15678]
["5050000000-N","LIT STD MTLT ************","(35' SA 15' ARM)","",25,2350,58750]
["5070000000-N","STD FOUNDAT ***********","( R1)","",20,1125,22500]
["","","( R2)","",5,1300,6500]
["5120000000-N","SERVICE POLE ************","(30' CL 4)","",1,760,760]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",100,20,2000]
["5145000000-N","LITE CNTRL RW************","(240/480 VOLT)","",1,9350,9350]
["5155000000-E","ELECT DUCT BD SIZE *****","(2\")","",380,7,2660]
["5160000000-E","ELECT DUCT JA SIZE *****","(3\")","",465,18.100000000000001,8416.5]
["","","(4\")","",255,18.7,4768.5]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",485,6,2910]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",330,7,2310]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2 1-1/2\")","",7225,9.5,68637.5]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2 1-1/2\")","",1230,11.1,13653]
["5240000000-N","ELEC JB ************","(PC18)","",13,350,4550]
["","","(PC30)","",4,525,2100]
["5255000000-N","PORTABLE LIGHTING","","",8,54750,438000]
["5270000000-N","GENERIC LIGHT ITEM (EA)","HIGH MT LUMINAIRE - LED","",24,2275,54600]
["","","ROADWAY LIGHT STD ","LUMIN- AIRE - LED",25,1050,26250]
["5325600000-E","6\" WATER LINE","","",45,194,8730]
["5325800000-E","8\" WATER LINE","","",740,87,64380]
["5326200000-E","12\" WATER LINE","","",70,237,16590]
["5327400000-E","24\" WATER LINE","","",60,670,40200]
["5571800000-E","8\" TAPPING VALVE","","",1,16750,16750]
["5572200000-E","12\" TAPPING VALVE","","",1,21000,21000]
["5643000000-E","**\" WATER METER","(1\")","",1,7100,7100]
["5643150000-E","1-1/2\" WATER METER","","",1,6500,6500]
["5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1-1/2\")","",1,5800,5800]
["5666000000-E","FIRE HYDRANT","","",1,5350,5350]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",150,30,4500]
["5882000000-N","GENERIC UTILITY ITEM (EA)","ROTATE TOP FOR EXT MH","(CONCENTRIC TOP)",3,1500,4500]
["","","","HOLE (ECCENTRIC TOP)",3,1500,4500]
["6000000000-E","TEMP SILT FENCE","","",110260,2.3000317429999999,253601.5]
["6006000000-E","EROS CNTRL STONE CL A","","",11085,32.000451060000003,354725]
["6009000000-E","EROS CNTRL STONE CL B","","",40790,32.938220152,1343550]
["6012000000-E","SEDIMENT CNTROL STONE","","",21615,31.424473745,679240]
["6015000000-E","TEMP MULCHING","","",607,729.94233937399997,443075]
["6018000000-E","SEED FOR TEMP SEEDING","","",26750,2.2513271029999999,60223]
["6021000000-E","FERT FOR TEMP SEEDING","","",111,1004.65990991,111517.25]
["6024000000-E","TEMP SLOPE DRNS","","",20875,7.4035928139999996,154550]
["6029000000-E","SAFETY FENCE","","",10900,1.708715596,18625]
["6030000000-E","SILT EXCAVATION","","",163920,4.896864324,802694]
["6036000000-E","MAT FOR EROS CONTROL","","",661190,1.2185179749999999,805671.9]
["6037000000-E","COIR FIBER MAT","","",2850,5.5456140349999998,15805]
["6038000000-E","PERM SOIL REINF MAT","","",24125,4.4444559589999999,107222.5]
["6042000000-E","1/4\" HARDWARE CLOTH","","",14700,4.7278911560000001,69500]
["6045000000-E","**\" TEMP PIPE","(15\")","",115,45.91,5279.65]
["","","(72\")","",100,208.87,20887]
["6048000000-E","FLOAT TURBIDITY CURTN","","",50,27.58,1379]
["6070000000-N","SPECIAL STILLING BASINS","","",42,354.01428571399998,14868.6]
["6071010000-E","WATTLE","","",257,4.8225680930000001,1239.4000000000001]
["6071012000-E","COIR FIBER WATTLE","","",5350,7.3808411209999996,39487.5]
["6071013000-E","WATTLE BARRIER","","",2500,8.82,22050]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",8050,7.4762732920000001,60184]
["6071030000-E","COIR FIBER BAFFLE","","",47150,5.5152873810000003,260045.8]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",165,643.27272727299999,106140]
["","","(2\")","",13,1095.384615385,14240]
["","","(3\")","",1,1018,1018]
["6084000000-E","SEEDING AND MULCHING","","",425.41,1728.5794880230001,735355]
["6087000000-E","MOWING","","",204.3,62.909936367999997,12852.5]
["6090000000-E","SEED FOR REPAIR SEEDING","","",6200,6.5383064519999996,40537.5]
["6093000000-E","FERT FOR REPAIR SEEDING","","",22,694.5,15279]
["6096000000-E","SEED FOR SUPP SEEDING","","",10275,5.4671776159999999,56175.25]
["6108000000-E","FERTILIZER TOPDRESSING","","",305.25,1004.553644554,306640]
["6111000000-E","IMPERVIOUS DIKE","","",3900,19.96,77844]
["6114500000-N","SPECIALIZED HAND MOW","","",195,52.815384614999999,10299]
["6117000000-N","RESP FOR EROS CONTROL","","",238,124.55882352899999,29645]
["6120000000-E","CLVT DIVERSION CHANNEL","","",2700,11.03,29781]
["6123000000-E","REFORESTATION","","",31.2,1347.156730769,42031.29]
["6126000000-E","STRMBK REFORESTATION","","",4.62,13380,61815.6]
["6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","DIVERSION PUMPING FOR MITIGA- TION","",1,8000,8000]
["","","GRADING FOR MITIGATN","",1,33225,33225]
["","","SURVEY FOR MITIGATION","",1,4300,4300]
["6150000000-E","GENERIC EROSION CONTROL ITEM (TON)","AERIAL FERTILIZER TOPDRESSING","",75,10,750]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",12,816.6,9799.2000000000007]
["7060000000-E","SIGNAL CABLE","","",13410,2.3426174500000001,31414.5]
["7120000000-E","VEH SIGNL HD(12\" 3 SECT)","","",99,836.45959596,82809.5]
["7132000000-E","VEH SIGNL HD(12\" 4 SECT)","","",8,940.625,7525]
["7144000000-E","VEH SIGNL HD(12\" 5 SECT)","","",2,1225,2450]
["7264000000-E","MESSENGER CABLE (3/8\")","","",4455,2.391750842,10655.25]
["7300000000-E","UNPAVED TRENCH (********)","(1 1\")","",370,6,2220]
["","","(1 2\")","",4580,5.55,25419]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",155,2.124193548,329.25]
["7301000000-E","DIRECT DRILL (***********)","(2 2\")","",195,19,3705]
["","","(3 2\")","",90,25.5,2295]
["","","(5 2\")","",110,32.75,3602.5]
["","","(7 2\")","",90,37.5,3375]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",30,310.5,9315]
["7348000000-N","JUNCTION BOX (OVER-SIZED HVY-DUTY)","","",16,440,7040]
["7360000000-N","WOOD POLE","","",19,930.52631578900002,17680]
["7372000000-N","GUY ASSEM","","",37,324.32432432399997,12000]
["7408000000-E","1\" RISER W/ WEATHERHD","","",4,337.5,1350]
["7420000000-E","2\" RISER W/ WEATHERHD","","",12,429.16666666700002,5150]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",5970,7.3077889450000004,43627.5]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",14845,1.460508589,21681.25]
["7481000000-N","SITE SURVEY","","",4,350,1400]
["7481240000-N","CAMERA W/O INT LOOP EMUL PORCESS","","",11,4100,45100]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",4,5250,21000]
["7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",6,585,3510]
["7575142060-N","MOD RADIO INSTALL","","",8,820,6560]
["7576000000-N","MTL STRAIN SIGNAL POLE","","",8,7125,57000]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",6,10750,64500]
["7613000000-N","SOIL TEST","","",14,882.14285714300001,12350]
["7614100000-E","DRILLED PIER FOUND","","",92,555.43478260899997,51100]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",6,60,360]
["7636000000-N","SIGN FOR SIGNALS","","",31,321,9951]
["7642200000-N"," II PED W/ FOUND","","",16,1170,18720]
["7684000000-N","SIGNAL CABINET FOUND","","",3,1050,3150]
["7756000000-N","CONTLR WITH CBNT 2070L BASE MTD","","",3,12500,37500]
["7768000000-N","CONTLR WITH CBNT 2070L POLE MTD","","",4,11075,44300]
["7780000000-N","DETECTOR CARD ( 2070L)","","",35,115.428571429,4040]
["7901000000-N","CABINET BASE EXTENDER","","",3,410,1230]
["7960000000-N","METAL POLE FOUND REML","","",4,875,3500]
["7972000000-N","METAL POLE REML","","",8,470,3760]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","PROTECTIVE BLACK COATING FOR","METAL STRAIN POLE ASSEM",4,760,3040]
["","","","PEDESTRIAN SIG-NAL PEDESTAL",16,62,992]
["","","","SINGLE MAST ARM ASSEM",6,1600,9600]
["8007000000-N","CM&R TEMP STR ***********","(13+0130-L-)","",1,165000,165000]
["8017000000-N","CM&R TEMP ACCESS ******","(122+2250-L-LT)","",1,62869.31,62869.31]
["8021000000-N","REMV EXIST STR **********","(13+0130-L-)","",1,25000,25000]
["","","(13+5295 -L-)","",1,112000,112000]
["","","(16+0000-L-)","",1,12000,12000]
["8035000000-N","REMV EXIST STR **********","(122+2250-L-LT)","",1,134124.97,134124.97]
["","","(24+1131-L-RT)","",1,63872.18,63872.18]
["","","(247+8750-L-LT)","",1,14577.88,14577.88]
["","","(247+8750-L-RT)","",1,42568.55,42568.55]
["8070000000-E","FOUND EXCAVATION","","",95,100,9500]
["8096000000-E","PILE EXCAVATION IN SOIL","","",37,370,13690]
["8097000000-E","PILE EXCAV NOT IN SOIL","","",13,1500,19500]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",192,461.39,88586.880000000005]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",4.5,550,2475]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",134,1582.81,212096.54]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",16,1400,22400]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",117.6,128.16003401399999,15071.62]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",2,2800,5600]
["8112730000-N","PDA TESTING","","",8,2500,20000]
["8113000000-N","SID INSPECTIONS","","",9,1409.973333333,12689.76]
["8114000000-N","SPT TESTING","","",9,1764.4,15879.6]
["8115000000-N","CSL TESTING","","",5,3575.9119999999998,17879.560000000001]
["8121000000-N","UNCL STR EXCAV STA ****","(122+2250-L-LT)","",1,10396.790000000001,10396.790000000001]
["","","(122+2250-L-RT)","",1,3465.61,3465.61]
["","","(13+0130-L-)","",1,17000,17000]
["","","(247+8750-L-LT)","",1,13862.38,13862.38]
["","","(247+8750-L-RT)","",1,55449.55,55449.55]
["8126000000-N","CULV EXCAV @ ************","(11+0796-Y34-)","",1,16455.84,16455.84]
["","","(134+8045-L-)","",1,75608.19,75608.19]
["","","(14+9030-Y17-)","",1,28730.9,28730.9]
["","","(155+4457-L-)","",1,42518.34,42518.34]
["","","(16+0000-L-)","",1,12000,12000]
["","","(319+7616-L-)","",1,55149.760000000002,55149.760000000002]
["","","(323+5866-L-)","",1,41273.230000000003,41273.230000000003]
["","","(327+5047-L-)","",1,11029.95,11029.95]
["","","(345+9842-L-)","",1,16544.919999999998,16544.919999999998]
["","","(44+192-L-)","",1,70093.22,70093.22]
["8133000000-E","FND COND MAT BOX CULV","","",1520,45.567236842,69262.2]
["8147000000-E","REINF CONC DECK SLAB","","",54715,29.693412774999999,1624675.08]
["8161000000-E","GROOVING BRG FLOORS","","",56025,0.58397643899999996,32717.279999999999]
["8182000000-E","CL A CONC (BRG)","","",915.6,677.95507863700004,620735.67000000004]
["8196000000-E","CL A CONC (CULV)","","",2567,519.73770159699995,1334166.68]
["8210000000-N","BRG APPR SLAB ***********","(122+2250-L-LT)","",1,43500,43500]
["","","(122+2250-L-RT)","",1,43500,43500]
["","","(13+0130-L-)","",1,25000,25000]
["","","(13+5295 -L-)","",1,30000,30000]
["","","(24+1131-L-LT)","",1,44500,44500]
["","","(24+1131-L-RT)","",1,44500,44500]
["","","(247+8750-L-LT)","",1,44500,44500]
["","","(247+8750-L-RT)","",1,44500,44500]
["8217000000-E","REINF STL (BRG)","","",187036,0.90352333200000001,168991.39]
["8238000000-E","SPIRL COL REINF STL BRG","","",14558,1.8216547599999999,26519.65]
["8245000000-E","REINF STL (CULVERT)","","",312968,1.2525594950000001,392011.04]
["8262000000-E","45\" PRESTR CONC GIRDR","","",659.79,190,125360.1]
["8280000000-E","STRUCTURAL STL","","",795200,1.867454728,1485000]
["8364000000-E","HP12X53 PILES","","",2098,43.760009533000002,91808.5]
["8384000000-E","HP14X73 PILES","","",5300,55.69,295157]
["8385200000-E","PP**X**** GALV STL PILE","(PP 24 x 050)","",775,125,96875]
["8393000000-N","PILE REDRIVES","","",47,588.6,27664.2]
["8475000000-E","TWO BAR METAL RAIL","","",379.93,142.90290316599999,54293.1]
["8503000000-E","CONC BARRIER RAIL","","",3343.39,103.02342532599999,344447.49]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-11 1/4\")","",140,100,14000]
["","","(1'-2\" x 2'-6\")","",271.67,100,27167]
["8531000000-E","4\" SLOPE PROTECTION","","",2211,55,121605]
["8559000000-E","SURFACE PREP CL II","","",76,350,26600]
["8594000000-E","RIP RAP B","","",400,40,16000]
["8608000000-E","RIP RAP II (2'-0\")","","",2047,40.732779678,83380]
["8622000000-E","GEOTEXTILE FOR DRNG","","",3140,3.0541401270000001,9590]
["8657000000-N","ELASTOMERIC BEARINGS","","",3,21978.99,65936.97]
["8706000000-N","EXPANSION JOINT SEALS","","",1,242870.37,242870.37]
["8741000000-N","STR DRN SYS ************","(122+2250-L-LT)","",1,56773.42,56773.42]
["","","(122+2250-L-RT)","",1,56773.42,56773.42]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",700,170,119000]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",6700,30.44,203948]
["","","(2)","",2300,29.17,67091]
["","","(5)","",2400,66.959999999999994,160704]
["","","(6)","",2625,66.709999999999994,175113.75]
["","","(7)","",1800,34.090000000000003,61362]
["8802010000-E","SOIL NAIL RET WALLS","","",3700,98.38,364006]
["8802014000-E","SOLDIER PILE RET WALLS","","",6595,112.909401061,744637.5]
["8802015100-N","SOIL NAIL VERIFICA TESTS","","",2,1477.68,2955.36]
["8802015110-N","SOIL NAIL PROOF TESTS","","",8,615.41,4923.28]
["8802031000-E","PRECAST GRAVITY RETAINING WALLS","","",1359,75.5,102604.5]
["8860000000-N","GENERIC STR ITEM (LS)","EXPANSION JOINT SEALS","",1,88000,88000]
["","","FOAM JOINT SEALS","",1,47000,47000]
["","","VOLUMETRIC MIXER","",1,1,1]
["8867000000-E","GENERIC STR ITEM (LF)","74\" MOD PRESTR CONC ","GDRS",3783.26,290.34999973599997,1098469.54]
["","","CONC BARR RAIL WITH","MOMENT SLAB",2175,309.19,672488.25]
["8882000000-E","GENERIC STR ITEM (CF)","CONC FOR DECK REPAIR","",220,75,16500]
["8893000000-E","GENERIC STR ITEM (SY)","HYDRODEMOLITION OF ","BRG DECK",186,315,58590]
["","","SCARIFYING BRG DECK","",186,100,18600]

{"sheet":"Items - Div 14","index":16,"n_rows":653,"n_cols":7,"rows_kept":653,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2014 BID AVERAGES - DIVISION 14"]
["Item #","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",15,204724.006666667,3070860.1]
["0000400000-N","CONST SURVEYING","","",6,40438,242628]
["0000900000-N","GENERIC MISC ITEM (LS)","DESIGN & CONST OF","BRIDGES",1,3536927,3536927]
["","","","CLVT 430020",1,327000,327000]
["","","","CLVT 430273",1,614000,614000]
["","","","CLVT 430305",1,470000,470000]
["","","","CLVT 430309",1,390000,390000]
["","","","CLVT 430310",1,458000,458000]
["","","","CLVT 430314",1,369000,369000]
["","","","CLVT 430315",1,507000,507000]
["","","","CLVT 430317",1,410000,410000]
["","","","CLVT 430372",1,504000,504000]
["","","","CLVT 490055",1,512000,512000]
["","","DESIGN & CONST OF","CLVT 430102",1,411000,411000]
["0000915000-N","GENERIC MISC ITEM (EA)","END BENTS STR 430326","",2,46290,92580]
["","","END BENTS STR 430334","",2,80437.5,160875]
["","","END BENTS STR 490103","",2,53595,107190]
["","","END BENTS STR 490164","",2,57111.5,114223]
["","","END BENTS STR 490182","",2,58790,117580]
["","","END BENTS STR 490337","",2,87745,175490]
["","","RIGHT OF WAY ACQUISIT","",34,4470.5882352939998,152000]
["0000930000-E","GENERIC MISC ITEM (LF)","AVE FOUND LENGTH AT END","BENT 1 STR 430326",40,1151.5,46060]
["","","","BENT 1 STR 430334",18,1569,28242]
["","","","BENT 1 STR 490103",10,4151,41510]
["","","","BENT 1 STR 490164",11,3129,34419]
["","","","BENT 1 STR 490182",11,4137.5,45512.5]
["","","","BENT 1 STR 490337",47,387.5,18212.5]
["","","","BENT 2 STR 430326",16,1525,24400]
["","","","BENT 2 STR 430334",24,232,5568]
["","","","BENT 2 STR 490103",10,4151,41510]
["","","","BENT 2 STR 490164",20,427.5,8550]
["","","","BENT 2 STR 490182",10,3891,38910]
["","","","BENT 2 STR 490337",55,356.5,19607.5]
["","","BRG LGTH STR 430326","",50,2894,144700]
["","","BRG LGTH STR 430334","",40,1567.5,62700]
["","","BRG LGTH STR 490103","",30,1802,54060]
["","","BRG LGTH STR 490164","",55,1865,102575]
["","","BRG LGTH STR 490182","",35,1987.5,69562.5]
["","","BRG LGTH STR 490337","",35,1961,68635]
["0001000000-E","CLEARING & GRUBBING","","",9,19720.430107527001,183400]
["0008000000-E","SUPP CLEAR & GRUBBING","","",2,2330,4660]
["0015000000-N","SEALING ABANDONED WELLS","","",2,2000,4000]
["0022000000-E","UNCLAS EXCAVATION","","",568800,6.2744198310000003,3568890]
["0029000000-N","REINF BRG APPR **********","(27+1172)","",1,85000,85000]
["0030000000-N","BRG APP SUB REG TIER**","(10+5800-L-)","",1,6000,6000]
["","","(12+1950)","",1,36700,36700]
["","","(12+7150-L-)","",1,10000,10000]
["","","(12+8100-L2-)","",1,20000,20000]
["0036000000-E","UNDERCUT EXCAVATION","","",6525,6.674329502,43550]
["0043000000-N","GRADING","","",8,69258.429999999993,554067.43999999994]
["0050000000-E","SUPP CLEAR & GRUBBING","","",8,450.625,3605]
["0057000000-E","UNDERCUT EXCAVATION","","",825,15.812121211999999,13045]
["0063000000-N","GRADING","","",3,83366.666666667006,250100]
["0106000000-E","BORROW EXCAVATION","","",7825,3.5,27387.5]
["0134000000-E","DRNG DITCH EXCAVATION","","",2130,9.9107981219999992,21110]
["0141000000-E","BERM DITCH CONST","","",800,16.2,12960]
["0156000000-E","REM OF EXT ASPH PVMT","","",24500,3.5,85750]
["0192000000-N","PROOF ROLLING","","",11,168.181818182,1850]
["0194000000-E","SEL GRANULR MATL CL III","","",130,25,3250]
["0195000000-E","SELECT GRANULAR MAT'L","","",4875,42.443076923,206910]
["0196000000-E","GEOTEXTILE SOIL STABIL","","",8115,2.3240911889999998,18860]
["0199000000-E","TEMP SHORING","","",1492,61.521447721000001,91790]
["0223000000-E","ROCK PLATING","","",40,100,4000]
["0248000000-N","GENERIC GRADING ITEM (LS)","ENERGY DISSIPATOR BASIN","",1,3000,3000]
["","","HAZARDOUS SPILL BASIN/","BIORETENTION BASIN",1,4500,4500]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",2460,33.43495935,82250]
["0320000000-E","FND CONDIT GEOTEXTILE","","",9053,5.5025405940000001,49814.5]
["0335200000-E","15\" DRNG PIPE","","",196,30.555102041000001,5988.8]
["0335300000-E","18\" DRNG PIPE","","",312,37.557692308,11718]
["0343000000-E","15\" SIDE DRN PIPE","","",32,42,1344]
["0344000000-E","18\" SIDE DRN PIPE","","",60,49.066666667,2944]
["0345000000-E","24\" SIDE DRN PIPE","","",64,48.8,3123.2]
["0354000000-E","***\" RC PIPE CULV *****","(18\" V)","",80,48,3840]
["0366000000-E","15\" RC PIPE CULV III","","",900,24.057777777999998,21652]
["0372000000-E","18\" RC PIPE CULV III","","",536,46.835820896000001,25104]
["0378000000-E","24\" RC PIPE CULV III","","",724,45.254143646000003,32764]
["0384000000-E","30\" RC PIPE CULV III","","",904,45,40680]
["0448200000-E","15\" RCP CULV CL IV","","",8884,39.483025664000003,350767.2]
["0448300000-E","18\" RCP CULV CL IV","","",1892,49.754756870999998,94136]
["0448400000-E","24\" RCP CULV CL IV","","",492,70.694308942999996,34781.599999999999]
["0448500000-E","30\" RCP CULV CL IV","","",44,81.599999999999994,3590.4]
["0448700000-E","42\" RCP CULV CL IV","","",224,128.80000000000001,28851.200000000001]
["0542000000-E","**\" PVC PIPE CLVTS","(8\")","",10,500,5000]
["0576000000-E","**\" CS PIPE CULV *****\"","(120\" 0138\")","",104,525,54600]
["","","(30\" 0138\")","",328,65,21320]
["","","(36\" 0079\")","",156,83.9,13088.4]
["","","(60\" 0138\")","",40,195,7800]
["0582000000-E","15\" CS PIPE CULV 0064\"","","",460,38.017391304,17488]
["0588000000-E","18\" CS PIPE CULV 0064\"","","",128,43.5,5568]
["0594000000-E","24\" CS PIPE CULV 0064\"","","",128,55.1,7052.8]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\" 0064\")","",8,424.5,3396]
["","","(18\" 0064\")","",2,514,1028]
["","","(24\" 0064\")","",2,598.1,1196.2]
["","","(30\" 0138\")","",3,900,2700]
["0974000000-E","**\"WLD STL PIPE ***\" B RR","(36\" 05\")","",130,229.4,29822]
["0986000000-E","GENERIC PIPE ITEM (LF)","15\" DUCTILE IRON PIPE","",1020,80.7,82314]
["","","18\" DUCTILE IRON PIPE","",448,88.8,39782.400000000001]
["","","24\" DUCTILE IRON PIPE","",460,140.5,64630]
["","","36\" DUCTILE IRON PIPE","",240,355.9,85416]
["","","48\" DUCTILE IRON PIPE","",12,697.1,8365.2000000000007]
["0992000000-E","GENERIC PIPE ITEM (EA)","15\" DUCTILE IRON PIPE ELBOW","",2,1737.5,3475]
["0995000000-E","PIPE REMOVAL","","",4085,7.1793145650000003,29327.5]
["0996000000-N","PIPE CLEAN-OUT","","",2,3600,7200]
["1011000000-N","FINE GRADING","","",2,97980,195960]
["1077000000-E","57 STONE","","",180,30.2,5436]
["1099500000-E","SHALLOW UNDERCUT","","",2926,10.766233765999999,31502]
["1099700000-E","CL IV SUBGRD STABIL","","",4989,28.339346561999999,141385]
["1110000000-E","STABILIZER AGG","","",1750,23.942857143000001,41900]
["1115000000-E","GEOTEXT FOR PVT STABIL","","",5000,5.9,29500]
["1121000000-E","AGG BASE COURSE","","",1599,35.627892433,56969]
["1220000000-E","INCIDENTAL STONE BASE","","",2895,31.126079446999999,90110]
["1231000000-E","SHOULDER BORROW","","",900,1.1000000000000001,990]
["1275000000-E","PRIME COAT","","",1130,10.606194690000001,11985]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",4382,3.204472843,14042]
["","","(3\")","",64142,2.3693640669999998,151975.75]
["","","(5\")","",310,73.03,22639.3]
["","","(5-1/2\")","",170,17,2890]
["1308000000-E","MILL ASPH PVMT **** - *****","(0\" TO 3\")","",2000,7.7,15400]
["","","(0\" TO 5-1/2\")","",420,12.4,5208]
["1330000000-E","INCIDENTAL MILLING","","",1760,16.907670455000002,29757.5]
["1489000000-E","ASP CNC BAS CRS B250B","","",9645,64.878693623999993,625755]
["1491000000-E","ASP CNC BAS CRS B250C","","",15139,71.288321554000007,1079233.8999999999]
["1498000000-E","ASP CONC INTR CRS I190B","","",15414,48.266997535000002,743987.5]
["1503000000-E","ASP CONC INTR CRS I190C","","",10912,72.471361803999997,790807.5]
["1519000000-E","ASP CONC SURF CRS S95B","","",22225,52.802362205000001,1173532.5]
["1523000000-E","ASP CONC SURF CRS S95C","","",15235,74.629215622000004,1136976.1000000001]
["1525000000-E","ASP CONC SURF CRS SF95A","","",1340,93.843731343000002,125750.6]
["1525100000-E","ASP CONC SURF CRS SF95A LEVEL","","",5959,49.5,294970.5]
["1575000000-E","ASP FOR PLANT MIX","","",5087,665.42200707699999,3385001.75]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",9,780,7020]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",145,70,10150]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",1085,201.53594469999999,218666.5]
["1840000000-E","MILLED RUMBLE STRIPS","","",12550,2.0860557769999999,26180]
["1847000000-E","******\"PCC PVMT THRU LNS","(8-1/2\")","",232,68,15776]
["2022000000-E","SUBDRN EXCAVATION","","",1193.9000000000001,12.443420722000001,14856.2]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",500,4.9000000000000004,2450]
["2033000000-E","SUBDRN FINE AGG","","",750.5,52.397068621000003,39324]
["2036000000-E","SUBDRN COARSE AGG","","",84,74.400000000000006,6249.6]
["2044000000-E","6\" PERF SUBDRN PIPE","","",4904,5.6937194130000002,27922]
["2070000000-N","SUBDRN PIPE OUTLET","","",16,305.79374999999999,4892.7]
["2077000000-E","6\" OUTLET PIPE","","",96,15.25,1464]
["2209000000-E","ENDWALLS","","",5.6,1809,10130.4]
["2220000000-E","REINF ENDWALLS","","",5.9,1000,5900]
["2253000000-E","PIPE COLLARS","","",2.2229999999999999,1080,2400.84]
["2264000000-E","PIPE PLUGS","","",0.68100000000000005,1164.7870778270001,793.22]
["2275000000-E","FLOWABLE FILL","","",42,270,11340]
["2286000000-N","MASNRY DRNG STRUCT","","",261,1330.7287356320001,347320.2]
["2297000000-E","MASNRY DRNG STRUCT","","",30.5,1454.458360656,44360.98]
["2308000000-E","MASNRY DRNG STRUCT","","",80.5,285.15155279499999,22954.7]
["2354200000-N","FRM W/GRATE 84024 STD","","",4,700,2800]
["2364000000-N","FRM W/2GRTS 84016 STD","","",11,423.27272727299999,4656]
["2364200000-N","FRM W/2GRTS 84020 STD","","",9,398.6,3587.4]
["2365000000-N","FRM W/2GRTS 84022 STD","","",22,415.45454545500002,9140]
["2366000000-N","FRM W/2GRTS 84024 STD","","",18,376.444444444,6776]
["2367000000-N","FRM W/2GRTS 84029 STD","","",16,407.73124999999999,6523.7]
["2374000000-N","FRM-GRT-HD 84003 **","(E)","",18,476.73333333300002,8581.2000000000007]
["","","(F)","",52,465.27692307699999,24194.400000000001]
["","","(G)","",60,456.27333333299998,27376.400000000001]
["2396000000-N","FRM W/COVER STD 84054","","",8,316.8,2534.4]
["2407000000-N","STL FRAM W/ 2 GTR STD 84037","","",32,1285.2,41126.400000000001]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",34,607.47941176500001,20654.3]
["2462000000-E","**\" SLUICE GATE","(18\")","",1,4000,4000]
["","","(6\")","",1,2300,2300]
["2473000000-N","GENERIC DRNG ITEM (EA)","RETICULINE FRM & GRATE","",2,7000,14000]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",100,15.25,1525]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",330,14,4620]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",21340,18.502225867,394837.5]
["2556000000-E","SHOULDER BERM GUTTER","","",1176,23.332482992999999,27439]
["2570000000-N","MOD CONC FLUME","","",1,1800,1800]
["2577000000-E","CONC EXPRESSWY GUTR","","",195,52.32,10202.4]
["2591000000-E","4\" CONC SIDEWALK","","",6455,32.989930287,212950]
["2605000000-N","CONC CURB RAMP","","",25,1135.2,28380]
["2612000000-E","6\" CONC DRIVEWAY","","",90,47.422222222000002,4268]
["2619000000-E","4\" CONC PAVED DITCH","","",491,62.596741344000002,30735]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",400,55.924999999999997,22370]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",3380,46.136094675000002,155940]
["2703000000-E","CONC BARR ******","(IV)","",1865,54.71,102034.15]
["2717000000-E","VAR HT CONC BARR *******","(T1)","",960,96.6,92736]
["","","(T2)","",280,178.6,50008]
["2724000000-E","PC REINF BARR SNGL FC","","",1100,99.8,109780]
["2738000000-E","GENERIC PAVING ITEM (SY)","3' x 6\" CONCRETE PAD","",230,46.5,10695]
["","","7\" CONC TRUCK APRON","",325,63,20475]
["2815000000-N","ADJ DROP INLETS","","",2,1026,2052]
["2893000000-N","CONVERT CB TO JB W/MH","","",1,1242,1242]
["3030000000-E","STL BM GRDRL","","",7087.5,16.888818342,119699.5]
["3045000000-E","SBGR SHOP CURVED","","",600,17.201049999999999,10320.629999999999]
["3090000000-N","TRIPLE CORRU GR TERM SECT","","",4,150,600]
["3105000000-N","SBGR TERM SECT","","",2,57.8,115.6]
["3150000000-N","ADDIT GRDRL POSTS","","",65,22.303846153999999,1449.75]
["3165000000-N","GR ANCHOR **********","(350 TL-2)","",12,2195,26340]
["","","(350 TL-2)","",2,1700,3400]
["3180000000-N","GR ANCHOR **********","(III SHOP CURVED)","",5,1702,8510]
["","","(T-101)","",4,2550,10200]
["3195000000-N","GR ANCHOR AT-1","","",7,585.771428571,4100.3999999999996]
["3210000000-N","GR ANCHOR CAT-1","","",10,560.77,5607.7]
["3215000000-N","GR ANCHOR III","","",11,1545.2727272730001,16998]
["3270000000-N","GR ANCHOR 350","","",17,1988.088235294,33797.5]
["3317000000-N","GR ANCHOR B-77","","",5,1523.1,7615.5]
["3345000000-E","REM & RESET GRDRL","","",740,6.5,4810]
["3360000000-E","REM EXISTING GRDRL","","",4758,1.291929382,6147]
["3380000000-E","TEMP STL BM GRDRL","","",375,17.666666667000001,6625]
["3382000000-E","TEMP STL BM GDRAIL SHP CURV","","",50,12,600]
["3387000000-N","TEMP GDRL ANCH UNIT****","(350 TL-2)","",4,1100,4400]
["","","(AT-1)","",2,300,600]
["","","(TEMP RETROFIT)","",2,1500,3000]
["3389000000-N","TEMP GDRL ANCH UNIT****","(350 TL-2)","",2,1100,2200]
["3389100000-N","TEMP GDRL ANCH UNIT350","","",1,1100,1100]
["3420000000-E","GENERIC GRDRL ITEM (LF)","WEATHERING STEEL BEAM GUARD-","RAIL W/ PAINTED LAPS",150,21.5,3225]
["","","","RAIL W/ PAINT LAPS SHP CURV",81.25,21.500061538000001,1746.88]
["3435000000-N","GENERIC GRDRL ITEM (EA)","IMPACT ATTENUATOR UNIT"," 350 (TEMP)",2,5500,11000]
["","","PAINTED GRDRL ANCHOR","UNITS 350",1,1160,1160]
["","","WEATHERING SB GRDRL ANCHOR","UNITS AT-1 W/ PAINTED LAPS",1,1160,1160]
["","","WEATHERING STL ADDIT","GRDRL POSTS",5,22,110]
["3503000000-E","WOVEN WIRE FEN 47\" FAB","","",2150,4,8600]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",130,15.8,2054]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",50,33.6,1680]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",1405,5.4,7587]
["3542000000-E","MET LINE PST 48\" CL FEN","","",118,41,4838]
["3548000000-E","MET TERM PST 48\" CL FEN","","",7,135,945]
["3574000000-E","GENERIC FENCING ITEM 867 (LF)","BARBED WIRE FENCE RESET (ELEC-","TRIC FENCE)",800,6.5,5200]
["3628000000-E","RIP RAP CL I","","",1224,54.553104574999999,66773]
["3635000000-E","RIP RAP CL II","","",270,47.348148148,12784]
["3649000000-E","RIP RAP CL B","","",698,50.64469914,35350]
["3656000000-E","GEOTEXTILE FOR DRNGE","","",13497,3.2131584800000002,43368]
["3804000000-E","ABC (SUB-BALLAST)","","",2242,27.3,61206.6]
["4048000000-E","REINF CONC FOUNDTN","","",36,787.8,28360.799999999999]
["4054000000-E","PLN CONC FOUNDTN","","",3,203.5,610.5]
["4057000000-E","OVERHEAD FOOTING","","",48,1391.8,66806.399999999994]
["4060000000-E","SUPPT BRKAWAY STL BM","","",17475,3.9804005720000002,69557.5]
["4066000000-E","SUPPTS SIMPLE STL BM","","",10552,3.2,33766.400000000001]
["4072000000-E","SUPPT 3-LB STL U-CHAN","","",5061,5.5334321280000003,28004.7]
["4078000000-E","SUPPT 2-LB STL U-CHAN","","",3,61.666666667000001,185]
["4079000000-N","SUPPT BARR SMALL","","",3,157.5,472.5]
["4082100000-N","SUPPT OVRHD SIGN STR**","(12+50-Y2L2-)","",1,47268,47268]
["","","(20+00-Y2L2-)","",1,36764,36764]
["4096000000-N","SIGN ERECTION D","","",25,112.56,2814]
["4102000000-N","SIGN ERECTION E","","",242,55.339586777000001,13392.18]
["4108000000-N","SIGN ERECTION F","","",16,106.875,1710]
["4109000000-N","SIGN ERECT *** (OVRHD)","(A)","",5,1050.4000000000001,5252]
["","","(B)","",5,367.6,1838]
["4110000000-N","SIGN ERECT *** (GRD MTD)","(A)","",25,411.68,10292]
["","","(B)","",2,262.60000000000002,525.20000000000005]
["4114000000-N","SIGN ERECTION MILEMKRS","","",3,58.333333332999999,175]
["4116000000-N","SIGN ERECTION OVERLAY (GRD MTD)","","",1,500,500]
["4116100000-N","SIGN ERECT RELOC ** GRD MTD","(A)","",2,367.6,735.2]
["","","(D)","",7,105,735]
["","","(E)","",1,350,350]
["4138000000-N","DISPOSE SUPPT STL BM","","",2,525.20000000000005,1050.4000000000001]
["4152000000-N","DISP SIGN SYST STL BM","","",11,468.30909090900002,5151.3999999999996]
["4155000000-N","DISP SIGN SYST U-CHAN","","",114,1.561403509,178]
["4192000000-N","DISPOSE SUPPT U-CHAN","","",1,5,5]
["4234000000-N","DISP SIGN A OR B(OVRHD)","","",1,52.5,52.5]
["4236000000-N","DISPOSE SIGN A B OR C (GRD MTD)","","",1,1,1]
["4238000000-N","DISPOSE SIGN D E F","","",1,1,1]
["4360000000-N","GENERIC SIGNING ITM(EA)","DISP OF SIGN ON SPAN ","WIRE",2,525.20000000000005,1050.4000000000001]
["4400000000-E","WORK ZONE SIGN (STAT)","","",5370,4.9526741149999998,26595.86]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",2585,13.99098646,36166.699999999997]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",1229,6.1745728230000001,7588.55]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",1120,4.4000000000000004,4928]
["4415000000-N","FLASHING ARROW BOARD","","",17,2622.5764705880001,44583.8]
["4420000000-N","PORT CHANGE MSG SIGN","","",16,8958.75,143340]
["4430000000-N","DRUMS","","",1562,53.712195903000001,83898.45]
["4435000000-N","CONES","","",309,25.097087379000001,7755]
["4445000000-E","BARRICADES ( III)","","",1248,21.149935896999999,26395.119999999999]
["4450000000-N","FLAGGER","","",3752,17.552238805999998,65856]
["4455000000-N","FLAGGER","","",60,250,15000]
["4457000000-N","TEMP TRAFFIC CONTROL","","",1,21600,21600]
["4465000000-N","TEMP CRASH CUSHIONS","","",12,4608.2916666669998,55299.5]
["4470000000-N","RESET CRASH CUSHION","","",2,1000,2000]
["4480000000-N","TMA","","",12,16758.333333333001,201100]
["4485000000-E","PORT CONC BARR","","",5751,21.828499391000001,125535.7]
["4490000000-E","PORT CONC BARR(ANCH)","","",620,35.158064516000003,21798]
["4500000000-E","RESET PORT CONC BARR","","",2560,3.25,8320]
["4505000000-E","RESET PORT CONC BARR ANCH","","",400,15,6000]
["4507000000-E","H2O FILLED BARR","","",40,75,3000]
["4510000000-N","LAW ENFORCEMENT","","",5050,42.920348515000001,216747.76]
["4516000000-N","SKINNY DRUM","","",289,31.320415225000001,9051.6]
["4520000000-N","TUBULAR MKRS (FIXED)","","",50,47.3,2365]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","TEMP TRAF SIGNAL SYS","",1,14000,14000]
["4650000000-N","TEMP RAISED PVMT MRKS","","",1415,8.7827915189999999,12427.65]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",123340,0.584303146,72067.95]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",49115,0.72580677999999998,35648]
["4688000000-E","THERMO PVT MKG LINES6\"90 MILS","","",8208,0.7,5745.6]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",3373,0.7,2361.1]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",4555,1.579143798,7193]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",973,1.482168551,1442.15]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",1167,3.2,3734.4]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",90,5.25,472.5]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",1818,9.2802805280000005,16871.55]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",16,78.8,1260.8]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",283,99.089752649999994,28042.400000000001]
["4770000000-E","4\" COLD APPL PLSTIC LINES **","(II)","",971,3.36,3262.56]
["","","(IV)","",8067,1.92,15488.64]
["4780000000-E","8\" COLD APPL PLSTIC LINES **","(II)","",178,6.72,1196.1600000000001]
["4800000000-N","COLD APP PLAS CHAR *","(II)","",4,63,252]
["4805000000-N","COLD APP PLASTIC SYM**","(II)","",10,157.5,1575]
["4810000000-E","PAINT PVMT MKGS 4\"","","",293033,0.210753738,61757.8]
["4815000000-E","PAINT PVMT MKGS 6\"","","",21444,0.1,2144.4]
["4820000000-E","PAINT PVMT MKGS 8\"","","",6471,0.2,1294.2]
["4825000000-E","PAINT PVMT MKGS 12\"","","",2967,0.1,296.7]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",2521,1.463903213,3690.5]
["4840000000-N","PAINT PVT MKG CHAR","","",32,25.2,806.4]
["4845000000-N","PAINT PVT MKG SYMBOL","","",402,26.427860697,10624]
["4847000000-E","POLYUREA LINES (4\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",13691,1.133535899,15519.24]
["4847100000-E","POLYUREA LINES (6\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",370,35.102459459000002,12987.91]
["4847110000-E","POLYUREA LINES (8\" *****)","(HIGHLY REFLECTIVE ELEMENTS)","",334,4.5,1503]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",33593,0.69620516200000004,23387.62]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",1326,1.1000000000000001,1458.6]
["4865000000-E","LINE REMOVAL 12\" WIDE","","",45,2.1,94.5]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",107,2.1,224.7]
["4875000000-N","REM OF SYMBL & CHAR","","",25,26.3,657.5]
["4900000000-N","PERM RAISED PVMT MKRS","","",68,14.555147058999999,989.75]
["4905000000-N","SNOWPLB PVMT MRKER","","",2079,32.152717653000003,66845.5]
["5010000000-E","100' HIGH MOUNT STD","","",3,17230.099999999999,51690.3]
["5020000000-N","PORTABLE DRIVE UNIT","","",1,4110.5,4110.5]
["5025000000-E","HIGH MOUNT FOUNDS","","",19,592.4,11255.6]
["5030000000-N","HM LUMINAIRE ************","(750W HPS)","",18,860.2,15483.6]
["5050000000-N","LIT STD MTLT ************","(45' TA 15' ARM)","",3,2797,8391]
["5070000000-N","STD FOUNDAT ***********","(R1)","",21,1097.8761904759999,23055.4]
["","","(R2)","",1,1236.2,1236.2]
["5090000000-N","LITE STD LUM RDW 400W HPS","","",6,412.1,2472.6]
["5120000000-N","SERVICE POLE ************","(30' CL 4)","",1,669.6,669.6]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",25,17.5,437.5]
["5145000000-N","LITE CNTRL RW************","(240/480 V)","",1,10817.1,10817.1]
["5155000000-E","ELECT DUCT BD SIZE *****","(2\")","",1554,6.9078507079999998,10734.8]
["","","(3\")","",60,7.75,465]
["","","(4\")","",130,9.7346153849999997,1265.5]
["5160000000-E","ELECT DUCT JA SIZE *****","(3\")","",172,16,2752]
["","","(4\")","",122,17,2074]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",664,5.2632530119999998,3494.8]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",138,6.2,855.6]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2 1 1/2)","",5450,10.75,58587.5]
["","","(2 1-1/2\")","",3330,30.08,100166.39999999999]
["","","(2 15)","",2434,8.8000000000000007,21419.200000000001]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2 15)","",1067,10.3,10990.1]
["5240000000-N","ELEC JB ************","(PC18)","",15,318.85333333300002,4782.8]
["","","(PC30)","",8,515.98749999999995,4127.8999999999996]
["","","(PC36)","",1,992,992]
["5255000000-N","PORTABLE LIGHTING","","",1,40500,40500]
["5265000000-E","GENERIC LIGHTING ITEM (LF)","146 W/G FEEDER CKT THHN/THWN WIRE","IN 2\" RGS CONDUIT",192,72.209999999999994,13864.32]
["","","166 W/G FEEDER CKT THHN/THWN WIRE","IN 2\" RGS CONDUIT",251,59.07,14826.57]
["","","","IN 3\"PVC CONDUT",140,68.77,9627.7999999999993]
["","","","IN3\"RGS CONDUT",60,107.74,6464.4]
["","","28 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",1276,21.33,27217.08]
["","","","IN 1 1/4\" RGS CONDUIT",415,25.78,10698.7]
["","","28 26 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",4766,18.57,88504.62]
["","","286 W/G FEEDER CKT THHN/THWN WIRE","IN 3\" PVC CONDUIT",97,83.9,8138.3]
["","","","IN3\"RGS CONDUT",29,245.39,7116.31]
["","","326 W/G FEEDER CKT THHN/THWN WIRE","IN 3\" PVC CONDUIT",97,89.96,8726.1200000000008]
["","","","IN3\"RGS CONDUT",29,130.9,3796.1]
["","","46 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" RGS CONDUIT",101,49.73,5022.7299999999996]
["","","48 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",6075,17.34,105340.5]
["","","48 26 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",2656,22.04,58538.239999999998]
["","","66 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" RGS CONDUIT",82,49.39,4049.98]
["","","68 W/G FEEDER CKT THHN/THWN WIRE","IN 1 1/4\" PVC80 CONDUIT",5593,19.309999999999999,108000.83]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","DAVIT STYLE LGT STD MH 35' SA 6'","",19,2270,43130]
["","","EQUIP DISCONNECT","",1,698.69,698.69]
["","","INSTALL LED LUMINAIRE","(ROADWAY)",19,1270.9000000000001,24147.1]
["","","","(TUNNEL)",652,1875.9,1223086.8]
["","","LIGHT CONTROL EQUIP ","RA 120/240",1,6850,6850]
["","","LIGHT CONTRL EQUIP TU","(TUNNEL 104)",1,14026,14026]
["","","","(TUNNEL 17)",1,14026,14026]
["","","LIGHT STD JUNCTION BX","",28,594.04999999999995,16633.400000000001]
["","","LIGHTING CONTRL EQUIP ","TU (TUNNEL 15)",1,14026,14026]
["","","PACKAGED DIESEL GENERATOR","SET (FOR TUNNEL 104)",1,116312,116312]
["","","","SET (FOR TUNNEL 15 & 17)",1,152520,152520]
["","","PACKAGED EQUIP ENCLOSURE","(FOR TUNNEL 104 LIGHTING SYS)",1,256564,256564]
["","","PACKAGED EQUIP ENCLOSURE","(FOR TUNNEL 15 & 17 LIGHT SYS)",1,261189,261189]
["","","POST TOP LIGHT STD","",15,2150,32250]
["","","PT LUMINAIRES LED V","",15,2040,30600]
["","","RDW LUMINAIRES LED III","",19,1125,21375]
["","","REM LUMINAIRE (RDWY)","",19,717.22,13627.18]
["","","REM LUMINAIRE (TUNNEL)","",584,161.32,94210.880000000005]
["","","SPARE LED LUMINAIRE ","(TUNNEL)",30,1037.7,31131]
["","","STD FOUND R1S","",15,820,12300]
["5325200000-E","2\" H2O LINE","","",775,30.9,23947.5]
["5325300000-E","3\" H2O LINE","","",330,24,7920]
["5325600000-E","6\" H2O LINE","","",2532,39.629028435999999,100340.7]
["5325800000-E","8\" H2O LINE","","",1262,61.793660856000002,77983.600000000006]
["5326000000-E","10\" H2O LINE","","",5119,70.099999999999994,358841.9]
["5534000000-E","**\" VALVE","(1-1/2\")","",1,700,700]
["","","(3\")","",2,850,1700]
["","","(3/4\")","",4,740,2960]
["5536000000-E","2\" VALVE","","",2,824.2,1648.4]
["5540000000-E","6\" VALVE","","",6,1134.3333333329999,6806]
["5546000000-E","8\" VALVE","","",9,1461.533333333,13153.8]
["5552000000-E","10\" VALVE","","",18,2163.4,38941.199999999997]
["5571600000-E","6\" TAPPING VALVE","","",1,2275,2275]
["5589200000-E","2\" AIR RELEASE VALVE","","",6,4800,28800]
["5643150000-E","1-1/2\" H2O METER","","",1,3800,3800]
["5648000000-N","RELOCATE H2O METER","","",8,1339.3,10714.4]
["5649000000-N","RECONNECT H2O METER","","",3,1339.3,4017.9]
["5666000000-E","FIRE HYDRANT","","",1,4450,4450]
["5672000000-N","RELOCATE FIRE HYDRANT","","",4,2033.9749999999999,8135.9]
["5691100000-E","4\" SANIT GRAVITY SEWER","","",375,18,6750]
["5691300000-E","8\" SANIT GRAVITY SEWER","","",2902,129.80000000000001,376679.6]
["5691500000-E","12\" SANIT GRAV SEWER","","",400,54,21600]
["5709000000-E","**\" FORCE MAIN SEWER","(3\")","",17482,26,454532]
["5768000000-N","SANIT SEWER CLEAN-OUT","","",16,702.625,11242]
["5775000000-E","4' DIA UTILITY MH","","",15,2298.3200000000002,34474.800000000003]
["5776000000-E","5' DIA UTILITY MH","","",3,4532.8999999999996,13598.7]
["5781000000-E","UTILITY MH WALL 4' DIA","","",18.809999999999999,164.80010632599999,3099.89]
["5782000000-E","UTILITY MH WALL 5' DIA","","",20.350000000000001,206,4192.1000000000004]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",5753,10.3,59255.9]
["5816000000-N","ABANDON UTILITY MH","","",12,1030.2,12362.4]
["5835400000-E","6\" ENCASEMENT PIPE","","",370,60.5,22385]
["5835600000-E","12\" ENCASEMENT PIPE","","",378,80.066666667000007,30265.200000000001]
["5835700000-E","16\" ENCASEMENT PIPE","","",1129,85.127989370999998,96109.5]
["5836000000-E","24\" ENCASEMENT PIPE","","",223,139.1,31019.3]
["5871200000-E","3\" TRENCHLESS INSTALL (IN SOIL)","","",425,72.5,30812.5]
["5871210000-E","3\" TRENCHLESS INSTALL (NOT IN SOIL)","","",425,172,73100]
["5871700000-E","12\" TRENCHLESS INSTALL (IN SOIL)","","",189,191.73333333299999,36237.599999999999]
["5871710000-E","12\" TRENCHLESS INSTALL (NOT IN SOIL)","","",189,769.29523809499995,145396.79999999999]
["5871900000-E","16\" TRENCHLESS INSTALL (IN SOIL)","","",447,193.91140939600001,86678.399999999994]
["5871910000-E","16\" TRENCHLESS INSTALL (NOT IN SOIL)","","",447,787.25861297500001,351904.6]
["5882000000-N","GENERIC UTILITY ITEM (EA)","3\" PLUG VALVE","",4,1700,6800]
["","","FORCE MAIN FLUSHING ","CONNECTION",2,10400,20800]
["5888000000-E","GENERIC UTILITY ITEM (LF)","3/4\" PVC H2O PIPE SCH80","",455,8.1999999999999993,3731]
["5912000000-N","GENERIC UTILITY ITEM (LS)","NORTHBOUND SEWER ","PUMP STATION",1,72000,72000]
["","","SOUTHBOUND SEWER ","PUMP STATION",1,124000,124000]
["6000000000-E","TEMP SILT FENCE","","",32150,2.6416345259999998,84928.55]
["6006000000-E","EROS CONTRL STONE CLA","","",3615,35.024896265999999,126615]
["6009000000-E","EROS CONTRL STONE CLB","","",5355,40.603408029999997,217431.25]
["6012000000-E","SEDIMENT CNTRL STONE","","",7905,31.991461100999999,252892.5]
["6015000000-E","TEMP MULCHING","","",151.69999999999999,927.07712590599999,140637.6]
["6018000000-E","SEED FOR TEMP SEEDING","","",6590,2.9821699540000002,19652.5]
["6021000000-E","FERT FOR TEMP SEEDING","","",36.950000000000003,1024.4925575100001,37855]
["6024000000-E","TEMP SLOPE DRNS","","",2350,13.034042553000001,30630]
["6029000000-E","SAFETY FENCE","","",4680,2.4082051280000001,11270.4]
["6030000000-E","SILT EXCAVATION","","",9700,10.177835052000001,98725]
["6036000000-E","MAT FOR EROS CONTROL","","",187600,1.3465884859999999,252620]
["6037000000-E","COIR FIBER MAT","","",2260,6.5752212390000002,14860]
["6038000000-E","PERM SOIL REINF MAT","","",2810,4.4360498220000002,12465.3]
["6042000000-E","1/4\" HARDWARE CLOTH","","",11815,5.5808294539999999,65937.5]
["6045000000-E","**\" TEMP PIPE","(24\")","",425,32.808823529000001,13943.75]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",25,20,500]
["6048000000-E","FLOAT TURBIDITY CURTN","","",60,96.9,5814]
["6069000000-E","STILLING BASINS","","",45,13,585]
["6070000000-N","SPECIAL STILLING BASINS","","",40,663.5,26540]
["6071010000-E","WATTLE","","",1070,5.7927102799999997,6198.2]
["6071012000-E","COIR FIBER WATTLE","","",1700,13.317647059,22640]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1710,15.864152046999999,27127.7]
["6071030000-E","COIR FIBER BAFFLE","","",3020,8.7044701989999993,26287.5]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",15,590.33333333300004,8855]
["6084000000-E","SEEDING AND MULCHING","","",122.4,1767.362745098,216325.2]
["6087000000-E","MOWING","","",88.15,122.66591038,10813]
["6090000000-E","SEED FOR REPAIR SEED","","",1970,4.7741116750000003,9405]
["6093000000-E","FERT FOR REPAIR SEED","","",6.65,1199.646616541,7977.65]
["6096000000-E","SEED FOR SUPP SEEDING","","",3295,8.7811077389999994,28933.75]
["6102000000-E","SODDING","","",2480,6.5,16120]
["6108000000-E","FERTILIZER TOPDRESSING","","",93.55,984.50400855199996,92100.35]
["6111000000-E","IMPERVIOUS DIKE","","",575,40.513043478,23295]
["6114500000-N","SPECIALIZED HAND MOW","","",160,42.34375,6775]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",467,171.17612419700001,79939.25]
["6120000000-E","CLVT DIVERSION CHANL","","",227,15,3405]
["6123000000-E","REFORESTATION","","",1.65,4221.2121212120001,6965]
["6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","SEEDING & MULCHING BLUEGRASS","FESCUE MIX REST AREA LAWN",3,1325,3975]
["6645000000-N","GENERIC PLANT ITEM (EA)","BOULDERS","",30,105,3150]
["","","STEPPING STONE","",5,40,200]
["6650000000-E","MULCH FOR PLANTING","","",145,50,7250]
["6655000000-E","H2O FOR PLANTING","","",20,360,7200]
["6665000000-E","POSTEMERGENT HERBICIDAL TRTMENT","","",1300,0.1,130]
["6670000000-E","PREEMERGENT HERBICIDAL TRTMENT","","",1300,0.35,455]
["6674000000-N","GENERIC PLANT ITEM (LS)","BOULDER H2O FEATURE","",1,51000,51000]
["","","LANDSCAPE PLANTING ","(NBL)",1,12600,12600]
["","","LANDSCAPE PLANTING ","(SBL)",1,64600,64600]
["","","SPECIAL SIDEWALK CLVT","",1,4100,4100]
["6676000000-E","GENERIC PLANT ITEM (SF)","PAVERS","",2130,12,25560]
["","","SEGMENTED RET WALL","",350,75,26250]
["6677000000-E","GENERIC PLANT ITEM(TON)","RIVER STONE","",7,200,1400]
["6680000000-E","GENERIC PLANT ITEM (CY)","12 MTH AGED HARD-","WOOD MULCH",190,50,9500]
["6690000000-E","GENERIC PLANT ITEM (LF)","TREE PROTECTION FENCE","",300,1.3,390]
["","","WORMSTYLE FENCING","",1350,26,35100]
["6890000000-E","CONC STEPS","","",6,720,4320]
["6895000000-E","HANDRAIL ON STEPS","","",28,200,5600]
["6900000000-E","TOPSOIL","","",100,52,5200]
["6905000000-N","PICNIC TABLE TERRZO &STL","","",3,4000,12000]
["6915000000-N","OUTDOOR PARK STOVE","","",2,2550,5100]
["6945000000-E","3/4\"POST YARD HYDRNT","","",3,525,1575]
["6970000000-N","GENERIC REST AREA ITEM (EA)","FLAGPOLE","",3,3350,10050]
["","","FLAGPOLE & SIGN ","LIGHTING",4,2150,8600]
["","","PICNIC SHELTER SINGLE PICNIC","TABLE STONE VENEER BASE",5,25000,125000]
["","","RECYCLING CONTAINER","",10,850,8500]
["","","SITTING BENCH","",7,1750,12250]
["","","WASTE CONTAINER","",10,765,7650]
["","","WHEEL STOPS @ H/C ","PARKING",4,85,340]
["6975000000-N","GENERIC REST AREA ITEM (LS)","(NBL) REST AREA - SOLAR H2O","HEATING SYS",1,20000,20000]
["","","(SBL) REST AREA - SOLAR H2O","HEATING SYS",1,20000,20000]
["","","ELECT INSTALL FOR NBL","REST AREA BLDG",1,60100,60100]
["","","ELECT INSTALL FOR SBL","REST AREA BLDG",1,90500,90500]
["","","","(SBL) STORAGE BLDG",1,5650,5650]
["","","GENERL CONST OF (SBL)","REST AREA BLDG",1,520000,520000]
["","","","STORAGE BLDG",1,37750,37750]
["","","GENERAL RENO OF (NBL)","REST AREA BLDG",1,410000,410000]
["","","LANDSCAPE GRAD (NBL)","",1,1700,1700]
["","","LANDSCAPE GRAD (SBL)","",1,12650,12650]
["","","MECHANICAL INSTALLATION FOR","(NBL) REST AREA BLDG",1,30600,30600]
["","","","(SBL) REST AREA BLDG",1,48500,48500]
["","","PLUMB INSTALL OF (NBL)","REST AREA BLDG",1,143300,143300]
["","","PLUMB INSTALL OF (SBL)","REST AREA BLDG",1,192900,192900]
["","","SITE DEMOLITION (NBL)","",1,15000,15000]
["","","SPECIAL REST AREA ","SIGNAGE",1,35500,35500]
["","","STORMH2O DRNG SYS ","(NBL)",1,16600,16600]
["","","STORMH2O DRNG SYS ","(SBL)",1,24500,24500]
["6980000000-E","GENERIC REST AREA ITEM (LF)","LANDSCAPE METAL EDGING","",1790,4.5,8055]
["","","STONE SEATWALL","",470,275,129250]
["7060000000-E","SIGNAL CABLE","","",11485,2.1252416200000002,24408.400000000001]
["7120000000-E","VEHICLE SIGNAL HD (12\" 3 SECT)","","",70,781.35285714300005,54694.7]
["7132000000-E","VEHICLE SIGNAL HD (12\" 4 SECT)","","",23,886.29130434800004,20384.7]
["7144000000-E","VEHICLE SIGNAL HD (12\" 5 SECT)","","",8,1133.2,9065.6]
["7204000000-N","LOUVER","","",2,206,412]
["7264000000-E","MESSENGER CABLE (3/8\")","","",2275,2.5054945050000001,5700]
["7279000000-E","TRACER WIRE","","",4075,1,4075]
["7300000000-E","UNPAVED TRENCH (*******)","(1 2\")","",4710,5.2,24492]
["","","(1 5\")","",250,10.3,2575]
["","","(2 2\")","",970,6.3,6111]
["7301000000-E","DIRECT DRILL (***********)","(1 2\")","",1675,13.9,23282.5]
["","","(3 2\")","",1095,22.4,24528]
["7324000000-N","JUNCTION BOX (STD SIZE)","","",59,278.36440678000002,16423.5]
["7348000000-N","JUNCTION BOX (OVER-SIZED HVY-DUTY)","","",21,386.3,8112.3]
["7360000000-N","WOOD POLE","","",12,824.2,9890.4]
["7372000000-N","GUY ASSEM","","",25,283.3,7082.5]
["7408000000-E","1\" RISER W/ WEATHERHEAD","","",3,309.10000000000002,927.3]
["7420000000-E","2\" RISER W/ WEATHERHEAD","","",7,386.3,2704.1]
["7432000000-E","2\" RISER W/ TUBING","","",1,412.1,412.1]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",8025,7.048311526,56562.7]
["7456000000-E","LEAD-IN CABLE(********)","(14-12)","",17808,1.3,23150.400000000001]
["","","(14-2)","",3870,1.58,6114.6]
["7481000000-N","SITE SURVEY","","",4,257.60000000000002,1030.4000000000001]
["7481240000-N","CAMERA W/O INT LOOP EMUL PORCESS","","",15,1493.8,22407]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",4,9271.7999999999993,37087.199999999997]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",4350,2,8700]
["7541000000-N","MOD SPLICE ENCLOSURE","","",1,721.1,721.1]
["7552000000-N","INTERCONNECT CENTER","","",5,1442.3,7211.5]
["7564000000-N","FIBER-OPTIC TRANS DROP/REP","","",4,1390.8,5563.2]
["7566000000-N","DELINEATOR MKR","","",15,77.3,1159.5]
["7575142000-N","900MHZ RADIO","","",5,3605.7,18028.5]
["7575142060-N","MOD RADIO INSTALL","","",1,721.1,721.1]
["7575160000-E","REM EXT COMM CABLE","","",4500,0.8,3600]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",4,7691,30764]
["7588000000-N","SGNL MAST ARM W/ METAL POLE","","",15,11795.8,176937]
["7590000000-N","DBL MAST ARM W/ METAL POLE","","",2,13701.7,27403.4]
["7613000000-N","SOIL TEST","","",21,930.59047619,19542.400000000001]
["7614100000-E","DRILLED PIER FOUND","","",117,546.52564102600002,63943.5]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",17,103,1751]
["7636000000-N","SIGN FOR SIGNALS","","",18,309.10000000000002,5563.8]
["7684000000-N","SIGNAL CABINET FOUND","","",6,877.66666666699996,5266]
["7756000000-N","CONTLR W/ CBNT 2070L BASE MTD","","",6,11293.916666667001,67763.5]
["7780000000-N","DETECTOR CARD ( 2070L)","","",47,103.29787234,4855]
["7901000000-N","CABINET BASE EXTENDER","","",6,361.75,2170.5]
["7948000000-N","TRAFFIC SIGNAL REML","","",1,1802.9,1802.9]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","PROTECTIVE HUNTER GREEN COAT FOR ","DUAL MAST ARM ASSEM",2,1596.8,3193.6]
["","","","SINGLE MAST ARM ASSEM-BLY",15,1313.5,19702.5]
["","","STRAIN POLE ASSEM W/","PROTECTIVE COATING",4,1044,4176]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","BACK PULL FIBER OPTIC ","CABLE",500,3.1,1550]
["8017000000-N","CM&R TEMP ACCESS *****","(10+5800-L-)","",1,66400,66400]
["","","(27+1172-L-)","",1,175000,175000]
["8021000000-N","REMV EXIST STR **********","(27+1172-L-)","",1,570500,570500]
["8035000000-N","REMV EXIST STR **********","(10+5800-L-)","",1,12000,12000]
["","","(12+8100-L2-)","",1,10000,10000]
["","","(15+1600-L-)","",1,66000,66000]
["","","(42+6093-L-)","",1,22000,22000]
["8056000000-N","REMV EXIST STR **********","(15-8400-L-)","",1,35000,35000]
["8070000000-E","FOUND EXCAVATION","","",1040,34.098557692,35462.5]
["8084000000-N","FND EXCAV EB** STA*****","(ABUT 1 18+8173-RR-)","",1,3000,3000]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(5'-0\")","",156,425,66300]
["","","(5'-6\")","",366,500,183000]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",24,1500,36000]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",209.41,1415,296315.15000000002]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(5'-0\")","",30,1550,46500]
["","","(5'-6\")","",51,1900,96900]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",93,806.45161290299995,75000]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",60,1880,112800]
["8111000000-E","PERM STL CASING FOR ** PIER","(5'-6\")","",24,500,12000]
["8111600000-E","PERM STL CASING FOR 4' PIER","","",64.95,40,2598]
["8112730000-N","PDA TESTING","","",3,2366.6666666669998,7100]
["8113000000-N","SID INSPECTIONS","","",22,795.45454545500002,17500]
["8114000000-N","SPT TESTING","","",28,767.85714285699999,21500]
["8115000000-N","CSL TESTING","","",12,1745.8333333329999,20950]
["8121000000-N","UNCL STR EXCAV STA ****","(10+5800-L-)","",1,10000,10000]
["","","(12+8100-L2-)","",1,50000,50000]
["","","(27+1172-L-)","",1,40250,40250]
["8126000000-N","CULV EXCAV @ ************","(11+4187-Y4-)","",1,6320,6320]
["","","(15+1600-L-)","",1,15500,15500]
["","","(15-8400-L-)","",1,45000,45000]
["8133000000-E","FND CONDIT MAT BOX CULV","","",482,39.624481328000002,19099]
["8147000000-E","REINF CONC DECK SLAB","","",48175,22.537571976999999,1085747.53]
["8161000000-E","GROOVING BRG FLOORS","","",41432,0.26743821200000001,11080.5]
["8175000000-E","CL AA CONC (BRIDGE)","","",491.4,475,233415]
["8182000000-E","CL A CONC (BRIDGE)","","",1045.8,797.86001147399998,834402]
["8196000000-E","CL A CONC (CULV)","","",653.9,643.71845847999998,420927.5]
["8210000000-N","BRG APPR SLAB ***********","(12+1950)","",1,74600,74600]
["","","(12+7150-L-)","",1,25000,25000]
["","","(12+8100-L2-)","",1,12000,12000]
["","","(27+1172-L-)","",1,60000,60000]
["8217000000-E","REINF STEEL (BRIDGE)","","",430338,0.99917529900000002,429983.1]
["8238000000-E","SPIRAL COL REINF STL BRG","","",46201,1.635176728,75546.8]
["8245000000-E","REINF STEEL (CLVT)","","",85878,1.0441131610000001,89666.35]
["8280000000-E","STRUCTURAL STEEL","","",2574000,1.572416472,4047400]
["8294000000-N","PAINTING STR STL","","",1,93000,93000]
["8364000000-E","HP12X53 PILES","","",670,59.626865672000001,39950]
["8365000000-E","HP12X53 GALV PILES","","",1820,53.75,97825]
["8384000000-E","HP14X73 PILES","","",4230,45,190350]
["8391000000-N","STEEL PILE POINTS","","",99,101.515151515,10050]
["8453000000-E","METHD B DAMPPROOFING","","",217.8,35,7623]
["8475000000-E","TWO BAR METAL RAIL","","",707.38,106.679578162,75463]
["8482000000-E","THREE BAR METAL RAIL","","",376.8,160,60288]
["8505000000-E","VERT CONC BARR RAIL","","",140.25,125,17531.25]
["8510000000-E","CONC MEDIAN BARR","","",360.17,85,30614.45]
["8517000000-E","1'-**\"X****\"CONC PARAPET","(1'-0\" X 2'-0\")","",558,319,178002]
["","","(1'-2\" X 2'-11 1/2\" )","",120,115,13800]
["","","(1'-2\" x 2'-6\")","",637.67999999999995,90,57391.199999999997]
["8531000000-E","4\" SLOPE PROTECTION","","",137,150,20550]
["8590000000-E","RIP RAP CL **","(I)","",505,45.841584158000003,23150]
["8608000000-E","RIP RAP II (2'-0\")","","",1154,41.291161178999999,47650]
["8622000000-E","GEOTEXTILE FOR DRNG","","",1710,4.5251461989999999,7738]
["8650000000-N","POT BEARINGS","","",1,50000,50000]
["8654000000-N","DISC BEARINGS","","",1,62000,62000]
["8657000000-N","ELASTOMERIC BEARINGS","","",4,6925,27700]
["8664000000-E","SHOTCRETE REPAIRS","","",1985.5,875,1737312.5]
["8692000000-N","FOAM JOINT SEALS","","",1,11600,11600]
["8706000000-N","EXPANSION JOINT SEALS","","",1,150000,150000]
["8741000000-N","STR DRN SYS ************","(18+8173-RR-)","",1,200000,200000]
["8755000000-E","3'-0\"X 1'-6\"PRESTR SLABS","","",405,140,56700]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",1230,166.95121951199999,205350]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",4114,52,213928]
["","","(2)","",3694,52,192088]
["8802010000-E","SOIL NAIL RET WALLS","","",9959,71.628476754999994,713348]
["8802014000-E","SOLDIER PILE RET WALLS","","",3164,167.53097345099999,530068]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",3,1033.3333333329999,3100]
["8802015110-N","SOIL NAIL PROOF TESTS","","",16,512.5,8200]
["8847000000-E","GENERIC RET WALL ITEM (SF)","ANCHORED RET WALLS","",800,150,120000]
["","","ARCH CONC SURF TRTMT","",675,25,16875]
["8860000000-N","GENERIC STR ITEM (LS)","APPLIC OF BRG COATING","",1,2500,2500]
["","","CONDUIT IN PARAPET @","STA18+8173-RR-",1,2000,2000]
["","","ELECTRL CONDUIT SYS","AT12+9050",1,19000,19000]
["","","REHAB OF EXISTING STR","",1,30000,30000]
["","","REML OF EXIST STR 42","",1,5000,5000]
["","","SELF-LUBRICATING EXP","BEARING ASSEM",1,110000,110000]
["","","TEMP RAILRD SHORNG","",1,350000,350000]
["","","UTILITY HANGER SYS","",1,174000,174000]
["8867000000-E","GENERIC STR ITEM (LF)","METAL HANDRAIL","W/ FENCING",635,350,222250]
["",""," T101 RAIL","",84.67,325,27517.75]
["8874000000-E","GENERIC STR ITEM (TON)","FOUND CONDITIONING","MATL FOR CONC SLABS",62,54.5,3379]
["8881000000-E","GENERIC STR ITEM (CY)","CONCRETE SLABS","",17,599.5,10191.5]
["8892000000-E","GENERIC STR ITEM (SF)","ARCH CONC SURF TRTMT","",289,30,8670]
["8893000000-E","GENERIC STR ITEM (SY)","EPOXY COATING","",21200,52,1102400]
["","","MEMBRANE LAYER H2O-","PROOF FOR DECK",682,120,81840]
["","","1\" ASPHALT PLANKING","PROTECTIVE CRS FOR DECK",682,60,40920]
["","","2-PART MEMBRANE H2O-","PROOFING SYS",35.200000000000003,140,4928]
["8897000000-N","GENERIC STR ITEM (EA)","DRNG PIPE CLEANOUT","",3,20000,60000]