{"text_format":"1","workbook":"xlsx","n_sheets":17,"sheets":["STATEWIDE - SUMMARY","ITEMS - STATEWIDE","BExRepositorySheet","ITEMS - DIV 01","ITEMS - DIV 02","ITEMS - DIV 03","ITEMS - DIV 04","ITEMS - DIV 05","ITEMS - DIV 06","ITEMS - DIV 07","ITEMS - DIV 08","ITEMS - DIV 09","ITEMS - DIV 10","ITEMS - DIV 11","ITEMS - DIV 12","ITEMS - DIV 13","ITEMS - DIV 14"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"STATEWIDE - SUMMARY","index":0,"n_rows":863,"n_cols":24,"rows_kept":863,"cut":false,"hidden":false,"merged":[[0,0,0,23]]}
["NORTH CAROLINA DEPARTMENT OF TRANSPORATION  -  2018 BID AVERAGES"]
["LET DATE","RPN","TIP","CONTR ","PROJECT","CAT ","COUNTY","VENDOR NAME","$TOTAL","JOB","FED WRK ","PROJ LGTH (MI/ KM)"," LN / CVT FILL DPTH","CVT CODE OVR/UND RET WLL X-SECT","BOX LTH /WLL HT","BOX SPAN","BRG SUP STR","SUB STR"," SPAN","BRG WTH","BRG LTH","AREA","DIV","LOC"]
["1/16/2018","1","B-4637","C204010","C204010-EC","1","SAMPSON","CIVIL WORKS CONTRACTING LLC",81520,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204010-RW","1","SAMPSON","CIVIL WORKS CONTRACTING LLC",488126,"RW1","I000",0.16400000000000001,2,"B810",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204010-SI","1","SAMPSON","CIVIL WORKS CONTRACTING LLC",9264,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204010-ST","1","SAMPSON","CIVIL WORKS CONTRACTING LLC",212983.3,"BR01","X080",1.2E-2,null,"15",null,30,"722","A",1,27.833300000000001,62.25,"COAST","03","12+68.00 -L-"]
["","","","","","2","SAMPSON","CIVIL WORKS CONTRACTING LLC",208873.3,"BR02","X080",1.2E-2,null,"15",null,30,"721","A",1,27.833300000000001,62.25,"COAST","03","15+56.00 -L-"]
["","","","","","3","SAMPSON","CIVIL WORKS CONTRACTING LLC",395101.6,"BR03","X080",0.02,null,"15",null,30,"722","A",2,27.833300000000001,107.375,"COAST","03","19+45.50 -L-"]
["","","","","C204010-TC","1","SAMPSON","CIVIL WORKS CONTRACTING LLC",9112,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",1404980.2,"","",0.20799999999999999," ","",null," ","",""," "," "," ","","",""]
["","2","W-5203Y","C204094","C204094C-RW","1","BRUNSWICK","S T WOOTEN CORPORATION",1667858.69,"RW1","I000",7.46,2,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",1667858.69,"","",7.46," ","",null,null,"","",null,null,null,"","",""]
["","","","C204094","C204094A-RW","1","BRUNSWICK","S T WOOTEN CORPORATION",2912991.17,"RW1","",14.116,4,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204094B-RW","1","BRUNSWICK","S T WOOTEN CORPORATION",3865514.05,"RW1","",35.505000000000003,2,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",6778505.2199999997,"","",49.621000000000002," ","",null,null,"","",null,null,null,"","",""]
["","3","U-3334B","C204060","C204060-EC","1","JOHNSTON","BRANCH CIVIL INC",224443.89,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204060-RW","1","JOHNSTON","BRANCH CIVIL INC",11398116.810000001,"RW1","",2.1240000000000001,4,"G401",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204060-SG","1","JOHNSTON","BRANCH CIVIL INC",788304.65,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204060-SI","1","JOHNSTON","BRANCH CIVIL INC",85118.95,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204060-ST","1","JOHNSTON","BRANCH CIVIL INC",330787,"CV01","",5.4999999999999997E-3,6.36,"C003",191,6,"","",null,null,null,"PDMT","04","120+01.00 -L-"]
["","","","","","2","JOHNSTON","BRANCH CIVIL INC",152122.5,"CV02","",null,2.5499999999999998,"C002",74,7,"","",null,null,null,"PDMT","04","11+51.56 -DRW1-"]
["","","","","C204060-TC","1","JOHNSTON","BRANCH CIVIL INC",254191.2,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",13233085,"","",2.1295000000000002," ",""," "," ","","",null,null,null,"","",""]
["","5","B-4943","C203987","C203987-EC","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",40642.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203987-RW","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",657535,"RW1","I000",0.16300000000000001,2,"B801",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203987-SI","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",5487,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203987-ST","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",754687.5,"BR01","X080",1.7000000000000001E-2,null,"15",null,36,"729","Q",1,33.833300000000001,87.25,"PDMT","05","14+67.00 -L-"]
["","","","","C203987-TC","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",17123,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",1475475,"","",0.18," ","",null," ","",""," "," "," ","","",""]
["","6","W-5522","C203908","C203908-EC","1","WAKE","CROWDER CONSTRUCTION COMPANY",110685.95,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203908-LI","1","WAKE","CROWDER CONSTRUCTION COMPANY",134100.12,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203908-RW","1","WAKE","CROWDER CONSTRUCTION COMPANY",1105393.02,"RW1","",0.159,4,"M720",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203908-SI","1","WAKE","CROWDER CONSTRUCTION COMPANY",20549.22,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C203908-ST","1","WAKE","CROWDER CONSTRUCTION COMPANY",2862345.65,"CV01","X028",5.0000000000000001E-3,4.53,"13",120,25,"","",null,null,null,"PDMT","05","15+58.58 -L-"]
["","","","","C203908-TC","1","WAKE","CROWDER CONSTRUCTION COMPANY",113851.58,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",4346925.54,"","",0.16400000000000001," ",""," "," ","","",null,null,null,"","",""]
["","7","","C204127","C204127A-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",2425796.4700000002,"RW1","",6,5,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204127B-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",4442062.26,"RW1","",9.5299999999999994,5,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",6867858.7300000004,"","",15.53," ","",null,null,"","",null,null,null,"","",""]
["","8","","C204121","C204121A-RW","1","WAKE","CAROLINA SUNROCK LLC",991423.07,"RW1","",2.19,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204121B-RW","1","WAKE","CAROLINA SUNROCK LLC",4668376.1100000003,"RW1","",27.21,5,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",5659799.1799999997,"","",29.4," ","",null,null,"","",null,null,null,"","",""]
["","9","I-5793","C204053","C204053-RW","1","DAVIDSON","TRIANGLE GRADING & PAVING INC",14166111.52,"RW1","I000",6.7690000000000001,6,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204053-ST","1","DAVIDSON","TRIANGLE GRADING & PAVING INC",338847,"BR01","X231",6.7000000000000004E-2,null,"11",null,58.833300000000001,"582","I",3,56,318.14690000000002,"PDMT","09","BRIDGE NO. 474"]
["","","","","","2","DAVIDSON","TRIANGLE GRADING & PAVING INC",108475.4,"BR02","X081",2.5999999999999999E-2,null,"15",null,58.833300000000001,"736","I",3,56,135.72399999999999,"PDMT","09","BRIDGE NO. 475"]
["","","","","","3","DAVIDSON","TRIANGLE GRADING & PAVING INC",117952,"BR03","X231",2.4E-2,null,"11",null,58.833300000000001,"333","I",3,56,128.65100000000001,"PDMT","09","BRIDGE NO. 478"]
["","","","","","4","DAVIDSON","TRIANGLE GRADING & PAVING INC",283532,"BR04","X231",3.2000000000000001E-2,null,"11",null,58.833300000000001,"557","I",3,56,168.75,"PDMT","09","BRIDGE NO. 479"]
["","","","","","5","DAVIDSON","TRIANGLE GRADING & PAVING INC",282782,"BR05","X231",3.2000000000000001E-2,null,"11",null,58.833300000000001,"557","I",3,56,166.5,"PDMT","09","BRIDGE NO. 480"]
["","","","","","6","DAVIDSON","TRIANGLE GRADING & PAVING INC",681995,"BR06","X231",5.3999999999999999E-2,null,"11",null,58.833300000000001,"587","I",3,56,285,"PDMT","09","BRIDGE NO. 485"]
["","","","","","7","DAVIDSON","TRIANGLE GRADING & PAVING INC",397711,"BR07","X231",5.0999999999999997E-2,null,"11",null,74.833299999999994,"548","I",4,72,268,"PDMT","09","BRIDGE NO. 489"]
["","","","","","8","DAVIDSON","TRIANGLE GRADING & PAVING INC",282340,"BR08","X231",2.9000000000000001E-2,null,"11",null,58.833300000000001,"300","I",3,56,151.1302,"PDMT","09","BRIDGE NO. 493"]
["","","","","","9","DAVIDSON","TRIANGLE GRADING & PAVING INC",261495,"BR09","X231",3.2000000000000001E-2,null,"11",null,58.833300000000001,"300","I",3,56,169.3802,"PDMT","09","BRIDGE NO. 494"]
["","","","","","10","DAVIDSON","TRIANGLE GRADING & PAVING INC",107413,"BR10","X181",2.3E-2,null,"12",null,58.833300000000001,"736","I",3,56,119.474,"PDMT","09","BRIDGE NO. 495"]
["","","","","","11","DAVIDSON","TRIANGLE GRADING & PAVING INC",143156,"BR11","X181",2.5999999999999999E-2,null,"12",null,74.833299999999994,"736","I",3,72,137,"PDMT","09","BRIDGE NO. 496"]
["","","","","","","","Result",17171809.920000002,"","",7.165," ","",null," ","",""," "," "," ","","",""]
["","10","R-2707F","C203845","C203845-EC","1","CLEVELAND","THE LANE CONSTRUCTION CORPORATION",288940,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203845-RW","1","CLEVELAND","THE LANE CONSTRUCTION CORPORATION",15041978.699999999,"RW1","",5.66,4,"P501",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203845-SG","1","CLEVELAND","THE LANE CONSTRUCTION CORPORATION",48632.5,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203845-SI","1","CLEVELAND","THE LANE CONSTRUCTION CORPORATION",559865.93999999994,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C203845-TC","1","CLEVELAND","THE LANE CONSTRUCTION CORPORATION",117525.1,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",16056942.24,"","",5.66," ","",null,null,"","",null,null,null,"","",""]
["","11","B-4848","C204011","C204011-EC","1","YANCEY","DANE CONSTRUCTION INC",93275,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204011-RW","1","YANCEY","DANE CONSTRUCTION INC",538834.75,"RW1","",0.158,2,"C000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204011-SI","1","YANCEY","DANE CONSTRUCTION INC",11370.14,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204011-ST","1","YANCEY","DANE CONSTRUCTION INC",348726.25,"CV01","X028",8.9999999999999993E-3,2.09,"C002",79.25,13,"","",null,null,null,"V MTN","13","13+07.00 -L-"]
["","","","","C204011-TC","1","YANCEY","DANE CONSTRUCTION INC",36767.75,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1028973.89,"","",0.16700000000000001," ",""," "," ","","",null,null,null,"","",""]
["","12","B-5864","C204061","C204061-EC","1","YANCEY","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",58445.3,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204061-RW","1","YANCEY","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",604795.53,"RW1","",0.13900000000000001,2,"B812",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204061-SI","1","YANCEY","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",10224,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204061-ST","1","YANCEY","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",509909.5,"BR01","X081",0.01,null,"15",null,42,"721","A",1,38.5,52.25,"V MTN","13","14+21.00 -L-"]
["","","","","C204061-TC","1","YANCEY","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",51674.75,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1235049.08,"","",0.14899999999999999," ","",null," ","",""," "," "," ","","",""]
["","13","I-5888A","C204054","C204054-RW","1","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",8682191.1199999992,"RW1","I000",6.74,4,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204054-ST","1","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",474516.23,"BR01","X231",3.4000000000000002E-2,null,"11",null,90.75,"333","I",3,86.5,178,"MTN","13","BRIDGE NO. 24"]
["","","","","","2","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",322775.28999999998,"BR02","X231",0.03,null,"11",null,73.416700000000006,"333","I",3,68,160,"MTN","13","BRIDGE NO. 71"]
["","","","","","3","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",254594.08,"BR03","X231",3.4000000000000002E-2,null,"11",null,42,"336","I",3,40,177,"MTN","13","BRIDGE NO. 156"]
["","","","","","4","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",255955.64,"BR04","X231",3.4000000000000002E-2,null,"11",null,42,"336","I",3,40,178.41669999999999,"MTN","13","BRIDGE NO. 164"]
["","","","","","5","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",200495.81,"BR05","X231",2.5000000000000001E-2,null,"11",null,42,"333","I",3,40,132.5,"MTN","13","BRIDGE NO. 210"]
["","","","","","6","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",200128.09,"BR06","X231",2.8000000000000001E-2,null,"11",null,42,"333","I",3,40,145.5,"MTN","13","BRIDGE NO. 215"]
["","","","","","","","Result",10390656.26,"","",6.9249999999999998," ","",null," ","",""," "," "," ","","",""]
["","14","I-5889A","C204055","C204055-RW","1","BUNCOMBE","GLF CONSTRUCTION CORPORATION",976649,"RW1","I000",4,4,"M720",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204055-ST","1","BUNCOMBE","GLF CONSTRUCTION CORPORATION",72636,"BR01","X031",3.5000000000000003E-2,null,"15",null,45.583300000000001,"","I",3,40,182,"MTN","13","BRIDGE  334"]
["","","","","","2","BUNCOMBE","GLF CONSTRUCTION CORPORATION",89953,"BR02","X031",3.3000000000000002E-2,null,"15",null,45.583300000000001,"","I",3,40,171.5,"MTN","13","BRIDGE 339"]
["","","","","","3","BUNCOMBE","GLF CONSTRUCTION CORPORATION",248881,"BR03","X431",6.7000000000000004E-2,null,"16",null,45.25,"","I",5,40,355,"MTN","13","BRIDGE 344"]
["","","","","","4","BUNCOMBE","GLF CONSTRUCTION CORPORATION",216217,"BR04","X431",6.7000000000000004E-2,null,"16",null,45.25,"","I",5,40,355,"MTN","13","BRIDGE 347"]
["","","","","","5","BUNCOMBE","GLF CONSTRUCTION CORPORATION",89700,"BR05","X031",0.109,null,"15",null,33.25,"","I",8,28,576,"MTN","13","BRIDGE 352"]
["","","","","","6","BUNCOMBE","GLF CONSTRUCTION CORPORATION",138540,"BR06","X031",0.109,null,"15",null,33.25,"","I",8,28,576,"MTN","13","BRIDGE 356"]
["","","","","","7","BUNCOMBE","GLF CONSTRUCTION CORPORATION",1034702.5,"BR07","X231",2.3E-2,null,"11",null,40,"","I",3,35,121,"MTN","13","BRIDGE 358"]
["","","","","","8","BUNCOMBE","GLF CONSTRUCTION CORPORATION",1055582.5,"BR08","X231",2.3E-2,null,"11",null,40,"","I",3,35,121,"MTN","13","BRIDGE 366"]
["","","","","","9","BUNCOMBE","GLF CONSTRUCTION CORPORATION",745468.65,"BR09","X231",2.5999999999999999E-2,null,"11",null,40,"","I",3,35,135,"MTN","13","BRIDGE 369"]
["","","","","","10","BUNCOMBE","GLF CONSTRUCTION CORPORATION",756970.65,"BR10","X231",2.5999999999999999E-2,null,"11",null,40,"","I",3,35,135,"MTN","13","BRIDGE 374"]
["","","","","","11","BUNCOMBE","GLF CONSTRUCTION CORPORATION",1554228.75,"BR11","X431",4.8000000000000001E-2,null,"16",null,33.25,"","I",3,28,252,"MTN","13","BRIDGE 377"]
["","","","","","12","BUNCOMBE","GLF CONSTRUCTION CORPORATION",1692979.75,"BR12","X431",4.8000000000000001E-2,null,"16",null,33.25,"","I",3,28,252,"MTN","13","BRIDGE 378"]
["","","","","","","","Result",8672508.8000000007,"","",4.6139999999999999," ","",null," ","",""," "," "," ","","",""]
["","15","I-5891A","C204056","C204056-RW","1","BURKE","MAYMEAD INC",35993795.619999997,"RW1","I000",26,4,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",35993795.619999997,"","",26," ","",null,null,"","",null,null,null,"","",""]
["","16","","C204113","C204113-RW","1","WATAUGA","BLYTHE DEVELOPMENT CO",2563061,"RW1","",0.16300000000000001,2,"M720",null,null,"","",null,null,null,"V MTN","11",""]
["","","","","","","","Result",2563061,"","",0.16300000000000001," ","",null,null,"","",null,null,null,"","",""]
["","17","","C204114","C204114-RW","1","CALDWELL","JAMES R VANNOY & SONS CONSTRUCTION COMPA",4046406.68,"RW1","",0.38900000000000001,2,"M720",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",4046406.68,"","",0.38900000000000001," ","",null,null,"","",null,null,null,"","",""]
["1/30/2018","1","P-5705BA","C204156","C204156-RW","1","MECKLENBURG","BLYTHE CONSTRUCTION INC",3393690,"RW1","Y108",null,null,"M720",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",3393690,"","",null,null,"",null,null,"","",null,null,null,"","",""]
["2/20/2018","1","","C204135","C204135A-RW","1","BRUNSWICK","HIGHLAND PAVING CO LLC",423321.54,"RW1","",0.93300000000000005,4,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204135B-RW","1","NEW HANOVER","HIGHLAND PAVING CO LLC",4113744.14,"RW1","",6.9779999999999998,4,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204135C-RW","1","NEW HANOVER","HIGHLAND PAVING CO LLC",3207901.05,"RW1","",19.353000000000002,2,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204135D-RW","1","NEW HANOVER","HIGHLAND PAVING CO LLC",450956,"RW1","",4.9749999999999996,2,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",8195922.7300000004,"","",32.238999999999997," ","",null,null,"","",null,null,null,"","",""]
["","2","","C204119","C204119-ST","1","NEW HANOVER","PCL CIVIL CONSTRUCTORS INC",12146488.199999999,"BR01","X071",0.57499999999999996,null,"15",null,61.5,"0","J",32,56,3033.9167000000002,"COAST","03",""]
["","","","","C204119-TC","1","NEW HANOVER","PCL CIVIL CONSTRUCTORS INC",853503.08,"RW1","",null,4,"M720",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",12999991.279999999,"","",0.57499999999999996," ","",null," ","",""," "," "," ","","",""]
["","3","I-5506","C204069","C204069-EC","1","WAKE","FLATIRON CONSTRUCTORS INC",630491.05000000005,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204069-LI","1","WAKE","FLATIRON CONSTRUCTORS INC",604818.25,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204069-RW","1","WAKE","FLATIRON CONSTRUCTORS INC",12353797.039999999,"RW1","I000",0.79300000000000004,4,"64",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204069-SG","1","WAKE","FLATIRON CONSTRUCTORS INC",934897,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204069-SI","1","WAKE","FLATIRON CONSTRUCTORS INC",568441.98,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204069-ST","1","WAKE","FLATIRON CONSTRUCTORS INC",148123.25,"CV01","X928",6.0000000000000001E-3,8.9169999999999998,"C203",19,9,"","",null,null,null,"PDMT","05","(67+46.44-Y-)"]
["","","","","","2","WAKE","FLATIRON CONSTRUCTORS INC",4796293.3499999996,"BR01","X231",5.5E-2,null,"11",null,103.08329999999999,"564","I",2,95,291.5,"PDMT","05","(50+61.09-L-)"]
["","","","","C204069-TC","1","WAKE","FLATIRON CONSTRUCTORS INC",1100634.6599999999,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204069-UT","2","WAKE","FLATIRON CONSTRUCTORS INC",408150,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",21545646.579999998,"","",0.85399999999999998," ",""," "," ","",""," "," "," ","","",""]
["","4","U-5925","C204015","C204015-RW","1","ROBESON","BMCO CONSTRUCTION, INC.",4959946.82,"RW1","I000",0.90800000000000003,2,"M720",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","2","ROBESON","BMCO CONSTRUCTION, INC.",15000,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","3","ROBESON","BMCO CONSTRUCTION, INC.",15000,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","","","Result",4989946.82,"","",0.90800000000000003," ","",null,null,"","",null,null,null,"","",""]
["","5","R-5749","C204115","C204115-RW","1","COLUMBUS","BMCO CONSTRUCTION, INC.",8389965.1799999997,"RW1","I000",1.196,4,"I602",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204115-ST","1","COLUMBUS","BMCO CONSTRUCTION, INC.",13250,"CV01","Y007",null,null,"C202",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","2","COLUMBUS","BMCO CONSTRUCTION, INC.",995462.8,"BR01","X281",null,null,"11",null,39.25,"864","I",2,36,218.33330000000001,"COAST","06","(30+02.30-Y-)"]
["","","","","","","","Result",9398677.9800000004,"","",1.196," ","",null," ","",""," "," "," ","","",""]
["","6","B-5370","C204063","C204063-EC","1","UNION","BOGGS PAVING, INC.",53046.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204063-RW","1","UNION","BOGGS PAVING, INC.",244415,"RW1","I000",5.0999999999999997E-2,2,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204063-SI","1","UNION","BOGGS PAVING, INC.",6348,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204063-ST","1","UNION","BOGGS PAVING, INC.",195129.54,"CV01","Y007",6.0000000000000001E-3,3.6,"C003",43.5,10,"","",null,null,null,"PDMT","10","18+16.00 -L-"]
["","","","","C204063-TC","1","UNION","BOGGS PAVING, INC.",13007,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",511946.04,"","",5.7000000000000002E-2," ",""," "," ","","",null,null,null,"","",""]
["","7","B-5371","C204064","C204064-EC","1","UNION","SLOAN CONSTRUCTION A DIVISION OF REEVES",152497.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204064-RW","1","UNION","SLOAN CONSTRUCTION A DIVISION OF REEVES",1168010,"RW1","I000",0.34100000000000003,2,"B801",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204064-SI","1","UNION","SLOAN CONSTRUCTION A DIVISION OF REEVES",19445.07,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204064-ST","1","UNION","SLOAN CONSTRUCTION A DIVISION OF REEVES",833479.85,"BR01","X081",2.8000000000000001E-2,null,"15",null,43.25,"854","Q",2,40,150,"PDMT","10","23+20.00 -L-"]
["","","","","C204064-TC","1","UNION","SLOAN CONSTRUCTION A DIVISION OF REEVES",26537.16,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",2199969.58,"","",0.36899999999999999," ","",null," ","",""," "," "," ","","",""]
["","8","B-5373","C204065","C204065-EC","1","STANLY","SMITH-ROWE, LLC",16521.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204065-RW","1","STANLY","SMITH-ROWE, LLC",203789.4,"RW1","",7.1999999999999995E-2,2,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204065-SI","1","STANLY","SMITH-ROWE, LLC",6700.3,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204065-ST","1","STANLY","SMITH-ROWE, LLC",384735.89,"BR01","X080",1.4E-2,null,"15",null,33,"722","A",1,29.5,72.604200000000006,"PDMT","10","13+70.00 -L-"]
["","","","","C204065-TC","1","STANLY","SMITH-ROWE, LLC",7263,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",619010.09,"","",8.5999999999999993E-2," ","",null," ","",""," "," "," ","","",""]
["","9","B-5374","C204066","C204066-EC","1","UNION","BOGGS PAVING, INC.",54474.11,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204066-RW","1","UNION","BOGGS PAVING, INC.",321442.36,"RW1","I000",0.16700000000000001,2,"C003",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204066-ST","1","UNION","BOGGS PAVING, INC.",244753.5,"CV01","Y007",7.0000000000000001E-3,3.77,"C003",43.92,11,"","",null,null,null,"PDMT","10","15+40.00 -L-"]
["","","","","C204066-TC","1","UNION","BOGGS PAVING, INC.",36682.959999999999,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",657352.93000000005,"","",0.17399999999999999," ",""," "," ","","",null,null,null,"","",""]
["","10","B-5170","C204062","C204062-EC","1","MITCHELL","NATIONAL BRIDGE BUILDERS LLC",73215,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204062-RW","1","MITCHELL","NATIONAL BRIDGE BUILDERS LLC",605952,"RW1","",0.10299999999999999,2,"B812",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204062-SI","1","MITCHELL","NATIONAL BRIDGE BUILDERS LLC",8338,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204062-ST","1","MITCHELL","NATIONAL BRIDGE BUILDERS LLC",613879.5,"BR01","X080",1.2999999999999999E-2,null,"15",null,42,"722","A",1,39.83,67.25,"V MTN","13","15+54.50 -L-"]
["","","","","C204062-TC","1","MITCHELL","NATIONAL BRIDGE BUILDERS LLC",67137.5,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",1368522,"","",0.11600000000000001," ","",null," ","",""," "," "," ","","",""]
["","11","B-4823","C203943","C203943-EC","1","TRANSYLVANIA","DANE CONSTRUCTION INC",73578.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203943-RW","1","TRANSYLVANIA","DANE CONSTRUCTION INC",263928.75,"RW1","I000",0.11799999999999999,2,"C003",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203943-SI","1","TRANSYLVANIA","DANE CONSTRUCTION INC",3801.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C203943-ST","1","TRANSYLVANIA","DANE CONSTRUCTION INC",341029.66,"CV01","X928",7.0000000000000001E-3,3.62,"C004",39.5,11,"","",null,null,null,"V MTN","14","(17+23.00-L-)"]
["","","","","C203943-TC","1","TRANSYLVANIA","DANE CONSTRUCTION INC",56881.4,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",739220.16,"","",0.125," ",""," "," ","","",null,null,null,"","",""]
["","12","B-5405","C204067","C204067-EC","1","TRANSYLVANIA","BUCKEYE BRIDGE LLC",64399,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204067-RW","1","TRANSYLVANIA","BUCKEYE BRIDGE LLC",420054.5,"RW1","",0.13,2,"B801",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204067-SI","1","TRANSYLVANIA","BUCKEYE BRIDGE LLC",6713,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204067-ST","1","TRANSYLVANIA","BUCKEYE BRIDGE LLC",443407.4,"BR01","X008",1.2E-2,null,"15",null,30.5,"722","A",1,30.5,62.322899999999997,"V MTN","14","(14+27.00-L-)"]
["","","","","C204067-TC","1","TRANSYLVANIA","BUCKEYE BRIDGE LLC",40699,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",975272.9,"","",0.14199999999999999," ","",null," ",""," "," "," "," ","","",""]
["","13","B-5406","C204012","C204012-EC","1","MACON","BUCKEYE BRIDGE LLC",74902.5,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204012-RW","1","MACON","BUCKEYE BRIDGE LLC",451719.25,"RW1","",9.0999999999999998E-2,2,"B801",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204012-SI","1","MACON","BUCKEYE BRIDGE LLC",8996.84,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204012-ST","1","MACON","BUCKEYE BRIDGE LLC",386156.6,"BR01","X080",1.4E-2,null,"15",null,33,"722","A",1,30.5,72.333299999999994,"V MTN","14","13+86.00 -L-"]
["","","","","C204012-TC","1","MACON","BUCKEYE BRIDGE LLC",14610.16,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",936385.35,"","",0.105," ","",null," ","",""," ","  "," ","","",""]
["2/21/2018","1","R-5868","C204145","C204145A-RW","1","EDGECOMBE","BARNHILL CONTRACTING COMPANY",282900,"RW1","",null,null,"M713",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204145B-RW","1","EDGECOMBE","BARNHILL CONTRACTING COMPANY",38693533.799999997,"RW1","",null,null,"M713",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",38976433.799999997,"","",null,null,"",null,null,"","",null,null,null,"","",""]
["3/20/2018","1","U-2525C","C204096","C204096-EC","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",18712922.550000001,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204096-LI","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",4566495.75,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204096-RW","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",251722247.91,"RW1","I000",5.1790000000000003,6,"N211",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204096-SG","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",5791952.5499999998,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204096-SI","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",5298271.26,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204096-ST","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",1992034.95,"CV01","Y007",null,78,"C001",483.75,8,"","",null,null,null,"PDMT","07","(364+68.00-L-)"]
["","","","","","2","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",1572842.4,"CV02","Y007",null,44.5,"C001",634.5,6,"","",null,null,null,"PDMT","07","(382.49.00-L-)"]
["","","","","","3","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",1103318.3999999999,"CV03","Y007",null,39.25,"C001",336.5,8,"","",null,null,null,"PDMT","07","(430+93.00-L-)"]
["","","","","","4","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",995170.2,"CV04","Y007",null,39.25,"C001",313,8,"","",null,null,null,"PDMT","07","(430+93.00-L-)"]
["","","","","","5","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",5688358.6500000004,"CV05","Y007",8.0000000000000002E-3,39.25,"C003",417,11,"","",null,null,null,"PDMT","07","(430-93.00-L-)"]
["","","","","","6","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",222358.35,"CV06","Y007",null,7.5,"C001",78,8,"","",null,null,null,"PDMT","07","(430+93.00-L-)"]
["","","","","","7","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",610824,"WL1","Y007",null,null,"W001",18.32,null,"","",null,null,null,"PDMT","07","(292+96.51-L-)"]
["","","","","","8","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",788580,"WL2","Y007",null,null,"W001",21.25,null,"","",null,null,null,"PDMT","07","(292+96.51-L-)"]
["","","","","","9","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",972477,"WL3","Y007",null,null,"W001",18.170000000000002,null,"","",null,null,null,"PDMT","07","(13+07.82-Y1-)"]
["","","","","","10","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",1082484,"WL4","Y007",null,null,"W001",19.579999999999998,null,"","",null,null,null,"PDMT","07","(13+07.82-Y1-)"]
["","","","","","11","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",843612,"WL5","Y007",null,null,"W001",19.57,null,"","",null,null,null,"PDMT","07","(400+72.19-L-)"]
["","","","","","12","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",828450,"WL6","Y007",null,null,"W001",18.68,null,"","",null,null,null,"PDMT","07","(400+72.19-L-)"]
["","","","","","13","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",735480,"WL7","Y007",null,null,"W001",19.37,null,"","",null,null,null,"PDMT","07","(447+77.20-L-)"]
["","","","","","14","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",807732,"WL8","Y007",null,null,"W001",18.28,null,"","",null,null,null,"PDMT","07","(447+77.20-L-)"]
["","","","","","15","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",855399,"WL9","Y007",null,null,"W001",16.57,null,"","",null,null,null,"PDMT","07","(24+51.12-Y6-)"]
["","","","","","16","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",959904,"WL10","Y007",null,null,"W001",18.05,null,"","",null,null,null,"PDMT","07","(24+51.12-Y6-)"]
["","","","","","17","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",331170,"WL11","Y007",null,null,"W001",6.64,null,"","",null,null,null,"PDMT","07","(22+45.00-Y6RPD-)"]
["","","","","","18","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",3040463.73,"BR01","X281",null,null,"11",null,51.25,"864","I",2,49,202,"PDMT","07","(17+37.28-Y16-)"]
["","","","","","19","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",2643263.67,"BR02","X281",2.1000000000000001E-2,null,"11",null,64.166700000000006,"854","B",1,60.916699999999999,109.25,"PDMT","07","(329+95.42-L-) LT"]
["","","","","","20","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",2643185.31,"BR03","X281",null,null,"11",null,64.166700000000006,"854","B",1,60.916699999999999,109.25,"PDMT","07","(329+95.42-L-) RT"]
["","","","","","21","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",5125347.1500000004,"BR04","X181",3.5999999999999997E-2,null,"11",null,63.25,"845","I",3,60,192.66669999999999,"PDMT","07","(337+20.09-L-) LT"]
["","","","","","22","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",4775652.66,"BR05","X181",null,null,"11",null,63.25,"845","I",3,60,192.66669999999999,"PDMT","07","(337+20.09-L-) RT"]
["","","","","","23","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",4971800.88,"BR06","X281",null,null,"11",null,81.25,"864","B",2,73.5,201,"PDMT","07","(28+98.81-Y4-)"]
["","","","","","24","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",3034943.58,"BR07","X281",null,null,"11",null,53.583300000000001,"864","I",2,40,240,"PDMT","07","(25+52.71-Y7-)"]
["","","","","","25","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",2302179.15,"BR08","X281",null,null,"11",null,69.75,"864","B",1,66.5,111,"PDMT","07","(470+43.12-L-) LT"]
["","","","","","26","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",2302179.12,"BR09","X281",2.1000000000000001E-2,null,"11",null,69.75,"864","B",1,66.5,111.0104,"PDMT","07","(470+43.12-L-) RT"]
["","","","","","27","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",48469299.450000003,"BR10","X281",null,null,"11",null,53.583300000000001,"864","I",2,40,240,"PDMT","07","(25+52.71-Y7-)"]
["","","","","C204096-TC","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",2571137.64,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204096-UT","1","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",10693627.890000001,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","2","GUILFORD","ES WAGNER COMPANY LLC/SMITH-ROWE LLC-JV",6938383.2599999998,"RW1","NPAR",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",405993548.45999998,"","",5.2649999999999997," ",""," "," "," ",""," "," "," ","","",""]
["","2","I-6002","C204139","C204139-RW","1","CRAVEN","BARNHILL CONTRACTING COMPANY",76476691.290000007,"RW1","",32.04,4,"R000",null,null,"","",null,null,null,"COAST","02",""]
["","","","","","","","Result",76476691.290000007,"","",32.04," ","",null,null,"","",null,null,null,"","",""]
["","3","U-4762","C203972","C203972-RW","1","EDGECOMBE","BARNHILL CONTRACTING COMPANY",13254735.539999999,"RW1","",1.29,2,"D340",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C203972-SG","1","EDGECOMBE","BARNHILL CONTRACTING COMPANY",31950.75,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C203972-SI","1","EDGECOMBE","BARNHILL CONTRACTING COMPANY",547519.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C203972-UT","1","EDGECOMBE","BARNHILL CONTRACTING COMPANY",2714278.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",16548484.289999999,"","",1.29," ","",null,null,"","",null,null,null,"","",""]
["","4","I-5937","C204138","C204138-RW","1","WILSON","FSC II LLC DBA FRED SMITH COMPANY",17498514.780000001,"RW1","I000",7.7,4,"RH10",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",17498514.780000001,"","",7.7," ","",null,null,"","",null,null,null,"","",""]
["","5","U-5828","C203981","C203981-RW","1","WAKE","BARNHILL CONTRACTING COMPANY",34727005.950000003,"RW1","",1.649,4,"N250",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",34727005.950000003,"","",1.649," ","",null,null,"","",null,null,null,"","",""]
["","6","","C204128","C204128A-RW","1","VANCE","CAROLINA SUNROCK LLC",1472134.02,"RW1","",1.9,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204128B-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",1443056.1,"RW1","",4.13,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204128C-RW","1","VANCE","CAROLINA SUNROCK LLC",11006575.439999999,"RW1","",28.914000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204128D-RW","1","VANCE","CAROLINA SUNROCK LLC",59776.08,"RW1","",0.12,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",13981541.640000001,"","",35.064," ","",null,null,"","",null,null,null,"","",""]
["","7","","C204143","C204143A-RW","1","FRANKLIN","FSC II LLC DBA FRED SMITH COMPANY",5135802.0599999996,"RW1","",13.13,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204143B-RW","1","FRANKLIN","FSC II LLC DBA FRED SMITH COMPANY",11752876.68,"RW1","",39.119999999999997,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204143C-RW","1","WARREN","FSC II LLC DBA FRED SMITH COMPANY",252551.28,"RW1","",0.85899999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",17141230.02,"","",53.109000000000002," ","",null,null,"","",null,null,null,"","",""]
["","8","B-4491","C204076","C204076-EC","1","CUMBERLAND","BARNHILL CONTRACTING COMPANY",2637862.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204076-RW","1","CUMBERLAND","BARNHILL CONTRACTING COMPANY",35854676.880000003,"RW1","I000",1.0509999999999999,4,"64",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204076-SG","1","CUMBERLAND","BARNHILL CONTRACTING COMPANY",1854275.7,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204076-SI","1","CUMBERLAND","BARNHILL CONTRACTING COMPANY",532260.15,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204076-ST","1","CUMBERLAND","BARNHILL CONTRACTING COMPANY",5732451.5700000003,"BR01","X081",3.5999999999999997E-2,null,"11",null,92.583299999999994,"854","I",2,90,190,"COAST","06","55+88.11 -L-"]
["","","","","C204076-TC","1","CUMBERLAND","BARNHILL CONTRACTING COMPANY",1424728.32,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204076-UT","2","CUMBERLAND","BARNHILL CONTRACTING COMPANY",1574776.8,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","","","Result",49611031.920000002,"","",1.087," ","",null," ","",""," "," "," ","","",""]
["","10","","C204136","C204136A-RW","1","DAVIDSON","J T RUSSELL & SONS INC",8845132.8000000007,"RW1","",10.818,5,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204136B-RW","1","DAVIDSON","J T RUSSELL & SONS INC",8450830.8000000007,"RW1","",20.155999999999999,5,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204136C-RW","1","DAVIDSON","J T RUSSELL & SONS INC",203249.34,"RW1","",0.69399999999999995,5,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",17499212.940000001,"","",31.667999999999999," ","",null,null,"","",null,null,null,"","",""]
["","11","","C204140","C204140A-RW","1","DAVIDSON","SHARPE BROTHERS A  DIVISION OF VECELLIO",926131.44,"RW1","",0.88600000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204140B-RW","1","DAVIDSON","SHARPE BROTHERS A  DIVISION OF VECELLIO",143489.91,"RW1","",0.47699999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204140C-RW","1","FORSYTH","SHARPE BROTHERS A  DIVISION OF VECELLIO",16104655.77,"RW1","",24.265000000000001,3,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204140D-RW","1","FORSYTH","SHARPE BROTHERS A  DIVISION OF VECELLIO",7151384.4900000002,"RW1","",13.83,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",24325661.609999999,"","",39.457999999999998," ","",null,null,"","",null,null,null,"","",""]
["","12","","C204141","C204141A-RW","1","ROWAN","J T RUSSELL & SONS INC",5116227.75,"RW1","",5.056,5,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204141B-RW","1","ROWAN","J T RUSSELL & SONS INC",9777039.7799999993,"RW1","",18.858000000000001,5,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",14893267.529999999,"","",23.914000000000001," ","",null,null,"","",null,null,null,"","",""]
["","13","U-6084","C204126","C204126-RW","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",19333485.030000001,"RW1","",0.63200000000000001,6,"M720",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204126-SG","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",2217058.5,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",21550543.530000001,"","",0.63200000000000001," ","",null,null,"","",null,null,null,"","",""]
["","14","I-5770","C204116","C204116-RW","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",24005040.27,"RW1","I000",7.57,10,"RH12",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204116-ST","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",1927223.1,"BR01","X231",3.1E-2,null,"",null,145.08330000000001,"336","I",3,142,140,"PDMT","10","590071"]
["","","","","","2","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",1516020.9,"BR02","X231",7.0000000000000007E-2,null,"11",null,72.332999999999998,"586","I",3,69.5,317,"PDMT","10","590113 (NBL)"]
["","","","","","3","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",1634948.25,"BR03","X231",7.0000000000000007E-2,null,"11",null,72.332999999999998,"586","I",3,69.5,317,"PDMT","10","590115 (SBL)"]
["","","","","","4","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",2743554,"BR04","X231",6.8000000000000005E-2,null,"11",null,156.52080000000001,"652","Q",3,153.4376,334.3802,"PDMT","10","5900819"]
["","","","","","","","Result",31826786.52,"","",7.8090000000000002," ","",null," "," "," "," "," "," ","","",""]
["","15","","C204142","C204142A-RW","1","CLEVELAND","ASPHALT PAVING OF SHELBY INC",9108332.4000000004,"RW1","",15.25,4,"R000",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C204142B-RW","1","CLEVELAND","ASPHALT PAVING OF SHELBY INC",18010683.300000001,"RW1","",41.72,4,"R000",null,null,"","",null,null,null,"MTN","12",""]
["","","","","","","","Result",27119015.699999999,"","",56.97," ","",null,null,"","",null,null,null,"","",""]
["","16","","C204144","C204144A-RW","1","IREDELL","MAYMEAD INC",10842096.9,"RW1","",19.451000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C204144B-RW","1","IREDELL","MAYMEAD INC",14954699.1,"RW1","",37.432000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",25796796,"","",56.883000000000003," ","",null,null,"","",null,null,null,"","",""]
["","17","U-2579D","C204088","C204088-RW","1","FORSYTH","FLATIRON CONSTRUCTORS INC - BLYTHE DEVEL",422334000,"RW1","",6.9,6,"M713",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",422334000,"","",6.9," ","",null,null,"","",null,null,null,"","",""]
["4/17/2018","1","R-2633D","C204080","C204080-SG","1","NEW HANOVER","FULCHER ELECTRIC OF FAYETTEVILLE INC",5678793.5999999996,"RW1","Y033",21,4,"M705",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",5678793.5999999996,"","",21," ","",null,null,"","",null,null,null,"","",""]
["","2","U-5795","C204057","C204057-RW","1","JOHNSTON","FSC II LLC DBA FRED SMITH COMPANY",9974220.3300000001,"RW1","",0.58899999999999997,2,"D340",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204057-SG","1","JOHNSTON","FSC II LLC DBA FRED SMITH COMPANY",795179.67,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",10769400,"","",0.58899999999999997," ","",null,null,"","",null,null,null,"","",""]
["","3","","C204158","C204158A-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",9269432.1300000008,"RW1","",14.605,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204158B-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",8331755.9100000001,"RW1","",13.93,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",17601188.039999999,"","",28.535," ","",null,null,"","",null,null,null,"","",""]
["","4","R-2501C","C203615","C203615-EC","1","RICHMOND","R E GOODSON CONSTRUCTION CO INC",2054973.75,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C203615-RW","1","RICHMOND","R E GOODSON CONSTRUCTION CO INC",30426945.300000001,"RW1","",3.5640000000000001,4,"D303",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C203615-SI","1","RICHMOND","R E GOODSON CONSTRUCTION CO INC",750151.95,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C203615-TC","1","RICHMOND","R E GOODSON CONSTRUCTION CO INC",964013.67,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",34196084.670000002,"","",3.5640000000000001," ","",null,null,"","",null,null,null,"","",""]
["","5","","C204159","C204159A-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",491160.72,"RW1","",0.5,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159B-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",7136094.0300000003,"RW1","",8.49,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159C-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",318908.84999999998,"RW1","",0.63,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159D-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",1743965.85,"RW1","",1.78,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159E-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",1897859.85,"RW1","",2.31,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159F-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",2225718.9900000002,"RW1","",3.11,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159G-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",680029.98,"RW1","",0.84,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159H-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",556691.1,"RW1","",0.69,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159I-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",588451.53,"RW1","",1.25,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159J-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",502978.89,"RW1","",1.03,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159K-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",193763.49,"RW1","",0.19,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159L-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",957356.85,"RW1","",1.18,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159M-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",427811.58,"RW1","",0.35,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204159N-RW","1","MECKLENBURG","THE LANE CONSTRUCTION CORPORATION",378044.1,"RW1","",0.48,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",18098835.809999999,"","",22.83," ","",null,null,"","",null,null,null,"","",""]
["","6","","C204162","C204162A-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",3838373.16,"RW1","",3.9,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162B-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1856921.82,"RW1","",1.8,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162C-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",492314.25,"RW1","",1.08,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162D-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",383387.25,"RW1","",0.79,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162E-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1257182.3999999999,"RW1","",1.6,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162F-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1613278.5,"RW1","",2.1,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162G-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",637926.24,"RW1","",1.45,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162H-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1634572.5,"RW1","",1.96,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162I-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",506229,"RW1","",0.73,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162J-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",602944.5,"RW1","",0.88,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162K-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",942262.32,"RW1","",1.5,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162L-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1528594.56,"RW1","",1.95,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162M-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",824837.88,"RW1","",1.29,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162N-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",906423,"RW1","",1.23,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162O-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",2437509.9,"RW1","",2.4,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162P-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1126970.1000000001,"RW1","",0.74,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162Q-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1630324.62,"RW1","",2.4,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162R-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",305013.42,"RW1","",1.2,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162S-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1868521.62,"RW1","",3.8,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162T-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",496492.5,"RW1","",1.3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162U-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",276959.15999999997,"RW1","",1.1000000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162V-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1329249,"RW1","",1.3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162W-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",592388.25,"RW1","",1.2,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162X-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1104529.5,"RW1","",2.2999999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162Y-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",560625,"RW1","",1.3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204162Z-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",478719.75,"RW1","",1.1000000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",29232550.199999999,"","",42.4," ","",null,null,"","",null,null,null,"","",""]
["","7","","C204161","C204161A-RW","1","GASTON","BLYTHE CONSTRUCTION INC",17529423.57,"RW1","",18.149999999999999,5,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C204161B-RW","1","GASTON","BLYTHE CONSTRUCTION INC",14905499.220000001,"RW1","",45.1,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",32434922.789999999,"","",63.25," ","",null,null,"","",null,null,null,"","",""]
["","8","","C204160","C204160A-RW","1","CATAWBA","MAYMEAD INC",6666228,"RW1","",14.89,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C204160B-RW","1","BURKE","MAYMEAD INC",384098.16,"RW1","",0.35,2,"R000",null,null,"","",null,null,null,"MTN","12",""]
["","","","","C204160C-RW","1","CATAWBA","MAYMEAD INC",14531958.630000001,"RW1","",36.21,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",21582284.789999999,"","",51.45," ","",null,null,"","",null,null,null,"","",""]
["5/15/2018","1","","C204171","C204171-ST","1","CURRITUCK","FREYSSINET, INC",16103475.33,"BR01","X081",0.48,null,"15",null,62.833300000000001,"754","A",27,60,2507,"COAST","01","BRIDGE NO. 15"]
["","","","","C204171-TC","1","CURRITUCK","FREYSSINET, INC",1752177,"RW1","",null,4,"M720",null,null,"","",null,null,null,"COAST","01",""]
["","","","","","","","Result",17855652.329999998,"","",0.48," ","",null," ","",""," "," "," ","","",""]
["","2","","C204185","C204185-ST","1","BRUNSWICK","SLOAN CONSTRUCTION A DIVISION OF REEVES",39178935.899999999,"BR01","X080",0.8,null,"15",null,42.583300000000001,"100","I",65,40,4249.4166999999998,"COAST","03","BRIDGE NO. 4"]
["","","","","C204185-TC","1","BRUNSWICK","SLOAN CONSTRUCTION A DIVISION OF REEVES",1885390.83,"RW1","",null,2,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204185A-RW","1","BRUNSWICK","SLOAN CONSTRUCTION A DIVISION OF REEVES",1514600.55,"RW1","",0.3,3,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204185B-RW","1","BRUNSWICK","SLOAN CONSTRUCTION A DIVISION OF REEVES",4828610.82,"RW1","",5.2,3,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",47407538.100000001,"","",6.3," ","",null," ","",""," "," "," ","","",""]
["","3","","C204168","C204168A-RW","1","DURHAM","CAROLINA SUNROCK LLC",4728535.9800000004,"RW1","",5.2249999999999996,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204168B-RW","1","WAKE","CAROLINA SUNROCK LLC",11275775.4,"RW1","",9.9629999999999992,5,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",16004311.380000001,"","",15.188000000000001," ","",null,null,"","",null,null,null,"","",""]
["","4","","C204167","C204167A-RW","1","DURHAM","CAROLINA SUNROCK LLC",11864369.58,"RW1","",21.62,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204167B-RW","1","DURHAM","CAROLINA SUNROCK LLC",1200955.83,"RW1","",3.15,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",13065325.41,"","",24.77," ","",null,null,"","",null,null,null,"","",""]
["","5","B-5140","C204097","C204097-EC","1","FRANKLIN","NATIONAL BRIDGE BUILDERS LLC",76957.2,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204097-RW","1","FRANKLIN","NATIONAL BRIDGE BUILDERS LLC",736425,"RW1","",0.114,2,"B810",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204097-SI","1","FRANKLIN","NATIONAL BRIDGE BUILDERS LLC",13249.8,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204097-ST","1","FRANKLIN","NATIONAL BRIDGE BUILDERS LLC",1669695.75,"BR01","X080",1.6E-2,null,"15",null,33,"729","Q",1,30.833300000000001,82.25,"PDMT","05","13+25.00 -L-"]
["","","","","C204097-TC","1","FRANKLIN","NATIONAL BRIDGE BUILDERS LLC",29994.45,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",2526322.2000000002,"","",0.13," ","",null," ","",""," "," "," ","","",""]
["","6","B-5161","C204098","C204098-EC","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",278755.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204098-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",3011779.5,"RW1","",0.20599999999999999,2,"B810",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204098-SI","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",27162,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204098-ST","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",3296814,"BR01","X080",3.1E-2,null,"15",null,42,"729","Q",2,34,162.375,"PDMT","05","15+14.00-L-"]
["","","","","C204098-TC","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",20355,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204098-UT","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",337830,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",6972696,"","",0.23699999999999999," ","",null," ","",""," "," "," ","","",""]
["","7","B-5320","C204099","C204099-EC","1","GRANVILLE","NATIONAL BRIDGE BUILDERS LLC",172734.57,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204099-RW","1","GRANVILLE","NATIONAL BRIDGE BUILDERS LLC",1035277.5,"RW1","I000",0.104,2,"B810",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204099-SI","1","GRANVILLE","NATIONAL BRIDGE BUILDERS LLC",23462.880000000001,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204099-ST","1","GRANVILLE","NATIONAL BRIDGE BUILDERS LLC",3630409.5,"BR01","X080",0.04,null,"15",null,33,"733","Q",3,30.833300000000001,212.8802,"PDMT","05","15+98.00 -L-"]
["","","","","C204099-TC","1","GRANVILLE","NATIONAL BRIDGE BUILDERS LLC",35201.4,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",4897085.8499999996,"","",0.14399999999999999," ","",null," ","",""," "," "," ","","",""]
["","8","B-5352","C204101","C204101-EC","1","ROCKINGHAM","SMITH-ROWE, LLC",160030.32,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204101-RW","1","ROCKINGHAM","SMITH-ROWE, LLC",5294557.5,"RW1","I000",0.78100000000000003,2,"B812",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204101-SI","1","ROCKINGHAM","SMITH-ROWE, LLC",39506.400000000001,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204101-ST","1","ROCKINGHAM","SMITH-ROWE, LLC",4782909.8099999996,"BR01","X581",3.1E-2,null,"14",null,42.25,"736","Q",3,42,162,"PDMT","07","12+16.89 -L-"]
["","","","","C204101-TC","1","ROCKINGHAM","SMITH-ROWE, LLC",711026.4,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",10988030.43,"","",0.81200000000000006," ","",null," ","",""," "," "," ","","",""]
["","9","I-5853","C204183","C204120-RW","1","GUILFORD","BLYTHE CONSTRUCTION INC",15329138.25,"RW1","I000",1.8740000000000001,6,"R000",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",15329138.25,"","",1.8740000000000001," ","",null,null,"","",null,null,null,"","",""]
["","10","","C204172","C204172A-RW","1","MOORE","RILEY PAVING INC",15449392.23,"RW1","",24.652999999999999,4,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204172B-RW","1","MOORE","RILEY PAVING INC",8727180.3000000007,"RW1","",26.611999999999998,4,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",24176572.530000001,"","",51.265000000000001," ","",null,null,"","",null,null,null,"","",""]
["","11","","C204169","C204169A-RW","1","RANDOLPH","RILEY PAVING INC",10997916.359999999,"RW1","",13.108000000000001,5,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204169B-RW","1","RANDOLPH","RILEY PAVING INC",26055785.640000001,"RW1","",52.482999999999997,5,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",37053702,"","",65.590999999999994," ","",null,null,"","",null,null,null,"","",""]
["","12","","C204170","C204170A-RW","1","RICHMOND","BARNHILL CONTRACTING COMPANY",2037526.8,"RW1","",3.0150000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204170B-RW","1","RICHMOND","BARNHILL CONTRACTING COMPANY",5650369.7400000002,"RW1","",11.94,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204170C-RW","1","RICHMOND","BARNHILL CONTRACTING COMPANY",2493038.52,"RW1","",6.1669999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204170D-RW","1","RICHMOND","BARNHILL CONTRACTING COMPANY",3320400.78,"RW1","",7.59,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204170E-RW","1","RICHMOND","BARNHILL CONTRACTING COMPANY",437568.9,"RW1","",1.5529999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204170F-RW","1","RICHMOND","BARNHILL CONTRACTING COMPANY",793743.45,"RW1","",2.96,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",14732648.189999999,"","",33.225000000000001," ","",null,null,"","",null,null,null,"","",""]
["","13","","C204173","C204173A-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1788396.15,"RW1","",1.88,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173B-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",2880024.15,"RW1","",2.2599999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173C-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1124132.43,"RW1","",0.8,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173D-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",659051.55000000005,"RW1","",0.76,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173E-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1780433.4,"RW1","",1.48,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173F-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1759777.95,"RW1","",1.72,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173G-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1943201.85,"RW1","",1.7,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173H-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1343262.6,"RW1","",1.1299999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173I-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1434156.9,"RW1","",0.71,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173J-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",2972143.95,"RW1","",3.73,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173K-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",2053302,"RW1","",2.44,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173L-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",790208.25,"RW1","",1.38,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173M-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",308061.75,"RW1","",0.28000000000000003,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173N-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1439907.75,"RW1","",1.64,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204173O-RW","1","MECKLENBURG","BLYTHE BROTHERS ASPHALT CO LLC",1024476.9,"RW1","",1.38,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",23300537.579999998,"","",23.29," ","",null,null,"","",null,null,null,"","",""]
["","14","","C204166","C204166A-RW","1","UNION","BLYTHE CONSTRUCTION INC",1221636.6000000001,"RW1","",1.5,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166B-RW","1","UNION","BLYTHE CONSTRUCTION INC",989517.36,"RW1","",1.1000000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166C-RW","1","UNION","BLYTHE CONSTRUCTION INC",2038138.92,"RW1","",2.8,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166D-RW","1","UNION","BLYTHE CONSTRUCTION INC",1228289.3999999999,"RW1","",1.3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166E-RW","1","UNION","BLYTHE CONSTRUCTION INC",1022658.12,"RW1","",1.3,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166F-RW","1","UNION","BLYTHE CONSTRUCTION INC",308850,"RW1","",1.27,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166G-RW","1","UNION","BLYTHE CONSTRUCTION INC",296058.59999999998,"RW1","",1.1000000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166H-RW","1","UNION","BLYTHE CONSTRUCTION INC",1424928.3,"RW1","",2.74,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204166I-RW","1","UNION","BLYTHE CONSTRUCTION INC",518505.6,"RW1","",1.0900000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",9048582.9000000004,"","",14.2," ","",null,null,"","",null,null,null,"","",""]
["","15","B-2506","C203790","C203790-EC","1","ANSON","NATIONAL BRIDGE BUILDERS LLC",236901,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203790-RW","1","ANSON","NATIONAL BRIDGE BUILDERS LLC",1263661.5,"RW1","I000",0.27,2,"B810",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203790-SI","1","ANSON","NATIONAL BRIDGE BUILDERS LLC",49577.58,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C203790-ST","1","ANSON","NATIONAL BRIDGE BUILDERS LLC",1946359.5,"BR01","X080",2.4E-2,null,"15",null,30,"722","Q",2,27.833300000000001,127.375,"PDMT","10","18+62.50 -L-"]
["","","","","C203790-TC","1","ANSON","NATIONAL BRIDGE BUILDERS LLC",30919.95,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",3527419.53,"","",0.29399999999999998," ","",null," ","",""," "," "," ","","",""]
["","17","I-5825","C204117","C204117-RW","1","MECKLENBURG","BLYTHE CONSTRUCTION INC",34224627.899999999,"RW1","I000",4.7,6,"RH11",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204117-ST","1","MECKLENBURG","BLYTHE CONSTRUCTION INC",1541118,"BR01","X271",0.03,null,"11",null,52.875,"336","I",3,50,158.8854,"PDMT","10","BRIDGE 207"]
["","","","","","2","MECKLENBURG","BLYTHE CONSTRUCTION INC",1851952.5,"BR02","X271",0.03,null,"11",null,64.541700000000006,"336","I",3,62,158.8854,"PDMT","10","BRIDGE 213"]
["","","","","","3","MECKLENBURG","BLYTHE CONSTRUCTION INC",860422.5,"BR03","X031",6.5000000000000002E-2,null,"15",null,26,"336","I",4,24,341,"PDMT","10","BRIDGE 215"]
["","","","","","","","Result",38478120.899999999,"","",4.8250000000000002," ","",null," ","",""," "," "," ","","",""]
["","18","B-5407","C204079","C204079-EC","1","POLK","APPLE TUCK & ASSOCIATES INC",108657.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204079-RW","1","POLK","APPLE TUCK & ASSOCIATES INC",703466.7,"RW1","I000",4.5999999999999999E-2,2,"B810",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204079-SI","1","POLK","APPLE TUCK & ASSOCIATES INC",11140.5,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204079-ST","1","POLK","APPLE TUCK & ASSOCIATES INC",1330452.3,"BR01","X081",2.1000000000000001E-2,null,"15",null,33,"722","E",2,30.5,112.375,"V MTN","14","13+52.00 -L-"]
["","","","","C204079-TC","1","POLK","APPLE TUCK & ASSOCIATES INC",14382.9,"RW1","I000",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",2168100.15,"","",6.7000000000000004E-2," ","",null," ","",""," "," "," ","","",""]
["5/29/2018","1","P-5705BA","C204058","C204058A-EC","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",1455180,"RW1","",null,null,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204058A-RW","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",23542763.879999999,"RW1","",0.61199999999999999,null,"M720",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204058A-ST","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",45537,"CV01","X688",null,null,"0",21.26,21.2578,"","",null,null,null,"PDMT","10","42+05.33 -A1-"]
["","","","","","2","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",1810079.4,"CV02","Y007",8.9999999999999993E-3,null,"C002",37.75,47.5,"","",null,null,null,"PDMT","10","25+30.89 -S1-"]
["","","","","","3","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",525162,"CV03","Y007",null,7.98,"C101",41.58,9,"","",null,null,null,"PDMT","10","29+35.21 -S1-"]
["","","","","","4","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",1714920.63,"WL1","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","13+12.11 -S1-"]
["","","","","","5","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",2721657.6,"WL2","Y007",null,null,"",6.7,null,"","",null,null,null,"PDMT","10","19+44.29 -S2-"]
["","","","","","6","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",2687008.5,"WL3","Y007",null,null,"37",6.78,null,"","",null,null,null,"PDMT","10","24+29.66 -S2-"]
["","","","","","7","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",5554793.7000000002,"WL4","Y007",null,null,"32",13.8,null,"","",null,null,null,"PDMT","10","28+78.65 -S2-"]
["","","","","","8","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",739222.2,"WL5","Y007",null,null,"32",1.91,null,"","",null,null,null,"PDMT","10","38+59.08 -A1-"]
["","","","","","9","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",6772087.1100000003,"WL7","Y007",null,null,"32",null,null,"","",null,null,null,"PDMT","10","15+39.55 -S1-"]
["","","","","","10","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",101488.68,"WL8","Y007",null,null,"32",null,null,"","",null,null,null,"PDMT","10","27+73.49 -S2-"]
["","","","","","11","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",172471.11,"WL9","Y007",null,null,"32",null,null,"","",null,null,null,"PDMT","10","42+01.20 -A1-"]
["","","","","","12","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",12200866.65,"BR01","X631",3.4000000000000002E-2,null,"21",null,29.5,"676","Q",3,27,179,"PDMT","10","15+39.55 -S1-"]
["","","","","","13","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",3613589.37,"BR02","X631",2.3E-2,null,"21",null,22.5,"440","J",3,20.5,120.33329999999999,"PDMT","10","18+82.25 -S1-"]
["","","","","","14","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",6955626,"BR03","X631",null,null,"21",null,22.5,"440","J",3,20.5,120.0885,"PDMT","10","18+79.37 -S2-"]
["","","","","","15","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",4950019.6500000004,"BR04","X631",3.2000000000000001E-2,null,"21",null,22,"440","Q",4,20,169.33330000000001,"PDMT","10","23+65.83 -S1-"]
["","","","","","16","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",11060054.85,"BR05","X631",null,null,"21",null,22.083300000000001,"440","J",4,20.083300000000001,169.33330000000001,"PDMT","10","23+62.98 -S2-"]
["","","","","","17","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",4070447.19,"BR06","X631",3.2000000000000001E-2,null,"21",null,22.083300000000001,"652","J",3,20.083300000000001,169.33330000000001,"PDMT","10","28+17.22 -S1-"]
["","","","","","18","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",9781309.5899999999,"BR07","X631",null,null,"21",null,22.5,"652","J",3,20.5,119,"PDMT","10","28+12.88 -S2-"]
["","","","","","19","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",7533585.1200000001,"BR08","X631",null,null,"21",null,22,"648","Q",3,20,131,"PDMT","10","42+59.46 -A1-"]
["","","","","","20","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",517291.5,"BR09","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","5TH ST-S2-TRACK S1"]
["","","","","","21","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",732207,"BR10","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","TRADE ST-S4-TRACK S1"]
["","","","","","22","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",510259.5,"BR11","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","4TH ST -S6-TRACK S1"]
["","","","","","23","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",45000,"BR12","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","23+65.83-S1-"]
["","","","","","24","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",4056978,"BR13","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","19+15.71-S1-"]
["","","","","","25","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",394185,"BR14","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","19+68.93-S1-"]
["","","","","","26","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",21155148.93,"BR15","Y007",null,null,"",null,402.42,"100","Q",null,null,1100,"PDMT","10","19+68.93-S1-"]
["","","","","","27","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",97941,"BR16","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","19+15.17-S1-"]
["","","","","","28","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",5702505,"BR17","Y007",null,null,"3",null,35,"101","Q",null,64.666700000000006,656,"PDMT","10","19+68.93-S1-"]
["","","","","C204058A-TC","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",328908,"RW1","",null,null,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204058A-UT","2","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",3460239,"RW1","NPAR",null,null,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204058B-RW","1","MECKLENBURG","CROWDER CONSTRUCTION COMPANY",695352,"RW1","I000",null,null,"M720",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",145703885.16,"","",0.74199999999999999," ",""," "," ","",""," "," "," ","","",""]
["6/5/2018","1","I-5912","C204165","C204165-RW","1","YADKIN","ARCHER WESTERN CONSTRUCTION LLC",148500000,"RW1","I000",5,4,"M720",null,null,"","",null,null,null,"PDMT","11",""]
["","","","","","","","Result",148500000,"","",5," ","",null,null,"","",null,null,null,"","",""]
["6/19/2018","1","U-2412A","C204103","C204103-EC","1","GUILFORD","BRANCH CIVIL INC",1256781.78,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204103-RW","1","GUILFORD","BRANCH CIVIL INC",32272805.760000002,"RW1","",3.589,6,"N210",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204103-SG","1","GUILFORD","BRANCH CIVIL INC",1276682.6100000001,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204103-SI","1","GUILFORD","BRANCH CIVIL INC",270988.62,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204103-ST","1","GUILFORD","BRANCH CIVIL INC",273538.83,"CV01","Y007",null,13,"C001",270,6,"","",null,null,null,"PDMT","07","(173+47.00 -L-)"]
["","","","","","2","GUILFORD","BRANCH CIVIL INC",69085.5,"WL1","Y007",null,null,"W005",7.4,null,"","",null,null,null,"PDMT","07","(18+50.00 -Y17-)"]
["","","","","","3","GUILFORD","BRANCH CIVIL INC",3808877.87,"BR01","X381",0.122,null,"17",null,39.75,"864","I",6,36.5,642.05730000000005,"PDMT","07","(93+43.36-L-) LEFT"]
["","","","","","4","GUILFORD","BRANCH CIVIL INC",3875465.08,"BR02","X381",null,null,"17",null,39.75,"864","I",6,36.5,642.02080000000001,"PDMT","07","(93+43.36-L-) RIGHT"]
["","","","","","5","GUILFORD","BRANCH CIVIL INC",2087441.59,"BR03","X081",7.4999999999999997E-2,null,"15",null,43.25,"878","Q",3,40,400,"PDMT","07","(140+21.50-L-) LEFT"]
["","","","","","6","GUILFORD","BRANCH CIVIL INC",2021620.04,"BR04","X081",null,null,"15",null,39.25,"878","Q",3,36,400,"PDMT","07","(140+21.50-L-) RIGHT"]
["","","","","","7","GUILFORD","BRANCH CIVIL INC",1587178.43,"BR05","X081",5.8000000000000003E-2,null,"15",null,44.5,"872","Q",3,41.25,305,"PDMT","07","(155+02.50-L-) LEFT"]
["","","","","","8","GUILFORD","BRANCH CIVIL INC",1550221.81,"BR06","X081",null,null,"15",null,40.75,"872","Q",3,37.5,305,"PDMT","07","(155+02.50-L-) RIGHT"]
["","","","","","9","GUILFORD","BRANCH CIVIL INC",1071254.0900000001,"BR07","X081",null,null,"11",null,49.58,"854","D",2,36,209,"PDMT","07","(14+97.65-Y8-)"]
["","","","","","10","GUILFORD","BRANCH CIVIL INC",474416,"WL2","Y007",null,null,"W001",26.41,null,"","",null,null,null,"PDMT","07","93+23.34 -L-"]
["","","","","C204103-TC","1","GUILFORD","BRANCH CIVIL INC",1904588.84,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204103-UT","1","GUILFORD","BRANCH CIVIL INC",1960277.26,"RW1","",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","2","GUILFORD","BRANCH CIVIL INC",201895.58,"RW1","NPAR",null,6,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",55963119.689999998,"","",3.8439999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","2","","C204118","C204118-ST","1","CAMDEN","COASTAL GUNITE CONSTRUCTION COMPANY",2421904.6800000002,"BR01","X441",0.40400000000000003,null,"16",null,40.833300000000001,"565","I",24,38,2132.25,"COAST","01","(BRIDGE NO. 43)"]
["","","","","","2","CAMDEN","COASTAL GUNITE CONSTRUCTION COMPANY",2339615.6800000002,"BR02","X441",0.40400000000000003,null,"16",null,40.832999999999998,"565","I",24,38,2132.25,"COAST","01","(BRIDGE NO. 44)"]
["","","","","C204118-TC","1","CAMDEN","COASTAL GUNITE CONSTRUCTION COMPANY",532261.25,"RW1","",null,4,"M720",null,null,"","",null,null,null,"COAST","01",""]
["","","","","","","","Result",5293781.6100000003,"","",0.80800000000000005,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C204194","C204194A-RW","1","JOHNSTON","S T WOOTEN CORPORATION",189717.52,"RW1","",1.28,2,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204194B-RW","1","JOHNSTON","S T WOOTEN CORPORATION",2098463.67,"RW1","",12.5,5,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204194C-RW","1","JOHNSTON","S T WOOTEN CORPORATION",2476270.02,"RW1","",21.951000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",4764451.21,"","",35.731000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C204195","C204195A-RW","1","NASH","BARNHILL CONTRACTING COMPANY",59255.55,"RW1","I000",0.21,4,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204195B-RW","1","NASH","BARNHILL CONTRACTING COMPANY",193491.27,"RW1","I000",1.8,2,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204195C-RW","1","NASH","BARNHILL CONTRACTING COMPANY",2949223.71,"RW1","I000",18.27,5,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204195D-RW","1","NASH","BARNHILL CONTRACTING COMPANY",1417594.06,"RW1","I000",18.510000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",4619564.59,"","",38.79,null,"",null,null,"","",null,null,null,"","",""]
["","6","B-4932","C203938","C203938-EC","1","EDGECOMBE","S T WOOTEN CORPORATION",261357.7,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C203938-RW","1","EDGECOMBE","S T WOOTEN CORPORATION",3608629.8,"RW1","",0.378,2,"B801",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C203938-SI","1","EDGECOMBE","S T WOOTEN CORPORATION",23608,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C203938-ST","1","EDGECOMBE","S T WOOTEN CORPORATION",3408001.38,"BR01","X081",0.11600000000000001,null,"15",null,37.25,"864","A",6,34,610,"PDMT","04","25+00.00 -L-"]
["","","","","C203938-TC","1","EDGECOMBE","S T WOOTEN CORPORATION",203575,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",7505171.8799999999,"","",0.49399999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","7","B-5237","C204112","C204112-EC","1","WAKE","DANE CONSTRUCTION INC",158739.03,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204112-RW","1","WAKE","DANE CONSTRUCTION INC",1031738.72,"RW1","",0.14399999999999999,2,"B812",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204112-SI","1","WAKE","DANE CONSTRUCTION INC",10179.719999999999,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204112-ST","1","WAKE","DANE CONSTRUCTION INC",937782.6,"BR01","X080",1.7000000000000001E-2,null,"15",null,48,"743","A",1,40,87.25,"PDMT","05","38+62.00 -L-"]
["","","","","C204112-TC","1","WAKE","DANE CONSTRUCTION INC",44911.75,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204112-UT","2","WAKE","DANE CONSTRUCTION INC",1215185,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",3398536.82,"","",0.161,null,"",null,null,"","",null,null,null,"","",""]
["","8","U-5169","C204071","C204071-EC","1","GUILFORD","BRANCH CIVIL INC",404419.75,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204071-LI","1","GUILFORD","BRANCH CIVIL INC",297151.32,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204071-RW","1","GUILFORD","BRANCH CIVIL INC",12661644.93,"RW1","I000",0.63800000000000001,4,"D352",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204071-SG","1","GUILFORD","BRANCH CIVIL INC",585122.15,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204071-SI","1","GUILFORD","BRANCH CIVIL INC",663025.4,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204071-ST","1","GUILFORD","BRANCH CIVIL INC",357610,"WL1","Y007",null,null,"W001",5.0999999999999996,null,"","",null,null,null,"PDMT","07","(16+05.73-YRC-)"]
["","","","","","2","GUILFORD","BRANCH CIVIL INC",16593,"WL2","Y007",null,null,"W005",4,null,"","",null,null,null,"PDMT","07","(49+50.00-Y-)"]
["","","","","","3","GUILFORD","BRANCH CIVIL INC",8296.5,"WL3","Y007",null,null,"W005",3,null,"","",null,null,null,"PDMT","07","(54+10.00-Y-)"]
["","","","","","4","GUILFORD","BRANCH CIVIL INC",2258944.7799999998,"BR01","X281",4.7E-2,null,"11",null,101.91670000000001,"790","I",4,93.45,247.5,"PDMT","07","(28+17.37-Y-)"]
["","","","","","5","GUILFORD","BRANCH CIVIL INC",562360.1,"WL4","Y007",null,null,"W001",18.37,null,"","",null,null,null,"PDMT","07","10+00-NW4-"]
["","","","","","6","GUILFORD","BRANCH CIVIL INC",1543756.9,"WL6","Y007",null,null,"W001",23.83,null,"","",null,null,null,"PDMT","07","10+00-NW7-"]
["","","","","C204071-TC","1","GUILFORD","BRANCH CIVIL INC",988857.72,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204071-UT","1","GUILFORD","BRANCH CIVIL INC",144636.46,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","2","GUILFORD","BRANCH CIVIL INC",1988935.64,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",22481354.649999999,"","",0.68500000000000005,null,"",null,null,"","",null,null,null,"","",""]
["","9","B-5351","C204100","C204100-EC","1","GUILFORD","SMITH-ROWE, LLC",121765,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204100-RW","1","GUILFORD","SMITH-ROWE, LLC",3295314.45,"RW1","I000",0.42299999999999999,4,"B813",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204100-SG","1","GUILFORD","SMITH-ROWE, LLC",195480,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204100-SI","1","GUILFORD","SMITH-ROWE, LLC",46658.2,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204100-ST","1","GUILFORD","SMITH-ROWE, LLC",1376565.95,"BR01","X081",4.1000000000000002E-2,null,"15",null,41.25,"854","Q",3,38,221.25,"PDMT","07","(23+26.00 -L-)WBL"]
["","","","","","2","GUILFORD","SMITH-ROWE, LLC",2899196.65,"BR02","X081",null,null,"15",null,41.25,"854","Q",3,38,221.25,"PDMT","07","(23+26.00 -L-)EBL"]
["","","","","C204100-TC","1","GUILFORD","SMITH-ROWE, LLC",91707.58,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",8026687.8300000001,"","",0.46400000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","10","I-5811","C204122","C204122-RW","1","GUILFORD","SHARPE BROTHERS A  DIVISION OF VECELLIO",8292044.4500000002,"RW1","I000",4.72,6,"R000",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",8292044.4500000002,"","",4.72,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C204189","C204189A-RW","1","CHATHAM","S T WOOTEN CORPORATION",4609947.3600000003,"RW1","",19.649000000000001,4,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204189B-RW","1","CHATHAM","S T WOOTEN CORPORATION",6205443.5899999999,"RW1","",48.988,4,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",10815390.949999999,"","",68.637,null,"",null,null,"","",null,null,null,"","",""]
["","12","","C204193","C204193A-RW","1","LEE","S T WOOTEN CORPORATION",6182945.0099999998,"RW1","",16.902000000000001,5,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204193B-RW","1","LEE","S T WOOTEN CORPORATION",1954552.65,"RW1","",11.41,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204193C-RW","1","LEE","S T WOOTEN CORPORATION",109613.7,"RW1","",1.46,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",8247111.3600000003,"","",29.771999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","13","","C204190","C204190A-RW","1","HOKE","BARNHILL CONTRACTING COMPANY",1301057.04,"RW1","",5.96,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204190B-RW","1","SCOTLAND","BARNHILL CONTRACTING COMPANY",615733.25,"RW1","",3.41,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204190C-RW","1","HOKE","BARNHILL CONTRACTING COMPANY",1763807.7,"RW1","",23.22,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204190D-RW","1","SCOTLAND","BARNHILL CONTRACTING COMPANY",1641097,"RW1","",10.24,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","C204190E-RW","1","HOKE","BARNHILL CONTRACTING COMPANY",70166.600000000006,"RW1","",0.47,2,"R000",null,null,"","",null,null,null,"PDMT","08",""]
["","","","","","","","Result",5391861.5899999999,"","",43.3,null,"",null,null,"","",null,null,null,"","",""]
["","14","U-4734","C204124","C204124-RW","1","FORSYTH","JIMMY R LYNCH & SONS INC",9761429.9299999997,"RW1","",1.694,2,"G401",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204124-SG","1","FORSYTH","JIMMY R LYNCH & SONS INC",309646.90000000002,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204124-SI","1","FORSYTH","JIMMY R LYNCH & SONS INC",195534.01,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204124-ST","1","FORSYTH","JIMMY R LYNCH & SONS INC",433661.94,"CV01","Y007",null,29.5,"C002",225,7,"","",null,null,null,"PDMT","09","(27+85.00-L-)"]
["","","","","","2","FORSYTH","JIMMY R LYNCH & SONS INC",1973599.32,"BR01","X081",3.5000000000000003E-2,null,"15",null,98.583299999999994,"754","A",2,85,185,"PDMT","09","(38+35.00-L-)"]
["","","","","C204124-UT","1","FORSYTH","JIMMY R LYNCH & SONS INC",70710.100000000006,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","2","FORSYTH","JIMMY R LYNCH & SONS INC",75163.789999999994,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",12819745.99,"","",1.7290000000000001,null,"",null,null,null,"",null,null,null,"","",""]
["","15","B-4982","C203956","C203956-EC","1","IREDELL","EASTERN STRUCTURES LLC",105815,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203956-RW","1","IREDELL","EASTERN STRUCTURES LLC",1324172.8,"RW1","I000",0.308,2,"B812",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203956-SI","1","IREDELL","EASTERN STRUCTURES LLC",26686.76,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C203956-ST","1","IREDELL","EASTERN STRUCTURES LLC",2024071.6,"BR01","X081",4.1000000000000002E-2,null,"15",null,61.583300000000001,"845","Q",3,59,215.1354,"PDMT","12","21+10.00 -L-"]
["","","","","C203956-TC","1","IREDELL","EASTERN STRUCTURES LLC",196633.92,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",3677380.08,"","",0.34899999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","16","I-5915A","C204155","C204155-RW","1","CATAWBA","MAYMEAD INC",34460409.810000002,"RW1","",20,2,"R000",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",34460409.810000002,"","",20,null,"",null,null,"","",null,null,null,"","",""]
["","17","U-5963","C204095","C204095-SG","1","IREDELL","TRAFFIC CONTROL DEVICES INC",180650,"RW1","",1.5,2,"M705",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",180650,"","",1.5,null,"",null,null,"","",null,null,null,"","",""]
["","18","","C204192","C204192A-RW","1","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",5442120.4100000001,"RW1","",17.95,5,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204192B-RW","1","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",7556633.6900000004,"RW1","",38.68,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204192C-RW","1","BUNCOMBE","HARRISON CONSTRUCTION COMPANY DIVISION O",1886639.49,"RW1","",18.45,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",14885393.59,"","",75.08,null,"",null,null,"","",null,null,null,"","",""]
["","19","","C204187","C204187A-RW","1","BURKE","MAYMEAD INC",2463765.65,"RW1","",10.943,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204187B-RW","1","BURKE","MAYMEAD INC",4216689.68,"RW1","",44.484000000000002,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204187C-RW","1","BURKE","MAYMEAD INC",665636.36,"RW1","",13.933,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",7346091.6900000004,"","",69.36,null,"",null,null,"","",null,null,null,"","",""]
["","20","","C204186","C204186A-RW","1","RUTHERFORD","ROGERS GROUP INC",2694769.96,"RW1","",10.252000000000001,3,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204186B-RW","1","RUTHERFORD","ROGERS GROUP INC",4074115.3,"RW1","",49.24,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204186C-RW","1","RUTHERFORD","ROGERS GROUP INC",840709.32,"RW1","",18.86,2,"R000",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",7609594.5800000001,"","",78.352000000000004,null,"",null,null,"","",null,null,null,"","",""]
["","21","B-4448","C204072","C204072-EC","1","BURKE","DANE CONSTRUCTION INC",479552.98,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204072-RW","1","BURKE","DANE CONSTRUCTION INC",7911279.79,"RW1","",0.54900000000000004,4,"B813",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204072-SI","1","BURKE","DANE CONSTRUCTION INC",119064.29,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204072-ST","1","BURKE","DANE CONSTRUCTION INC",342600,"WL1","Y007",null,null,"W001",14.88,null,"","",null,null,null,"MTN","13","(27+53.80-L-)"]
["","","","","","2","BURKE","DANE CONSTRUCTION INC",312000,"WL2","Y007",null,null,"W001",13.48,null,"","",null,null,null,"MTN","13","(23+91.03-L-)"]
["","","","","","3","BURKE","DANE CONSTRUCTION INC",1087028.3,"BR01","X231",1.9E-2,null,"11",null,45.25,"538","A",1,42,100,"MTN","13","(28+26.49-WBL-)"]
["","","","","","4","BURKE","DANE CONSTRUCTION INC",1635202.3,"BR02","X231",null,null,"11",null,45.25,"538","A",1,42,100,"MTN","13","(28+45.42-EBL-)"]
["","","","","C204072-TC","1","BURKE","DANE CONSTRUCTION INC",472785.09,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",12359512.75,"","",0.56799999999999995,null,"",null,null,null,null,null,null,null,"","",""]
["","22","B-5400","C204077","C204077-EC","1","BUNCOMBE","BUCKEYE BRIDGE LLC",75340,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204077-RW","1","BUNCOMBE","BUCKEYE BRIDGE LLC",253953.75,"RW1","I000",3.4000000000000002E-2,2,"B801",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204077-SI","1","BUNCOMBE","BUCKEYE BRIDGE LLC",4973.6000000000004,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204077-ST","1","BUNCOMBE","BUCKEYE BRIDGE LLC",325779.75,"BR01","X081",1.2999999999999999E-2,null,"15",null,30,"722","A",1,27.833300000000001,67.25,"MTN","13","(10+53.50 -L-)"]
["","","","","C204077-TC","1","BUNCOMBE","BUCKEYE BRIDGE LLC",66859.899999999994,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",726907,"","",4.7E-2,null,"",null,null,"","",null,null,null,"","",""]
["","23","","C204184","C204184-ST","1","BUNCOMBE","SOUTHERN ROAD & BRIDGE LLC",3169666.68,"BR01","X331",0.249,null,"17",null,57.457999999999998,"500","I",11,52,1314.68,"MTN","13","BRIDGE NO. 322"]
["","","","","","2","BUNCOMBE","SOUTHERN ROAD & BRIDGE LLC",3059141.68,"BR02","X331",0.23200000000000001,null,"17",null,60,"500","J",10,52,1227.81,"MTN","13","BRIDGE NO. 323"]
["","","","","C204184-TC","1","BUNCOMBE","SOUTHERN ROAD & BRIDGE LLC",471528,"RW1","",null,2,"M720",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",6700336.3600000003,"","",0.48099999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","24","","C204191","C204191A-RW","1","MACON","HARRISON CONSTRUCTION COMPANY DIVISION O",8767411.0999999996,"RW1","",7.0229999999999997,4,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204191B-RW","1","MACON","HARRISON CONSTRUCTION COMPANY DIVISION O",2303833.4,"RW1","",8.9,2,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",11071244.5,"","",15.923,null,"",null,null,"","",null,null,null,"","",""]
["","25","","C204188","C204188A-RW","1","HAYWOOD","HARRISON CONSTRUCTION COMPANY DIVISION O",8351414.4800000004,"RW1","",10.4,2,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204188B-RW","1","JACKSON","HARRISON CONSTRUCTION COMPANY DIVISION O",281249.19,"RW1","",0.37,2,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204188C-RW","1","JACKSON","HARRISON CONSTRUCTION COMPANY DIVISION O",1833445.09,"RW1","",4.5599999999999996,2,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204188D-RW","1","HAYWOOD","HARRISON CONSTRUCTION COMPANY DIVISION O",1199632.1200000001,"RW1","",5.32,2,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204188E-RW","1","JACKSON","HARRISON CONSTRUCTION COMPANY DIVISION O",1386448.99,"RW1","",6.04,2,"R000",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",13052189.869999999,"","",26.69,null,"",null,null,"","",null,null,null,"","",""]
["","26","I-5111","C204134","C204134A-RW","1","WAKE","S T WOOTEN CORPORATION",360175000,"RW1","I000",12.8,5,"M713",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",360175000,"","",12.8,null,"",null,null,"","",null,null,null,"","",""]
["7/17/2018","1","","C204212","C204212A-RW","1","BERTIE","ROSE BROTHERS PAVING CO INC",2804691.72,"RW1","I000",12.57,2,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","C204212B-RW","1","BERTIE","ROSE BROTHERS PAVING CO INC",1854265.44,"RW1","I000",11.48,2,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","C204212C-RW","1","BERTIE","ROSE BROTHERS PAVING CO INC",1117449.3700000001,"RW1","I000",7.95,2,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","","","","Result",5776406.5300000003,"","",32,null,"",null,null,"","",null,null,null,"","",""]
["","2","","C204201","C204201A-RW","1","DUPLIN","BARNHILL CONTRACTING COMPANY",595304.31999999995,"RW1","",1.93,2,"R000",null,null,"","",null,null,null,"PDMT","03",""]
["","","","","C204201B-RW","1","DUPLIN","BARNHILL CONTRACTING COMPANY",2575094.5,"RW1","",17.04,2,"R000",null,null,"","",null,null,null,"PDMT","03",""]
["","","","","","","","Result",3170398.82,"","",18.97,null,"",null,null,"","",null,null,null,"","",""]
["","3","","C204199","C204199A-RW","1","FRANKLIN","S T WOOTEN CORPORATION",4552690.1399999997,"RW1","",11.82,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",4552690.1399999997,"","",11.82,null,"",null,null,"","",null,null,null,"","",""]
["","4","R-2814C","C204105","C204105-EC","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",1318870.8500000001,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204105-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",31477648.5,"RW1","I000",6.58,4,"D310",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204105-SG","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",528077,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204105-SI","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",364398.03,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204105-ST","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",826582.92,"CV01","X028",7.0000000000000001E-3,7,"C003",136.25,12,"","",null,null,null,"PDMT","05","(107+88.00 -L-)"]
["","","","","","2","WAKE","FSC II LLC DBA FRED SMITH COMPANY",338578,"CV02","Y007",null,4.6900000000000004,"C001",170.5,12,"","",null,null,null,"PDMT","05","(137+22.00 -L-)"]
["","","","","","3","WAKE","FSC II LLC DBA FRED SMITH COMPANY",409031,"CV03","Y007",null,2.5099999999999998,"C002",177.25,7,"","",null,null,null,"PDMT","05","(168+21.00 -L-)"]
["","","","","","4","WAKE","FSC II LLC DBA FRED SMITH COMPANY",303949,"CV04","Y007",null,10.81,"C001",152,10,"","",null,null,null,"PDMT","05","(283+77.00 -L-)"]
["","","","","","5","WAKE","FSC II LLC DBA FRED SMITH COMPANY",857928,"CV05","X028",8.0000000000000002E-3,10.56,"C003",160.75,11,"","",null,null,null,"PDMT","05","(314+63.00 -L-)"]
["","","","","","6","WAKE","FSC II LLC DBA FRED SMITH COMPANY",180516,"CV06","Y007",null,3.27,"C001",81.25,12,"","",null,null,null,"PDMT","05","(21+86.00 -Y6-)"]
["","","","","C204105-TC","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",636958.69999999995,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204105-UT","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",641345,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",37883883,"","",6.5949999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","6","U-3109B","C204106","C204106-EC","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",580838.05000000005,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204106-RW","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",5470199.2000000002,"RW1","",1.3939999999999999,2,"N200",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204106-SG","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",137544.25,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204106-SI","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",77369.05,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204106-ST","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",225038.35,"CV01","Y007",null,14.02,"C001",112.83,12,"","",null,null,null,"PDMT","07","(207+85.77-L-)"]
["","","","","","2","ALAMANCE","THALLE CONSTRUCTION CO., INC.",1215868.3999999999,"BR01","X041",0.03,null,"15",null,39.25,"572","A",1,36,160,"PDMT","07","(227+33.50-L-)"]
["","","","","C204106-TC","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",88608.4,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204106-UT","1","ALAMANCE","THALLE CONSTRUCTION CO., INC.",295666.33,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","2","ALAMANCE","THALLE CONSTRUCTION CO., INC.",60528.77,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",8151660.7999999998,"","",1.4239999999999999,null,"",null,null,"","",null,null,null,"","",""]
["8/21/2018","3","","C204229","C204229A-RW","1","SAMPSON","BARNHILL CONTRACTING COMPANY",6067104.6299999999,"RW1","",23.75,3,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204229B-RW","1","SAMPSON","BARNHILL CONTRACTING COMPANY",3832858.04,"RW1","",26.15,3,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",9899962.6699999999,"","",49.9,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C204227","C204227A-RW","1","WAKE","THE LANE CONSTRUCTION CORPORATION",4265543.75,"RW1","",17.170000000000002,5,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",4265543.75,"","",17.170000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","5","W-5601EV","C204133","C204133-RW","1","COLUMBUS","HIGHLAND PAVING CO LLC",8935437.4000000004,"RW1","I000",2.7490000000000001,4,"D304",null,null,"","",null,null,null,"COAST","06",""]
["","","","","C204133-SG","1","COLUMBUS","HIGHLAND PAVING CO LLC",88695,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","","","Result",9024132.4000000004,"","",2.7490000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C204223","C204223A-RW","1","MADISON","HARRISON CONSTRUCTION COMPANY DIVISION O",2340272.44,"RW1","",10.220000000000001,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","C204223B-RW","1","MADISON","HARRISON CONSTRUCTION COMPANY DIVISION O",3488399.3,"RW1","",28.96,2,"R000",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",5828671.7400000002,"","",39.18,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C204221","C204221-RW","1","BUNCOMBE","R.E. BURNS & SONS CO., INC.",3013751.7,"RW1","",0.246,2,"M720",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",3013751.7,"","",0.246,null,"",null,null,"","",null,null,null,"","",""]
["","8","R-2247EB","C204137","C204137-RW","1","FORSYTH","BLYTHE CONSTRUCTION INC",134150000,"RW1","I000",2.6,4,"M713",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",134150000,"","",2.6,null,"",null,null,"","",null,null,null,"","",""]
["9/18/2018","15","I-5507","C203970","C203970-RW","1","MECKLENBURG","BLYTHE CONSTRUCTION INC",346000000,"RW1","",16.600000000000001,6,"M713",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",346000000,"","",16.600000000000001,null,"",null,null,"","",null,null,null,"","",""]
["10/2/2018","2","","C204254","C204200-ST","1","BRUNSWICK","COASTAL GUNITE CONSTRUCTION COMPANY",2901391.55,"BR01","X081",0.34,null,"15",null,32.25,"754","I",23,30,1800,"COAST","03","BRIDGE NO. 71"]
["","","","","C204200-TC","1","BRUNSWICK","COASTAL GUNITE CONSTRUCTION COMPANY",464797.65,"RW1","",null,2,"M720",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",3366189.2,"","",0.34,null,"",null,null,"","",null,null,null,"","",""]
["","4","R-3825B","C204108","C204108-EC","1","JOHNSTON","W C ENGLISH INCORPORATED",3247831.25,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204108-RW","1","JOHNSTON","W C ENGLISH INCORPORATED",33667231.25,"RW1","",4.5640000000000001,4,"D320",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204108-SG","1","JOHNSTON","W C ENGLISH INCORPORATED",1542842.1,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204108-SI","1","JOHNSTON","W C ENGLISH INCORPORATED",340637.27,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204108-ST","1","JOHNSTON","W C ENGLISH INCORPORATED",973153.8,"CV01","Y007",null,16.399999999999999,"C102",198,12,"","",null,null,null,"PDMT","04","(167+03.45-L-)"]
["","","","","","2","JOHNSTON","W C ENGLISH INCORPORATED",106257.60000000001,"CV02","Y007",null,21,"C000",172,null,"","",null,null,null,"PDMT","04","(114+23.00-L-)"]
["","","","","","3","JOHNSTON","W C ENGLISH INCORPORATED",499560.3,"WL1","Y007",null,null,"W001",13.5,null,"","",null,null,null,"PDMT","04","(72+09.00-L-)"]
["","","","","","4","JOHNSTON","W C ENGLISH INCORPORATED",280631.40000000002,"WL2","Y007",null,null,"W001",12.21,null,"","",null,null,null,"PDMT","04","(82+15.00-L-)"]
["","","","","","5","JOHNSTON","W C ENGLISH INCORPORATED",615491.69999999995,"WL3","Y007",null,null,"W001",15.11,null,"","",null,null,null,"PDMT","04","(102+88.25-L-)"]
["","","","","","6","JOHNSTON","W C ENGLISH INCORPORATED",5262884.03,"BR01","X081",7.5999999999999998E-2,null,"11",null,96.75,"873","Q",3,87,376,"PDMT","04","(64+20.00-L-)"]
["","","","","C204108-TC","1","JOHNSTON","W C ENGLISH INCORPORATED",717638.01,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204108-UT","1","JOHNSTON","W C ENGLISH INCORPORATED",4551538.7,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","2","JOHNSTON","W C ENGLISH INCORPORATED",4239954.54,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","3","JOHNSTON","W C ENGLISH INCORPORATED",29820.07,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","4","JOHNSTON","W C ENGLISH INCORPORATED",2660964.89,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","","","","Result",58736436.909999996,"","",4.6399999999999997,null,"",null,null,"","",null,null,null,"","",""]
["","5","R-3822","C204149","C204149-RW","1","HALIFAX","W C ENGLISH INCORPORATED",20960190.629999999,"RW1","",3.0630000000000002,4,"D351",null,null,"","",null,null,null,"PDMT","04",""]
["","","","","C204149-ST","1","HALIFAX","W C ENGLISH INCORPORATED",194912,"CV01","Y007",null,6.68,"C001",154,6,"","",null,null,null,"PDMT","04","(84+52.00-L-)"]
["","","","","","2","HALIFAX","W C ENGLISH INCORPORATED",3356710.59,"BR01","X081",7.8E-2,null,"15",null,58.083300000000001,"854","Q",5,55.5,410,"PDMT","04","(99+17.60-L1-)"]
["","","","","","","","Result",24511813.219999999,"","",3.141,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C204240","C204240A-RW","1","FRANKLIN","FSC II LLC DBA FRED SMITH COMPANY",3877212.55,"RW1","",30.934000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",3877212.55,"","",30.934000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C204250","C204250A-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",5978967.04,"RW1","",40.44,5,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",5978967.04,"","",40.44,null,"",null,null,"","",null,null,null,"","",""]
["","8","U-6015","C204111","C204111-SG","1","ALAMANCE","ALS OF NORTH CAROLINA LLC",7938392.2000000002,"RW1","Y033",55,4,"M705",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","","","","Result",7938392.2000000002,"","",55,null,"",null,null,"","",null,null,null,"","",""]
["","9","","C204226","C204226A-RW","1","MECKLENBURG","BLYTHE CONSTRUCTION INC",2658683.86,"RW1","",5.76,7,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204226B-RW","1","MECKLENBURG","BLYTHE CONSTRUCTION INC",7166586.2800000003,"RW1","",28.93,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",9825270.1400000006,"","",34.69,null,"",null,null,"","",null,null,null,"","",""]
["","10","I-5714","C204252","C204104B-EC","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",274908.5,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104B-LI","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",422814,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104B-RW","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",7249338.79,"RW1","I000",0.42499999999999999,8,"I602",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104B-SG","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",1157224,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104B-SI","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",522816.5,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104B-ST","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",3390908.53,"BR01","X231",6.7000000000000004E-2,null,"11",null,54.92,"669","I",2,52,353.5,"PDMT","10","26+20.73-YEB-"]
["","","","","","2","MECKLENBURG","BLYTHE DEVELOPMENT CO",245015.83,"BR02","Y007",null,null,"",null,null,"","",null,null,null,"PDMT","10","26+20.73-YEB-EXIST"]
["","","","","C204104B-TC","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",1350243.15,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104B-UT","2","MECKLENBURG","BLYTHE DEVELOPMENT CO",1667177,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",16280446.300000001,"","",0.49199999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","","U-5114","C204252","C204104A-RW","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",10849053.300000001,"RW1","",0.67100000000000004,8,"D312",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104A-SG","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",745860,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104A-SI","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",450147.9,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204104A-ST","1","MECKLENBURG","BLYTHE DEVELOPMENT CO",560560,"WL1","Y007",null,null,"W001",7.4,null,"","",null,null,null,"PDMT","10","34+02.56-L-"]
["","","","","","2","MECKLENBURG","BLYTHE DEVELOPMENT CO",915530,"WL2","Y007",null,null,"W001",10.27,null,"","",null,null,null,"PDMT","10","36+50.65-L-"]
["","","","","","3","MECKLENBURG","BLYTHE DEVELOPMENT CO",56000,"WL3","Y007",null,null,"W005",1.49,null,"","",null,null,null,"PDMT","10","10+09.00-W3-"]
["","","","","C204104A-UT","2","MECKLENBURG","BLYTHE DEVELOPMENT CO",997252.5,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",14574403.699999999,"","",0.67100000000000004,null,"",null,null,"","",null,null,null,"","",""]
["","11","I-5798","C204146","C204146-RW","1","MECKLENBURG","BOGGS PAVING, INC.",9297146.6400000006,"RW1","",12.526,6,"R000",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","C204146-ST","1","MECKLENBURG","BOGGS PAVING, INC.",820665.62,"BR01","X281",9.2999999999999999E-2,null,"11",null,99.380200000000002,"845","",7,96.398499999999999,455.5,"PDMT","10","BRIDGE NO. 939"]
["","","","","","2","MECKLENBURG","BOGGS PAVING, INC.",589606.72,"BR02","X281",0.09,null,"11",null,null,"845","",7,null,443,"PDMT","10","BRIDGE NO. 940"]
["","","","","","3","MECKLENBURG","BOGGS PAVING, INC.",259487.98,"BR03","X281",0.107,null,"11",null,null,"854","",7,null,531,"PDMT","10","BRIDGE NO. 941"]
["","","","","","","","Result",10966906.960000001,"","",12.816000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","13","B-5993","C204251","C204251-RW","1","CUMBERLAND","ES WAGNER COMPANY LLC",970553.74,"RW1","I000",7.4999999999999997E-2,2,"M720",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","","","Result",970553.74,"","",7.4999999999999997E-2,null,"",null,null,"","",null,null,null,"","",""]
["","14","","C204222","C204222-RW","1","RUTHERFORD","APPLE TUCK & ASSOCIATES INC",4497946.5,"RW1","",0.37769999999999998,2,"M720",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","","","Result",4497946.5,"","",0.37769999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","17","U-2719","C204157","C204157B-RW","1","WAKE","THE LANE CONSTRUCTION CORPORATION",311688512,"RW1","",3,6,"M713",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",311688512,"","",3,null,"",null,null,"","",null,null,null,"","",""]
["","","U-4437","C204157","C204157A-RW","1","WAKE","THE LANE CONSTRUCTION CORPORATION",34511488,"RW1","",3.5,5,"M713",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",34511488,"","",3.5,null,"",null,null,"","",null,null,null,"","",""]
["10/16/2018","1","","C204243","C204243-FE","1","DARE","GULF ISLAND SHIPYARDS LLC",11883016.52,"0","",null,null,"M720",null,null,"","",null,null,null,"COAST","01",""]
["","","","","","","","Result",11883016.52,"","",null,null,"",null,null,"","",null,null,null,"","",""]
["","2","","C204224","C204224A-RW","1","BERTIE","BARNHILL CONTRACTING COMPANY",2231111.38,"RW1","",3.92,4,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","C204224B-RW","1","CHOWAN","BARNHILL CONTRACTING COMPANY",2446215.91,"RW1","",15.13,4,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","C204224C-RW","1","MARTIN","BARNHILL CONTRACTING COMPANY",1110194.02,"RW1","",6.72,4,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","C204224D-RW","1","WASHINGTON","BARNHILL CONTRACTING COMPANY",2773051.75,"RW1","",10.86,4,"R000",null,null,"","",null,null,null,"COAST","01",""]
["","","","","","","","Result",8560573.0600000005,"","",36.630000000000003,null,"",null,null,"","",null,null,null,"","",""]
["","4","","C204261","C204261A-RW","1","GRANVILLE","SLURRY PAVERS INC",953302.78,"RW1","",12.33,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204261B-RW","1","WAKE","SLURRY PAVERS INC",848668.79,"RW1","",14.974,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",1801971.57,"","",27.303999999999998,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C204257","C204257A-RW","1","PERSON","WHITEHURST PAVING CO INC",785405.72,"RW1","",12.96,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",785405.72,"","",12.96,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C204258","C204258A-RW","1","FRANKLIN","WHITEHURST PAVING CO INC",825782.03,"RW1","",18,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204258B-RW","1","VANCE","WHITEHURST PAVING CO INC",693591.56,"RW1","",12.69,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204258C-RW","1","WARREN","WHITEHURST PAVING CO INC",1022950.46,"RW1","",15.11,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",2542324.0499999998,"","",45.8,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C204256","C204256A-RW","1","DURHAM","CAROLINA SUNROCK LLC",2070222.79,"RW1","",7.85,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204256B-RW","1","DURHAM","CAROLINA SUNROCK LLC",516376.27,"RW1","",1.1200000000000001,4,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204256C-RW","1","DURHAM","CAROLINA SUNROCK LLC",1195533.96,"RW1","",6.92,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",3782133.02,"","",15.89,null,"",null,null,"","",null,null,null,"","",""]
["","8","I-5938B","C204253","C204253-RW","1","ROBESON","JOHNSON BROTHERS UTILITY & PAVING CO INC",11955472.98,"RW1","I000",15.1,4,"R000",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","","","Result",11955472.98,"","",15.1,null,"",null,null,"","",null,null,null,"","",""]
["","9","I-5850B","C204148","C204148-RW","1","ROBESON","HIGHLAND PAVING CO LLC",11897342.789999999,"RW1","I000",17.8,4,"",null,null,"","",null,null,null,"COAST","06",""]
["","","","","","","","Result",11897342.789999999,"","",17.8,null,"",null,null,"","",null,null,null,"","",""]
["","10","I-5852A","C204174","C204174-RW","1","GUILFORD","DIAMOND SURFACE INC",12294388.58,"RW1","I000",6.7949999999999999,6,"RH12",null,null,"","",null,null,null,"PDMT","07",""]
["","","","","C204174-ST","1","GUILFORD","DIAMOND SURFACE INC",62601.9,"BR01","X231",null,null,"11",null,72.5,"557","A",1,69.416700000000006,141,"PDMT","07","BRIDGE NO. 820"]
["","","","","","2","GUILFORD","DIAMOND SURFACE INC",121375.8,"BR02","X231",null,null,"11",null,72.5,"661","I",3,69.416700000000006,398.9479,"PDMT","07","BRIDGE NO. 821"]
["","","","","","3","GUILFORD","DIAMOND SURFACE INC",27846.7,"BR03","X231",null,null,"12",null,60.833300000000001,"654","I",4,57.083300000000001,586.39580000000001,"PDMT","07","BRIDGE NO. 823"]
["","","","","","4","GUILFORD","DIAMOND SURFACE INC",37469.5,"BR04","X231",null,null,"11",null,62.75,"699","A",1,59.666699999999999,237.85939999999999,"PDMT","07","BRIDGE NO. 824"]
["","","","","","5","GUILFORD","DIAMOND SURFACE INC",48063.199999999997,"BR05","X231",null,null,"11",null,48.333300000000001,"577","A",1,45.25,180.125,"PDMT","07","BRIDGE NO. 825"]
["","","","","","6","GUILFORD","DIAMOND SURFACE INC",39570.5,"BR06","X231",null,null,"11",null,40.416699999999999,"679","N",3,37.333300000000001,618.10940000000005,"PDMT","07","BRIDGE NO. 827"]
["","","","","","7","GUILFORD","DIAMOND SURFACE INC",87132.3,"BR07","X281",null,null,"11",null,72,"873","I",3,68.916700000000006,282.28649999999999,"PDMT","07","BRIDGE NO. 861"]
["","","","","","8","GUILFORD","DIAMOND SURFACE INC",85631.6,"BR08","X281",null,null,"11",null,72,"873","I",3,68.916700000000006,257.04169999999999,"PDMT","07","BRIDGE NO. 862"]
["","","","","","9","GUILFORD","DIAMOND SURFACE INC",73098.899999999994,"BR09","X231",null,null,"11",null,79.416700000000006,"654","I",2,76.333299999999994,225,"PDMT","07","BRIDGE NO. 864"]
["","","","","","10","GUILFORD","DIAMOND SURFACE INC",73098.899999999994,"BR10","X231",null,null,"11",null,79.416700000000006,"654","I",2,76.333299999999994,225,"PDMT","07","BRIDGE NO. 865"]
["","","","","","11","GUILFORD","DIAMOND SURFACE INC",75696.899999999994,"BR11","X281",null,null,"11",null,85.333299999999994,"854","I",3,82.25,177.6875,"PDMT","07","BRIDGE NO. 866"]
["","","","","","12","GUILFORD","DIAMOND SURFACE INC",75964.5,"BR12","X281",null,null,"11",null,85.729200000000006,"854","I",3,82.645899999999997,177.6875,"PDMT","07","BRIDGE NO. 867"]
["","","","","","13","GUILFORD","DIAMOND SURFACE INC",62357.599999999999,"BR13","X231",null,null,"11",null,72,"558","A",1,68.916700000000006,136.15629999999999,"PDMT","07","BRIDGE NO. 869"]
["","","","","","14","GUILFORD","DIAMOND SURFACE INC",62357.599999999999,"BR14","X230",null,null,"11",null,72,"558","A",1,68.916700000000006,136.15629999999999,"PDMT","07","BRIDGE NO. 870"]
["","","","","","15","GUILFORD","DIAMOND SURFACE INC",62707.6,"BR15","X231",null,null,"11",null,72,"565","A",1,68.916700000000006,131.83330000000001,"PDMT","07","BRIDGE NO. 871"]
["","","","","","16","GUILFORD","DIAMOND SURFACE INC",62707.6,"BR16","X231",null,null,"11",null,72,"565","A",1,68.916700000000006,131.9479,"PDMT","07","BRIDGE NO. 872"]
["","","","","","17","GUILFORD","DIAMOND SURFACE INC",41251.199999999997,"BR17","X231",null,null,"11",null,40.5,"651","A",3,37.416699999999999,290.51560000000001,"PDMT","07","BRIDGE NO. 879"]
["","","","","","","","Result",13393320.880000001,"","",6.7949999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C204215","C204215-ST","1","DAVIE","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",1058473.3999999999,"BR01","X081",0.17,null,"15",null,38.833300000000001,"754","I",10,36,900,"PDMT","09","BRIDGE NO. 63"]
["","","","","C204215-TC","1","DAVIE","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",203592.5,"RW1","K000",null,null,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",1262065.8999999999,"","",0.17,null,"",null,null,"","",null,null,null,"","",""]
["","12","B-4746","C204109","C204109-EC","1","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",109326.75,"RW1","I000",null,3,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204109-RW","1","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1543595.38,"RW1","I000",0.17899999999999999,3,"B810",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204109-SG","1","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",392709.25,"RW1","I000",null,3,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204109-SI","1","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",21960.799999999999,"RW1","I000",null,3,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204109-ST","1","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",430100,"WL1","Y007",null,null,"W001",20.76,null,"","A",null,null,null,"PDMT","09","(18+03.65-L-)"]
["","","","","","2","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",415140,"WL2","Y007",null,null,"W001",20.53,null,"","A",null,null,null,"PDMT","09","(18+03.65-L-)"]
["","","","","","3","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1980241.65,"BR01","X131",0.03,null,"12",null,54.333300000000001,"572","A",1,41,160,"PDMT","09","(18+03.65-L-)"]
["","","","","C204109-TC","1","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",117808.25,"RW1","I000",null,3,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204109-UT","2","FORSYTH","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",348497,"RW1","NPAR",null,3,"",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",5359379.08,"","",0.20899999999999999,null,"",null,null,"","",null,null,null,"","",""]
["","13","U-5604","C204216","C204216-RW","1","MACON","WATSON CONTRACTING INC",5391576.6500000004,"RW1","",0.49099999999999999,4,"M720",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204216-ST","1","MACON","WATSON CONTRACTING INC",31950,"WL1","Y007",null,null,"W005",5.68,null,"","",null,null,null,"V MTN","14","(36+50.00-L-)"]
["","","","","","2","MACON","WATSON CONTRACTING INC",44100,"WL2","Y007",null,null,"W005",4.3600000000000003,null,"","",null,null,null,"V MTN","14","(40+50.00-L-)"]
["","","","","","3","MACON","WATSON CONTRACTING INC",320000,"WL3","Y007",null,null,"W001",7.23,null,"","",null,null,null,"V MTN","14","(39+50.00-L-)"]
["","","","","","","","Result",5787626.6500000004,"","",0.49099999999999999,null,"",null,null,"","",null,null,null,"","",""]
["10/30/2018","1","I-3819B","C204163","C204163-RW","1","IREDELL","THE LANE CONSTRUCTION CORPORATION",260290000,"RW1","I000",4,6,"M713",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",260290000,"","",4,null,"",null,null,"","",null,null,null,"","",""]
["11/9/2018","1","","C204282","C204282-RW","1","NEW HANOVER","S T WOOTEN CORPORATION",2302340.9,"RW1","I000",0.123,5,"",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204282-ST","1","NEW HANOVER","S T WOOTEN CORPORATION",3153519.59,"BR01","X081",0.106,null,"15",null,37.25,"745","A",7,34,561.83330000000001,"COAST","03","(606+95.00-L-)RT"]
["","","","","","2","NEW HANOVER","S T WOOTEN CORPORATION",2520095.34,"BR02","X081",null,null,"15",null,37.25,"745","A",7,34,561.83330000000001,"COAST","03","(606+95.00-L-)LT"]
["","","","","","","","Result",7975955.8300000001,"","",0.22900000000000001,null,"",null,null,"","",null,null,null,"","",""]
["11/20/2018","2","R-5734A","C204130","C204130B-RW","1","MACON","BUCHANAN AND SONS INC",11275534.65,"RW1","",1.0469999999999999,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204130B-SG","1","MACON","BUCHANAN AND SONS INC",1066041.75,"RW1","",null,2,"",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204130B-ST","1","MACON","BUCHANAN AND SONS INC",81582.7,"CV01","X928",null,8.81,"C201",42,5,"","",null,null,null,"V MTN","14","(19+20.00-L-)"]
["","","","","","2","MACON","BUCHANAN AND SONS INC",158950,"WL1","Y007",null,null,"W001",35.67,null,"","",null,null,null,"V MTN","14","(13+50.00-Y1-)"]
["","","","","","3","MACON","BUCHANAN AND SONS INC",20935.099999999999,"BR01","Y007",null,null,"15",null,null,"","",5,null,null,"V MTN","14","(42+00.00-L-)"]
["","","","","","","","Result",12603044.199999999,"","",1.0469999999999999,null,null,null,null,"","",null,null,null,"","",""]
["","","","C204130","C204130A-RW","1","MACON","BUCHANAN AND SONS INC",672402,"RW1","",4.7E-2,2,"B810",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204130A-ST","1","MACON","BUCHANAN AND SONS INC",757358.8,"BR01","X080",1.9E-2,null,"15",null,33,"733","A",1,25.041699999999999,102.3229,"V MTN","14","(14+94.00-L-)"]
["","","","","","","","Result",1429760.8,"","",6.6000000000000003E-2,null,"",null,null,"","",null,null,null,"","",""]
["","3","","C204271","C204271A-RW","1","ONSLOW","ONSLOW GRADING & PAVING INC",1964165.38,"RW1","",2.98,5,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","C204271B-RW","1","ONSLOW","ONSLOW GRADING & PAVING INC",6693150.0800000001,"RW1","",33.53,5,"R000",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",8657315.4600000009,"","",36.51,10,"",null,null,"","",null,null,null,"","",""]
["","4","B-4833","C204263","C204263-RW","1","WAKE","NATIONAL BRIDGE BUILDERS LLC",710304.3,"RW1","C000",0.245,2,"B810",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","C204263-ST","1","WAKE","NATIONAL BRIDGE BUILDERS LLC",369881.5,"BR01","X080",1.4E-2,null,"15",null,33,"722","A",1,30.833300000000001,72.25,"PDMT","05","(18+64.00 -L-)"]
["","","","","","","","Result",1080185.8,"","",0.25900000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C204267","C204267A-RW","1","PERSON","CAROLINA SUNROCK LLC",4123554.26,"RW1","",25.61,2,"R000",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",4123554.26,"","",25.61,null,"",null,null,"","",null,null,null,"","",""]
["","6","I-5952","C204175","C204175-RW","1","FORSYTH","SHARPE BROTHERS A  DIVISION OF VECELLIO",17558977.210000001,"RW1","I000",6.226,6,"RH11",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",17558977.210000001,"","",6.226,null,"",null,null,"","",null,null,null,"","",""]
["","7","W-5212N","C204262","C204262-RW","1","GASTON","SLOAN CONSTRUCTION A DIVISION OF REEVES",15644746.529999999,"RW1","I000",7.8440000000000003,3,"D300",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","C204262-ST","1","GASTON","SLOAN CONSTRUCTION A DIVISION OF REEVES",133039.20000000001,"CV01","Y007",6.0000000000000001E-3,16,"C203",24.5,9,"","",null,null,null,"PDMT","12","(42+19.00-L-)"]
["","","","","","2","GASTON","SLOAN CONSTRUCTION A DIVISION OF REEVES",75912.7,"CV02","Y007",null,15,"C202",25,7,"","",null,null,null,"PDMT","12","(324+60.00-L-)"]
["","","","","","","","Result",15853698.43,"","",7.85,null,"",null,null,"","",null,null,null,"","",""]
["","8","","C204232","C204232-ST","1","MADISON","SOUTHERN ROAD & BRIDGE LLC",433274.7,"BR01","X031",0.08,null,"15",null,38,"555","I",3,36,316,"V MTN","13","BRIDGE NO. 560093"]
["","","","","","2","MADISON","SOUTHERN ROAD & BRIDGE LLC",912011.05,"BR02","X031",0.13,null,"15",null,32.833300000000001,"336","N",7,30,560,"V MTN","13","BRIDGE NO. 560113"]
["","","","","","3","MADISON","SOUTHERN ROAD & BRIDGE LLC",1446564,"BR03","X031",0.14000000000000001,null,"17",null,63.083300000000001,"572","Q",4,60,618,"V MTN","13","BRIDGE NO. 600247"]
["","","","","C204232-TC","1","MADISON","SOUTHERN ROAD & BRIDGE LLC",666871,"RW1","",null,2,"M720",null,null,"","",null,null,null,"V MTN","13",""]
["","","","","","","","Result",3458720.75,"","",0.35,null,"",null,null,"","",null,null,null,"","",""]
["","9","R-2828","C204197","C204197-RW","1","WAKE","THE LANE BLYTHE CONSTRUCTION JV",403200000,"RW1","",8.6170000000000009,6,"M713",null,null,"","",null,null,null,"PDMT","05",""]
["","","","","","","","Result",403200000,"","",8.6170000000000009,null,"",null,null,"","",null,null,null,"","",""]
["","10","B-4974","C204259","C204259B-RW","1","STANLY","PCL CIVIL CONSTRUCTORS INC",15927850,"RW1","",0.32700000000000001,2,"M713",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",15927850,"","",0.32700000000000001,null,"",null,null,"","",null,null,null,"","",""]
["","","","C204259","C204259A-RW","1","STANLY","PCL CIVIL CONSTRUCTORS INC",4226278,"RW1","",0.32700000000000001,2,"M713",null,null,"","",null,null,null,"PDMT","10",""]
["","","","","","","","Result",4226278,"","",0.32700000000000001,null,"",null,null,"","",null,null,null,"","",""]
["12/18/2018","1","F-5703A","C204260","C204260-FE","1","DARE","SHARKTECH ALABAMA DBA METAL SHARK BOATS",5217228,"RW1","Y219",null,null,"M702",null,null,"","",null,null,null,"COAST","01",""]
["","","","","","","","Result",5217228,"","",null,null,"",null,null,"","",null,null,null,"","",""]
["","3","W-5602","C204264","C204264-RW","1","ONSLOW","WELLS BROTHERS CONSTRUCTION COMPANY INC",12199566.800000001,"RW1","I000",2.7040000000000002,3,"D340",null,null,"","",null,null,null,"COAST","03",""]
["","","","","","","","Result",12199566.800000001,"","",2.7040000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","5","","C204268","C204268A-RW","1","DAVIDSON","J T RUSSELL & SONS INC",5848557.3499999996,"RW1","",18.096,4,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204268B-RW","1","DAVIDSON","J T RUSSELL & SONS INC",6259482.75,"RW1","",36.387999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",12108040.1,"","",54.484000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","6","","C204278","C204278A-RW","1","FORSYTH","APAC - ATLANTIC INC THOMPSON ARTHUR DIVI",9549724.4299999997,"RW1","",13.162000000000001,4,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204278B-RW","1","FORSYTH","APAC - ATLANTIC INC THOMPSON ARTHUR DIVI",2621746.2400000002,"RW1","",7.6429999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",12171470.67,"","",20.805,null,"",null,null,"","",null,null,null,"","",""]
["","7","","C204269","C204269A-RW","1","ROWAN","J T RUSSELL & SONS INC",934796.23,"RW1","",3.863,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","C204269B-RW","1","ROWAN","J T RUSSELL & SONS INC",4816118.26,"RW1","",21.98,2,"R000",null,null,"","",null,null,null,"PDMT","09",""]
["","","","","","","","Result",5750914.4900000002,"","",25.843,null,"",null,null,"","",null,null,null,"","",""]
["","8","B-5388","C204255","C204255-EC","1","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",207196.55,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C204255-RW","1","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",1448895.22,"RW1","",0.223,2,"B812",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C204255-SI","1","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",21792.35,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","C204255-ST","1","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",96558,"WL1","Y007",null,null,"W001",8.89,null,"","",null,null,null,"MTN","11","(16+01.36 -L-)"]
["","","","","","2","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",168210.99,"WL2","Y007",null,null,"W001",6.47,null,"","",null,null,null,"MTN","11","(21+50.00-L-)"]
["","","","","","3","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",2863031.43,"BR01","X081",5.9799999999999999E-2,null,"15",null,34.583300000000001,"764","Q",3,32,315.79169999999999,"MTN","11","(19+78.50 -L-)"]
["","","","","C204255-TC","1","ALLEGHANY","JAMES R VANNOY & SONS CONSTRUCTION COMPA",38615.379999999997,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
["","","","","","","","Result",4844299.92,"","",0.2828,null,"",null,null,"","",null,null,null,"","",""]
["","9","","C204234","C204234-ST","1","GASTON","LANFORD BROTHERS CO INC",360850.47,"BR01","X281",4.3999999999999997E-2,null,"11",null,28.416699999999999,"745","I",4,24,234,"PDMT","12","BRIDGE NO. 39"]
["","","","","C204234-TC","1","GASTON","LANFORD BROTHERS CO INC",41755.4,"RW1","I000",null,4,"M720",null,null,"","",null,null,null,"PDMT","12",""]
["","","","","","","","Result",402605.87,"","",4.3999999999999997E-2,null,"",null,null,"","",null,null,null,"","",""]
["","10","U-5833","C204228","C204228-RW","1","RUTHERFORD","SITE DEVELOPMENT CORPORATION",5166542.62,"RW1","",0.64600000000000002,3,"D300",null,null,"","",null,null,null,"MTN","13",""]
["","","","","","2","RUTHERFORD","SITE DEVELOPMENT CORPORATION",28069.18,"RW1","",null,3,"D300",null,null,"","",null,null,null,"MTN","13",""]
["","","","","C204228-ST","1","RUTHERFORD","SITE DEVELOPMENT CORPORATION",85245.2,"WL1","Y007",null,null,"W005",4.6500000000000004,null,"","",null,null,null,"MTN","13","(41+53.66-L-)"]
["","","","","","","","Result",5279857,"","",0.64600000000000002,null,"",null,null,"","",null,null,null,"","",""]
["","11","","C204233","C204233-ST","1","CHEROKEE","BUCKEYE BRIDGE LLC",1037409.5,"BR01","X031",0.09,null,"15",null,42.5,"551","I",5,40,476,"V MTN","14","BRIDGE NO. 31"]
["","","","","","2","CHEROKEE","BUCKEYE BRIDGE LLC",1120556.5,"BR02","X031",0.09,null,"15",null,42.5,"552","I",5,40,476,"V MTN","14","BRIDGE NO. 33"]
["","","","","C204233-TC","1","CHEROKEE","BUCKEYE BRIDGE LLC",275712.5,"RW1","",null,4,"M720",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","","","Result",2433678.5,"","",0.18,null,"",null,null,"","",null,null,null,"","",""]
["","12","U-5840","C204214","C204214-RW","1","HENDERSON","NHM CONSTRUCTORS LLC",8054569.2300000004,"RW1","",1.028,6,"D340",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","","2","HENDERSON","NHM CONSTRUCTORS LLC",573783.55000000005,"RW1","",null,6,"D340",null,null,"","",null,null,null,"V MTN","14",""]
["","","","","C204214-ST","1","HENDERSON","NHM CONSTRUCTORS LLC",221419.1,"CV01","X994",null,7.21,"C005",90,9.5832999999999995,"","",null,null,null,"V MTN","14","(22+17.00-Y7-)"]
["","","","","","2","HENDERSON","NHM CONSTRUCTORS LLC",8568.4,"WL1","Y007",null,null,"W005",1.55,null,"","",null,null,null,"V MTN","14","(10+00.00-W1-)"]
["","","","","","3","HENDERSON","NHM CONSTRUCTORS LLC",29643.9,"WL2","Y007",null,null,"W005",2.74,null,"","",null,null,null,"V MTN","14","(10+00.00-W2-)"]
["","","","","","4","HENDERSON","NHM CONSTRUCTORS LLC",106448.8,"WL3","Y007",null,null,"W001",4.95,null,"","",null,null,null,"V MTN","14","(10+00.00-W3-)"]
["","","","","","5","HENDERSON","NHM CONSTRUCTORS LLC",73724.2,"WL4","Y007",null,null,"W001",5.34,null,"","",null,null,null,"V MTN","14","(10+00.00-W4-)"]
["","","","","","","","Result",9068157.1799999997,"","",1.028,null,"",null,null,"","",null,null,null,"","",""]
[null,null,null,"","","","","Result",4828931704.6099997,"","",2332.6,null,"",null,null,"","",null,null,null,"","",""]

{"sheet":"ITEMS - STATEWIDE","index":1,"n_rows":2252,"n_cols":7,"rows_kept":2252,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - STATEWIDE"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",144,491713.19333333301,70806699.840000004]
["0000400000-N","CONST SURVEYING","","",58,109165.186724138,6331580.8300000001]
["0000500000-N","SUPP FIELD SURVEYING","","",100,108,10800]
["0000600000-N","SUPP SURVEYING OFF CALC","","",30,140,4200]
["0000700000-N","FIELD OFFICE","","",3,94172.72,282518.15999999997]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","CONSTRUCTION SURVEYING","",1,65000,65000]
["","","DESIGN & CONSTRUCTION","",1,360175000,360175000]
["","","DESIGN & CONSTRUCTION OF","BRIDGE",1,415403.74,415403.74]
["","","","BRIDGES",3,1979800.93,5939402.79]
["","","","CULVERT 040023",1,972400,972400]
["","","","CULVERT 940278",1,1440661,1440661]
["","","DESIGN AND CONSTRUCTION","",2,271989000,543978000]
["","","DESIGN AND CONSTRUCTION 15BPR.43","",1,4101260,4101260]
["","","DESIGN AND CONSTRUCTION B-4974","",1,15927850,15927850]
["","","DESIGN AND CONSTRUCTION U-2719","",1,311688512,311688512]
["","","DESIGN AND CONSTRUCTION U-4437","",1,34511488,34511488]
["","","DESIGN SUPPORT","",1,94300,94300]
["","","INTERIOR BENT CAPS","STRUCTURE 250211",1,20000,20000]
["","","MOBILIZATION","",1,449500,449500]
["","","REMOVE & STOCKPILE TEMPORARY BRIDGE","",1,200000,200000]
["","","UTILITY COORDINATOR","",1,289000,289000]
["0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","BOA MOBILIZATION","",4,20088,80352]
["","","END BENTS STRUCTURE 040177","",2,96335.87,192671.74]
["","","END BENTS STRUCTURE 100088","",2,62000,124000]
["","","END BENTS STRUCTURE 100099","",2,45000,90000]
["","","END BENTS STRUCTURE 100100","",2,42000,84000]
["","","END BENTS STRUCTURE 110126","",2,30000,60000]
["","","END BENTS STRUCTURE 130115","",2,26690.23,53380.46]
["","","END BENTS STRUCTURE 250211","",2,20000,40000]
["","","END BENTS STRUCTURE 580108","",2,36000,72000]
["","","END BENTS STRUCTURE 600157","",2,70000,140000]
["","","END BENTS STRUCTURE 800058","",2,31000,62000]
["","","END BENTS STRUCTURE 800088","",2,41000,82000]
["","","END BENTS STRUCTURE 800265","",2,28500,57000]
["","","END BENTS STRUCTURE 850012","",2,23216.99,46433.98]
["","","END BENTS STRUCTURE 980020","",2,22409.58,44819.16]
["","","INTERIOR BENT CAPS STRUCTURE 580108","",2,36000,72000]
["","","INTERIOR BENT CAPS STRUCTURE 800058","",1,34000,34000]
["","","INTERIOR BENT CAPS STRUCTURE 850012","",1,51153.42,51153.42]
["","","INTERIOR BENT CAPS STRUCTURE 980020","",1,49044.79,49044.79]
["","","RIGHT OF WAY ACQUISITION","",31,4938.3638709677398,153089.28]
["0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT 1 STRUCTURE 040177",28,419.56,11747.68]
["","","","BENT 1 STRUCTURE 100088",10,4500,45000]
["","","","BENT 1 STRUCTURE 100099",28,0.01,0.28000000000000003]
["","","","BENT 1 STRUCTURE 100100",19,0.01,0.19]
["","","","BENT 1 STRUCTURE 110126",35,190,6650]
["","","","BENT 1 STRUCTURE 130115",26,433.15,11261.9]
["","","","BENT 1 STRUCTURE 250211",45,210,9450]
["","","","BENT 1 STRUCTURE 580108",11,2675,29425]
["","","","BENT 1 STRUCTURE 600157",20,0.01,0.2]
["","","","BENT 1 STRUCTURE 800058",14,252.5,3535]
["","","","BENT 1 STRUCTURE 800088",30,175,5250]
["","","","BENT 1 STRUCTURE 800265",18,255,4590]
["","","","BENT 1 STRUCTURE 850012",36,329.86,11874.96]
["","","","BENT 1 STRUCTURE 980020",15,2273.88,34108.199999999997]
["","","","BENT 2 STRUCTURE 040177",18,537.47,9674.4599999999991]
["","","","BENT 2 STRUCTURE 100088",26,0.01,0.26]
["","","","BENT 2 STRUCTURE 100099",33,0.01,0.33]
["","","","BENT 2 STRUCTURE 100100",15,0.01,0.15]
["","","","BENT 2 STRUCTURE 110126",27,190,5130]
["","","","BENT 2 STRUCTURE 130115",22,429.94,9458.68]
["","","","BENT 2 STRUCTURE 250211",45,210,9450]
["","","","BENT 2 STRUCTURE 580108",27,320,8640]
["","","","BENT 2 STRUCTURE 600157",29,0.01,0.28999999999999998]
["","","","BENT 2 STRUCTURE 800058",20,252.5,5050]
["","","","BENT 2 STRUCTURE 800088",17,217,3689]
["","","","BENT 2 STRUCTURE 800265",17,252.5,4292.5]
["","","","BENT 2 STRUCTURE 850012",47,299.66000000000003,14084.02]
["","","","BENT 2 STRUCTURE 980020",22,427.89,9413.58]
["","","AVE FOUNDATION LENGTH AT INTE-","RIOR BENT 1 STRUCTURE 580108",29,3000,87000]
["","","","RIOR BENT 1 STRUCTURE 800058",27,2285,61695]
["","","","RIOR BENT 1 STRUCTURE 850012",60,1654.09,99245.4]
["","","","RIOR BENT 1 STRUCTURE 980020",30,2225.87,66776.100000000006]
["","","","RIOR BENT 2 STRUCTURE 580108",29,3000,87000]
["","","","RIOR BENT STRUCTURE 250211",55,450,24750]
["","","BRIDGE LENGTH","STRUCTURE 250211",100,3500,350000]
["","","BRIDGE LENGTH STRUCTURE 040177","",60,2303.38,138202.79999999999]
["","","BRIDGE LENGTH STRUCTURE 100088","",70,3005,210350]
["","","BRIDGE LENGTH STRUCTURE 100099","",50,3000,150000]
["","","BRIDGE LENGTH STRUCTURE 100100","",70,3100,217000]
["","","BRIDGE LENGTH STRUCTURE 110126","",60,1555,93300]
["","","BRIDGE LENGTH STRUCTURE 130115","",70,2476.13,173329.1]
["","","BRIDGE LENGTH STRUCTURE 580108","",170,1730,294100]
["","","BRIDGE LENGTH STRUCTURE 600157","",50,2800,140000]
["","","BRIDGE LENGTH STRUCTURE 800058","",120,2215,265800]
["","","BRIDGE LENGTH STRUCTURE 800088","",100,2750,275000]
["","","BRIDGE LENGTH STRUCTURE 800265","",60,1455,87300]
["","","BRIDGE LENGTH STRUCTURE 850012","",130,2592.1999999999998,336986]
["","","BRIDGE LENGTH STRUCTURE 980020","",115,1824.59,209827.85]
["0000960000-E","GENERIC MISCELLANEOUS ITEM (SY)","PAVEMENT REPLACEMENT","",156000,175,27300000]
["0000996000-N","DESIGN AND CONST","DESIGN & CONSTRUCTION","",1,17300000,17300000]
["","","","",3,246813333.33333299,740440000]
["0001000000-E","CLEARING & GRUBBING","","",407,69295.551118210904,28196359.75]
["0001010000-N","SELECT TREE REMOVAL","","",1,5000,5000]
["0005000000-N","GENERIC FERRY ITEM (LS)","CONSTR 70'-6\" X 30' X 11'","SOUND CLASS TUG",1,5217228,5217228]
["","","CONSTRUCT 183'-7\" X 46' X 11'","PASSENGER/VEHICLE FERRY \"H\"",1,11883016.52,11883016.52]
["0008000000-E","SUPP CLEARING & GRUBBING","","",39,6037.4074358974403,235458.89]
["0015000000-N","SEALING ABANDONED WELLS","","",31,2117.7825806451601,65651.259999999995]
["0022000000-E","UNCLAS EXCAVATION","","",4268189,7.0334158585760802,30019948.199999999]
["0028000000-N","TYPE I STANDARD APPR **********","(14+21.00)","",1,11800,11800]
["","","(14+97.65 -Y8-)","",1,49875,49875]
["","","(140+21.50 -L- LT)","",1,69675,69675]
["","","(140+21.50 -L- RT)","",1,64375,64375]
["","","(155+02.50 -L- LT)","",1,69675,69675]
["","","(155+02.50 -L- RT)","",1,64500,64500]
["","","(19+78.50-L-)","",1,17855.189999999999,17855.189999999999]
["","","(22+16.89 -L-)","",1,35720,35720]
["","","(227+33.50)","",1,48000,48000]
["","","(23+20 -L-)","",1,40000,40000]
["","","(23+26.00 -L- EB)","",1,31000,31000]
["","","(23+26.00 -L- WB)","",1,31000,31000]
["","","(25+00)","",1,35000,35000]
["","","(25+52.71 -Y7-)","",1,60500,60500]
["","","(26+20.73 -YEB-)","",1,66287.490000000005,66287.490000000005]
["","","(28+26.49 WB)","",1,140000,140000]
["","","(28+45.42 EB)","",1,140000,140000]
["","","(30+02)","",1,41500,41500]
["","","(337+20.09 -L- LT)","",1,66100,66100]
["","","(337+20.09 -L- RT)","",1,66100,66100]
["","","(38+35.00)","",1,43600,43600]
["","","(50+61.09 -L-)","",1,97000,97000]
["","","(55+88.11 -L-)","",1,100000,100000]
["","","(606+95 -L- LT)","",1,53200,53200]
["","","(606+95 -L- RT)","",1,53200,53200]
["","","(64+20 -L-)","",1,80000,80000]
["","","(93+43.36 -L- LT)","",1,35500,35500]
["","","(93+43.36 -L- RT)","",1,35500,35500]
["0029000000-N","TYPE III REINF APPR **********","(12+68.00 -L-)","",1,15000,15000]
["","","(15+56.00 -L-)","",1,15000,15000]
["","","(17+37.28 -Y16-)","",1,69100,69100]
["","","(18+03.65)","",1,78000,78000]
["","","(19+45.50 -L-)","",1,15000,15000]
["","","(21+10.00 -L-)","",1,38000,38000]
["","","(22+29.98 -Y5-)","",1,82700,82700]
["","","(28+98.81 -Y4-)","",1,135500,135500]
["","","(329+95.42 -L- LT)","",1,89600,89600]
["","","(329+95.42 -L- RT)","",1,89600,89600]
["","","(470+43.12 -L- LT)","",1,96200,96200]
["","","(470+43.12 -L- RT)","",1,90900,90900]
["","","(93+43.36 -L- LT)","",1,29400,29400]
["","","(93+43.36 -L- RT)","",1,30200,30200]
["0030000000-N","TYPE II MOD APPR **********","(10+53.50)","",1,24000,24000]
["","","(13+25 -L-)","",1,10000,10000]
["","","(13+52 -L-)","",1,7500,7500]
["","","(13+70 -L-)","",1,6000,6000]
["","","(13+86 -L-)","",1,18500,18500]
["","","(14+27 -L-)","",1,22000,22000]
["","","(14+67.00)","",1,12000,12000]
["","","(14+94.00 -L-)","",1,15000,15000]
["","","(15+14.00)","",1,14468,14468]
["","","(15+54.50 -L-)","",1,15000,15000]
["","","(15+98.00)","",1,12500,12500]
["","","(18+62.50 -L-)","",1,12500,12500]
["","","(18+64.00 -L-)","",1,10000,10000]
["","","(28+17.37-Y-)","",1,2265.62,2265.62]
["","","(38+62.00)","",1,8580,8580]
["","","(99+17.60 -L1-)","",1,25000,25000]
["0036000000-E","UNDERCUT EXCAVATION","","",277250,7.0361429756537399,1950770.64]
["0043000000-N","GRADING","","",31,541092.51451612904,16773867.949999999]
["0050000000-E","SUPP CLEARING & GRUBBING","","",38,2549.2007894736798,96869.63]
["0057000000-E","UNDERCUT EXCAVATION","","",81600,12.7410661764706,1039671]
["0063000000-N","GRADING","","",5,707763,3538815]
["0106000000-E","BORROW EXCAVATION","","",6024308,2.4022176073998902,14471698.75]
["0127000000-N","EMBM'T SETTLEMENT GAUGE","","",9,671.25555555555604,6041.3]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",144367,6.6862627193195099,965275.69]
["0141000000-E","BERM DITCH CONST","","",15680,3.2342793367346898,50713.5]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",269796.59999999998,7.7225265255381297,2083511.4]
["0163000000-E","REMOVAL OF EXT CONC PVMT","","",106,56.792452830188701,6020]
["0170000000-E","REMOVAL OF CONC PVMT SLBS","","",4600,100,460000]
["0177000000-E","BREAKING OF EXT ASPH PVMT","","",32996.6,3.6507397731887501,120462]
["0185000000-E","BREAKING OF EXT CONC PVMT","","",880,31,27280]
["0192000000-N","PROOF ROLLING","","",451,211.57450110864701,95420.1]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",103410,30.457884150468999,3149649.8]
["0195000000-E","SELECT GRANULAR MAT'L","","",233365,11.248418786021899,2624987.25]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",489452,1.7787233886060301,870599.72]
["0199000000-E","TEMP SHORING","","",67997,44.427660337956098,3020947.62]
["0220000000-E","ROCK EMBANKMENTS","","",18410,38.531439435089602,709363.8]
["0222000000-E","GEOTEXTILE ROCK EMBANK","","",9870,2.2170010131712301,21881.8]
["0223000000-E","ROCK PLATING","","",7440,61.988407258064498,461193.75]
["0225000000-E","REINF SOIL SLOPES","","",5980,78.016722408026794,466540]
["0234000000-E","GENERIC GRADING ITEM (CY)","CLASS II, TYPE 2","GRANULAR SOIL",5500,18.850000000000001,103675]
["","","HAULING & DISPOSAL OF CONTAMI-NATED SOIL","",440,135,59400]
["","","SHALLOW UNDERCUT","",4422,11.8,52179.6]
["0241000000-E","GENERIC GRADING ITEM (SY)","7\" TRENCHING FOR SHOULDER","CONSTRUCTION",31443,12,377316]
["","","8\" TRENCHING FOR SHOULDER","CONSTRUCTION",74848,13.5,1010448]
["","","GEOCELLS","",3850,45.4,174790]
["","","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",7860,4.5999363867684497,36155.5]
["","","SOIL CEMENT BASE (FULL DEPTH","RECLAMATION)",91694,3.1020355748467701,284438.05]
["0245000000-E","GENERIC GRADING ITEM (GAL)","FOAM INSTALLATION SOIL STABI- LIZATION","",2085,69,143865]
["","","HAULING & DISPOSAL OF CONTAMI-","NATED GROUND WATER",1000,1,1000]
["0248000000-N","GENERIC GRADING ITEM (LS)","CHANNEL BLOCK","",1,1652.64,1652.64]
["","","DRY DETENTION BASIN 1","",1,2902.87,2902.87]
["","","DRY DETENTION BASIN 2","",1,3977.61,3977.61]
["","","DRY DETENTION BASIN (NO 1)","",1,28000,28000]
["","","DRY DETENTION BASIN (NO 8)","",1,35000,35000]
["","","FILTRATION BASIN 1","",1,77877.009999999995,77877.009999999995]
["","","FILTRATION BASIN 2","",1,102117.45,102117.45]
["","","INSTRUMENTATION INSTALLATION","ASSIST AT STR 7 (BR 1246) - END BENT 1",1,2000,2000]
["","","","ASSIST AT STR 7 (BR 1246) - END BENT 2",1,2000,2000]
["","","INSTRUMENTATION INSTALLATION ASSIST AT","STRS 2 & 3 (BR 1241 & 1242) - END BENT 1",1,4000,4000]
["","","","STRS 2 & 3 (BR 1241 & 1242) - END BENT 2",1,4000,4000]
["","","MEDIA FILTER BASIN (NO 2)","",1,60000,60000]
["","","MEDIA FILTER BASIN (NO 3)","",1,40000,40000]
["","","MEDIA FILTER BASIN (NO 4)","",1,51500,51500]
["","","MEDIA FILTER BASIN (NO 5)","",1,40000,40000]
["","","MEDIA FILTER BASIN (NO 6)","",1,57500,57500]
["","","MEDIA FILTER BASIN (NO 7)","",1,90500,90500]
["","","MEDIA FILTER BASIN (NO 9)","",1,72500,72500]
["","","MEDIA FILTER BASIN NO 1","",1,39000,39000]
["","","MEDIA FILTER BASIN NO 2","",1,65000,65000]
["","","REMOVAL & DISPOSAL OF 5 FOAM","FILLED USTS",1,16500,16500]
["","","SELECT DEMOLITION OF CONCRETE","SHEET PILE WALL",1,107500,107500]
["","","SELECT DEMOLITION OF CRIB WALL","",1,22089,22089]
["","","SETTLEMENT MONITORING ASSIST","AT STR 7 (BR 1246) - END BENT 1",1,1000,1000]
["","","","AT STR 7 (BR 1246) - END BENT 2",1,1000,1000]
["","","SETTLEMENT MONITORING ASSIST AT STRS 2","& 3 (BR 1241 & 1242) - END BENT 1",1,2000,2000]
["","","","& 3 (BR 1241 & 1242) - END BENT 2",1,2000,2000]
["","","SITE GRADING","",1,7125750,7125750]
["0255000000-E","GENERIC GRADING ITEM (TON)","CLASS IV SUBGRADE STABILIZA- TION","",41721,30,1251630]
["","","EARTH MOUND","",5,843,4215]
["","","FLY ASH HAULING AND DISPOSAL","",2405,77.5,186387.5]
["","","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",400,113.0825,45233]
["","","HAULING AND DISPOSAL OF","CONTAMINATED SOIL",4555,54,245970]
["","","","PETROLEUM CONTAMINATED SOIL",1602,81.318039950062399,130271.5]
["","","HAULING AND DISPOSAL OF PETR-","OLEUM CONTAMINATED SOIL",100,114,11400]
["","","REPAIR EXISTING AGGREGATE BASECOURSE","",15,108.19,1622.85]
["","","STOCKPILING PETROLEUM CONTAMI-NATED SOIL","",3000,6.75,20250]
["","","SURGE STONE","",200,69,13800]
["0257000000-E","GENERIC GRADING ITEM (LF)","RAILROAD SIGNAL CONDUIT","",3000,17,51000]
["0264000000-E","GENERIC GRADING ITEM (SMI)","MEDIAN SHOULDER RECONSTRUC- TION (T1)","",63.35,2500,158375]
["","","OUTSIDE SHOULDER RECONSTRUC- TION (T2)","",50.57,3300,166881]
["","","SHOULDER GRADING","",513.5,2119.9533787731302,1088596.06]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",48907,34.297157871061401,1677371.1]
["0320000000-E","FND CONDIT GEOTEXTILE","","",165933,2.2735845793181602,377262.71]
["0335000000-E","**\" DRAINAGE PIPE","(54\")","",108,240.76851851851899,26003]
["","","(60\")","",264,305,80520]
["","","(66\")","",456,363,165528]
["","","(8\")","",178,39.269662921348299,6990]
["0335100000-E","12\" DRAINAGE PIPE","","",28,33,924]
["0335200000-E","15\" DRAINAGE PIPE","","",11940,43.396512562814102,518154.36]
["0335300000-E","18\" DRAINAGE PIPE","","",5000,50.297111999999998,251485.56]
["0335400000-E","24\" DRAINAGE PIPE","","",3080,59.312389610389602,182682.16]
["0335500000-E","30\" DRAINAGE PIPE","","",1772,77.664988713318294,137622.35999999999]
["0335600000-E","36\" DRAINAGE PIPE","","",1532,87.264673629242793,133689.48000000001]
["0335700000-E","42\" DRAINAGE PIPE","","",988,113.245020242915,111886.08]
["0335800000-E","48\" DRAINAGE PIPE","","",56,132,7392]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",56,371.474285714286,20802.560000000001]
["","","(15)","",4,125,500]
["","","(18\")","",20,374.2,7484]
["","","(24\")","",5,407.072,2035.36]
["0342000000-E","**\" SIDE DRAIN PIPE","(12\")","",16,52.04,832.64]
["","","(30\")","",3316,97.006767189384803,321674.44]
["","","(36\")","",284,118.7,33710.800000000003]
["","","(42\")","",320,117.346875,37551]
["","","(48\")","",80,133.19,10655.2]
["","","(54\")","",44,278.2,12240.8]
["0343000000-E","15\" SIDE DRAIN PIPE","","",22492,49.0589205050685,1103433.24]
["0344000000-E","18\" SIDE DRAIN PIPE","","",8546,51.543079803416802,440487.16]
["0345000000-E","24\" SIDE DRAIN PIPE","","",7464,67.932073954983906,507045]
["0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",23,338.43652173913,7784.04]
["","","(18\")","",14,643.42999999999995,9008.02]
["","","(24\")","",4,318.54000000000002,1274.1600000000001]
["","","(30\")","",8,412.53,3300.24]
["0350000000-E","***\" RC PIPE CULV, CONTR DESIGN","(24\")","",1696,169.8,287980.79999999999]
["","","(36\")","",752,199.83079787234001,150272.76]
["","","(42\")","",732,273.97333333333302,200548.48000000001]
["","","(48\")","",124,322.2,39952.800000000003]
["","","(54\")","",860,359.2,308912]
["0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",18876,48.504810341174,915576.8]
["","","(18\", V)","",3280,57.3423902439024,188083.04]
["","","(24\", V)","",3632,77.792466960352399,282542.24]
["","","(30\", V)","",1296,108.02160493827201,139996]
["","","(36\", V)","",212,239.06,50680.72]
["","","(42\", V)","",144,221.45,31888.799999999999]
["","","(66\", V)","",716,460.35888268156401,329616.96000000002]
["0366000000-E","15\" RC PIPE CULV III","","",26972,53.626758119531402,1446420.92]
["0372000000-E","18\" RC PIPE CULV III","","",14409,54.800011104170999,789613.36]
["0378000000-E","24\" RC PIPE CULV III","","",12708,69.073657538558393,877788.04]
["0384000000-E","30\" RC PIPE CULV III","","",9336,76.220865467009403,711598]
["0390000000-E","36\" RC PIPE CULV III","","",8322,103.595962509012,862125.6]
["0396000000-E","42\" RC PIPE CULV III","","",1836,136.31054466230901,250266.16]
["0402000000-E","48\" RC PIPE CULV III","","",3312,150.160990338164,497333.2]
["0408000000-E","54\" RC PIPE CULV III","","",1996,254.01779559118199,507019.52000000002]
["0414000000-E","60\" RC PIPE CULV III","","",3728,251.355643776824,937053.84]
["0420000000-E","66\" RC PIPE CULV III","","",264,310,81840]
["0426000000-E","72\" RC PIPE CULV III","","",1970,330.791370558376,651659]
["0448000000-E","***\" RCP CULV CLASS IV","(12\")","",80,57,4560]
["","","(48\")","",2108,210.335863377609,443388]
["","","(54\")","",2104,267.476121673004,562769.76]
["","","(60\")","",1052,337.12167300380202,354652]
["","","(66\")","",244,564.36721311475401,137705.60000000001]
["","","(72\")","",424,444.43396226415098,188440]
["0448200000-E","15\" RCP CULV CLASS IV","","",80161,53.591031174760801,4295910.6500000004]
["0448300000-E","18\" RCP CULV CLASS IV","","",51238,58.290646395253503,2986696.14]
["0448400000-E","24\" RCP CULV CLASS IV","","",24923,80.897314127512701,2016203.76]
["0448500000-E","30\" RCP CULV CLASS IV","","",11963,103.810174705341,1241881.1200000001]
["0448600000-E","36\" RCP CULV CLASS IV","","",8028,135.57368211260601,1088385.52]
["0448700000-E","42\" RCP CULV CLASS IV","","",3208,169.12219451371601,542544]
["0450000000-E","***\" RC PIPE CULV ** (RR)","(72\", V)","",1200,413.65,496380]
["0453000000-E","**\" PIPE END SECTION","(15\")","",5,1322.4,6612]
["","","(18\")","",6,1050,6300]
["","","(24\")","",2,845,1690]
["","","(30\")","",5,970,4850]
["","","(36\")","",1,1645,1645]
["0536000000-E","***\" HDPE PIPE CULVTS","(12\")","",156,42,6552]
["","","(15\")","",280,46,12880]
["","","(18\")","",68,65,4420]
["","","(30\")","",432,97,41904]
["0546000000-E","**\" CAA PIPE CLVT *****\"","(18\", 0.064\")","",68,92,6256]
["0564000000-E","**\" CAA PIPE ELBOW *****\"","(18\", 0.064\")","",4,1600,6400]
["0570000000-E","6\" CS PIPE 0.064\" SPR BOX","","",24,50,1200]
["0576000000-E","**\" CS PIPE CULV *****\"","(36\", 0.079\")","",48,78,3744]
["","","(42\", 0.109\")","",112,134,15008]
["","","(48\", 0.109\")","",32,275,8800]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",6199,57.454921761574397,356163.06]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",2164,67.311737523105407,145662.6]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",1924,78.009979209979207,150091.20000000001]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",904,97.220796460176999,87887.6]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.0625\")","",1,368,368]
["","","(15\", 0.064\")","",138,452.75159420289901,62479.72]
["","","(15\", 0.064)","",2,125,250]
["","","(18\", 0.064\")","",37,543.55351351351396,20111.48]
["","","(24\", 0.064\")","",36,696.11111111111097,25060]
["","","(30\", 0.079\")","",18,889.1,16003.8]
["","","(42\", 0.109\")","",2,1465,2930]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\", 0.500\")","",38,315,11970]
["","","(18\", 0.500\")","",222,325,72150]
["","","(24\", 0.375\")","",83,255,21165]
["","","(24\", 0.500\")","",134,346,46364]
["","","(30\", 0.375\")","",205,305,62525]
["","","(30\", 0.500\")","",264,441,116424]
["","","(36\", 0.25\")","",108,399,43092]
["","","(36\", 0.500\")","",204,710.25,144891]
["","","(42\", 0.25\")","",76,501,38076]
["","","(42\", 0.500\")","",284,746,211864]
["","","(48\", 0.500\")","",36,809,29124]
["","","(54\", 0.750\")","",232,1145,265640]
["","","(66\", 0.750\")","",178,1357,241546]
["","","(72\", 0.750\")","",64,2315,148160]
["","","(84\", 0.750\")","",90,2503,225270]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\", 0.500\")","",38,525,19950]
["","","(18\", 0.500\")","",222,535.54999999999995,118892.1]
["","","(24\", 0.375\")","",83,1450,120350]
["","","(24\", 0.500\")","",134,640.79999999999995,85867.199999999997]
["","","(30\", 0.375\")","",205,1450,297250]
["","","(30\", 0.500\")","",264,935.4,246945.6]
["","","(36\", 0.25\")","",108,709,76572]
["","","(36\", 0.500\")","",204,1183,241332]
["","","(42\", 0.25\")","",76,829,63004]
["","","(42\", 0.500\")","",284,1167,331428]
["","","(48\", 0.500\")","",36,1230,44280]
["","","(54\", 0.750\")","",232,1610,373520]
["","","(66\", 0.750\")","",178,1820,323960]
["","","(72\", 0.750\")","",64,2880,184320]
["","","(84\", 0.750\")","",90,2587,232830]
["0974000000-E","**\"WLD STL PIPE ***\" B RR","(36\", 0.532\")","",68,650,44200]
["","","(54\", 0.750\")","",88,1420,124960]
["0986000000-E","GENERIC PIPE ITEM (LF)","15\" CURED IN PLACE PIPE","",106,132,13992]
["","","18\" CURED IN PLACE PIPE","",255,177,45135]
["","","24\" CURED IN PLACE PIPE","",155,268,41540]
["","","24\" DUCTILE IRON PIPE, CLASS 250","",144,147.09,21180.959999999999]
["","","30\" CURED IN PLACE PIPE","",185,285,52725]
["","","30\" HDPE PIPE CULVERTS WITH","WRAPPED JOINTS",436,80,34880]
["","","4\" PVC IRRIGATION CONDUIT","",588,24,14112]
["0987000000-E","GENERIC PIPE ITEM (LF) 310","15\" RC PIPE CULVERT, CLASS V","",40,38.549999999999997,1542]
["0995000000-E","PIPE REMOVAL","","",66307,19.8558660473253,1316582.9099999999]
["0996000000-N","PIPE CLEAN OUT","","",23,2880.96956521739,66262.3]
["1000000000-E","6\" SLOPE PROTECTION","","",390,100.769230769231,39300]
["1011000000-N","FINE GRADING","","",21,565175.563333333,11868686.83]
["1022000000-E","SEALING PVMT CRACKS","","",38900,5.1002570694087401,198400]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",401120,2.87390805743917,1152782]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",3800,205.432157894737,780642.2]
["1077000000-E","57 STONE","","",5515,28.6629918404352,158076.4]
["1099500000-E","SHALLOW UNDERCUT","","",83529,11.3627422811239,949118.5]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",342817,21.591943806753999,7402085.4000000004]
["1110000000-E","STABILIZER AGGREGATE","","",5765,28.421509106678201,163850]
["1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",6590,39.635053110773903,261195]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",660480,2.2980940830910899,1517845.18]
["1121000000-E","AGGREGATE BASE COURSE","","",799363,22.920232259936999,18321585.620000001]
["1146000000-E","CONDITIONING EXISTING BASE","","",1,5188.16,5188.16]
["1165000000-E","PORT CEM FOR CEM TRTD BASE CRSE","","",1293,185,239205]
["1176000000-E","SOIL CEMENT BASE","","",507050,2.52975465930382,1282712.1000000001]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",17791,181.78454499466,3234128.84]
["1198000000-E","AGGREGATE FOR SOIL CEM BS","","",1030,26.54,27336.2]
["1209000000-E","ASPHALT CURING SEAL","","",126920,2.70939568231957,343876.5]
["1220000000-E","INCIDENTAL STONE BASE","","",87329,32.503411352471701,2838490.41]
["1231000000-E","SHOULDER BORROW","","",18280,6.6621881838074399,121784.8]
["1243000000-E","SHOULDER CONST","","",9.0299999999999994,500,4515]
["1245000000-E","SHOULDER RECONST","","",2168.75,2917.1995665706099,6326676.5599999996]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",181981,20.8088397140361,3786813.46]
["1264000000-E","DITCHING","","",2385,13.041928721173999,31105]
["1275000000-E","PRIME COAT","","",152586,3.5135101516521798,536112.46]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",243031,1.7953381667359301,436322.83]
["","","(1\")","",1149037,1.97341049069786,2267521.67]
["","","(1-1/2\")","",10448484,1.85006068440168,19330329.460000001]
["","","(1-1/4\")","",41455,1.94513207092027,80635.45]
["","","(1.5\")","",261108,1.3669516062319,356922]
["","","(1/2\")","",745387,1.5206155996817801,1133447.1000000001]
["","","(2\")","",3168645,2.0441736704490401,6477260.6799999997]
["","","(2-1/2\")","",1396042,2.4547550933281399,3426941.21]
["","","(2-5/8\")","",281600,2.95,830720]
["","","(3\")","",258422,2.8511559000394699,736801.41]
["","","(4\")","",101824,3.85019563167819,392042.32]
["","","(4-1/2\")","",229490,4.9814214126977197,1143186.3999999999]
["","","(5-1/2\")","",170516,3.5391250674423498,603477.44999999995]
["","","(5/8\")","",309760,2.4500000000000002,758912]
["","","(6\")","",67514,5.9,398332.6]
["","","(7\")","",15559,8,124472]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0 TO 1-1/2\")","",5106,6.15,31401.9]
["","","(0 TO 2\")","",6248,8.9499999999999993,55919.6]
["","","(0\" - 1-1/2\")","",59278,3.25,192653.5]
["","","(0\" TO 1\")","",26525,2.7,71617.5]
["","","(0\" TO 1\")","",1242,8.51,10569.42]
["","","(0\" TO 1-1/2\")","",280673,3.4604623173586302,971258.34]
["","","(0\" TO 1-1/4\")","",3061,4,12244]
["","","(0\" TO 1/2\")","",369,11.5,4243.5]
["","","(0\" TO 2\")","",152246,2.4971010732630101,380173.65]
["","","(0\" TO 2-1/2\")","",6500,10.57,68705]
["","","(0\" TO 3\")","",5360,8.8991604477611901,47699.5]
["","","(0\" TO 3/4\")","",125,36.99,4623.75]
["","","(0\" TO 4\")","",15157,18.381685030019099,278611.20000000001]
["","","(0\" TO 5-1/2\")","",611,15.04,9189.44]
["","","(0\" TO 6\")","",6300,11,69300]
["","","(1-1/2\" TO 2\")","",88889,2.1,186666.9]
["","","(1-1/2\" TO 2-1/2\")","",7944,3,23832]
["","","(1-1/2\" TO 3\")","",38752,2.1,81379.199999999997]
["","","(1-1/2\" TO 4\")","",840,3,2520]
["","","(2\" TO 4-1/2\")","",107149,2.25,241085.25]
["","","(2\", 4\")","",3500,2.95,10325]
["1330000000-E","INCIDENTAL MILLING","","",657081.59999999998,8.1378664232874591,5347242.29]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",36415,58.841480159275001,2142712.5]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",617040,55.530818034487197,34264735.960000001]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",38272,52.740534855769198,2018485.75]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",803508,52.081709926970198,41848070.579999998]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",1328960,44.387432360642897,58989122.109999999]
["1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",16390,68.140771812080501,1116827.25]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",1970890,48.4503764796615,95490362.5]
["1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",39049,47.298714435709002,1846967.5]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",516349,54.6418343988272,28214256.550000001]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",36565,54.010117598796697,1974879.95]
["1525100000-E","ASP CONC SURF CRS SF9.5A LEVEL","","",125,85,10625]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",7326,67.100211575211603,491576.15]
["1575000000-E","ASP FOR PLANT MIX","","",278611,504.90642763566399,140672484.71000001]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",36446,716.29480903254102,26106080.609999999]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",34958,81.486158819154397,2848593.14]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",20093,136.548443238939,2743667.87]
["1704000000-E","PATCHING EXIST PVMT","","",247171,118.033691209729,29174505.489999998]
["1735000000-E","REP JNT CONC PVT SLABS","","",6225,586.84899598393599,3653135]
["1736000000-E","SELECT MAT'L, CLASS IV","","",2666,43.942235558889699,117150]
["1737000000-E","PATCHING CONC PVMT SPALLS","","",4917,112.573455358959,553523.68000000005]
["1748500000-E","AST, MAT & SINGLE SEAL","","",61532,1.45,89221.4]
["1770000000-E","AST, MAT COAT, 6 STONE","","",12807,1.98,25357.86]
["1771000000-E","AST, MAT COAT, 6M STONE","","",282104,1,282104]
["1775000000-E","AST, MAT COAT, 78M STONE","","",21741,1,21741]
["1775500000-E","AST, MAT COAT, *** STONE","(67)","",1213325,1.3173941277069201,1598427.23]
["","","(78)","",53800,0.63,33894]
["1803500000-E","AST, DOUBLE SEAL","","",1427879,1.2587385625812799,1797326.36]
["1814500000-E","AST, SINGLE SEAL","","",244742,0.85,208030.7]
["1820000000-E","AST, FOG SEAL","","",999150,0.44154169043687003,441166.38]
["1838000000-E","EMULSION FOR AST","","",1527296,2.1691071344388999,3312868.65]
["1838500000-N","VACUUM TRUCK","","",51.19,3123.1978902129299,159876.5]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",99381,115.49078797758099,11477590]
["1840000000-E","MILLED RUMBLE STRIPS","","",4419005,0.16849366542920999,744574.35]
["1847000000-E","******\"PCC PVMT THRU LNS","(13\")","",307732,55.5,17079126]
["1869000000-E","******\"PCC PVMT MISC","(12\")","",1220,125,152500]
["1880000000-E","GENERIC PAVING ITEM (TON)","ASPHALT FOR PAVEMENT INTERLAYER","",893,91,81263]
["","","ASPHALT FOR PAVEMENT INTERLAY-ER S4.75A","",500,90,45000]
["","","ASPHALT PAVEMENT INTERLAYER","",150,130,19500]
["","","JOINT REPAIR","",1131,242.161803713528,273885]
["","","PATCHING EXISTING PAVEMENT","(FULL DEPTH)",1543,180.19051198963101,278033.96000000002]
["","","","(MILL)",1005,144.341890547264,145063.6]
["","","","(MILL) I19.0C",1350,140,189000]
["","","","(MILL) S9.5C",300,170,51000]
["","","","I19.0C (MILL)",430,156.75,67402.5]
["","","PATCHING EXISTING PAVEMENT (MILL)","",7192,159.283912680756,1145569.8999999999]
["1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR & SEALING","",1093782,1.84072085662408,2013347.34]
["","","JOINT CONSTRUCTION, REPAIR ANDSEALING","",713000,2.6,1853800]
["","","JOINT CONSTRUCTION, REPAIR,","AND SEALING",1047712,2,2095424]
["","","MEDIAN HAZARD PROTECTION","",103,586,60358]
["","","MILLED RUMBLE STRIPS, ASPHALT","CONCRETE (CENTERLINE)",11088,0.22,2439.36]
["1881500000-E","GENERIC PAVING ITEM (CF)","CONCRETE/ASPHALT REPAIR (HOT","APPLIED SYNTHETIC POLYMER RES)",945,325,307125]
["1891000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE GREENWAY PATH","",460,43.6,20056]
["","","8\" REINFORCED CONCRETE","PAVEMENT",740,87.25,64565]
["","","DIAMOND GRINDING PCC PAVEMENT","",2081755,4.9379513679563596,10279604.949999999]
["","","FINE MILLING (1-1/2\")","",760000,2.15,1634000]
["","","FINE MILLING (5/8\")","",876358,1.92614285486068,1687990.7]
["","","LATEX MODIFIED MICRO-SURFACING","TYPE III",118720,3.06335865902965,363681.94]
["","","LATEX MODIFIED MICROSURFACING","TYPE II",203709,2.4602656730925001,501178.26]
["","","LATEX MODIFIED MICROSURFACING,TYPE III","",324317,2.59,839981.03]
["","","PAVEMENT INTERLAYER","",112524,4.25,478227]
["","","PAVEMENT INTERLAYER (HIGH STRENGTH)","",91225,5.95,542788.75]
["","","PAVEMENT INTERLAYER (REGULAR)","",136545,4.6472152037789698,634554]
["1924000000-N","FIELD LAB RENTAL, PCCP","","",1,200000,200000]
["1925000000-E","MILL RUMBLE STRPS (CONC SHLDR)","","",79048,0.47965236312114001,37915.56]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",1343,267.06221146686499,358664.55]
["2020000000-N","CONTROL-OF-ACCESS MARKERS","","",48,307.63333333333298,14766.4]
["2021000000-N","GENERIC GRADING ITEM (EA)","RIGHT OF WAY MARKERS","",99,135,13365]
["2022000000-E","SUBDRAIN EXCAVATION","","",22927,18.203389889649799,417349.12]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",67787,4.8378107896794402,327940.68]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",2593,27.6415040493637,71674.42]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",11171.4,49.688107130708801,555085.72]
["2044000000-E","6\" PERF SUBDRN PIPE","","",82831,9.7731586000410502,809520.5]
["2070000000-N","SUBDRN PIPE OUTLET","","",185,309.47070270270302,57252.08]
["2077000000-E","6\" OUTLET PIPE","","",1199,38.205354462051702,45808.22]
["2099000000-E","SHOULDER DRAIN","","",83963,7.6996742612817597,646487.75]
["2110000000-E","4\" SHOULDER DRAIN PIPE","","",83963,1.1907709348165301,99980.7]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",6248,13.890925096030699,86790.5]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",131,299.682442748092,39258.400000000001]
["2143000000-E","BLOTTING SAND","","",136,86.001470588235307,11696.2]
["2165000000-E","12\" FUNNEL DRAIN PIPE","","",30,93,2790]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",25,508.68360000000001,12717.09]
["2209000000-E","ENDWALLS","","",287.5,1182.6509217391299,340012.14]
["2220000000-E","REINF ENDWALLS","","",287.7,1374.6606882168901,395489.88]
["2253000000-E","PIPE COLLARS","","",95.308000000000007,1301.5171863851899,124045]
["2264000000-E","PIPE PLUGS","","",3.2869999999999999,1285.9598418010301,4226.95]
["2275000000-E","FLOWABLE FILL","","",1361,363.50096987509198,494724.82]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",3638,2006.6066739967,7300035.0800000001]
["2297000000-E","MASNRY DRAINAGE STRUCT","","",278.39400000000001,2283.6396976946298,635751.59]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",1891.84,311.071242811231,588497.02]
["2352000000-N","FRAME W/GRATE 840.***** STD","(20)","",1,1052.3,1052.3]
["","","(840.D13)","",3,583.33333333333303,1750]
["2354000000-N","FRAME W/GRATE 840.22 STD","","",4,810.125,3240.5]
["2354200000-N","FRAME W/GRATE 840.24 STD","","",4,544.92750000000001,2179.71]
["2355000000-N","FRAME W/GRATE 840.29 STD","","",6,516.66666666666697,3100]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",538,629.31014869888497,338568.86]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",295,703.68837288135603,207588.07]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",446,599.07858744394605,267189.05]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",233,758.26793991416298,176676.43]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",195,613.92430769230805,119715.24]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",229,713.70890829694304,163439.34]
["","","(F)","",696,706.85265804597702,491969.45]
["","","(G)","",769,697.45344603381,536341.69999999995]
["2396000000-N","FRAME W/COVER STD 840.54","","",212,512.09754716981104,108564.68]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",86,1782.6334883720899,153306.48000000001]
["2418000000-E","FRM W/GRATES, DRIVEWY DI","","",149,392.23557046979897,58443.1]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",54,540.70037037037002,29197.82]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",394,774.13799492385795,305010.37]
["2462000000-E","**\" SLUICE GATE","(18\")","",6,6000,36000]
["","","(24\")","",1,15000,15000]
["","","(30\")","",2,15000,30000]
["","","(36\")","",4,12000,48000]
["","","(8\")","",9,1329.0033333333299,11961.03]
["2473000000-N","GENERIC DRAINAGE ITEM (EA)","ADJUSTMENT OF JUNCTION BOXES","",2,2000,4000]
["","","DRAINAGE STRUCTURE CLEANOUT","",10,550,5500]
["","","DRAINAGE STRUCTURE REPAIR","",8,3300,26400]
["","","GDI FRAME W/ 2 ADA GRATES","",5,1950,9750]
["","","REMOVE & REPLACE CONC APRON","",16,3234.1875,51747]
["","","REMOVE AND REPLACE","CONCRETE APRON",1,13800,13800]
["","","REMOVE AND REPLACE CONCRETE APRON","",70,2424.6428571428601,169725]
["","","REMOVE AND REPLACE METAL FUN- NELS","",1,2270,2270]
["2484000000-E","GENERIC DRAINAGE ITEM (LF)","8\" UNDERDRAIN","",5250,31,162750]
["","","MODIFIED SHOULDER BERM GUTTER","",28,83.5,2338]
["","","REMOVE & REPLACE","2'-6\" CURB & GUTTER",625,55,34375]
["2489000000-E","GENERIC DRAINAGE ITEM (SY)","REMOVE & REPLACE 4\" CONC PAVEDDITCH","",2000,100,200000]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",1010,22.600297029703,22826.3]
["","","(8\" X 18\")","",670,27.7649253731343,18602.5]
["","","(9\" X 12\")","",1030,26.601941747572798,27400]
["2538000000-E","**'-**\" CONC CURB & GUTTER","(2'-0\")","",1170,26,30420]
["","","(2'-9\")","",11540,25.428266897747001,293442.2]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",127990,18.649277287288101,2386921]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",290515,21.496195032958699,6244967.0999999996]
["2556000000-E","SHOULDER BERM GUTTER","","",53304,24.404191805492999,1300841.04]
["2570000000-N","MOD CONC FLUME","","",15,2251.6666666666702,33775]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",18460,31.0195666305526,572621.19999999995]
["2580000000-E","CONC VALLEY GUTTER","","",555,32.095315315315297,17812.900000000001]
["2591000000-E","4\" CONC SIDEWALK","","",68584,41.798091391578197,2866680.3]
["2600000000-N","RETROFIT EXT CURB RAMPS","","",265,866.15094339622601,229530]
["2605000000-N","CONC CURB RAMPS","","",752,2024.88694148936,1522714.98]
["2612000000-E","6\" CONC DRIVEWAY","","",31808,64.135871478873199,2040033.8]
["2613000000-N","REM & REP CURB RAMPS","","",10,5925.7089999999998,59257.09]
["2619000000-E","4\" CONC PAVED DITCH","","",17321,92.869205011258003,1608587.5]
["2627000000-E","4\" CONC ISLAND COVER","","",2320,61.508448275862101,142699.6]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",13409,58.826265940786001,788801.4]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",41390,63.174967383426001,2614811.9]
["2657000000-E","**\" MONO CONC MEDIAN (*****)","(5-1/2\", KEYED IN)","",20,85,1700]
["2703000000-E","CONC BARRIER TYPE ******","(T1)","",5735,227.7,1305859.5]
["2710000000-N","CONC BARRIER TRANS SECTN","","",6,35062.5,210375]
["2724000000-E","PC REINF BARRIER SNGL FC","","",10045,118.466236933798,1189993.3500000001]
["2738000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE GREENWAY PATH","",160,48,7680]
["","","4\" CONCRETE ISLAND CAP","",170,350,59500]
["","","4\" CONCRETE MULTIUSE PATH","",1180,56.88,67118.399999999994]
["","","6\" CONCRETE DRIVEWAY","",40,70,2800]
["","","7\" CONCRETE TRUCK APRON","",580,101.36120689655201,58789.5]
["","","PEDESTRIAN REFUGE ISLAND","(PASS THRU)",130,200,26000]
["","","REINFORCED CONCRETE DRIVEWAY","",259,90,23310]
["","","REMOVE & REPLACE 4\" CONC SIDE-WALK","",24,100,2400]
["","","REMOVE & REPLACE 5\" MONOLITHIC","CONC ISLANDS",146,75,10950]
["","","REMOVE AND REPLACE 4\" CONCRETE","PAVED DITCH",577,92,53084]
["","","REMOVE AND REPLACE 5\"","MONOLITHIC CONCRETE ISLANDS",69,162.04,11180.76]
["","","REMOVE MONOLITHIC CONC ISLAND","",38,40,1520]
["","","ROLLER COMPACTED CONCRETE","",74848,38,2844224]
["2738100000-E","GENERIC PAVING ITEM (SF)","PATCHING CONCRETE PAVEMENT SPALLS","",11000,199,2189000]
["2752000000-E","GENERIC PAVING ITEM (LF)","1'-6\" MODIFIED CONCRETE CURB &","GUTTER",1390,22,30580]
["","","2'-6\" MODIFIED CONCRETE CURB &","GUTTER",150,33,4950]
["","","MEDIAN HAZARD PROTECTION","",234,79.723076923076903,18655.2]
["","","MODIFIED SHOULDER BERM","GUTTER",135,40,5400]
["","","REMOVE & REPLACE 2'-0\" CURB & GUTTER","",195,70,13650]
["","","REMOVE & REPLACE 2'-6\" CURB AND GUTTER","",140,85,11900]
["","","REMOVE & REPLACE 2'-6\" CURB & GUTTER","",179,78.659217877095003,14080]
["","","REMOVE 4\" X 8\" CONCRETE CURB","",118,20,2360]
["","","REMOVE AND REPLACE 2'-6\" C & G","",10,75,750]
["","","REMOVE AND REPLACE 2'-6\" CURB & GUTTER","",40,100,4000]
["2759000000-N","GENERIC PAVING ITEM (EA)","ADJUSTMENT OF MONUMENTS","",178,600,106800]
["","","MEDIAN HAZARD PROTECTION","",1,51636.87,51636.87]
["2761000000-E","GENERIC PAVING ITEM 848 (SY)","8\" CONCRETE DRIVEWAY","",90,120,10800]
["2762000000-E","GENERIC PAVING ITEM (LB)","PAVEMENT SLAB STABILIZATION MATERIAL","",21000,10,210000]
["","","POLYMER MODIFIED CONCRETE","PAVEMENT REPAIR",3760,7,26320]
["","","SEALING EXISTING PAVEMENT","CRACKS (POLYMER PATCH)",250,20,5000]
["","","SLAB LEVELING, UNDERSEALING","AND VOID FILLING",3750,6.25,23437.5]
["2800000000-N","ADJ CATCH BASINS","","",49,1027.47387755102,50346.22]
["2815000000-N","ADJ DROP INLETS","","",151,1075.91304635762,162462.87]
["2830000000-N","ADJ MANHOLES","","",2085,912.36872422062299,1902288.79]
["2845000000-N","ADJ METER OR VALVE BOXES","","",2068,788.623824951644,1630874.07]
["2860000000-N","CONVERT CB TO JB","","",4,2079.9775,8319.91]
["2893000000-N","CONVERT CB TO JB W/MH","","",2,1017.5,2035]
["2905000000-N","CONVERT DI TO JB","","",14,2276.8535714285699,31875.95]
["2910000000-N","CONVERT TRAF BR DI TO TRAF BR JB","","",1,8461.5400000000009,8461.5400000000009]
["2920000000-N","CONVERT DI TO CB","","",3,932.96666666666704,2798.9]
["2938000000-N","CONVERT DI TO JB W/MH","","",6,1449.1666666666699,8695]
["2950000000-N","CONVERT JB TO DI","","",3,1400,4200]
["2995000000-N","GENERIC DRAINAGE ITEM (EA)","ADJUSTMENT OF COMMUNICATION/","OVERSIZE MANHOLES",10,2150,21500]
["","","ADJUSTMENT OF OVERSIZED","MANHOLES",3,3200,9600]
["","","CONVERT EXISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION BOX",3,1633.3333333333301,4900]
["","","CONVERT EXT DROP INLET TO TB","DROP INLET",1,4470,4470]
["","","CONVERT EXTISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION BOX",2,1000,2000]
["3000000000-N","IMPACT ATTEN TYPE 350","","",43,18481.434418604698,794701.68]
["3030000000-E","STL BEAM GUARDRAIL","","",465659,16.8334475657079,7838646.3600000003]
["3045000000-E","SBGR SHOP CURVED","","",3562.5,21.2699677192983,75774.259999999995]
["3060000000-E","SBGR DOUBLE FACED","","",155912.5,22.0284614767899,3434512.5]
["3075000000-E","TRIPLE CORRUGATED SBGR","","",762.5,62.163934426229503,47400]
["3105000000-N","SBGR TERM SECT","","",14,490.65285714285699,6869.14]
["3120000000-E","20\"TUBULAR 3C GUARDRAIL","","",3622,178.60298177802301,646900]
["3135000000-N","W-TR SBGR TRANS SECTIONS","","",51,157.5,8032.5]
["3145000000-E","EX LENGTH GR POST ** STL","(8')","",46,89.220869565217399,4104.16]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",484,28.9134917355372,13994.13]
["3165500000-N","GR END UNIT TYPE **********","(AT-1)","",1,544.01,544.01]
["","","(BIC)","",1,2100,2100]
["3180000000-N","GR ANCHOR TYPE **********","(B-83, SHOP CURVED)","",3,2100,6300]
["","","(III MOD)","",10,2090,20900]
["","","(III SHOP CURVED)","",4,1800,7200]
["","","(III, SHOP CURVED)","",2,1850,3700]
["3195000000-N","GR END TYPE AT-1","","",21,677.07619047619096,14218.6]
["3210000000-N","GR END TYPE CAT-1","","",500,619.78635999999995,309893.18]
["3215000000-N","GR ANCHOR TYPE III","","",146,1528.0086986301401,223089.27]
["3287000000-N","GR END TYPE TL-3","","",762,2988.0102493438299,2276863.81]
["3288000000-N","GR END TYPE TL-2","","",40,3201.5940000000001,128063.76]
["3317000000-N","GR ANCHOR TYPE B-77","","",285,1750.07024561404,498770.02]
["3319000000-N","GR ANCHOR TYPE B-83","","",16,1650,26400]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",15452.5,15.636944183789,241629.88]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",384263,2.17826889396065,837028.14]
["3365000000-E","REMOVE EXISTING GUIDERAIL","","",4700,1.2417021276595701,5836]
["3380000000-E","TEMP STL BM GUARDRAIL","","",8512.5,11.2491923641703,95758.75]
["3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",87.5,14.214285714285699,1243.75]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",20,902.32299999999998,18046.46]
["","","(B-83)","",4,950,3800]
["","","(III)","",14,971.42857142857099,13600]
["","","(III-MODIFIED)","",2,1250,2500]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",16,2681.2049999999999,42899.28]
["","","(TL-3)","",19,2110.5263157894701,40100]
["3389200000-E","CABLE GUIDERAIL","","",27650,6.7145027124774002,185656]
["3389400000-E","DBL FACED CABLE GUIDERAIL","","",26500,6.75,178875]
["3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",135,53.805925925925898,7263.8]
["3389600000-N","CBL GUIDERAIL ANCH UNIT","","",99,1699.09494949495,168210.4]
["3420000000-E","GENERIC GUARDRAIL ITEM (LF)","REMOVE & REPLACE EXISTING","GUARDRAIL",400,20.52,8208]
["","","REMOVE & REPLACE EXISTING GUARDRAIL","",6425,16.824902723735399,108100]
["","","REMOVE AND REPLACE EXISTING GUARDRAIL","",87703,16.2,1420788.6]
["","","VINYL COATED GLARE SCREEN","(GUARDRAIL MOUNTED)",525,26.25,13781.25]
["3435000000-N","GENERIC GUARDRAIL ITEM (EA)","BOLLARDS (PERMANENT)","",10,1280.06,12800.6]
["","","BOLLARDS (REMOVABLE)","",3,2403.37,7210.11]
["","","EXTRA LENGTH GUARDRAIL POSTS (8' STEEL)","",70,61,4270]
["","","GUARDRAIL POST CAPS","",161,45.4,7309.4]
["3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY ADDITIONAL GUARDRAILPOSTS","",5,22.5,112.5]
["","","TEMPORARY GUARDRAIL END","UNITS, TYPE AT-1",1,325,325]
["","","TEMPORARY GUARDRAIL END UNITS,","TYPE CAT-1",3,100,300]
["","","TEMPORARY GUARDRAIL END UNITS,TYPE AT-1","",1,400,400]
["","","TEMPORARY GUARDRAIL END UNITS,TYPE CAT-1","",3,333.33333333333297,1000]
["3500000000-E","WOVEN WIRE FENCE **\" FAB","(47\")","",9920,3.11,30851.200000000001]
["","","(48\")","",16090,3.25,52292.5]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",234570,3.4001193673530299,797566]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",15709,22.400171875994701,351884.3]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",5501,31.735066351572399,174574.6]
["3533000000-E","CHN LK FENCE **\" FABRIC","(60\")","",89,25.275168539325801,2249.4899999999998]
["","","(72\")","",1183,18,21294]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",6839,8.26207047814008,56504.3]
["3539000000-E","MET LINE PST **\" CL FEN","(60\")","",9,119.037777777778,1071.3399999999999]
["","","(72\")","",102,75,7650]
["3542000000-E","MET LINE PST 48\" CL FEN","","",558,58.915860215053797,32875.050000000003]
["3545000000-E","MET TERM PST **\" CL FEN","(60\")","",6,310.94,1865.64]
["","","(72\")","",10,210,2100]
["3548000000-E","MET TERM PST 48\" CL FEN","","",146,156.49390410958901,22848.11]
["3551000000-E","MET GATE PST **\" CL FEN S","(72\")","",2,450,900]
["3554000000-E","MET GATE PST **\" CL FEN D","(48\")","",2,280,560]
["","","(72\")","",2,450,900]
["3557000000-E","ADDITIONAL BARBED WIRE","","",860,0.79302325581394995,682]
["3559000000-E","** STRAND BW FENCE W/ POSTS","(3)","",100,6,600]
["","","(4)","",580,8.7931034482758594,5100]
["3563000000-E","TEMP **\" WW FENCE W/POSTS","(47\")","",310,10,3100]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 12')","",1,600,600]
["","","(48\", 12', 12')","",2,490.5,981]
["","","(72\", 12', 12')","",1,2400,2400]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 10', 20')","",2,1500,3000]
["","","(48\", 8', 16')","",1,1650,1650]
["","","(58\", 12', 24')","",4,800,3200]
["","","(72\", 12', 24')","",1,4200,4200]
["3566000000-E","WOVEN WIRE FENCE RESET","","",155,8.7200000000000006,1351.6]
["3572000000-E","CHAIN LINK FENCE RESET","","",455,19.240549450549501,8754.4500000000007]
["3574000000-E","GENERIC FENCING ITEM 867 (LF)","VINYL 3 RAIL FENCE RESET","",190,35,6650]
["3575000000-E","GENERIC FENCING ITEM (LF)","BIKE/PED SAFETY RAIL","",320,65.400000000000006,20928]
["","","BLACK VINYL COATED CHAIN LINK","FENCE, 48\" FABRIC",510,14.8,7548]
["","","CHAIN LINK FENCE","",585,31.25,18281.25]
["","","DECORATIVE FENCE RESET","",50,40,2000]
["","","HANDRAIL HUNTERSVILLE STANDARD","DRAWING 700.1",750,105.5,79125]
["","","PEDESTRIAN SAFETY RAIL","",185,128,23680]
["","","RETAINING WALL ALUMINUM PICKETFENCE","",745,71,52895]
["","","STEEL PIPE HANDRAIL FOR","RETAINING WALL",80,173.26,13860.8]
["","","TEMP CHAIN LINK FENCE, 60\" FABRIC","",195,40,7800]
["","","TEMPORARY 5 STRAND BARBED WIRE","FENCE WITH POSTS",400,9.25,3700]
["","","TEMPORARY 72\" CHAIN LINK FENCE","WITH POSTS",286,18,5148]
["","","WALL MOUNTED PEDESTRIAN HANDRAIL","",182,170,30940]
["3578000000-N","GENERIC FENCING ITEM (EA)","30' STEEL PIPE GATE","",1,7845.5,7845.5]
["","","BLACK VINYL COATED METAL","TERMINAL POST FOR 48\" CHAIN LINK FENCE",6,159.1,954.6]
["","","BLACK VINYL COATED METAL LINE","POST FOR 48\" CHAIN LINK FENCE",42,79.5,3339]
["","","GATE","",2,3450,6900]
["3628000000-E","RIP RAP, CLASS I","","",23801,52.407917314398603,1247360.8400000001]
["3635000000-E","RIP RAP, CLASS II","","",9507,45.440201956453102,432000]
["3642000000-E","RIP RAP, CLASS A","","",2737,48.430690537084402,132554.79999999999]
["3649000000-E","RIP RAP, CLASS B","","",23658,49.250583312198799,1165170.3]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",164357,2.1096513686669902,346735.97]
["3659000000-N","PREFORMED SCOUR HOLES","","",14,2011.52357142857,28161.33]
["3832000000-E","RR TRACK TO BE REMOVED","","",3740,12,44880]
["3884000000-N","GENERIC TRACKWORK ITEM (EA)","CROSSTIE DISPOSAL","",2120,6,12720]
["3885000000-E","GENERIC TRACKWORK ITEM (TON)","SUB-BALLAST","",6615,32,211680]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(A)","",3156,17,53652]
["","","(B)","",419,17,7123]
["","","(D)","",213.5,17.501826697892302,3736.64]
["","","(E)","",2772.55,17.916152999945901,49673.43]
["","","(F)","",255.77,19.634984556437399,5022.04]
["4048000000-E","REINF CONC FOUNDTN","","",79,924.50886075949404,73036.2]
["4054000000-E","PLN CONC FOUNDTN","","",16,558.234375,8931.75]
["4057000000-E","OVERHEAD FOOTING","","",843,1060.60367734282,894088.9]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",63687,5.1104228492471,325467.5]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",21305,4.9647810373151797,105774.66]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",46807.9,7.1776172398249001,335969.19]
["4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",45,65,2925]
["4079000000-N","SUPPORT, BARR SMALL","","",2,560,1120]
["4080000000-N","SUPPORT, BARR LARGE","","",9,800,7200]
["4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(111+35 -Y-)","",1,41000,41000]
["","","(12+50 -LSB-)","",1,51704.75,51704.75]
["","","(123+03 -Y-)","",1,43000,43000]
["","","(13+25 -LPD-)","",1,85000,85000]
["","","(14+50 -RPB- LT)","",1,55000,55000]
["","","(149+00 -Y-)","",1,29000,29000]
["","","(171+68 -Y-)","",1,33000,33000]
["","","(20+50 -Y-)","",1,52000,52000]
["","","(20+50 -YRPC-)","",1,56013.51,56013.51]
["","","(22+50 -LACFLY-)","",1,44000,44000]
["","","(24+50 -Y-)","",1,25000,25000]
["","","(25+00 -RPD-)","",1,59000,59000]
["","","(25+00 -YRPA-)","",1,61399.360000000001,61399.360000000001]
["","","(25+50 -L-)","",1,85250,85250]
["","","(25+85 -RPC-)","",1,39000,39000]
["","","(26+50 -Y-)","",1,30161.13,30161.13]
["","","(29+50 -Y- LT)","",1,46000,46000]
["","","(291+50 -L-)","",1,45000,45000]
["","","(294+00 -L- LT)","",1,46000,46000]
["","","(30+25 -Y-)","",1,30161.13,30161.13]
["","","(316+00 -L- LT)","",1,38000,38000]
["","","(32+75 -Y- LT)","",1,45000,45000]
["","","(328+50 -L-)","",1,26000,26000]
["","","(34+00 -Y-)","",1,32500,32500]
["","","(346+00 -L- LT)","",1,29800,29800]
["","","(357+00 -L-)","",1,16000,16000]
["","","(383+50 -L-)","",1,42000,42000]
["","","(385+00 -L- LT)","",1,32000,32000]
["","","(419+00 -L- LT)","",1,27500,27500]
["","","(428+50 -L-)","",1,21500,21500]
["","","(43+00 -L-)","",1,83000,83000]
["","","(44+00 -L-)","",1,30875,30875]
["","","(44+25 -L-)","",1,35000,35000]
["","","(450+00 -L- LT)","",1,29500,29500]
["","","(456+00 -L-)","",1,21000,21000]
["","","(468+50 -L-)","",1,16000,16000]
["","","(47+50-L-LT)","",1,32000,32000]
["","","(488+00 -L- LT)","",1,48500,48500]
["","","(507+00 -L- LT)","",1,53500,53500]
["","","(512+00 -L-)","",1,25500,25500]
["","","(52+00 -L-)","",1,65000,65000]
["","","(529+50 -L- LT)","",1,22500,22500]
["","","(540+00 -L-)","",1,23000,23000]
["","","(59+00 -L-)","",1,30000,30000]
["","","(60+42 -Y-)","",1,24000,24000]
["","","(69+00 -L-)","",1,75000,75000]
["","","(84+00 -Y-)","",1,24000,24000]
["","","(EXIT 17 NB US-421)","",1,80660,80660]
["4096000000-N","SIGN ERECTION, TYPE D","","",146,143.93068493150699,21013.88]
["4102000000-N","SIGN ERECTION, TYPE E","","",2359,88.978100890207699,209899.34]
["4108000000-N","SIGN ERECTION, TYPE F","","",309,122.50598705501601,37854.35]
["4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",39,923.227692307692,36005.879999999997]
["","","(B)","",12,343.634166666667,4123.6099999999997]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",103,641.42281553398095,66066.55]
["","","(B)","",34,430.62823529411799,14641.36]
["","","(E)","",2,60,120]
["4114000000-N","SIGN ERECTION, MILEMARKERS","","",65,80.092307692307699,5206]
["4115000000-N","SIGN ERECTION, OVERLAY (OVRHD)","","",115,410.89130434782601,47252.5]
["4116000000-N","SIGN ERECTION, OVERLAY (GRD MTD)","","",15,546.29999999999995,8194.5]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",15,742.35733333333303,11135.36]
["","","(B)","",14,557.34357142857095,7802.81]
["","","(D)","",29,233.57310344827599,6773.62]
["","","(E)","",59,161.84983050847501,9549.14]
["","","(F)","",20,164.15049999999999,3283.01]
["","","(LOGO TRAILBLAZER)","",2,50,100]
["","","(MILEMARKER)","",2,100,200]
["4116200000-N","SIGN ERECTION, REPOSIT OVRHD","","",16,610.625,9770]
["4138000000-N","DISPOSE SUPPORT, STL BM","","",39,469.01743589743597,18291.68]
["4141000000-N","DISPOSE SUPPORT, WOOD","","",1,5,5]
["4149000000-N","DISPOSE SIGN SYST OVRHD","","",6,5180.9466666666704,31085.68]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",44,326.71727272727298,14375.56]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",1417,10.243041637261801,14514.39]
["4158000000-N","DISPOSE SIGN SYST WOOD","","",12,3.8541666666666701,46.25]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",164,6.5351219512195096,1071.76]
["4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",48,145.32208333333301,6975.46]
["4236000000-N","DISPOSE SIGN, A & B (GRD MTD)","","",7,16.875714285714299,118.13]
["4237000000-N","STOCKPILE SIGN, D, E, F","","",37,32.101621621621597,1187.76]
["4238000000-N","DISPOSE SIGN, D, E, F","","",179,4.3925139664804496,786.26]
["4241000000-N","DISPOSE SIGN, OVERLAY OVRHD","","",35,1.5,52.5]
["4242000000-N","DISPOSE SIGN, OVERLAY GM","","",2,1.5,3]
["4251000000-N","DISPOSE LIGHT SYSTEM","","",6,1472.44,8834.64]
["4263000000-N","DISPOSE WALKWAY","","",6,817.85,4907.1000000000004]
["4360000000-N","GENERIC SIGNING ITEM (EA)","DISPOSAL OF SIGN SYSTEM ON SPAN WIRE","",2,3900,7800]
["4370000000-N","GENERIC SIGNING ITEM (LS)","DISPOSAL OF FLASHER SYSTEM","",1,2000,2000]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",43135,11.684396893474,504006.46]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",25213,13.863192004124899,349532.66]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",9161,9.9626852963650308,91268.160000000003]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",231580,8.9138546506606797,2064270.46]
["4415000000-N","FLASHING ARROW BOARD","","",146,2462.4448630136999,359516.95]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",184,9338.1205434782605,1718214.18]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",1273,72.916535742340898,92822.75]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",86,7122.0344186046495,612494.96]
["4424000000-N","WZ PRESENCE LIGHTING","","",262,5100.1454198473302,1336238.1000000001]
["4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",9,28688.888888888901,258200]
["4430000000-N","DRUMS","","",15620,47.010386043533899,734302.23]
["4432000000-N","HIGH VISIBILITY DRUMS","","",250,62.37,15592.5]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",521,151.71257197696701,79042.25]
["4435000000-N","CONES","","",3193,22.896580018791099,73108.78]
["4445000000-E","BARRICADES (TYPE III)","","",13483,29.276086924274999,394729.48]
["4447000000-E","PED CHANNEL DEVICES","","",160,46.5,7440]
["4450000000-N","FLAGGER","","",3960,32.121212121212103,127200]
["4455000000-N","FLAGGER","","",13268,284.57142975580302,3775693.73]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",57,178256.55368421099,10160623.560000001]
["4465000000-N","TEMP CRASH CUSHIONS","","",108,6078.6452777777804,656493.68999999994]
["4470000000-N","REM & RES CRASH CUSHION","","",60,2742.1413333333298,164528.48000000001]
["4480000000-N","TMA","","",104,11046.1032692308,1148794.74]
["4485000000-E","PORT CONC BARRIER","","",23950,25.190159081419601,603304.31000000006]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",32133,39.813251174804698,1279319.2]
["4500000000-E","REM & RES PORT CONC BARRIER","","",26084,7.5751337984971601,197589.79]
["4505000000-E","REM & RES PORT CONC BARR, ANCH","","",10535,11.0101471286189,115991.9]
["4507000000-E","WATER FILLED BARRIER","","",8353,71.695019753381999,598868.5]
["4508000000-E","REM & RES H2O FILL BARR","","",5500,14.817090909090901,81494]
["4510000000-N","LAW ENFORCEMENT","","",26773,50.0507675643372,1340009.2]
["4516000000-N","SKINNY DRUM","","",3603,39.304746044962499,141615]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",113,77.743362831858406,8785]
["4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","PROTECTIVE CANOPY","",1,57450,57450]
["4590000000-E","GENERIC TRAFFIC CONTROL ITEM (LF)","PEDESTRIAN BARRICADE","",48,45,2160]
["4595000000-E","GENERIC TRAFFIC CONTROL ITEM (SF)","HIGH VISIBILITY RIGID PORTABLE","WORK ZONE SIGNS",482,10.16,4897.12]
["","","HIGH VISIBILITY STATIONARY","WORK ZONE SIGNS",1143,15.91,18185.13]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","ADA BARRICADE (SAFETY RAIL)","",13,499.05153846153797,6487.67]
["","","AUDIBLE WARNING DEVICES","",6,3000,18000]
["","","DOUBLE LANE CLOSURE","",155,3712,575360]
["","","LANE CLOSURE","",1901,2794.73619147817,5312793.5]
["","","RAMP/LOOP CLOSURE","",265,2490,659850]
["","","RAMP/LOOP CLOSURE (TYPE A)","",40,2160,86400]
["","","RAMP/LOOP CLOSURE (TYPE B)","",1,6412,6412]
["","","RAMP/LOOP CLOSURE (TYPE C)","",1,2362,2362]
["","","RAMP/LOOP TRAFFIC CONTROL","",146,2565,374490]
["","","SINGLE LANE CLOSURE","",35,2937,102795]
["","","TEMPORARY CURB RAMPS","",6,1850,11100]
["","","TRIPLE LANE CLOSURE","",194,3940,764360]
["","","WARNING FLAGS","",2,500,1000]
["4650000000-N","TEMP RAISED PVMT MRKS","","",22913,7.1199572295203604,163139.57999999999]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",8646053,0.53365658989136,4614023.16]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",8514465,0.65272754659276999,5557625.8499999996]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",2468,5.0887358184764997,12559]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",2806585,0.79710598111228004,2237145.69]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",405395,1.03916328519099,421271.6]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",158392,1.93185849032779,305990.93]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",124343,2.53202078122612,314839.06]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",230570,2.4579928004510601,566739.4]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",17664,2.74870244565217,48553.08]
["4705000000-E","THERMO LINES 16\" 120MILS","","",8375,7.1860895522388102,60183.5]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",109733,10.6721815679877,1171090.5]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",3545,125.95401410437201,446506.98]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",14317,134.160767618915,1920779.71]
["4726000000-E","HIP THERMO PVT MKG LINE 4\" 90 MILS","","",93,20,1860]
["4726100000-E","HIP THERMO PVT MKG CHAR 120 MILS","","",100,200.6,20060]
["4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",270,491.277777777778,132645]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(2)","",3200,2.75,8800]
["","","(II)","",66248,3.4283244777200799,227119.64]
["","","(III)","",2968,4.8311994609164399,14339]
["","","(IV)","",38501,2.8732661489311999,110623.62]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",18216,4.2676432806324103,77739.39]
["","","(IV)","",4155,2.3594464500601702,9803.5]
["","","II","",1184,10,11840]
["4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",1180,8.3018898305084701,9796.23]
["","","(III)","",2225,7.0337078651685401,15650]
["","","(IV)","",486,10.5,5103]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",1194,9.6117336683417101,11476.41]
["4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",620,15.322580645161301,9500]
["","","(IV)","",91,29.945054945054899,2725]
["4800000000-N","COLD APP PLAS CHAR TYPE *","(III)","",9,180,1620]
["","","(IV)","",32,90,2880]
["4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",81,702.59259259259295,56910]
["","","(III)","",20,346.25,6925]
["","","(IV)","",22,307.11727272727302,6756.58]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",35740685,0.14139411317941999,5053522.46]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",5013993,0.30065363274340001,1507475.21]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",335906,0.62263281989604002,209146.1]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",322008,0.88493466000845,284956.03999999998]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",6229,2.9989725477604798,18680.599999999999]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",99556,3.4810969705492401,346564.09]
["4840000000-N","PAINT PVT MKG CHARACTER","","",2841,45.240337909186898,128527.8]
["4845000000-N","PAINT PVT MKG SYMBOL","","",12610,47.038949246629699,593161.15]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",2548491.2999999998,0.83840144559254004,2136658.79]
["4847020000-E","POLYUREA LINES (4\", 30 MILS)","","",1380,5.5,7590]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",2191976,1.1098106183644301,2432678.2400000002]
["4847040000-E","POLYUREA LINES (6\", 30 MILS)","","",515751,1.6194279797809401,835221.6]
["4847050000-E","POLYUREA LINES (8\", 20 MILS)","","",13065,2.65147034060467,34641.46]
["4847070000-E","POLYUREA LINES (12\", 20 MILS)","","",123651,2.4045282286435201,297322.32]
["4847080000-E","POLYUREA LINES (12\", 30 MILS)","","",14000,3.62,50680]
["4847400000-E","WZ PERF PVMT MKG LINES 4\"","","",4614,0.65,2999.1]
["4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",154157,0.78936506289042996,121686.15]
["4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",8900,2.2190786516853902,19749.8]
["4848000000-E","WZ TRAF PATTERN MASKING","","",949364,0.32059863234754998,304364.79999999999]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",2229896,0.38435483089793998,857071.3]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",541151,0.57662013005612001,312038.56]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",14990,1.2838959306204101,19245.599999999999]
["4865000000-E","LINE REMOVAL 12\" WIDE","","",44059,1.01937402119885,44912.6]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",5013,4.3760143626570898,21936.959999999999]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",1035,65.240801932367106,67524.23]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","COLD APPLIED PLASTIC PAVEMENT","MARKING LINES, TYPE II (9\")",61700,7.5,462750]
["","","EPOXY PAVEMENT MARKING LINES","(BLACK) 6\"",54201,0.45,24390.45]
["","","HOT SPRAY THERMOPLASTIC","PAVEMENT MARKING LINES, 6\" 50 MILS",121987,0.72,87830.64]
["","","","PAVEMENT MARKING LINES,12\" 50 MILS",16802,1.73,29067.46]
["","","HOT SPRAY THERMOPLASTIC PAVEMENT","MARKING LINES (12\", 50MILS)",11787,2,23574]
["","","","MARKING LINES (6\", 50MILS)",204673,0.7,143271.1]
["","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES (4\", 50 MILS)",20200,0.35,7070]
["","","HOT SPRAY THERMOPLASTIC PAVEM-","ENT MARKING LINES, 4\", 40 MIL",233495,0.38,88728.1]
["","","","ENT MARKING LINES, 4\", 40 MIL",838035,0.34,284931.90000000002]
["","","THERMO PVT MKG LINES, 4\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",387597,0.86332845713460005,334623.52]
["","","THERMO PVT MKG LINES, 4\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",197914,0.95,188018.3]
["","","THERMO PVT MKG LINES, 4\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",178130,0.65,115784.5]
["","","THERMOPLASTIC PAVEMENT MARKING","LINES (12\", 120MILS) (HRM)",600,8,4800]
["","","","LINES (12\", 90MILS) (HRM)",2153,7.5,16147.5]
["","","","LINES (24\", 120MILS) (HRM)",6002,16,96032]
["","","","LINES (4\", 120MILS) (HRM)",24066,1,24066]
["","","","LINES (4\", 90MILS) (HRM)",15681,0.9,14112.9]
["","","","LINES (6\", 120MILS) (HRM)",6756,1.4,9458.4]
["","","","LINES (6\", 90MILS) (HRM)",24908,1.3,32380.400000000001]
["","","","LINES (8\", 120MILS) (HRM)",1464,4,5856]
["","","","LINES (8\", 90MILS) (HRM)",3730,2.2999999999999998,8579]
["","","","LINES, 12\", 120 MILS (HRM)",2470,5.5,13585]
["","","","LINES, 12\", 90 MILS (HRM)",20072,2.1606715823037099,43369]
["","","","LINES, 24\", 120 MILS (HRM)",186,20,3720]
["","","","LINES, 4\", 120 MILS (HRM)",136893,1.04068659463961,142462.71]
["","","","LINES, 4\", 90 MILS (HRM)",110352,0.90445791648542995,99808.74]
["","","","LINES, 50 MILS, 4\"",291132,0.48,139743.35999999999]
["","","","LINES, 6\", 120 MILS (HRM)",154017,1.0974058707804999,169019.16]
["","","","LINES, 6\", 90 MILS (HRM)",230111,0.98174307182186005,225909.88]
["","","","LINES, 8\", 120 MILS (HRM)",722,3,2166]
["","","","LINES, 8\", 90 MILS (HRM)",2298,3,6894]
["","","","LINES,12\", 90 MILS (HRM)",10157,1.9,19298.3]
["","","THERMOPLASTIC PAVEMENT MARKINGLINES, 4\",","120 MILS (HIGHLY REFLECTIVE MEDIA)",204662,0.75,153496.5]
["","","","90 MILS (HIGHLY REFLECTIVE MEDIA)",152140,0.69,104976.6]
["","","THERMOPLASTIC PM LINES, 12\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",265,4,1060]
["","","THERMOPLASTIC PM LINES, 24\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",550,12,6600]
["","","THERMOPLASTIC PM LINES, 4\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",8206,0.78,6400.68]
["","","THERMOPLASTIC PM LINES, 4\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",17100,0.72,12312]
["","","THERMOPLASTIC PM LINES, 8\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",3125,3,9375]
["","","THERMOPLASTIC PM LINES, 8\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",1325,2,2650]
["","","THERMOPLASTIC PROFILED","PAVEMENT MARKING LINES (EDGE LINES)",78760,0.95,74822]
["4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","COLD APPLIED PLASTIC PAVEMENT","MARKING LINES, TYPE II, (9\")",340,9,3060]
["","","THERMOPLASTIC PAVEMENT MARKING","LINES (50 MIL)",386877,0.46,177963.42]
["4895000000-N","GENERIC PVMT MARKING ITEM (EA)","IN LANE ROUTE SHIELD","",1,4000,4000]
["","","IN LANE ROUTE SHIELDS","",9,2744.4444444444398,24700]
["","","IN LANE ROUTE SHIELDS (I-85)","",9,2800,25200]
["","","REMOVE AND REPLACE SNOWPLOW-","ABLE PAVEMENT MARKERS",5720,75,429000]
["4900000000-N","PERM RAISED PVMT MARKERS","","",29036,7.1554921476787401,207766.87]
["4905000000-N","SNOWPLB PVMT MRKER","","",133893,28.717613691529799,3845087.45]
["4915000000-E","7' U-CHANNEL POSTS","","",35,77.748857142857105,2721.21]
["4935000000-N","FLEX DELINATR (CRYSTAL)","","",267,55.310861423220999,14768]
["4940000000-N","FLEX DELINATR (YELLOW)","","",233,54.8841201716738,12788]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",25,60.2,1505]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",25,53,1325]
["4955000000-N","OBJECT MARKERS (END OF RD)","","",24,161.85,3884.4]
["4957000000-N","OBJECT MARKERS (TYPE **)","(1)","",13,100,1300]
["","","(III)","",3,195,585]
["4960000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","REPLACE EXISTING BARRIER","DELINEATOR",537,28.75,15438.75]
["","","REPLACEMENT OF EXISTING","BARRIER DELINEATORS",77,25,1925]
["5000000000-E","***' HIGH MOUNT STANDARD","(60')","",2,15500,31000]
["","","(70')","",3,23000,69000]
["5005000000-E","80' HIGH MOUNT STANDARD","","",12,17250,207000]
["5010000000-E","100' HIGH MOUNT STANDARD","","",8,22336.181250000001,178689.45]
["5015000000-E","120' HIGH MOUNT STANDARD","","",12,24924.143333333301,299089.71999999997]
["5020000000-N","PORTABLE DRIVE UNIT","","",3,4882.17,14646.51]
["5025000000-E","HIGH MOUNT FOUNDS","","",289.2,812.40034578146594,234946.18]
["5045000000-N","LIT STD MTLS ************","(30' SA, 10' ARM)","",20,2300,46000]
["5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",33,3065.7575757575801,101170]
["","","(45' TA, 15' ARM)","",6,3257.58,19545.48]
["5070000000-N","STD FOUNDAT ***********","(R1)","",49,1038.8828571428601,50905.26]
["","","(R2)","",5,1050,5250]
["","","(TYPE R1)","",12,748.13,8977.56]
["","","(TYPE R2)","",4,842.495,3369.98]
["5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",6,962.5,5775]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",265,31.071698113207599,8234]
["5130000000-N","LITE CONTROL ************","(120/240V)","",1,18573.91,18573.91]
["5155000000-E","ELECT DUCT BD, SIZE *****","(1\")","",265,7.47,1979.55]
["","","(1.5\")","",425,8.01,3404.25]
["","","(2\")","",3519,6.8684057971014498,24169.919999999998]
["","","(3\")","",685,8.4534306569343105,5790.6]
["","","(3/4\")","",285,7.47,2128.9499999999998]
["","","(4\")","",120,7.75,930]
["5160000000-E","ELECT DUCT JA, SIZE *****","(2\" HDPE)","",1229,22,27038]
["","","(2\")","",640,12.8125,8200]
["","","(3\")","",2702,15.8914877868246,42938.8]
["","","(4\")","",2219,17.5302208201893,38899.56]
["","","(6\")","",105,26,2730]
["5165000000-E","** 10 W/G FEEDER CIRCUIT","(2)","",130,4.4000000000000004,572]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",3100,3.0661290322580599,9505]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",4728,4.2246785109983103,19974.28]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2)","",4695,4.6871671991480302,22006.25]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(2)","",390,5.9948717948717896,2338]
["5200000000-E","**-10 W/G FEEDR N *****\"","(2, 1.5\")","",1020,13.59,13861.8]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2, 1.5)","",8590,14.714086146682201,126394]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",20822,8.0468485255979303,167551.48000000001]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",16880,8.3671949052132693,141238.25]
["5220000000-E","**-2 W/G FEEDER N *****\"","(2, 1.5)","",4945,9.6496461071789703,47717.5]
["5240000000-N","ELEC JB ************","(CS36)","",2,1456.175,2912.35]
["","","(CSJB, 36\" X 24\")","",5,1250,6250]
["","","(HM18)","",7,564.24,3949.68]
["","","(HMJB, 18\" X 12\")","",21,490,10290]
["","","(HMJB, 30\" X 17\")","",5,740,3700]
["","","(HMJB, 36\" X 24\")","",4,1250,5000]
["","","(IG11)","",1,382.69,382.69]
["","","(IG18)","",18,535.74,9643.32]
["","","(IG30)","",2,868.68,1737.36]
["","","(IG36)","",4,1175,4700]
["","","(IGJB, 18\" X 12\")","",35,490,17150]
["","","(IGJB, 30\" X 17\")","",5,740,3700]
["","","(IGJB, 36\" X 24\")","",8,1250,10000]
["","","(LS18)","",14,558.68857142857098,7821.64]
["","","(LSJB, 18\" X 12\")","",2,490,980]
["","","(STANDARD SIZE)","",18,450,8100]
["","","ELECTRICAL JUNCTION BOXES PC18","",57,255,14535]
["","","ELECTRICAL JUNCTION BOXES PC30","",7,420,2940]
["","","ELECTRICAL JUNCTION BOXES PC36","",1,1015,1015]
["5252000000-N","UNDERPASS LUMINARIES *****","(TYPE PM, LED, 62W)","",10,525,5250]
["5253000000-N","UNDERPASS CIRCUITRY *************","(STATION 15+58)","",1,6233.14,6233.14]
["","","LAWNDALE DRIVE, UPL-1","",1,8600,8600]
["5255000000-N","PORTABLE LIGHTING","","",46,241650.154130435,11115907.09]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","LUMINAIRE STORAGE","",2,952.2,1904.4]
["","","PRIMARY ELECTRICAL SERVICE","",1,11567.96,11567.96]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","100' HIGH MOUNT LUMINAIRE - LED","",36,1642.06833333333,59114.46]
["","","120' HIGH MOUNT LUMINAIRE - LED","",96,1613.5333333333299,154899.20000000001]
["","","240/480V LIGHTING CONTROL SYSTEM","",5,8340,41700]
["","","60' HIGH MOUNT LUMINAIRE - LED","",8,1160,9280]
["","","80' HIGH MOUNT LUMINAIRE - LED","",96,1160,111360]
["","","COMMUNICATION GATEWAY","",6,4504.1666666666697,27025]
["","","CONTROL NODE","",297,144.747474747475,42990]
["","","HIGH MOUNT LUMINAIRE - LED","",30,1550,46500]
["","","INSTALL ROADWAY LIGHT STANDARD","LUMINAIRE",12,173.74,2084.88]
["","","LIGHTING CONTROL SYSTEM","",1,10150,10150]
["","","PEDESTRIAN LIGHT STANDARD - 100W LED","",6,3725.94,22355.64]
["","","PEDESTRIAN LIGHT STANDARD - 60W LED","",5,3509.17,17545.849999999999]
["","","RELOCATE HIGH MOUNT LIGHT","STANDARD",4,28270,113080]
["","","RELOCATE HIGH MOUNT LIGHT STANDARD","",2,5755.07,11510.14]
["","","REMOVE LIGHT STANDARD","",28,260.61,7297.08]
["","","REMOVE LIGHT STANDARD FOUNDATION","",28,1031.57,28883.96]
["","","ROADWAY LIGHT STANDARD","LUMINAIRE 185W LED",8,860,6880]
["","","ROADWAY LIGHT STANDARD LUMIN-","AIRE - 285W LED",2,815,1630]
["","","ROADWAY LIGHT STANDARD LUMINAIRE -","285W LED",43,740,31820]
["","","SMART CONTROL NODE","",22,148.92454545454501,3276.34]
["","","UNDERPASS LUMINAIRE - LED","",12,920.76,11049.12]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",8,499.10124999999999,3992.81]
["5325000000-E","**\" WATER LINE","(36\")","",1215,433.36,526532.4]
["5325300000-E","3\" WATER LINE","","",7,178.97,1252.79]
["5325400000-E","4\" WATER LINE","","",1125,73.253351111111101,82410.02]
["5325600000-E","6\" WATER LINE","","",5226,89.147516264829704,465884.92]
["5325800000-E","8\" WATER LINE","","",21986,49.629487855908302,1091153.9199999999]
["5326000000-E","10\" WATER LINE","","",2764,111.163314037627,307255.40000000002]
["5326200000-E","12\" WATER LINE","","",26607,90.960282632390005,2420180.2400000002]
["5326600000-E","16\" WATER LINE","","",5938,148.23648703267099,880228.26]
["5327000000-E","20\" WATER LINE","","",1641,205.54402193784301,337297.74]
["5327400000-E","24\" WATER LINE","","",26534,163.758473656441,4345167.34]
["5328000000-E","30\" WATER LINE","","",476,330.77,157446.51999999999]
["5329000000-E","DI H2O PIPE FITTINGS","","",351004,8.8219568722863606,3096542.15]
["5534000000-E","**\" VALVE","(36\")","",4,66882.31,267529.24]
["5538000000-E","4\" VALVE","","",8,1371.5574999999999,10972.46]
["5540000000-E","6\" VALVE","","",84,1628.9314285714299,136830.24]
["5546000000-E","8\" VALVE","","",55,1926.9259999999999,105980.93]
["5552000000-E","10\" VALVE","","",10,2519.44,25194.400000000001]
["5558000000-E","12\" VALVE","","",56,3273.35089285714,183307.65]
["5558600000-E","16\" VALVE","","",9,9477.1722222222197,85294.55]
["5559000000-E","20\" VALVE","","",3,15726.78,47180.34]
["5559400000-E","24\" VALVE","","",22,22535.445454545501,495779.8]
["5560000000-E","30\" VALVE","","",4,44203.16,176812.64]
["5571000000-E","**\" TAPPING SLEEVE & VALVE","(1\")","",15,710,10650]
["5571600000-E","6\" TAPPING SLEEVE & VALVE","","",10,6685.3639999999996,66853.64]
["5571800000-E","8\" TAPPING SLEEVE & VALVE","","",5,9147.1759999999995,45735.88]
["5572000000-E","10\" TAPPING SLEEVE & VALVE","","",2,13000,26000]
["5572200000-E","12\" TAPPING SLEEVE & VALVE","","",5,11660,58300]
["5588000000-E","*\" AIR RELEASE VALVE","(12\")","",3,7233.3333333333303,21700]
["5589100000-E","1\" AIR RELEASE VALVE","","",1,1435,1435]
["5589200000-E","2\" AIR RELEASE VALVE","","",35,8147.68857142857,285169.09999999998]
["5600000000-E","**\" BLOW OFF","(1\")","",1,3151.2,3151.2]
["5606000000-E","2\" BLOW OFF","","",6,3621.1666666666702,21727]
["5606400000-E","4\" BLOW OFF","","",1,5100,5100]
["5606800000-E","8\" BLOW OFF","","",3,8068.2133333333304,24204.639999999999]
["5643000000-E","**\" WATER METER","(1\")","",7,840,5880]
["5643100000-E","3/4\" WATER METER","","",7,440,3080]
["5643150000-E","1-1/2\" WATER METER","","",2,6050,12100]
["5643200000-E","2\" WATER METER","","",6,8208.3333333333303,49250]
["5648000000-N","RELOCATE WATER METER","","",196,1602.4849999999999,314087.06]
["5649000000-N","RECONNECT WATER METER","","",114,1147.4834210526301,130813.11]
["5656000000-E","**\" RPZ BACKFLOW PREVNT ASMBLY","(3/4\")","",1,5690.17,5690.17]
["5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1\")","",3,1133.73,3401.19]
["5656200000-E","2\" RPZ BACKFLOW PREVNT ASMBLY","","",1,5921.6,5921.6]
["5656210000-E","RELC 2\" RPZ BACKFLOW PREVNT A","","",1,850,850]
["5656600000-E","6\" RPZ BACKFLOW PREVNT ASMBLY","","",1,14370.35,14370.35]
["5666000000-N","FIRE HYDRANT","","",54,5191.9027777777801,280362.75]
["5672000000-N","RELOCATE FIRE HYDRANT","","",89,3629.2611235955101,323004.24]
["5673000000-E","FIRE HYDRANT LEG","","",2244,48.028400178253101,107775.73]
["5678400000-E","6\" LINE STOP","","",4,11697,46788]
["5678600000-E","8\" LINE STOP","","",8,11275.2,90201.600000000006]
["5678800000-E","10\" LINE STOP","","",4,10842.5,43370]
["5679000000-E","12\" LINE STOP","","",7,15054.285714285699,105380]
["5685800000-E","30\" LINE STOP W/ BYPASS","","",1,265000,265000]
["5686000000-E","**\" H2O SERVICE LINE","(2\")","",437,43.825125858123599,19151.580000000002]
["","","(3/4\")","",3678,16.989999999999998,62489.22]
["","","(4\")","",217,77.157142857142901,16743.099999999999]
["5686500000-E","WATER SERVICE LINE","","",6687,27.0203454463885,180685.05]
["5691100000-E","4\" SANITARY GRAVITY SEWER","","",160,100.8125,16130]
["5691200000-E","6\" SANITARY GRAVITY SEWER","","",35,105,3675]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",15864,142.349282652547,2258229.02]
["5691400000-E","10\" SANITARY GRAVITY SEWER","","",180,189.88,34178.400000000001]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",4451,197.40788811503,878662.51]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",2042,217.556214495593,444249.79]
["5691800000-E","20\" SANITARY GRAVITY SEWER","","",1077,341.55198700092899,367851.49]
["5691900000-E","24\" SANITARY GRAVITY SEWER","","",504,801,403704]
["5709000000-E","**\" FORCE MAIN SEWER","(2-3/4\")","",202,47.45,9584.9]
["","","(30\")","",585,300,175500]
["5709300000-E","6\" FORCE MAIN SEWER","","",733,81.766712141882707,59935]
["5709400000-E","8\" FORCE MAIN SEWER","","",7307,42.1,307624.7]
["5709600000-E","12\" FORCE MAIN SEWER","","",21754,81.101183690355796,1764275.15]
["5709700000-E","16\" FORCE MAIN SEWER","","",762,210.83,160652.46]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",109,1779.7642201834899,193994.3]
["5768500000-E","SEWER SERVICE LINE","","",1929,42.395127008812899,81780.2]
["5769000000-E","DI SEWER PIPE FITTINGS","","",37695,9.5738811513463293,360887.45]
["5775000000-E","4' DIA UTILITY MANHOLE","","",247,3870.25129554656,955952.07]
["5776000000-E","5' DIA UTILITY MANHOLE","","",34,5052.0035294117697,171768.12]
["5780000000-E","UTILITY MANHOLE WALL **' DIA","(4')","",8.8000000000000007,530,4664]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",425.3,329.077051493064,139956.47]
["5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",130,467.56569230769202,60783.54]
["5798000000-E","ABANDON **\" UTILITY PIPE","(15\")","",659,27.548194233687401,18154.259999999998]
["","","(2\")","",1051,5.25,5517.75]
["","","(2-3/4\")","",190,5.25,997.5]
["","","(21\")","",820,43.8409756097561,35949.599999999999]
["","","(36\")","",2109,85.557467994310102,180440.7]
["","","(8\")","",2272,15.15,34420.800000000003]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",7006,13.594833000285499,95245.4]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",31557,9.8680891719745194,311407.28999999998]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",8126,19.365616539502799,157365]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",61719,15.587041915779601,962016.64]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",4142,37.782339449541297,156494.45000000001]
["5811000000-E","ABANDON 18\" UTILITY PIPE","","",524,43,22532]
["5812000000-E","ABANDON 20\" UTILITY PIPE","","",1282,34.192683307332302,43835.02]
["5813000000-E","ABANDON 24\" UTILITY PIPE","","",1780,41.769123595505597,74349.039999999994]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",948,32.580485232067502,30886.3]
["5815000000-N","REMOVE WATER METER","","",92,1013.70739130435,93261.08]
["5815500000-N","REMOVE FIRE HYDRANT","","",40,2085.7080000000001,83428.320000000007]
["5816000000-N","ABANDON UTILITY MANHOLE","","",100,1523.7881,152378.81]
["5828000000-N","REMOVE UTILITY MANHOLE","","",22,1617.21454545455,35578.720000000001]
["5835000000-E","**\" ENCASEMENT PIPE","(42\")","",260,295,76700]
["","","(48\")","",1042,435.16046065259098,453437.2]
["5835600000-E","12\" ENCASEMENT PIPE","","",198,154.494949494949,30590]
["5835700000-E","16\" ENCASEMENT PIPE","","",440,124.057954545455,54585.5]
["5835800000-E","18\" ENCASEMENT PIPE","","",789,218.53231939163501,172422]
["5835900000-E","20\" ENCASEMENT PIPE","","",1928,141.36545643153499,272552.59999999998]
["5836000000-E","24\" ENCASEMENT PIPE","","",1379,150.44568527918801,207464.6]
["5836200000-E","30\" ENCASEMENT PIPE","","",1642,252.00840438489601,413797.8]
["5836400000-E","36\" ENCASEMENT PIPE","","",2692,229.77559435364,618555.9]
["5872500000-E","BORE & JACK **\"","(12\")","",80,625,50000]
["","","(16\")","",90,740,66600]
["","","(18\")","",589,1032.9779286927001,608424]
["","","(20\")","",185,606.57837837837803,112217]
["","","(24\")","",981,659.08256880733995,646560]
["","","(30\")","",138,940,129720]
["","","(36\")","",51,880,44880]
["","","(42\")","",260,1265,328900]
["","","(48\")","",402,1920,771840]
["5872600000-E","DIRECT DRILL **\"","(24\")","",815,1990,1621850]
["","","(8\")","",315,390,122850]
["5875000000-N","CONC PIERS","","",2,3462.16,6924.32]
["5882000000-N","GENERIC UTILITY ITEM (EA)","10\" PLUG VALVE","",1,7365,7365]
["","","12\" GATE VALVE ASSEMBLY","",19,4990,94810]
["","","12\" INSERT VALVE","",2,21000,42000]
["","","12\" INSERTION VALVE ASSEMBLY","",3,20713.333333333299,62140]
["","","12\" PLUG VALVE","",24,8945,214680]
["","","12\" x 16\" TAPPING SLEEVE AND","VALVE ASSEMBLY",1,22820,22820]
["","","16 INCH INSERTION VALVE","",1,45500,45500]
["","","16 INCH LINE STOP","",1,27100,27100]
["","","16\" BUTTERFLY VALVE","",2,9453.6,18907.2]
["","","16\" INSERT VALVE","",1,36764,36764]
["","","30\" PLUG VALVE ASSEMBLY","",1,82000,82000]
["","","6\" GATE VALVE ASSEMBLY","",3,1200,3600]
["","","8\" GATE VALVE ASSEMBLY","",7,1700,11900]
["","","8\" PLUG VALVE","",1,6315,6315]
["","","ABANDON SEWER CONNECTION","",2,654,1308]
["","","ARV MANHOLE ASSEMBLY (POTABLE WATER)","",1,7100,7100]
["","","BLOW OFF ASSEMBLY","",11,1750,19250]
["","","BREAKDOWN & CAP EXISTING MAN- HOLE","",1,1400,1400]
["","","BYPASS CONNECTION ASSEMBLY","ABANDONMENT",2,5000,10000]
["","","COMBINATION AIR VALVE ASSEMBLY","(SANITARY)",1,8650,8650]
["","","CONNECTION TO EXISTING 16-INCH","WATER MAIN",2,6100,12200]
["","","CONNECTION TO EXISTING 6-INCH","FORCE MAIN",2,5800,11600]
["","","CONNECTION TO EXISTING WATER- LINE","",3,3090,9270]
["","","CUT AND CAP EXISTING WATER LINE","",1,3090,3090]
["","","FIRE HYDRANT ASSEMBLY","",9,5530,49770]
["","","RECONNECT TO EXISTING 6\" WATER","LINE",1,660,660]
["","","RELOCATE WATER METER WITH","BACKFLOW PREVENTER",1,2225,2225]
["","","RELOCATE WATER MONITORING STATION","",1,725,725]
["","","REMOVE EXISTING VAULT","",2,4638.9049999999997,9277.81]
["","","REUSE TEMPORARY INTERCONNECT","",1,23650,23650]
["","","THRUST COLLAR","",6,2000,12000]
["5888000000-E","GENERIC UTILITY ITEM (LF)","12\" DIA C900 RJ PVC REUSE WATER MAIN","",7488,61.2,458265.59999999998]
["","","12\" DIA DUCTILE IRON,","CLASS 350 WATER MAIN",8218,55.6,456920.8]
["","","12\" RESTRAINED JOINT ADDER FOR","DI WATER MAIN",1401,20.2,28300.2]
["","","16 INCH CLASS 350 DUCTILE IRON","WATER DISTRIBUTION PIPE",600,115,69000]
["","","16\" DIA STEEL CASING","",135,129,17415]
["","","16-INCH CLASS 350 DUCTILE IRON","CARRIER PIPE",45,210,9450]
["","","16-INCH ENCASEMENT PIPE, BY OPEN CUT","",45,305,13725]
["","","16-INCH RESTRAINED JOINT ADDER","FOR DUCTILE IRON WATER PIPE",410,51,20910]
["","","30-INCH ENCASEMENT PIPE, BY OPEN CUT","",45,360,16200]
["","","6\" DIA C900 RJ PVC REUSE WATER MAIN","",103,31.4,3234.2]
["","","6\" DIA DUCTILE IRON, CLASS 350WATER MAIN","",44,43.3,1905.2]
["","","6\" RESTRAINED JOINT ADDER FOR","DI WATER MAIN",44,11,484]
["","","6-INCH C-900 DR 18 PVC CARRIERPIPE","",45,122,5490]
["","","6-INCH C-900 DR 18 PVC RE-","TRAINED JOINT FORCE MAIN",800,60,48000]
["","","8\" CURED IN PLACE PIPE","",517,101,52217]
["","","8\" DIA C900 RJ PVC REUSE WATER MAIN","",637,39,24843]
["","","8\" DIA DUCTILE IRON, CLASS 350WATER MAIN","",155,41,6355]
["","","8\" RESTRAINED JOINT ADDER FOR","DI WATER MAIN",155,12.9,1999.5]
["","","ABANDON EXISTING 16-INCH WATER","DISTRIBUTION PIPE",565,55,31075]
["","","ADJUST 48\" FRP MANHOLE RISER","",52,1852.42,96325.84]
["","","POLYETHYLENE ENCASEMENT","",100,17.420000000000002,1742]
["5906000000-E","GENERIC UTILITY ITEM (LB)","DUCTILE IRON FITTINGS","",18580,10.335522066738401,192034]
["","","DUCTILE IRON WATER PIPE FITTINGS","",4970,8,39760]
["5912000000-N","GENERIC UTILITY ITEM (LS)","6\" WATER METER ASSEMBLY IN VAULT","",1,30000,30000]
["","","RELOCATE 3\" PRESSURE REDUCING","VALVE WITH MANHOLE",1,7783.21,7783.21]
["","","RELOCATE 3\" WM ASSEMBLY WITH","NEW VAULT",1,27825.62,27825.62]
["","","REMOVAL OF TEMPORARY BYPASS PIPING","",1,6500,6500]
["","","REMOVE METER VAULT","",1,4250,4250]
["","","TEMPORARY SANITARY SEWER BY-","PASS PUMBING",1,73110,73110]
["","","","PASS PUMPING",1,34000,34000]
["","","TEMPORARY WATER SERVICE","",1,232000,232000]
["","","WATER LINE CONNECTION/ACTIVA-","TION",1,9200,9200]
["6000000000-E","TEMP SILT FENCE","","",1022216,2.13053596304499,2177867.9500000002]
["6006000000-E","EROS CONTRL STONE CL A","","",36540,39.391435413245802,1439363.05]
["6009000000-E","EROS CONTRL STONE CL B","","",149932,27.795866326067799,4167489.83]
["6012000000-E","SEDIMENT CONTROL STONE","","",168796,14.342539396668201,2420963.2799999998]
["6015000000-E","TEMP MULCHING","","",2197.64,903.52006698094306,1985611.84]
["6018000000-E","SEED FOR TEMP SEEDING","","",108763,2.9520048178148799,321068.90000000002]
["6021000000-E","FERT FOR TEMP SEEDING","","",584.24,854.75114678899104,499379.81]
["6024000000-E","TEMP SLOPE DRAINS","","",94406,12.060784695888,1138610.44]
["6029000000-E","SAFETY FENCE","","",58700,2.2065247018739398,129523]
["6030000000-E","SILT EXCAVATION","","",473670,3.3451079865729301,1584477.3]
["6036000000-E","MATTING FOR EROS CONTROL","","",1988800,1.1375251910699899,2262310.1]
["6037000000-E","COIR FIBER MAT","","",27100,4.66413653136531,126398.1]
["6038000000-E","PERM SOIL REINF MAT","","",48572,5.1721125339701901,251219.85]
["6042000000-E","1/4\" HARDWARE CLOTH","","",182636,4.25590239602269,777280.99]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",2180,4.8468348623853199,10566.1]
["6045000000-E","**\" TEMP PIPE","(18\")","",1555,31.465659163987102,48929.1]
["","","(24\")","",1652,48.0060532687651,79306]
["","","(30\")","",475,35.421684210526301,16825.3]
["","","(36\")","",540,67.1388888888889,36255]
["","","(42\")","",604,66.026490066225193,39880]
["","","(48\")","",124,75,9300]
["","","(54\")","",220,82,18040]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",1450,52.671724137931001,76374]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",9408,26.115125425170099,245691.1]
["6069000000-E","STILLING BASINS","","",7172,8.7665114333519192,62873.42]
["6070000000-N","SPECIAL STILLING BASINS","","",227,429.69427312775298,97540.6]
["6071010000-E","WATTLE","","",85987,6.2076797655459499,533779.76]
["6071012000-E","COIR FIBER WATTLE","","",73869,7.5686945809473496,559091.9]
["6071013000-E","WATTLE BARRIER","","",32310,13.8493655215104,447473]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",3296.5,13.5375337479145,44626.48]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",55856,8.1791383199656291,456853.95]
["6071030000-E","COIR FIBER BAFFLE","","",100800,4.3685724206349201,440352.1]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",360,1124.8891388888901,404960.09]
["","","(2\")","",67,1048.6429850746299,70259.08]
["","","(2-1/2\")","",12,1059.04833333333,12708.58]
["","","(3\")","",8,1733.6775,13869.42]
["","","(4\")","",9,1448.48,13036.32]
["","","(5\")","",1,2426.34,2426.34]
["6084000000-E","SEEDING AND MULCHING","","",2296.84,1886.0450053116499,4331943.6100000003]
["6087000000-E","MOWING","","",1165.05,129.032015793314,150328.75]
["6090000000-E","SEED FOR REPAIR SEEDING","","",27038,5.3004667504993002,143314.01999999999]
["6093000000-E","FERT FOR REPAIR SEEDING","","",97.15,1028.79382398353,99947.32]
["6096000000-E","SEED FOR SUPP SEEDING","","",43925,3.65389299943085,160497.25]
["6102000000-E","SODDING","","",7270,7.4,53798]
["6105000000-E","WATER","","",135,185,24975]
["6108000000-E","FERTILIZER TOPDRESSING","","",1293.25,874.30731877053904,1130697.94]
["6111000000-E","IMPERVIOUS DIKE","","",8171,39.1017194957778,319500.15000000002]
["6114500000-N","SPECIALIZED HAND MOWING","","",1010,66.228811881188093,66891.100000000006]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",2369,175.38168847615,415479.22]
["6117500000-N","CONC WASHOUT STR","","",307,1075.84892508143,330285.62]
["6120000000-E","CULVERT DIVERSION CHANNEL","","",9940,21.598394366197201,214688.04]
["6123000000-E","REFORESTATION","","",57.39,2406.5316257187701,138110.85]
["6126000000-E","STREAMBANK REFORESTATION","","",1.52,4433.3026315789502,6738.62]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","CONCRETE WASHOUT STRUCTURE","",17,843.52941176470597,14340]
["","","FABRIC INSERT INLET PROTECTION","DEVICE",8,200,1600]
["","","","DEVICE CLEAN-OUT",16,85,1360]
["","","","DEVICE CLEANOUT",1205,131.48517842323699,158439.64000000001]
["","","FABRIC INSERT INLET PROTECTION DEVICE","",50,131.26,6563]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",399,154.03714285714301,61460.82]
["","","FILTER SACK INLET PROTECTION","",20,200,4000]
["","","FILTER SACK INLET PROTECTION CLEANOUT","",50,200,10000]
["","","FLOCCULANT BLOCK","",40,185,7400]
["","","SEDIMENT TUBE","",20,200,4000]
["","","SUPPLEMENTAL RESPONSE FOR","EROSION CONTROL",10,500,5000]
["6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","REMOVAL OF EROSION CONTROL DEVICES","",1,65000,65000]
["6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","COMPOST BLANKET","",5,8250,41250]
["6138000000-E","GENERIC EROSION CONTROL ITEM (CY)","COMPOST BLANKET","",430,25,10750]
["6640000000-N","GENERIC PLANTING ITEM (EA) 1670","HEMEROCALLIS X 'AZTEC GOLD' (1 CONT.)","",472,12.6,5947.2]
["","","ILEX CORNUTA 'CARISSA' (5 CONT 24\")","",92,75.5,6946]
["","","ILEX GLABRA 'COMPACTA' (3 CONT 18\")","",357,28.5,10174.5]
["","","ILEX VOMITORIA 'SCHILLINGS","DWARF' (3 CONT 18\")",357,28.5,10174.5]
["","","LIRIOPE MUSCARI 'EVERGREEN","GIANT' (1 CONT)",2755,6.5,17907.5]
["","","MUHLENBERGIA CAPILLARIS (1 CONT 24\")","",760,10.75,8170]
["","","PANICUM VIRGATUM 'SHENENDOAH'","(1 CONT 24\")",457,14.25,6512.25]
["","","PENNISETUM ALOPECUROIDES","'HAMELN' (1 CONT 18\")",167,14.25,2379.75]
["","","PRUNUS X OKAME (B & B 2.5\" CAL 8-10')","",125,442,55250]
["6650000000-E","MULCH FOR PLANTING","","",368,79,29072]
["6675000000-E","GENERIC PLANTING ITEM (SY)","CYNODON DACTYLON 'TIFGRAND'","",7657,1.05,8039.85]
["6900000000-E","TOPSOIL","","",2132,60,127920]
["7000000000-E","PEDEST SIG HEAD (**************)","(16\", 1 SECTION W/ COUNTDOWN)","",8,1100,8800]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",183,833.70076502732195,152567.24]
["7060000000-E","SIGNAL CABLE","","",251474,2.5684587671091199,645900.6]
["7096000000-E","VEHICLE SIGNAL HD (8\", 3 SECT)","","",19,911.05,17309.95]
["7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",1,388.9,388.9]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",1197,755.55852965747704,904403.56]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",232,874.31788793103499,202841.75]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",86,1246.06802325581,107161.85]
["7180000000-N","BACKPLATE","","",77,96.168831168831204,7405]
["7204000000-N","LOUVER","","",24,219.495,5267.88]
["7252000000-E","MESSENGER CABLE (1/4\")","","",85890,2.0445092560251501,175602.9]
["7264000000-E","MESSENGER CABLE (3/8\")","","",47222,4.6375678709076302,218995.23]
["7279000000-E","TRACER WIRE","","",265035,0.56287226215406005,149180.85]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",755,20.303642384105999,15329.25]
["","","(2, 2\")","",260,15.5,4030]
["7300000000-E","UNPAVED TRENCH (***********)","(1 CONDUIT, 2\")","",10,10,100]
["","","(1, 2\")","",70728,7.0294770105191704,497180.85]
["","","(2, 2\")","",171460,6.0155951825498697,1031433.95]
["","","(3, 2\")","",3895,8.9544287548138595,34877.5]
["","","(4, 2\")","",50,14,700]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",11850,4.4590928270042198,52840.25]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",7032,14.510547497155899,102038.17]
["","","(1,2\")","",1305,16,20880]
["","","(2, 2\")","",42015,15.6331464952993,656826.65]
["","","(3, 2\")","",3000,19.266666666666701,57800]
["","","(4, 2\")","",130,18.600000000000001,2418]
["7312000000-N","JUNCTION BOX (***************)","(OVER-SIZED, HEAVY-DUTY)","",129,382.5,49342.5]
["","","(SPECIAL SIZE, HEAVY-DUTY)","",9,2525,22725]
["","","(SPECIAL-SIZE, HEAVY-DUTY)","",12,855,10260]
["","","(SPECIAL-SIZED)","",38,647.49,24604.62]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",908,336.744537444934,305764.03999999998]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",411,555.55603406325997,228333.53]
["7360000000-N","WOOD POLE","","",194,1106.2604639175299,214614.53]
["7372000000-N","GUY ASSEMBLY","","",685,451.83167883211701,309504.7]
["7384000000-E","***\" RISER WITH **************","(1-1/2\" RISER W/ WEATHERHEAD)","",5,270,1350]
["","","(1.25\", HEAT SHRINK TUBING)","",11,381.1,4192.1000000000004]
["","","(2\", HEAT SHRINK TUBING)","",77,452.08,34810.160000000003]
["7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",26,318.62923076923101,8284.36]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",66,347.74409090909103,22951.11]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",191,465.62298429319401,88933.99]
["7430000000-N","HEAT SHRINK TUB KIT","","",5,125,625]
["7432000000-E","2\" RISER WITH TUBING","","",59,540.16677966101702,31869.84]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",332231,7.0993274257971102,2358616.65]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",414217,1.7134815084846799,709753.17]
["","","(3/8\")","",200,6,1200]
["7481000000-N","SITE SURVEY","","",23,1251.69,28788.87]
["7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",47,650.781276595745,30586.720000000001]
["7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",86,3434.7832558139498,295391.35999999999]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",18,8254.8805555555591,148587.85]
["7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",56,681.030714285714,38137.72]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",77440,1.3979836002066099,108259.85]
["","","(144)","",47805,2.9986193912770598,143349]
["","","(24)","",216672,1.6999653854674299,368334.9]
["","","(36)","",119155,1.73329780537955,206531.1]
["","","(48)","",38830,1.64,63681.2]
["","","(72)","",126450,1.98,250371]
["7528000000-E","DROP CABLE","","",100220,1.5099570943923399,151327.9]
["7540000000-N","SPLICE ENCLOSURE","","",251,1853.51362549801,465231.92]
["7541000000-N","MOD SPLICE ENCLOSURE","","",17,1885.89176470588,32060.16]
["7552000000-N","INTERCONNECT CENTER","","",295,1437.9266440678,424188.36]
["7564100000-N","FIBER-OPTIC TRANS SELF HEAL","","",1,1575.6,1575.6]
["7566000000-N","DELINEATOR MARKER","","",340,123.350764705882,41939.26]
["7574000000-N","FURN FIB-OPT TRANSCEIVER","","",1,1575.6,1575.6]
["7574500000-N","FURN WIRELESS RADIO MODEM","","",1,2385,2385]
["7574550000-N","FURN WRLESS LIGHTNING ARSTR","","",1,260,260]
["7575142000-N","900MHZ SPECTRUM RADIO","","",15,4196.45,62946.75]
["7575142010-N","900MHZ SER/ETH SPEC RADIO","","",11,4035,44385]
["7575142060-N","MOD RADIO INSTALL","","",5,523.52800000000002,2617.64]
["7575142200-N","NEW ELECTRICAL SERVICE","","",10,1270.47,12704.7]
["7575160000-E","REM EXT COMM CABLE","","",38370,0.81218139171227999,31163.4]
["7575180000-N","CABLE TRANSFER","","",21,180.67809523809501,3794.24]
["7575200000-N","GPS UNIT","","",2,1091.03,2182.06]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",143,9162.94839160839,1310301.6200000001]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",63,16165.8103174603,1018446.05]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",8,21869.552500000002,174956.42]
["7613000000-N","SOIL TEST","","",232,1039.8347413793099,241241.66]
["7614100000-E","DRILLED PIER FOUND","","",1586,869.54069356872606,1379091.54]
["7630000000-N","METAL STRAIN POLE DESIGN","","",5,105,525]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",70,224.16414285714299,15691.49]
["7636000000-N","SIGN FOR SIGNALS","","",363,376.98586776859503,136845.87]
["7642100000-N","TYPE I POST W/ FOUND","","",56,1132.85035714286,63439.62]
["7642200000-N","TYPE II PED W/ FOUND","","",124,1709.45564516129,211972.5]
["7642300000-N","TYPE III PED W/ FOUND","","",2,3700,7400]
["7675000000-N","LED BLANKOUT SIGN","","",5,3668.56,18342.8]
["7684000000-N","SIGNAL CABINET FOUND","","",117,1011.55333333333,118351.74]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",27,881.02814814814803,23787.759999999998]
["7687000000-N","MODIFY FOUND FOR CONTRLR CBNT","","",6,965.61,5793.66]
["7696000000-N","CONTLRS WITH CBNT (**************)","(2070, BASE MOUNTED)","",1,15366.81,15366.81]
["","","(2070E, BASE MOUNTED)","",2,12693.7,25387.4]
["","","(2070LX, 332)","",133,10833.47,1440851.51]
["","","(2070LX, 336S)","",67,9563.2099999999991,640735.06999999995]
["","","(TYPE 2070E, BASE MOUNTED)","",24,13516.125,324387]
["","","(TYPE 2070E, POLE MOUNTED)","",2,13625,27250]
["7708000000-N","DETECTOR CARD (***********)","(2070)","",22,143.94772727272701,3166.85]
["","","(MODEL 222)","",946,75.45,71375.7]
["","","(TYPE 2070)","",30,105,3150]
["","","(TYPE 2070E)","",54,125,6750]
["7744000000-N","DETECTOR CARD (TYPE 170)","","",85,131.749411764706,11198.7]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",36,13000.4580555556,468016.49]
["7768000000-N","CONTLR WITH CBNT, 2070L POLE MTD","","",6,11867.333333333299,71204]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",277,131.06317689530701,36304.5]
["7852000000-N","DETECTOR CARD (NEMA TS-2)","","",156,152.88461538461499,23850]
["7901000000-N","CABINET BASE EXTENDER","","",135,398.34807407407402,53776.99]
["7901010000-N","CABINET BASE ADAPTER","","",8,409.8,3278.4]
["7912000000-N","BEACON CNTRL ASSM & CBNT *****","(TYPE F3)","",2,1600,3200]
["7948000000-N","TRAFFIC SIGNAL REMOVAL","","",7,5651.4228571428603,39559.96]
["7960000000-N","METAL POLE FOUND REMVL","","",26,1776.0707692307701,46177.84]
["7972000000-N","METAL POLE REMOVAL","","",26,884.32346153846197,22992.41]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","10KVA SINGLE PHASE TRANSFORMER","",2,1825,3650]
["","","2.4 GHZ ETHERNET RADIO","",2,4374.1099999999997,8748.2199999999993]
["","","2.4GHZ BROADBAND ETHERNET RADIO","",3,3450,10350]
["","","5/8\" X 10' GROUNDING ELECTRODE","",120,75.625,9075]
["","","60 FT CCTV WOOD POLE","",1,2527.96,2527.96]
["","","ANALOG CCTV CAMERA ASSEMBLY","",1,4250,4250]
["","","BRIDGE JUNCTION BOX","",10,1440,14400]
["","","CCTV CABINET (336A)","",6,4550.6499999999996,27303.9]
["","","CCTV CABINET (NEMA)","",1,3369.99,3369.99]
["","","CCTV CABINET DISCONNECT","",2,428.74,857.48]
["","","CCTV CAMERA ASSEMBLY","",18,4981.0194444444396,89658.35]
["","","CCTV CAMERA ASSEMBLY","",50,5219.5039999999999,260975.2]
["","","CCTV ELECTRICAL SERVICE","",4,1510,6040]
["","","CCTV EXTENSION POLE","",1,1190,1190]
["","","CCTV METAL POLE","",19,5423.1,103038.9]
["","","CCTV METAL POLE (40')","",1,4950,4950]
["","","CCTV METAL POLE (50')","",7,7375,51625]
["","","CCTV TEST CABINET","",1,11026.65,11026.65]
["","","CCTV WOOD POLE","",3,1603.8,4811.3999999999996]
["","","CCTV WOOD POLE (60')","",1,1470,1470]
["","","CENTRAL MEDIA CONVERTER","",1,1200,1200]
["","","COMMUNICATIONS RACK","",2,4277.07,8554.14]
["","","COMPUTER WORKSTATION","",4,4565.75,18263]
["","","CONSOLES","",2,29882.41,59764.82]
["","","CONTROLLER (TYPE 2070E)","",5,2940,14700]
["","","CONTROLLER WITH CABINET (NEMA TS-2, 2070","CONTROLLER, TYPE I CABINET, BASE MTD.)",2,24000,48000]
["","","DIGITAL CCTV CAMERA ASSEMBLY","",1,4210,4210]
["","","DIGITAL DISPLAY MONITOR","",10,6540.35,65403.5]
["","","DIGITAL DISPLAY MONITOR (RELO-CATE)","",4,284.27999999999997,1137.1199999999999]
["","","DMS","",4,70000,280000]
["","","DMS ACCESS LADDER","",4,6000,24000]
["","","DMS PEDESTAL STRUCTURE","",4,31000,124000]
["","","ENCLOSED COMMUNICATIONS RACK","",1,4615,4615]
["","","EQUIPMENT CABINET DISCONNECT","",13,610,7930]
["","","ETEHERNET EDGE SWITCH","",5,2333.48,11667.4]
["","","ETHERNET CORE SWITCH","",1,72738.45,72738.45]
["","","ETHERNET EDGE SWITCH","",259,1629.73081081081,422100.28]
["","","ETHERNET HUB SWITCH","",1,16892,16892]
["","","ETHERNET SWITCH UNIT","",1,2600,2600]
["","","FIBER OPTIC VIDEO TRANSCEIVER","W/DATE RECEIVER",1,3110,3110]
["","","FIELD EQUIPMENT CABINET","",10,4032.5,40325]
["","","FIELD ETHERNET SWITCH","",12,1325,15900]
["","","FIELD VIDEO ENCODER","",1,1710,1710]
["","","FIRESTATION PREEMPTION PUSH- BUTTON","",1,6115,6115]
["","","FIREWALL","",1,5016.1499999999996,5016.1499999999996]
["","","FURNISH 2.4 GHZ ETHERNET RADIO","",1,2570.96,2570.96]
["","","FURNISH 2018 ENHANCED CONFLICTMONITOR","",10,1018.26,10182.6]
["","","FURNISH 2070 CONTROLLER TESTER","",2,4241.22,8482.44]
["","","FURNISH 2070LX CONTROLLER","",10,1599.37,15993.7]
["","","FURNISH 332 CABINET","",7,7376.74,51637.18]
["","","FURNISH 336S CABINET","",3,2808.84,8426.52]
["","","FURNISH CCTV CABINET","",1,2789.11,2789.11]
["","","FURNISH CCTV CAMERA ASSEMBLY","",1,3135.78,3135.78]
["","","FURNISH CONFLICT MONITOR TESTER","",2,21617.23,43234.46]
["","","FURNISH DETECTOR CARD (MODEL 222)","",48,75.11,3605.28]
["","","FURNISH ETHERNET EDGE SWITCH","",13,1074.52692307692,13968.85]
["","","FURNISH FIBER-OPTIC POWER METER","",2,1882.9,3765.8]
["","","FURNISH OPTICAL LIGHT GENERA- TOR","",4,1056.69,4226.76]
["","","FURNISH VIDEO MONITOR","",1,5194.09,5194.09]
["","","FURNISH VISUAL FAULT LOCATOR","",2,1227.7,2455.4]
["","","GUY ASSEMBLY (AERIAL)","",63,348.4,21949.200000000001]
["","","GUY ASSEMBLY (SIDEWALK)","",38,515.35,19583.3]
["","","HEAT SHRINK TUBING KIT","",130,77.47,10071.1]
["","","HIGH DEFINITION CCTV CAMERA ASSEMBLY","",1,6667.1,6667.1]
["","","HUB INTERCONNECT CENTER","",1,5175,5175]
["","","ITS FIELD ETHERNET SWITCH","",11,2170,23870]
["","","ITS SERVER","",8,17426.52,139412.16]
["","","ITS SOIL TEST","",7,720,5040]
["","","JUNCTION BOX (SPECIAL OVER-","SIZED HEAVY-DUTY)",7,1460,10220]
["","","","SIZED, HEAVY DUTY)",7,670,4690]
["","","JUNCTION BOX MARKER","",71,118.58591549295799,8419.6]
["","","KVM SWITCH","",2,3230.5349999999999,6461.07]
["","","LAPTOP COMPUTER","",8,2930.1,23440.799999999999]
["","","METER BASE/DISCONNECT COMBINA-TION PANEL","",11,705,7755]
["","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",6,6307.8450000000003,37847.07]
["","","","SYSTEM-MULTIPLE ZONES",3,8647.6766666666699,25943.03]
["","","MICROWAVE VEHICLE DETECTOR -","SINGLE ZONE",3,1244.4933333333299,3733.48]
["","","MICROWAVE VEHICLE DETECTOR,","SINGLE ZONE",1,3500,3500]
["","","MODIFY ETHERNET RADIO INSTALL-ATION","",1,1220,1220]
["","","MODIFY EXISTING ELECTRICAL SERVICE","",124,469.43,58209.32]
["","","MODIFY EXISTING SPLICE","",1,516.51,516.51]
["","","MULTIZONE MICROWAVE VEHICLE","DETECTION SYSTEM-MULTIPLE ZONES",1,29551.56,29551.56]
["","","NEMA TS-2, TYPE 1 CABINET,","BASE MOUNTED W/2070LN2 CON- TROLLER",3,22500,67500]
["","","NEMA TS-2, TYPE I CABINET,","BASE MOUNTED, W/2070LN2 CONT- ROLLER",4,21020,84080]
["","","NETWORK VIDEO RECORDER","",1,7959.46,7959.46]
["","","POWDER COAT FOR DUAL MAST ARM POLE","",1,4137.22,4137.22]
["","","POWDER COAT FOR SIGNAL PEDESTAL","",2,177.31,354.62]
["","","POWDER COAT FOR SINGLE MAST ARM POLE","",1,2955.15,2955.15]
["","","PROTECTIVE COAT FOR DUAL MAST","ARM POLE (BLACK)",2,3910,7820]
["","","PROTECTIVE COAT FOR SIGNAL","PEDESTAL (BLACK)",8,68.400000000000006,547.20000000000005]
["","","PROTECTIVE COAT FOR SINGLE","MAST ARM POLE (BLACK)",14,3000,42000]
["","","PROTECTIVE COATING FOR","PUSHBUTTON POST (BLACK)",14,230,3220]
["","","PROTECTIVE COATING FOR SINGLE","MAST ARM POLE (BLACK)",16,2850,45600]
["","","PTZ JOYSTICK","",3,929.72,2789.16]
["","","REMOVE 900MHZ RADIO","",14,115,1610]
["","","REMOVE RADIO INSTALLATION","",2,480,960]
["","","REPLACE CONFLICT MONITOR","",4,1330,5320]
["","","SMALL FORM FACTOR COMPUTER","",3,6300,18900]
["","","SOIL TEST FOR CCTV METAL POLE","",1,715,715]
["","","TERMINAL SPLICE CABINET","",9,295.45,2659.05]
["","","TRAVEL TIME DYNAMIC MESSAGE SIGN","",2,35000,70000]
["","","TYPE 332 TEST CONTROLLER WITH CABINET","",1,14000,14000]
["","","TYPE 336 TEST CONTROLLER WITH CABINET","",1,13500,13500]
["","","UPS (TCC)","",1,4613.1099999999997,4613.1099999999997]
["","","VIDEO PROCESSING UNIT","",2,8135,16270]
["","","WIRELESS ACCESS POINT","",1,2311.62,2311.62]
["","","WOOD PEDESTAL","",6,360,2160]
["","","WORKSTATION","",1,2880,2880]
["","","WORKSTATION MONITOR","",19,438.83,8337.77]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","BUILDING MODIFICATIONS","",1,24500,24500]
["","","CCTV SOFTWARE (MODIFY)","",1,11000,11000]
["","","INTEGRATION AND CONFIGURATION","",1,15125,15125]
["","","MAINTENANCE MANAGEMENT SYSTEM SOFTWARE","",1,291000,291000]
["","","NETWORK MANAGEMENT SOFTWARE (MODIFY)","",1,50000,50000]
["","","SIGNAL SYSTEM SOFTWARE","",1,470000,470000]
["","","SIGNAL TIMING DATABASE CONVER-","SION SOFTWARE",1,4014.53,4014.53]
["","","SYSTEM SUPPORT SOFTWARE & DEVICES","",1,17267.900000000001,17267.900000000001]
["","","TCC BUILDING MODIFICATIONS","",1,13000,13000]
["","","TRAINING","",1,125000,125000]
["","","VIDEO MANAGEMENT SOFTWARE","",1,5300,5300]
["","","VIDEO WALL SOFTWARE","",1,103000,103000]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","4 SOLID BARE GROUNDING CONDUCTOR","",580,3.5,2030]
["","","3-WIRE COPPER FEEDER CONDUCTOR","",4880,8,39040]
["","","3-WIRE COPPER SERVICE ENTRANCECONDUCTOR","",150,7,1050]
["","","4-WIRE COPPER FEEDER CONDUCTOR","",2500,17.600000000000001,44000]
["","","AERIAL CABLE PROTECTOR","",190,9.5,1805]
["","","BACK PULL FIBER OPTIC CABLE","",400,2.7850000000000001,1114]
["","","BACK PULL FIBER OPTICS CABLE","",150,2.76,414]
["","","BACK PULL FIBER-OPTIC CABLE","",2660,1.81,4814.6000000000004]
["","","BRIDGE CONDUIT SYSTEM","",7100,89.5,635450]
["","","ETHERNET CABLE","",7185,2.5099999999999998,18034.349999999999]
["","","SERVICE CONDUCTORS","",405,3.34,1352.7]
["","","UNDERGROUND CONDUIT (1, 1\")","",75,5.68,426]
["","","UNDERGROUND CONDUIT (1, 2\")","",5637,6.77,38162.49]
["","","UNDERGROUND CONDUIT (2, 2\")","",9100,7.49,68159]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","DRILLED PIER FOUNDATION FOR","CCTV METAL POLE",6,1160,6960]
["","","ITS DRILLED PIER FOUNDATION","",49,900,44100]
["","","ITS OVERHEAD FOOTINGS","",32,900,28800]
["8007000000-N","CM&R TEMP STR ***********","(12+71.50 -DET-)","",1,120000,120000]
["","","(14+40.00 -DET-)","",1,150000,150000]
["","","(19+77.50-LDET-)","",1,992282.95,992282.95]
["","","(21+95.50 -DET1-)","",1,1366300,1366300]
["","","(28+45.42-EBL-)","",1,550000,550000]
["","","(38+50.00-DET-)","",1,300000,300000]
["8017000000-N","CM&R TEMP ACCESS ***********","(14+94.00 -L-)","",1,62500,62500]
["","","(140+21.50 -L- LT)","",1,1,1]
["","","(140+21.50 -L- RT)","",1,1,1]
["","","(15+54.50 -L-)","",1,10000,10000]
["","","(15+98.00 -L-)","",1,25000,25000]
["","","(155+02.50 -L- LT)","",1,1,1]
["","","(155+02.50 -L- RT)","",1,1,1]
["","","(18+62.50-L-)","",1,50000,50000]
["","","(19+78.50-L-)","",1,397578.9,397578.9]
["","","(21+10.00 -L-)","",1,79000,79000]
["","","(23+20.00-L-)","",1,15000,15000]
["","","(23+26.00 -L- EBL)","",1,47200,47200]
["","","(23+26.00 -L- WBL)","",1,47200,47200]
["","","(25+00.00-L-)","",1,233000,233000]
["","","(606+95.00 -L-)","",1,1,1]
["","","(64+20.00 -L-)","",1,1300000,1300000]
["","","(99+17.60 -L1-)","",1,660000,660000]
["8021000000-N","REMV EXIST STR **********","(10+53.50-L-)","",1,6000,6000]
["","","(15+54.50 -L-)","",1,50000,50000]
["","","(38+62.00-L-)","",1,22860,22860]
["8035000000-N","REMV EXIST STR **********","(12+68.00 -L-)","",1,35000,35000]
["","","(13+07.00 -L-)","",1,25000,25000]
["","","(13+25.00-L-)","",1,100000,100000]
["","","(13+52.00-L-)","",1,12000,12000]
["","","(13+70.00-L-)","",1,44590,44590]
["","","(14+21.00 -L-)","",1,38000,38000]
["","","(14+27.00-L-)","",1,25000,25000]
["","","(14+67.00-L-)","",1,40000,40000]
["","","(14+94.00 -L-)","",1,49600,49600]
["","","(15+14.00-L-)","",1,95000,95000]
["","","(15+39.55-S1-)","",1,47633,47633]
["","","(15+40.00-L-)","",1,20234.28,20234.28]
["","","(15+56.00 -L-)","",1,35000,35000]
["","","(15+98.00 -L-)","",1,130000,130000]
["","","(17+23.00-L-)","",1,65000,65000]
["","","(18+03.65-L-)","",1,310000,310000]
["","","(18+16.00-L-)","",1,17300,17300]
["","","(18+62.50-L-)","",1,125000,125000]
["","","(18+64.00 -L-)","",1,150000,150000]
["","","(19+45.50 -L-)","",1,35000,35000]
["","","(19+78.50-L-)","",1,148125.92000000001,148125.92000000001]
["","","(21+10.00 -L-)","",1,70000,70000]
["","","(22+16.89-L-)","",1,409800,409800]
["","","(23+20.00-L-)","",1,25000,25000]
["","","(23+26.00 -L- EBL)","",1,245900,245900]
["","","(23+26.00 -L- WBL)","",1,178083.02,178083.02]
["","","(23+62.98-S2-)","",1,7253,7253]
["","","(25+00.00-L-)","",1,300000,300000]
["","","(28+12.88-S2-)","",1,7253,7253]
["","","(28+17.37-Y-)","",1,113279.61,113279.61]
["","","(28+26.49-WBL-)","",1,130019,130019]
["","","(28+45.42-EBL-)","",1,130019,130019]
["","","(42+59.46-A1-)","",1,225715,225715]
["","","(43+95.83 TO 55+16.87)","",1,800000,800000]
["","","(50+61.09-L-)","",1,325000,325000]
["","","(55+88.11 -L-)","",1,135000,135000]
["","","(64+20.00 -L-)","",1,100000,100000]
["8049000000-N","REMV EXIST STR **********","(13+86.00-L-)","",1,50000,50000]
["8056000000-N","REMV EXIST STR **********","(107+88.00-L-)","",1,65239.92,65239.92]
["","","(11+51.56 -DRW1-)","",1,10000,10000]
["","","(114+23.00 -L-)","",1,1000,1000]
["","","(137+22.00-L-)","",1,22000,22000]
["","","(167+03.45 -L-)","",1,1000,1000]
["","","(168+21.00-L-)","",1,22000,22000]
["","","(21+86.00-Y6-)","",1,16000,16000]
["","","(22+17.00-Y7)","",1,11880,11880]
["","","(283+77.00-L-)","",1,23000,23000]
["","","(314+63.00-L-)","",1,50000,50000]
["","","(84+52.00 -L-)","",1,8000,8000]
["8065000000-N","ASBESTOS ASSESSMENT","","",32,1722.0928125,55106.97]
["8070000000-E","FOUND EXCAVATION BRIDGE","","",1600,17,27200]
["8077000000-E","FOUNDATN EXCAV RET WALL","","",16613.7,16.159074137609299,268462.01]
["8084000000-N","FND EXCAV EB** STA*******","(1,14+67.00-L-)","",1,15000,15000]
["8091000000-N","FND EXCAV B** STA *******","(1, 14+97.65 -Y8-)","",1,26000,26000]
["","","(1, 17+37.28 -Y16-)","",1,7500,7500]
["","","(1, 22+29.98 -Y5-)","",1,8250,8250]
["","","(1, 25+52.71 -Y7-)","",1,6750,6750]
["","","(1, 26+20.73 -YEB-)","",1,43260,43260]
["","","(1, 28+17.37-Y-)","",1,5663.98,5663.98]
["","","(1, 28+98.81 -Y4-)","",1,10500,10500]
["","","(1, 30+02.30-Y-)","",1,6300,6300]
["","","(1, 55+88.11 -L-)","",1,20000,20000]
["","","(2, 28+17.37-Y-)","",1,5663.98,5663.98]
["","","(3, 28+17.37-Y-)","",1,11327.96,11327.96]
["","","(PIER 1, 18+79.37-S2-)","",1,6265,6265]
["","","(PIER 1, 23+62.98-S2-)","",1,11857,11857]
["","","(PIER 1, 28+12.88-S2-)","",1,19466,19466]
["","","(PIER 2, 18+79.37-S2-)","",1,8213,8213]
["","","(PIER 2, 28+12.88-S2-)","",1,11857,11857]
["","","(PIER 3, 23+62.98-S2-)","",1,11353,11353]
["8096000000-E","PILE EXCAVATION IN SOIL","","",1173,214.295950554135,251369.15]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",884,297.05100678732998,262593.09000000003]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",288,1238.85850694444,356791.25]
["","","(5'-0\")","",104.5,1709.24,178615.58]
["","","(5'-6\")","",124,1960.77,243135.48]
["","","(6'-0\")","",461.42,1660.9182523514401,766380.9]
["","","(6'-6\")","",85.17,2520.19995303511,214645.43]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",194.62,1363.60189086425,265384.2]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",1174.8699999999999,914.91024538885199,1074900.6000000001]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",557.1,1096.9689463292,611121.4]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",357,2042.8522408963599,729298.25]
["","","(5'-0\")","",188,1349.52914893617,253711.48]
["","","(5'-6\")","",481,1867.0415384615401,898046.98]
["","","(6'-0\")","",170,2091.8023529411798,355606.4]
["","","(6'-6\")","",183,2520.1999999999998,461196.6]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",243,865.74074074074099,210375]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",279,1014.06143369176,282923.14]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",328,1407.0815853658501,461522.76]
["8108000000-E","**'-**\" DIA DRILLD PIERS","(5'-0\")","",356.3,1100,391930]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",143.55000000000001,427.74294670846399,61402.5]
["","","(5'-0\")","",47.8,320,15296]
["","","(6'-0\")","",193.4,450,87030]
["","","(6'-6\")","",108.68,489.27999631947,53174.95]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",130.9,171.27578304048899,22420]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",187,199.272727272727,37264]
["8111600000-E","PERM STL CASING FOR 4' PIER","","",281.8,358.66621717530199,101072.14]
["8112730000-N","PDA TESTING","","",19,3292.4757894736799,62557.04]
["8113000000-N","SID INSPECTIONS","","",66,766.530303030303,50591]
["8114000000-N","SPT TESTING","","",57,570.45614035087704,32516]
["8115000000-N","CSL TESTING","","",75,3220.5553333333301,241541.65]
["8121000000-N","UNCL STR EXCAV STA *****","(12+68.00 -L-)","",1,7500,7500]
["","","(13+25.00-L-)","",1,10000,10000]
["","","(13+52.00-L-)","",1,7500,7500]
["","","(13+70.00-L-)","",1,4000,4000]
["","","(13+86.00-L-)","",1,25000,25000]
["","","(14+21.00 -L-)","",1,7630,7630]
["","","(14+27.00-L-)","",1,75000,75000]
["","","(14+67.00-L-)","",1,35000,35000]
["","","(14+94.00 -L-)","",1,10000,10000]
["","","(15+14.00-L-)","",1,50000,50000]
["","","(15+54.50 -L-)","",1,7500,7500]
["","","(15+56.00 -L-)","",1,7500,7500]
["","","(15+98.00 -L-)","",1,5000,5000]
["","","(18+03.65-L-)","",1,15000,15000]
["","","(18+62.50-L-)","",1,10000,10000]
["","","(18+64.00 -L-)","",1,5000,5000]
["","","(19+45.50 -L-)","",1,7500,7500]
["","","(19+78.50-L-)","",1,10684.66,10684.66]
["","","(21+10.00 -L-)","",1,8000,8000]
["","","(22+16.89-L-)","",1,35500,35500]
["","","(23+20.00-L-)","",1,15000,15000]
["","","(23+26.00 -L- EBL)","",1,28300,28300]
["","","(23+26.00 -L- WBL)","",1,32300,32300]
["","","(28+26.49-WBL-)","",1,30000,30000]
["","","(28+45.42-EBL-)","",1,30000,30000]
["","","(38+62.00-L-)","",1,20000,20000]
["","","(42+59.46-A1-)","",1,13453,13453]
["","","(64+20.00 -L-)","",1,17000,17000]
["","","(93+43.36 -L- LT)","",1,1000,1000]
["","","(93+43.36 -L- RT)","",1,1000,1000]
["","","(99+17.60 -L1-)","",1,55000,55000]
["8126000000-N","CULV EXCAV @ ************","(107+88.00-L-)","",1,80000,80000]
["","","(11+51.56 -DRW1-)","",1,15000,15000]
["","","(114+23.00 -L-)","",1,58000,58000]
["","","(120+01.00 -L-)","",1,25000,25000]
["","","(13+07.00 -L-)","",1,75990,75990]
["","","(137+22.00-L-)","",1,67000,67000]
["","","(15+40.00-L-)","",1,23143.02,23143.02]
["","","(167+03.45 -L-)","",1,110000,110000]
["","","(168+21.00-L-)","",1,67000,67000]
["","","(17+23.00-L-)","",1,60000,60000]
["","","(173+47.00 -L-)","",1,39286.769999999997,39286.769999999997]
["","","(18+16.00-L-)","",1,22950,22950]
["","","(19+20.00 -L-)","",1,11000,11000]
["","","(207+85.77-L-)","",1,42000,42000]
["","","(21+86.00-Y6-)","",1,37000,37000]
["","","(22+17.00-Y7)","",1,21384,21384]
["","","(25+30.89-S1-)","",1,5363,5363]
["","","(26+62.00 -Y6RPD-)","",1,24000,24000]
["","","(27+85.00-L-)","",1,33811.800000000003,33811.800000000003]
["","","(283+77.00-L-)","",1,67000,67000]
["","","(29+35.21-S1-)","",1,1612,1612]
["","","(314+63.00-L-)","",1,67000,67000]
["","","(324+60.00-L-)","",1,10550,10550]
["","","(364+68.00 -L-)","",1,73000,73000]
["","","(382+49.00 -L-)","",1,64000,64000]
["","","(42+05.33-A1-)","",1,1758,1758]
["","","(42+19.00-L-)","",1,10550,10550]
["","","(430+93.00 -L-)","",1,22000,22000]
["","","(472+13.00 -L-)","",1,53000,53000]
["","","(493+43.00 -L-)","",1,110000,110000]
["","","(67+46.44-Y-)","",1,5000,5000]
["","","(84+52.00 -L-)","",1,28000,28000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",8847,51.663559398666202,457067.51]
["8147000000-E","REINF CONC DECK SLAB","","",563376.19999999995,35.2530268584296,19860716.309999999]
["8156000000-E","CONC WEARING SURFACE","","",5464.8,16.94751866491,92614.8]
["8161000000-E","GROOVING BRIDGE FLOORS","","",1732778.4,0.54197659666118003,939125.34]
["8175000000-E","CLASS AA CONC (BRIDGE)","","",8025.1,926.82889434399601,7437894.5599999996]
["8182000000-E","CLASS A CONC (BRIDGE)","","",11348,816.34814152273498,9263918.7100000009]
["8196000000-E","CLASS A CONC (CULV)","","",13373.6,536.33275333492895,7172699.71]
["8210000000-N","BRG APPR SLAB ***********","(10+53.50-L-)","",1,27000,27000]
["","","(12+68.00 -L-)","",1,25000,25000]
["","","(13+25.00-L-)","",1,22500,22500]
["","","(13+52.00-L-)","",1,20000,20000]
["","","(13+70.00-L-)","",1,23975,23975]
["","","(13+86.00-L-)","",1,28000,28000]
["","","(14+21.00 -L-)","",1,34750,34750]
["","","(14+27.00-L-)","",1,37000,37000]
["","","(14+67.00-L-)","",1,30000,30000]
["","","(14+94.00 -L-)","",1,29500,29500]
["","","(14+97.65 -Y8-)","",1,37500,37500]
["","","(140+21.50 -L- LT)","",1,53800,53800]
["","","(140+21.50 -L- RT)","",1,49600,49600]
["","","(15+14.00-L-)","",1,33000,33000]
["","","(15+54.50 -L-)","",1,45000,45000]
["","","(15+56.00 -L-)","",1,25000,25000]
["","","(15+98.00 -L-)","",1,25000,25000]
["","","(155+02.50 -L- LT)","",1,51550,51550]
["","","(155+02.50 -L- RT)","",1,48150,48150]
["","","(17+37.28 -Y16-)","",1,56200,56200]
["","","(18+03.65-L-)","",1,60000,60000]
["","","(18+62.50-L-)","",1,25000,25000]
["","","(18+64.00 -L-)","",1,22500,22500]
["","","(19+45.50 -L-)","",1,25000,25000]
["","","(19+78.50-L-)","",1,30679.49,30679.49]
["","","(21+10.00 -L-)","",1,68000,68000]
["","","(22+16.89-L-)","",1,49800,49800]
["","","(22+29.98 -Y5-)","",1,56500,56500]
["","","(227+33.50-L-)","",1,55000,55000]
["","","(23+20.00-L-)","",1,45000,45000]
["","","(23+26.00 -L- EBL)","",1,46125,46125]
["","","(23+26.00 -L- WBL)","",1,46125,46125]
["","","(25+00.00-L-)","",1,34000,34000]
["","","(25+52.71 -Y7-)","",1,60900,60900]
["","","(26+20.73 -YEB-)","",1,94160,94160]
["","","(28+17.37-Y-)","",1,28319.91,28319.91]
["","","(28+26.49-WBL-)","",1,51000,51000]
["","","(28+45.42-EBL-)","",1,51000,51000]
["","","(28+98.81 -Y4-)","",1,86200,86200]
["","","(30+02.30-Y-)","",1,32500,32500]
["","","(329+95.42 -L- LT)","",1,68500,68500]
["","","(329+95.42 -L- RT)","",1,68500,68500]
["","","(337+20.09 -L- LT)","",1,67200,67200]
["","","(337+20.09 -L- RT)","",1,67200,67200]
["","","(38+35.00-L-)","",1,109000,109000]
["","","(38+62.00-L-)","",1,19475,19475]
["","","(470+43.12 -L- LT)","",1,73600,73600]
["","","(470+43.12 -L- RT)","",1,73600,73600]
["","","(50+61.09-L-)","",1,135000,135000]
["","","(55+88.11 -L-)","",1,65000,65000]
["","","(606+95.00 -L- LT)","",1,54000,54000]
["","","(606+95.00 -L- RT)","",1,54000,54000]
["","","(64+20.00 -L-)","",1,125000,125000]
["","","(93+43.36 -L- LT)","",1,49200,49200]
["","","(93+43.36 -L- RT)","",1,49200,49200]
["","","(99+17.60 -L1-)","",1,45000,45000]
["8217000000-E","REINF STEEL (BRIDGE)","","",3796881,1.0692693924302601,4059888.64]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",8490,2.8531507656066002,24223.25]
["8238000000-E","SPIRAL COL REINF STL BRG","","",344071,2.3742755419666302,816919.36]
["8245000000-E","REINF STEEL (CULVERT)","","",1812749,1.06655949058585,1933404.65]
["8252000000-E","REINF STEEL (RET WALL)","","",552030,0.95088643733129996,524917.84]
["8259000000-E","36\" PRESTR CONC GIRDR","","",1368.38,237.39847118490499,324851.32]
["8262000000-E","45\" PRESTR CONC GIRDR","","",9838.92,226.093526525269,2224516.12]
["8265000000-E","54\" PRESTR CONC GIRDR","","",13068.02,270.176061867062,3530666.18]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",15269.13,288.80269209837098,4409765.8499999996]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",6500.16,301.23788491360199,1958094.45]
["8280000000-E","STRUCTURAL STEEL","","",3008143,1.99478548725908,6000600]
["8296000000-N","POLLUTION CONTROL","","",10,57222.5,572225]
["8328000000-E","PILE DRV EQUIP SETUP * PRESTR CONC PILES","(20\")","",60,2780,166800]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(30+02.30-Y-)","",36,550,19800]
["","","(HP 12 X 53)","",688,632.00581395348797,434820]
["","","(HP 14 X 73)","",89,340.89887640449399,30340]
["","","(HP12 X 53)","",98,899.06938775510196,88108.800000000003]
["","","(HP12X53)","",133,1010.36090225564,134378]
["","","(HP14X89)","",38,1090,41420]
["8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",7,1500,10500]
["","","(HP14X89)","",26,1090,28340]
["","","(PP 18 X 0.50)","",7,600,4200]
["","","(PP 24 X 0.625)","",12,3200,38400]
["","","(PP 3 6X 0.50)","",15,6100,91500]
["8336000000-E","20\" PRESTR CONC PILES","","",4200,92.5,388500]
["8355000000-E","HP**X** PILES","(HP14X89)","",2090,54.5,113905]
["8356000000-E","HP**X** GALV PILES","(HP14X89)","",1560,76.3,119028]
["8364000000-E","HP12X53 PILES","","",37200,44.659431451612903,1661330.85]
["8384000000-E","HP14X73 PILES","","",4225,75.937278106508899,320835]
["8384200000-E","HP14X73 GALV PILES","","",490,65,31850]
["8385200000-E","PP**X**** GALV STL PILE","(PP 24 X 0.625)","",1020,210.37,214577.4]
["","","(PP 36 X 0.50)","",1800,229,412200]
["8387000000-E","PP18X0.50 GALV STL PILE","","",490,85,41650]
["8391000000-N","STEEL PILE POINTS","","",273,220.03194139194099,60068.72]
["8392500000-E","PREDRILLING FOR PILES","","",90,177.9,16011]
["8393000000-N","PILE REDRIVES","","",177,76.864406779660996,13605]
["8453000000-E","METHOD B DAMPPROOFING","","",2642,14.5972747918244,38566]
["8475000000-E","TWO BAR METAL RAIL","","",13401.5,121.808598291236,1632417.93]
["8482000000-E","THREE BAR METAL RAIL","","",1540.62,196.19179940543401,302257.01]
["8484000000-E","42\" OREGON RAIL","","",240,429.47500000000002,103074]
["8503000000-E","CONC BARRIER RAIL","","",14100.2,99.922676274095394,1408929.72]
["8504000000-E","CONC BARR RAIL MOMENT SLAB","","",1290,537,692730]
["8505000000-E","VERT CONC BARRIER RAIL","","",3151.75,121.912724676767,384238.43]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-2 3/4\")","",376.39,110,41402.9]
["","","(1'-2\" X 2'-6\")","",1818.54,108.076599909818,196541.62]
["","","(1'-2\" X 2'-8\")","",423.33,111,46989.63]
["","","(1'-2\" X 2'-9 1/2\")","",640.35,132.237838681971,84678.5]
["","","(1'-2\" X 2'-9\")","",2240,100,224000]
["","","(1'-2\" X 2-6\")","",401.45,108.500012454851,43557.33]
["","","(1'-2\" X 3\"-3\")","",427.9,122,52203.8]
["","","(1'-2\" X 3'-3 1/2\")","",160.1,135,21613.5]
["","","(1'-2\" X 3'-3\")","",1020.95,95.458739409373607,97458.6]
["","","(1'-2\" X 3'-7\")","",170,115,19550]
["8531000000-E","4\" SLOPE PROTECTION","","",10850.7,87.334897287732602,947644.77]
["8559000000-E","SURFACE PREP, CLASS II","","",870.7,420.53083725737901,366156.2]
["8566000000-E","SURFACE PREP, CLASS III","","",123.9,1926.29136400323,238667.5]
["8573000000-E","LATEX MOD CONC OVERLAY","","",264.7,1788.6176803929,473447.1]
["8580000000-E","PLACING LATEX MOD CONC","","",4572,30,137160]
["8590000000-E","RIP RAP, CLASS **","(A, 1'-0\" THICK)","",970,86.5,83905]
["8608000000-E","RIP RAP II (2'-0\")","","",27995,43.973149848187198,1231028.33]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",31178,2.9013586503303599,90458.559999999998]
["8629000000-E","EROS CONTRL STONE CL B","","",1,550,550]
["8654000000-N","DISC BEARINGS","","",2,46100,92200]
["8657000000-N","ELASTOMERIC BEARINGS","(14+67.00-L-)","",1,4042,4042]
["","","","",39,14105.886153846201,550129.56000000006]
["8660000000-E","CONC REPAIRS","","",385.64,873.27559381806896,336770]
["8664000000-E","SHOTCRETE REPAIRS","","",12545.6,523.19526367810204,6563798.5]
["8678000000-E","EPOXY RESIN INJECTION","","",10602.46,94.6092699241497,1003091]
["8685000000-E","EPOXY MORTAR REPAIR","","",55.3,414.35117540687202,22913.62]
["8692000000-N","FOAM JOINT SEALS","","",14,79859.02,1118026.28]
["8699000000-N","STRIP SEALS","","",2,65000,130000]
["8706000000-N","EXPANSION JOINT SEALS","","",7,165685.714285714,1159800]
["8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(140+21.50 -L- RT)","",1,49600.92,49600.92]
["","","(155+02.50 -L- RT)","",1,48498.67,48498.67]
["","","(18+03.65-L-)","",1,35500,35500]
["","","(337+20.09 -L-)","",1,53570,53570]
["","","(93+43.36 -L- RT)","",1,76054.740000000005,76054.740000000005]
["8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",5500,249.85454545454499,1374200]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",3410,275.48387096774201,939400]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",2040,148.01470588235301,301950]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",6700,167.58674626865701,1122831.2]
["8801000000-E","MSE RETAIN WALL NO **","(-WL1-)","",2855,120,342600]
["","","(-WL2-)","",2600,120,312000]
["","","(1)","",7825,76.133354632587896,595743.5]
["","","(2)","",12400,71.738387096774204,889556]
["","","(W3)","",1084,98.2,106448.8]
["","","(W4)","",682,108.1,73724.2]
["8802010000-E","SOIL NAIL RETAINING WALLS","","",2617,105.105139472679,275060.15000000002]
["8802014000-E","SOLDIER PILE RETAINING WALLS","","",8287.5,235.90226244343901,1955040]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",4,551.41,2205.64]
["8802015110-N","SOIL NAIL PROOF TESTS","","",8,166.9,1335.2]
["8802030000-E","SEGMENTAL GRAVITY RETAIN WALLS","","",2693,51.671667285555102,139151.79999999999]
["8802031000-E","PRECAST GRAVITY RETAINING WALLS","","",680,82.6,56168]
["8802040000-E","CIP GRAVITY RETAINING WALLS","","",2480,166.77822580645201,413610]
["8804000000-N","GENERIC CULVERT ITEM (LS)","ALUMINUM STRUCTURAL PLATE ARCH","CULVERT",1,170332.1,170332.1]
["8806000000-N","GENERIC CULVERT ITEM (EA)","PDA TESTING","",2,4441,8882]
["","","PILE DRIVING EQUIPMENT SETUP","FOR HP14X73 STEEL PILES",43,630,27090]
["8811000000-E","GENERIC CULVERT ITEM (LF)","HP14X73 STEEL PILES","",1602,66,105732]
["","","METAL HANDRAIL (SIDE MOUNTED)","",944,62.76,59245.440000000002]
["","","METAL HANDRAIL (TOP MOUNTED)","",1188,189.75,225423]
["","","METAL RAIL (ALUMINUM)","",47.2,263,12413.6]
["8815000000-E","GENERIC CULVERT ITEM (LB)","REINFORCING STEEL, STAIRS","",1564,0.84,1313.76]
["","","REINFORCING STEEL, UNDERPASS","",96200,0.84,80808]
["8818000000-E","GENERIC CULVERT ITEM (TON)","CULVERT BACKFILL","",320,40.1,12832]
["","","FOUNDATION CONDITIONING MATE-","RIAL, UNDERPASS",237,65.180000000000007,15447.66]
["","","NO 57 STONE","",5645,34.04,192155.8]
["8821000000-E","GENERIC CULVERT ITEM (SF)","TEMPORARY SHORING FOR RISER","CONSTRUCTION",10600,0.01,106]
["8822000000-E","GENERIC CULVERT ITEM (SY)","6\" RAMPS & WALKWAYS","",1150,67.66,77809]
["","","BENTONITE GEOTEXTILE WATER-","PROOFING MEMBRANE",2785,74.400000000000006,207204]
["","","WATERPROOFING","",562,75,42150]
["8825000000-E","GENERIC CULVERT ITEM (CY)","CLASS A CONCRETE, STAIRS","",36.1,1130.3398891966799,40805.269999999997]
["","","CLASS AA CONCRETE, RETAINING WALL","",1159,774,897066]
["","","CLASS AA CONCRETE, UNDERPASS","",692,609,421428]
["","","UNCLASSIFIED STRUCTURE EXCAVA-","TION, RAMPS, STAIRS & WALKWAYS",4430,8.81,39028.300000000003]
["","","UNDERPASS EXCAVATION","",5705,12.85,73309.25]
["8826000000-E","GENERIC CULVERT ITEM (CY)","CLASS AA CONCRETE","",646.6,650,420290]
["8834000000-N","GENERIC RET WALL ITEM (EA)","7\" DIA MICROPILES","",6,4765,28590]
["","","MICROPILE VERIFICATION TEST","",1,18673,18673]
["","","PDA TESTING","",2,4441,8882]
["","","PILE DRIVING EQUIPMENT SETUP","FOR HP14X73 STEEL PILES",316,535,169060]
["8839000000-E","GENERIC RET WALL ITEM (LF)","HP14X73 STEEL PILES","",11113.4,68,755711.2]
["","","METAL RAIL (ALUMINUM)","",594.4,252,149788.79999999999]
["","","METAL RAIL (STEEL) & FENCE","",1320.1,600,792060]
["8846000000-E","GENERIC RET WALL ITEM (TON)","FOUNDATION CONDITIONING MATE-","RIAL, RETAINING WALL",1047,58.85,61615.95]
["","","SELECT MATERIAL CLASS VI","",2300,25.82,59386]
["8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL SURFACE","TREATMENT",54652,1.95,106571.4]
["","","ARCHITECTURAL SURFACE TREAT- MENT","",101508,3.15,319750.2]
["","","MSE ABUTMENT WALL NO 1A","",3100,65.680000000000007,203608]
["","","MSE ABUTMENT WALL NO 1B","",3900,67.400000000000006,262860]
["","","MSE ABUTMENT WALL NO 2A","",4700,68.97,324159]
["","","MSE ABUTMENT WALL NO 2B","",5200,69.39,360828]
["","","MSE ABUTMENT WALL NO 4A","",4400,63.91,281204]
["","","MSE ABUTMENT WALL NO 4B","",4200,65.75,276150]
["","","MSE ABUTMENT WALL NO 5A","",3600,68.099999999999994,245160]
["","","MSE ABUTMENT WALL NO 5B","",3200,64.489999999999995,206368]
["","","MSE ABUTMENT WALL NO 6A","",4300,66.31,285133]
["","","MSE ABUTMENT WALL NO 6B","",4800,66.66,319968]
["","","PILE PANEL RETAINING WALLS","",10304.799999999999,297,3060525.6]
["","","SOUND BARRIER WALL","",61812,28.9,1786366.8]
["","","SOUND BARRIER WALL NW2","",6822,38,259236]
["","","SOUND BARRIER WALL NW2A","",12147,38,461586]
["","","SOUND BARRIER WALL NW3","",14955,38,568290]
["","","TEMPORARY SHORING","",5200,19,98800]
["","","TEMPORARY SHORING FOR","RETAINING WALL NO 1",410,70.92,29077.200000000001]
["8853000000-E","GENERIC RET WALL ITEM (CY)","CLASS AA CONCRETE","",2296.9,605,1389624.5]
["8860000000-N","GENERIC STR ITEM (LS)","APPLICATION OF BRIDGE COATING","",1,50000,50000]
["","","APPROX 160,000 LBS STRUCTURAL","STEEL",1,561207,561207]
["","","APPROX 177,727 LBS STRUCTURAL STEEL","",1,655396,655396]
["","","APPROX 177,963 LBS STRUCTURAL STEEL","",1,648926,648926]
["","","APPROX 231,350 LBS STRUCTURAL STEEL","",1,850680,850680]
["","","APPROX 233,588 LBS STRUCTURAL STEEL","STA 28+12.88-S2-",1,850791,850791]
["","","","STA 28+17.22-S1-",1,846065,846065]
["","","APPROX 338,035 LBS STRUCTURAL STEEL","STA 23+62.98-S2-",1,936000,936000]
["","","","STA 23+65.83-S1-",1,1018350,1018350]
["","","APPROX 764,875 LBS STRUCTURAL STEEL","",1,1626392,1626392]
["","","ASBESTOS ASSESSMENT","",4,2625,10500]
["","","AUXILIARY COUNTERWEIGHT & SPAN","GUIDE REPAIRS",1,700000,700000]
["","","CLEANING & PAINTING EXISTING","WEATHERING STEEL FOR BRIDGE 43",1,245000,245000]
["","","","WEATHERING STEEL FOR BRIDGE 44",1,245000,245000]
["","","CLEANING & PAINTING EXISTING WEATHERING","STEEL FOR BRIDGE 560093",1,100000,100000]
["","","","STEEL FOR BRIDGE 560113",1,100000,100000]
["","","","STEEL FOR BRIDGE 600247",1,100000,100000]
["","","CLEANING & REPAINTING OF BRIDGE 13","",1,1350000,1350000]
["","","CLEANING & REPAINTING OF BRIDGE 31","",1,230000,230000]
["","","CLEANING & REPAINTING OF BRIDGE 33","",1,230000,230000]
["","","CLEANING AND REPAINTING OF","BRIDGE 207",1,168000,168000]
["","","","BRIDGE 213",1,200000,200000]
["","","","BRIDGE 358",1,100000,100000]
["","","","BRIDGE 366",1,100000,100000]
["","","","BRIDGE 369",1,100000,100000]
["","","","BRIDGE 374",1,100000,100000]
["","","","BRIDGE 377",1,220000,220000]
["","","","BRIDGE 378",1,220000,220000]
["","","FIELD MEASURING","",1,30000,30000]
["","","INSTALL NEW SIGNS","",1,10000,10000]
["","","INSTALLATION OF 3'-0\" X 2'-0\"","PRESTRESSED CONCRETE CORED SLABS",1,66700,66700]
["","","MECHANICAL OPERATING MACHINERY","",1,225000,225000]
["","","MOLDED RUBBER SEGMENTAL","EXPANSION JOINT",1,450000,450000]
["","","OPERATOR HOUSE RENOVATION","",1,1588780.45,1588780.45]
["","","PAINTING CONTAINMENT","FOR BRIDGE NO 39",1,8175,8175]
["","","PAINTING CONTAINMENT FOR","BRIDGE 207",1,65000,65000]
["","","","BRIDGE 213",1,65000,65000]
["","","","BRIDGE 358",1,30000,30000]
["","","","BRIDGE 366",1,30000,30000]
["","","","BRIDGE 369",1,30000,30000]
["","","","BRIDGE 374",1,30000,30000]
["","","","BRIDGE 377",1,75000,75000]
["","","","BRIDGE 378",1,75000,75000]
["","","","BRIDGE 43",1,122500,122500]
["","","","BRIDGE 44",1,122500,122500]
["","","","BRIDGE 560093",1,15000,15000]
["","","","BRIDGE 560113",1,15000,15000]
["","","","BRIDGE 600247",1,15000,15000]
["","","","BRIDGE NO 479",1,50000,50000]
["","","","BRIDGE NO 480",1,50000,50000]
["","","","BRIDGE NO 489",1,65000,65000]
["","","","BRIDGE NO 493",1,65000,65000]
["","","","BRIDGE NO 494",1,40000,40000]
["","","","BRIDGE NO. 485",1,40000,40000]
["","","PAINTING CONTAINMENT FOR BRIDGE 13","",1,886000,886000]
["","","PAINTING CONTAINMENT FOR BRIDGE 31","",1,135000,135000]
["","","PAINTING CONTAINMENT FOR BRIDGE 33","",1,135000,135000]
["","","PAINTING CONTAINMENT FOR ZONE","PAINTING FOR BRIDGE NO 474",1,50000,50000]
["","","","PAINTING, BRIDGE 334",1,10000,10000]
["","","","PAINTING, BRIDGE 339",1,10000,10000]
["","","","PAINTING, BRIDGE 344",1,20000,20000]
["","","","PAINTING, BRIDGE 347",1,20000,20000]
["","","PAINTING EXISTING WEATHERING","STEEL STRUCTURE FOR BRIDGE NO 479",1,80000,80000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 480",1,80000,80000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 485",1,95000,95000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 489",1,65000,65000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 493",1,55000,55000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 494",1,55000,55000]
["","","PAINTING OF STRUCTURAL STEEL","",1,1119975,1119975]
["","","PARTIAL REMOVAL OF EXISTING","STRUCTURE",1,47000,47000]
["","","","STRUCTURE 369",1,20000,20000]
["","","PLATFORM STRUCTURE DRAINAGE","SYSTEM",1,131395,131395]
["","","PREFORMED SILICONE EXPANSION","JOINT SEALS",1,12000,12000]
["","","REMOVAL OF EXISTING FENDER SYSTEM","",1,302200,302200]
["","","REMOVE EXISTING BRIDGE RAIL","",1,43500,43500]
["","","REPAIR OF EXISTING DECK DRAINS","",1,10500,10500]
["","","REPLACE AIR HORN","",1,5000,5000]
["","","REPLACEMENT OF STEEL GRID DECK","",1,3600000,3600000]
["","","SELF LUBRICATING EXPANSION","BEARING ASSEMBLIES",1,555465,555465]
["","","SPOT PAINTING OF STEEL STRUCTURE","REPAIR AREAS",1,75000,75000]
["","","STRUCTURE DRAINAGE SYSTEM AT","STA 15+39.55-S1-",1,254741,254741]
["","","","STA 18+79.37-S2-",1,147606,147606]
["","","","STA 18+82.25-S1-",1,147606,147606]
["","","","STA 23+62.98-S2-",1,187468,187468]
["","","","STA 23+65.83-S1-",1,187468,187468]
["","","","STA 28+12.88-S2-",1,153599,153599]
["","","","STA 28+17.22-S1-",1,153599,153599]
["","","","STA 42+59.46-A1-",1,126535,126535]
["","","STRUCTURE GROUNDING AND","BONDING AT STA 23+65.83-S1-",1,15000,15000]
["","","TEMPORARY RAILROAD SHORING/","ABUTMENT 1 (23+62.98-S2-)",1,17065,17065]
["","","","ABUTMENT 1 (28+12.88-S2-)",1,16005,16005]
["","","","ABUTMENT 1 (42+59.46-A1-)",1,43501,43501]
["","","","ABUTMENT 2 (23+62.98-S2-)",1,15475,15475]
["","","","ABUTMENT 2 (28+12.88-S2-)",1,17065,17065]
["","","","ABUTMENT 2 (42+59.46-A1-)",1,37311,37311]
["","","","PIER 1 (18+79.37-S2-)",1,64021,64021]
["","","","PIER 1 (23+62.98-S2-)",1,108223,108223]
["","","","PIER 1 (28+12.88-S2-)",1,89568,89568]
["","","","PIER 2 (18+79.37-S2-)",1,104940,104940]
["","","","PIER 2 (28+12.88-S2-)",1,86917,86917]
["","","","PIER 3 (23+62.98-S2-)",1,90098,90098]
["","","UNDER STRUCTURE WORK PLATFORM","",1,575000,575000]
["","","UNDER STRUCTURE WORKPLATFORM","",1,0.01,0.01]
["","","VOLUMETRIC MIXER","",8,15499.504999999999,123996.04]
["","","ZONE PAINTING OF EXISTING","STRUCTURE FOR BRIDGE NO 474",1,25000,25000]
["","","","STRUCTURE, BRIDGE 334",1,25000,25000]
["","","","STRUCTURE, BRIDGE 339",1,30000,30000]
["","","","STRUCTURE, BRIDGE 344",1,60000,60000]
["","","","STRUCTURE, BRIDGE 347",1,60000,60000]
["8867000000-E","GENERIC STR ITEM (LF)","1'-2\" X 1'-11\" CONCRETE","PARAPET FOR RAIL RETROFIT",6249,125,781125]
["","","10\" X 10\" TREATED LUMBER","",3332,69.900000000000006,232906.8]
["","","12\" DIA. TREATED TIMBER PILES","",12300,40,492000]
["","","3'-0\" X 1'-8\" PRESTRESSED","CONC CORED SLABS",13398,228,3054744]
["","","3'-2\" X 1'-6\" PRESTRESSED","CONC CORED SLABS",2233,228,509124]
["","","78\" FIB PRESTRESSED","CONCRETE GIRDERS",3121.8,403.46000064065601,1259521.43]
["","","8\" X 8\" TREATED LUMBER","",516,66.400000000000006,34262.400000000001]
["","","ABRASIVE METAL NOSINGS","",999,26,25974]
["","","ADHESIVELY ANCHORED 2'-6\"","CONCRETE PARAPET",350.79,148.50001425354199,52092.32]
["","","ADHESIVELY ANCHORED CONCRETE","BARRIER RAIL",350.83,160,56132.800000000003]
["","","ADHESIVELY ANCHORED VERTICAL","CONCRETE RAIL",403.96,140,56554.400000000001]
["","","ANODIZED TWO BAR METAL RAIL","",229.4,220.422842197036,50565]
["","","ARCHITECTURAL FIN RAIL","(ALUMINUM HAND RAIL AND FIN ASSEMBLY)",400.4,1465,586586]
["","","ARMORLESS EXPANSION JOINT SYSTEM","",335,66,22110]
["","","BRIDGE JOINT REMOVAL","",1871,32.2771512560128,60390.55]
["","","CLASSIC CONCRETE BRIDGE RAIL","",416,430,178880]
["","","CONCRETE PARAPET","",2205.1999999999998,99,218314.8]
["","","CP INTEGRAL PILE JACKET","(STRUCTURAL), 16 TO 30 IN.",998,1450,1447100]
["","","EXPANSION JOINT SEAL REPAIR","",583,220.97770154373899,128830]
["","","FOAM JOINT SEALS","",719,170,122230]
["","","FOAM JOINT SEALS FOR","PRESERVATION",80.400000000000006,72,5788.8]
["","","FOAM JOINT SEALS FOR PRESERVA-TION","",184.8,60,11088]
["","","HP14X73 STEEL PILES","",27972.7,50,1398635]
["","","METAL RAIL (ALUMINUM)","",842.7,258,217416.6]
["","","METAL RAIL (STEEL) & FENCE","",660.4,645,425958]
["","","MODIFIED ALASKA BARRIER RAIL","",3034,250,758500]
["","","PLATFORM EXPANSION JOINTS","",315,26,8190]
["","","PLATFORM PAINT","",2200,13,28600]
["","","POURABLE SILICONE JOINT SEAL- ANT","",184.8,40,7392]
["","","PREDRILLING FOR PILES","",128,150,19200]
["","","RAIL REMOVAL (SPANS 29-65)","",6249,40,249960]
["","","RAIL RETROFIT","",3599,140,503860]
["","","REMOVE AND RESET BRIDGE DECK","MOUNTED GUARDRAIL FOR BRIDGE 358",242,140,33880]
["","","","MOUNTED GUARDRAIL FOR BRIDGE 366",242,140,33880]
["","","","MOUNTED GUARDRAIL FOR BRIDGE 369",270,130,35100]
["","","","MOUNTED GUARDRAIL FOR BRIDGE 374",270,130,35100]
["","","RUB RAIL","",2200,48,105600]
["","","SILICONE JOINT SEALANT","",8743.9,56.231338418783402,491681.2]
["","","SOIL/ROCK BORING","",640,150,96000]
["","","STAINLESS STEEL HANDRAILS","",370,261,96570]
["","","STAINLESS STEEL RAILINGS","",368,761,280048]
["","","TACTILE WARNING SURFACE","",2200,188,413600]
["8881000000-E","GENERIC STR ITEM (CY)","FLOWABLE FILL","",8,1000,8000]
["","","LATEX MODIFIED CONC. OVERLAY-","VERY EARLY STRENGTH",21.3,1200,25560]
["","","LATEX MODIFIED CONCRETE-EARLY","STRENGTH",438.3,1450,635535]
["","","LATEX MODIFIED CONCRETE-VERY","EARLY STRENGTH",614.70000000000005,1269.31836668293,780250]
["","","POLYESTER POLYMER CONCRETE","MATERIALS",432.7,3000,1298100]
["","","PPC MATERIALS","",4003.65,2934.25967554606,11747748.75]
["","","UNCLASSIFIED STRUCTURE","EXCAVATION AT 606+95.00 -L- LT",12000,10.5,126000]
["","","","EXCAVATION AT 606+95.00 -L- RT.",3200,10.5,33600]
["8882000000-E","GENERIC STR ITEM (CF)","CONCRETE DECK REPAIR","",170,270,45900]
["","","CONCRETE FOR DECK REPAIR","",2164,82.395286506469503,178303.4]
["","","ELASTOMERIC CONCRETE","",1344.6,373.95507957757002,502820]
["","","ELASTOMERIC CONCRETE FOR","PRESERVATION",20.100000000000001,525,10552.5]
["","","ELASTOMERIC CONCRETE FOR PRES-ERVATION","",46.4,400,18560]
["","","REPAIRS TO PRESTRESSED","CONCRETE GIRDERS",257.72000000000003,957.64395467949703,246804]
["","","REPAIRS TO PRESTRESSED CONC GIRDER","",18.399999999999999,953,17535.2]
["","","REPAIRS TO PRESTRESSED CONC-","RETE GIRDERS",211.5,763.82978723404301,161550]
["","","REPAIRS TO REINFORCED CONCRETE","DECK GIRDERS",29.5,1050,30975]
["8889000000-E","GENERIC STR ITEM (LB)","ADDITIONAL REINFORCING STEEL","",1200,2,2400]
["","","BEAM PLATED REPAIR","",1155.9000000000001,30,34677]
["","","BEAM PLATING REPAIR","",169,150,25350]
["","","BEAM REPAIR","",3158.9,82.492323277090094,260585]
["","","BEAM REPAIR FOR BRIDGE 50","",364,12,4368]
["","","BEAM SECTION REPLACEMENT AND","STIFFENER/CONNECTOR PLATE REPAIR",37850,16,605600]
["","","HARDWARE","",8115,4.5999999999999996,37329]
["","","REINFORCING STEEL, BLACK (GRADE 75)","",139300,1,139300]
["","","REINFORCING STEEL, GALVANIZED","(GRADE 75)",67320,2,134640]
["","","SPIRAL REINFORCING STEEL,","BLACK (GRADE 75)",69800,2,139600]
["","","","GALVANIZED (GRADE 75)",18000,3,54000]
["","","STEEL CONNECTION HARDWARE","",300,5,1500]
["","","STEEL DIAPHRAGM REPLACEMENT","",2295,24,55080]
["","","STRUCTURAL STEEL FOR REPAIRS","",25000,24,600000]
["","","STRUCTURAL STEEL REPAIR","",975,146,142350]
["8892000000-E","GENERIC STR ITEM (SF)","ANCHORED VENEER","",17075,118,2014850]
["","","BRIDGE JOINT DEMOLITION","",7686.9,91.8793792035801,706267.6]
["","","CONCRETE DECK REPAIR FOR","EPOXY OVERLAY",60,350,21000]
["","","CONCRETE DECK REPAIR FOR EPOXY","OVERLAY",52,50,2600]
["","","CONCRETE WORK FOR JOINT","REPLACEMENT",240,170,40800]
["","","CONCRETE WORK FOR JOINT RE- PLACEMENT","",184.8,100,18480]
["","","CP SYSTEM, ZINC ALUMINUM SPRAY","",13375,32.738317757009298,437875]
["","","EPOXY COATING","",30048.400000000001,17.1849715791856,516380.9]
["","","EPOXY COATING AND DEBRIS","REMOVAL",1159,51,59109]
["","","EPOXY OVERLAY SYSTEM","",151687.4,5.9025627705399399,895344.4]
["","","EPOXY PROTECTIVE COATING","",3527,33,116391]
["","","JOINT REPAIR","",286,169.92,48597.120000000003]
["","","LIQUID FLOOR TREATMENTS","",38400,0.41,15744]
["","","STAINLESS STEEL ENCLOSURE","",442,476,210392]
["","","TEMPORARY SHORING FOR MSE WALL","CONSTRUCTION",4272,36.700000000000003,156782.39999999999]
["8893000000-E","GENERIC STR ITEM (SY)","CONC DECK REPAIR FOR PPC OVERLAY","",30.9,332,10258.799999999999]
["","","CONCRETE DECK REPAIR FOR","POLYESTER POLYMER CONC OVERLAY",4,500,2000]
["","","","PPC OVERLAY",11,354.54545454545502,3900]
["","","CONCRETE DECK REPAIR FOR PPC","OVERLAY",74.400000000000006,541.93548387096803,40320]
["","","CONCRETE DECK REPAIR FOR PPC OVERLAY","",124.6,429.75120385232702,53547]
["","","FOUNDATION WATERPROOFING","",2400,57,136800]
["","","HYDRO-DEMOLITION OF BRIDGE","DECK",14248,55.495906793936001,790705.68]
["","","HYDRO-DEMOLITION OF BRIDGE DECK","",11050,76.682280542986405,847339.2]
["","","HYDRO-DEMOLITION OF BRIDGE DECK","",13.5,1.0370370370370001E-2,0.14000000000000001]
["","","PLACING & FINISHING PPC OVER-LAY","",17655,18.899999999999999,333679.5]
["","","PLACING & FINISHING LATEX MODIFIED","CONC. OVERLAY-VERY EARLY STRENGTH",4548,30,136440]
["","","PLACING & FINISHING OF LATEX","MOD CONC OVERLAY-VERY EARLY STRENGTH",6226,30,186780]
["","","PLACING & FINISHING OF LATEX MODIFIED","CONC OVERLAY-VERY EARLY STRENGTH",614.4,75,46080]
["","","PLACING & FINISHING POLYESTER","POLYMER CONCRETE OVERLAY",14139,26,367614]
["","","PLACING & FINISHING PPC OVER- LAY","",16223.4,24,389361.6]
["","","PLACING AND FINISHING LATEX MODIFIED","CONC. OVERLAY-EARLY STRENGTH",7398,40,295920]
["","","PLACING AND FINISHING PPC","OVERLAY",24585,31.7333231645312,780163.75]
["","","PLACING AND FINISHING PPC OVERLAY","",28530,28.6663862600771,817852]
["","","PLACING AND FINISHING PPC OVERLAY","",25401,35.285638360694499,896290.5]
["","","PLACING LATEX MODIFIED CONCRETE","",2548,101.95,259768.6]
["","","SCARIFYING BRIDGE DECK","",147273.4,19.228117840696299,2831790.29]
["","","SHOTBLASTING BRIDGE DECK","",159487.4,4.3213927244409298,689207.69]
["","","SILANE DECK TREATMENT","",32035,5,160175]
["","","WATERPROOFING","",3075.7,73.062587378482903,224718.6]
["8897000000-N","GENERIC STR ITEM (EA)","3'-6\" STAINLESS STEEL GATES","",3,11746,35238]
["","","7\" DIA MICROPILES","",12,4450,53400]
["","","8'-0\" STAINLESS STEEL GATES","",2,60957,121914]
["","","9-5/8\" DIAMETER MICROPILES","",11,7329.7,80626.7]
["","","BRIDGE JACKING","",160,1000,160000]
["","","CLEANING & PAINTING EXISTING","BEARINGS WITH HRCSA",84,500,42000]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 474",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 479",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 480",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 485",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 489",80,650,52000]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 493",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 494",48,650,31200]
["","","","BEARINGS WITH HRSCA BRIDGE NO 39",32,817.5,26160]
["","","CP INTEGRAL PILE JACKET, 16\" TO 30\"","",150,300,45000]
["","","CP SYSTEM (ZINC BULK ANODE)","",22,4500,99000]
["","","CP SYSTEM (ZINC BULK ANODES)","",22,7800,171600]
["","","ELASTOMERIC BEARING, MODIFIED","TYPE I-A",64,160,10240]
["","","","TYPE I-B",48,170,8160]
["","","","TYPE I-C",16,180,2880]
["","","GUARDRAIL ANCHOR UNIT REPAIR","",4,600,2400]
["","","HINGE","",30,740,22200]
["","","LIGHTNING PROTECTION SYSTEM","",2,8000,16000]
["","","MICROPILE VERIFICATION TEST","",1,18673,18673]
["","","OVERHANG DIAPHRAGM REMOVAL","",20,850,17000]
["","","PANIC DEVICE","",4,1000,4000]
["","","PDA TESTING","",20,4441,88820]
["","","PILE DRIVING EQUIPMENT SETUP","FOR HP14X73 STEEL PILES",593,423,250839]
["","","SPLICING OF PRESTRESSING STRAND","",1,3500,3500]
["","","STEEL KEEPER ANGLE ASSEMBLY","",80,1000,80000]
["","","STEEL KEEPER ASSEMBLY","",3,4000,12000]
["","","STEEL PILE POINTS","",12,168,2016]
["","","STEEL PLATE BEARING","",1,500,500]
["","","STUB COLUMN ASSEMBLY","",34,2800,95200]
["","","THERMAL INTEGRITY PROFILER","",27,3311.1111111111099,89400]
["","","TYPE I BRIDGE JACKING","BRIDGE 560113",28,3500,98000]
["","","","BRIDGE 600247",2,7200,14400]
["","","","",9,15666.666666666701,141000]
["","","TYPE I BRIDGE JACKING BRIDGE 31","",3,10000,30000]
["","","TYPE I BRIDGE JACKING BRIDGE 33","",3,10000,30000]
["","","TYPE I BRIDGE JACKING BRIDGE NO 39","",7,2000,14000]
["","","TYPE I BRIDGE JACKING FOR","BRIDGE 215",3,9000,27000]

{"sheet":"BExRepositorySheet","index":2,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
[7]

{"sheet":"ITEMS - DIV 01","index":3,"n_rows":93,"n_cols":7,"rows_kept":93,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 01"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",4,394912.5,1579650]
["0005000000-N","GENERIC FERRY ITEM (LS)","CONSTR 70'-6\" X 30' X 11'","SOUND CLASS TUG",1,5217228,5217228]
["","","CONSTRUCT 183'-7\" X 46' X 11'","PASSENGER/VEHICLE FERRY \"H\"",1,11883016.52,11883016.52]
["0106000000-E","BORROW EXCAVATION","","",3275,19.381679389313,63475]
["1220000000-E","INCIDENTAL STONE BASE","","",1525,57.049180327868797,87000]
["1245000000-E","SHOULDER RECONST","","",28.36,2500,70900]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",1131650,1.13654177528388,1286167.5]
["1330000000-E","INCIDENTAL MILLING","","",81000,3.4931944444444398,282948.75]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",5600,42,235200]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",11150,38,423700]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",113600,39.8345422535211,4525204]
["1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",1775,48,85200]
["1575000000-E","ASP FOR PLANT MIX","","",7921,570.53212978159297,4519185]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",206,730,150380]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",4085,75.599999999999994,308826]
["1704000000-E","PATCHING EXIST PVMT","","",250,200,50000]
["1840000000-E","MILLED RUMBLE STRIPS","","",80700,0.09,7263]
["2830000000-N","ADJ MANHOLES","","",11,600,6600]
["2845000000-N","ADJ METER OR VALVE BOXES","","",11,500,5500]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",11000,17,187000]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",672,15.685714285714299,10540.8]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",906,10.254304635761599,9290.4]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",94,25,2350]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",10854,7,75978]
["4415000000-N","FLASHING ARROW BOARD","","",6,2996.6666666666702,17980]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",4,12325,49300]
["4430000000-N","DRUMS","","",160,48.3,7728]
["4435000000-N","CONES","","",100,22.3,2230]
["4445000000-E","BARRICADES (TYPE III)","","",80,35,2800]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",2,30750,61500]
["4465000000-N","TEMP CRASH CUSHIONS","","",4,10000,40000]
["4480000000-N","TMA","","",4,23200,92800]
["4510000000-N","LAW ENFORCEMENT","","",160,52.9,8464]
["4516000000-N","SKINNY DRUM","","",150,37.74,5661]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",649840,0.47524042841315001,308830.24]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",418923,0.57102219262250997,239214.33]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",146152,0.74,108152.48]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",20760,0.95,19722]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",37,3,111]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",2500,3,7500]
["4705000000-E","THERMO LINES 16\" 120MILS","","",200,7.125,1425]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",875,10.08,8820]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",74,95.135135135135101,7040]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",131,125.725190839695,16470]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",1133041,0.11450330570562001,129736.94]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",185480,0.2263890985551,41990.65]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",1400,0.85,1190]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",200,1.75,350]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",875,3,2625]
["4840000000-N","PAINT PVT MKG CHARACTER","","",74,29.5945945945946,2190]
["4845000000-N","PAINT PVT MKG SYMBOL","","",131,37.137404580152698,4865]
["4847020000-E","POLYUREA LINES (4\", 30 MILS)","","",1380,5.5,7590]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",21060,1.5175213675213699,31959]
["4847040000-E","POLYUREA LINES (6\", 30 MILS)","","",4175,4,16700]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",5555,1.43631863186319,7978.75]
["4900000000-N","PERM RAISED PVMT MARKERS","","",132,23.639393939393901,3120.4]
["4905000000-N","SNOWPLB PVMT MRKER","","",5104,29.358610893416898,149846.35]
["6000000000-E","TEMP SILT FENCE","","",4125,2.99545454545455,12356.25]
["6071012000-E","COIR FIBER WATTLE","","",1850,9.6386486486486493,17831.5]
["6084000000-E","SEEDING AND MULCHING","","",17.82,1705.30303030303,30388.5]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",23,25,575]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",1500,9,13500]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",400,1,400]
["8161000000-E","GROOVING BRIDGE FLOORS","","",287953.40000000002,0.47673192954138,137276.57999999999]
["8296000000-N","POLLUTION CONTROL","","",1,82500,82500]
["8559000000-E","SURFACE PREP, CLASS II","","",92.9,554.54897739504895,51517.599999999999]
["8664000000-E","SHOTCRETE REPAIRS","","",6274.7,413.19561094554302,2592678.5]
["8678000000-E","EPOXY RESIN INJECTION","","",1595.2,82.530341023069198,131652.4]
["8860000000-N","GENERIC STR ITEM (LS)","CLEANING & PAINTING EXISTING","WEATHERING STEEL FOR BRIDGE 43",1,245000,245000]
["","","","WEATHERING STEEL FOR BRIDGE 44",1,245000,245000]
["","","PAINTING CONTAINMENT FOR","BRIDGE 43",1,122500,122500]
["","","","BRIDGE 44",1,122500,122500]
["","","REMOVAL OF EXISTING FENDER SYSTEM","",1,302200,302200]
["8867000000-E","GENERIC STR ITEM (LF)","10\" X 10\" TREATED LUMBER","",3332,69.900000000000006,232906.8]
["","","12\" DIA. TREATED TIMBER PILES","",12300,40,492000]
["","","8\" X 8\" TREATED LUMBER","",516,66.400000000000006,34262.400000000001]
["","","SILICONE JOINT SEALANT","",3532,51.7460928652322,182767.2]
["8881000000-E","GENERIC STR ITEM (CY)","PPC MATERIALS","",958.05,3167.6830541203499,3034798.75]
["8882000000-E","GENERIC STR ITEM (CF)","REPAIRS TO PRESTRESSED","CONCRETE GIRDERS",83.42,800,66736]
["","","REPAIRS TO PRESTRESSED CONC GIRDER","",18.399999999999999,953,17535.2]
["8889000000-E","GENERIC STR ITEM (LB)","HARDWARE","",8115,4.5999999999999996,37329]
["","","STRUCTURAL STEEL REPAIR","",975,146,142350]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",228,50,11400]
["","","EPOXY COATING","",14958,17.5,261765]
["8893000000-E","GENERIC STR ITEM (SY)","CONC DECK REPAIR FOR PPC OVERLAY","",30.9,332,10258.799999999999]
["","","CONCRETE DECK REPAIR FOR PPC OVERLAY","",62,450,27900]
["","","PLACING & FINISHING PPC OVER- LAY","",16223.4,24,389361.6]
["","","PLACING AND FINISHING PPC OVERLAY","",18256,22,401632]
["","","SCARIFYING BRIDGE DECK","",34479.4,16.0005423528252,551689.1]
["","","SHOTBLASTING BRIDGE DECK","",34479.4,4.6354791556697599,159828.54]
["8897000000-N","GENERIC STR ITEM (EA)","CLEANING & PAINTING EXISTING","BEARINGS WITH HRCSA",84,500,42000]

{"sheet":"ITEMS - DIV 02","index":4,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 02"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",1,920000,920000]
["0106000000-E","BORROW EXCAVATION","","",39047,3.35,130807.45]
["0255000000-E","GENERIC GRADING ITEM (TON)","CLASS IV SUBGRADE STABILIZA- TION","",41721,30,1251630]
["0264000000-E","GENERIC GRADING ITEM (SMI)","MEDIAN SHOULDER RECONSTRUC- TION (T1)","",63.35,2500,158375]
["","","OUTSIDE SHOULDER RECONSTRUC- TION (T2)","",50.57,3300,166881]
["1099500000-E","SHALLOW UNDERCUT","","",29686,2.25,66793.5]
["1297000000-E","MILL ASP PVMT *****\" DTH","(2-1/2\")","",900551,2,1801102]
["1330000000-E","INCIDENTAL MILLING","","",4388,16,70208]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",93432,39,3643848]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",116924,41.75,4881577]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",113640,39,4431960]
["1575000000-E","ASP FOR PLANT MIX","","",16635,365,6071775]
["1840000000-E","MILLED RUMBLE STRIPS","","",536419,0.2,107283.8]
["3030000000-E","STL BEAM GUARDRAIL","","",6979,16.5,115153.5]
["3287000000-N","GR END TYPE TL-3","","",36,3000,108000]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",6979,1.25,8723.75]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",672,9.89,6646.08]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",3,5305,15915]
["4424000000-N","WZ PRESENCE LIGHTING","","",20,6140,122800]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",15,325,4875]
["4510000000-N","LAW ENFORCEMENT","","",1152,50,57600]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","LANE CLOSURE","",130,2450,318500]
["","","RAMP/LOOP CLOSURE","",48,2125,102000]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",615414,0.64,393864.96000000002]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",68677,0.88,60435.76]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",23550,1.8,42390]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",1965,2.65,5207.25]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",439,5.8,2546.1999999999998]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",32,45,1440]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",126,120,15120]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",2330,4.2,9786]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",670,8.5,5695]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",678364,0.12,81403.679999999993]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",24765,0.45,11144.25]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",439,2.5,1097.5]
["4840000000-N","PAINT PVT MKG CHARACTER","","",24,25,600]
["4845000000-N","PAINT PVT MKG SYMBOL","","",114,40,4560]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",2290,0.75,1717.5]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",670,1,670]
["4905000000-N","SNOWPLB PVMT MRKER","","",5182,24,124368]
["6000000000-E","TEMP SILT FENCE","","",2530,2.9,7337]
["6071010000-E","WATTLE","","",1265,7.95,10056.75]
["6084000000-E","SEEDING AND MULCHING","","",83.86,1775,148851.5]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",3,495,1485]

{"sheet":"ITEMS - DIV 03","index":5,"n_rows":357,"n_cols":7,"rows_kept":357,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 03"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",12,357268.88250000001,4287226.59]
["0000400000-N","CONST SURVEYING","","",3,52546.396666666697,157639.19]
["0000500000-N","SUPP FIELD SURVEYING","","",80,60,4800]
["0000600000-N","SUPP SURVEYING OFF CALC","","",20,110,2200]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","REMOVE & STOCKPILE TEMPORARY BRIDGE","",1,200000,200000]
["0001000000-E","CLEARING & GRUBBING","","",1,16611.0846153846,21594.41]
["0008000000-E","SUPP CLEARING & GRUBBING","","",1,16119.58,16119.58]
["0022000000-E","UNCLAS EXCAVATION","","",6100,15.41,94001]
["0028000000-N","TYPE I STANDARD APPR **********","(606+95 -L- LT)","",1,53200,53200]
["","","(606+95 -L- RT)","",1,53200,53200]
["0029000000-N","TYPE III REINF APPR **********","(12+68.00 -L-)","",1,15000,15000]
["","","(15+56.00 -L-)","",1,15000,15000]
["","","(19+45.50 -L-)","",1,15000,15000]
["0036000000-E","UNDERCUT EXCAVATION","","",2700,7.9133333333333304,21366]
["0043000000-N","GRADING","","",1,325000,325000]
["0050000000-E","SUPP CLEARING & GRUBBING","","",2,1,2]
["0063000000-N","GRADING","","",1,33000,33000]
["0106000000-E","BORROW EXCAVATION","","",38473,24.3006100382086,934917.37]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",690,14.51,10011.9]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",780,14.68,11450.4]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",1700,23.02,39134]
["0195000000-E","SELECT GRANULAR MAT'L","","",1300,10.8461538461539,14100]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",4000,1.6335,6534]
["0199000000-E","TEMP SHORING","","",1370,37,50690]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",50,79.430000000000007,3971.5]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",3822,50.490266875981199,192973.8]
["0320000000-E","FND CONDIT GEOTEXTILE","","",8898,1.7308833445718099,15401.4]
["0335200000-E","15\" DRAINAGE PIPE","","",148,50,7400]
["0366000000-E","15\" RC PIPE CULV III","","",188,75,14100]
["0448200000-E","15\" RCP CULV CLASS IV","","",5604,57.73,323518.92]
["0448300000-E","18\" RCP CULV CLASS IV","","",7122,71.230870541982597,507306.26]
["0448400000-E","24\" RCP CULV CLASS IV","","",3312,95.11,315004.32]
["0448500000-E","30\" RCP CULV CLASS IV","","",840,118.55,99582]
["0448600000-E","36\" RCP CULV CLASS IV","","",136,502.57,68349.52]
["0546000000-E","**\" CAA PIPE CLVT *****\"","(18\", 0.064\")","",68,92,6256]
["0564000000-E","**\" CAA PIPE ELBOW *****\"","(18\", 0.064\")","",4,1600,6400]
["0995000000-E","PIPE REMOVAL","","",2207,44.429202537381101,98055.25]
["1011000000-N","FINE GRADING","","",1,774722.16,774722.16]
["1099500000-E","SHALLOW UNDERCUT","","",400,17.422499999999999,6969]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",780,43.181794871794899,33681.800000000003]
["1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",5790,39.731865284974099,230047.5]
["1220000000-E","INCIDENTAL STONE BASE","","",6803,60.865757753932101,414069.75]
["1245000000-E","SHOULDER RECONST","","",167.77,2263.42099302617,379734.14]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",42154,2.0841139630877299,87853.74]
["","","(1-1/2\")","",704022,1.98833990983236,1399835.04]
["","","(1-1/4\")","",41268,1.92698458854318,79522.8]
["","","(2\")","",322235,2.47273455707791,796801.62]
["","","(2-1/2\")","",23183,3.3834059440107001,78437.5]
["","","(4\")","",2200,12.79,28138]
["","","(5-1/2\")","",5015,6.67,33450.050000000003]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" - 1-1/2\")","",59278,3.25,192653.5]
["","","(0\" TO 1-1/2\")","",8173,5.1119784656796803,41780.199999999997]
["","","(0\" TO 1-1/4\")","",3061,4,12244]
["","","(0\" TO 2-1/2\")","",6500,10.57,68705]
["","","(0\" TO 4\")","",670,7.26,4864.2]
["","","(2\", 4\")","",3500,2.95,10325]
["1330000000-E","INCIDENTAL MILLING","","",30868,13.88386030841,428567]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",11505,67.172968274663205,772825]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",30955,78.309384590534606,2424067]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",6460,58,374680]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",23725,67.196164383561594,1594229]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",211672,51.001259448580797,10795538.59]
["1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",2721,91.532249173098094,249059.25]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",51147,58.501593446340898,2992181]
["1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",340,103.529411764706,35200]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",25780,56.396431342125702,1453900]
["1525100000-E","ASP CONC SURF CRS SF9.5A LEVEL","","",125,85,10625]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",3345,63,210735]
["1575000000-E","ASP FOR PLANT MIX","","",22165,483.85034062711497,10724542.800000001]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",750,294.26,220695]
["1770000000-E","AST, MAT COAT, 6 STONE","","",12807,1.98,25357.86]
["1775500000-E","AST, MAT COAT, *** STONE","(67)","",380505,1.8791769621949801,715036.23]
["1838000000-E","EMULSION FOR AST","","",156700,2.3003216336949599,360460.4]
["1840000000-E","MILLED RUMBLE STRIPS","","",8045,1.1000000000000001,8849.5]
["1880000000-E","GENERIC PAVING ITEM (TON)","ASPHALT FOR PAVEMENT INTERLAY-ER S4.75A","",500,90,45000]
["","","PATCHING EXISTING PAVEMENT","(FULL DEPTH)",1543,180.19051198963101,278033.96000000002]
["","","","(MILL)",1005,144.341890547264,145063.6]
["","","","(MILL) I19.0C",1350,140,189000]
["","","","(MILL) S9.5C",300,170,51000]
["","","","I19.0C (MILL)",430,156.75,67402.5]
["","","PATCHING EXISTING PAVEMENT (MILL)","",7192,159.283912680756,1145569.8999999999]
["1891000000-E","GENERIC PAVING ITEM (SY)","PAVEMENT INTERLAYER","",112524,4.25,478227]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",8,500,4000]
["2022000000-E","SUBDRAIN EXCAVATION","","",560,9.48,5308.8]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2500,2.6320000000000001,6580]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",420,68.712000000000003,28859.040000000001]
["2044000000-E","6\" PERF SUBDRN PIPE","","",2700,10.6444444444444,28740]
["2070000000-N","SUBDRN PIPE OUTLET","","",5,294.56,1472.8]
["2077000000-E","6\" OUTLET PIPE","","",30,18.216000000000001,546.48]
["2209000000-E","ENDWALLS","","",3.4,3298.2205882352901,11213.95]
["2253000000-E","PIPE COLLARS","","",2.16,563.38888888888903,1216.92]
["2275000000-E","FLOWABLE FILL","","",2,417,834]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",164,1797.4660365853699,294784.43]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",18.3,897.15027322404399,16417.849999999999]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",26,710.163461538462,18464.25]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",8,740,5920]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",6,500,3000]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",16,756.3,12100.8]
["","","(F)","",49,777.88,38116.120000000003]
["","","(G)","",54,777.88,42005.52]
["2396000000-N","FRAME W/COVER STD 840.54","","",5,593.92999999999995,2969.65]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",1,1500,1500]
["2484000000-E","GENERIC DRAINAGE ITEM (LF)","REMOVE & REPLACE","2'-6\" CURB & GUTTER",625,55,34375]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",28690,18.4974729871035,530692.5]
["2556000000-E","SHOULDER BERM GUTTER","","",60,45,2700]
["2580000000-E","CONC VALLEY GUTTER","","",85,47.74,4057.9]
["2591000000-E","4\" CONC SIDEWALK","","",7,100,700]
["2605000000-N","CONC CURB RAMPS","","",1,2500,2500]
["2612000000-E","6\" CONC DRIVEWAY","","",2768,54.764414739884401,151587.9]
["2613000000-N","REM & REP CURB RAMPS","","",5,2750,13750]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",269,60.3271375464684,16228]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",85,90,7650]
["2738000000-E","GENERIC PAVING ITEM (SY)","6\" CONCRETE DRIVEWAY","",40,70,2800]
["","","REMOVE & REPLACE 4\" CONC SIDE-WALK","",24,100,2400]
["","","REMOVE & REPLACE 5\" MONOLITHIC","CONC ISLANDS",146,75,10950]
["","","REMOVE AND REPLACE 5\"","MONOLITHIC CONCRETE ISLANDS",69,162.04,11180.76]
["","","REMOVE MONOLITHIC CONC ISLAND","",38,40,1520]
["2752000000-E","GENERIC PAVING ITEM (LF)","REMOVE & REPLACE 2'-0\" CURB & GUTTER","",195,70,13650]
["","","REMOVE & REPLACE 2'-6\" CURB & GUTTER","",179,78.659217877095003,14080]
["","","REMOVE 4\" X 8\" CONCRETE CURB","",118,20,2360]
["2759000000-N","GENERIC PAVING ITEM (EA)","ADJUSTMENT OF MONUMENTS","",178,600,106800]
["2800000000-N","ADJ CATCH BASINS","","",3,631.09,1893.27]
["2815000000-N","ADJ DROP INLETS","","",2,631.08000000000004,1262.1600000000001]
["2830000000-N","ADJ MANHOLES","","",156,643.16615384615397,100333.92]
["2845000000-N","ADJ METER OR VALVE BOXES","","",125,639.35440000000006,79919.3]
["3000000000-N","IMPACT ATTEN TYPE 350","","",1,15000,15000]
["3030000000-E","STL BEAM GUARDRAIL","","",3100,18.2802419354839,56668.75]
["3060000000-E","SBGR DOUBLE FACED","","",275,22,6050]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",19,25,475]
["3210000000-N","GR END TYPE CAT-1","","",11,765.22545454545502,8417.48]
["3215000000-N","GR ANCHOR TYPE III","","",18,1751.1111111111099,31520]
["3287000000-N","GR END TYPE TL-3","","",32,3229.86375,103355.64]
["3317000000-N","GR ANCHOR TYPE B-77","","",12,1997.6866666666699,23972.240000000002]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",1300,12.21,15873]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",1545,1.3980582524271801,2160]
["3420000000-E","GENERIC GUARDRAIL ITEM (LF)","REMOVE & REPLACE EXISTING","GUARDRAIL",400,20.52,8208]
["","","REMOVE & REPLACE EXISTING GUARDRAIL","",6425,16.824902723735399,108100]
["3649000000-E","RIP RAP, CLASS B","","",107,108.621121495327,11622.46]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",2215,2.56406320541761,5679.4]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",30,15.5,465]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",715,7.4035664335664304,5293.55]
["4102000000-N","SIGN ERECTION, TYPE E","","",20,87.968000000000004,1759.36]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",1,277.60000000000002,277.60000000000002]
["","","(E)","",26,94.39,2454.14]
["","","(F)","",1,161.01,161.01]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",18,1,18]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",10,6.66,66.599999999999994]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",1656,9.7139371980676295,16086.28]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",1643,8.3398356664637898,13702.35]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",295,11.3643389830508,3352.48]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",21695,8.4289472228624103,182866.01]
["4415000000-N","FLASHING ARROW BOARD","","",4,2500,10000]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",25,11200,280000]
["4430000000-N","DRUMS","","",175,40,7000]
["4445000000-E","BARRICADES (TYPE III)","","",216,40.983703703703704,8852.48]
["4455000000-N","FLAGGER","","",190,333.15789473684202,63300]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",9,190222.685555556,1712004.17]
["4480000000-N","TMA","","",5,12200,61000]
["4485000000-E","PORT CONC BARRIER","","",100,100,10000]
["4500000000-E","REM & RES PORT CONC BARRIER","","",1000,25,25000]
["4510000000-N","LAW ENFORCEMENT","","",1280,45.465312500000003,58195.6]
["4516000000-N","SKINNY DRUM","","",230,45,10350]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",838517,0.54519502884258997,457155.3]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",913427,0.61282337833236999,559769.42000000004]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",16320,1.1464270833333301,18709.689999999999]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",3332,1.1615126050420199,3870.16]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",5524,2.7958725561187499,15444.4]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",805,5.67,4564.3500000000004]
["4705000000-E","THERMO LINES 16\" 120MILS","","",300,7.3333333333333304,2200]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",5744,10.5593071030641,60652.66]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",180,108.94244444444401,19609.64]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",1421,105.243814215341,149551.46]
["4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",28,125,3500]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",14560,3.375,49140]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",2808387,0.12643142843204999,355068.38]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",150,0.45,67.5]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",484,0.79214876033058002,383.4]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",400,1.125,450]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",1277,2.5088801879404898,3203.84]
["4840000000-N","PAINT PVT MKG CHARACTER","","",22,43.181818181818201,950]
["4845000000-N","PAINT PVT MKG SYMBOL","","",260,42.567807692307703,11067.63]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",17196,2.39301465457083,41150.28]
["4847050000-E","POLYUREA LINES (8\", 20 MILS)","","",630,2.56,1612.8]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",520,2,1040]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","THERMOPLASTIC PROFILED","PAVEMENT MARKING LINES (EDGE LINES)",78760,0.95,74822]
["4900000000-N","PERM RAISED PVMT MARKERS","","",9268,5.1513185153215399,47742.42]
["4905000000-N","SNOWPLB PVMT MRKER","","",9208,28.876106646394401,265891.19]
["5255000000-N","PORTABLE LIGHTING","","",3,31835.38,95506.14]
["5325400000-E","4\" WATER LINE","","",257,42.91,11027.87]
["5325800000-E","8\" WATER LINE","","",12896,23.42,302024.32000000001]
["5329000000-E","DI H2O PIPE FITTINGS","","",3760,5.15,19364]
["5538000000-E","4\" VALVE","","",4,1152.99,4611.96]
["5540000000-E","6\" VALVE","","",4,1343.01,5372.04]
["5546000000-E","8\" VALVE","","",13,2118.67,27542.71]
["5648000000-N","RELOCATE WATER METER","","",18,627.52,11295.36]
["5649000000-N","RECONNECT WATER METER","","",47,814.41,38277.269999999997]
["5672000000-N","RELOCATE FIRE HYDRANT","","",5,1883.49,9417.4500000000007]
["5673000000-E","FIRE HYDRANT LEG","","",76,62.08,4718.08]
["5686000000-E","**\" H2O SERVICE LINE","(3/4\")","",3678,16.989999999999998,62489.22]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",12896,4.79,61771.839999999997]
["6000000000-E","TEMP SILT FENCE","","",48423,3.9286413481197,190236.6]
["6006000000-E","EROS CONTRL STONE CL A","","",975,92.320820512820504,90012.800000000003]
["6009000000-E","EROS CONTRL STONE CL B","","",2910,70.654529209621998,205604.68]
["6012000000-E","SEDIMENT CONTROL STONE","","",3835,45.957204693611502,176245.88]
["6015000000-E","TEMP MULCHING","","",119.14,1100.6776901124699,131134.74]
["6018000000-E","SEED FOR TEMP SEEDING","","",6063,4.8726538017483101,29542.9]
["6021000000-E","FERT FOR TEMP SEEDING","","",30.74,953.20624593363698,29301.56]
["6024000000-E","TEMP SLOPE DRAINS","","",830,18.971927710843399,15746.7]
["6029000000-E","SAFETY FENCE","","",6900,2.3136231884058001,15964]
["6030000000-E","SILT EXCAVATION","","",1950,7.47974358974359,14585.5]
["6036000000-E","MATTING FOR EROS CONTROL","","",54000,2.1897037037036999,118244]
["6037000000-E","COIR FIBER MAT","","",2770,4.48043321299639,12410.8]
["6038000000-E","PERM SOIL REINF MAT","","",215,4.4400000000000004,954.6]
["6042000000-E","1/4\" HARDWARE CLOTH","","",10916,3.6856485892268198,40232.54]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",55,7.68,422.4]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",300,70,21000]
["6070000000-N","SPECIAL STILLING BASINS","","",2,580,1160]
["6071010000-E","WATTLE","","",1440,17.294722222222202,24904.400000000001]
["6071012000-E","COIR FIBER WATTLE","","",5090,16.467269155206299,83818.399999999994]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",825,22,18150]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",2135,9.9668149882904,21279.15]
["6071030000-E","COIR FIBER BAFFLE","","",210,9.99,2097.9]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",3,776.04,2328.12]
["6084000000-E","SEEDING AND MULCHING","","",95.06,2514.5494424573999,239033.07]
["6087000000-E","MOWING","","",25.5,430.77803921568602,10984.84]
["6090000000-E","SEED FOR REPAIR SEEDING","","",4538,10.3349537241075,46900.02]
["6093000000-E","FERT FOR REPAIR SEEDING","","",22.15,936.696613995485,20747.830000000002]
["6096000000-E","SEED FOR SUPP SEEDING","","",675,2.1955555555555599,1482]
["6108000000-E","FERTILIZER TOPDRESSING","","",19.25,907.96571428571394,17478.34]
["6111000000-E","IMPERVIOUS DIKE","","",100,150,15000]
["6114500000-N","SPECIALIZED HAND MOWING","","",30,34.76,1042.8]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",178,258.406853932584,45996.42]
["6117500000-N","CONC WASHOUT STR","","",12,2921.0416666666702,35052.5]
["6123000000-E","REFORESTATION","","",0.1,4441.6000000000004,444.16]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","CONCRETE WASHOUT STRUCTURE","",2,500,1000]
["7252000000-E","MESSENGER CABLE (1/4\")","","",300,2.5,750]
["7279000000-E","TRACER WIRE","","",109390,0.53,57976.7]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",1170,7.7679487179487197,9088.5]
["","","(2, 2\")","",99700,4.28,426716]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",60,19.440000000000001,1166.4000000000001]
["","","(2, 2\")","",9030,13.15,118744.5]
["7312000000-N","JUNCTION BOX (***************)","(OVER-SIZED, HEAVY-DUTY)","",129,382.5,49342.5]
["","","(SPECIAL-SIZE, HEAVY-DUTY)","",12,855,10260]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",11,319.25,3511.75]
["7360000000-N","WOOD POLE","","",2,1450,2900]
["7372000000-N","GUY ASSEMBLY","","",2,525,1050]
["7432000000-E","2\" RISER WITH TUBING","","",2,580,1160]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",24550,6.2165091649694499,152615.29999999999]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",5312,2.0097740963855402,10675.92]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",9100,1.74,15834]
["","","(72)","",126450,1.98,250371]
["7540000000-N","SPLICE ENCLOSURE","","",12,3075,36900]
["7552000000-N","INTERCONNECT CENTER","","",10,1640,16400]
["7566000000-N","DELINEATOR MARKER","","",140,148,20720]
["7744000000-N","DETECTOR CARD (TYPE 170)","","",2,199.85,399.7]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","BRIDGE JUNCTION BOX","",10,1440,14400]
["","","ENCLOSED COMMUNICATIONS RACK","",1,4615,4615]
["","","ETHERNET HUB SWITCH","",1,16892,16892]
["","","FIELD ETHERNET SWITCH","",12,1325,15900]
["","","HUB INTERCONNECT CENTER","",1,5175,5175]
["","","KVM SWITCH","",1,1985,1985]
["","","VIDEO PROCESSING UNIT","",1,8105,8105]
["","","WORKSTATION","",1,2880,2880]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","BUILDING MODIFICATIONS","",1,24500,24500]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","BRIDGE CONDUIT SYSTEM","",7100,89.5,635450]
["8017000000-N","CM&R TEMP ACCESS ***********","(606+95.00 -L-)","",1,1,1]
["8035000000-N","REMV EXIST STR **********","(12+68.00 -L-)","",1,35000,35000]
["","","(15+56.00 -L-)","",1,35000,35000]
["","","(19+45.50 -L-)","",1,35000,35000]
["","","(43+95.83 TO 55+16.87)","",1,800000,800000]
["8065000000-N","ASBESTOS ASSESSMENT","","",1,5000,5000]
["8112730000-N","PDA TESTING","","",9,2900,26100]
["8121000000-N","UNCL STR EXCAV STA *****","(12+68.00 -L-)","",1,7500,7500]
["","","(15+56.00 -L-)","",1,7500,7500]
["","","(19+45.50 -L-)","",1,7500,7500]
["8147000000-E","REINF CONC DECK SLAB","","",41662,40,1666480]
["8161000000-E","GROOVING BRIDGE FLOORS","","",356367,0.39223595338513001,139779.95000000001]
["8182000000-E","CLASS A CONC (BRIDGE)","","",594,879.444444444444,522390]
["8210000000-N","BRG APPR SLAB ***********","(12+68.00 -L-)","",1,25000,25000]
["","","(15+56.00 -L-)","",1,25000,25000]
["","","(19+45.50 -L-)","",1,25000,25000]
["","","(606+95.00 -L- LT)","",1,54000,54000]
["","","(606+95.00 -L- RT)","",1,54000,54000]
["8217000000-E","REINF STEEL (BRIDGE)","","",75266,1.33318895650094,100343.8]
["8262000000-E","45\" PRESTR CONC GIRDR","","",5541.66,210.650000180451,1167350.68]
["8296000000-N","POLLUTION CONTROL","","",2,62500,125000]
["8328000000-E","PILE DRV EQUIP SETUP * PRESTR CONC PILES","(20\")","",60,2780,166800]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",58,1388.96551724138,80560]
["8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",7,1500,10500]
["8336000000-E","20\" PRESTR CONC PILES","","",4200,92.5,388500]
["8364000000-E","HP12X53 PILES","","",3600,39.75,143100]
["8384200000-E","HP14X73 GALV PILES","","",490,65,31850]
["8393000000-N","PILE REDRIVES","","",81,65.679012345678998,5320]
["8475000000-E","TWO BAR METAL RAIL","","",8482,125,1060250]
["8503000000-E","CONC BARRIER RAIL","","",2319.4,107.5,249335.5]
["8505000000-E","VERT CONC BARRIER RAIL","","",451,100,45100]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-9\")","",2240,100,224000]
["8559000000-E","SURFACE PREP, CLASS II","","",25,1068,26700]
["8566000000-E","SURFACE PREP, CLASS III","","",13.5,4135,55822.5]
["8590000000-E","RIP RAP, CLASS **","(A, 1'-0\" THICK)","",970,86.5,83905]
["8608000000-E","RIP RAP II (2'-0\")","","",2665,78.105065666041298,208150]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2966,3.26323331085637,9678.75]
["8657000000-N","ELASTOMERIC BEARINGS","","",4,30750,123000]
["8660000000-E","CONC REPAIRS","","",265,714.39622641509402,189315]
["8664000000-E","SHOTCRETE REPAIRS","","",1431,602.16701607267601,861701]
["8678000000-E","EPOXY RESIN INJECTION","","",1940,112.74587628866,218727]
["8692000000-N","FOAM JOINT SEALS","","",1,87500,87500]
["8699000000-N","STRIP SEALS","","",1,110000,110000]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",350,135,47250]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",700,145,101500]
["8860000000-N","GENERIC STR ITEM (LS)","ASBESTOS ASSESSMENT","",1,2500,2500]
["","","AUXILIARY COUNTERWEIGHT & SPAN","GUIDE REPAIRS",1,700000,700000]
["","","CLEANING & REPAINTING OF BRIDGE 13","",1,1350000,1350000]
["","","INSTALL NEW SIGNS","",1,10000,10000]
["","","INSTALLATION OF 3'-0\" X 2'-0\"","PRESTRESSED CONCRETE CORED SLABS",1,66700,66700]
["","","MECHANICAL OPERATING MACHINERY","",1,225000,225000]
["","","OPERATOR HOUSE RENOVATION","",1,1588780.45,1588780.45]
["","","PAINTING CONTAINMENT FOR BRIDGE 13","",1,886000,886000]
["","","REPLACE AIR HORN","",1,5000,5000]
["","","REPLACEMENT OF STEEL GRID DECK","",1,3600000,3600000]
["","","UNDER STRUCTURE WORKPLATFORM","",1,0.01,0.01]
["8867000000-E","GENERIC STR ITEM (LF)","1'-2\" X 1'-11\" CONCRETE","PARAPET FOR RAIL RETROFIT",6249,125,781125]
["","","3'-0\" X 1'-8\" PRESTRESSED","CONC CORED SLABS",13398,228,3054744]
["","","3'-2\" X 1'-6\" PRESTRESSED","CONC CORED SLABS",2233,228,509124]
["","","BRIDGE JOINT REMOVAL","",1871,32.2771512560128,60390.55]
["","","CP INTEGRAL PILE JACKET","(STRUCTURAL), 16 TO 30 IN.",998,1450,1447100]
["","","MODIFIED ALASKA BARRIER RAIL","",3034,250,758500]
["","","RAIL REMOVAL (SPANS 29-65)","",6249,40,249960]
["","","RAIL RETROFIT","",3599,140,503860]
["","","SILICONE JOINT SEALANT","",2990,53.953177257525098,161320]
["8881000000-E","GENERIC STR ITEM (CY)","FLOWABLE FILL","",8,1000,8000]
["","","PPC MATERIALS","",1706,2659.0855803048098,4536400]
["","","UNCLASSIFIED STRUCTURE","EXCAVATION AT 606+95.00 -L- LT",12000,10.5,126000]
["","","","EXCAVATION AT 606+95.00 -L- RT.",3200,10.5,33600]
["8882000000-E","GENERIC STR ITEM (CF)","REPAIRS TO PRESTRESSED","CONCRETE GIRDERS",152,991,150632]
["","","REPAIRS TO PRESTRESSED CONC-","RETE GIRDERS",211.5,763.82978723404301,161550]
["8889000000-E","GENERIC STR ITEM (LB)","STRUCTURAL STEEL FOR REPAIRS","",25000,24,600000]
["8892000000-E","GENERIC STR ITEM (SF)","CONCRETE DECK REPAIR FOR EPOXY","OVERLAY",52,50,2600]
["","","CP SYSTEM, ZINC ALUMINUM SPRAY","",13375,32.738317757009298,437875]
["","","EPOXY OVERLAY SYSTEM","",7390,4,29560]
["","","EPOXY PROTECTIVE COATING","",3527,33,116391]
["8893000000-E","GENERIC STR ITEM (SY)","CONCRETE DECK REPAIR FOR","PPC OVERLAY",6,400,2400]
["","","CONCRETE DECK REPAIR FOR PPC","OVERLAY",9,500,4500]
["","","CONCRETE DECK REPAIR FOR PPC OVERLAY","",10,750,7500]
["","","HYDRO-DEMOLITION OF BRIDGE DECK","",13.5,1.0370370370370001E-2,0.14000000000000001]
["","","PLACING & FINISHING PPC OVER-LAY","",17655,18.899999999999999,333679.5]
["","","PLACING AND FINISHING PPC","OVERLAY",20905,29.75,621923.75]
["","","PLACING AND FINISHING PPC OVERLAY","",6674,30,200220]
["","","SCARIFYING BRIDGE DECK","",40676,14.178864686793199,576739.5]
["","","SHOTBLASTING BRIDGE DECK","",46153,3.09434056291032,142813.1]
["8897000000-N","GENERIC STR ITEM (EA)","CP INTEGRAL PILE JACKET, 16\" TO 30\"","",150,300,45000]
["","","CP SYSTEM (ZINC BULK ANODE)","",22,4500,99000]
["","","CP SYSTEM (ZINC BULK ANODES)","",22,7800,171600]
["","","SPLICING OF PRESTRESSING STRAND","",1,3500,3500]
["","","TYPE I BRIDGE JACKING","",3,35000,105000]

{"sheet":"ITEMS - DIV 04","index":6,"n_rows":574,"n_cols":7,"rows_kept":574,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 04"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",9,707837,6370533]
["0000400000-N","CONSTRUCTION SURVEYING","","",6,194791.66666666701,1168750]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN SUPPORT","",1,94300,94300]
["","","UTILITY COORDINATOR","",1,289000,289000]
["0001000000-E","CLEARING & GRUBBING","","",48,149708.07301255199,7156045.8899999997]
["0008000000-E","SUPP CLEARING & GRUBBING","","",8,4841.25,38730]
["0015000000-N","SEALING ABANDONED WELLS","","",6,2995.8333333333298,17975]
["0022000000-E","UNCLASSIFIED EXCAVATION","","",222450,6.5286356484603303,1452295]
["0028000000-N","TYPE I STANDARD APPR **********","(25+00)","",1,35000,35000]
["","","(64+20 -L-)","",1,80000,80000]
["0030000000-N","TYPE II MODIFIED APPR **********","(99+17.60 -L1-)","",1,25000,25000]
["0036000000-E","UNDERCUT EXCAVATION","","",52500,8.8011904761904791,462062.5]
["0043000000-N","GRADING","","",1,640000,640000]
["0050000000-E","SUPP CLEARING & GRUBBING","","",1,1,1]
["0057000000-E","UNDERCUT EXCAVATION","","",65250,10.7356321839081,700500]
["0106000000-E","BORROW EXCAVATION","","",615900,7.5813646695892203,4669362.5]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",9928,19.662610797743799,195210.4]
["0141000000-E","BERM DITCH CONSTRUCTION","","",3600,2.0499999999999998,7380]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",59410,6.7331375189362097,400015.7]
["0177000000-E","BREAKING OF EXT ASPH PVMT","","",21060,3.3464387464387499,70476]
["0192000000-N","PROOF ROLLING","","",76,210.831578947368,16023.2]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",10100,31,313100]
["0195000000-E","SELECT GRANULAR MATERIAL","","",70450,5.0733853797019197,357420]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",142950,1.4844001399090601,212195]
["0199000000-E","TEMPORARY SHORING","","",5589,43.6441223832528,243927]
["0222000000-E","GEOTEXTILE ROCK EMBANK","","",440,3.35,1474]
["0223000000-E","ROCK PLATING","","",3150,65.952380952380906,207750]
["0225000000-E","REINFORCED SOIL SLOPES","","",3850,78.400000000000006,301840]
["0234000000-E","GENERIC GRADING ITEM (CY)","CLASS II, TYPE 2","GRANULAR SOIL",5500,18.850000000000001,103675]
["","","SHALLOW UNDERCUT","",4422,11.8,52179.6]
["0241000000-E","GENERIC GRADING ITEM (SY)","GEOCELLS","",3850,45.4,174790]
["","","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",1550,11.927419354838699,18487.5]
["0248000000-N","GENERIC GRADING ITEM (LS)","SITE GRADING","",1,7125750,7125750]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",190,160.13157894736801,30425]
["","","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",102,200,20400]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",12056,30.512591240875899,367859.8]
["0320000000-E","FND CONDIT GEOTEXTILE","","",47446,2.5870821565569302,122746.7]
["0335000000-E","**\" DRAINAGE PIPE","(54\")","",108,240.76851851851899,26003]
["","","(60\")","",264,305,80520]
["","","(66\")","",456,363,165528]
["","","(8\")","",8,45,360]
["0335100000-E","12\" DRAINAGE PIPE","","",28,33,924]
["0335200000-E","15\" DRAINAGE PIPE","","",7384,42.996803900324998,317488.40000000002]
["0335300000-E","18\" DRAINAGE PIPE","","",3992,50.213236472945901,200451.24]
["0335400000-E","24\" DRAINAGE PIPE","","",2312,63.011937716262999,145683.6]
["0335500000-E","30\" DRAINAGE PIPE","","",1300,78.236923076923105,101708]
["0335600000-E","36\" DRAINAGE PIPE","","",964,90.917717842323697,87644.68]
["0335700000-E","42\" DRAINAGE PIPE","","",912,115.115438596491,104985.28]
["0335800000-E","48\" DRAINAGE PIPE","","",56,132,7392]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",26,279.30769230769198,7262]
["","","(18\")","",10,327.8,3278]
["","","(24\")","",1,421,421]
["0343000000-E","15\" SIDE DRAIN PIPE","","",28,75,2100]
["0344000000-E","18\" SIDE DRAIN PIPE","","",204,48.5,9894]
["0345000000-E","24\" SIDE DRAIN PIPE","","",260,61,15860]
["0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",1828,65.364551422319494,119486.39999999999]
["","","(18\", V)","",236,65.69,15502.84]
["","","(24\", V)","",44,106.44,4683.3599999999997]
["","","(30\", V)","",28,280,7840]
["","","(36\", V)","",212,239.06,50680.72]
["","","(42\", V)","",92,262.39999999999998,24140.799999999999]
["0366000000-E","15\" RC PIPE CULV III","","",860,57.5,49450]
["0372000000-E","18\" RC PIPE CULV III","","",566,62.027420494699598,35107.519999999997]
["0378000000-E","24\" RC PIPE CULV III","","",2694,63.967765404602801,172329.16]
["0384000000-E","30\" RC PIPE CULV III","","",2204,64.431506352087098,142007.04000000001]
["0390000000-E","36\" RC PIPE CULV III","","",2950,94.462413559322002,278664.12]
["0396000000-E","42\" RC PIPE CULV III","","",392,101.75,39886]
["0402000000-E","48\" RC PIPE CULV III","","",1996,126.95,253392.2]
["0408000000-E","54\" RC PIPE CULV III","","",1336,182.05853293413199,243230.2]
["0414000000-E","60\" RC PIPE CULV III","","",3020,233.21252980132499,704301.84]
["0426000000-E","72\" RC PIPE CULV III","","",1634,306.7,501147.8]
["0448000000-E","***\" RCP CULV CLASS IV","(48\")","",1288,210.515527950311,271144]
["","","(54\")","",1192,274.55503355704701,327269.59999999998]
["","","(60\")","",388,359,139292]
["","","(66\")","",244,564.36721311475401,137705.60000000001]
["","","(72\")","",136,475,64600]
["0448200000-E","15\" RCP CULV CLASS IV","","",11605,56.845515725980199,659692.21]
["0448300000-E","18\" RCP CULV CLASS IV","","",23812,56.734735427515503,1350967.52]
["0448400000-E","24\" RCP CULV CLASS IV","","",9180,83.111699346405203,762965.4]
["0448500000-E","30\" RCP CULV CLASS IV","","",3812,103.067618048269,392893.76]
["0448600000-E","36\" RCP CULV CLASS IV","","",1432,153.41670391061501,219692.72]
["0448700000-E","42\" RCP CULV CLASS IV","","",748,179.32834224598901,134137.60000000001]
["0450000000-E","***\" RC PIPE CULV ** (RR)","(72\", V)","",1200,413.65,496380]
["0453000000-E","**\" PIPE END SECTION","(15\")","",4,1578,6312]
["","","(18\")","",5,1170,5850]
["","","(24\")","",2,845,1690]
["","","(30\")","",4,1150,4600]
["","","(36\")","",1,1645,1645]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",991,55.110454086780997,54614.46]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",56,65.25,3654]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",400,80,32000]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",124,100,12400]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.0625\")","",1,368,368]
["","","(15\", 0.064\")","",2,268.33999999999997,536.67999999999995]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\", 0.500\")","",38,315,11970]
["","","(18\", 0.500\")","",222,325,72150]
["","","(24\", 0.500\")","",134,346,46364]
["","","(30\", 0.500\")","",264,441,116424]
["","","(36\", 0.25\")","",108,399,43092]
["","","(36\", 0.500\")","",204,710.25,144891]
["","","(42\", 0.25\")","",76,501,38076]
["","","(42\", 0.500\")","",284,746,211864]
["","","(48\", 0.500\")","",36,809,29124]
["","","(54\", 0.750\")","",232,1145,265640]
["","","(66\", 0.750\")","",178,1357,241546]
["","","(72\", 0.750\")","",64,2315,148160]
["","","(84\", 0.750\")","",90,2503,225270]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\", 0.500\")","",38,525,19950]
["","","(18\", 0.500\")","",222,535.54999999999995,118892.1]
["","","(24\", 0.500\")","",134,640.79999999999995,85867.199999999997]
["","","(30\", 0.500\")","",264,935.4,246945.6]
["","","(36\", 0.25\")","",108,709,76572]
["","","(36\", 0.500\")","",204,1183,241332]
["","","(42\", 0.25\")","",76,829,63004]
["","","(42\", 0.500\")","",284,1167,331428]
["","","(48\", 0.500\")","",36,1230,44280]
["","","(54\", 0.750\")","",232,1610,373520]
["","","(66\", 0.750\")","",178,1820,323960]
["","","(72\", 0.750\")","",64,2880,184320]
["","","(84\", 0.750\")","",90,2587,232830]
["0995000000-E","PIPE REMOVAL","","",13675,22.4522179159049,307034.08]
["0996000000-N","PIPE CLEAN OUT","","",1,4218,4218]
["1011000000-N","FINE GRADING","","",5,410701.87,2053509.35]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",65300,3.18,207654]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",660,231.5,152790]
["1077000000-E","57 STONE","","",200,36.25,7250]
["1099500000-E","SHALLOW UNDERCUT","","",16050,11.0477258566978,177316]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",31650,23.874249605055301,755620]
["1110000000-E","STABILIZER AGGREGATE","","",500,33.75,16875]
["1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",550,30.722727272727301,16897.5]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",23262,3.55,82580.100000000006]
["1121000000-E","AGGREGATE BASE COURSE","","",205282,19.321078565095799,3966269.65]
["1176000000-E","SOIL CEMENT BASE","","",65300,3.05,199165]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",1796,185,332260]
["1209000000-E","ASPHALT CURING SEAL","","",19590,2.65,51913.5]
["1220000000-E","INCIDENTAL STONE BASE","","",4450,34.394157303370797,153054]
["1245000000-E","SHOULDER RECONSTRUCTION","","",9.1300000000000008,1300,11869]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",1826,20.5,37433]
["1275000000-E","PRIME COAT","","",32638,5.7969158649426999,189199.74]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",554675,1.0967298868706901,608328.65]
["","","(1-1/2\")","",20000,3.1512150000000001,63024.3]
["","","(2\")","",318071,1.2054200162856701,383409.15]
["","","(3\")","",5250,3.53,18532.5]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",5590,10.8103756708408,60430]
["","","(0\" TO 2\")","",94515,1.25,118143.75]
["","","(2\" TO 4-1/2\")","",107149,2.25,241085.25]
["1330000000-E","INCIDENTAL MILLING","","",16717,9.3597056888197603,156466.20000000001]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",21630,51.158807212205303,1106565]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",63360,52.237720959595997,3309782]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",22325,52.325722284434498,1168171.75]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",89572,48.5012838833564,4344357]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",74689,45.809631940446401,3421475.6]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",108945,44.312889990362102,4827667.8]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",34206,33,1128798]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",228,95,21660]
["1575000000-E","ASP FOR PLANT MIX","","",19115,499.46020141250301,9547181.75]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",2754,600,1652400]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",13186,60,791160]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",4476,222.85234584450399,997487.1]
["1704000000-E","PATCHING EXIST PAVEMENT","","",100,165,16500]
["1840000000-E","MILLED RUMBLE STRIPS","","",160723,0.11,17679.53]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",554,304.87003610108297,168898]
["2020000000-N","CONTROL-OF-ACCESS MARKERS","","",19,338,6422]
["2022000000-E","SUBDRAIN EXCAVATION","","",4267,17.6493883290368,75309.94]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",9495,9.2630331753554493,87952.5]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",756,5.5644444444444403,4206.72]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",1596,57.816165413533803,92274.6]
["2044000000-E","6\" PERF SUBDRN PIPE","","",13995,10.8507324044302,151856]
["2070000000-N","SUBDRN PIPE OUTLET","","",29,197.94931034482801,5740.53]
["2077000000-E","6\" OUTLET PIPE","","",174,28.0113793103448,4873.9799999999996]
["2143000000-E","BLOTTING SAND","","",20,117,2340]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",17,526.11764705882399,8944]
["2209000000-E","ENDWALLS","","",81.900000000000006,1130.59645909646,92595.85]
["2220000000-E","REINFORCED ENDWALLS","","",130.19999999999999,1364.8645161290301,177705.36]
["2253000000-E","PIPE COLLARS","","",12.105,1259.6117306898,15247.6]
["2275000000-E","FLOWABLE FILL","","",449,337.991091314031,151758]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",889,1660.49390326209,1476179.08]
["2297000000-E","MASNRY DRAINAGE STRUCT","","",207.84800000000001,2553.6267368461599,530766.21]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",376.4,319.19415515409099,120144.68]
["2352000000-N","FRAME W/GRATE 840.***** STD","(840.D13)","",1,450,450]
["2354200000-N","FRAME W/GRATE 840.24 STD","","",2,621.85500000000002,1243.71]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",127,572.58685039370096,72718.53]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",19,771.12,14651.28]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",5,755.82,3779.1]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",134,871.99880597014896,116847.84]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",89,601.82573033707899,53562.49]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",91,716.82494505494503,65231.07]
["","","(F)","",201,738.63258706467695,148465.15]
["","","(G)","",224,692.02803571428603,155014.28]
["2396000000-N","FRAME W/COVER STD 840.54","","",31,516.35548387096799,16007.02]
["2418000000-E","FRM W/GRATES, DRIVEWY DI","","",84,470.65,39534.6]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",16,548.125,8770]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",40,1160.4749999999999,46419]
["2535000000-E","**\"X**\" CONCRETE CURB","(9\" X 12\")","",520,25.230769230769202,13120]
["2538000000-E","**'-**\" CONCRETE CURB & GUTTER","(2'-9\")","",5810,25.939759036144601,150710]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",48500,21.251649484536099,1030705]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",74020,23.252452039989201,1721146.5]
["2556000000-E","SHOULDER BERM GUTTER","","",5930,36.172428330522798,214502.5]
["2570000000-N","MODIFIED CONCRETE FLUME","","",10,2275,22750]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",780,49.6,38688]
["2580000000-E","CONCRETE VALLEY GUTTER","","",170,34.5,5865]
["2591000000-E","4\" CONCRETE SIDEWALK","","",15175,40.6825700164745,617358]
["2600000000-N","RETROFIT EXT CURB RAMPS","","",35,1137.1428571428601,39800]
["2605000000-N","CONCRETE CURB RAMPS","","",131,1573.8549618320601,206175]
["2612000000-E","6\" CONCRETE DRIVEWAY","","",8840,46.151300904977397,407977.5]
["2619000000-E","4\" CONCRETE PAVED DITCH","","",262,152.70839694656499,40009.599999999999]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",110,101,11110]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",10380,57.649566473988401,598402.5]
["2724000000-E","PC REINF BARRIER SNGL FC","","",2082,86.4,179884.79999999999]
["2800000000-N","ADJ CATCH BASINS","","",8,789.46875,6315.75]
["2815000000-N","ADJ DROP INLETS","","",2,1250,2500]
["2830000000-N","ADJ MANHOLES","","",67,762.92537313432797,51116]
["2845000000-N","ADJ METER OR VALVE BOXES","","",188,629.494680851064,118345]
["2860000000-N","CONVERT CB TO JB","","",1,2741.73,2741.73]
["2920000000-N","CONVERT DI TO CB","","",1,1000,1000]
["2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXTISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION BOX",2,1000,2000]
["3030000000-E","STL BEAM GUARDRAIL","","",11275,18.812638580931299,212112.5]
["3045000000-E","SBGR SHOP CURVED","","",1025,21.157317073170699,21686.25]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",35,21.171428571428599,741]
["3210000000-N","GR END TYPE CAT-1","","",37,675.513513513514,24994]
["3215000000-N","GR ANCHOR TYPE III","","",8,1842.5,14740]
["3287000000-N","GR END TYPE TL-3","","",33,3252.9393939393899,107347]
["3317000000-N","GR ANCHOR TYPE B-77","","",8,1800,14400]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",4709,1.9497876406880399,9181.5499999999993]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",7110,3.45534458509142,24567.5]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",459,16.3058823529412,7484.4]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",94,31.297872340425499,2942]
["3572000000-E","CHAIN LINK FENCE RESET","","",65,26.4,1716]
["3628000000-E","RIP RAP, CLASS I","","",4774,52.062997486384603,248548.75]
["3635000000-E","RIP RAP, CLASS II","","",1376,47.6704215116279,65594.5]
["3642000000-E","RIP RAP, CLASS A","","",230,51.7,11891]
["3649000000-E","RIP RAP, CLASS B","","",6263,44.448810474213602,278382.90000000002]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",26717,2.5161676086386899,67224.45]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(D)","",13,21.069230769230799,273.89999999999998]
["","","(E)","",485.5,16.250257466529401,7889.5]
["","","(F)","",108.38,17.526296364642899,1899.5]
["4048000000-E","REINF CONC FOUNDTN","","",1,900,900]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",174,3.5,609]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",5737,6.1588896635872397,35333.550000000003]
["4096000000-N","SIGN ERECTION, TYPE D","","",5,155.69999999999999,778.5]
["4102000000-N","SIGN ERECTION, TYPE E","","",304,79.677631578947398,24222]
["4108000000-N","SIGN ERECTION, TYPE F","","",39,118.94230769230801,4638.75]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(B)","",1,575,575]
["","","(D)","",12,148.458333333333,1781.5]
["","","(E)","",1,158,158]
["","","(F)","",1,250,250]
["4138000000-N","DISPOSE SUPPORT, STL BM","","",2,50,100]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",151,6.10761589403974,922.25]
["4158000000-N","DISPOSE SIGN SYST WOOD","","",7,5.25,36.75]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",12,6.0416666666666696,72.5]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",4245,10.293568904593601,43696.2]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",1584,21.504166666666698,34062.6]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",1052,9.6576045627376406,10159.799999999999]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",11365,7.5866256049274101,86222]
["4415000000-N","FLASHING ARROW BOARD","","",9,3896.6666666666702,35070]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",18,10347.867222222199,186261.61]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",310,56.774193548387103,17600]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",8,4700,37600]
["4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",1,67200,67200]
["4430000000-N","DRUMS","","",2352,40.669005102040799,95653.5]
["4435000000-N","CONES","","",972,26.617283950617299,25872]
["4445000000-E","BARRICADES (TYPE III)","","",888,38.951351351351299,34588.800000000003]
["4450000000-N","FLAGGER","","",2000,37.6,75200]
["4455000000-N","FLAGGER","","",855,412.15204678362602,352390]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",2,43452.71,86905.42]
["4465000000-N","TEMPORARY CRASH CUSHIONS","","",13,5283.8461538461497,68690]
["4470000000-N","REM & RES CRASH CUSHION","","",7,2508.5714285714298,17560]
["4480000000-N","TMA","","",2,7150,14300]
["4485000000-E","PORT CONC BARRIER","","",3136,21.356249999999999,66973.2]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",1623,38.406038200862596,62333]
["4500000000-E","REM & RES PORT CONC BARRIER","","",930,3.7,3441]
["4505000000-E","REM & RES PORT CONC BARR, ANCH","","",216,34,7344]
["4507000000-E","WATER FILLED BARRIER","","",30,84,2520]
["4510000000-N","LAW ENFORCEMENT","","",868,60.077880184331804,52147.6]
["4516000000-N","SKINNY DRUM","","",930,35.803763440860202,33297.5]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","LANE CLOSURE","",256,1,256]
["","","RAMP/LOOP CLOSURE","",8,2680,21440]
["4650000000-N","TEMP RAISED PVMT MRKS","","",3268,7.7422582619339,25301.7]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",454099,0.53249405966539998,241805.02]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",537646,0.72873970977185998,391803.99]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",248510,0.97683996619853997,242754.5]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",43272,1.1399121833980399,49326.28]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",11496,2.8170328810020901,32384.61]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",5350,3.2262859813084099,17260.63]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",24961,3.6933291935419299,92189.19]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",501,4.21,2109.21]
["4705000000-E","THERMO LINES 16\" 120MILS","","",360,6.5555555555555598,2360]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",6256,12.708751598465501,79505.95]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",190,104.631578947368,19880]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",1104,132.56802536231899,146355.1]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(2)","",3200,2.75,8800]
["","","(II)","",3790,3.3410290237467,12662.5]
["","","(IV)","",2720,2.63,7153.6]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",1063,3.89,4135.07]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",241,5.26,1267.6600000000001]
["4805000000-N","COLD APPL PLASTIC SYM TYPE **","(III)","",1,275,275]
["","","(IV)","",4,263.05,1052.2]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",2794205,0.13044204702232001,364481.82]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",291636,0.47425324719855999,138309.32]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",24482,1.0155828772159099,24863.5]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",24706,1.0651177851533999,26314.799999999999]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",360,2.7777777777777799,1000]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",9847,3.2137178836193798,31645.48]
["4840000000-N","PAINT PVT MKG CHARACTER","","",202,33.146138613861403,6695.52]
["4845000000-N","PAINT PVT MKG SYMBOL","","",1510,33.635377483443698,50789.42]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",1972,4.75,9367]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",4430,3.5,15505]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",140679,0.47803879754619,67250.02]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",4430,1,4430]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",1675,0.58471641791045004,979.4]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",521,3.1567178502879099,1644.65]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",85,44.824705882352902,3810.1]
["4900000000-N","PERM RAISED PVMT MARKERS","","",7170,5.9714086471408603,42815]
["4905000000-N","SNOWPLB PVMT MRKER","","",3373,27.633264156537201,93207]
["4915000000-E","7' U-CHANNEL POSTS","","",15,93.26,1398.9]
["4955000000-N","OBJECT MARKERS (END OF RD)","","",15,120.96,1814.4]
["4957000000-N","OBJECT MARKERS (TYPE **)","(III)","",3,195,585]
["5255000000-N","PORTABLE LIGHTING","","",2,51957.5,103915]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",5,550,2750]
["5325400000-E","4\" WATER LINE","","",168,94,15792]
["5325600000-E","6\" WATER LINE","","",982,87.921435845213907,86338.85]
["5325800000-E","8\" WATER LINE","","",1539,70.458349577647795,108435.4]
["5326000000-E","10\" WATER LINE","","",98,63.15,6188.7]
["5326200000-E","12\" WATER LINE","","",12679,66.6869705812761,845524.1]
["5326600000-E","16\" WATER LINE","","",500,142.35,71175]
["5327400000-E","24\" WATER LINE","","",23951,158,3784258]
["5329000000-E","DI H2O PIPE FITTINGS","","",126300,10.302494061757701,1301205]
["5538000000-E","4\" VALVE","","",1,1900,1900]
["5540000000-E","6\" VALVE","","",35,1293.7714285714301,45282]
["5546000000-E","8\" VALVE","","",17,1647.0588235294099,28000]
["5552000000-E","10\" VALVE","","",2,2525,5050]
["5558000000-E","12\" VALVE","","",30,3020.9333333333302,90628]
["5558600000-E","16\" VALVE","","",2,7980,15960]
["5559400000-E","24\" VALVE","","",17,23150,393550]
["5571600000-E","6\" TAPPING SLEEVE & VALVE","","",1,4735,4735]
["5571800000-E","8\" TAPPING SLEEVE & VALVE","","",1,9024,9024]
["5589200000-E","2\" AIR RELEASE VALVE","","",24,7249.1666666666697,173980]
["5606000000-E","2\" BLOW OFF","","",3,4428,13284]
["5648000000-N","RELOCATE WATER METER","","",53,1211.8867924528299,64230]
["5649000000-N","RECONNECT WATER METER","","",31,1033.9354838709701,32052]
["5666000000-N","FIRE HYDRANT","","",30,6040.0666666666702,181202]
["5672000000-N","RELOCATE FIRE HYDRANT","","",23,5317.04347826087,122292]
["5673000000-E","FIRE HYDRANT LEG","","",362,50.039226519336999,18114.2]
["5678400000-E","6\" LINE STOP","","",2,7365,14730]
["5678600000-E","8\" LINE STOP","","",3,8100,24300]
["5678800000-E","10\" LINE STOP","","",1,9470,9470]
["5679000000-E","12\" LINE STOP","","",6,14730,88380]
["5686500000-E","WATER SERVICE LINE","","",1941,28.260226687274599,54853.1]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",292,108.698630136986,31740]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",161,157.85,25413.85]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",205,263,53915]
["5709000000-E","**\" FORCE MAIN SEWER","(2-3/4\")","",202,47.45,9584.9]
["5709300000-E","6\" FORCE MAIN SEWER","","",325,52.6,17095]
["5709400000-E","8\" FORCE MAIN SEWER","","",7307,42.1,307624.7]
["5709600000-E","12\" FORCE MAIN SEWER","","",21754,81.101183690355796,1764275.15]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",46,1500,69000]
["5769000000-E","DI SEWER PIPE FITTINGS","","",24365,11.55,281415.75]
["5775000000-E","4' DIA UTILITY MANHOLE","","",10,2945.5,29455]
["5776000000-E","5' DIA UTILITY MANHOLE","","",21,4321.9047619047597,90760]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",37,633.513513513514,23440]
["5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",57,345.31052631578899,19682.7]
["5798000000-E","ABANDON **\" UTILITY PIPE","(15\")","",198,18,3564]
["","","(2\")","",1051,5.25,5517.75]
["","","(2-3/4\")","",190,5.25,997.5]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",616,10.089285714285699,6215]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",8253,10.397328244274799,85809.15]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",58,12.65,733.7]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",51335,14.583648582838199,748651.6]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",450,19,8550]
["5815500000-N","REMOVE FIRE HYDRANT","","",20,2187.9,43758]
["5816000000-N","ABANDON UTILITY MANHOLE","","",9,1556.6666666666699,14010]
["5828000000-N","REMOVE UTILITY MANHOLE","","",2,1580,3160]
["5835600000-E","12\" ENCASEMENT PIPE","","",108,180,19440]
["5835700000-E","16\" ENCASEMENT PIPE","","",270,105.25,28417.5]
["5836000000-E","24\" ENCASEMENT PIPE","","",920,118.918043478261,109404.6]
["5836200000-E","30\" ENCASEMENT PIPE","","",65,190,12350]
["5836400000-E","36\" ENCASEMENT PIPE","","",1157,140,161980]
["5872500000-E","BORE & JACK **\"","(24\")","",782,632.19948849104901,494380]
["","","(36\")","",51,880,44880]
["5872600000-E","DIRECT DRILL **\"","(24\")","",815,1990,1621850]
["5882000000-N","GENERIC UTILITY ITEM (EA)","10\" PLUG VALVE","",1,7365,7365]
["","","12\" INSERTION VALVE ASSEMBLY","",1,26140,26140]
["","","12\" PLUG VALVE","",24,8945,214680]
["","","8\" PLUG VALVE","",1,6315,6315]
["","","RELOCATE WATER METER WITH","BACKFLOW PREVENTER",1,2225,2225]
["","","RELOCATE WATER MONITORING STATION","",1,725,725]
["5906000000-E","GENERIC UTILITY ITEM (LB)","DUCTILE IRON WATER PIPE FITTINGS","",4970,8,39760]
["6000000000-E","TEMPORARY SILT FENCE","","",141005,1.87007375624978,263689.75]
["6006000000-E","EROS CONTRL STONE CL A","","",8145,40.480982197667302,329717.59999999998]
["6009000000-E","EROS CONTRL STONE CL B","","",18675,40.739678714859402,760813.5]
["6012000000-E","SEDIMENT CONTROL STONE","","",18415,32.4066630464295,596768.69999999995]
["6015000000-E","TEMPORARY MULCHING","","",533,784.59052532833005,418186.75]
["6018000000-E","SEED FOR TEMP SEEDING","","",25600,3.2804687499999998,83980]
["6021000000-E","FERT FOR TEMP SEEDING","","",142.5,998.67368421052595,142311]
["6024000000-E","TEMPORARY SLOPE DRAINS","","",11745,14.0911025968497,165500]
["6029000000-E","SAFETY FENCE","","",9000,1.81,16290]
["6030000000-E","SILT EXCAVATION","","",64510,0.37647651526894998,24286.5]
["6036000000-E","MATTING FOR EROS CONTROL","","",181705,1.4544013648496199,264272]
["6037000000-E","COIR FIBER MAT","","",6350,4.2401574803149602,26925]
["6038000000-E","PERM SOIL REINF MAT","","",16750,6.1698507462686596,103345]
["6042000000-E","1/4\" HARDWARE CLOTH","","",38860,4.0726453937210501,158263]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",1485,5.1492929292929297,7646.7]
["6045000000-E","**\" TEMPORARY PIPE","(18\")","",200,20,4000]
["","","(24\")","",97,50,4850]
["","","(36\")","",160,90,14400]
["","","(42\")","",120,50,6000]
["","","(54\")","",220,82,18040]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",3000,30,90000]
["6069000000-E","STILLING BASINS","","",502,0.01,5.0199999999999996]
["6070000000-N","SPECIAL STILLING BASINS","","",30,541.06666666666695,16232]
["6071010000-E","WATTLE","","",2670,7.6460674157303403,20415]
["6071012000-E","COIR FIBER WATTLE","","",10094,9.3580245690509205,94459.9]
["6071013000-E","WATTLE BARRIER","","",190,9.5,1805]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",991.5,7.8500050428643497,7783.28]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",9720,9.8097993827160508,95351.25]
["6071030000-E","COIR FIBER BAFFLE","","",14770,5.87711577522004,86805]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",73,852.76109589041096,62251.56]
["","","(2\")","",12,1057.9849999999999,12695.82]
["","","(2-1/2\")","",2,1220,2440]
["6084000000-E","SEEDING AND MULCHING","","",376.5,2019.72111553785,760425]
["6087000000-E","MOWING","","",316.2,103.03605313093,32580]
["6090000000-E","SEED FOR REPAIR SEEDING","","",5800,4.3232758620689697,25075]
["6093000000-E","FERT FOR REPAIR SEEDING","","",16.75,1114.0298507462701,18660]
["6096000000-E","SEED FOR SUPP SEEDING","","",10350,3.4467391304347799,35673.75]
["6102000000-E","SODDING","","",7270,7.4,53798]
["6105000000-E","WATER","","",135,185,24975]
["6108000000-E","FERTILIZER TOPDRESSING","","",309.25,964.73015359741305,298342.8]
["6111000000-E","IMPERVIOUS DIKE","","",973,32.787255909558098,31902]
["6114500000-N","SPECIALIZED HAND MOWING","","",125,45.28,5660]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",368,99.4701086956522,36605]
["6117500000-N","CONC WASHOUT STRUCTURE","","",30,1085.5813333333299,32567.439999999999]
["6120000000-E","CULVERT DIVERSION CHANNEL","","",110,30,3300]
["6123000000-E","REFORESTATION","","",6.3,5712.2857142857101,35987.4]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","CONCRETE WASHOUT STRUCTURE","",4,1440,5760]
["","","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",586,123.242320819113,72220]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",164,149.02439024390199,24440]
["","","FLOCCULANT BLOCK","",40,185,7400]
["6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","COMPOST BLANKET","",5,8250,41250]
["6138000000-E","GENERIC EROSION CONTROL ITEM (CY)","COMPOST BLANKET","",430,25,10750]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",28,682.42857142857099,19108]
["7060000000-E","SIGNAL CABLE","","",35599,3.4981698924127098,124531.35]
["7096000000-E","VEHICLE SIGNAL HD (8\", 3 SECT)","","",19,911.05,17309.95]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",169,764.72721893491098,129238.9]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",32,916.9375,29342]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",16,1153.6775,18458.84]
["7252000000-E","MESSENGER CABLE (1/4\")","","",15600,2.19,34164]
["7264000000-E","MESSENGER CABLE (3/8\")","","",7795,3.6417960230917301,28387.8]
["7279000000-E","TRACER WIRE","","",13700,0.71525547445255,9799]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",24153,6.53087608164617,157740.25]
["","","(2, 2\")","",3790,7.9009762532981496,29944.7]
["","","(3, 2\")","",450,10.793333333333299,4857]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",365,4.25,1551.25]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",432,16.010000000000002,6916.32]
["","","(1,2\")","",1305,16,20880]
["","","(2, 2\")","",3140,22.5764331210191,70890]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",132,368.13348484848501,48593.62]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",82,577.92780487804896,47390.080000000002]
["7360000000-N","WOOD POLE","","",30,1082.93333333333,32488]
["7372000000-N","GUY ASSEMBLY","","",103,393.81087378640802,40562.519999999997]
["7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",14,395,5530]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",19,421.31578947368399,8005]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",16,525.43124999999998,8406.9]
["7432000000-E","2\" RISER WITH TUBING","","",10,605,6050]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",32572,5.9879267468991797,195038.75]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",55860,1.5129323308270699,84512.4]
["7481000000-N","SITE SURVEY","","",7,1290.5528571428599,9033.8700000000008]
["7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",11,663.15636363636395,7294.72]
["7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",34,3517.27529411765,119587.36]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",7,7120.2642857142901,49841.85]
["7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",4,1016.93,4067.72]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",360,2.75,990]
["","","(24)","",31020,2.47272727272727,76704]
["7528000000-E","DROP CABLE","","",700,2.57,1799]
["7540000000-N","SPLICE ENCLOSURE","","",11,1819.45454545455,20014]
["7552000000-N","INTERCONNECT CENTER","","",11,1648.6363636363601,18135]
["7566000000-N","DELINEATOR MARKER","","",20,175,3500]
["7575142060-N","MOD RADIO INSTALL","","",5,523.52800000000002,2617.64]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",26,9431.5884615384603,245221.3]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",18,15973.655555555601,287525.8]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,21200,42400]
["7613000000-N","SOIL TEST","","",46,895.76652173912998,41205.26]
["7614100000-E","DRILLED PIER FOUND","","",342,1007.88795321637,344697.68]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",20,183.46799999999999,3669.36]
["7636000000-N","SIGN FOR SIGNALS","","",45,477.222222222222,21475]
["7642200000-N","TYPE II PED W/ FOUNDATION","","",20,1636,32720]
["7684000000-N","SIGNAL CABINET FOUNDATION","","",15,1181.472,17722.080000000002]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",5,400,2000]
["7696000000-N","CONTLRS WITH CBNT (**************)","(2070E, BASE MOUNTED)","",2,12693.7,25387.4]
["","","(TYPE 2070E, BASE MOUNTED)","",10,13449,134490]
["7708000000-N","DETECTOR CARD (***********)","(2070)","",17,116.75,1984.75]
["","","(TYPE 2070)","",30,105,3150]
["7744000000-N","DETECTOR CARD (TYPE 170)","","",46,131.5,6049]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",3,13500,40500]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",21,131.80000000000001,2767.8]
["7901000000-N","CABINET BASE EXTENDER","","",15,411.03800000000001,6165.57]
["7901010000-N","CABINET BASE ADAPTER","","",1,400,400]
["7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,2635,2635]
["7960000000-N","METAL POLE FOUND REMVL","","",6,2052.3333333333298,12314]
["7972000000-N","METAL POLE REMOVAL","","",6,1243.3333333333301,7460]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","ETHERNET EDGE SWITCH","",11,3939.0909090909099,43330]
["","","FIRESTATION PREEMPTION PUSH- BUTTON","",1,6115,6115]
["","","JUNCTION BOX MARKER","",46,144.565217391304,6650]
["","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",1,11180,11180]
["","","","SYSTEM-MULTIPLE ZONES",2,10491.465,20982.93]
["","","PROTECTIVE COAT FOR DUAL MAST","ARM POLE (BLACK)",2,3910,7820]
["","","PROTECTIVE COAT FOR SIGNAL","PEDESTAL (BLACK)",8,68.400000000000006,547.20000000000005]
["","","PROTECTIVE COAT FOR SINGLE","MAST ARM POLE (BLACK)",14,3000,42000]
["8017000000-N","CM&R TEMP ACCESS ***********","(25+00.00-L-)","",1,233000,233000]
["","","(64+20.00 -L-)","",1,1300000,1300000]
["","","(99+17.60 -L1-)","",1,660000,660000]
["8035000000-N","REMV EXIST STR **********","(25+00.00-L-)","",1,300000,300000]
["","","(64+20.00 -L-)","",1,100000,100000]
["8056000000-N","REMV EXIST STR **********","(11+51.56 -DRW1-)","",1,10000,10000]
["","","(114+23.00 -L-)","",1,1000,1000]
["","","(167+03.45 -L-)","",1,1000,1000]
["","","(84+52.00 -L-)","",1,8000,8000]
["8065000000-N","ASBESTOS ASSESSMENT","","",3,2033.3333333333301,6100]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",108.5,680,73780]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",186,600,111600]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",144,2500,360000]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",116,1875,217500]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",125.55,432,54237.599999999999]
["8111600000-E","PERM STL CASING FOR 4' PIER","","",126,400,50400]
["8112730000-N","PDA TESTING","","",3,5066.6666666666697,15200]
["8113000000-N","SID INSPECTIONS","","",1,1050,1050]
["8115000000-N","CSL TESTING","","",5,2600,13000]
["8121000000-N","UNCL STR EXCAV STA *****","(64+20.00 -L-)","",1,17000,17000]
["","","(99+17.60 -L1-)","",1,55000,55000]
["8126000000-N","CULV EXCAV @ ************","(11+51.56 -DRW1-)","",1,15000,15000]
["","","(114+23.00 -L-)","",1,58000,58000]
["","","(120+01.00 -L-)","",1,25000,25000]
["","","(167+03.45 -L-)","",1,110000,110000]
["","","(84+52.00 -L-)","",1,28000,28000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",1096,51.6605839416058,56620]
["8147000000-E","REINF CONCRETE DECK SLAB","","",82783,33.269598830677801,2754157.2]
["8161000000-E","GROOVING BRIDGE FLOORS","","",70912,0.57488746615523001,40766.42]
["8182000000-E","CLASS A CONCRETE (BRIDGE)","","",950.3,997.10428285804505,947548.2]
["8196000000-E","CLASS A CONCRETE (CULV)","","",1652.9,693.79424042591802,1146772.5]
["8210000000-N","BRG APPR SLAB ***********","(25+00.00-L-)","",1,34000,34000]
["","","(64+20.00 -L-)","",1,125000,125000]
["","","(99+17.60 -L1-)","",1,45000,45000]
["8217000000-E","REINF STEEL (BRIDGE)","","",193555,0.98215261811887999,190100.55]
["8238000000-E","SPIRAL COL REINF STL BRG","","",22382,1.67294611741578,37443.879999999997]
["8245000000-E","REINF STEEL (CULVERT)","","",238193,1.23947555133862,295234.40000000002]
["8265000000-E","54\" PRESTR CONCRETE GIRDR","","",2423.5,250,605875]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",2414.1,295,712159.5]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",4097.5,285,1167787.5]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",12,1500,18000]
["","","(HP 14 X 73)","",16,750,12000]
["","","(HP12 X 53)","",40,750,30000]
["8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(PP 24 X 0.625)","",12,3200,38400]
["","","(PP 3 6X 0.50)","",15,6100,91500]
["8364000000-E","HP12X53 PILES","","",1890,48.904761904761898,92430]
["8384000000-E","HP14X73 PILES","","",400,61,24400]
["8385200000-E","PP**X**** GALV STL PILE","(PP 24 X 0.625)","",1020,210.37,214577.4]
["","","(PP 36 X 0.50)","",1800,229,412200]
["8391000000-N","STEEL PILE POINTS","","",16,140,2240]
["8393000000-N","PILE REDRIVES","","",39,115,4485]
["8475000000-E","TWO BAR METAL RAIL","","",1574.37,110,173180.7]
["8503000000-E","CONCRETE BARRIER RAIL","","",1216.3599999999999,102,124068.72]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",1176.57,105.635788775848,124287.9]
["","","(1'-2\" X 2'-8\")","",423.33,111,46989.63]
["","","(1'-2\" X 3\"-3\")","",427.9,122,52203.8]
["8608000000-E","RIP RAP II (2'-0\")","","",2510,41.056175298804803,103051]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2792,3,8376]
["8657000000-N","ELASTOMERIC BEARINGS","","",3,30666.666666666701,92000]
["8706000000-N","EXPANSION JOINT SEALS","","",2,69000,138000]
["8821000000-E","GENERIC CULVERT ITEM (SF)","TEMPORARY SHORING FOR RISER","CONSTRUCTION",10600,0.01,106]
["8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL SURFACE","TREATMENT",54652,1.95,106571.4]
["","","SOUND BARRIER WALL NW2","",6822,38,259236]
["","","SOUND BARRIER WALL NW2A","",12147,38,461586]
["","","SOUND BARRIER WALL NW3","",14955,38,568290]

{"sheet":"ITEMS - DIV 05","index":7,"n_rows":682,"n_cols":7,"rows_kept":682,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 05"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",26,259187.47615384599,6738874.3799999999]
["0000400000-N","CONST SURVEYING","","",9,102311.11111111099,920800]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN & CONSTRUCTION","",1,360175000,360175000]
["","","DESIGN AND CONSTRUCTION","",1,403200000,403200000]
["","","DESIGN AND CONSTRUCTION U-2719","",1,311688512,311688512]
["","","DESIGN AND CONSTRUCTION U-4437","",1,34511488,34511488]
["0001000000-E","CLEARING & GRUBBING","","",40,163801.72500000001,6552069]
["0008000000-E","SUPP CLEARING & GRUBBING","","",8,5350,42800]
["0015000000-N","SEALING ABANDONED WELLS","","",9,2500,22500]
["0022000000-E","UNCLAS EXCAVATION","","",420940,7.1060008552287703,2991200]
["0028000000-N","TYPE I STANDARD APPR **********","(50+61.09 -L-)","",1,97000,97000]
["0030000000-N","TYPE II MOD APPR **********","(13+25 -L-)","",1,10000,10000]
["","","(14+67.00)","",1,12000,12000]
["","","(15+14.00)","",1,14468,14468]
["","","(15+98.00)","",1,12500,12500]
["","","(18+64.00 -L-)","",1,10000,10000]
["","","(38+62.00)","",1,8580,8580]
["0036000000-E","UNDERCUT EXCAVATION","","",23180,11.4408973252804,265200]
["0043000000-N","GRADING","","",6,116450,698700]
["0050000000-E","SUPP CLEARING & GRUBBING","","",7,140.04857142857099,980.34]
["0057000000-E","UNDERCUT EXCAVATION","","",1850,14.597297297297301,27005]
["0063000000-N","GRADING","","",1,261000,261000]
["0106000000-E","BORROW EXCAVATION","","",321205,6.4229340452359098,2063078.53]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",13872,7.4286332179930801,103050]
["0141000000-E","BERM DITCH CONST","","",4000,3.9049999999999998,15620]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",74710,7.2448266630973102,541261]
["0177000000-E","BREAKING OF EXT ASPH PVMT","","",4410,4,17640]
["0192000000-N","PROOF ROLLING","","",76,183.68421052631601,13960]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",300,11,3300]
["0195000000-E","SELECT GRANULAR MAT'L","","",25590,19.973739742086799,511128]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",67980,1.53139158576052,104104]
["0199000000-E","TEMP SHORING","","",10351,49.450750652110898,511864.72]
["0220000000-E","ROCK EMBANKMENTS","","",12990,38.7990762124711,504000]
["0222000000-E","GEOTEXTILE ROCK EMBANK","","",6570,2.6578386605783901,17462]
["0223000000-E","ROCK PLATING","","",1550,31.2,48360]
["0248000000-N","GENERIC GRADING ITEM (LS)","MEDIA FILTER BASIN NO 1","",1,39000,39000]
["","","MEDIA FILTER BASIN NO 2","",1,65000,65000]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",1000,75,75000]
["","","REPAIR EXISTING AGGREGATE BASECOURSE","",15,108.19,1622.85]
["0264000000-E","GENERIC GRADING ITEM (SMI)","SHOULDER GRADING","",513.5,2119.9533787731302,1088596.06]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",5335,31.6687160262418,168952.6]
["0320000000-E","FND CONDIT GEOTEXTILE","","",16680,2.0845083932853701,34769.599999999999]
["0335200000-E","15\" DRAINAGE PIPE","","",356,36.3862921348315,12953.52]
["0335300000-E","18\" DRAINAGE PIPE","","",224,43.6928571428571,9787.2000000000007]
["0335400000-E","24\" DRAINAGE PIPE","","",248,53.870967741935502,13360]
["0335500000-E","30\" DRAINAGE PIPE","","",220,56.3,12386]
["0335600000-E","36\" DRAINAGE PIPE","","",232,73,16936]
["0335700000-E","42\" DRAINAGE PIPE","","",76,90.8,6900.8]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",6,616.66666666666697,3700]
["","","(18\")","",4,575,2300]
["0342000000-E","**\" SIDE DRAIN PIPE","(12\")","",16,52.04,832.64]
["","","(30\")","",84,82,6888]
["","","(42\")","",180,107,19260]
["","","(48\")","",16,130,2080]
["0343000000-E","15\" SIDE DRAIN PIPE","","",5336,47.409295352323802,252976]
["0344000000-E","18\" SIDE DRAIN PIPE","","",1232,50.454545454545503,62160]
["0345000000-E","24\" SIDE DRAIN PIPE","","",1328,62.680722891566298,83240]
["0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",6,500,3000]
["","","(18\")","",2,525,1050]
["0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",12068,44.170367915147501,533048]
["","","(18\", V)","",2272,54.264084507042199,123288]
["","","(24\", V)","",1648,75,123600]
["","","(30\", V)","",964,102.402489626556,98716]
["","","(42\", V)","",52,149,7748]
["0366000000-E","15\" RC PIPE CULV III","","",1372,44.129329446064098,60545.440000000002]
["0372000000-E","18\" RC PIPE CULV III","","",1784,51.080089686098702,91126.88]
["0378000000-E","24\" RC PIPE CULV III","","",1692,85.769385342789604,145121.79999999999]
["0384000000-E","30\" RC PIPE CULV III","","",2608,66.757055214723906,174102.39999999999]
["0390000000-E","36\" RC PIPE CULV III","","",1456,85.554945054945094,124568]
["0396000000-E","42\" RC PIPE CULV III","","",52,123,6396]
["0408000000-E","54\" RC PIPE CULV III","","",176,218,38368]
["0420000000-E","66\" RC PIPE CULV III","","",264,310,81840]
["0448000000-E","***\" RCP CULV CLASS IV","(48\")","",84,400,33600]
["0448200000-E","15\" RCP CULV CLASS IV","","",7644,41.492412349555202,317168]
["0448300000-E","18\" RCP CULV CLASS IV","","",3472,42.347926267281103,147032]
["0448400000-E","24\" RCP CULV CLASS IV","","",2228,67.516337522441603,150426.4]
["0448500000-E","30\" RCP CULV CLASS IV","","",584,98.109589041095902,57296]
["0448600000-E","36\" RCP CULV CLASS IV","","",152,132,20064]
["0570000000-E","6\" CS PIPE 0.064\" SPR BOX","","",24,50,1200]
["0576000000-E","**\" CS PIPE CULV *****\"","(36\", 0.079\")","",48,78,3744]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",936,57.414529914529901,53740]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",144,72,10368]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",132,71.636363636363598,9456]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",27,387.03703703703701,10450]
["","","(18\", 0.064\")","",2,380,760]
["","","(24\", 0.064\")","",4,560,2240]
["0995000000-E","PIPE REMOVAL","","",8670,17.106767012687399,148315.67000000001]
["0996000000-N","PIPE CLEAN OUT","","",4,1800,7200]
["1011000000-N","FINE GRADING","","",3,705000,2115000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",114900,2.5057441253263701,287910]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",920,211,194120]
["1077000000-E","57 STONE","","",3650,28.131506849315102,102680]
["1099500000-E","SHALLOW UNDERCUT","","",5400,19.1666666666667,103500]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",10700,22.682242990654199,242700]
["1110000000-E","STABILIZER AGGREGATE","","",1000,22.5,22500]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",14850,2.4525252525252501,36420]
["1121000000-E","AGGREGATE BASE COURSE","","",157229,20.780507031145699,3267298.34]
["1146000000-E","CONDITIONING EXISTING BASE","","",1,5188.16,5188.16]
["1165000000-E","PORT CEM FOR CEM TRTD BASE CRSE","","",1293,185,239205]
["1176000000-E","SOIL CEMENT BASE","","",160640,3.05205428286853,490282]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",5067,187.44819419775001,949800]
["1209000000-E","ASPHALT CURING SEAL","","",41340,2.6670053217223,110254]
["1220000000-E","INCIDENTAL STONE BASE","","",17947,41.310383908174103,741397.46]
["1231000000-E","SHOULDER BORROW","","",290,27,7830]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",24143,18.272247028124099,441146.86]
["1275000000-E","PRIME COAT","","",584,7.5178424657534197,4390.42]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",102729,1.5919218526414201,163536.54]
["","","(1\")","",175842,1.51,265521.42]
["","","(1-1/2\")","",2747628,1.6001738845287601,4396682.57]
["","","(2\")","",45584,2.2999999999999998,104843.2]
["","","(2-1/2\")","",23731,2.3618275673170102,56048.53]
["","","(3\")","",39831,2.5490211142075299,101530.06]
["","","(4\")","",15335,3.6871548744701701,56542.52]
["","","(4-1/2\")","",2508,3.3,8276.4]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1\")","",1242,8.51,10569.42]
["","","(0\" TO 1-1/2\")","",45761,3.4070306592950299,155909.13]
["","","(0\" TO 1/2\")","",369,11.5,4243.5]
["","","(0\" TO 2\")","",220,20,4400]
["","","(0\" TO 3\")","",3000,10.3828333333333,31148.5]
["","","(0\" TO 4\")","",6450,5.0599999999999996,32637]
["","","(0\" TO 5-1/2\")","",611,15.04,9189.44]
["","","(0\" TO 6\")","",6300,11,69300]
["1330000000-E","INCIDENTAL MILLING","","",223355,6.5928783326990699,1472552.34]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",1030,72.864077669902898,75050]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",52709,50.5223407767174,2662982.06]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",2287,50.561434193266301,115634]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",109042,42.399774765686601,4623356.24]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",384055,36.541381234458598,14033900.17]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",250370,38.757714662299797,9703769.0199999996]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",5110,61,311710]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",9135,39.671477832512302,362398.95]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",3045,70.417454844006599,214421.15]
["1575000000-E","ASP FOR PLANT MIX","","",47707,479.36351059592897,22868995]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",295,600,177000]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",3780,107.656878306878,406943]
["1704000000-E","PATCHING EXIST PVMT","","",67445,104.77709956260701,7066691.4800000004]
["1803500000-E","AST, DOUBLE SEAL","","",680338,0.93002357651638001,632730.38]
["1820000000-E","AST, FOG SEAL","","",322389,0.25,80597.25]
["1838000000-E","EMULSION FOR AST","","",412872,2.3020116161909701,950436.14]
["1840000000-E","MILLED RUMBLE STRIPS","","",36364,0.44231107688922999,16084.2]
["1891000000-E","GENERIC PAVING ITEM (SY)","LATEX MODIFIED MICROSURFACING,TYPE III","",324317,2.59,839981.03]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",318,262.36679245283,83432.639999999999]
["2020000000-N","CONTROL-OF-ACCESS MARKERS","","",20,300,6000]
["2022000000-E","SUBDRAIN EXCAVATION","","",1336,23.369760479041901,31222]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",1456,2.78,4047.68]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",668,45.540419161676702,30421]
["2044000000-E","6\" PERF SUBDRN PIPE","","",5050,12.1881188118812,61550]
["2070000000-N","SUBDRN PIPE OUTLET","","",10,355,3550]
["2077000000-E","6\" OUTLET PIPE","","",150,41.25,6187.5]
["2099000000-E","SHOULDER DRAIN","","",26890,8.9,239321]
["2110000000-E","4\" SHOULDER DRAIN PIPE","","",26890,2,53780]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",1980,10,19800]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",100,300,30000]
["2143000000-E","BLOTTING SAND","","",35,156.57142857142901,5480]
["2209000000-E","ENDWALLS","","",26.3,1296.9429657794699,34109.599999999999]
["2220000000-E","REINF ENDWALLS","","",11.4,1650,18810]
["2253000000-E","PIPE COLLARS","","",3,2580,7740]
["2275000000-E","FLOWABLE FILL","","",82,434.14634146341501,35600]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",521,2139.0642994241798,1114452.5]
["2297000000-E","MASNRY DRAINAGE STRUCT","","",9.9,4883.5303030303003,48346.95]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",327.39999999999998,333.66731826511898,109242.68]
["2352000000-N","FRAME W/GRATE 840.***** STD","(840.D13)","",2,650,1300]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",61,652.04918032786895,39775]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",42,650,27300]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",87,643.44827586206895,55980]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",12,593.94333333333304,7127.32]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",13,648.461538461538,8430]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",20,669.65,13393]
["","","(F)","",102,677.21166666666704,69075.59]
["","","(G)","",148,669.53581081081097,99091.3]
["2396000000-N","FRAME W/COVER STD 840.54","","",29,488.45862068965499,14165.3]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",1,1500,1500]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",31,426.61290322580601,13225]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",85,803.76470588235304,68320]
["2473000000-N","GENERIC DRAINAGE ITEM (EA)","GDI FRAME W/ 2 ADA GRATES","",5,1950,9750]
["2538000000-E","**'-**\" CONC CURB & GUTTER","(2'-9\")","",4080,26,106080]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",34110,14.851949574904699,506600]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",54230,18.944311266826499,1027350]
["2556000000-E","SHOULDER BERM GUTTER","","",2120,24.207547169811299,51320]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",1470,40.816326530612201,60000]
["2591000000-E","4\" CONC SIDEWALK","","",19420,29.310762100926901,569215]
["2605000000-N","CONC CURB RAMPS","","",61,2060.24590163934,125675]
["2612000000-E","6\" CONC DRIVEWAY","","",1650,69.915151515151507,115360]
["2619000000-E","4\" CONC PAVED DITCH","","",99,124.777777777778,12353]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",1740,60,104400]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",9595,67.251016154246997,645273.5]
["2738000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE GREENWAY PATH","",160,48,7680]
["2752000000-E","GENERIC PAVING ITEM (LF)","MEDIAN HAZARD PROTECTION","",114,31,3534]
["","","REMOVE AND REPLACE 2'-6\" C & G","",10,75,750]
["","","REMOVE AND REPLACE 2'-6\" CURB & GUTTER","",40,100,4000]
["2800000000-N","ADJ CATCH BASINS","","",1,550,550]
["2815000000-N","ADJ DROP INLETS","","",26,1128.8461538461499,29350]
["2830000000-N","ADJ MANHOLES","","",293,534.04436860068301,156475]
["2845000000-N","ADJ METER OR VALVE BOXES","","",428,525.52570093457905,224925]
["2893000000-N","CONVERT CB TO JB W/MH","","",1,1280,1280]
["3030000000-E","STL BEAM GUARDRAIL","","",16175,16.817650695517798,272025.5]
["3045000000-E","SBGR SHOP CURVED","","",562.5,20.798222222222201,11699]
["3060000000-E","SBGR DOUBLE FACED","","",87.5,29,2537.5]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",64,23.900625000000002,1529.64]
["3180000000-N","GR ANCHOR TYPE **********","(III SHOP CURVED)","",4,1800,7200]
["3195000000-N","GR END TYPE AT-1","","",5,630,3150]
["3210000000-N","GR END TYPE CAT-1","","",30,675.82666666666705,20274.8]
["3215000000-N","GR ANCHOR TYPE III","","",22,1772.72727272727,39000]
["3287000000-N","GR END TYPE TL-3","","",46,3078.2608695652202,141600]
["3288000000-N","GR END TYPE TL-2","","",7,3114.2857142857101,21800]
["3317000000-N","GR ANCHOR TYPE B-77","","",4,1650,6600]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",7371,0.45203364536697999,3331.94]
["3380000000-E","TEMP STL BM GUARDRAIL","","",1900,11.6315789473684,22100]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(III)","",4,1200,4800]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",4,2600,10400]
["","","(TL-3)","",6,2800,16800]
["3435000000-N","GENERIC GUARDRAIL ITEM (EA)","BOLLARDS (PERMANENT)","",10,1280.06,12800.6]
["","","BOLLARDS (REMOVABLE)","",3,2403.37,7210.11]
["","","EXTRA LENGTH GUARDRAIL POSTS (8' STEEL)","",70,61,4270]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",74050,3.5323295070898002,261569]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",4174,19.365596550071899,80832]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",2058,26.882653061224499,55324.5]
["3572000000-E","CHAIN LINK FENCE RESET","","",305,20.29,6188.45]
["3578000000-N","GENERIC FENCING ITEM (EA)","30' STEEL PIPE GATE","",1,7845.5,7845.5]
["3628000000-E","RIP RAP, CLASS I","","",3971,51.056408964996201,202745]
["3635000000-E","RIP RAP, CLASS II","","",2551,58.357506860054897,148870]
["3642000000-E","RIP RAP, CLASS A","","",1810,47.961325966850801,86810]
["3649000000-E","RIP RAP, CLASS B","","",5462,50.733170999633799,277104.58]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",29897,2.1392447402749402,63957]
["3659000000-N","PREFORMED SCOUR HOLES","","",5,1424,7120]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",377,24.984084880636601,9419]
["","","(F)","",25,35,875]
["4048000000-E","REINF CONC FOUNDTN","","",11,850,9350]
["4054000000-E","PLN CONC FOUNDTN","","",1,480,480]
["4057000000-E","OVERHEAD FOOTING","","",107,910,97370]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",10217,3.8,38824.6]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",1614,2.4,3873.6]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",6789,6.4954485196641603,44097.599999999999]
["4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",1,88,88]
["4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(111+35 -Y-)","",1,41000,41000]
["","","(123+03 -Y-)","",1,43000,43000]
["","","(149+00 -Y-)","",1,29000,29000]
["","","(171+68 -Y-)","",1,33000,33000]
["","","(25+85 -RPC-)","",1,39000,39000]
["","","(59+00 -L-)","",1,30000,30000]
["","","(60+42 -Y-)","",1,24000,24000]
["","","(84+00 -Y-)","",1,24000,24000]
["4096000000-N","SIGN ERECTION, TYPE D","","",18,136.944444444444,2465]
["4102000000-N","SIGN ERECTION, TYPE E","","",326,87.849693251533694,28639]
["4108000000-N","SIGN ERECTION, TYPE F","","",60,145,8700]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",12,354,4248]
["","","(B)","",3,127,381]
["","","(E)","",2,60,120]
["4114000000-N","SIGN ERECTION, MILEMARKERS","","",1,56,56]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",6,660,3960]
["","","(E)","",19,215.789473684211,4100]
["4138000000-N","DISPOSE SUPPORT, STL BM","","",6,860,5160]
["4149000000-N","DISPOSE SIGN SYST OVRHD","","",4,3840,15360]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",5,884,4420]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",172,6.22540697674419,1070.77]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",21,6.4285714285714297,135]
["4238000000-N","DISPOSE SIGN, D, E, F","","",2,20,40]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",6002,9.6959480173275594,58195.08]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",2526,12.349833729216201,31195.68]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",1901,9.8987112046291408,18817.45]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",53905,7.3051280957239602,393782.93]
["4415000000-N","FLASHING ARROW BOARD","","",17,2494.1176470588198,42400]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",19,8842.1052631579005,168000]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",354,63.548022598870098,22496]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",6,5500,33000]
["4430000000-N","DRUMS","","",1710,35.262865497076,60299.5]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",126,118.650793650794,14950]
["4435000000-N","CONES","","",65,40.769230769230802,2650]
["4445000000-E","BARRICADES (TYPE III)","","",1636,25.4481907090465,41633.24]
["4450000000-N","FLAGGER","","",40,100,4000]
["4455000000-N","FLAGGER","","",900,339.60711111111101,305646.40000000002]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",16,117958.685625,1887338.97]
["4465000000-N","TEMP CRASH CUSHIONS","","",18,5821.9688888888904,104795.44]
["4470000000-N","REM & RES CRASH CUSHION","","",10,3023.97,30239.7]
["4480000000-N","TMA","","",10,6520,65200]
["4485000000-E","PORT CONC BARRIER","","",3366,24.045668449197901,80937.72]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",6910,31,214210]
["4500000000-E","REM & RES PORT CONC BARRIER","","",2770,9.6763537906137191,26803.5]
["4505000000-E","REM & RES PORT CONC BARR, ANCH","","",4570,10,45700]
["4507000000-E","WATER FILLED BARRIER","","",777,57,44289]
["4510000000-N","LAW ENFORCEMENT","","",7240,45.508066298342499,329478.40000000002]
["4516000000-N","SKINNY DRUM","","",200,40,8000]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",30,75,2250]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","ADA BARRICADE (SAFETY RAIL)","",13,499.05153846153797,6487.67]
["4650000000-N","TEMP RAISED PVMT MRKS","","",5315,6.1068673565380998,32458]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",3350569,0.53378690902948001,1788489.87]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",3414037,0.64473337576598999,2201143.6]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",200,8,1600]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",82595,0.91943943337973999,75941.100000000006]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",19981,0.98778839897903004,19737]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",67537,1.9107311547744199,129045.05]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",74525,2.4308262998993602,181157.33]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",26646,3.1167225850033802,83048.19]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",1576,1.9887309644670099,3134.24]
["4705000000-E","THERMO LINES 16\" 120MILS","","",2050,9.2439024390243905,18950]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",39402,10.7346984924623,422968.59]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",1014,104.499013806706,105962]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",4213,118.95549489674799,501159.5]
["4726100000-E","HIP THERMO PVT MKG CHAR 120 MILS","","",12,205,2460]
["4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",30,272,8160]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",33047,2.9973325869216598,99052.85]
["","","(III)","",1980,3.25,6435]
["","","(IV)","",3053,1.67,5098.51]
["4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",180,6.0330555555555598,1085.95]
["","","(III)","",2100,6.5,13650]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",103,6.25,643.75]
["4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",600,15,9000]
["4800000000-N","COLD APP PLAS CHAR TYPE *","(III)","",9,180,1620]
["4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",16,258.75,4140]
["","","(III)","",19,350,6650]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",2977621,0.14977308730694999,445967.49]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",41806,0.62766205807778996,26240.04]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",7795,0.78128287363695004,6090.1]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",1400,2,2800]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",39349,2.7247820783247398,107217.45]
["4840000000-N","PAINT PVT MKG CHARACTER","","",973,29.614594039054499,28815]
["4845000000-N","PAINT PVT MKG SYMBOL","","",3592,27.854955456570199,100055]
["4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",42145,0.71,29922.95]
["4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",3040,1.42,4316.8]
["4848000000-E","WZ TRAF PATTERN MASKING","","",737000,0.32,235840]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",659458,0.22646479381553,149344.01999999999]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",288,2.3656250000000001,681.3]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",1173,3.9677749360613799,4654.2]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",145,41.379310344827601,6000]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","HOT SPRAY THERMOPLASTIC PAVEM-","ENT MARKING LINES, 4\", 40 MIL",233495,0.38,88728.1]
["","","","ENT MARKING LINES, 4\", 40 MIL",838035,0.34,284931.90000000002]
["4900000000-N","PERM RAISED PVMT MARKERS","","",543,7.9792081031307598,4332.71]
["4905000000-N","SNOWPLB PVMT MRKER","","",18866,26.490114491678099,499762.5]
["4935000000-N","FLEX DELINATR (CRYSTAL)","","",77,50,3850]
["4940000000-N","FLEX DELINATR (YELLOW)","","",73,50,3650]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",10,50,500]
["5000000000-E","***' HIGH MOUNT STANDARD","(70')","",3,23000,69000]
["5010000000-E","100' HIGH MOUNT STANDARD","","",2,25000,50000]
["5020000000-N","PORTABLE DRIVE UNIT","","",1,5000,5000]
["5025000000-E","HIGH MOUNT FOUNDS","","",27.8,1360,37808]
["5045000000-N","LIT STD MTLS ************","(30' SA, 10' ARM)","",20,2300,46000]
["5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",23,2500,57500]
["5070000000-N","STD FOUNDAT ***********","(R1)","",49,1038.8828571428601,50905.26]
["","","(R2)","",5,1050,5250]
["5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",1,1925,1925]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",140,33.814285714285703,4734]
["5130000000-N","LITE CONTROL ************","(120/240V)","",1,18573.91,18573.91]
["5155000000-E","ELECT DUCT BD, SIZE *****","(1\")","",265,7.47,1979.55]
["","","(1.5\")","",425,8.01,3404.25]
["","","(2\")","",465,5.7609677419354801,2678.85]
["","","(3\")","",190,12.24,2325.6]
["","","(3/4\")","",285,7.47,2128.9499999999998]
["5160000000-E","ELECT DUCT JA, SIZE *****","(3\")","",1128,17,19176]
["","","(4\")","",345,21,7245]
["5165000000-E","** 10 W/G FEEDER CIRCUIT","(2)","",130,4.4000000000000004,572]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",520,3.05,1586]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2)","",700,4.05,2835]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(2)","",170,5.6,952]
["5200000000-E","**-10 W/G FEEDR N *****\"","(2, 1.5\")","",1020,13.59,13861.8]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",7480,7.5,56100]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",5910,8.5,50235]
["5220000000-E","**-2 W/G FEEDER N *****\"","(2, 1.5)","",3020,10,30200]
["5240000000-N","ELEC JB ************","(IG11)","",1,382.69,382.69]
["","","(IG18)","",6,471.3,2827.8]
["","","ELECTRICAL JUNCTION BOXES PC18","",57,255,14535]
["","","ELECTRICAL JUNCTION BOXES PC30","",7,420,2940]
["","","ELECTRICAL JUNCTION BOXES PC36","",1,1015,1015]
["5253000000-N","UNDERPASS CIRCUITRY *************","(STATION 15+58)","",1,6233.14,6233.14]
["5255000000-N","PORTABLE LIGHTING","","",3,30562.8966666667,91688.69]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","PRIMARY ELECTRICAL SERVICE","",1,11567.96,11567.96]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","COMMUNICATION GATEWAY","",1,4150,4150]
["","","CONTROL NODE","",73,190,13870]
["","","HIGH MOUNT LUMINAIRE - LED","",30,1550,46500]
["","","LIGHTING CONTROL SYSTEM","",1,10150,10150]
["","","PEDESTRIAN LIGHT STANDARD - 100W LED","",6,3725.94,22355.64]
["","","PEDESTRIAN LIGHT STANDARD - 60W LED","",5,3509.17,17545.849999999999]
["","","ROADWAY LIGHT STANDARD LUMINAIRE -","285W LED",43,740,31820]
["","","UNDERPASS LUMINAIRE - LED","",12,920.76,11049.12]
["5325400000-E","4\" WATER LINE","","",623,76.5,47659.5]
["5325800000-E","8\" WATER LINE","","",1032,85.515988372093005,88252.5]
["5326200000-E","12\" WATER LINE","","",1665,108.172972972973,180108]
["5326600000-E","16\" WATER LINE","","",80,175,14000]
["5329000000-E","DI H2O PIPE FITTINGS","","",8860,5.7883747178329603,51285]
["5538000000-E","4\" VALVE","","",2,1600,3200]
["5558000000-E","12\" VALVE","","",1,3500,3500]
["5571800000-E","8\" TAPPING SLEEVE & VALVE","","",2,10800,21600]
["5572000000-E","10\" TAPPING SLEEVE & VALVE","","",2,13000,26000]
["5572200000-E","12\" TAPPING SLEEVE & VALVE","","",2,15000,30000]
["5606400000-E","4\" BLOW OFF","","",1,5100,5100]
["5606800000-E","8\" BLOW OFF","","",1,8500,8500]
["5643200000-E","2\" WATER METER","","",1,13250,13250]
["5648000000-N","RELOCATE WATER METER","","",4,1695,6780]
["5672000000-N","RELOCATE FIRE HYDRANT","","",5,3300,16500]
["5685800000-E","30\" LINE STOP W/ BYPASS","","",1,265000,265000]
["5709000000-E","**\" FORCE MAIN SEWER","(30\")","",585,300,175500]
["5769000000-E","DI SEWER PIPE FITTINGS","","",8380,4,33520]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",1249,11.724579663730999,14644]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",1178,25.7478777589134,30331]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",65,78,5070]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",578,40,23120]
["5835000000-E","**\" ENCASEMENT PIPE","(42\")","",260,295,76700]
["5835800000-E","18\" ENCASEMENT PIPE","","",149,150,22350]
["5836000000-E","24\" ENCASEMENT PIPE","","",110,135,14850]
["5836200000-E","30\" ENCASEMENT PIPE","","",138,220,30360]
["5872500000-E","BORE & JACK **\"","(18\")","",149,160,23840]
["","","(24\")","",110,720,79200]
["","","(30\")","",138,940,129720]
["","","(42\")","",260,1265,328900]
["5872600000-E","DIRECT DRILL **\"","(8\")","",315,390,122850]
["5882000000-N","GENERIC UTILITY ITEM (EA)","12\" GATE VALVE ASSEMBLY","",19,4990,94810]
["","","12\" INSERTION VALVE ASSEMBLY","",2,18000,36000]
["","","12\" x 16\" TAPPING SLEEVE AND","VALVE ASSEMBLY",1,22820,22820]
["","","16 INCH INSERTION VALVE","",1,45500,45500]
["","","16 INCH LINE STOP","",1,27100,27100]
["","","30\" PLUG VALVE ASSEMBLY","",1,82000,82000]
["","","6\" GATE VALVE ASSEMBLY","",3,1200,3600]
["","","8\" GATE VALVE ASSEMBLY","",7,1700,11900]
["","","ARV MANHOLE ASSEMBLY (POTABLE WATER)","",1,7100,7100]
["","","BLOW OFF ASSEMBLY","",11,1750,19250]
["","","BYPASS CONNECTION ASSEMBLY","ABANDONMENT",2,5000,10000]
["","","COMBINATION AIR VALVE ASSEMBLY","(SANITARY)",1,8650,8650]
["","","CONNECTION TO EXISTING 16-INCH","WATER MAIN",2,6100,12200]
["","","CONNECTION TO EXISTING 6-INCH","FORCE MAIN",2,5800,11600]
["","","CONNECTION TO EXISTING WATER- LINE","",3,3090,9270]
["","","CUT AND CAP EXISTING WATER LINE","",1,3090,3090]
["","","FIRE HYDRANT ASSEMBLY","",9,5530,49770]
["","","REUSE TEMPORARY INTERCONNECT","",1,23650,23650]
["","","THRUST COLLAR","",6,2000,12000]
["5888000000-E","GENERIC UTILITY ITEM (LF)","12\" DIA C900 RJ PVC REUSE WATER MAIN","",7488,61.2,458265.59999999998]
["","","12\" DIA DUCTILE IRON,","CLASS 350 WATER MAIN",8218,55.6,456920.8]
["","","12\" RESTRAINED JOINT ADDER FOR","DI WATER MAIN",1401,20.2,28300.2]
["","","16 INCH CLASS 350 DUCTILE IRON","WATER DISTRIBUTION PIPE",600,115,69000]
["","","16\" DIA STEEL CASING","",135,129,17415]
["","","16-INCH CLASS 350 DUCTILE IRON","CARRIER PIPE",45,210,9450]
["","","16-INCH ENCASEMENT PIPE, BY OPEN CUT","",45,305,13725]
["","","16-INCH RESTRAINED JOINT ADDER","FOR DUCTILE IRON WATER PIPE",410,51,20910]
["","","30-INCH ENCASEMENT PIPE, BY OPEN CUT","",45,360,16200]
["","","6\" DIA C900 RJ PVC REUSE WATER MAIN","",103,31.4,3234.2]
["","","6\" DIA DUCTILE IRON, CLASS 350WATER MAIN","",44,43.3,1905.2]
["","","6\" RESTRAINED JOINT ADDER FOR","DI WATER MAIN",44,11,484]
["","","6-INCH C-900 DR 18 PVC CARRIERPIPE","",45,122,5490]
["","","6-INCH C-900 DR 18 PVC RE-","TRAINED JOINT FORCE MAIN",800,60,48000]
["","","8\" DIA C900 RJ PVC REUSE WATER MAIN","",637,39,24843]
["","","8\" DIA DUCTILE IRON, CLASS 350WATER MAIN","",155,41,6355]
["","","8\" RESTRAINED JOINT ADDER FOR","DI WATER MAIN",155,12.9,1999.5]
["","","ABANDON EXISTING 16-INCH WATER","DISTRIBUTION PIPE",565,55,31075]
["5906000000-E","GENERIC UTILITY ITEM (LB)","DUCTILE IRON FITTINGS","",18580,10.335522066738401,192034]
["5912000000-N","GENERIC UTILITY ITEM (LS)","REMOVAL OF TEMPORARY BYPASS PIPING","",1,6500,6500]
["","","REMOVE METER VAULT","",1,4250,4250]
["6000000000-E","TEMP SILT FENCE","","",174814,1.8704721017767501,326984.71000000002]
["6006000000-E","EROS CONTRL STONE CL A","","",4960,39.198588709677402,194425]
["6009000000-E","EROS CONTRL STONE CL B","","",24085,14.0973884160266,339535.6]
["6012000000-E","SEDIMENT CONTROL STONE","","",27295,10.2282304451365,279179.55]
["6015000000-E","TEMP MULCHING","","",128.80000000000001,927.21281055900602,119425.01]
["6018000000-E","SEED FOR TEMP SEEDING","","",7400,2.6793243243243201,19827]
["6021000000-E","FERT FOR TEMP SEEDING","","",43,903.00488372093002,38829.21]
["6024000000-E","TEMP SLOPE DRAINS","","",8216,15.2680185004868,125442.04]
["6029000000-E","SAFETY FENCE","","",12200,2.2823770491803299,27845]
["6030000000-E","SILT EXCAVATION","","",66720,1.8015062949640299,120196.5]
["6036000000-E","MATTING FOR EROS CONTROL","","",341640,1.12784510010537,385317]
["6037000000-E","COIR FIBER MAT","","",2170,5.9177419354838703,12841.5]
["6038000000-E","PERM SOIL REINF MAT","","",5235,5.0167144221585502,26262.5]
["6042000000-E","1/4\" HARDWARE CLOTH","","",27355,3.9327472125753999,107580.3]
["6045000000-E","**\" TEMP PIPE","(18\")","",765,38,29070]
["","","(24\")","",1235,42,51870]
["","","(36\")","",380,57.5131578947368,21855]
["","","(42\")","",484,70,33880]
["","","(48\")","",124,75,9300]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",500,46,23000]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",1335,21.610486891385801,28850]
["6069000000-E","STILLING BASINS","","",2400,11,26400]
["6070000000-N","SPECIAL STILLING BASINS","","",54,470.444444444444,25404]
["6071010000-E","WATTLE","","",47303,3.87334735640446,183220.95]
["6071012000-E","COIR FIBER WATTLE","","",4470,9.4697986577181208,42330]
["6071013000-E","WATTLE BARRIER","","",900,8,7200]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",5585,5.2623634735899696,29390.3]
["6071030000-E","COIR FIBER BAFFLE","","",15245,5.1472154804854098,78469.3]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",75,1599.6,119970]
["","","(2\")","",10,1345,13450]
["","","(3\")","",3,1800,5400]
["","","(4\")","",2,2300,4600]
["6084000000-E","SEEDING AND MULCHING","","",360.15,1667.6255449118401,600595.34]
["6087000000-E","MOWING","","",78.650000000000006,150.08645899555,11804.3]
["6090000000-E","SEED FOR REPAIR SEEDING","","",1500,5.0616666666666701,7592.5]
["6093000000-E","FERT FOR REPAIR SEEDING","","",5.75,1172.3704347826099,6741.13]
["6096000000-E","SEED FOR SUPP SEEDING","","",3125,4.5124000000000004,14101.25]
["6108000000-E","FERTILIZER TOPDRESSING","","",89.25,877.50274509803899,78317.119999999995]
["6111000000-E","IMPERVIOUS DIKE","","",1766,43.725934314835797,77220]
["6114500000-N","SPECIALIZED HAND MOWING","","",115,80.852173913043501,9298]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",387,81.548062015503902,31559.1]
["6117500000-N","CONC WASHOUT STR","","",35,896.19971428571398,31366.99]
["6120000000-E","CULVERT DIVERSION CHANNEL","","",867,30,26010]
["6123000000-E","REFORESTATION","","",26.85,1670.39106145251,44850]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","CONCRETE WASHOUT STRUCTURE","",3,610,1830]
["","","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",40,240,9600]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",20,135,2700]
["","","FILTER SACK INLET PROTECTION","",20,200,4000]
["","","FILTER SACK INLET PROTECTION CLEANOUT","",50,200,10000]
["","","SEDIMENT TUBE","",20,200,4000]
["6640000000-N","GENERIC PLANTING ITEM (EA) 1670","HEMEROCALLIS X 'AZTEC GOLD' (1 CONT.)","",472,12.6,5947.2]
["","","ILEX CORNUTA 'CARISSA' (5 CONT 24\")","",92,75.5,6946]
["","","ILEX GLABRA 'COMPACTA' (3 CONT 18\")","",357,28.5,10174.5]
["","","ILEX VOMITORIA 'SCHILLINGS","DWARF' (3 CONT 18\")",357,28.5,10174.5]
["","","LIRIOPE MUSCARI 'EVERGREEN","GIANT' (1 CONT)",2755,6.5,17907.5]
["","","MUHLENBERGIA CAPILLARIS (1 CONT 24\")","",760,10.75,8170]
["","","PANICUM VIRGATUM 'SHENENDOAH'","(1 CONT 24\")",457,14.25,6512.25]
["","","PENNISETUM ALOPECUROIDES","'HAMELN' (1 CONT 18\")",167,14.25,2379.75]
["","","PRUNUS X OKAME (B & B 2.5\" CAL 8-10')","",125,442,55250]
["6650000000-E","MULCH FOR PLANTING","","",368,79,29072]
["6675000000-E","GENERIC PLANTING ITEM (SY)","CYNODON DACTYLON 'TIFGRAND'","",7657,1.05,8039.85]
["6900000000-E","TOPSOIL","","",2132,60,127920]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",26,753.84615384615404,19600]
["7060000000-E","SIGNAL CABLE","","",29905,2.1976926935295098,65722]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",147,749.27891156462601,110144]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",33,842.12121212121201,27790]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",9,1157.7777777777801,10420]
["7252000000-E","MESSENGER CABLE (1/4\")","","",1300,2.85,3705]
["7264000000-E","MESSENGER CABLE (3/8\")","","",7020,2.4615384615384599,17280]
["7279000000-E","TRACER WIRE","","",13425,0.89068901303537995,11957.5]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",325,17.399999999999999,5655]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",8880,5.4630630630630597,48512]
["","","(2, 2\")","",11555,7.5374296841194299,87095]
["","","(3, 2\")","",300,10.199999999999999,3060]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",6850,5.3781021897810204,36840]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",950,16.294736842105301,15480]
["","","(2, 2\")","",1665,18.726726726726699,31180]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",125,275.36,34420]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",25,477.6,11940]
["7360000000-N","WOOD POLE","","",28,1113.57142857143,31180]
["7372000000-N","GUY ASSEMBLY","","",66,553.81818181818198,36552]
["7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",2,115,230]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",7,306.28571428571399,2144]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",29,414.31034482758599,12015]
["7430000000-N","HEAT SHRINK TUB KIT","","",3,115,345]
["7432000000-E","2\" RISER WITH TUBING","","",2,440,880]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",126657,6.0187964344647398,762322.7]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",66650,1.46181545386347,97430]
["7481000000-N","SITE SURVEY","","",2,1241,2482]
["7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",12,756,9072]
["7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",12,3662,43944]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",2,9698,19396]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(144)","",9250,3.7,34225]
["","","(36)","",5035,3.43962264150943,17318.5]
["7528000000-E","DROP CABLE","","",4415,3.1412231030577602,13868.5]
["7540000000-N","SPLICE ENCLOSURE","","",10,2580,25800]
["7541000000-N","MOD SPLICE ENCLOSURE","","",4,1300,5200]
["7552000000-N","INTERCONNECT CENTER","","",9,1705.55555555556,15350]
["7566000000-N","DELINEATOR MARKER","","",27,139.81481481481501,3775]
["7575142000-N","900MHZ SPECTRUM RADIO","","",4,6748,26992]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",12,8833.3333333333303,106000]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",6,12940.333333333299,77642]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,18000,36000]
["7613000000-N","SOIL TEST","","",19,708.31578947368405,13458]
["7614100000-E","DRILLED PIER FOUND","","",114,951.15789473684197,108432]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",7,147.142857142857,1030]
["7636000000-N","SIGN FOR SIGNALS","","",59,371.28813559321998,21906]
["7642100000-N","TYPE I POST W/ FOUND","","",18,1010,18180]
["7642200000-N","TYPE II PED W/ FOUND","","",14,1739.7142857142901,24356]
["7675000000-N","LED BLANKOUT SIGN","","",1,3650,3650]
["7684000000-N","SIGNAL CABINET FOUND","","",10,1125.5999999999999,11256]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",4,12208,48832]
["7768000000-N","CONTLR WITH CBNT, 2070L POLE MTD","","",4,11501,46004]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",26,104,2704]
["7852000000-N","DETECTOR CARD (NEMA TS-2)","","",48,159.375,7650]
["7901000000-N","CABINET BASE EXTENDER","","",4,282,1128]
["7948000000-N","TRAFFIC SIGNAL REMOVAL","","",4,5759,23036]
["7960000000-N","METAL POLE FOUND REMVL","","",4,2950,11800]
["7972000000-N","METAL POLE REMOVAL","","",4,385,1540]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","2.4GHZ BROADBAND ETHERNET RADIO","",3,3450,10350]
["","","ANALOG CCTV CAMERA ASSEMBLY","",1,4250,4250]
["","","CCTV ELECTRICAL SERVICE","",2,1420,2840]
["","","CCTV METAL POLE (40')","",1,4950,4950]
["","","CCTV WOOD POLE (60')","",1,1470,1470]
["","","CONTROLLER WITH CABINET (NEMA TS-2, 2070","CONTROLLER, TYPE I CABINET, BASE MTD.)",2,24000,48000]
["","","DIGITAL CCTV CAMERA ASSEMBLY","",1,4210,4210]
["","","ETHERNET EDGE SWITCH","",2,3600,7200]
["","","FIBER OPTIC VIDEO TRANSCEIVER","W/DATE RECEIVER",1,3110,3110]
["","","FIELD EQUIPMENT CABINET","",2,4310,8620]
["","","FIELD VIDEO ENCODER","",1,1710,1710]
["","","JUNCTION BOX (SPECIAL OVER-","SIZED, HEAVY DUTY)",7,670,4690]
["","","MODIFY ETHERNET RADIO INSTALL-ATION","",1,1220,1220]
["","","NEMA TS-2, TYPE I CABINET,","BASE MOUNTED, W/2070LN2 CONT- ROLLER",4,21020,84080]
["","","REMOVE RADIO INSTALLATION","",2,480,960]
["","","SOIL TEST FOR CCTV METAL POLE","",1,715,715]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","DRILLED PIER FOUNDATION FOR","CCTV METAL POLE",6,1160,6960]
["8007000000-N","CM&R TEMP STR ***********","(38+50.00-DET-)","",1,300000,300000]
["8017000000-N","CM&R TEMP ACCESS ***********","(15+98.00 -L-)","",1,25000,25000]
["8021000000-N","REMV EXIST STR **********","(38+62.00-L-)","",1,22860,22860]
["8035000000-N","REMV EXIST STR **********","(13+25.00-L-)","",1,100000,100000]
["","","(14+67.00-L-)","",1,40000,40000]
["","","(15+14.00-L-)","",1,95000,95000]
["","","(15+98.00 -L-)","",1,130000,130000]
["","","(18+64.00 -L-)","",1,150000,150000]
["","","(50+61.09-L-)","",1,325000,325000]
["8056000000-N","REMV EXIST STR **********","(107+88.00-L-)","",1,65239.92,65239.92]
["","","(137+22.00-L-)","",1,22000,22000]
["","","(168+21.00-L-)","",1,22000,22000]
["","","(21+86.00-Y6-)","",1,16000,16000]
["","","(283+77.00-L-)","",1,23000,23000]
["","","(314+63.00-L-)","",1,50000,50000]
["8065000000-N","ASBESTOS ASSESSMENT","","",6,2114.1666666666702,12685]
["8077000000-E","FOUNDATN EXCAV RET WALL","","",13920,15.41,214507.2]
["8084000000-N","FND EXCAV EB** STA*******","(1,14+67.00-L-)","",1,15000,15000]
["8096000000-E","PILE EXCAVATION IN SOIL","","",240,165,39600]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",160,325,52000]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",116.62,1223.7111987652199,142709.20000000001]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",104,1800,187200]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",41.1,1700,69870]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",137,1199.2700729927001,164300]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",48,100,4800]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",29,100,2900]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",55.3,160,8848]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",52,10,520]
["8112730000-N","PDA TESTING","","",1,2500,2500]
["8113000000-N","SID INSPECTIONS","","",2,500,1000]
["8114000000-N","SPT TESTING","","",4,1000,4000]
["8115000000-N","CSL TESTING","","",4,2887.5,11550]
["8121000000-N","UNCL STR EXCAV STA *****","(13+25.00-L-)","",1,10000,10000]
["","","(14+67.00-L-)","",1,35000,35000]
["","","(15+14.00-L-)","",1,50000,50000]
["","","(15+98.00 -L-)","",1,5000,5000]
["","","(18+64.00 -L-)","",1,5000,5000]
["","","(38+62.00-L-)","",1,20000,20000]
["8126000000-N","CULV EXCAV @ ************","(107+88.00-L-)","",1,80000,80000]
["","","(137+22.00-L-)","",1,67000,67000]
["","","(168+21.00-L-)","",1,67000,67000]
["","","(21+86.00-Y6-)","",1,37000,37000]
["","","(283+77.00-L-)","",1,67000,67000]
["","","(314+63.00-L-)","",1,67000,67000]
["","","(67+46.44-Y-)","",1,5000,5000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",1637,59.587660354306699,97545]
["8147000000-E","REINF CONC DECK SLAB","","",30049,41,1232009]
["8156000000-E","CONC WEARING SURFACE","","",2875.8,16,46012.800000000003]
["8161000000-E","GROOVING BRIDGE FLOORS","","",36329,0.46801591015442001,17002.55]
["8175000000-E","CLASS AA CONC (BRIDGE)","","",44.8,605.70000000000005,27135.360000000001]
["8182000000-E","CLASS A CONC (BRIDGE)","","",785.1,1204.08131448223,945324.24]
["8196000000-E","CLASS A CONC (CULV)","","",2244.9,929.02579179473503,2085570]
["8210000000-N","BRG APPR SLAB ***********","(13+25.00-L-)","",1,22500,22500]
["","","(14+67.00-L-)","",1,30000,30000]
["","","(15+14.00-L-)","",1,33000,33000]
["","","(15+98.00 -L-)","",1,25000,25000]
["","","(18+64.00 -L-)","",1,22500,22500]
["","","(38+62.00-L-)","",1,19475,19475]
["","","(50+61.09-L-)","",1,135000,135000]
["8217000000-E","REINF STEEL (BRIDGE)","","",154874,1.2002947557369199,185894.45]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",1874,2.5245464247598699,4731]
["8238000000-E","SPIRAL COL REINF STL BRG","","",14203,2.30391466591565,32722.5]
["8245000000-E","REINF STEEL (CULVERT)","","",292840,1.00175266357055,293353.25]
["8252000000-E","REINF STEEL (RET WALL)","","",169451,0.84,142338.84]
["8280000000-E","STRUCTURAL STEEL","","",1197800,1.5862414426448499,1900000]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",44,540.90909090909099,23800]
["","","(HP12X53)","",56,1971.42857142857,110400]
["8364000000-E","HP12X53 PILES","","",1888,44.415254237288103,83856]
["8391000000-N","STEEL PILE POINTS","","",32,192.5,6160]
["8475000000-E","TWO BAR METAL RAIL","","",1024.24,124.220397563071,127231.5]
["8505000000-E","VERT CONC BARRIER RAIL","","",890.25,101.23279977534401,90122.5]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-9 1/2\")","",160.1,135,21613.5]
["","","(1'-2\" X 3'-3 1/2\")","",160.1,135,21613.5]
["","","(1'-2\" X 3'-3\")","",579.54999999999995,92,53318.6]
["","","(1'-2\" X 3'-7\")","",170,115,19550]
["8531000000-E","4\" SLOPE PROTECTION","","",1035,155,160425]
["8608000000-E","RIP RAP II (2'-0\")","","",2483,47.202980265807497,117205]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2764,2.5137481910275001,6948]
["8654000000-N","DISC BEARINGS","","",1,55000,55000]
["8657000000-N","ELASTOMERIC BEARINGS","(14+67.00-L-)","",1,4042,4042]
["","","","",6,7916.6666666666697,47500]
["8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",5500,249.85454545454499,1374200]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",2310,250,577500]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",770,145,111650]
["8811000000-E","GENERIC CULVERT ITEM (LF)","METAL HANDRAIL (SIDE MOUNTED)","",944,62.76,59245.440000000002]
["","","METAL HANDRAIL (TOP MOUNTED)","",1188,189.75,225423]
["8815000000-E","GENERIC CULVERT ITEM (LB)","REINFORCING STEEL, STAIRS","",1564,0.84,1313.76]
["","","REINFORCING STEEL, UNDERPASS","",96200,0.84,80808]
["8818000000-E","GENERIC CULVERT ITEM (TON)","FOUNDATION CONDITIONING MATE-","RIAL, UNDERPASS",237,65.180000000000007,15447.66]
["","","NO 57 STONE","",5645,34.04,192155.8]
["8822000000-E","GENERIC CULVERT ITEM (SY)","6\" RAMPS & WALKWAYS","",1150,67.66,77809]
["","","BENTONITE GEOTEXTILE WATER-","PROOFING MEMBRANE",2785,74.400000000000006,207204]
["8825000000-E","GENERIC CULVERT ITEM (CY)","CLASS A CONCRETE, STAIRS","",36.1,1130.3398891966799,40805.269999999997]
["","","CLASS AA CONCRETE, RETAINING WALL","",1159,774,897066]
["","","CLASS AA CONCRETE, UNDERPASS","",692,609,421428]
["","","UNCLASSIFIED STRUCTURE EXCAVA-","TION, RAMPS, STAIRS & WALKWAYS",4430,8.81,39028.300000000003]
["","","UNDERPASS EXCAVATION","",5705,12.85,73309.25]
["8846000000-E","GENERIC RET WALL ITEM (TON)","FOUNDATION CONDITIONING MATE-","RIAL, RETAINING WALL",1047,58.85,61615.95]
["8847000000-E","GENERIC RET WALL ITEM (SF)","TEMPORARY SHORING","",5200,19,98800]
["8860000000-N","GENERIC STR ITEM (LS)","ASBESTOS ASSESSMENT","",1,1500,1500]

{"sheet":"ITEMS - DIV 06","index":8,"n_rows":366,"n_cols":7,"rows_kept":366,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 06"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",7,402750.372857143,2819252.61]
["0000400000-N","CONST SURVEYING","","",5,107600,538000]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","CONSTRUCTION SURVEYING","",1,65000,65000]
["","","DESIGN & CONSTRUCTION OF","BRIDGE",1,415403.74,415403.74]
["","","INTERIOR BENT CAPS","STRUCTURE 250211",1,20000,20000]
["0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","END BENTS STRUCTURE 250211","",2,20000,40000]
["","","RIGHT OF WAY ACQUISITION","",1,4500,4500]
["0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT 1 STRUCTURE 250211",45,210,9450]
["","","","BENT 2 STRUCTURE 250211",45,210,9450]
["","","AVE FOUNDATION LENGTH AT INTE-","RIOR BENT STRUCTURE 250211",55,450,24750]
["","","BRIDGE LENGTH","STRUCTURE 250211",100,3500,350000]
["0001000000-E","CLEARING & GRUBBING","","",50,44642.26,2232113]
["0008000000-E","SUPP CLEARING & GRUBBING","","",6,2583.3333333333298,15500]
["0022000000-E","UNCLAS EXCAVATION","","",76500,11.9248366013072,912250]
["0028000000-N","TYPE I STANDARD APPR **********","(30+02)","",1,41500,41500]
["","","(55+88.11 -L-)","",1,100000,100000]
["0036000000-E","UNDERCUT EXCAVATION","","",21700,9.8792626728110609,214380]
["0043000000-N","GRADING","","",1,900000,900000]
["0057000000-E","UNDERCUT EXCAVATION","","",200,12.5,2500]
["0106000000-E","BORROW EXCAVATION","","",406500,6.5461254612546096,2661000]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",20460,6.5361876832844601,133730.4]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",55490,6.3874571994954001,354440]
["0177000000-E","BREAKING OF EXT ASPH PVMT","","",4200,4.5,18900]
["0192000000-N","PROOF ROLLING","","",14,340,4760]
["0195000000-E","SELECT GRANULAR MAT'L","","",25350,13.631163708086801,345550]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",45220,2.1418288367978802,96853.5]
["0199000000-E","TEMP SHORING","","",6592,19.350000000000001,127555.2]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,71.650000000000006,3582.5]
["","","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",100,100,10000]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",3164,35.369785082174502,111910]
["0320000000-E","FND CONDIT GEOTEXTILE","","",10344,2.1787509667440101,22537]
["0335200000-E","15\" DRAINAGE PIPE","","",516,33.9,17492.400000000001]
["0335400000-E","24\" DRAINAGE PIPE","","",40,51,2040]
["0335500000-E","30\" DRAINAGE PIPE","","",24,178.85,4292.3999999999996]
["0335600000-E","36\" DRAINAGE PIPE","","",308,79.599999999999994,24516.799999999999]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",8,542.5,4340]
["0343000000-E","15\" SIDE DRAIN PIPE","","",1496,38.476737967914403,57561.2]
["0344000000-E","18\" SIDE DRAIN PIPE","","",908,40.518942731277498,36791.199999999997]
["0345000000-E","24\" SIDE DRAIN PIPE","","",356,51.943820224719097,18492]
["0354000000-E","***\" RC PIPE CULV *****","(24\", V)","",80,86,6880]
["0366000000-E","15\" RC PIPE CULV III","","",2644,46.8865355521936,123968]
["0372000000-E","18\" RC PIPE CULV III","","",784,54.530612244898002,42752]
["0378000000-E","24\" RC PIPE CULV III","","",1204,73.086378737541494,87996]
["0384000000-E","30\" RC PIPE CULV III","","",688,90,61920]
["0390000000-E","36\" RC PIPE CULV III","","",1044,115,120060]
["0396000000-E","42\" RC PIPE CULV III","","",136,141,19176]
["0402000000-E","48\" RC PIPE CULV III","","",212,173,36676]
["0408000000-E","54\" RC PIPE CULV III","","",320,210,67200]
["0448000000-E","***\" RCP CULV CLASS IV","(48\")","",644,166.71428571428601,107364]
["","","(54\")","",680,240.46352941176499,163515.20000000001]
["","","(60\")","",664,324.33734939759,215360]
["","","(72\")","",288,430,123840]
["0448200000-E","15\" RCP CULV CLASS IV","","",7708,47.3040996367411,364620]
["0448300000-E","18\" RCP CULV CLASS IV","","",788,58.615482233502497,46189]
["0448400000-E","24\" RCP CULV CLASS IV","","",992,70.451612903225794,69888]
["0448500000-E","30\" RCP CULV CLASS IV","","",824,79.565533980582501,65562]
["0448600000-E","36\" RCP CULV CLASS IV","","",1636,110.31246943765299,180471.2]
["0448700000-E","42\" RCP CULV CLASS IV","","",1676,165.61097852028601,277564]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",220,45,9900]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",4,350,1400]
["0986000000-E","GENERIC PIPE ITEM (LF)","4\" PVC IRRIGATION CONDUIT","",588,24,14112]
["0995000000-E","PIPE REMOVAL","","",7173,15.158371671546099,108731]
["0996000000-N","PIPE CLEAN OUT","","",2,3500,7000]
["1000000000-E","6\" SLOPE PROTECTION","","",150,110,16500]
["1011000000-N","FINE GRADING","","",3,675000,2025000]
["1099500000-E","SHALLOW UNDERCUT","","",6500,15.422307692307699,100245]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",12840,39.234423676012497,503770]
["1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",250,57,14250]
["1121000000-E","AGGREGATE BASE COURSE","","",31980,31.512789243277101,1007779]
["1220000000-E","INCIDENTAL STONE BASE","","",800,55.518749999999997,44415]
["1231000000-E","SHOULDER BORROW","","",1930,30,57900]
["1245000000-E","SHOULDER RECONST","","",88.05,1636.91084611016,144130]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",14211,21.055520371543199,299220]
["1275000000-E","PRIME COAT","","",2700,5,13500]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1.5\")","",46980,1.9,89262]
["","","(1/2\")","",708693,1.4,992170.2]
["","","(2\")","",829094,1.671674695511,1385975.46]
["","","(4\")","",45310,3.55,160850.5]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",13800,4.5,62100]
["","","(0\" TO 2\")","",20000,4.67,93400]
["1330000000-E","INCIDENTAL MILLING","","",25540,19.170634299138602,489618]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",34770,57.989142939315499,2016282.5]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",49671,53.720495862777099,2668350.75]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",16290,58.475076734192797,952559]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",105267,42.913461483655901,4517371.3499999996]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",131400,43.047627625570797,5656458.2699999996]
["1575000000-E","ASP FOR PLANT MIX","","",11225,525.24097995545696,5895830]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",7490,711.49679572763705,5329111]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",795,194.16352201257899,154360]
["1704000000-E","PATCHING EXIST PVMT","","",300,250,75000]
["1840000000-E","MILLED RUMBLE STRIPS","","",783112,0.14786893828723999,115797.94]
["1880000000-E","GENERIC PAVING ITEM (TON)","ASPHALT PAVEMENT INTERLAYER","",150,130,19500]
["1881000000-E","GENERIC PAVING ITEM (LF)","MEDIAN HAZARD PROTECTION","",103,586,60358]
["1891000000-E","GENERIC PAVING ITEM (SY)","PAVEMENT INTERLAYER (REGULAR)","",45320,5.95,269654]
["2022000000-E","SUBDRAIN EXCAVATION","","",8871,14.3104497801826,126948]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",29050,4.5335628227194498,131700]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",933,25,23325]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",4881,35.357713583282099,172581]
["2044000000-E","6\" PERF SUBDRN PIPE","","",34600,8.63583815028902,298800]
["2070000000-N","SUBDRN PIPE OUTLET","","",71,320.42253521126798,22750]
["2077000000-E","6\" OUTLET PIPE","","",426,38.239436619718298,16290]
["2209000000-E","ENDWALLS","","",44.5,1019.7752808988801,45380]
["2220000000-E","REINF ENDWALLS","","",63.3,1292.7330173775699,81830]
["2253000000-E","PIPE COLLARS","","",7.8570000000000002,1282.05421916762,10073.1]
["2275000000-E","FLOWABLE FILL","","",18,396,7128]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",253,1761.22134387352,445589]
["2297000000-E","MASNRY DRAINAGE STRUCT","","",16.425999999999998,1306.09460611226,21453.91]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",89.7,377.76755852842803,33885.75]
["2354200000-N","FRAME W/GRATE 840.24 STD","","",1,471,471]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",85,625.83529411764698,53196]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",26,484.61538461538498,12600]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",22,952.54545454545496,20956]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",12,591.66666666666697,7100]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",19,597.63157894736798,11355]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",22,710.36363636363603,15628]
["","","(F)","",38,714.21052631578902,27140]
["","","(G)","",23,730.43478260869597,16800]
["2396000000-N","FRAME W/COVER STD 840.54","","",7,485.71428571428601,3400]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",88,607.95454545454595,53500]
["2535000000-E","**\"X**\" CONC CURB","(9\" X 12\")","",510,28,14280]
["2538000000-E","**'-**\" CONC CURB & GUTTER","(2'-9\")","",1190,17.579999999999998,20920.2]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",15080,16.817354111405798,253605.7]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",7520,20.060398936170198,150854.20000000001]
["2556000000-E","SHOULDER BERM GUTTER","","",933,25.515969989281899,23806.400000000001]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",1270,32.100551181102396,40767.699999999997]
["2591000000-E","4\" CONC SIDEWALK","","",3660,45,164700]
["2605000000-N","CONC CURB RAMPS","","",70,1200,84000]
["2612000000-E","6\" CONC DRIVEWAY","","",210,50.7542857142857,10658.4]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",9150,56.081147540983601,513142.5]
["2738000000-E","GENERIC PAVING ITEM (SY)","7\" CONCRETE TRUCK APRON","",470,110,51700]
["2800000000-N","ADJ CATCH BASINS","","",1,1000,1000]
["2830000000-N","ADJ MANHOLES","","",15,1140,17100]
["2845000000-N","ADJ METER OR VALVE BOXES","","",15,950,14250]
["2950000000-N","CONVERT JB TO DI","","",1,1200,1200]
["3000000000-N","IMPACT ATTEN TYPE 350","","",2,14000,28000]
["3030000000-E","STL BEAM GUARDRAIL","","",1800,18.1875,32737.5]
["3045000000-E","SBGR SHOP CURVED","","",62.5,21,1312.5]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",30,38.3333333333333,1150]
["3195000000-N","GR END TYPE AT-1","","",1,650,650]
["3210000000-N","GR END TYPE CAT-1","","",2,560,1120]
["3215000000-N","GR ANCHOR TYPE III","","",2,1750,3500]
["3287000000-N","GR END TYPE TL-3","","",9,3183.3333333333298,28650]
["3317000000-N","GR ANCHOR TYPE B-77","","",8,1600,12800]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",1874,1,1874]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",19230,3.5457098283931399,68184]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1215,16.493827160493801,20040]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",305,31.524590163934398,9615]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",350,7.5,2625]
["3542000000-E","MET LINE PST 48\" CL FEN","","",36,52,1872]
["3548000000-E","MET TERM PST 48\" CL FEN","","",46,70,3220]
["3554000000-E","MET GATE PST **\" CL FEN D","(48\")","",2,280,560]
["3557000000-E","ADDITIONAL BARBED WIRE","","",510,0.50980392156862997,260]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(48\", 8', 16')","",1,1650,1650]
["3574000000-E","GENERIC FENCING ITEM 867 (LF)","VINYL 3 RAIL FENCE RESET","",190,35,6650]
["3628000000-E","RIP RAP, CLASS I","","",806,65.6017369727047,52875]
["3649000000-E","RIP RAP, CLASS B","","",94,59.893617021276597,5630]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",5095,2.2615309126594698,11522.5]
["4048000000-E","REINF CONC FOUNDTN","","",7,1035.7142857142901,7250]
["4054000000-E","PLN CONC FOUNDTN","","",2,10,20]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",7982,5.3345965923327503,42580.75]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",657,5.5,3613.5]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",7179,6.1755119097367297,44334]
["4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",2,55,110]
["4096000000-N","SIGN ERECTION, TYPE D","","",15,107,1605]
["4102000000-N","SIGN ERECTION, TYPE E","","",384,89.9348958333333,34535]
["4108000000-N","SIGN ERECTION, TYPE F","","",36,101.388888888889,3650]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",12,675,8100]
["","","(B)","",7,500,3500]
["4114000000-N","SIGN ERECTION, MILEMARKERS","","",2,100,200]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",5,150,750]
["4141000000-N","DISPOSE SUPPORT, WOOD","","",1,5,5]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",9,26.6666666666667,240]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",221,11.221719457013601,2480]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",2,5,10]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",3289,10.0929157798723,33195.599999999999]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",2681,13.7914957105558,36975]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",729,9.9322359396433502,7240.6]
["4415000000-N","FLASHING ARROW BOARD","","",11,2828.54545454545,31114]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",11,7749.4545454545496,85244]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",40,52,2080]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",10,7450,74500]
["4424000000-N","WZ PRESENCE LIGHTING","","",30,750.5,22515]
["4430000000-N","DRUMS","","",1950,43.3333333333333,84500]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",31,68.064516129032299,2110]
["4435000000-N","CONES","","",510,23.372549019607799,11920]
["4445000000-E","BARRICADES (TYPE III)","","",952,26.747899159663898,25464]
["4450000000-N","FLAGGER","","",1920,25,48000]
["4455000000-N","FLAGGER","","",1024,239.4287109375,245175]
["4465000000-N","TEMP CRASH CUSHIONS","","",8,5625,45000]
["4470000000-N","REM & RES CRASH CUSHION","","",3,2200,6600]
["4480000000-N","TMA","","",9,8111.1111111111104,73000]
["4485000000-E","PORT CONC BARRIER","","",3406,22.324427480916,76037]
["4500000000-E","REM & RES PORT CONC BARRIER","","",2964,4,11856]
["4507000000-E","WATER FILLED BARRIER","","",1344,80,107520]
["4510000000-N","LAW ENFORCEMENT","","",2386,40.310142497904401,96180]
["4516000000-N","SKINNY DRUM","","",510,45.294117647058798,23100]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",48,75,3600]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","LANE CLOSURE","",262,1891.7938931297699,495650]
["","","RAMP/LOOP CLOSURE","",68,1142.35294117647,77680]
["4650000000-N","TEMP RAISED PVMT MRKS","","",2986,4.9618218352310803,14816]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",74282,0.70464984787701002,52342.8]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",42998,0.64550025582585002,27755.22]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",923115,0.68830685234234001,635386.38]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",109166,0.94914259018376002,103614.1]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",4522,2.35128261831048,10632.5]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",970,3.1945360824742299,3098.7]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",53888,1.98463015884798,106947.75]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",100,1.8,180]
["4705000000-E","THERMO LINES 16\" 120MILS","","",210,9.9,2079]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",3637,11.561245532031901,42048.25]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",50,97,4850]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",496,126.864919354839,62925]
["4726000000-E","HIP THERMO PVT MKG LINE 4\" 90 MILS","","",93,20,1860]
["4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",32,400,12800]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",1140,5,5700]
["","","(IV)","",1740,4.5,7830]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",1388849,0.13559983122715,188327.69]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",182766,0.19472462055306,35589.040000000001]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",43544,0.51868914201727001,22585.8]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",29693,0.78858653554710001,23415.5]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",130,1.4,182]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",5317,3.1094602219296599,16533]
["4840000000-N","PAINT PVT MKG CHARACTER","","",48,56.6666666666667,2720]
["4845000000-N","PAINT PVT MKG SYMBOL","","",658,43.566869300911797,28667]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",49722,0.52558223723904995,26133]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",35,9,315]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",44,41.818181818181799,1840]
["4900000000-N","PERM RAISED PVMT MARKERS","","",2601,4.13802383698577,10763]
["4905000000-N","SNOWPLB PVMT MRKER","","",6057,26.815502724120901,162421.5]
["4935000000-N","FLEX DELINATR (CRYSTAL)","","",36,68,2448]
["4940000000-N","FLEX DELINATR (YELLOW)","","",26,68,1768]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",10,68,680]
["5255000000-N","PORTABLE LIGHTING","","",1,540000,540000]
["5325600000-E","6\" WATER LINE","","",1940,63,122220]
["5325800000-E","8\" WATER LINE","","",699,77.397711015736803,54101]
["5326600000-E","16\" WATER LINE","","",702,233,163566]
["5329000000-E","DI H2O PIPE FITTINGS","","",12775,7.5694716242661402,96700]
["5540000000-E","6\" VALVE","","",4,1900,7600]
["5546000000-E","8\" VALVE","","",3,1600,4800]
["5558600000-E","16\" VALVE","","",4,11875,47500]
["5606000000-E","2\" BLOW OFF","","",2,1550,3100]
["5648000000-N","RELOCATE WATER METER","","",3,2333.3333333333298,7000]
["5649000000-N","RECONNECT WATER METER","","",7,2242.8571428571399,15700]
["5672000000-N","RELOCATE FIRE HYDRANT","","",6,6033.3333333333303,36200]
["5673000000-E","FIRE HYDRANT LEG","","",56,65,3640]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",433,170,73610]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",463,173.755939524838,80449]
["5709300000-E","6\" FORCE MAIN SEWER","","",408,105,42840]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",3,2900,8700]
["5769000000-E","DI SEWER PIPE FITTINGS","","",1235,12,14820]
["5775000000-E","4' DIA UTILITY MANHOLE","","",9,3761.1111111111099,33850]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",16,388.25,6212]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",104,27,2808]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",712,31.8,22641.599999999999]
["5828000000-N","REMOVE UTILITY MANHOLE","","",4,1770,7080]
["5836000000-E","24\" ENCASEMENT PIPE","","",260,255,66300]
["5836200000-E","30\" ENCASEMENT PIPE","","",159,493,78387]
["5882000000-N","GENERIC UTILITY ITEM (EA)","BREAKDOWN & CAP EXISTING MAN- HOLE","",1,1400,1400]
["","","REMOVE EXISTING VAULT","",1,5000,5000]
["5912000000-N","GENERIC UTILITY ITEM (LS)","6\" WATER METER ASSEMBLY IN VAULT","",1,30000,30000]
["6000000000-E","TEMP SILT FENCE","","",84075,2.1225393993458201,178452.5]
["6006000000-E","EROS CONTRL STONE CL A","","",1700,52.788235294117598,89740]
["6009000000-E","EROS CONTRL STONE CL B","","",8715,47.210556511761297,411440]
["6012000000-E","SEDIMENT CONTROL STONE","","",6595,45.812736921910499,302135]
["6015000000-E","TEMP MULCHING","","",183.5,769.34604904632204,141175]
["6018000000-E","SEED FOR TEMP SEEDING","","",10800,4.4796296296296303,48380]
["6021000000-E","FERT FOR TEMP SEEDING","","",56.5,984.07079646017701,55600]
["6024000000-E","TEMP SLOPE DRAINS","","",2690,11.6505576208178,31340]
["6029000000-E","SAFETY FENCE","","",7300,1.5753424657534201,11500]
["6030000000-E","SILT EXCAVATION","","",20530,4.1911836337067703,86045]
["6036000000-E","MATTING FOR EROS CONTROL","","",83650,1.4548714883442899,121700]
["6037000000-E","COIR FIBER MAT","","",465,6.3870967741935498,2970]
["6038000000-E","PERM SOIL REINF MAT","","",715,9.0419580419580399,6465]
["6042000000-E","1/4\" HARDWARE CLOTH","","",11145,6.1728129205921896,68796]
["6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",640,3.9015624999999998,2497]
["6070000000-N","SPECIAL STILLING BASINS","","",12,666.66666666666697,8000]
["6071010000-E","WATTLE","","",2900,7,20300]
["6071012000-E","COIR FIBER WATTLE","","",8060,6.2047146401985103,50010]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",3980,11.128768844221099,44292.5]
["6071030000-E","COIR FIBER BAFFLE","","",5000,5.9669999999999996,29835]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",20,904,18080]
["","","(2\")","",7,952.57142857142901,6668]
["6084000000-E","SEEDING AND MULCHING","","",185,1892.97297297297,350200]
["6087000000-E","MOWING","","",114,103.289473684211,11775]
["6090000000-E","SEED FOR REPAIR SEEDING","","",1950,9.5,18525]
["6093000000-E","FERT FOR REPAIR SEEDING","","",6,1212.5,7275]
["6096000000-E","SEED FOR SUPP SEEDING","","",4325,6,25950]
["6108000000-E","FERTILIZER TOPDRESSING","","",128.75,923.88349514563095,118950]
["6111000000-E","IMPERVIOUS DIKE","","",344,46.744186046511601,16080]
["6114500000-N","SPECIALIZED HAND MOWING","","",40,73.75,2950]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",122,437.29508196721298,53350]
["6117500000-N","CONC WASHOUT STR","","",22,618.18181818181802,13600]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","CONCRETE WASHOUT STRUCTURE","",5,850,4250]
["","","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",40,500,20000]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",20,450,9000]
["7000000000-E","PEDEST SIG HEAD (**************)","(16\", 1 SECTION W/ COUNTDOWN)","",8,1100,8800]
["7060000000-E","SIGNAL CABLE","","",7880,2.7341370558375599,21545]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",52,720.38461538461502,37460]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",6,916.66666666666697,5500]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",2,1050,2100]
["7252000000-E","MESSENGER CABLE (1/4\")","","",405,3.5,1417.5]
["7264000000-E","MESSENGER CABLE (3/8\")","","",3620,2.9298342541436502,10606]
["7279000000-E","TRACER WIRE","","",4610,0.89,4102.8999999999996]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",80,18,1440]
["7300000000-E","UNPAVED TRENCH (***********)","(1 CONDUIT, 2\")","",10,10,100]
["","","(1, 2\")","",2990,6.6153846153846203,19780]
["","","(2, 2\")","",2815,7.5621669626998198,21287.5]
["","","(3, 2\")","",20,10,200]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",1565,3,4695]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",100,24.84,2484]
["","","(2, 2\")","",1885,17.8,33553]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",45,238.91111111111101,10751]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",15,650,9750]
["7360000000-N","WOOD POLE","","",10,900,9000]
["7372000000-N","GUY ASSEMBLY","","",19,220,4180]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",3,250,750]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",7,375,2625]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",7115,5.9265635980323301,42167.5]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",18705,1.4334803528468301,26813.25]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",425,2.75,1168.75]
["","","(24)","",4990,2.9,14471]
["7540000000-N","SPLICE ENCLOSURE","","",5,2250,11250]
["7552000000-N","INTERCONNECT CENTER","","",5,1890,9450]
["7566000000-N","DELINEATOR MARKER","","",15,125,1875]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",19,9900.3684210526299,188107]
["7613000000-N","SOIL TEST","","",19,892.05263157894694,16949]
["7614100000-E","DRILLED PIER FOUND","","",133,799.68421052631595,106358]
["7636000000-N","SIGN FOR SIGNALS","","",1,480,480]
["7642200000-N","TYPE II PED W/ FOUND","","",8,1800,14400]
["7684000000-N","SIGNAL CABINET FOUND","","",5,771,3855]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",4,500,2000]
["7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070E, BASE MOUNTED)","",1,12897,12897]
["7744000000-N","DETECTOR CARD (TYPE 170)","","",3,110,330]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",4,12800,51200]
["7768000000-N","CONTLR WITH CBNT, 2070L POLE MTD","","",1,11500,11500]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",43,127.44186046511599,5480]
["7901000000-N","CABINET BASE EXTENDER","","",5,313.2,1566]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","ETHERNET EDGE SWITCH","",4,3000,12000]
["","","MICROWAVE VEHICLE DETECTOR,","SINGLE ZONE",1,3500,3500]
["8035000000-N","REMV EXIST STR **********","(55+88.11 -L-)","",1,135000,135000]
["8065000000-N","ASBESTOS ASSESSMENT","","",1,1064,1064]
["8091000000-N","FND EXCAV B** STA *******","(1, 30+02.30-Y-)","",1,6300,6300]
["","","(1, 55+88.11 -L-)","",1,20000,20000]
["8112730000-N","PDA TESTING","","",1,2850,2850]
["8147000000-E","REINF CONC DECK SLAB","","",25994,34.175771331845802,888365]
["8161000000-E","GROOVING BRIDGE FLOORS","","",28721,0.39281501340482999,11282.04]
["8182000000-E","CLASS A CONC (BRIDGE)","","",460.7,615.708704145865,283657]
["8196000000-E","CLASS A CONC (CULV)","","",6.7,1900,12730]
["8210000000-N","BRG APPR SLAB ***********","(30+02.30-Y-)","",1,32500,32500]
["","","(55+88.11 -L-)","",1,65000,65000]
["8217000000-E","REINF STEEL (BRIDGE)","","",74914,1,74914]
["8238000000-E","SPIRAL COL REINF STL BRG","","",4201,2.3020471316353199,9670.9]
["8245000000-E","REINF STEEL (CULVERT)","","",520,1,520]
["8265000000-E","54\" PRESTR CONC GIRDR","","",1676.25,261,437501.25]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",861.33,350,301465.5]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(30+02.30-Y-)","",36,550,19800]
["","","(HP 12 X 53)","",74,600,44400]
["8364000000-E","HP12X53 PILES","","",8210,36.309378806333697,298100]
["8393000000-N","PILE REDRIVES","","",57,66.6666666666667,3800]
["8475000000-E","TWO BAR METAL RAIL","","",360.43,150,54064.5]
["8503000000-E","CONC BARRIER RAIL","","",433.32,95,41165.4]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-2 3/4\")","",376.39,110,41402.9]
["8531000000-E","4\" SLOPE PROTECTION","","",1411.5,85,119977.5]
["8657000000-N","ELASTOMERIC BEARINGS","","",2,7000,14000]

{"sheet":"ITEMS - DIV 07","index":9,"n_rows":928,"n_cols":7,"rows_kept":928,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 07"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",10,1295525.8559999999,12955258.560000001]
["0000400000-N","CONST SURVEYING","","",6,280820.66833333299,1684924.01]
["0000700000-N","FIELD OFFICE","","",1,106457.16,106457.16]
["0001000000-E","CLEARING & GRUBBING","","",259,41944.052702702698,10863509.65]
["0008000000-E","SUPP CLEARING & GRUBBING","","",10,9914.2219999999998,99142.22]
["0015000000-N","SEALING ABANDONED WELLS","","",10,1600.26,16002.6]
["0022000000-E","UNCLAS EXCAVATION","","",3324025,6.9656666240476497,23154050]
["0028000000-N","TYPE I STANDARD APPR **********","(14+97.65 -Y8-)","",1,49875,49875]
["","","(140+21.50 -L- LT)","",1,69675,69675]
["","","(140+21.50 -L- RT)","",1,64375,64375]
["","","(155+02.50 -L- LT)","",1,69675,69675]
["","","(155+02.50 -L- RT)","",1,64500,64500]
["","","(22+16.89 -L-)","",1,35720,35720]
["","","(227+33.50)","",1,48000,48000]
["","","(23+26.00 -L- EB)","",1,31000,31000]
["","","(23+26.00 -L- WB)","",1,31000,31000]
["","","(25+52.71 -Y7-)","",1,60500,60500]
["","","(337+20.09 -L- LT)","",1,66100,66100]
["","","(337+20.09 -L- RT)","",1,66100,66100]
["","","(93+43.36 -L- LT)","",1,35500,35500]
["","","(93+43.36 -L- RT)","",1,35500,35500]
["0029000000-N","TYPE III REINF APPR **********","(17+37.28 -Y16-)","",1,69100,69100]
["","","(22+29.98 -Y5-)","",1,82700,82700]
["","","(28+98.81 -Y4-)","",1,135500,135500]
["","","(329+95.42 -L- LT)","",1,89600,89600]
["","","(329+95.42 -L- RT)","",1,89600,89600]
["","","(470+43.12 -L- LT)","",1,96200,96200]
["","","(470+43.12 -L- RT)","",1,90900,90900]
["","","(93+43.36 -L- LT)","",1,29400,29400]
["","","(93+43.36 -L- RT)","",1,30200,30200]
["0030000000-N","TYPE II MOD APPR **********","(28+17.37-Y-)","",1,2265.62,2265.62]
["0036000000-E","UNDERCUT EXCAVATION","","",157776,3.9960735473075801,630484.5]
["0043000000-N","GRADING","","",1,464006.5,464006.5]
["0050000000-E","SUPP CLEARING & GRUBBING","","",3,2784,8352]
["0057000000-E","UNDERCUT EXCAVATION","","",350,36.5,12775]
["0063000000-N","GRADING","","",2,692079,1384158]
["0106000000-E","BORROW EXCAVATION","","",4417000,7.8752546977590002E-2,347850]
["0127000000-N","EMBM'T SETTLEMENT GAUGE","","",4,810,3240]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",82523,3.5234460695805998,290765.34000000003]
["0141000000-E","BERM DITCH CONST","","",6250,3.1917599999999999,19948.5]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",47250,12.2216190476191,577471.5]
["0177000000-E","BREAKING OF EXT ASPH PVMT","","",2900,2.4300000000000002,7047]
["0192000000-N","PROOF ROLLING","","",170,216.10529411764699,36737.9]
["0195000000-E","SELECT GRANULAR MAT'L","","",79050,4.7113092979127096,372429]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",139802,1.6435832105406201,229776.22]
["0199000000-E","TEMP SHORING","","",25696,43.5794948630137,1119818.7]
["0220000000-E","ROCK EMBANKMENTS","","",5420,37.89,205363.8]
["0222000000-E","GEOTEXTILE ROCK EMBANK","","",2860,1.03,2945.8]
["0223000000-E","ROCK PLATING","","",1000,65.83,65830]
["0248000000-N","GENERIC GRADING ITEM (LS)","DRY DETENTION BASIN (NO 1)","",1,28000,28000]
["","","DRY DETENTION BASIN (NO 8)","",1,35000,35000]
["","","FILTRATION BASIN 1","",1,77877.009999999995,77877.009999999995]
["","","FILTRATION BASIN 2","",1,102117.45,102117.45]
["","","INSTRUMENTATION INSTALLATION","ASSIST AT STR 7 (BR 1246) - END BENT 1",1,2000,2000]
["","","","ASSIST AT STR 7 (BR 1246) - END BENT 2",1,2000,2000]
["","","INSTRUMENTATION INSTALLATION ASSIST AT","STRS 2 & 3 (BR 1241 & 1242) - END BENT 1",1,4000,4000]
["","","","STRS 2 & 3 (BR 1241 & 1242) - END BENT 2",1,4000,4000]
["","","MEDIA FILTER BASIN (NO 2)","",1,60000,60000]
["","","MEDIA FILTER BASIN (NO 3)","",1,40000,40000]
["","","MEDIA FILTER BASIN (NO 4)","",1,51500,51500]
["","","MEDIA FILTER BASIN (NO 5)","",1,40000,40000]
["","","MEDIA FILTER BASIN (NO 6)","",1,57500,57500]
["","","MEDIA FILTER BASIN (NO 7)","",1,90500,90500]
["","","MEDIA FILTER BASIN (NO 9)","",1,72500,72500]
["","","REMOVAL & DISPOSAL OF 5 FOAM","FILLED USTS",1,16500,16500]
["","","SETTLEMENT MONITORING ASSIST","AT STR 7 (BR 1246) - END BENT 1",1,1000,1000]
["","","","AT STR 7 (BR 1246) - END BENT 2",1,1000,1000]
["","","SETTLEMENT MONITORING ASSIST AT STRS 2","& 3 (BR 1241 & 1242) - END BENT 1",1,2000,2000]
["","","","& 3 (BR 1241 & 1242) - END BENT 2",1,2000,2000]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,101.23,5061.5]
["","","STOCKPILING PETROLEUM CONTAMI-NATED SOIL","",3000,6.75,20250]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",12989,31.244252829317102,405831.6]
["0320000000-E","FND CONDIT GEOTEXTILE","","",45126,1.7207931126180001,77652.509999999995]
["0335200000-E","15\" DRAINAGE PIPE","","",316,45,14220]
["0335300000-E","18\" DRAINAGE PIPE","","",296,47,13912]
["0335400000-E","24\" DRAINAGE PIPE","","",20,57,1140]
["0335500000-E","30\" DRAINAGE PIPE","","",36,95,3420]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15)","",4,125,500]
["0342000000-E","**\" SIDE DRAIN PIPE","(30\")","",3008,98.373151595744702,295906.44]
["","","(36\")","",284,118.7,33710.800000000003]
["","","(42\")","",140,130.65,18291]
["","","(48\")","",16,235.95,3775.2]
["","","(54\")","",44,278.2,12240.8]
["0343000000-E","15\" SIDE DRAIN PIPE","","",12672,50.507695707070702,640033.52]
["0344000000-E","18\" SIDE DRAIN PIPE","","",5188,52.749491133384701,273664.36]
["0345000000-E","24\" SIDE DRAIN PIPE","","",5208,71.894969278033798,374429]
["0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",17,281.41411764705902,4784.04]
["","","(18\")","",12,663.16833333333295,7958.02]
["","","(24\")","",4,318.54000000000002,1274.1600000000001]
["","","(30\")","",8,412.53,3300.24]
["0350000000-E","***\" RC PIPE CULV, CONTR DESIGN","(24\")","",1696,169.8,287980.79999999999]
["","","(36\")","",752,199.83079787234001,150272.76]
["","","(42\")","",732,273.97333333333302,200548.48000000001]
["","","(48\")","",124,322.2,39952.800000000003]
["","","(54\")","",860,359.2,308912]
["0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",4524,52.6,237962.4]
["","","(18\", V)","",772,63.85,49292.2]
["","","(24\", V)","",1860,79.235956989247299,147378.88]
["","","(66\", V)","",716,460.35888268156401,329616.96000000002]
["0366000000-E","15\" RC PIPE CULV III","","",9192,50.093794604003499,460462.16]
["0372000000-E","18\" RC PIPE CULV III","","",5211,49.439117251966998,257627.24]
["0378000000-E","24\" RC PIPE CULV III","","",5054,65.522809655718206,331152.28000000003]
["0384000000-E","30\" RC PIPE CULV III","","",3052,85.966107470511105,262368.56]
["0390000000-E","36\" RC PIPE CULV III","","",2056,114.219494163424,234835.28]
["0396000000-E","42\" RC PIPE CULV III","","",1044,148.64766283524901,155188.16]
["0402000000-E","48\" RC PIPE CULV III","","",276,169.25,46713]
["0408000000-E","54\" RC PIPE CULV III","","",20,363.81,7276.2]
["0414000000-E","60\" RC PIPE CULV III","","",708,328.74576271186402,232752]
["0426000000-E","72\" RC PIPE CULV III","","",336,447.95,150511.20000000001]
["0448000000-E","***\" RCP CULV CLASS IV","(54\")","",232,310.27999999999997,71984.960000000006]
["0448200000-E","15\" RCP CULV CLASS IV","","",20308,51.828900925743497,1052541.32]
["0448300000-E","18\" RCP CULV CLASS IV","","",6472,54.547305315203999,353030.16]
["0448400000-E","24\" RCP CULV CLASS IV","","",4123,69.981576521950004,288534.03999999998]
["0448500000-E","30\" RCP CULV CLASS IV","","",1919,89.216425221469507,171206.32]
["0448600000-E","36\" RCP CULV CLASS IV","","",2264,113.014558303887,255864.95999999999]
["0448700000-E","42\" RCP CULV CLASS IV","","",356,145.4,51762.400000000001]
["0576000000-E","**\" CS PIPE CULV *****\"","(42\", 0.109\")","",112,134,15008]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",2390,57.201757322175702,136712.20000000001]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",1264,70.529272151898695,89149]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",1268,77.194952681388003,97883.199999999997]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",612,92.986274509803906,56907.6]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",72,472.12555555555599,33993.040000000001]
["","","(15\", 0.064)","",2,125,250]
["","","(18\", 0.064\")","",32,570.98374999999999,18271.48]
["","","(24\", 0.064\")","",28,765,21420]
["","","(30\", 0.079\")","",16,893.98749999999995,14303.8]
["","","(42\", 0.109\")","",2,1465,2930]
["0974000000-E","**\"WLD STL PIPE ***\" B RR","(36\", 0.532\")","",68,650,44200]
["0986000000-E","GENERIC PIPE ITEM (LF)","24\" DUCTILE IRON PIPE, CLASS 250","",144,147.09,21180.959999999999]
["0995000000-E","PIPE REMOVAL","","",12295,21.455978853192299,263801.26]
["0996000000-N","PIPE CLEAN OUT","","",4,801.32500000000005,3205.3]
["1011000000-N","FINE GRADING","","",3,1247333.33333333,3742000]
["1022000000-E","SEALING PVMT CRACKS","","",3900,6,23400]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",100540,2.8498706982295601,286526]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",1010,202.95683168316799,204986.4]
["1077000000-E","57 STONE","","",1565,29.103130990415298,45546.400000000001]
["1099500000-E","SHALLOW UNDERCUT","","",6500,9.0296153846153793,58692.5]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",245680,18.391028980788001,4518308]
["1110000000-E","STABILIZER AGGREGATE","","",2000,31.5975,63195]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",527522,2.2836035274358202,1204651.1000000001]
["1121000000-E","AGGREGATE BASE COURSE","","",151200,25.259966931216901,3819307]
["1176000000-E","SOIL CEMENT BASE","","",100540,2.59948279291824,261352]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",2760,192.63333333333301,531668]
["1209000000-E","ASPHALT CURING SEAL","","",30170,3.2921113689095098,99323]
["1220000000-E","INCIDENTAL STONE BASE","","",4996,27.8175120096077,138976.29]
["1231000000-E","SHOULDER BORROW","","",5600,9.24,51744]
["1275000000-E","PRIME COAT","","",14283,3,42849]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",418520,3.33,1393671.6]
["","","(1-1/2\")","",403006,3.9947889609584002,1609923.92]
["","","(3\")","",1650,5.3,8745]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 3/4\")","",125,36.99,4623.75]
["","","(1-1/2\" TO 3\")","",22700,2.1,47670]
["1330000000-E","INCIDENTAL MILLING","","",23090,13.5021221307926,311764]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",130430,50.526397301234397,6590158]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",124280,52.323688445445796,6502788]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",58670,47.353707175728701,2778242]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",101626,66.649309723889601,6773302.75]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",54597,73.3547931205011,4004951.64]
["1575000000-E","ASP FOR PLANT MIX","","",21378,508.34186640471501,10867332.42]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",4193,660.46282136894797,2769320.61]
["1662000000-E","OG ASP FRICT FC-1 MOD","","",17687,98.863975801436098,1748607.14]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",6012,44.189499334663999,265667.27]
["1704000000-E","PATCHING EXIST PVMT","","",190,376.68552631578899,71570.25]
["1735000000-E","REP JNT CONC PVT SLABS","","",204,515,105060]
["1736000000-E","SELECT MAT'L, CLASS IV","","",71,45,3195]
["1737000000-E","PATCHING CONC PVMT SPALLS","","",3512,72.39,254233.68]
["1820000000-E","AST, FOG SEAL","","",14438,0.4,5775.2]
["1840000000-E","MILLED RUMBLE STRIPS","","",409466,0.28872944273760998,118224.89]
["1847000000-E","******\"PCC PVMT THRU LNS","(13\")","",307732,55.5,17079126]
["1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR & SEALING","",494886,1.89,935334.54]
["1891000000-E","GENERIC PAVING ITEM (SY)","DIAMOND GRINDING PCC PAVEMENT","",472626,6.15,2906649.9]
["1924000000-N","FIELD LAB RENTAL, PCCP","","",1,200000,200000]
["1925000000-E","MILL RUMBLE STRPS (CONC SHLDR)","","",6511,0.81,5273.91]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",4,210,840]
["2022000000-E","SUBDRAIN EXCAVATION","","",5680,22.433186619718299,127420.5]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",16550,3.6776132930513601,60864.5]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",118,59.15,6979.7]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",2811,63.131020988971898,177461.3]
["2044000000-E","6\" PERF SUBDRN PIPE","","",17050,9.9692961876832804,169976.5]
["2070000000-N","SUBDRN PIPE OUTLET","","",36,316.48055555555601,11393.3]
["2077000000-E","6\" OUTLET PIPE","","",215,55.791162790697697,11995.1]
["2099000000-E","SHOULDER DRAIN","","",55893,6.5359195248063298,365312.15]
["2110000000-E","4\" SHOULDER DRAIN PIPE","","",55893,0.58612885334478004,32760.5]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",4218,13.572190611664301,57247.5]
["2132000000-N","CONC PAD SHLDR DRN OUTLET","","",31,298.658064516129,9258.4]
["2143000000-E","BLOTTING SAND","","",30,32.56,976.8]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",6,250,1500]
["2209000000-E","ENDWALLS","","",93.1,1074.0283566057999,99992.04]
["2220000000-E","REINF ENDWALLS","","",82.8,1414.7888888888899,117144.52]
["2253000000-E","PIPE COLLARS","","",33.29,1311.82427155302,43670.63]
["2264000000-E","PIPE PLUGS","","",2.66,787.27819548872196,2094.16]
["2275000000-E","FLOWABLE FILL","","",155,414.66399999999999,64272.92]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",782,2503.4239897698199,1957677.56]
["2297000000-E","MASNRY DRAINAGE STRUCT","","",20,671.3,13426]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",530.94000000000005,264.62879044713202,140502.01]
["2352000000-N","FRAME W/GRATE 840.***** STD","(20)","",1,1052.3,1052.3]
["2354000000-N","FRAME W/GRATE 840.22 STD","","",3,856.83333333333303,2570.5]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",49,807.02408163265295,39544.18]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",201,732.99398009950198,147331.79]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",287,536.82442508710801,154068.60999999999]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",12,384.64083333333298,4615.6899999999996]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",3,1081.3800000000001,3244.14]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",19,741.57,14089.83]
["","","(F)","",68,759.27352941176503,51630.6]
["","","(G)","",81,754.98716049382699,61153.96]
["2396000000-N","FRAME W/COVER STD 840.54","","",59,476.39711864406797,28107.43]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",2,763.91,1527.82]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",37,606.69810810810804,22447.83]
["2462000000-E","**\" SLUICE GATE","(18\")","",6,6000,36000]
["","","(24\")","",1,15000,15000]
["","","(30\")","",2,15000,30000]
["","","(36\")","",4,12000,48000]
["","","(8\")","",7,1236.77,8657.39]
["2473000000-N","GENERIC DRAINAGE ITEM (EA)","DRAINAGE STRUCTURE REPAIR","",8,3300,26400]
["","","REMOVE & REPLACE CONC APRON","",16,3234.1875,51747]
["","","REMOVE AND REPLACE","CONCRETE APRON",1,13800,13800]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 18\")","",90,26.25,2362.5]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",5005,17.400159840159802,87087.8]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",29980,19.351400933956,580155]
["2556000000-E","SHOULDER BERM GUTTER","","",37651,22.679972377891701,853923.64]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",2590,42.796525096525102,110843]
["2591000000-E","4\" CONC SIDEWALK","","",7762,46.014480803916499,357164.4]
["2605000000-N","CONC CURB RAMPS","","",58,1830.7979310344799,106186.28]
["2612000000-E","6\" CONC DRIVEWAY","","",420,56.2,23604]
["2613000000-N","REM & REP CURB RAMPS","","",4,10925,43700]
["2619000000-E","4\" CONC PAVED DITCH","","",429,144.48648018648001,61984.7]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",5700,58.038947368420999,330822]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",1960,70.930000000000007,139022.79999999999]
["2724000000-E","PC REINF BARRIER SNGL FC","","",6320,102.94968354430399,650642]
["2738000000-E","GENERIC PAVING ITEM (SY)","7\" CONCRETE TRUCK APRON","",110,64.45,7089.5]
["2752000000-E","GENERIC PAVING ITEM (LF)","MEDIAN HAZARD PROTECTION","",120,126.01,15121.2]
["2800000000-N","ADJ CATCH BASINS","","",6,1863.86666666667,11183.2]
["2815000000-N","ADJ DROP INLETS","","",5,1507.242,7536.21]
["2830000000-N","ADJ MANHOLES","","",6,1459.1033333333301,8754.6200000000008]
["2860000000-N","CONVERT CB TO JB","","",2,1689.09,3378.18]
["2905000000-N","CONVERT DI TO JB","","",3,1689.07,5067.21]
["2950000000-N","CONVERT JB TO DI","","",2,1500,3000]
["3000000000-N","IMPACT ATTEN TYPE 350","","",20,14185.084000000001,283701.68]
["3030000000-E","STL BEAM GUARDRAIL","","",79987.5,16.1870527269886,1294761.8799999999]
["3045000000-E","SBGR SHOP CURVED","","",587.5,18.339795744680799,10774.63]
["3105000000-N","SBGR TERM SECT","","",6,878.19,5269.14]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",60,14.08,844.8]
["3180000000-N","GR ANCHOR TYPE **********","(III MOD)","",4,2300,9200]
["3210000000-N","GR END TYPE CAT-1","","",57,607.36666666666702,34619.9]
["3215000000-N","GR ANCHOR TYPE III","","",3,1805.7166666666701,5417.15]
["3287000000-N","GR END TYPE TL-3","","",117,2813.74324786325,329207.96000000002]
["3317000000-N","GR ANCHOR TYPE B-77","","",107,1754.0891588785,187687.54]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",275,6,1650]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",8023,0.75782126386638005,6080]
["3365000000-E","REMOVE EXISTING GUIDERAIL","","",1700,1.58,2686]
["3380000000-E","TEMP STL BM GUARDRAIL","","",1325,7.02830188679245,9312.5]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",6,600,3600]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-3)","",11,1527.27272727273,16800]
["3389200000-E","CABLE GUIDERAIL","","",27650,6.7145027124774002,185656]
["3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",75,63.117333333333299,4733.8]
["3389600000-N","CBL GUIDERAIL ANCH UNIT","","",28,1728.2285714285699,48390.400000000001]
["3420000000-E","GENERIC GUARDRAIL ITEM (LF)","VINYL COATED GLARE SCREEN","(GUARDRAIL MOUNTED)",525,26.25,13781.25]
["3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNITS,","TYPE CAT-1",3,100,300]
["","","TEMPORARY GUARDRAIL END UNITS,TYPE CAT-1","",1,400,400]
["3500000000-E","WOVEN WIRE FENCE **\" FAB","(48\")","",16090,3.25,52292.5]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",102130,3.35496426123568,342642.5]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",7366,25.0895194135216,184809.4]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",2083,35.9057609217475,74791.7]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",5031,6.5189823096799797,32797]
["3542000000-E","MET LINE PST 48\" CL FEN","","",399,55.691854636591501,22221.05]
["3548000000-E","MET TERM PST 48\" CL FEN","","",76,191.81723684210499,14578.11]
["3557000000-E","ADDITIONAL BARBED WIRE","","",300,1.0900000000000001,327]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(58\", 12', 24')","",4,800,3200]
["3572000000-E","CHAIN LINK FENCE RESET","","",85,10,850]
["3575000000-E","GENERIC FENCING ITEM (LF)","STEEL PIPE HANDRAIL FOR","RETAINING WALL",80,173.26,13860.8]
["3628000000-E","RIP RAP, CLASS I","","",10238,47.929174643485098,490698.89]
["3635000000-E","RIP RAP, CLASS II","","",2030,16.1114778325123,32706.3]
["3642000000-E","RIP RAP, CLASS A","","",680,48.91,33258.800000000003]
["3649000000-E","RIP RAP, CLASS B","","",7950,46.7093974842767,371339.71]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",60711,1.53135708520696,92970.22]
["3659000000-N","PREFORMED SCOUR HOLES","","",4,1357.5,5430]
["4048000000-E","REINF CONC FOUNDTN","","",18,975.569444444444,17560.25]
["4054000000-E","PLN CONC FOUNDTN","","",5,193.82400000000001,969.12]
["4057000000-E","OVERHEAD FOOTING","","",410,1041.0387804878001,426825.9]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",20946,5.0009911200229196,104750.76]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",1836,5.3986002178649199,9911.83]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",7848,6.4954115698267101,50975.99]
["4080000000-N","SUPPORT, BARR LARGE","","",9,800,7200]
["4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(12+50 -LSB-)","",1,51704.75,51704.75]
["","","(20+50 -YRPC-)","",1,56013.51,56013.51]
["","","(22+50 -LACFLY-)","",1,44000,44000]
["","","(25+00 -YRPA-)","",1,61399.360000000001,61399.360000000001]
["","","(26+50 -Y-)","",1,30161.13,30161.13]
["","","(291+50 -L-)","",1,45000,45000]
["","","(294+00 -L- LT)","",1,46000,46000]
["","","(30+25 -Y-)","",1,30161.13,30161.13]
["","","(316+00 -L- LT)","",1,38000,38000]
["","","(328+50 -L-)","",1,26000,26000]
["","","(346+00 -L- LT)","",1,29800,29800]
["","","(357+00 -L-)","",1,16000,16000]
["","","(383+50 -L-)","",1,42000,42000]
["","","(385+00 -L- LT)","",1,32000,32000]
["","","(419+00 -L- LT)","",1,27500,27500]
["","","(428+50 -L-)","",1,21500,21500]
["","","(450+00 -L- LT)","",1,29500,29500]
["","","(456+00 -L-)","",1,21000,21000]
["","","(468+50 -L-)","",1,16000,16000]
["","","(488+00 -L- LT)","",1,48500,48500]
["","","(507+00 -L- LT)","",1,53500,53500]
["","","(512+00 -L-)","",1,25500,25500]
["","","(529+50 -L- LT)","",1,22500,22500]
["","","(540+00 -L-)","",1,23000,23000]
["4096000000-N","SIGN ERECTION, TYPE D","","",28,146.61500000000001,4105.22]
["4102000000-N","SIGN ERECTION, TYPE E","","",355,90.653183098591597,32181.88]
["4108000000-N","SIGN ERECTION, TYPE F","","",44,95.662272727272693,4209.1400000000003]
["4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",27,874.44,23609.88]
["","","(B)","",10,322.36099999999999,3223.61]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",39,655.25256410256395,25554.85]
["","","(B)","",3,636.52,1909.56]
["4114000000-N","SIGN ERECTION, MILEMARKERS","","",50,75,3750]
["4115000000-N","SIGN ERECTION, OVERLAY (OVRHD)","","",112,400,44800]
["4116000000-N","SIGN ERECTION, OVERLAY (GRD MTD)","","",4,400,1600]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",2,700.18,1400.36]
["","","(B)","",2,269.27999999999997,538.55999999999995]
["","","(D)","",3,475.73333333333301,1427.2]
["4116200000-N","SIGN ERECTION, REPOSIT OVRHD","","",13,500,6500]
["4138000000-N","DISPOSE SUPPORT, STL BM","","",14,275.83428571428601,3861.68]
["4149000000-N","DISPOSE SIGN SYST OVRHD","","",2,7862.84,15725.68]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",17,404.01529411764699,6868.26]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",217,9.7196313364055307,2109.16]
["4158000000-N","DISPOSE SIGN SYST WOOD","","",5,1.9,9.5]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",63,2.5646031746031701,161.57]
["4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",45,58.088000000000001,2613.96]
["4236000000-N","DISPOSE SIGN, A & B (GRD MTD)","","",7,16.875714285714299,118.13]
["4238000000-N","DISPOSE SIGN, D, E, F","","",166,2.6054216867469902,432.5]
["4241000000-N","DISPOSE SIGN, OVERLAY OVRHD","","",35,1.5,52.5]
["4242000000-N","DISPOSE SIGN, OVERLAY GM","","",2,1.5,3]
["4251000000-N","DISPOSE LIGHT SYSTEM","","",6,1472.44,8834.64]
["4263000000-N","DISPOSE WALKWAY","","",6,817.85,4907.1000000000004]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",6842,16.103019584916701,110176.86]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",5977,15.272116446377799,91281.44]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",1429,10.6130860741777,15166.1]
["4415000000-N","FLASHING ARROW BOARD","","",29,2274.4,65957.600000000006]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",29,9655.8206896551692,280018.8]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",8,100,800]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",15,9055,135825]
["4424000000-N","WZ PRESENCE LIGHTING","","",45,4041.5,181867.5]
["4430000000-N","DRUMS","","",2586,52.208043310131501,135010]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",103,177.252427184466,18257]
["4435000000-N","CONES","","",441,18.580498866213201,8194]
["4445000000-E","BARRICADES (TYPE III)","","",4790,29.0186388308977,138999.28]
["4447000000-E","PED CHANNEL DEVICES","","",52,60,3120]
["4455000000-N","FLAGGER","","",5309,316.607965718591,1680871.69]
["4465000000-N","TEMP CRASH CUSHIONS","","",14,5854.3685714285702,81961.16]
["4470000000-N","REM & RES CRASH CUSHION","","",14,2789.37142857143,39051.199999999997]
["4480000000-N","TMA","","",23,8218.3091304347799,189021.11]
["4485000000-E","PORT CONC BARRIER","","",7573,23.652514195167001,179120.49]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",6270,38.979999999999997,244404.6]
["4500000000-E","REM & RES PORT CONC BARRIER","","",6392,7.7790738423028802,49723.839999999997]
["4505000000-E","REM & RES PORT CONC BARR, ANCH","","",4379,10.1,44227.9]
["4507000000-E","WATER FILLED BARRIER","","",2953,65.5,193421.5]
["4508000000-E","REM & RES H2O FILL BARR","","",3100,10.5,32550]
["4510000000-N","LAW ENFORCEMENT","","",564,101.525531914894,57260.4]
["4516000000-N","SKINNY DRUM","","",296,42.516891891891902,12585]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",20,98,1960]
["4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","PROTECTIVE CANOPY","",1,57450,57450]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",6,3000,18000]
["","","DOUBLE LANE CLOSURE","",155,3712,575360]
["","","LANE CLOSURE","",165,3162.5,521812.5]
["","","RAMP/LOOP CLOSURE","",12,2645,31740]
["","","RAMP/LOOP CLOSURE (TYPE A)","",40,2160,86400]
["","","RAMP/LOOP CLOSURE (TYPE B)","",1,6412,6412]
["","","RAMP/LOOP CLOSURE (TYPE C)","",1,2362,2362]
["","","RAMP/LOOP TRAFFIC CONTROL","",146,2565,374490]
["","","SINGLE LANE CLOSURE","",35,2937,102795]
["","","TEMPORARY CURB RAMPS","",6,1850,11100]
["","","TRIPLE LANE CLOSURE","",194,3940,764360]
["4650000000-N","TEMP RAISED PVMT MRKS","","",3969,6.7394507432602699,26748.880000000001]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",111415,0.87740214513306003,97755.76]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",63808,1.1798674147442301,75284.98]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",226838,1.0878285825126299,246760.86]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",57670,1.2937497832495199,74610.55]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",11977,2.3089621775068898,27654.44]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",1757,3.5202162777461599,6185.02]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",23133,2.6748614533350601,61877.57]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",11094,2.4905336217775398,27629.98]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",9584,9.7304559682804701,93256.69]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",212,151.216037735849,32057.8]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",864,179.27209490740699,154891.09]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",1388,3.9575504322766601,5493.08]
["","","(IV)","",21283,2.3839923882911198,50738.51]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",1434,4.7703765690376603,6840.72]
["","","(IV)","",425,3.32,1411]
["4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",434,4.42,1918.28]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",120,4,480]
["4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",42,500,21000]
["","","(IV)","",2,812.19,1624.38]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",634590,0.27379950834396999,173750.43]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",790763,0.35299562574373999,279135.88]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",18826,0.75823329438011,14274.5]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",93134,0.94201516095089,87733.64]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",6376,3.2327195734002498,20611.82]
["4840000000-N","PAINT PVT MKG CHARACTER","","",240,66.6726666666667,16001.44]
["4845000000-N","PAINT PVT MKG SYMBOL","","",976,62.701782786885303,61196.94]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",40621,1.13152704266266,45963.76]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",460353,1.21597193892513,559776.32999999996]
["4847050000-E","POLYUREA LINES (8\", 20 MILS)","","",1009,2.0299999999999998,2048.27]
["4847070000-E","POLYUREA LINES (12\", 20 MILS)","","",31321,2.3362814086395698,73174.67]
["4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",22980,0.7,16086]
["4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",200,5,1000]
["4848000000-E","WZ TRAF PATTERN MASKING","","",172284,0.2,34456.800000000003]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",543399,0.27356220751234001,148653.43]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",283920,0.62250260636799004,176740.94]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",1365,2.1398901098901102,2920.95]
["4865000000-E","LINE REMOVAL 12\" WIDE","","",31875,0.80496941176471004,25658.400000000001]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",1175,4.4765191489361698,5259.91]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",224,65.332723214285707,14634.53]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","EPOXY PAVEMENT MARKING LINES","(BLACK) 6\"",54201,0.45,24390.45]
["","","HOT SPRAY THERMOPLASTIC","PAVEMENT MARKING LINES, 6\" 50 MILS",121987,0.72,87830.64]
["","","","PAVEMENT MARKING LINES,12\" 50 MILS",16802,1.73,29067.46]
["","","HOT SPRAY THERMOPLASTIC PAVEMENT","MARKING LINES (12\", 50MILS)",11787,2,23574]
["","","","MARKING LINES (6\", 50MILS)",204673,0.7,143271.1]
["4895000000-N","GENERIC PVMT MARKING ITEM (EA)","IN LANE ROUTE SHIELDS (I-85)","",9,2800,25200]
["4900000000-N","PERM RAISED PVMT MARKERS","","",1230,5.6043739837398396,6893.38]
["4905000000-N","SNOWPLB PVMT MRKER","","",14454,34.498098796180997,498635.52000000002]
["4915000000-E","7' U-CHANNEL POSTS","","",3,57.77,173.31]
["4955000000-N","OBJECT MARKERS (END OF RD)","","",3,42,126]
["4960000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","REPLACE EXISTING BARRIER","DELINEATOR",537,28.75,15438.75]
["","","REPLACEMENT OF EXISTING","BARRIER DELINEATORS",77,25,1925]
["5000000000-E","***' HIGH MOUNT STANDARD","(60')","",2,15500,31000]
["5005000000-E","80' HIGH MOUNT STANDARD","","",12,17250,207000]
["5010000000-E","100' HIGH MOUNT STANDARD","","",6,21448.241666666701,128689.45]
["5015000000-E","120' HIGH MOUNT STANDARD","","",12,24924.143333333301,299089.71999999997]
["5020000000-N","PORTABLE DRIVE UNIT","","",2,4823.2550000000001,9646.51]
["5025000000-E","HIGH MOUNT FOUNDS","","",233.4,765.45921165381299,178658.18]
["5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",2,3275,6550]
["","","(45' TA, 15' ARM)","",6,3257.58,19545.48]
["5070000000-N","STD FOUNDAT ***********","(TYPE R1)","",6,776.26,4657.5600000000004]
["","","(TYPE R2)","",2,884.99,1769.98]
["5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",5,770,3850]
["5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",125,28,3500]
["5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",2669,6.39324466092169,17063.57]
["","","(3\")","",495,7,3465]
["","","(4\")","",120,7.75,930]
["5160000000-E","ELECT DUCT JA, SIZE *****","(2\")","",240,15,3600]
["","","(3\")","",1144,15.734965034965001,18000.8]
["","","(4\")","",1564,17.246521739130401,26973.56]
["","","(6\")","",105,26,2730]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",2100,3.05,6405]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",3803,4.3879253221141203,16687.28]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2)","",3215,4.75,15271.25]
["5185000000-E","**-2 W/G FEEDER CIRCUIT","(2)","",220,6.3,1386]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2, 1.5)","",4105,7.3,29966.5]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",12547,7.4253989001354901,93166.48]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",9895,7.35,72728.25]
["5220000000-E","**-2 W/G FEEDER N *****\"","(2, 1.5)","",1925,9.1,17517.5]
["5240000000-N","ELEC JB ************","(CS36)","",1,1737.35,1737.35]
["","","(CSJB, 36\" X 24\")","",5,1250,6250]
["","","(HM18)","",4,580.91999999999996,2323.6799999999998]
["","","(HMJB, 18\" X 12\")","",21,490,10290]
["","","(HMJB, 30\" X 17\")","",5,740,3700]
["","","(HMJB, 36\" X 24\")","",4,1250,5000]
["","","(IG18)","",8,580.94000000000005,4647.5200000000004]
["","","(IG30)","",2,868.68,1737.36]
["","","(IGJB, 18\" X 12\")","",35,490,17150]
["","","(IGJB, 30\" X 17\")","",5,740,3700]
["","","(IGJB, 36\" X 24\")","",8,1250,10000]
["","","(LS18)","",6,580.94000000000005,3485.64]
["","","(LSJB, 18\" X 12\")","",2,490,980]
["5252000000-N","UNDERPASS LUMINARIES *****","(TYPE PM, LED, 62W)","",10,525,5250]
["5253000000-N","UNDERPASS CIRCUITRY *************","LAWNDALE DRIVE, UPL-1","",1,8600,8600]
["5255000000-N","PORTABLE LIGHTING","","",5,100362.39599999999,501811.98]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","LUMINAIRE STORAGE","",1,1004.4,1004.4]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","100' HIGH MOUNT LUMINAIRE - LED","",36,1642.06833333333,59114.46]
["","","120' HIGH MOUNT LUMINAIRE - LED","",96,1613.5333333333299,154899.20000000001]
["","","240/480V LIGHTING CONTROL SYSTEM","",5,8340,41700]
["","","60' HIGH MOUNT LUMINAIRE - LED","",8,1160,9280]
["","","80' HIGH MOUNT LUMINAIRE - LED","",96,1160,111360]
["","","COMMUNICATION GATEWAY","",5,4575,22875]
["","","CONTROL NODE","",224,130,29120]
["","","INSTALL ROADWAY LIGHT STANDARD","LUMINAIRE",12,173.74,2084.88]
["","","RELOCATE HIGH MOUNT LIGHT STANDARD","",2,5755.07,11510.14]
["","","REMOVE LIGHT STANDARD","",28,260.61,7297.08]
["","","REMOVE LIGHT STANDARD FOUNDATION","",28,1031.57,28883.96]
["","","ROADWAY LIGHT STANDARD LUMIN-","AIRE - 285W LED",2,815,1630]
["","","SMART CONTROL NODE","",14,168.31,2356.34]
["5325000000-E","**\" WATER LINE","(36\")","",1215,433.36,526532.4]
["5325300000-E","3\" WATER LINE","","",7,178.97,1252.79]
["5325400000-E","4\" WATER LINE","","",15,193.91,2908.65]
["5325600000-E","6\" WATER LINE","","",1783,69.234924284913106,123445.87]
["5325800000-E","8\" WATER LINE","","",1861,119.55120902740499,222484.8]
["5326200000-E","12\" WATER LINE","","",3888,103.680823045267,403111.04]
["5326600000-E","16\" WATER LINE","","",1275,181.74883137254901,231729.76]
["5327000000-E","20\" WATER LINE","","",1581,184.54,291757.74]
["5327400000-E","24\" WATER LINE","","",2526,217.09,548369.34]
["5328000000-E","30\" WATER LINE","","",476,330.77,157446.51999999999]
["5329000000-E","DI H2O PIPE FITTINGS","","",120955,8.4297333719151801,1019618.4]
["5534000000-E","**\" VALVE","(36\")","",4,66882.31,267529.24]
["5540000000-E","6\" VALVE","","",19,2549.2368421052602,48435.5]
["5546000000-E","8\" VALVE","","",6,2550.6550000000002,15303.93]
["5558000000-E","12\" VALVE","","",7,4012.0928571428599,28084.65]
["5558600000-E","16\" VALVE","","",1,8281.6200000000008,8281.6200000000008]
["5559000000-E","20\" VALVE","","",3,15726.78,47180.34]
["5559400000-E","24\" VALVE","","",5,20445.96,102229.8]
["5560000000-E","30\" VALVE","","",4,44203.16,176812.64]
["5571600000-E","6\" TAPPING SLEEVE & VALVE","","",8,6714.83,53718.64]
["5571800000-E","8\" TAPPING SLEEVE & VALVE","","",2,7555.94,15111.88]
["5572200000-E","12\" TAPPING SLEEVE & VALVE","","",1,16000,16000]
["5588000000-E","*\" AIR RELEASE VALVE","(12\")","",1,8200,8200]
["5589200000-E","2\" AIR RELEASE VALVE","","",10,10873.91,108739.1]
["5606800000-E","8\" BLOW OFF","","",2,7852.32,15704.64]
["5648000000-N","RELOCATE WATER METER","","",70,1915.1327142857101,134059.29]
["5649000000-N","RECONNECT WATER METER","","",10,1191.0229999999999,11910.23]
["5656000000-E","**\" RPZ BACKFLOW PREVNT ASMBLY","(3/4\")","",1,5690.17,5690.17]
["5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1\")","",1,1981.19,1981.19]
["5656200000-E","2\" RPZ BACKFLOW PREVNT ASMBLY","","",1,5921.6,5921.6]
["5656600000-E","6\" RPZ BACKFLOW PREVNT ASMBLY","","",1,14370.35,14370.35]
["5666000000-N","FIRE HYDRANT","","",2,5688.85,11377.7]
["5672000000-N","RELOCATE FIRE HYDRANT","","",44,2612.5463636363602,114952.04]
["5673000000-E","FIRE HYDRANT LEG","","",1140,39.718771929824598,45279.4]
["5686000000-E","**\" H2O SERVICE LINE","(2\")","",26,53.73,1396.98]
["5686500000-E","WATER SERVICE LINE","","",2365,25.2120718816068,59626.55]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",8131,145.19928422088299,1180615.3799999999]
["5691400000-E","10\" SANITARY GRAVITY SEWER","","",180,189.88,34178.400000000001]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",1257,231.22946698488499,290655.44]
["5691800000-E","20\" SANITARY GRAVITY SEWER","","",1077,341.55198700092899,367851.49]
["5709700000-E","16\" FORCE MAIN SEWER","","",762,210.83,160652.46]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",42,1875.2023809523801,78758.5]
["5768500000-E","SEWER SERVICE LINE","","",1507,31.710816191108201,47788.2]
["5769000000-E","DI SEWER PIPE FITTINGS","","",3715,8.3800000000000008,31131.7]
["5775000000-E","4' DIA UTILITY MANHOLE","","",54,4328.2014814814802,233722.88]
["5776000000-E","5' DIA UTILITY MANHOLE","","",8,6892.0150000000003,55136.12]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",222,312.69702702702699,69418.740000000005]
["5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",56,648.49714285714299,36315.839999999997]
["5798000000-E","ABANDON **\" UTILITY PIPE","(15\")","",222,42.92,9528.24]
["","","(21\")","",820,43.8409756097561,35949.599999999999]
["","","(36\")","",2109,85.557467994310102,180440.7]
["","","(8\")","",2272,15.15,34420.800000000003]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",520,10,5200]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",2945,17.617419354838699,51883.3]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",185,22.08,4084.8]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",2548,19.883375196232301,50662.84]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",1775,26.09,46309.75]
["5812000000-E","ABANDON 20\" UTILITY PIPE","","",1282,34.192683307332302,43835.02]
["5813000000-E","ABANDON 24\" UTILITY PIPE","","",1780,41.769123595505597,74349.039999999994]
["5814000000-E","ABANDON 30\" UTILITY PIPE","","",370,20.99,7766.3]
["5815000000-N","REMOVE WATER METER","","",61,1356.9488524590199,82773.88]
["5815500000-N","REMOVE FIRE HYDRANT","","",9,1829.41333333333,16464.72]
["5816000000-N","ABANDON UTILITY MANHOLE","","",53,1291.4216981132099,68445.350000000006]
["5828000000-N","REMOVE UTILITY MANHOLE","","",6,1774.79,10648.74]
["5835000000-E","**\" ENCASEMENT PIPE","(48\")","",640,428.98,274547.20000000001]
["5835600000-E","12\" ENCASEMENT PIPE","","",80,130,10400]
["5835800000-E","18\" ENCASEMENT PIPE","","",640,234.48750000000001,150072]
["5835900000-E","20\" ENCASEMENT PIPE","","",1680,131.21892857142899,220447.8]
["5836200000-E","30\" ENCASEMENT PIPE","","",1280,228.67250000000001,292700.79999999999]
["5836400000-E","36\" ENCASEMENT PIPE","","",1410,298.99,421575.9]
["5872500000-E","BORE & JACK **\"","(12\")","",80,625,50000]
["","","(18\")","",440,1328.6,584584]
["","","(20\")","",100,765,76500]
["5875000000-N","CONC PIERS","","",2,3462.16,6924.32]
["5882000000-N","GENERIC UTILITY ITEM (EA)","12\" INSERT VALVE","",2,21000,42000]
["","","REMOVE EXISTING VAULT","",1,4277.8100000000004,4277.8100000000004]
["5888000000-E","GENERIC UTILITY ITEM (LF)","ADJUST 48\" FRP MANHOLE RISER","",52,1852.42,96325.84]
["5912000000-N","GENERIC UTILITY ITEM (LS)","RELOCATE 3\" PRESSURE REDUCING","VALVE WITH MANHOLE",1,7783.21,7783.21]
["","","RELOCATE 3\" WM ASSEMBLY WITH","NEW VAULT",1,27825.62,27825.62]
["6000000000-E","TEMP SILT FENCE","","",285275,1.7924765577074799,511348.75]
["6006000000-E","EROS CONTRL STONE CL A","","",10395,27.6495719095719,287417.3]
["6009000000-E","EROS CONTRL STONE CL B","","",58110,16.263337635518798,945062.55]
["6012000000-E","SEDIMENT CONTROL STONE","","",86880,0.71301910681400005,61947.1]
["6015000000-E","TEMP MULCHING","","",859,824.00906868451705,707823.79]
["6018000000-E","SEED FOR TEMP SEEDING","","",36600,2.35775956284153,86294]
["6021000000-E","FERT FOR TEMP SEEDING","","",190.5,728.28671916010501,138738.62]
["6024000000-E","TEMP SLOPE DRAINS","","",57525,10.8257827031725,622753.15]
["6029000000-E","SAFETY FENCE","","",10600,2.52566037735849,26772]
["6030000000-E","SILT EXCAVATION","","",238520,2.8082051819553899,669813.1]
["6036000000-E","MATTING FOR EROS CONTROL","","",892700,0.76178671446174995,680047]
["6037000000-E","COIR FIBER MAT","","",7450,4.5507382550335604,33903]
["6038000000-E","PERM SOIL REINF MAT","","",14645,4.4388357801297396,65006.75]
["6042000000-E","1/4\" HARDWARE CLOTH","","",43835,4.1435873160716303,181634.15]
["6045000000-E","**\" TEMP PIPE","(18\")","",380,25.558157894736802,9712.1]
["","","(30\")","",65,77,5005]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",725,58.412413793103397,42349]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",1125,25.915199999999999,29154.6]
["6069000000-E","STILLING BASINS","","",4030,8.0384615384615401,32395]
["6070000000-N","SPECIAL STILLING BASINS","","",52,366.87884615384598,19077.7]
["6071010000-E","WATTLE","","",1470,16.258775510204099,23900.400000000001]
["6071012000-E","COIR FIBER WATTLE","","",31050,5.57829307568438,173206]
["6071013000-E","WATTLE BARRIER","","",30070,14.25,428497.5]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",370,11.55,4273.5]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",23580,7.9007739609838801,186300.25]
["6071030000-E","COIR FIBER BAFFLE","","",54385,3.2582449204744002,177199.65]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",145,1095.01262068966,158776.82999999999]
["","","(2\")","",31,867.34516129032295,26887.7]
["","","(2-1/2\")","",8,1012.2975,8098.38]
["","","(3\")","",5,1693.884,8469.42]
["","","(4\")","",6,1147.45,6884.7]
["6084000000-E","SEEDING AND MULCHING","","",720,1680.7584444444401,1210146.08]
["6087000000-E","MOWING","","",419,111.50105011933201,46718.94]
["6090000000-E","SEED FOR REPAIR SEEDING","","",8650,2.6252023121387298,22708]
["6093000000-E","FERT FOR REPAIR SEEDING","","",32,936.20500000000004,29958.560000000001]
["6096000000-E","SEED FOR SUPP SEEDING","","",17275,2.77997105643994,48024]
["6108000000-E","FERTILIZER TOPDRESSING","","",516.25,792.49869249394703,409127.45]
["6111000000-E","IMPERVIOUS DIKE","","",2020,41.158415841584201,83140]
["6114500000-N","SPECIALIZED HAND MOWING","","",340,72.356764705882398,24601.3]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",475,106.318421052632,50501.25]
["6117500000-N","CONC WASHOUT STR","","",71,790.82816901408501,56148.800000000003]
["6120000000-E","CULVERT DIVERSION CHANNEL","","",8835,20.792733446519499,183703.8]
["6123000000-E","REFORESTATION","","",17,1861.01058823529,31637.18]
["6126000000-E","STREAMBANK REFORESTATION","","",1.21,4685.2231404958702,5669.12]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",8,200,1600]
["","","","DEVICE CLEAN-OUT",16,85,1360]
["","","","DEVICE CLEANOUT",415,76.3903614457831,31702]
["","","FABRIC INSERT INLET PROTECTION DEVICE","",50,131.26,6563]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",135,72.755555555555603,9822]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",38,586.47473684210502,22286.04]
["7060000000-E","SIGNAL CABLE","","",93220,2.3597538081956699,219976.25]
["7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",1,388.9,388.9]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",487,703.99876796714602,342847.4]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",130,821.93899999999996,106852.07]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",30,1144.5136666666699,34335.410000000003]
["7180000000-N","BACKPLATE","","",2,140,280]
["7204000000-N","LOUVER","","",4,191.97,767.88]
["7252000000-E","MESSENGER CABLE (1/4\")","","",65685,1.90479409301972,125116.4]
["7264000000-E","MESSENGER CABLE (3/8\")","","",15587,4.0329075511644303,62860.93]
["7279000000-E","TRACER WIRE","","",102210,0.51458761373643003,52596]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",125,15.474,1934.25]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",13625,7.21721100917431,98334.5]
["","","(2, 2\")","",44150,8.4108890147225406,371340.75]
["","","(3, 2\")","",3035,8.5,25797.5]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",2950,3.1559322033898298,9310]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",3015,12.087645107794399,36444.25]
["","","(2, 2\")","",16710,13.935511669658901,232862.4]
["","","(3, 2\")","",1760,19.5,34320]
["7312000000-N","JUNCTION BOX (***************)","(SPECIAL SIZE, HEAVY-DUTY)","",9,2525,22725]
["","","(SPECIAL-SIZED)","",38,647.49,24604.62]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",315,325.41993650793597,102507.28]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",204,518.03651960784305,105679.45]
["7360000000-N","WOOD POLE","","",62,1076.23435483871,66726.53]
["7372000000-N","GUY ASSEMBLY","","",416,429.579759615385,178705.18]
["7384000000-E","***\" RISER WITH **************","(1-1/2\" RISER W/ WEATHERHEAD)","",5,270,1350]
["","","(1.25\", HEAT SHRINK TUBING)","",11,381.1,4192.1000000000004]
["","","(2\", HEAT SHRINK TUBING)","",77,452.08,34810.160000000003]
["7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",4,331.09,1324.36]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",32,323.03468750000002,10337.11]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",100,439.92090000000002,43992.09]
["7432000000-E","2\" RISER WITH TUBING","","",31,498.76903225806501,15461.84]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",38935,8.1961397200462294,319116.7]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",159185,1.74081477526149,277111.59999999998]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",66605,1.32459424968095,88224.6]
["","","(144)","",36370,2.7,98199]
["","","(24)","",153662,1.4342641642045499,220391.9]
["","","(36)","",110230,1.6388877800961601,180654.6]
["","","(48)","",38830,1.64,63681.2]
["7528000000-E","DROP CABLE","","",90215,1.4044161170537099,126699.4]
["7540000000-N","SPLICE ENCLOSURE","","",190,1793.38063157895,340742.32]
["7541000000-N","MOD SPLICE ENCLOSURE","","",7,2152.88,15070.16]
["7552000000-N","INTERCONNECT CENTER","","",235,1411.2453617021299,331642.65999999997]
["7566000000-N","DELINEATOR MARKER","","",105,86.335809523809502,9065.26]
["7575142200-N","NEW ELECTRICAL SERVICE","","",10,1270.47,12704.7]
["7575160000-E","REM EXT COMM CABLE","","",36720,0.75880718954248005,27863.4]
["7575180000-N","CABLE TRANSFER","","",21,180.67809523809501,3794.24]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",48,9136.2150000000001,438538.32]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",9,13354.833333333299,120193.5]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",1,25279.29,25279.29]
["7613000000-N","SOIL TEST","","",77,1017.31662337662,78333.38]
["7614100000-E","DRILLED PIER FOUND","","",519,817.56312138728299,424315.26]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",10,72.171000000000006,721.71]
["7636000000-N","SIGN FOR SIGNALS","","",89,345.07988764044899,30712.11]
["7642100000-N","TYPE I POST W/ FOUND","","",7,1291.08857142857,9037.6200000000008]
["7642200000-N","TYPE II PED W/ FOUND","","",22,1670.50090909091,36751.019999999997]
["7684000000-N","SIGNAL CABINET FOUND","","",62,971.56129032258104,60236.800000000003]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",16,524.23500000000001,8387.76]
["7687000000-N","MODIFY FOUND FOR CONTRLR CBNT","","",6,965.61,5793.66]
["7696000000-N","CONTLRS WITH CBNT (**************)","(2070LX, 332)","",133,10833.47,1440851.51]
["","","(2070LX, 336S)","",67,9563.2099999999991,640735.06999999995]
["7708000000-N","DETECTOR CARD (***********)","(MODEL 222)","",946,75.45,71375.7]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",15,12888.3526666667,193325.29]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",120,132.29083333333301,15874.9]
["7901000000-N","CABINET BASE EXTENDER","","",87,377.907931034483,32877.99]
["7901010000-N","CABINET BASE ADAPTER","","",7,411.2,2878.4]
["7912000000-N","BEACON CNTRL ASSM & CBNT *****","(TYPE F3)","",2,1600,3200]
["7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,1888.96,1888.96]
["7960000000-N","METAL POLE FOUND REMVL","","",11,1039.52727272727,11434.8]
["7972000000-N","METAL POLE REMOVAL","","",11,551.25181818181795,6063.77]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","10KVA SINGLE PHASE TRANSFORMER","",2,1825,3650]
["","","2.4 GHZ ETHERNET RADIO","",2,4374.1099999999997,8748.2199999999993]
["","","5/8\" X 10' GROUNDING ELECTRODE","",120,75.625,9075]
["","","60 FT CCTV WOOD POLE","",1,2527.96,2527.96]
["","","CCTV CABINET (336A)","",6,4550.6499999999996,27303.9]
["","","CCTV CABINET (NEMA)","",1,3369.99,3369.99]
["","","CCTV CABINET DISCONNECT","",2,428.74,857.48]
["","","CCTV CAMERA ASSEMBLY","",13,5502.95,71538.350000000006]
["","","CCTV CAMERA ASSEMBLY","",40,4336.88,173475.20000000001]
["","","CCTV EXTENSION POLE","",1,1190,1190]
["","","CCTV METAL POLE","",19,5423.1,103038.9]
["","","CCTV METAL POLE (50')","",7,7375,51625]
["","","CCTV TEST CABINET","",1,11026.65,11026.65]
["","","CCTV WOOD POLE","",3,1603.8,4811.3999999999996]
["","","CENTRAL MEDIA CONVERTER","",1,1200,1200]
["","","COMMUNICATIONS RACK","",2,4277.07,8554.14]
["","","COMPUTER WORKSTATION","",4,4565.75,18263]
["","","CONSOLES","",2,29882.41,59764.82]
["","","DIGITAL DISPLAY MONITOR","",10,6540.35,65403.5]
["","","DIGITAL DISPLAY MONITOR (RELO-CATE)","",4,284.27999999999997,1137.1199999999999]
["","","DMS","",4,70000,280000]
["","","DMS ACCESS LADDER","",4,6000,24000]
["","","DMS PEDESTAL STRUCTURE","",4,31000,124000]
["","","EQUIPMENT CABINET DISCONNECT","",13,610,7930]
["","","ETEHERNET EDGE SWITCH","",5,2333.48,11667.4]
["","","ETHERNET CORE SWITCH","",1,72738.45,72738.45]
["","","ETHERNET EDGE SWITCH","",221,1391.0057918552,307412.28000000003]
["","","FIELD EQUIPMENT CABINET","",7,3815,26705]
["","","FIREWALL","",1,5016.1499999999996,5016.1499999999996]
["","","FURNISH 2.4 GHZ ETHERNET RADIO","",1,2570.96,2570.96]
["","","FURNISH 2018 ENHANCED CONFLICTMONITOR","",10,1018.26,10182.6]
["","","FURNISH 2070 CONTROLLER TESTER","",2,4241.22,8482.44]
["","","FURNISH 2070LX CONTROLLER","",10,1599.37,15993.7]
["","","FURNISH 332 CABINET","",7,7376.74,51637.18]
["","","FURNISH 336S CABINET","",3,2808.84,8426.52]
["","","FURNISH CCTV CABINET","",1,2789.11,2789.11]
["","","FURNISH CCTV CAMERA ASSEMBLY","",1,3135.78,3135.78]
["","","FURNISH CONFLICT MONITOR TESTER","",2,21617.23,43234.46]
["","","FURNISH DETECTOR CARD (MODEL 222)","",48,75.11,3605.28]
["","","FURNISH ETHERNET EDGE SWITCH","",11,1005.35,11058.85]
["","","FURNISH FIBER-OPTIC POWER METER","",2,1882.9,3765.8]
["","","FURNISH OPTICAL LIGHT GENERA- TOR","",4,1056.69,4226.76]
["","","FURNISH VIDEO MONITOR","",1,5194.09,5194.09]
["","","FURNISH VISUAL FAULT LOCATOR","",2,1227.7,2455.4]
["","","GUY ASSEMBLY (AERIAL)","",63,348.4,21949.200000000001]
["","","GUY ASSEMBLY (SIDEWALK)","",38,515.35,19583.3]
["","","HEAT SHRINK TUBING KIT","",130,77.47,10071.1]
["","","HIGH DEFINITION CCTV CAMERA ASSEMBLY","",1,6667.1,6667.1]
["","","ITS FIELD ETHERNET SWITCH","",11,2170,23870]
["","","ITS SERVER","",8,17426.52,139412.16]
["","","ITS SOIL TEST","",7,720,5040]
["","","JUNCTION BOX MARKER","",2,127.8,255.6]
["","","KVM SWITCH","",1,4476.07,4476.07]
["","","LAPTOP COMPUTER","",8,2930.1,23440.799999999999]
["","","METER BASE/DISCONNECT COMBINA-TION PANEL","",11,705,7755]
["","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",3,2055.69,6167.07]
["","","","SYSTEM-MULTIPLE ZONES",1,4960.1000000000004,4960.1000000000004]
["","","MICROWAVE VEHICLE DETECTOR -","SINGLE ZONE",2,1416.74,2833.48]
["","","MODIFY EXISTING ELECTRICAL SERVICE","",124,469.43,58209.32]
["","","MODIFY EXISTING SPLICE","",1,516.51,516.51]
["","","NETWORK VIDEO RECORDER","",1,7959.46,7959.46]
["","","PTZ JOYSTICK","",3,929.72,2789.16]
["","","SMALL FORM FACTOR COMPUTER","",3,6300,18900]
["","","TERMINAL SPLICE CABINET","",9,295.45,2659.05]
["","","TRAVEL TIME DYNAMIC MESSAGE SIGN","",2,35000,70000]
["","","TYPE 332 TEST CONTROLLER WITH CABINET","",1,14000,14000]
["","","TYPE 336 TEST CONTROLLER WITH CABINET","",1,13500,13500]
["","","UPS (TCC)","",1,4613.1099999999997,4613.1099999999997]
["","","VIDEO PROCESSING UNIT","",1,8165,8165]
["","","WIRELESS ACCESS POINT","",1,2311.62,2311.62]
["","","WOOD PEDESTAL","",6,360,2160]
["","","WORKSTATION MONITOR","",19,438.83,8337.77]
["7985000000-N","GENERIC SIGNAL ITEM (LS)","CCTV SOFTWARE (MODIFY)","",1,11000,11000]
["","","INTEGRATION AND CONFIGURATION","",1,15125,15125]
["","","MAINTENANCE MANAGEMENT SYSTEM SOFTWARE","",1,291000,291000]
["","","NETWORK MANAGEMENT SOFTWARE (MODIFY)","",1,50000,50000]
["","","SIGNAL SYSTEM SOFTWARE","",1,470000,470000]
["","","SIGNAL TIMING DATABASE CONVER-","SION SOFTWARE",1,4014.53,4014.53]
["","","SYSTEM SUPPORT SOFTWARE & DEVICES","",1,17267.900000000001,17267.900000000001]
["","","TCC BUILDING MODIFICATIONS","",1,13000,13000]
["","","TRAINING","",1,125000,125000]
["","","VIDEO MANAGEMENT SOFTWARE","",1,5300,5300]
["","","VIDEO WALL SOFTWARE","",1,103000,103000]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","4 SOLID BARE GROUNDING CONDUCTOR","",580,3.5,2030]
["","","3-WIRE COPPER FEEDER CONDUCTOR","",4880,8,39040]
["","","3-WIRE COPPER SERVICE ENTRANCECONDUCTOR","",150,7,1050]
["","","4-WIRE COPPER FEEDER CONDUCTOR","",2500,17.600000000000001,44000]
["","","AERIAL CABLE PROTECTOR","",190,9.5,1805]
["","","BACK PULL FIBER OPTIC CABLE","",300,2.78,834]
["","","BACK PULL FIBER OPTICS CABLE","",150,2.76,414]
["","","BACK PULL FIBER-OPTIC CABLE","",2660,1.81,4814.6000000000004]
["","","ETHERNET CABLE","",7185,2.5099999999999998,18034.349999999999]
["","","SERVICE CONDUCTORS","",405,3.34,1352.7]
["","","UNDERGROUND CONDUIT (1, 1\")","",75,5.68,426]
["","","UNDERGROUND CONDUIT (1, 2\")","",5637,6.77,38162.49]
["","","UNDERGROUND CONDUIT (2, 2\")","",9100,7.49,68159]
["7992000000-E","GENERIC SIGNAL ITEM (CY)","ITS DRILLED PIER FOUNDATION","",49,900,44100]
["","","ITS OVERHEAD FOOTINGS","",32,900,28800]
["8007000000-N","CM&R TEMP STR ***********","(21+95.50 -DET1-)","",1,1366300,1366300]
["8017000000-N","CM&R TEMP ACCESS ***********","(140+21.50 -L- LT)","",1,1,1]
["","","(140+21.50 -L- RT)","",1,1,1]
["","","(155+02.50 -L- LT)","",1,1,1]
["","","(155+02.50 -L- RT)","",1,1,1]
["","","(23+26.00 -L- EBL)","",1,47200,47200]
["","","(23+26.00 -L- WBL)","",1,47200,47200]
["8035000000-N","REMV EXIST STR **********","(22+16.89-L-)","",1,409800,409800]
["","","(23+26.00 -L- EBL)","",1,245900,245900]
["","","(23+26.00 -L- WBL)","",1,178083.02,178083.02]
["","","(28+17.37-Y-)","",1,113279.61,113279.61]
["8065000000-N","ASBESTOS ASSESSMENT","","",3,2255.2066666666701,6765.62]
["8091000000-N","FND EXCAV B** STA *******","(1, 14+97.65 -Y8-)","",1,26000,26000]
["","","(1, 17+37.28 -Y16-)","",1,7500,7500]
["","","(1, 22+29.98 -Y5-)","",1,8250,8250]
["","","(1, 25+52.71 -Y7-)","",1,6750,6750]
["","","(1, 28+17.37-Y-)","",1,5663.98,5663.98]
["","","(1, 28+98.81 -Y4-)","",1,10500,10500]
["","","(2, 28+17.37-Y-)","",1,5663.98,5663.98]
["","","(3, 28+17.37-Y-)","",1,11327.96,11327.96]
["8096000000-E","PILE EXCAVATION IN SOIL","","",425,187.71383529411801,79778.38]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",285,317.506666666667,90489.4]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",95,1653.75,157106.25]
["","","(5'-0\")","",104.5,1709.24,178615.58]
["","","(5'-6\")","",124,1960.77,243135.48]
["","","(6'-0\")","",94.92,2224.3299620733301,211133.4]
["","","(6'-6\")","",85.17,2520.19995303511,214645.43]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",904.87,762.44666084630899,689915.11]
["8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",330,1301.9739393939401,429651.4]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",127,1653.75,210026.25]
["","","(5'-0\")","",77,1709.24,131611.48000000001]
["","","(5'-6\")","",74,1960.77,145096.98000000001]
["","","(6'-0\")","",80,2224.33,177946.4]
["","","(6'-6\")","",183,2520.1999999999998,461196.6]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",115,916.974086956522,105452.02]
["8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",183,1317.61071038251,241122.76]
["8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",18,398.05,7164.9]
["","","(6'-6\")","",108.68,489.27999631947,53174.95]
["8111600000-E","PERM STL CASING FOR 4' PIER","","",155.80000000000001,325.23838254172,50672.14]
["8112730000-N","PDA TESTING","","",3,3302.34666666667,9907.0400000000009]
["8113000000-N","SID INSPECTIONS","","",35,824.02857142857101,28841]
["8114000000-N","SPT TESTING","","",16,1,16]
["8115000000-N","CSL TESTING","","",35,2333.6,81676]
["8121000000-N","UNCL STR EXCAV STA *****","(22+16.89-L-)","",1,35500,35500]
["","","(23+26.00 -L- EBL)","",1,28300,28300]
["","","(23+26.00 -L- WBL)","",1,32300,32300]
["","","(93+43.36 -L- LT)","",1,1000,1000]
["","","(93+43.36 -L- RT)","",1,1000,1000]
["8126000000-N","CULV EXCAV @ ************","(173+47.00 -L-)","",1,39286.769999999997,39286.769999999997]
["","","(207+85.77-L-)","",1,42000,42000]
["","","(26+62.00 -Y6RPD-)","",1,24000,24000]
["","","(364+68.00 -L-)","",1,73000,73000]
["","","(382+49.00 -L-)","",1,64000,64000]
["","","(430+93.00 -L-)","",1,22000,22000]
["","","(472+13.00 -L-)","",1,53000,53000]
["","","(493+43.00 -L-)","",1,110000,110000]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",4903,49.497532123189899,242686.4]
["8147000000-E","REINF CONC DECK SLAB","","",262051,32.322175530717303,8470058.4199999999]
["8161000000-E","GROOVING BRIDGE FLOORS","","",279429,0.68278829326948998,190790.85]
["8182000000-E","CLASS A CONC (BRIDGE)","","",6534.1,722.17137019635402,4718739.95]
["8196000000-E","CLASS A CONC (CULV)","","",7940,344.42298236775798,2734718.48]
["8210000000-N","BRG APPR SLAB ***********","(14+97.65 -Y8-)","",1,37500,37500]
["","","(140+21.50 -L- LT)","",1,53800,53800]
["","","(140+21.50 -L- RT)","",1,49600,49600]
["","","(155+02.50 -L- LT)","",1,51550,51550]
["","","(155+02.50 -L- RT)","",1,48150,48150]
["","","(17+37.28 -Y16-)","",1,56200,56200]
["","","(22+16.89-L-)","",1,49800,49800]
["","","(22+29.98 -Y5-)","",1,56500,56500]
["","","(227+33.50-L-)","",1,55000,55000]
["","","(23+26.00 -L- EBL)","",1,46125,46125]
["","","(23+26.00 -L- WBL)","",1,46125,46125]
["","","(25+52.71 -Y7-)","",1,60900,60900]
["","","(28+17.37-Y-)","",1,28319.91,28319.91]
["","","(28+98.81 -Y4-)","",1,86200,86200]
["","","(329+95.42 -L- LT)","",1,68500,68500]
["","","(329+95.42 -L- RT)","",1,68500,68500]
["","","(337+20.09 -L- LT)","",1,67200,67200]
["","","(337+20.09 -L- RT)","",1,67200,67200]
["","","(470+43.12 -L- LT)","",1,73600,73600]
["","","(470+43.12 -L- RT)","",1,73600,73600]
["","","(93+43.36 -L- LT)","",1,49200,49200]
["","","(93+43.36 -L- RT)","",1,49200,49200]
["8217000000-E","REINF STEEL (BRIDGE)","","",1200741,1.20529632951652,1447248.72]
["8238000000-E","SPIRAL COL REINF STL BRG","","",168715,2.7338190439498602,461236.28]
["8245000000-E","REINF STEEL (CULVERT)","","",929300,1.0243335628968,951913.18]
["8259000000-E","36\" PRESTR CONC GIRDR","","",1368.38,237.39847118490499,324851.32]
["8262000000-E","45\" PRESTR CONC GIRDR","","",2637.26,240.34999962081901,633865.43999999994]
["8265000000-E","54\" PRESTR CONC GIRDR","","",6381.86,283.278141482264,1807841.44]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",10754.2,281.393547637202,3026162.49]
["8277000000-E","72\" MOD PRESTR CONC GIRDR","","",2402.66,328.92999841841998,790306.95]
["8280000000-E","STRUCTURAL STEEL","","",238000,2.7184873949579802,647000]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",374,512.13903743315495,191540]
["","","(HP 14 X 73)","",14,650,9100]
["","","(HP12 X 53)","",46,1132.8,52108.800000000003]
["8364000000-E","HP12X53 PILES","","",15222,44.294143345158297,674245.45]
["8384000000-E","HP14X73 PILES","","",385,75,28875]
["8391000000-N","STEEL PILE POINTS","","",182,242.68527472527501,44168.72]
["8392500000-E","PREDRILLING FOR PILES","","",90,177.9,16011]
["8482000000-E","THREE BAR METAL RAIL","","",1097.31,198.35007427253899,217651.52]
["8503000000-E","CONC BARRIER RAIL","","",9066.6200000000008,96.233282083069597,872510.6]
["8505000000-E","VERT CONC BARRIER RAIL","","",1199.5,141.63999999999999,169897.18]
["8531000000-E","4\" SLOPE PROTECTION","","",5836,81.015330705962995,472805.47]
["8559000000-E","SURFACE PREP, CLASS II","","",89,566.4,50409.599999999999]
["8573000000-E","LATEX MOD CONC OVERLAY","","",106.1,1472.6399622997201,156247.1]
["8608000000-E","RIP RAP II (2'-0\")","","",11801,36.9530073722566,436082.44]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",13110,3.0629061784896998,40154.699999999997]
["8657000000-N","ELASTOMERIC BEARINGS","","",6,21391.496666666699,128348.98]
["8685000000-E","EPOXY MORTAR REPAIR","","",29.8,169.920134228188,5063.62]
["8692000000-N","FOAM JOINT SEALS","","",3,200715.95666666701,602147.87]
["8706000000-N","EXPANSION JOINT SEALS","","",2,389900,779800]
["8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(140+21.50 -L- RT)","",1,49600.92,49600.92]
["","","(155+02.50 -L- RT)","",1,48498.67,48498.67]
["","","(337+20.09 -L-)","",1,53570,53570]
["","","(93+43.36 -L- RT)","",1,76054.740000000005,76054.740000000005]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",1325,52.14,69085.5]
["","","(2)","",7960,59.6,474416]
["8802010000-E","SOIL NAIL RETAINING WALLS","","",1000,108.59,108590]
["8802014000-E","SOLDIER PILE RETAINING WALLS","","",null,null,0]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",2,450,900]
["8802015110-N","SOIL NAIL PROOF TESTS","","",4,225,900]
["8802030000-E","SEGMENTAL GRAVITY RETAIN WALLS","","",450,55.31,24889.5]
["8802040000-E","CIP GRAVITY RETAINING WALLS","","",2200,162.55000000000001,357610]
["8846000000-E","GENERIC RET WALL ITEM (TON)","SELECT MATERIAL CLASS VI","",2300,25.82,59386]
["8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL SURFACE TREAT- MENT","",101508,3.15,319750.2]
["","","MSE ABUTMENT WALL NO 1A","",3100,65.680000000000007,203608]
["","","MSE ABUTMENT WALL NO 1B","",3900,67.400000000000006,262860]
["","","MSE ABUTMENT WALL NO 2A","",4700,68.97,324159]
["","","MSE ABUTMENT WALL NO 2B","",5200,69.39,360828]
["","","MSE ABUTMENT WALL NO 4A","",4400,63.91,281204]
["","","MSE ABUTMENT WALL NO 4B","",4200,65.75,276150]
["","","MSE ABUTMENT WALL NO 5A","",3600,68.099999999999994,245160]
["","","MSE ABUTMENT WALL NO 5B","",3200,64.489999999999995,206368]
["","","MSE ABUTMENT WALL NO 6A","",4300,66.31,285133]
["","","MSE ABUTMENT WALL NO 6B","",4800,66.66,319968]
["","","SOUND BARRIER WALL","",61812,28.9,1786366.8]
["8860000000-N","GENERIC STR ITEM (LS)","VOLUMETRIC MIXER","",2,1373.02,2746.04]
["8867000000-E","GENERIC STR ITEM (LF)","78\" FIB PRESTRESSED","CONCRETE GIRDERS",3121.8,403.46000064065601,1259521.43]
["","","EXPANSION JOINT SEAL REPAIR","",135,472,63720]
["8882000000-E","GENERIC STR ITEM (CF)","CONCRETE DECK REPAIR","",170,270,45900]
["","","CONCRETE FOR DECK REPAIR","",217,141.6,30727.200000000001]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",1861,128,238208]
["","","JOINT REPAIR","",286,169.92,48597.120000000003]
["","","TEMPORARY SHORING FOR MSE WALL","CONSTRUCTION",4272,36.700000000000003,156782.39999999999]
["8893000000-E","GENERIC STR ITEM (SY)","HYDRO-DEMOLITION OF BRIDGE DECK","",1930,56.64,109315.2]
["","","PLACING LATEX MODIFIED CONCRETE","",2548,101.95,259768.6]
["","","SCARIFYING BRIDGE DECK","",1930,28.32,54657.599999999999]
["","","SHOTBLASTING BRIDGE DECK","",32035,1.98,63429.3]
["","","SILANE DECK TREATMENT","",32035,5,160175]

{"sheet":"ITEMS - DIV 08","index":10,"n_rows":201,"n_cols":7,"rows_kept":201,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 08"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",7,349842.14285714302,2448895]
["0000400000-N","CONST SURVEYING","","",1,150000,150000]
["0015000000-N","SEALING ABANDONED WELLS","","",3,1200,3600]
["0036000000-E","UNDERCUT EXCAVATION","","",4250,6,25500]
["0043000000-N","GRADING","","",1,1757412,1757412]
["0050000000-E","SUPP CLEARING & GRUBBING","","",2,5000,10000]
["0106000000-E","BORROW EXCAVATION","","",670,5,3350]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",3500,6,21000]
["0141000000-E","BERM DITCH CONST","","",1100,4,4400]
["0192000000-N","PROOF ROLLING","","",12,500,6000]
["0195000000-E","SELECT GRANULAR MAT'L","","",6250,4,25000]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",2300,1.85,4255]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",200,40,8000]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",1340,37,49580]
["0320000000-E","FND CONDIT GEOTEXTILE","","",4210,3.2,13472]
["0342000000-E","**\" SIDE DRAIN PIPE","(30\")","",156,60,9360]
["","","(48\")","",48,100,4800]
["0343000000-E","15\" SIDE DRAIN PIPE","","",1124,32,35968]
["0344000000-E","18\" SIDE DRAIN PIPE","","",340,37,12580]
["0345000000-E","24\" SIDE DRAIN PIPE","","",284,46,13064]
["0366000000-E","15\" RC PIPE CULV III","","",556,42,23352]
["0372000000-E","18\" RC PIPE CULV III","","",992,46,45632]
["0378000000-E","24\" RC PIPE CULV III","","",524,58,30392]
["0384000000-E","30\" RC PIPE CULV III","","",228,74,16872]
["0448200000-E","15\" RCP CULV CLASS IV","","",3712,42,155904]
["0448300000-E","18\" RCP CULV CLASS IV","","",2244,49,109956]
["0448400000-E","24\" RCP CULV CLASS IV","","",1072,63,67536]
["0448500000-E","30\" RCP CULV CLASS IV","","",668,81,54108]
["0448600000-E","36\" RCP CULV CLASS IV","","",272,104,28288]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",314,44,13816]
["0974000000-E","**\"WLD STL PIPE ***\" B RR","(54\", 0.750\")","",88,1420,124960]
["0995000000-E","PIPE REMOVAL","","",2561,15,38415]
["1099500000-E","SHALLOW UNDERCUT","","",333,6,1998]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",632,26.05,16463.599999999999]
["1110000000-E","STABILIZER AGGREGATE","","",1000,26.05,26050]
["1121000000-E","AGGREGATE BASE COURSE","","",58500,26.05,1523925]
["1220000000-E","INCIDENTAL STONE BASE","","",2735,40.291590493601497,110197.5]
["1243000000-E","SHOULDER CONST","","",9.0299999999999994,500,4515]
["1245000000-E","SHOULDER RECONST","","",508.77,2521.1592664661798,1282690.2]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",52107,21.187740610666498,1104029.6000000001]
["1275000000-E","PRIME COAT","","",155,13.3,2061.5]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",7830,1.3,10179]
["","","(1-1/2\")","",1240941,1.6306942876413899,2023595.4]
["","","(1.5\")","",214128,1.25,267660]
["","","(1/2\")","",15844,1.35,21389.4]
["","","(2\")","",617907,1.6569774254054399,1023857.95]
["","","(3\")","",2249,3.55,7983.95]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",1200,5.84,7008]
["","","(1-1/2\" TO 2\")","",88889,2.1,186666.9]
["","","(1-1/2\" TO 4\")","",840,3,2520]
["1330000000-E","INCIDENTAL MILLING","","",96817,5.4424520487104502,526921.88]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",5645,73.775022143489807,416460]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",30365,51.9467479005434,1577363]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",348540,42.647315946519797,14864295.5]
["1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",150,72,10800]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",93865,45.810885314014797,4300038.75]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",180,58,10440]
["1575000000-E","ASP FOR PLANT MIX","","",29494,443.45636400623903,13079302]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",200,200,40000]
["1704000000-E","PATCHING EXIST PVMT","","",43083,120.184643594921,5177915]
["1775500000-E","AST, MAT COAT, *** STONE","(67)","",231200,0.85808391003460005,198389]
["","","(78)","",53800,0.63,33894]
["1814500000-E","AST, SINGLE SEAL","","",244742,0.85,208030.7]
["1838000000-E","EMULSION FOR AST","","",196929,1.8392984273519899,362211.2]
["1838500000-N","VACUUM TRUCK","","",18,1000.77777777778,18014]
["1840000000-E","MILLED RUMBLE STRIPS","","",146925,0.10369236004764,15235]
["1880000000-E","GENERIC PAVING ITEM (TON)","JOINT REPAIR","",1131,242.161803713528,273885]
["1891000000-E","GENERIC PAVING ITEM (SY)","LATEX MODIFIED MICROSURFACING","TYPE II",203709,2.4602656730925001,501178.26]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",76,325,24700]
["2020000000-N","CONTROL-OF-ACCESS MARKERS","","",5,325,1625]
["2022000000-E","SUBDRAIN EXCAVATION","","",168,15,2520]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",84,58,4872]
["2044000000-E","6\" PERF SUBDRN PIPE","","",500,8,4000]
["2070000000-N","SUBDRN PIPE OUTLET","","",1,500,500]
["2077000000-E","6\" OUTLET PIPE","","",6,40,240]
["2253000000-E","PIPE COLLARS","","",0.44700000000000001,2000,894]
["2275000000-E","FLOWABLE FILL","","",32,400,12800]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",54,1600,86400]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",7.2,450,3240]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",4,750,3000]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",10,750,7500]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",3,750,2250]
["","","(F)","",17,750,12750]
["","","(G)","",20,750,15000]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",3,550,1650]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",4470,14,62580]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",12470,16,199520]
["2556000000-E","SHOULDER BERM GUTTER","","",230,23,5290]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",1300,24,31200]
["2600000000-N","RETROFIT EXT CURB RAMPS","","",10,1200,12000]
["2612000000-E","6\" CONC DRIVEWAY","","",200,45,9000]
["2619000000-E","4\" CONC PAVED DITCH","","",93,57,5301]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",150,48,7200]
["2815000000-N","ADJ DROP INLETS","","",4,1300,5200]
["2830000000-N","ADJ MANHOLES","","",131,977.44274809160299,128045]
["2845000000-N","ADJ METER OR VALVE BOXES","","",146,902.5,131765]
["3030000000-E","STL BEAM GUARDRAIL","","",700,16.75,11725]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",5,30,150]
["3210000000-N","GR END TYPE CAT-1","","",3,825,2475]
["3287000000-N","GR END TYPE TL-3","","",3,3100,9300]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",30500,3,91500]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1825,22.5,41062.5]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",660,28.5,18810]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 10', 20')","",2,1500,3000]
["3628000000-E","RIP RAP, CLASS I","","",46,61.5,2829]
["3649000000-E","RIP RAP, CLASS B","","",450,56.5,25425]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",1775,1.85,3283.75]
["4054000000-E","PLN CONC FOUNDTN","","",1,2500,2500]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",352,8,2816]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",1511,15,22665]
["4096000000-N","SIGN ERECTION, TYPE D","","",3,160,480]
["4102000000-N","SIGN ERECTION, TYPE E","","",57,87,4959]
["4108000000-N","SIGN ERECTION, TYPE F","","",24,121,2904]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(B)","",2,750,1500]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(E)","",3,87,261]
["","","(F)","",12,121,1452]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",81,15,1215]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",8,15,120]
["4238000000-N","DISPOSE SIGN, D, E, F","","",6,10,60]
["4360000000-N","GENERIC SIGNING ITEM (EA)","DISPOSAL OF SIGN SYSTEM ON SPAN WIRE","",1,5500,5500]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",923,6.75,6230.25]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",320,7.6,2432]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",510,6.5,3315]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",38572,8.1580973244840802,314674.13]
["4415000000-N","FLASHING ARROW BOARD","","",2,2140,4280]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",4,10638,42552]
["4430000000-N","DRUMS","","",342,41,14022]
["4435000000-N","CONES","","",72,17.28,1244.1600000000001]
["4445000000-E","BARRICADES (TYPE III)","","",792,30.24,23950.080000000002]
["4455000000-N","FLAGGER","","",464,200,92800]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",6,113487.5,680925]
["4480000000-N","TMA","","",2,10000,20000]
["4510000000-N","LAW ENFORCEMENT","","",1659,42.0301386377336,69728]
["4516000000-N","SKINNY DRUM","","",200,26.95,5390]
["4650000000-N","TEMP RAISED PVMT MRKS","","",1931,5,9655]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",1746814,0.43396177841486999,758050.51]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",1441354,0.53321623279221997,768553.35]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",1440,6,8640]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",313351,0.93287907171190998,292318.59000000003]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",18711,1.05094596761263,19664.25]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",11882,1.67980979633058,19959.5]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",728,2.4862637362637399,1810]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",39092,1.43715466080016,56181.25]
["4705000000-E","THERMO LINES 16\" 120MILS","","",775,5.6129032258064502,4350]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",3875,7.56903225806452,29330]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",180,104.888888888889,18880]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",706,126.48725212464601,89300]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",2897,3.1850189851570598,9227]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",10781,3.7730822743715802,40677.599999999999]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",30,8,240]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",3881986,0.10968096484634,425779.97]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",58100,0.48114888123923999,27954.75]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",7430,1.0174966352624499,7560]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",900,2.6666666666666701,2400]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",4696,2.32176320272572,10903]
["4840000000-N","PAINT PVT MKG CHARACTER","","",70,41.571428571428598,2910]
["4845000000-N","PAINT PVT MKG SYMBOL","","",698,32.765042979942699,22870]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",144696,0.42387453696025001,61332.95]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",5000,0.71199999999999997,3560]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",235,3,705]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",79,54.620253164556999,4315]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES (4\",  50 MILS)",20200,0.35,7070]
["","","THERMOPLASTIC PAVEMENT MARKING","LINES, 12\", 90 MILS (HRM)",1075,5,5375]
["","","","LINES, 24\", 120 MILS (HRM)",186,20,3720]
["","","","LINES, 4\", 120 MILS (HRM)",55687,1.45,80746.149999999994]
["","","","LINES, 4\", 90 MILS (HRM)",32310,1.35,43618.5]
["","","","LINES, 8\", 120 MILS (HRM)",722,3,2166]
["","","","LINES, 8\", 90 MILS (HRM)",2298,3,6894]
["4900000000-N","PERM RAISED PVMT MARKERS","","",2694,7.05456570155902,19005]
["4905000000-N","SNOWPLB PVMT MRKER","","",12689,26.235676570257699,332904.5]
["5255000000-N","PORTABLE LIGHTING","","",1,5000,5000]
["6000000000-E","TEMP SILT FENCE","","",26475,1.22562795089707,32448.5]
["6006000000-E","EROS CONTRL STONE CL A","","",900,25,22500]
["6009000000-E","EROS CONTRL STONE CL B","","",5600,25,140000]
["6012000000-E","SEDIMENT CONTROL STONE","","",2050,25,51250]
["6015000000-E","TEMP MULCHING","","",83.5,1400,116900]
["6018000000-E","SEED FOR TEMP SEEDING","","",5300,1,5300]
["6021000000-E","FERT FOR TEMP SEEDING","","",26.5,400,10600]
["6024000000-E","TEMP SLOPE DRAINS","","",550,11,6050]
["6029000000-E","SAFETY FENCE","","",800,0.8,640]
["6030000000-E","SILT EXCAVATION","","",8870,6,53220]
["6036000000-E","MATTING FOR EROS CONTROL","","",48000,0.5,24000]
["6037000000-E","COIR FIBER MAT","","",100,2,200]
["6038000000-E","PERM SOIL REINF MAT","","",1000,2.5,2500]
["6042000000-E","1/4\" HARDWARE CLOTH","","",1600,2.5,4000]
["6071010000-E","WATTLE","","",1940,7.8556701030927796,15240]
["6071012000-E","COIR FIBER WATTLE","","",4600,4.5,20700]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",2850,4,11400]
["6071030000-E","COIR FIBER BAFFLE","","",1660,3,4980]
["6084000000-E","SEEDING AND MULCHING","","",195.6,2117.1661554192201,414117.7]
["6087000000-E","MOWING","","",30,200,6000]
["6090000000-E","SEED FOR REPAIR SEEDING","","",850,5,4250]
["6093000000-E","FERT FOR REPAIR SEEDING","","",2.25,800,1800]
["6096000000-E","SEED FOR SUPP SEEDING","","",1800,5,9000]
["6108000000-E","FERTILIZER TOPDRESSING","","",54,700,37800]
["6114500000-N","SPECIALIZED HAND MOWING","","",10,125,1250]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",25,100,2500]
["6117500000-N","CONC WASHOUT STR","","",9,500,4500]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",14895,6.4485934877475701,96051.8]

{"sheet":"ITEMS - DIV 09","index":11,"n_rows":426,"n_cols":7,"rows_kept":426,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 09"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",11,388090.70545454498,4268997.76]
["0000400000-N","CONST SURVEYING","","",3,122195.65,366586.95]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN AND CONSTRUCTION","",1,140778000,140778000]
["0000996000-N","DESIGN AND CONST","","",1,134150000,134150000]
["0001000000-E","CLEARING & GRUBBING","","",1,634555.69999999995,634555.69999999995]
["0008000000-E","SUPP CLEARING & GRUBBING","","",2,4033,8066]
["0015000000-N","SEALING ABANDONED WELLS","","",2,1635,3270]
["0022000000-E","UNCLAS EXCAVATION","","",177524,2.9252506703318999,519302.2]
["0028000000-N","TYPE I STANDARD APPR **********","(38+35.00)","",1,43600,43600]
["0029000000-N","TYPE III REINF APPR **********","(18+03.65)","",1,78000,78000]
["0036000000-E","UNDERCUT EXCAVATION","","",5899,7.7158230208509897,45515.64]
["0043000000-N","GRADING","","",1,300000,300000]
["0050000000-E","SUPP CLEARING & GRUBBING","","",1,2000,2000]
["0106000000-E","BORROW EXCAVATION","","",21669,43.472929069177198,942014.9]
["0127000000-N","EMBM'T SETTLEMENT GAUGE","","",5,560.26,2801.3]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",2204,4.4489564428312196,9805.5]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",18000,4.6119666666666701,83015.399999999994]
["0192000000-N","PROOF ROLLING","","",20,190.75,3815]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",6310,38.18,240915.8]
["0195000000-E","SELECT GRANULAR MAT'L","","",4275,3.1088304093567301,13290.25]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",24235,1.68165875799464,40755]
["0241000000-E","GENERIC GRADING ITEM (SY)","7\" TRENCHING FOR SHOULDER","CONSTRUCTION",31443,12,377316]
["","","8\" TRENCHING FOR SHOULDER","CONSTRUCTION",74848,13.5,1010448]
["","","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",6310,2.8,17668]
["0248000000-N","GENERIC GRADING ITEM (LS)","CHANNEL BLOCK","",1,1652.64,1652.64]
["","","DRY DETENTION BASIN 1","",1,2902.87,2902.87]
["","","DRY DETENTION BASIN 2","",1,3977.61,3977.61]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",60,38.15,2289]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",1615,31.783034055727601,51329.599999999999]
["0320000000-E","FND CONDIT GEOTEXTILE","","",4810,1.93794178794179,9321.5]
["0335200000-E","15\" DRAINAGE PIPE","","",812,26.626551724137901,21620.76]
["0335300000-E","18\" DRAINAGE PIPE","","",156,46.5061538461539,7254.96]
["0335400000-E","24\" DRAINAGE PIPE","","",348,36.4,12667.2]
["0335500000-E","30\" DRAINAGE PIPE","","",28,57.28,1603.84]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",4,277.64,1110.56]
["","","(18\")","",2,298.5,597]
["","","(24\")","",4,403.59,1614.36]
["0343000000-E","15\" SIDE DRAIN PIPE","","",156,26.77,4176.12]
["0366000000-E","15\" RC PIPE CULV III","","",1812,53.960441501103801,97776.320000000007]
["0372000000-E","18\" RC PIPE CULV III","","",584,40.580821917808201,23699.200000000001]
["0390000000-E","36\" RC PIPE CULV III","","",36,82.95,2986.2]
["0448200000-E","15\" RCP CULV CLASS IV","","",6596,45.4459005457853,299761.15999999997]
["0448300000-E","18\" RCP CULV CLASS IV","","",1584,41.171792929292899,65216.12]
["0448400000-E","24\" RCP CULV CLASS IV","","",424,58.433584905660403,24775.84]
["0448500000-E","30\" RCP CULV CLASS IV","","",240,64.69,15525.6]
["0448600000-E","36\" RCP CULV CLASS IV","","",264,88.23,23292.720000000001]
["0995000000-E","PIPE REMOVAL","","",1412,10.201607648725201,14404.67]
["0996000000-N","PIPE CLEAN OUT","","",2,436,872]
["1011000000-N","FINE GRADING","","",1,48556.78,48556.78]
["1022000000-E","SEALING PVMT CRACKS","","",35000,5,175000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",24860,3,74580]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",250,202.74,50685]
["1099500000-E","SHALLOW UNDERCUT","","",7150,23.406083916083901,167353.5]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",14300,33.662727272727302,481377]
["1110000000-E","STABILIZER AGGREGATE","","",500,35.270000000000003,17635]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",7146,2.63,18793.98]
["1121000000-E","AGGREGATE BASE COURSE","","",26400,29.81,786984]
["1176000000-E","SOIL CEMENT BASE","","",37290,2.83,105530.7]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",1026,191.84,196827.84]
["1198000000-E","AGGREGATE FOR SOIL CEM BS","","",1030,26.54,27336.2]
["1220000000-E","INCIDENTAL STONE BASE","","",16658,7.0078286709088697,116736.41]
["1231000000-E","SHOULDER BORROW","","",280,6.54,1831.2]
["1245000000-E","SHOULDER RECONST","","",362.49,3032.9315015586599,1099407.3400000001]
["1275000000-E","PRIME COAT","","",2108,3,6324]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",41239,1.85,76292.149999999994]
["","","(1-1/2\")","",2518586,1.77023817332424,4458497.08]
["","","(2\")","",127628,2.6832701288118601,342460.4]
["","","(2-1/2\")","",283773,3.31,939288.63]
["","","(3\")","",38417,3.2,122934.39999999999]
["","","(4\")","",9457,4,37828]
["","","(5-1/2\")","",21461,4.7480266529984601,101897.4]
["","","(6\")","",67514,5.9,398332.6]
["","","(7\")","",15559,8,124472]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",74527,2.11261556214526,157446.9]
["","","(0\" TO 2\")","",30705,4.2300000000000004,129882.15]
["1330000000-E","INCIDENTAL MILLING","","",17858,7.8999451226341098,141077.22]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",48626,60.9310821371283,2962834.8]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",65535,58.446909895475699,3830318.24]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",37235,54.040734523969398,2012206.75]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",318536,48.498362445688997,15448474.380000001]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",60998,60.68,3701358.64]
["1575000000-E","ASP FOR PLANT MIX","","",26932,529.67711050052003,14265263.939999999]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",3908,850.56397134083898,3324004]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",65,210,13650]
["1704000000-E","PATCHING EXIST PVMT","","",2789,184.37209035496599,514213.76]
["1735000000-E","REP JNT CONC PVT SLABS","","",866,850,736100]
["1736000000-E","SELECT MAT'L, CLASS IV","","",500,30,15000]
["1748500000-E","AST, MAT & SINGLE SEAL","","",61532,1.45,89221.4]
["1838000000-E","EMULSION FOR AST","","",18460,2.35,43381]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",9465,112,1060080]
["1840000000-E","MILLED RUMBLE STRIPS","","",409454,0.13588989239328,55640.66]
["1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR & SEALING","",598896,1.8,1078012.8]
["1891000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE GREENWAY PATH","",460,43.6,20056]
["","","DIAMOND GRINDING PCC PAVEMENT","",374309,4.25,1590813.25]
["","","FINE MILLING (5/8\")","",271358,1.65,447740.7]
["1925000000-E","MILL RUMBLE STRPS (CONC SHLDR)","","",72537,0.45,32641.65]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",129,192.429069767442,24823.35]
["2020000000-N","CONTROL-OF-ACCESS MARKERS","","",4,179.85,719.4]
["2022000000-E","SUBDRAIN EXCAVATION","","",90.2,18.6694013303769,1683.98]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",300,2.6033333333333299,781]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",50.6,59.773715415019801,3024.55]
["2044000000-E","6\" PERF SUBDRN PIPE","","",300,8.4733333333333292,2542]
["2070000000-N","SUBDRN PIPE OUTLET","","",2,342.36500000000001,684.73]
["2077000000-E","6\" OUTLET PIPE","","",12,26.26,315.12]
["2099000000-E","SHOULDER DRAIN","","",1180,35.47,41854.6]
["2110000000-E","4\" SHOULDER DRAIN PIPE","","",1180,11.39,13440.2]
["2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",50,194.86,9743]
["2143000000-E","BLOTTING SAND","","",20,28.72,574.4]
["2209000000-E","ENDWALLS","","",3.4,1035.5,3520.7]
["2253000000-E","PIPE COLLARS","","",1.1970000000000001,1984.8872180451101,2375.91]
["2275000000-E","FLOWABLE FILL","","",8,250,2000]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",203,2121.9204433497498,430749.85]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",101.2,303.76314229248999,30740.83]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",56,421.57857142857102,23608.400000000001]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",3,382.66,1147.98]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",6,375.66,2253.96]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",2,389.65,779.3]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",8,488.60624999999999,3908.85]
["","","(F)","",49,532.52857142857101,26093.9]
["","","(G)","",37,548.25135135135099,20285.3]
["2396000000-N","FRAME W/COVER STD 840.54","","",7,382.108571428571,2674.76]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",67,1841.44,123376.48]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",57,408.75,23298.75]
["2462000000-E","**\" SLUICE GATE","(8\")","",2,1651.82,3303.64]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",10800,20.170000000000002,217836]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",20910,21.8930894308943,457784.5]
["2591000000-E","4\" CONC SIDEWALK","","",660,43.83,28927.8]
["2605000000-N","CONC CURB RAMPS","","",2,2100,4200]
["2612000000-E","6\" CONC DRIVEWAY","","",670,46.989552238805999,31483]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",230,69,15870]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",3750,46.33,173737.5]
["2703000000-E","CONC BARRIER TYPE ******","(T1)","",5735,227.7,1305859.5]
["2710000000-N","CONC BARRIER TRANS SECTN","","",6,35062.5,210375]
["2738000000-E","GENERIC PAVING ITEM (SY)","ROLLER COMPACTED CONCRETE","",74848,38,2844224]
["2759000000-N","GENERIC PAVING ITEM (EA)","MEDIAN HAZARD PROTECTION","",1,51636.87,51636.87]
["2762000000-E","GENERIC PAVING ITEM (LB)","PAVEMENT SLAB STABILIZATION MATERIAL","",21000,10,210000]
["","","SEALING EXISTING PAVEMENT","CRACKS (POLYMER PATCH)",250,20,5000]
["2800000000-N","ADJ CATCH BASINS","","",1,1500,1500]
["2815000000-N","ADJ DROP INLETS","","",67,863.27611940298505,57839.5]
["2830000000-N","ADJ MANHOLES","","",654,935.21857798165104,611632.94999999995]
["2845000000-N","ADJ METER OR VALVE BOXES","","",542,892.12789667896698,483533.32]
["2905000000-N","CONVERT DI TO JB","","",1,8461.5400000000009,8461.5400000000009]
["2910000000-N","CONVERT TRAF BR DI TO TRAF BR JB","","",1,8461.5400000000009,8461.5400000000009]
["2920000000-N","CONVERT DI TO CB","","",1,773.9,773.9]
["3030000000-E","STL BEAM GUARDRAIL","","",4067.5,17.977991395205901,73125.48]
["3045000000-E","SBGR SHOP CURVED","","",137.5,20.5,2818.75]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",10,25.95,259.5]
["3210000000-N","GR END TYPE CAT-1","","",8,623.375,4987]
["3215000000-N","GR ANCHOR TYPE III","","",8,1966.25,15730]
["3287000000-N","GR END TYPE TL-3","","",6,2943,17658]
["3288000000-N","GR END TYPE TL-2","","",3,2900,8700]
["3317000000-N","GR ANCHOR TYPE B-77","","",1,2035,2035]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",13950,0.99071684587814002,13820.5]
["3500000000-E","WOVEN WIRE FENCE **\" FAB","(47\")","",9920,3.11,30851.200000000001]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",576,27.25,15696]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",249,43.6,10856.4]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(48\", 12', 12')","",2,490.5,981]
["3566000000-E","WOVEN WIRE FENCE RESET","","",155,8.7200000000000006,1351.6]
["3575000000-E","GENERIC FENCING ITEM (LF)","BIKE/PED SAFETY RAIL","",320,65.400000000000006,20928]
["3628000000-E","RIP RAP, CLASS I","","",380,46.82,17791.599999999999]
["3635000000-E","RIP RAP, CLASS II","","",690,53.68,37039.199999999997]
["3649000000-E","RIP RAP, CLASS B","","",755,38.031788079470203,28714]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",4736,1.8195945945945899,8617.6]
["3659000000-N","PREFORMED SCOUR HOLES","","",1,991.33,991.33]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",31.8,33.5,1065.3]
["","","(F)","",8.1999999999999993,33.5,274.7]
["4048000000-E","REINF CONC FOUNDTN","","",5,1199,5995]
["4054000000-E","PLN CONC FOUNDTN","","",1,1090,1090]
["4057000000-E","OVERHEAD FOOTING","","",17,1744,29648]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",875,7.63,6676.25]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",3781,5.45,20606.45]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",1742,7.6889839265212396,13394.21]
["4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(EXIT 17 NB US-421)","",1,80660,80660]
["4096000000-N","SIGN ERECTION, TYPE D","","",4,327,1308]
["4102000000-N","SIGN ERECTION, TYPE E","","",46,84.820652173913004,3901.75]
["4108000000-N","SIGN ERECTION, TYPE F","","",39,124.95641025641,4873.3]
["4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",4,1199,4796]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",5,763,3815]
["4115000000-N","SIGN ERECTION, OVERLAY (OVRHD)","","",3,817.5,2452.5]
["4116000000-N","SIGN ERECTION, OVERLAY (GRD MTD)","","",11,599.5,6594.5]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(B)","",3,844.75,2534.25]
["4116200000-N","SIGN ERECTION, REPOSIT OVRHD","","",3,1090,3270]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",4,81.75,327]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",64,10.918749999999999,698.8]
["4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",2,2180,4360]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",2181,10.7461164603393,23437.279999999999]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",2692,14.5447808320951,39154.550000000003]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",218,9.6913761467889898,2112.7199999999998]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",21723,7.3640514661879104,159969.29]
["4415000000-N","FLASHING ARROW BOARD","","",11,2945.4145454545501,32399.56]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",12,10547.5,126570]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",105,53.207142857142898,5586.75]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",11,4688.1818181818198,51570]
["4424000000-N","WZ PRESENCE LIGHTING","","",29,3630.3655172413801,105280.6]
["4430000000-N","DRUMS","","",972,69.792181069958801,67838]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",66,129.54545454545499,8550]
["4435000000-N","CONES","","",75,19.6933333333333,1477]
["4445000000-E","BARRICADES (TYPE III)","","",524,26.9360305343512,14114.48]
["4455000000-N","FLAGGER","","",195,242.98153846153801,47381.4]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",7,202707.14285714299,1418950]
["4465000000-N","TEMP CRASH CUSHIONS","","",6,10303.799999999999,61822.8]
["4480000000-N","TMA","","",10,15680,156800]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",14580,44.17,643998.6]
["4510000000-N","LAW ENFORCEMENT","","",3071,46.614197329859998,143152.20000000001]
["4516000000-N","SKINNY DRUM","","",150,29.28,4392]
["4650000000-N","TEMP RAISED PVMT MRKS","","",2594,7.4267540478026204,19265]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",1004363,0.58039449880173,582926.76]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",1179147,0.70855740632846997,835493.34]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",249635,0.95600304444489004,238651.82]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",66739,1.0879899309249501,72611.360000000001]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",10074,1.4947875719674399,15058.49]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",10510,2.80161941008563,29445.02]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",19754,2.97281816340994,58725.05]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",350,6,2100]
["4705000000-E","THERMO LINES 16\" 120MILS","","",1950,6.2212820512820501,12131.5]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",13114,9.02761628793656,118388.16]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",584,132.599760273973,77438.259999999995]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",1989,143.89948717948701,286216.08]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",2131,3.17396058188644,6763.71]
["4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",30,105,3150]
["4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",23,1381.30434782609,31770]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",2111286,0.22882218230974,483109.07]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",906024,0.30951542122504,280428.40000000002]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",21343,0.75001639881929005,16007.6]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",44770,0.80194683940138001,35903.160000000003]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",1850,4.4732432432432399,8275.5]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",12230,4.0727228127555204,49809.4]
["4840000000-N","PAINT PVT MKG CHARACTER","","",553,53.433164556961998,29548.54]
["4845000000-N","PAINT PVT MKG SYMBOL","","",1687,65.247990515708395,110073.36]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",1152004,0.77736986156298005,895533.19]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",513825,1.0288613827665101,528654.69999999995]
["4847050000-E","POLYUREA LINES (8\", 20 MILS)","","",10216,1.65320967110415,16889.189999999999]
["4847070000-E","POLYUREA LINES (12\", 20 MILS)","","",30925,2.1096103476152002,65239.7]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",22091,0.94834593273279,20949.91]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",218691,0.41921752609847002,91679.1]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",30,5.25,157.5]
["4865000000-E","LINE REMOVAL 12\" WIDE","","",9887,1.0672600384343101,10552]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",12,4.5,54]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",44,74.318181818181799,3270]
["4900000000-N","PERM RAISED PVMT MARKERS","","",382,3.27,1249.1400000000001]
["4905000000-N","SNOWPLB PVMT MRKER","","",14841,31.9778673943804,474583.53]
["5255000000-N","PORTABLE LIGHTING","","",8,425725.62375000003,3405804.99]
["5325800000-E","8\" WATER LINE","","",877,59.67,52330.59]
["5329000000-E","DI H2O PIPE FITTINGS","","",1065,37.577230046948401,40019.75]
["5540000000-E","6\" VALVE","","",3,1107.3,3321.9]
["5546000000-E","8\" VALVE","","",1,1450.17,1450.17]
["5571600000-E","6\" TAPPING SLEEVE & VALVE","","",1,8400,8400]
["5648000000-N","RELOCATE WATER METER","","",6,4503.9733333333297,27023.84]
["5649000000-N","RECONNECT WATER METER","","",1,269.49,269.49]
["5666000000-N","FIRE HYDRANT","","",4,3161.2624999999998,12645.05]
["5673000000-E","FIRE HYDRANT LEG","","",48,60,2880]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",593,165,97845]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",395,116.53,46029.35]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",8,3000,24000]
["5768500000-E","SEWER SERVICE LINE","","",210,100,21000]
["5775000000-E","4' DIA UTILITY MANHOLE","","",11,7475.00727272727,82225.08]
["5780000000-E","UTILITY MANHOLE WALL **' DIA","(4')","",8.8000000000000007,530,4664]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",31.8,261.47012578616398,8314.75]
["5798000000-E","ABANDON **\" UTILITY PIPE","(15\")","",239,21.18,5062.0200000000004]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",686,18,12348]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",320,55,17600]
["5816000000-N","ABANDON UTILITY MANHOLE","","",4,1750,7000]
["5828000000-N","REMOVE UTILITY MANHOLE","","",1,817.5,817.5]
["5882000000-N","GENERIC UTILITY ITEM (EA)","ABANDON SEWER CONNECTION","",2,654,1308]
["6000000000-E","TEMP SILT FENCE","","",108501,1.96475000230413,213177.34]
["6006000000-E","EROS CONTRL STONE CL A","","",1055,36.9317535545024,38963]
["6009000000-E","EROS CONTRL STONE CL B","","",4115,36.129283110571102,148672]
["6012000000-E","SEDIMENT CONTROL STONE","","",3585,33.361896792189697,119602.4]
["6015000000-E","TEMP MULCHING","","",65.5,1176.4427480915999,77057]
["6018000000-E","SEED FOR TEMP SEEDING","","",3300,0.90939393939393998,3001]
["6021000000-E","FERT FOR TEMP SEEDING","","",17,553.64705882352905,9412]
["6024000000-E","TEMP SLOPE DRAINS","","",1385,19.132527075812298,26498.55]
["6029000000-E","SAFETY FENCE","","",1600,1.64,2624]
["6030000000-E","SILT EXCAVATION","","",27270,2.56738173817382,70012.5]
["6036000000-E","MATTING FOR EROS CONTROL","","",85500,1.6723976608187101,142990]
["6037000000-E","COIR FIBER MAT","","",295,4.24,1250.8]
["6038000000-E","PERM SOIL REINF MAT","","",2082,4.6560999039385198,9694]
["6042000000-E","1/4\" HARDWARE CLOTH","","",10600,4.2275471698113201,44812]
["6045000000-E","**\" TEMP PIPE","(18\")","",90,20.3,1827]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",1300,0.01,13]
["6069000000-E","STILLING BASINS","","",105,13.08,1373.4]
["6070000000-N","SPECIAL STILLING BASINS","","",4,466.74,1866.96]
["6071010000-E","WATTLE","","",7133,7.5580625262862799,53911.66]
["6071012000-E","COIR FIBER WATTLE","","",2000,8.4499999999999993,16900]
["6071013000-E","WATTLE BARRIER","","",1150,8.67,9970.5]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1850,0.28013513513513999,518.25]
["6071030000-E","COIR FIBER BAFFLE","","",3520,4.24,14924.8]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",13,885.66,11513.58]
["","","(2\")","",1,997.62,997.62]
["","","(2-1/2\")","",2,1085.0999999999999,2170.1999999999998]
["","","(4\")","",1,1551.62,1551.62]
["","","(5\")","",1,2426.34,2426.34]
["6084000000-E","SEEDING AND MULCHING","","",49.5,2108.5959595959598,104375.5]
["6087000000-E","MOWING","","",40.75,117.15582822085899,4774.1000000000004]
["6090000000-E","SEED FOR REPAIR SEEDING","","",700,4.4392857142857096,3107.5]
["6093000000-E","FERT FOR REPAIR SEEDING","","",2,1350.75,2701.5]
["6096000000-E","SEED FOR SUPP SEEDING","","",1125,3.5748888888888901,4021.75]
["6108000000-E","FERTILIZER TOPDRESSING","","",32.75,958.46748091603104,31389.81]
["6111000000-E","IMPERVIOUS DIKE","","",1200,0.01,12]
["6114500000-N","SPECIALIZED HAND MOWING","","",20,67.474999999999994,1349.5]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",121,106.454545454545,12881]
["6117500000-N","CONC WASHOUT STR","","",13,1037.08153846154,13482.06]
["6120000000-E","CULVERT DIVERSION CHANNEL","","",128,13.08,1674.24]
["6123000000-E","REFORESTATION","","",1,3379,3379]
["7060000000-E","SIGNAL CABLE","","",7400,3.0287837837837799,22413]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",46,781.97391304347798,35970.800000000003]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",6,1003,6018]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",7,1324.2857142857099,9270]
["7204000000-N","LOUVER","","",20,225,4500]
["7264000000-E","MESSENGER CABLE (3/8\")","","",3000,5.2062499999999998,15618.75]
["7279000000-E","TRACER WIRE","","",3725,0.7,2607.5]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",1050,8,8400]
["","","(2, 2\")","",1425,9,12825]
["7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",120,3.7,444]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",200,16,3200]
["","","(2, 2\")","",1600,19.25,30800]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",43,361.57558139534899,15547.75]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",9,650,5850]
["7360000000-N","WOOD POLE","","",4,1140,4560]
["7372000000-N","GUY ASSEMBLY","","",5,255,1275]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",2,370,740]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",6,510,3060]
["7430000000-N","HEAT SHRINK TUB KIT","","",2,140,280]
["7432000000-E","2\" RISER WITH TUBING","","",6,570,3420]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",4975,10.038442211055299,49941.25]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",9475,1.94965699208443,18473]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",950,2.15,2042.5]
["","","(24)","",9200,2.25,20700]
["7528000000-E","DROP CABLE","","",300,3.4,1020]
["7541000000-N","MOD SPLICE ENCLOSURE","","",6,1965,11790]
["7552000000-N","INTERCONNECT CENTER","","",3,2200,6600]
["7566000000-N","DELINEATOR MARKER","","",7,85,595]
["7575142000-N","900MHZ SPECTRUM RADIO","","",7,3079.25,21554.75]
["7575160000-E","REM EXT COMM CABLE","","",1650,2,3300]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",15,7974,119610]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",1,31900,31900]
["7613000000-N","SOIL TEST","","",16,836.4,13382.4]
["7614100000-E","DRILLED PIER FOUND","","",96,812.6875,78018]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",1,74,74]
["7636000000-N","SIGN FOR SIGNALS","","",15,341.56333333333299,5123.45]
["7684000000-N","SIGNAL CABINET FOUND","","",5,1234.8,6174]
["7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",2,5700,11400]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",5,13775,68875]
["7768000000-N","CONTLR WITH CBNT, 2070L POLE MTD","","",1,13700,13700]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",26,122.115384615385,3175]
["7901000000-N","CABINET BASE EXTENDER","","",5,431.6,2158]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","ETHERNET EDGE SWITCH","",2,2500,5000]
["","","JUNCTION BOX MARKER","",2,85,170]
["","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",2,10250,20500]
["7990000000-E","GENERIC SIGNAL ITEM (LF)","BACK PULL FIBER OPTIC CABLE","",100,2.8,280]
["8035000000-N","REMV EXIST STR **********","(18+03.65-L-)","",1,310000,310000]
["8065000000-N","ASBESTOS ASSESSMENT","","",1,1100,1100]
["8096000000-E","PILE EXCAVATION IN SOIL","","",64,305,19520]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",32,375,12000]
["8112730000-N","PDA TESTING","","",1,4500,4500]
["8121000000-N","UNCL STR EXCAV STA *****","(18+03.65-L-)","",1,15000,15000]
["8126000000-N","CULV EXCAV @ ************","(27+85.00-L-)","",1,33811.800000000003,33811.800000000003]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",323,44.51,14376.73]
["8147000000-E","REINF CONC DECK SLAB","","",26796,33.9136288998358,908749.6]
["8161000000-E","GROOVING BRIDGE FLOORS","","",50994,1.1916288190767499,60765.919999999998]
["8182000000-E","CLASS A CONC (BRIDGE)","","",391.5,895.758620689655,350689.5]
["8196000000-E","CLASS A CONC (CULV)","","",511.5,583.15000977517104,298281.23]
["8210000000-N","BRG APPR SLAB ***********","(18+03.65-L-)","",1,60000,60000]
["","","(38+35.00-L-)","",1,109000,109000]
["8217000000-E","REINF STEEL (BRIDGE)","","",60623,1.4559797436616499,88265.86]
["8245000000-E","REINF STEEL (CULVERT)","","",71469,1.22,87192.18]
["8265000000-E","54\" PRESTR CONC GIRDR","","",1999.25,256.15000125046902,512107.89]
["8280000000-E","STRUCTURAL STEEL","","",352000,2.1633522727272698,761500]
["8296000000-N","POLLUTION CONTROL","","",1,25000,25000]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",8,300,2400]
["","","(HP 14 X 73)","",12,300,3600]
["","","(HP14X89)","",38,1090,41420]
["8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP14X89)","",26,1090,28340]
["8355000000-E","HP**X** PILES","(HP14X89)","",2090,54.5,113905]
["8356000000-E","HP**X** GALV PILES","(HP14X89)","",1560,76.3,119028]
["8364000000-E","HP12X53 PILES","","",320,91,29120]
["8384000000-E","HP14X73 PILES","","",480,98,47040]
["8482000000-E","THREE BAR METAL RAIL","","",351.11,163.500014240551,57406.49]
["8531000000-E","4\" SLOPE PROTECTION","","",61.4,80,4912]
["8559000000-E","SURFACE PREP, CLASS II","","",5,750,3750]
["8608000000-E","RIP RAP II (2'-0\")","","",1255,54.5,68397.5]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",1393,3.27,4555.1099999999997]
["8657000000-N","ELASTOMERIC BEARINGS","","",2,13450,26900]
["8660000000-E","CONC REPAIRS","","",5,1320,6600]
["8664000000-E","SHOTCRETE REPAIRS","","",469.8,1129.02937420179,530418]
["8678000000-E","EPOXY RESIN INJECTION","","",143.5,125,17937.5]
["8692000000-N","FOAM JOINT SEALS","","",3,59666.666666666701,179000]
["8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(18+03.65-L-)","",1,35500,35500]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",4600,93.5,430100]
["","","(2)","",4440,93.5,415140]
["8860000000-N","GENERIC STR ITEM (LS)","PAINTING CONTAINMENT FOR","BRIDGE NO 479",1,50000,50000]
["","","","BRIDGE NO 480",1,50000,50000]
["","","","BRIDGE NO 489",1,65000,65000]
["","","","BRIDGE NO 493",1,65000,65000]
["","","","BRIDGE NO 494",1,40000,40000]
["","","","BRIDGE NO. 485",1,40000,40000]
["","","PAINTING CONTAINMENT FOR ZONE","PAINTING FOR BRIDGE NO 474",1,50000,50000]
["","","PAINTING EXISTING WEATHERING","STEEL STRUCTURE FOR BRIDGE NO 479",1,80000,80000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 480",1,80000,80000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 485",1,95000,95000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 489",1,65000,65000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 493",1,55000,55000]
["","","","STEEL STRUCTURE FOR BRIDGE NO 494",1,55000,55000]
["","","ZONE PAINTING OF EXISTING","STRUCTURE FOR BRIDGE NO 474",1,25000,25000]
["8867000000-E","GENERIC STR ITEM (LF)","CLASSIC CONCRETE BRIDGE RAIL","",416,430,178880]
["","","SILICONE JOINT SEALANT","",1571.9,64.122399643743194,100794]
["8881000000-E","GENERIC STR ITEM (CY)","PPC MATERIALS","",127.8,2600,332280]
["8882000000-E","GENERIC STR ITEM (CF)","ELASTOMERIC CONCRETE","",769.6,300,230880]
["","","REPAIRS TO PRESTRESSED","CONCRETE GIRDERS",22.3,1320,29436]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",3107.9,100,310790]
["","","CONCRETE DECK REPAIR FOR","EPOXY OVERLAY",60,350,21000]
["","","EPOXY COATING","",1080,35,37800]
["","","EPOXY OVERLAY SYSTEM","",144297.4,6,865784.4]
["8893000000-E","GENERIC STR ITEM (SY)","CONCRETE DECK REPAIR FOR","PPC OVERLAY",5,300,1500]
["","","PLACING AND FINISHING PPC","OVERLAY",3680,43,158240]
["","","SCARIFYING BRIDGE DECK","",3680,24.75,91080]
["","","SHOTBLASTING BRIDGE DECK","",3680,12.75,46920]
["8897000000-N","GENERIC STR ITEM (EA)","CLEANING & PAINTING EXISTING","BEARINGS WITH HRCSA FOR BRIDGE NO 474",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 479",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 480",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 485",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 489",80,650,52000]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 493",48,650,31200]
["","","","BEARINGS WITH HRCSA FOR BRIDGE NO 494",48,650,31200]

{"sheet":"ITEMS - DIV 10","index":12,"n_rows":780,"n_cols":7,"rows_kept":780,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 10"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",17,493611.44235294103,8391394.5199999996]
["0000400000-N","CONST SURVEYING","","",9,52788.09,475092.81]
["0000500000-N","SUPP FIELD SURVEYING","","",20,300,6000]
["0000600000-N","SUPP SURVEYING OFF CALC","","",10,200,2000]
["0000700000-N","FIELD OFFICE","","",1,118061,118061]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN AND CONSTRUCTION 15BPR.43","",1,4101260,4101260]
["","","DESIGN AND CONSTRUCTION B-4974","",1,15927850,15927850]
["0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","BOA MOBILIZATION","",4,20088,80352]
["0000996000-N","DESIGN AND CONST","","",1,346000000,346000000]
["0001000000-E","CLEARING & GRUBBING","","",6,100634.920634921,634000]
["0008000000-E","SUPP CLEARING & GRUBBING","","",2,7500,15000]
["0022000000-E","UNCLAS EXCAVATION","","",19150,13,248950]
["0028000000-N","TYPE I STANDARD APPR **********","(23+20 -L-)","",1,40000,40000]
["","","(26+20.73 -YEB-)","",1,66287.490000000005,66287.490000000005]
["0030000000-N","TYPE II MOD APPR **********","(13+70 -L-)","",1,6000,6000]
["","","(18+62.50 -L-)","",1,12500,12500]
["0036000000-E","UNDERCUT EXCAVATION","","",5370,34.111731843575399,183180]
["0043000000-N","GRADING","","",6,682967.37666666706,4097804.26]
["0050000000-E","SUPP CLEARING & GRUBBING","","",6,2453.2333333333299,14719.4]
["0057000000-E","UNDERCUT EXCAVATION","","",2950,16.006271186440699,47218.5]
["0106000000-E","BORROW EXCAVATION","","",136769,18.117577813685799,2477923]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",1135,19.7136563876652,22375]
["0141000000-E","BERM DITCH CONST","","",300,4.05,1215]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",9600,8.6114583333333297,82670]
["0163000000-E","REMOVAL OF EXT CONC PVMT","","",60,62,3720]
["0185000000-E","BREAKING OF EXT CONC PVMT","","",880,31,27280]
["0192000000-N","PROOF ROLLING","","",23,157.565217391304,3624]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",84400,30,2532000]
["0195000000-E","SELECT GRANULAR MAT'L","","",7550,44.868079470198701,338754]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",21860,2.0441445562671499,44685]
["0199000000-E","TEMP SHORING","","",4167,42.073434125269998,175320]
["0223000000-E","ROCK PLATING","","",1015,83,84245]
["0234000000-E","GENERIC GRADING ITEM (CY)","HAULING & DISPOSAL OF CONTAMI-NATED SOIL","",440,135,59400]
["0241000000-E","GENERIC GRADING ITEM (SY)","SOIL CEMENT BASE (FULL DEPTH","RECLAMATION)",91694,3.1020355748467701,284438.05]
["0245000000-E","GENERIC GRADING ITEM (GAL)","FOAM INSTALLATION SOIL STABI- LIZATION","",2085,69,143865]
["","","HAULING & DISPOSAL OF CONTAMI-","NATED GROUND WATER",1000,1,1000]
["0248000000-N","GENERIC GRADING ITEM (LS)","SELECT DEMOLITION OF CONCRETE","SHEET PILE WALL",1,107500,107500]
["","","SELECT DEMOLITION OF CRIB WALL","",1,22089,22089]
["0255000000-E","GENERIC GRADING ITEM (TON)","EARTH MOUND","",5,843,4215]
["","","FLY ASH HAULING AND DISPOSAL","",2405,77.5,186387.5]
["","","HAULING AND DISPOSAL OF","CONTAMINATED SOIL",4555,54,245970]
["","","","PETROLEUM CONTAMINATED SOIL",100,54,5400]
["","","SURGE STONE","",200,69,13800]
["0257000000-E","GENERIC GRADING ITEM (LF)","RAILROAD SIGNAL CONDUIT","",3000,17,51000]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",2661,39.078955279969897,103989.1]
["0320000000-E","FND CONDIT GEOTEXTILE","","",8830,2.3970554926387302,21166]
["0335000000-E","**\" DRAINAGE PIPE","(8\")","",170,39,6630]
["0335200000-E","15\" DRAINAGE PIPE","","",264,70.6666666666667,18656]
["0335300000-E","18\" DRAINAGE PIPE","","",52,82,4264]
["0335600000-E","36\" DRAINAGE PIPE","","",28,164,4592]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",4,400,1600]
["0342000000-E","**\" SIDE DRAIN PIPE","(30\")","",68,140,9520]
["0343000000-E","15\" SIDE DRAIN PIPE","","",132,45.121212121212103,5956]
["0344000000-E","18\" SIDE DRAIN PIPE","","",132,56,7392]
["0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",456,55,25080]
["","","(30\", V)","",304,110,33440]
["0366000000-E","15\" RC PIPE CULV III","","",1940,50.5134020618557,97996]
["0372000000-E","18\" RC PIPE CULV III","","",1148,60.8340766550523,69837.52]
["0378000000-E","24\" RC PIPE CULV III","","",900,66.4177777777778,59776]
["0384000000-E","30\" RC PIPE CULV III","","",352,87.636363636363598,30848]
["0390000000-E","36\" RC PIPE CULV III","","",604,130,78520]
["0402000000-E","48\" RC PIPE CULV III","","",132,210,27720]
["0448000000-E","***\" RCP CULV CLASS IV","(12\")","",80,57,4560]
["0448200000-E","15\" RCP CULV CLASS IV","","",7084,58.6211180124224,415272]
["0448300000-E","18\" RCP CULV CLASS IV","","",2728,62.027859237536703,169212]
["0448400000-E","24\" RCP CULV CLASS IV","","",708,76.485875706214699,54152]
["0448500000-E","30\" RCP CULV CLASS IV","","",232,90,20880]
["0448600000-E","36\" RCP CULV CLASS IV","","",776,142,110192]
["0453000000-E","**\" PIPE END SECTION","(15\")","",1,300,300]
["","","(18\")","",1,450,450]
["","","(30\")","",1,250,250]
["0536000000-E","***\" HDPE PIPE CULVTS","(12\")","",156,42,6552]
["","","(15\")","",280,46,12880]
["","","(18\")","",68,65,4420]
["","","(30\")","",432,97,41904]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",116,60,6960]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",6,425,2550]
["0986000000-E","GENERIC PIPE ITEM (LF)","30\" HDPE PIPE CULVERTS WITH","WRAPPED JOINTS",436,80,34880]
["0995000000-E","PIPE REMOVAL","","",2935,22.6152129471891,66375.649999999994]
["0996000000-N","PIPE CLEAN OUT","","",1,2367,2367]
["1011000000-N","FINE GRADING","","",2,136100,272200]
["1099500000-E","SHALLOW UNDERCUT","","",5620,18.780427046263299,105546]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",11675,29.827751605995701,348239]
["1121000000-E","AGGREGATE BASE COURSE","","",6216,32.8773407335907,204365.55]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",3192,172.78195488721801,551520]
["1220000000-E","INCIDENTAL STONE BASE","","",7545,42.283167660702503,319026.5]
["1245000000-E","SHOULDER RECONST","","",223,2608.5466367713002,581705.9]
["1264000000-E","DITCHING","","",2335,13,30355]
["1275000000-E","PRIME COAT","","",1311,3,3933]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",2179,4.9386874713171203,10761.4]
["","","(1-1/2\")","",590180,2.4724805991392498,1459208.6]
["","","(2\")","",345765,2.4913987824100201,861438.5]
["","","(2-1/2\")","",142714,3.2956230643104401,470331.55]
["","","(3\")","",171025,2.7895073819617,477075.5]
["","","(4\")","",29522,3.6814341846758301,108683.3]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0 TO 1-1/2\")","",5106,6.15,31401.9]
["","","(0 TO 2\")","",6248,8.9499999999999993,55919.6]
["","","(0\" TO 1\")","",26525,2.7,71617.5]
["","","(0\" TO 1-1/2\")","",11180,5.3458855098390003,59767]
["","","(0\" TO 2\")","",6806,5.0466867469879499,34347.75]
["","","(0\" TO 3\")","",1630,5.25,8557.5]
["","","(1-1/2\" TO 2-1/2\")","",7944,3,23832]
["1330000000-E","INCIDENTAL MILLING","","",38549,11.1303302290591,429063.1]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",1050,62.25,65362.5]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",42428,66.849898651833698,2836307.5]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",44782,60.444503371890498,2706825.75]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",20964,51.266213508872298,1074744.8999999999]
["1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",1114,52.486535008976702,58470]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",202397,51.917943200739103,10508035.949999999]
["1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",15860,51.176733921815902,811663]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",86654,63.8785976411937,5535336]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",590,67.900000000000006,40061]
["1526000000-E","ASP CONC SURF CRS S4.75A","","",528,65,34320]
["1575000000-E","ASP FOR PLANT MIX","","",18775,539.082769640479,10121279]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",5978,745.81298093007695,4458470]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",1735,132.93256484149899,230638]
["1704000000-E","PATCHING EXIST PVMT","","",36287,114.952186733541,4171270]
["1735000000-E","REP JNT CONC PVT SLABS","","",1180,816.61016949152497,963600]
["1736000000-E","SELECT MAT'L, CLASS IV","","",195,69,13455]
["1737000000-E","PATCHING CONC PVMT SPALLS","","",405,368.61728395061698,149290]
["1775000000-E","AST, MAT COAT, 78M STONE","","",21741,1,21741]
["1775500000-E","AST, MAT COAT, *** STONE","(67)","",601620,1.13859579136332,685002]
["1803500000-E","AST, DOUBLE SEAL","","",85218,1.8881838344011801,160907.25]
["1838000000-E","EMULSION FOR AST","","",265145,2.3508095570348302,623305.4]
["1838500000-N","VACUUM TRUCK","","",7.19,1969.74965229485,14162.5]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",19926,91.877948409113699,1830760]
["1840000000-E","MILLED RUMBLE STRIPS","","",199251,0.11282658556293,22480.81]
["1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR ANDSEALING","",713000,2.6,1853800]
["1881500000-E","GENERIC PAVING ITEM (CF)","CONCRETE/ASPHALT REPAIR (HOT","APPLIED SYNTHETIC POLYMER RES)",945,325,307125]
["1891000000-E","GENERIC PAVING ITEM (SY)","8\" REINFORCED CONCRETE","PAVEMENT",740,87.25,64565]
["","","DIAMOND GRINDING PCC PAVEMENT","",580000,4.9000000000000004,2842000]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",34,183.82352941176501,6250]
["2021000000-N","GENERIC GRADING ITEM (EA)","RIGHT OF WAY MARKERS","",99,135,13365]
["2022000000-E","SUBDRAIN EXCAVATION","","",665,22.281684210526301,14817.32]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2836,7.2693935119887199,20616]
["2033000000-E","SUBDRAIN FINE AGGREGATE","","",34,55,1870]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",469,54.026631130063997,25338.49]
["2044000000-E","6\" PERF SUBDRN PIPE","","",3036,13.4617918313571,40870]
["2070000000-N","SUBDRN PIPE OUTLET","","",11,392.66,4319.26]
["2077000000-E","6\" OUTLET PIPE","","",66,38.240909090909099,2523.9]
["2209000000-E","ENDWALLS","","",6,1610,9660]
["2253000000-E","PIPE COLLARS","","",10.675000000000001,844.25105386416897,9012.3799999999992]
["2275000000-E","FLOWABLE FILL","","",434,364.513824884793,158199]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",277,2135.2815884476499,591473]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",198.4,312.62096774193498,62024]
["2354000000-N","FRAME W/GRATE 840.22 STD","","",1,670,670]
["2355000000-N","FRAME W/GRATE 840.29 STD","","",2,350,700]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",52,787.30769230769204,40940]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",1,955,955]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",19,736.94736842105306,14002]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",7,660,4620]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",8,652.5,5220]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",26,766.92307692307702,19940]
["","","(F)","",71,795.26760563380299,56464]
["","","(G)","",71,792.90140845070403,56296]
["2396000000-N","FRAME W/COVER STD 840.54","","",26,544.038461538462,14145]
["2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",5,1135,5675]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",37,1047.35783783784,38752.239999999998]
["2484000000-E","GENERIC DRAINAGE ITEM (LF)","8\" UNDERDRAIN","",5250,31,162750]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",130,30,3900]
["2538000000-E","**'-**\" CONC CURB & GUTTER","(2'-0\")","",1170,26,30420]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",5875,21.5,126312.5]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",22190,23.669671022983302,525230]
["2556000000-E","SHOULDER BERM GUTTER","","",87,72.241379310344797,6285]
["2570000000-N","MOD CONC FLUME","","",1,2900,2900]
["2591000000-E","4\" CONC SIDEWALK","","",11050,57.0027149321267,629880]
["2600000000-N","RETROFIT EXT CURB RAMPS","","",134,764.55223880596998,102450]
["2605000000-N","CONC CURB RAMPS","","",107,1975.64579439252,211394.1]
["2612000000-E","6\" CONC DRIVEWAY","","",8716,92.413951353832005,805480]
["2619000000-E","4\" CONC PAVED DITCH","","",475,112,53200]
["2627000000-E","4\" CONC ISLAND COVER","","",2320,61.508448275862101,142699.6]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",1780,80,142400]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",3490,90.798710601719193,316887.5]
["2738000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE MULTIUSE PATH","",1180,56.88,67118.399999999994]
["","","PEDESTRIAN REFUGE ISLAND","(PASS THRU)",130,200,26000]
["2752000000-E","GENERIC PAVING ITEM (LF)","1'-6\" MODIFIED CONCRETE CURB &","GUTTER",1390,22,30580]
["","","2'-6\" MODIFIED CONCRETE CURB &","GUTTER",150,33,4950]
["","","REMOVE & REPLACE 2'-6\" CURB AND GUTTER","",140,85,11900]
["2762000000-E","GENERIC PAVING ITEM (LB)","POLYMER MODIFIED CONCRETE","PAVEMENT REPAIR",3760,7,26320]
["","","SLAB LEVELING, UNDERSEALING","AND VOID FILLING",3750,6.25,23437.5]
["2800000000-N","ADJ CATCH BASINS","","",16,906.5,14504]
["2815000000-N","ADJ DROP INLETS","","",9,1061.1111111111099,9550]
["2830000000-N","ADJ MANHOLES","","",369,1023.4417344173399,377650]
["2845000000-N","ADJ METER OR VALVE BOXES","","",244,884.75409836065603,215880]
["2893000000-N","CONVERT CB TO JB W/MH","","",1,755,755]
["2905000000-N","CONVERT DI TO JB","","",1,4428,4428]
["2920000000-N","CONVERT DI TO CB","","",1,1025,1025]
["2938000000-N","CONVERT DI TO JB W/MH","","",6,1449.1666666666699,8695]
["2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION BOX",1,1500,1500]
["3030000000-E","STL BEAM GUARDRAIL","","",6325,18.895849802371501,119516.25]
["3045000000-E","SBGR SHOP CURVED","","",450,23,10350]
["3105000000-N","SBGR TERM SECT","","",8,200,1600]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",86,35.212093023255797,3028.24]
["3210000000-N","GR END TYPE CAT-1","","",16,877.5,14040]
["3215000000-N","GR ANCHOR TYPE III","","",8,1600,12800]
["3287000000-N","GR END TYPE TL-3","","",30,3179.3333333333298,95380]
["3288000000-N","GR END TYPE TL-2","","",9,3142.64,28283.759999999998]
["3317000000-N","GR ANCHOR TYPE B-77","","",4,1500,6000]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",1187.5,4.65000421052632,5521.88]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",3073,1.05829808005207,3252.15]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",490,8.5061224489795908,4168]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",28,23.285714285714299,652]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",17,56.176470588235297,955]
["3533000000-E","CHN LK FENCE **\" FABRIC","(72\")","",1183,18,21294]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",1076,13.9484200743494,15008.5]
["3539000000-E","MET LINE PST **\" CL FEN","(72\")","",102,75,7650]
["3542000000-E","MET LINE PST 48\" CL FEN","","",91,70.571428571428598,6422]
["3545000000-E","MET TERM PST **\" CL FEN","(72\")","",10,210,2100]
["3548000000-E","MET TERM PST 48\" CL FEN","","",20,218.5,4370]
["3551000000-E","MET GATE PST **\" CL FEN S","(72\")","",2,450,900]
["3554000000-E","MET GATE PST **\" CL FEN D","(72\")","",2,450,900]
["3559000000-E","** STRAND BW FENCE W/ POSTS","(4)","",300,10,3000]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(72\", 12', 12')","",1,2400,2400]
["3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(72\", 12', 24')","",1,4200,4200]
["3575000000-E","GENERIC FENCING ITEM (LF)","CHAIN LINK FENCE","",585,31.25,18281.25]
["","","DECORATIVE FENCE RESET","",50,40,2000]
["","","HANDRAIL HUNTERSVILLE STANDARD","DRAWING 700.1",750,105.5,79125]
["","","PEDESTRIAN SAFETY RAIL","",185,128,23680]
["","","TEMP CHAIN LINK FENCE, 60\" FABRIC","",195,40,7800]
["3578000000-N","GENERIC FENCING ITEM (EA)","GATE","",2,3450,6900]
["3628000000-E","RIP RAP, CLASS I","","",780,52.915384615384603,41274]
["3635000000-E","RIP RAP, CLASS II","","",800,57.256250000000001,45805]
["3649000000-E","RIP RAP, CLASS B","","",291,57.691408934707901,16788.2]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",6501,2.4914782341178299,16197.1]
["3659000000-N","PREFORMED SCOUR HOLES","","",1,1120,1120]
["3832000000-E","RR TRACK TO BE REMOVED","","",3740,12,44880]
["3884000000-N","GENERIC TRACKWORK ITEM (EA)","CROSSTIE DISPOSAL","",2120,6,12720]
["3885000000-E","GENERIC TRACKWORK ITEM (TON)","SUB-BALLAST","",6615,32,211680]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(D)","",9,17.61,158.49]
["","","(E)","",44,20.846136363636401,917.23]
["4048000000-E","REINF CONC FOUNDTN","","",1,5,5]
["4054000000-E","PLN CONC FOUNDTN","","",2,900,1800]
["4057000000-E","OVERHEAD FOOTING","","",260,1090.9615384615399,283650]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",3231,6.3167130919220096,20409.3]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",4456.8999999999996,7.8047970562498596,34785.199999999997]
["4079000000-N","SUPPORT, BARR SMALL","","",2,560,1120]
["4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(14+50 -RPB- LT)","",1,55000,55000]
["","","(20+50 -Y-)","",1,52000,52000]
["","","(24+50 -Y-)","",1,25000,25000]
["","","(25+00 -RPD-)","",1,59000,59000]
["","","(25+50 -L-)","",1,85250,85250]
["","","(29+50 -Y- LT)","",1,46000,46000]
["","","(32+75 -Y- LT)","",1,45000,45000]
["","","(34+00 -Y-)","",1,32500,32500]
["","","(43+00 -L-)","",1,83000,83000]
["","","(44+00 -L-)","",1,30875,30875]
["","","(44+25 -L-)","",1,35000,35000]
["","","(47+50-L-LT)","",1,32000,32000]
["","","(52+00 -L-)","",1,65000,65000]
["4096000000-N","SIGN ERECTION, TYPE D","","",12,154.43666666666701,1853.24]
["4102000000-N","SIGN ERECTION, TYPE E","","",277,80.36,22259.72]
["4108000000-N","SIGN ERECTION, TYPE F","","",24,138.75,3330]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",2,810,1620]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",6,840,5040]
["","","(B)","",2,335,670]
["","","(D)","",3,280,840]
["","","(E)","",7,314.28571428571399,2200]
["","","(F)","",3,280,840]
["","","(LOGO TRAILBLAZER)","",2,50,100]
["4138000000-N","DISPOSE SUPPORT, STL BM","","",16,560,8960]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",2,500,1000]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",191,4.2528272251308898,812.29]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",16,8.078125,129.25]
["4237000000-N","STOCKPILE SIGN, D, E, F","","",1,560,560]
["4238000000-N","DISPOSE SIGN, D, E, F","","",4,50,200]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",5924,10.697886563133,63374.28]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",2368,11.316216216216199,26796.799999999999]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",1137,9.8084520668425696,11152.21]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",9179,9.5258742782438208,87438]
["4415000000-N","FLASHING ARROW BOARD","","",15,2417.6666666666702,36265]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",12,9612.5,115350]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",165,80,13200]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",11,5090.9090909090901,56000]
["4424000000-N","WZ PRESENCE LIGHTING","","",48,5320.8333333333303,255400]
["4430000000-N","DRUMS","","",1711,46.104418468731701,78884.66]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",102,126.764705882353,12930]
["4435000000-N","CONES","","",323,19.792941176470599,6393.12]
["4445000000-E","BARRICADES (TYPE III)","","",1544,27.567046632124299,42563.519999999997]
["4447000000-E","PED CHANNEL DEVICES","","",108,40,4320]
["4455000000-N","FLAGGER","","",264,277.04969696969698,73141.119999999995]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",5,224200,1121000]
["4465000000-N","TEMP CRASH CUSHIONS","","",11,8404.14,92445.54]
["4470000000-N","REM & RES CRASH CUSHION","","",17,2758.8235294117599,46900]
["4480000000-N","TMA","","",12,14908.333333333299,178900]
["4485000000-E","PORT CONC BARRIER","","",1995,31.378446115288199,62600]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",1600,43.307000000000002,69291.199999999997]
["4500000000-E","REM & RES PORT CONC BARRIER","","",6303,7.0712359194034597,44570]
["4505000000-E","REM & RES PORT CONC BARR, ANCH","","",1220,13.5,16470]
["4507000000-E","WATER FILLED BARRIER","","",890,71.946067415730298,64032]
["4508000000-E","REM & RES H2O FILL BARR","","",380,5.2,1976]
["4510000000-N","LAW ENFORCEMENT","","",4436,56.1086564472498,248898]
["4516000000-N","SKINNY DRUM","","",80,33.5,2680]
["4590000000-E","GENERIC TRAFFIC CONTROL ITEM (LF)","PEDESTRIAN BARRICADE","",48,45,2160]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","LANE CLOSURE","",498,3942.1686746987998,1963200]
["","","RAMP/LOOP CLOSURE","",89,3263.9325842696599,290490]
["4650000000-N","TEMP RAISED PVMT MRKS","","",1847,12,22164]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",304807,0.72029175839138004,219549.97]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",343287,0.77941891187256995,267564.38]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",528,3,1584]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",6832,1.8470433255269301,12619]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",18759,2.51958526573911,47264.9]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",3382,4.8092844470727396,16265]
["4702000000-E","12\"WIDE THERMO 120 MILS","","",1273,2.85,3628.05]
["4705000000-E","THERMO LINES 16\" 120MILS","","",1004,6,6024]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",8704,10.844439338235301,94390]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",534,135.75842696629201,72495]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",1311,158.638443935927,207975]
["4726100000-E","HIP THERMO PVT MKG CHAR 120 MILS","","",88,200,17600]
["4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",128,694.8828125,88945]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",6245,5.9216172938350704,36980.5]
["","","(IV)","",3670,5.15,18900.5]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",2608,6.25,16300]
["","","II","",1184,10,11840]
["4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",566,12,6792]
["","","(IV)","",486,10.5,5103]
["4800000000-N","COLD APP PLAS CHAR TYPE *","(IV)","",32,90,2880]
["4805000000-N","COLD APPL PLASTIC SYM TYPE **","(IV)","",16,255,4080]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",1894768,0.21746798024877001,412051.37]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",490714,0.33753070016344,165631.04000000001]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",87399,0.59335015274773995,51858.21]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",23074,1.31236196584901,30281.439999999999]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",640,3,1920]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",11132,4.9403521379806001,54996]
["4840000000-N","PAINT PVT MKG CHARACTER","","",574,59.177700348432097,33968]
["4845000000-N","PAINT PVT MKG SYMBOL","","",1814,67.411245865490599,122284]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",1000,3,3000]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",182700,1,182700]
["4847070000-E","POLYUREA LINES (12\", 20 MILS)","","",19000,2,38000]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",330720,0.59991911586840996,198405.25]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",11504,1.7020514603616099,19580.400000000001]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",4231,1.8622666036397999,7879.25]
["4865000000-E","LINE REMOVAL 12\" WIDE","","",347,2.6,902.2]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",1431,5.1094339622641503,7311.6]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",367,78.746594005449595,28900]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","COLD APPLIED PLASTIC PAVEMENT","MARKING LINES, TYPE II (9\")",61700,7.5,462750]
["","","THERMO PVT MKG LINES, 4\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",387597,0.86332845713460005,334623.52]
["","","THERMO PVT MKG LINES, 4\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",197914,0.95,188018.3]
["","","THERMO PVT MKG LINES, 4\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",178130,0.65,115784.5]
["","","THERMOPLASTIC PAVEMENT MARKING","LINES (12\", 120MILS) (HRM)",600,8,4800]
["","","","LINES (12\", 90MILS) (HRM)",2153,7.5,16147.5]
["","","","LINES (24\", 120MILS) (HRM)",6002,16,96032]
["","","","LINES (4\", 120MILS) (HRM)",24066,1,24066]
["","","","LINES (4\", 90MILS) (HRM)",15681,0.9,14112.9]
["","","","LINES (6\", 120MILS) (HRM)",6756,1.4,9458.4]
["","","","LINES (6\", 90MILS) (HRM)",24908,1.3,32380.400000000001]
["","","","LINES (8\", 120MILS) (HRM)",1464,4,5856]
["","","","LINES (8\", 90MILS) (HRM)",3730,2.2999999999999998,8579]
["","","","LINES, 12\", 120 MILS (HRM)",2470,5.5,13585]
["","","","LINES, 12\", 90 MILS (HRM)",18997,2,37994]
["","","","LINES, 4\", 120 MILS (HRM)",81206,0.76,61716.56]
["","","","LINES, 4\", 90 MILS (HRM)",78042,0.72,56190.239999999998]
["","","","LINES, 6\", 120 MILS (HRM)",154017,1.0974058707804999,169019.16]
["","","","LINES, 6\", 90 MILS (HRM)",230111,0.98174307182186005,225909.88]
["","","","LINES,12\", 90 MILS (HRM)",10157,1.9,19298.3]
["","","THERMOPLASTIC PAVEMENT MARKINGLINES, 4\",","120 MILS (HIGHLY REFLECTIVE MEDIA)",204662,0.75,153496.5]
["","","","90 MILS (HIGHLY REFLECTIVE MEDIA)",152140,0.69,104976.6]
["","","THERMOPLASTIC PM LINES, 12\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",265,4,1060]
["","","THERMOPLASTIC PM LINES, 24\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",550,12,6600]
["","","THERMOPLASTIC PM LINES, 4\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",8206,0.78,6400.68]
["","","THERMOPLASTIC PM LINES, 4\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",17100,0.72,12312]
["","","THERMOPLASTIC PM LINES, 8\", 120 MILS","(HIGHLY REFLECTIVE MEDIA)",3125,3,9375]
["","","THERMOPLASTIC PM LINES, 8\", 90 MILS","(HIGHLY REFLECTIVE MEDIA)",1325,2,2650]
["4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","COLD APPLIED PLASTIC PAVEMENT","MARKING LINES, TYPE II, (9\")",340,9,3060]
["4895000000-N","GENERIC PVMT MARKING ITEM (EA)","IN LANE ROUTE SHIELDS","",7,2100,14700]
["","","REMOVE AND REPLACE SNOWPLOW-","ABLE PAVEMENT MARKERS",5720,75,429000]
["4900000000-N","PERM RAISED PVMT MARKERS","","",130,26.692307692307701,3470]
["4905000000-N","SNOWPLB PVMT MRKER","","",9869,34.738474009524801,342834]
["4915000000-E","7' U-CHANNEL POSTS","","",6,54,324]
["4955000000-N","OBJECT MARKERS (END OF RD)","","",6,324,1944]
["5025000000-E","HIGH MOUNT FOUNDS","","",28,660,18480]
["5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",8,4640,37120]
["5070000000-N","STD FOUNDAT ***********","(TYPE R1)","",6,720,4320]
["","","(TYPE R2)","",2,800,1600]
["5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",385,11.5,4427.5]
["5160000000-E","ELECT DUCT JA, SIZE *****","(2\")","",400,11.5,4600]
["","","(3\")","",430,13.4,5762]
["","","(4\")","",310,15.1,4681]
["5170000000-E","**-8 W/G FEEDER CIRCUIT","(2)","",1000,3.1,3100]
["5175000000-E","**-6 W/G FEEDER CIRCUIT","(2)","",405,4.2,1701]
["5180000000-E","**-4 W/G FEEDER CIRCUIT","(2)","",780,5,3900]
["5205000000-E","**-8 W/G FEEDR N *****\"","(2, 1.5)","",4485,21.5,96427.5]
["5210000000-E","**-6 W/G FEEDR N *****\"","(2, 1.5)","",795,23,18285]
["5215000000-E","**-4 W/G FEEDER N *****\"","(2, 1.5)","",1075,17,18275]
["5240000000-N","ELEC JB ************","(CS36)","",1,1175,1175]
["","","(HM18)","",3,542,1626]
["","","(IG18)","",4,542,2168]
["","","(IG36)","",4,1175,4700]
["","","(LS18)","",8,542,4336]
["5255000000-N","PORTABLE LIGHTING","","",9,167444.444444444,1507000]
["5260000000-N","GENERIC LIGHTING ITEM (LS)","LUMINAIRE STORAGE","",1,900,900]
["5270000000-N","GENERIC LIGHTING ITEM (EA)","RELOCATE HIGH MOUNT LIGHT","STANDARD",4,28270,113080]
["","","ROADWAY LIGHT STANDARD","LUMINAIRE 185W LED",8,860,6880]
["","","SMART CONTROL NODE","",8,115,920]
["5325400000-E","4\" WATER LINE","","",62,81,5022]
["5325600000-E","6\" WATER LINE","","",109,502,54718]
["5325800000-E","8\" WATER LINE","","",301,78.767441860465098,23709]
["5326000000-E","10\" WATER LINE","","",20,73,1460]
["5326200000-E","12\" WATER LINE","","",4137,115.97643219724399,479794.5]
["5326600000-E","16\" WATER LINE","","",2311,108,249588]
["5327000000-E","20\" WATER LINE","","",60,759,45540]
["5327400000-E","24\" WATER LINE","","",57,220,12540]
["5329000000-E","DI H2O PIPE FITTINGS","","",30679,8.1115095016134795,248853]
["5540000000-E","6\" VALVE","","",10,1355.4,13554]
["5546000000-E","8\" VALVE","","",3,1545,4635]
["5558000000-E","12\" VALVE","","",6,3379.6666666666702,20278]
["5558600000-E","16\" VALVE","","",1,6440,6440]
["5572200000-E","12\" TAPPING SLEEVE & VALVE","","",2,6150,12300]
["5589100000-E","1\" AIR RELEASE VALVE","","",1,1435,1435]
["5589200000-E","2\" AIR RELEASE VALVE","","",1,2450,2450]
["5606000000-E","2\" BLOW OFF","","",1,5343,5343]
["5643000000-E","**\" WATER METER","(1\")","",7,840,5880]
["5643100000-E","3/4\" WATER METER","","",7,440,3080]
["5643150000-E","1-1/2\" WATER METER","","",2,6050,12100]
["5643200000-E","2\" WATER METER","","",5,7200,36000]
["5648000000-N","RELOCATE WATER METER","","",5,696.6,3483]
["5649000000-N","RECONNECT WATER METER","","",6,396,2376]
["5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1\")","",2,710,1420]
["5656210000-E","RELC 2\" RPZ BACKFLOW PREVNT A","","",1,850,850]
["5666000000-N","FIRE HYDRANT","","",7,3190,22330]
["5672000000-N","RELOCATE FIRE HYDRANT","","",2,7053,14106]
["5673000000-E","FIRE HYDRANT LEG","","",397,41.770780856423201,16583]
["5678400000-E","6\" LINE STOP","","",2,16029,32058]
["5678600000-E","8\" LINE STOP","","",4,12799,51196]
["5678800000-E","10\" LINE STOP","","",3,11300,33900]
["5679000000-E","12\" LINE STOP","","",1,17000,17000]
["5686000000-E","**\" H2O SERVICE LINE","(2\")","",258,40,10320]
["","","(4\")","",186,55,10230]
["5686500000-E","WATER SERVICE LINE","","",1084,27.812730627306301,30149]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",1618,75,121350]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",265,425.67924528301899,112805]
["5691900000-E","24\" SANITARY GRAVITY SEWER","","",504,801,403704]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",1,1235,1235]
["5768500000-E","SEWER SERVICE LINE","","",27,70,1890]
["5775000000-E","4' DIA UTILITY MANHOLE","","",12,2826,33912]
["5776000000-E","5' DIA UTILITY MANHOLE","","",5,5174.3999999999996,25872]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",36,188.222222222222,6776]
["5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",17,281.47058823529397,4785]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",1388,18.613832853025901,25836]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",3329,16.656353259237001,55449]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",3629,17.000826674014899,61696]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",2264,18.25,41318]
["5811000000-E","ABANDON 18\" UTILITY PIPE","","",524,43,22532]
["5815000000-N","REMOVE WATER METER","","",29,245.72413793103399,7126]
["5815500000-N","REMOVE FIRE HYDRANT","","",4,1000,4000]
["5816000000-N","ABANDON UTILITY MANHOLE","","",10,1562,15620]
["5828000000-N","REMOVE UTILITY MANHOLE","","",6,1631,9786]
["5835000000-E","**\" ENCASEMENT PIPE","(48\")","",402,445,178890]
["5835600000-E","12\" ENCASEMENT PIPE","","",10,75,750]
["5836400000-E","36\" ENCASEMENT PIPE","","",125,280,35000]
["5872500000-E","BORE & JACK **\"","(48\")","",402,1920,771840]
["5882000000-N","GENERIC UTILITY ITEM (EA)","RECONNECT TO EXISTING 6\" WATER","LINE",1,660,660]
["5888000000-E","GENERIC UTILITY ITEM (LF)","8\" CURED IN PLACE PIPE","",517,101,52217]
["5912000000-N","GENERIC UTILITY ITEM (LS)","TEMPORARY SANITARY SEWER BY-","PASS PUMBING",1,73110,73110]
["","","TEMPORARY WATER SERVICE","",1,232000,232000]
["","","WATER LINE CONNECTION/ACTIVA-","TION",1,9200,9200]
["6000000000-E","TEMP SILT FENCE","","",68853,2.85530042263954,196596]
["6006000000-E","EROS CONTRL STONE CL A","","",2375,48.6357473684211,115509.9]
["6009000000-E","EROS CONTRL STONE CL B","","",7792,49.298382956878797,384133]
["6012000000-E","SEDIMENT CONTROL STONE","","",7421,41.860605039752102,310647.55]
["6015000000-E","TEMP MULCHING","","",92.4,1240.0651515151501,114582.02]
["6018000000-E","SEED FOR TEMP SEEDING","","",5400,2.9844444444444398,16116]
["6021000000-E","FERT FOR TEMP SEEDING","","",30.5,922.46688524590195,28135.24]
["6024000000-E","TEMP SLOPE DRAINS","","",3980,10.8763819095477,43288]
["6029000000-E","SAFETY FENCE","","",2100,3.0438095238095202,6392]
["6030000000-E","SILT EXCAVATION","","",14460,10.9477869986169,158305]
["6036000000-E","MATTING FOR EROS CONTROL","","",78745,2.2541329608229099,177501.7]
["6037000000-E","COIR FIBER MAT","","",1735,3.7945244956772299,6583.5]
["6038000000-E","PERM SOIL REINF MAT","","",2605,4.8642994241842601,12671.5]
["6042000000-E","1/4\" HARDWARE CLOTH","","",14425,3.60158405545927,51952.85]
["6045000000-E","**\" TEMP PIPE","(18\")","",40,30,1200]
["","","(24\")","",50,40,2000]
["","","(30\")","",165,4.82,795.3]
["6046000000-E","TEMP PIPE FOR STREAM CROSS","","",225,49,11025]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",298,54.013422818792002,16096]
["6070000000-N","SPECIAL STILLING BASINS","","",19,413.25684210526299,7851.88]
["6071010000-E","WATTLE","","",12566,9.9110297628521398,124542]
["6071012000-E","COIR FIBER WATTLE","","",3345,9.0541405082212307,30286.1]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",180,9.9983333333333295,1799.7]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1591,14.432306725329999,22961.8]
["6071030000-E","COIR FIBER BAFFLE","","",2835,8.0998236331569693,22963]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",9,811.11111111111097,7300]
["","","(2\")","",5,1661.9880000000001,8309.94]
["6084000000-E","SEEDING AND MULCHING","","",81.3,2537.3658056580598,206287.84]
["6087000000-E","MOWING","","",44.55,303.41301907968602,13517.05]
["6090000000-E","SEED FOR REPAIR SEEDING","","",1100,3.7218181818181799,4094]
["6093000000-E","FERT FOR REPAIR SEEDING","","",3.75,1051.0319999999999,3941.37]
["6096000000-E","SEED FOR SUPP SEEDING","","",2075,3.4267469879518102,7110.5]
["6108000000-E","FERTILIZER TOPDRESSING","","",58.5,934.28153846153896,54655.47]
["6111000000-E","IMPERVIOUS DIKE","","",468,35.891880341880302,16797.400000000001]
["6114500000-N","SPECIALIZED HAND MOWING","","",110,62.4718181818182,6871.9]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",226,408.04070796460201,92217.2]
["6117500000-N","CONC WASHOUT STR","","",26,911.29115384615397,23693.57]
["6123000000-E","REFORESTATION","","",0.14000000000000001,2800,392]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","CONCRETE WASHOUT STRUCTURE","",3,500,1500]
["","","SUPPLEMENTAL RESPONSE FOR","EROSION CONTROL",10,500,5000]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",66,1010.6060606060601,66700]
["7060000000-E","SIGNAL CABLE","","",54780,1.9250273822563,105453]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",215,788.06976744185999,169435]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",8,1035,8280]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",6,1182.5,7095]
["7180000000-N","BACKPLATE","","",75,95,7125]
["7252000000-E","MESSENGER CABLE (1/4\")","","",700,9.5,6650]
["7264000000-E","MESSENGER CABLE (3/8\")","","",8100,9.1530864197530892,74140]
["7279000000-E","TRACER WIRE","","",12875,0.55000000000000004,7081.25]
["7288000000-E","PAVED TRENCH (***********)","(2, 2\")","",260,15.5,4030]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",8205,8.6055149299207798,70608.25]
["","","(2, 2\")","",8025,10.246105919003099,82225]
["","","(3, 2\")","",80,10.6,848]
["","","(4, 2\")","",50,14,700]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",1140,13.9416666666667,15893.5]
["","","(2, 2\")","",6080,16.9536184210526,103078]
["","","(3, 2\")","",1240,18.935483870967701,23480]
["","","(4, 2\")","",130,18.600000000000001,2418]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",125,365.32,45665]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",52,603.92307692307702,31404]
["7360000000-N","WOOD POLE","","",44,1203.52272727273,52955]
["7372000000-N","GUY ASSEMBLY","","",56,694.46428571428601,38890]
["7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",6,200,1200]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",2,275,550]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",29,577.06896551724105,16735]
["7432000000-E","2\" RISER WITH TUBING","","",4,582.5,2330]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",20796,9.5859780727062898,199350]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",52970,1.71738720030206,90970]
["7481000000-N","SITE SURVEY","","",11,1338.1818181818201,14720]
["7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",12,445,5340]
["7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",28,3273.5714285714298,91660]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",6,8450,50700]
["7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",43,601.86046511627899,25880]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(144)","",2185,5,10925]
["","","(24)","",10000,2,20000]
["","","(36)","",3890,2.2000000000000002,8558]
["7528000000-E","DROP CABLE","","",4160,1.71310096153846,7126.5]
["7540000000-N","SPLICE ENCLOSURE","","",17,1291.4705882352901,21955]
["7552000000-N","INTERCONNECT CENTER","","",16,1076.5625,17225]
["7566000000-N","DELINEATOR MARKER","","",23,88.695652173913004,2040]
["7574500000-N","FURN WIRELESS RADIO MODEM","","",1,2385,2385]
["7574550000-N","FURN WRLESS LIGHTNING ARSTR","","",1,260,260]
["7575142010-N","900MHZ SER/ETH SPEC RADIO","","",11,4035,44385]
["7575200000-N","GPS UNIT","","",1,1000,1000]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",18,10000,180000]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",12,14050,168600]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,25000,50000]
["7613000000-N","SOIL TEST","","",32,1405,44960]
["7614100000-E","DRILLED PIER FOUND","","",192,682.5,131040]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",14,254.28571428571399,3560]
["7636000000-N","SIGN FOR SIGNALS","","",123,335.73170731707302,41295]
["7642100000-N","TYPE I POST W/ FOUND","","",27,1154.81481481481,31180]
["7642200000-N","TYPE II PED W/ FOUND","","",37,1598.5135135135099,59145]
["7642300000-N","TYPE III PED W/ FOUND","","",2,3700,7400]
["7675000000-N","LED BLANKOUT SIGN","","",2,3670,7340]
["7684000000-N","SIGNAL CABINET FOUND","","",12,763.75,9165]
["7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070E, BASE MOUNTED)","",9,13000,117000]
["","","(TYPE 2070E, POLE MOUNTED)","",2,13625,27250]
["7708000000-N","DETECTOR CARD (***********)","(TYPE 2070E)","",54,125,6750]
["7852000000-N","DETECTOR CARD (NEMA TS-2)","","",108,150,16200]
["7901000000-N","CABINET BASE EXTENDER","","",9,520,4680]
["7960000000-N","METAL POLE FOUND REMVL","","",1,1500,1500]
["7972000000-N","METAL POLE REMOVAL","","",1,450,450]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","CCTV CAMERA ASSEMBLY","",2,4710,9420]
["","","CCTV CAMERA ASSEMBLY","",10,8750,87500]
["","","CCTV ELECTRICAL SERVICE","",2,1600,3200]
["","","CONTROLLER (TYPE 2070E)","",5,2940,14700]
["","","ETHERNET EDGE SWITCH","",13,2990,38870]
["","","ETHERNET SWITCH UNIT","",1,2600,2600]
["","","FIELD EQUIPMENT CABINET","",1,5000,5000]
["","","FURNISH ETHERNET EDGE SWITCH","",2,1455,2910]
["","","JUNCTION BOX (SPECIAL OVER-","SIZED HEAVY-DUTY)",7,1460,10220]
["","","NEMA TS-2, TYPE 1 CABINET,","BASE MOUNTED W/2070LN2 CON- TROLLER",3,22500,67500]
["","","REMOVE 900MHZ RADIO","",14,115,1610]
["","","REPLACE CONFLICT MONITOR","",4,1330,5320]
["8017000000-N","CM&R TEMP ACCESS ***********","(18+62.50-L-)","",1,50000,50000]
["","","(23+20.00-L-)","",1,15000,15000]
["8035000000-N","REMV EXIST STR **********","(13+70.00-L-)","",1,44590,44590]
["","","(15+39.55-S1-)","",1,47633,47633]
["","","(15+40.00-L-)","",1,20234.28,20234.28]
["","","(18+16.00-L-)","",1,17300,17300]
["","","(18+62.50-L-)","",1,125000,125000]
["","","(23+20.00-L-)","",1,25000,25000]
["","","(23+62.98-S2-)","",1,7253,7253]
["","","(28+12.88-S2-)","",1,7253,7253]
["","","(42+59.46-A1-)","",1,225715,225715]
["8065000000-N","ASBESTOS ASSESSMENT","","",4,1158.1824999999999,4632.7299999999996]
["8070000000-E","FOUND EXCAVATION BRIDGE","","",1600,17,27200]
["8077000000-E","FOUNDATN EXCAV RET WALL","","",2693.7,20.029999628763399,53954.81]
["8091000000-N","FND EXCAV B** STA *******","(1, 26+20.73 -YEB-)","",1,43260,43260]
["","","(PIER 1, 18+79.37-S2-)","",1,6265,6265]
["","","(PIER 1, 23+62.98-S2-)","",1,11857,11857]
["","","(PIER 1, 28+12.88-S2-)","",1,19466,19466]
["","","(PIER 2, 18+79.37-S2-)","",1,8213,8213]
["","","(PIER 2, 28+12.88-S2-)","",1,11857,11857]
["","","(PIER 3, 23+62.98-S2-)","",1,11353,11353]
["8096000000-E","PILE EXCAVATION IN SOIL","","",142,247.30119718309899,35116.769999999997]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",143,286.31951048950998,40943.69]
["8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",84.5,1490,125905]
["","","(6'-0\")","",366.5,1515,555247.5]
["8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",78,1572.7564102564099,122675]
["8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",86,1852,159272]
["","","(5'-0\")","",111,1100,122100]
["","","(5'-6\")","",407,1850,752950]
["","","(6'-0\")","",90,1974,177660]
["8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",106,434.669811320755,46075]
["8108000000-E","**'-**\" DIA DRILLD PIERS","(5'-0\")","",356.3,1100,391930]
["8111000000-E","PERM STL CASING FOR ** PIER","(5'-0\")","",47.8,320,15296]
["","","(6'-0\")","",193.4,450,87030]
["8111200000-E","PERM STL CASING FOR 3' PIER","","",75.599999999999994,179.52380952381,13572]
["8112730000-N","PDA TESTING","","",1,1500,1500]
["8113000000-N","SID INSPECTIONS","","",28,703.57142857142901,19700]
["8114000000-N","SPT TESTING","","",37,770.27027027026998,28500]
["8115000000-N","CSL TESTING","","",29,4453.4482758620697,129150]
["8121000000-N","UNCL STR EXCAV STA *****","(13+70.00-L-)","",1,4000,4000]
["","","(18+62.50-L-)","",1,10000,10000]
["","","(23+20.00-L-)","",1,15000,15000]
["","","(42+59.46-A1-)","",1,13453,13453]
["8126000000-N","CULV EXCAV @ ************","(15+40.00-L-)","",1,23143.02,23143.02]
["","","(18+16.00-L-)","",1,22950,22950]
["","","(25+30.89-S1-)","",1,5363,5363]
["","","(29+35.21-S1-)","",1,1612,1612]
["","","(42+05.33-A1-)","",1,1758,1758]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",407,58.224742014741999,23697.47]
["8147000000-E","REINF CONC DECK SLAB","","",61234.2,46.271939537056099,2833425.2]
["8161000000-E","GROOVING BRIDGE FLOORS","","",265936,0.48626688376151,129315.87]
["8175000000-E","CLASS AA CONC (BRIDGE)","","",7935.7,929.09132149652805,7372990]
["8182000000-E","CLASS A CONC (BRIDGE)","","",559.70000000000005,837.406771484724,468696.57]
["8196000000-E","CLASS A CONC (CULV)","","",389.3,764.50552273311098,297622]
["8210000000-N","BRG APPR SLAB ***********","(13+70.00-L-)","",1,23975,23975]
["","","(18+62.50-L-)","",1,25000,25000]
["","","(23+20.00-L-)","",1,45000,45000]
["","","(26+20.73 -YEB-)","",1,94160,94160]
["8217000000-E","REINF STEEL (BRIDGE)","","",1859787,0.93851094775906996,1745430.46]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",5433,3.2,17385.599999999999]
["8238000000-E","SPIRAL COL REINF STL BRG","","",124245,2.0272051189182698,251870.1]
["8245000000-E","REINF STEEL (CULVERT)","","",203254,0.98349129660425005,199898.54]
["8252000000-E","REINF STEEL (RET WALL)","","",382579,1,382579]
["8265000000-E","54\" PRESTR CONC GIRDR","","",587.16,285,167340.6]
["8280000000-E","STRUCTURAL STEEL","","",950000,1.8074736842105299,1717100]
["8296000000-N","POLLUTION CONTROL","","",1,35000,35000]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",10,750,7500]
["","","(HP 14 X 73)","",47,120,5640]
["","","(HP12X53)","",39,613.84615384615404,23940]
["8364000000-E","HP12X53 PILES","","",845,43.330650887574002,36614.400000000001]
["8384000000-E","HP14X73 PILES","","",2960,74.5,220520]
["8391000000-N","STEEL PILE POINTS","","",10,150,1500]
["8453000000-E","METHOD B DAMPPROOFING","","",2642,14.5972747918244,38566]
["8475000000-E","TWO BAR METAL RAIL","","",737.28,107,78888.960000000006]
["8484000000-E","42\" OREGON RAIL","","",140,379.1,53074]
["8503000000-E","CONC BARRIER RAIL","","",671.3,108.29658870847599,72699.5]
["8504000000-E","CONC BARR RAIL MOMENT SLAB","","",1290,537,692730]
["8505000000-E","VERT CONC BARRIER RAIL","","",250.5,95,23797.5]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2-6\")","",401.45,108.500012454851,43557.33]
["8531000000-E","4\" SLOPE PROTECTION","","",2142.8000000000002,74.008213552361397,158584.79999999999]
["8559000000-E","SURFACE PREP, CLASS II","","",59.6,735.234899328859,43820]
["8566000000-E","SURFACE PREP, CLASS III","","",82.3,2000,164600]
["8608000000-E","RIP RAP II (2'-0\")","","",2116,67.229087901701305,142256.75]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2353,1.8040798980025501,4245]
["8654000000-N","DISC BEARINGS","","",1,37200,37200]
["8657000000-N","ELASTOMERIC BEARINGS","","",5,8273.7999999999993,41369]
["8660000000-E","CONC REPAIRS","","",50.2,1522.5099601593599,76430]
["8678000000-E","EPOXY RESIN INJECTION","","",100,450,45000]
["8685000000-E","EPOXY MORTAR REPAIR","","",25.5,700,17850]
["8692000000-N","FOAM JOINT SEALS","","",2,48750,97500]
["8699000000-N","STRIP SEALS","","",1,20000,20000]
["8706000000-N","EXPANSION JOINT SEALS","","",2,76000,152000]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",550,140,77000]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",1470,158.67428571428599,233251.20000000001]
["8802014000-E","SOLDIER PILE RETAINING WALLS","","",4792.5,308,1476090]
["8802040000-E","CIP GRAVITY RETAINING WALLS","","",280,200,56000]
["8806000000-N","GENERIC CULVERT ITEM (EA)","PDA TESTING","",2,4441,8882]
["","","PILE DRIVING EQUIPMENT SETUP","FOR HP14X73 STEEL PILES",43,630,27090]
["8811000000-E","GENERIC CULVERT ITEM (LF)","HP14X73 STEEL PILES","",1602,66,105732]
["","","METAL RAIL (ALUMINUM)","",47.2,263,12413.6]
["8822000000-E","GENERIC CULVERT ITEM (SY)","WATERPROOFING","",562,75,42150]
["8826000000-E","GENERIC CULVERT ITEM (CY)","CLASS AA CONCRETE","",646.6,650,420290]
["8834000000-N","GENERIC RET WALL ITEM (EA)","7\" DIA MICROPILES","",6,4765,28590]
["","","MICROPILE VERIFICATION TEST","",1,18673,18673]
["","","PDA TESTING","",2,4441,8882]
["","","PILE DRIVING EQUIPMENT SETUP","FOR HP14X73 STEEL PILES",316,535,169060]
["8839000000-E","GENERIC RET WALL ITEM (LF)","HP14X73 STEEL PILES","",11113.4,68,755711.2]
["","","METAL RAIL (ALUMINUM)","",594.4,252,149788.79999999999]
["","","METAL RAIL (STEEL) & FENCE","",1320.1,600,792060]
["8847000000-E","GENERIC RET WALL ITEM (SF)","PILE PANEL RETAINING WALLS","",10304.799999999999,297,3060525.6]
["8853000000-E","GENERIC RET WALL ITEM (CY)","CLASS AA CONCRETE","",2296.9,605,1389624.5]
["8860000000-N","GENERIC STR ITEM (LS)","APPLICATION OF BRIDGE COATING","",1,50000,50000]
["","","APPROX 160,000 LBS STRUCTURAL","STEEL",1,561207,561207]
["","","APPROX 177,727 LBS STRUCTURAL STEEL","",1,655396,655396]
["","","APPROX 177,963 LBS STRUCTURAL STEEL","",1,648926,648926]
["","","APPROX 231,350 LBS STRUCTURAL STEEL","",1,850680,850680]
["","","APPROX 233,588 LBS STRUCTURAL STEEL","STA 28+12.88-S2-",1,850791,850791]
["","","","STA 28+17.22-S1-",1,846065,846065]
["","","APPROX 338,035 LBS STRUCTURAL STEEL","STA 23+62.98-S2-",1,936000,936000]
["","","","STA 23+65.83-S1-",1,1018350,1018350]
["","","APPROX 764,875 LBS STRUCTURAL STEEL","",1,1626392,1626392]
["","","ASBESTOS ASSESSMENT","",2,3250,6500]
["","","CLEANING AND REPAINTING OF","BRIDGE 207",1,168000,168000]
["","","","BRIDGE 213",1,200000,200000]
["","","PAINTING CONTAINMENT FOR","BRIDGE 207",1,65000,65000]
["","","","BRIDGE 213",1,65000,65000]
["","","PAINTING OF STRUCTURAL STEEL","",1,1119975,1119975]
["","","PARTIAL REMOVAL OF EXISTING","STRUCTURE",1,47000,47000]
["","","PLATFORM STRUCTURE DRAINAGE","SYSTEM",1,131395,131395]
["","","REMOVE EXISTING BRIDGE RAIL","",1,43500,43500]
["","","SELF LUBRICATING EXPANSION","BEARING ASSEMBLIES",1,555465,555465]
["","","STRUCTURE DRAINAGE SYSTEM AT","STA 15+39.55-S1-",1,254741,254741]
["","","","STA 18+79.37-S2-",1,147606,147606]
["","","","STA 18+82.25-S1-",1,147606,147606]
["","","","STA 23+62.98-S2-",1,187468,187468]
["","","","STA 23+65.83-S1-",1,187468,187468]
["","","","STA 28+12.88-S2-",1,153599,153599]
["","","","STA 28+17.22-S1-",1,153599,153599]
["","","","STA 42+59.46-A1-",1,126535,126535]
["","","STRUCTURE GROUNDING AND","BONDING AT STA 23+65.83-S1-",1,15000,15000]
["","","TEMPORARY RAILROAD SHORING/","ABUTMENT 1 (23+62.98-S2-)",1,17065,17065]
["","","","ABUTMENT 1 (28+12.88-S2-)",1,16005,16005]
["","","","ABUTMENT 1 (42+59.46-A1-)",1,43501,43501]
["","","","ABUTMENT 2 (23+62.98-S2-)",1,15475,15475]
["","","","ABUTMENT 2 (28+12.88-S2-)",1,17065,17065]
["","","","ABUTMENT 2 (42+59.46-A1-)",1,37311,37311]
["","","","PIER 1 (18+79.37-S2-)",1,64021,64021]
["","","","PIER 1 (23+62.98-S2-)",1,108223,108223]
["","","","PIER 1 (28+12.88-S2-)",1,89568,89568]
["","","","PIER 2 (18+79.37-S2-)",1,104940,104940]
["","","","PIER 2 (28+12.88-S2-)",1,86917,86917]
["","","","PIER 3 (23+62.98-S2-)",1,90098,90098]
["","","VOLUMETRIC MIXER","",1,5000,5000]
["8867000000-E","GENERIC STR ITEM (LF)","ABRASIVE METAL NOSINGS","",999,26,25974]
["","","ADHESIVELY ANCHORED 2'-6\"","CONCRETE PARAPET",350.79,148.50001425354199,52092.32]
["","","ADHESIVELY ANCHORED CONCRETE","BARRIER RAIL",350.83,160,56132.800000000003]
["","","ADHESIVELY ANCHORED VERTICAL","CONCRETE RAIL",403.96,140,56554.400000000001]
["","","ARCHITECTURAL FIN RAIL","(ALUMINUM HAND RAIL AND FIN ASSEMBLY)",400.4,1465,586586]
["","","ARMORLESS EXPANSION JOINT SYSTEM","",335,66,22110]
["","","CONCRETE PARAPET","",2205.1999999999998,99,218314.8]
["","","EXPANSION JOINT SEAL REPAIR","",410,150,61500]
["","","FOAM JOINT SEALS","",719,170,122230]
["","","HP14X73 STEEL PILES","",27972.7,50,1398635]
["","","METAL RAIL (ALUMINUM)","",842.7,258,217416.6]
["","","METAL RAIL (STEEL) & FENCE","",660.4,645,425958]
["","","PLATFORM EXPANSION JOINTS","",315,26,8190]
["","","PLATFORM PAINT","",2200,13,28600]
["","","PREDRILLING FOR PILES","",128,150,19200]
["","","RUB RAIL","",2200,48,105600]
["","","SOIL/ROCK BORING","",640,150,96000]
["","","STAINLESS STEEL HANDRAILS","",370,261,96570]
["","","STAINLESS STEEL RAILINGS","",368,761,280048]
["","","TACTILE WARNING SURFACE","",2200,188,413600]
["8881000000-E","GENERIC STR ITEM (CY)","POLYESTER POLYMER CONCRETE","MATERIALS",432.7,3000,1298100]
["","","PPC MATERIALS","",486.7,2684.2408054242901,1306420]
["8882000000-E","GENERIC STR ITEM (CF)","CONCRETE FOR DECK REPAIR","",1442.3,89,128364.7]
["8889000000-E","GENERIC STR ITEM (LB)","ADDITIONAL REINFORCING STEEL","",1200,2,2400]
["","","BEAM REPAIR FOR BRIDGE 50","",364,12,4368]
["","","REINFORCING STEEL, BLACK (GRADE 75)","",139300,1,139300]
["","","REINFORCING STEEL, GALVANIZED","(GRADE 75)",67320,2,134640]
["","","SPIRAL REINFORCING STEEL,","BLACK (GRADE 75)",69800,2,139600]
["","","","GALVANIZED (GRADE 75)",18000,3,54000]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",73.8,93,6863.4]
["","","EPOXY COATING","",2118,18,38124]
["","","LIQUID FLOOR TREATMENTS","",38400,0.41,15744]
["","","STAINLESS STEEL ENCLOSURE","",442,476,210392]
["8893000000-E","GENERIC STR ITEM (SY)","CONCRETE DECK REPAIR FOR","POLYESTER POLYMER CONC OVERLAY",4,500,2000]
["","","CONCRETE DECK REPAIR FOR PPC","OVERLAY",3,500,1500]
["","","CONCRETE DECK REPAIR FOR PPC OVERLAY","",52.6,345,18147]
["","","FOUNDATION WATERPROOFING","",2400,57,136800]
["","","PLACING & FINISHING POLYESTER","POLYMER CONCRETE OVERLAY",14139,26,367614]
["","","PLACING AND FINISHING PPC OVERLAY","",3600,60,216000]
["","","PLACING AND FINISHING PPC OVERLAY","",10413,28.5,296770.5]
["","","SCARIFYING BRIDGE DECK","",28152,17.8459878516624,502400.25]
["","","SHOTBLASTING BRIDGE DECK","",28152,5.8186540920716103,163806.75]
["","","WATERPROOFING","",3075.7,73.062587378482903,224718.6]
["8897000000-N","GENERIC STR ITEM (EA)","3'-6\" STAINLESS STEEL GATES","",3,11746,35238]
["","","7\" DIA MICROPILES","",12,4450,53400]
["","","8'-0\" STAINLESS STEEL GATES","",2,60957,121914]
["","","HINGE","",30,740,22200]
["","","LIGHTNING PROTECTION SYSTEM","",2,8000,16000]
["","","MICROPILE VERIFICATION TEST","",1,18673,18673]
["","","PANIC DEVICE","",4,1000,4000]
["","","PDA TESTING","",20,4441,88820]
["","","PILE DRIVING EQUIPMENT SETUP","FOR HP14X73 STEEL PILES",593,423,250839]
["","","STEEL PILE POINTS","",12,168,2016]
["","","THERMAL INTEGRITY PROFILER","",27,3311.1111111111099,89400]
["","","TYPE I BRIDGE JACKING FOR","BRIDGE 215",3,9000,27000]

{"sheet":"ITEMS - DIV 11","index":13,"n_rows":165,"n_cols":7,"rows_kept":165,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 11"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",4,1368483.83,5473935.3200000003]
["0000400000-N","CONST SURVEYING","","",1,24262.87,24262.87]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN & CONSTRUCTION OF","BRIDGES",1,2217602.79,2217602.79]
["","","","CULVERT 040023",1,972400,972400]
["","","","CULVERT 940278",1,1440661,1440661]
["0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","END BENTS STRUCTURE 040177","",2,96335.87,192671.74]
["","","END BENTS STRUCTURE 130115","",2,26690.23,53380.46]
["","","END BENTS STRUCTURE 850012","",2,23216.99,46433.98]
["","","END BENTS STRUCTURE 980020","",2,22409.58,44819.16]
["","","INTERIOR BENT CAPS STRUCTURE 850012","",1,51153.42,51153.42]
["","","INTERIOR BENT CAPS STRUCTURE 980020","",1,49044.79,49044.79]
["","","RIGHT OF WAY ACQUISITION","",12,6249.1066666666702,74989.279999999999]
["0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT 1 STRUCTURE 040177",28,419.56,11747.68]
["","","","BENT 1 STRUCTURE 130115",26,433.15,11261.9]
["","","","BENT 1 STRUCTURE 850012",36,329.86,11874.96]
["","","","BENT 1 STRUCTURE 980020",15,2273.88,34108.199999999997]
["","","","BENT 2 STRUCTURE 040177",18,537.47,9674.4599999999991]
["","","","BENT 2 STRUCTURE 130115",22,429.94,9458.68]
["","","","BENT 2 STRUCTURE 850012",47,299.66000000000003,14084.02]
["","","","BENT 2 STRUCTURE 980020",22,427.89,9413.58]
["","","AVE FOUNDATION LENGTH AT INTE-","RIOR BENT 1 STRUCTURE 850012",60,1654.09,99245.4]
["","","","RIOR BENT 1 STRUCTURE 980020",30,2225.87,66776.100000000006]
["","","BRIDGE LENGTH STRUCTURE 040177","",60,2303.38,138202.79999999999]
["","","BRIDGE LENGTH STRUCTURE 130115","",70,2476.13,173329.1]
["","","BRIDGE LENGTH STRUCTURE 850012","",130,2592.1999999999998,336986]
["","","BRIDGE LENGTH STRUCTURE 980020","",115,1824.59,209827.85]
["0000960000-E","GENERIC MISCELLANEOUS ITEM (SY)","PAVEMENT REPLACEMENT","",156000,175,27300000]
["0000996000-N","DESIGN AND CONST","DESIGN & CONSTRUCTION","",1,17300000,17300000]
["0001000000-E","CLEARING & GRUBBING","","",1,52472.1,52472.1]
["0008000000-E","SUPP CLEARING & GRUBBING","","",1,1.0900000000000001,1.0900000000000001]
["0022000000-E","UNCLAS EXCAVATION","","",18000,34.299999999999997,617400]
["0028000000-N","TYPE I STANDARD APPR **********","(19+78.50-L-)","",1,17855.189999999999,17855.189999999999]
["0036000000-E","UNDERCUT EXCAVATION","","",450,12.46,5607]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",2080,5.98,12438.4]
["0195000000-E","SELECT GRANULAR MAT'L","","",400,35.89,14356]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",600,1.97,1182]
["0199000000-E","TEMP SHORING","","",450,69.56,31302]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",70,30.04,2102.8000000000002]
["0320000000-E","FND CONDIT GEOTEXTILE","","",210,2.5499999999999998,535.5]
["0335200000-E","15\" DRAINAGE PIPE","","",204,34.659999999999997,7070.64]
["0335300000-E","18\" DRAINAGE PIPE","","",72,39.28,2828.16]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(18\")","",4,327.25,1309]
["0448200000-E","15\" RCP CULV CLASS IV","","",200,37,7400]
["0448300000-E","18\" RCP CULV CLASS IV","","",96,44.68,4289.28]
["0987000000-E","GENERIC PIPE ITEM (LF) 310","15\" RC PIPE CULVERT, CLASS V","",40,38.549999999999997,1542]
["0995000000-E","PIPE REMOVAL","","",150,5.74,861]
["1011000000-N","FINE GRADING","","",1,42698.54,42698.54]
["1099500000-E","SHALLOW UNDERCUT","","",100,7.65,765]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",200,26.57,5314]
["1121000000-E","AGGREGATE BASE COURSE","","",798,27.96,22312.080000000002]
["1220000000-E","INCIDENTAL STONE BASE","","",75,26.98,2023.5]
["1231000000-E","SHOULDER BORROW","","",180,13.22,2379.6]
["1275000000-E","PRIME COAT","","",810,8.43,6828.3]
["1330000000-E","INCIDENTAL MILLING","","",130,32.64,4243.2]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",310,92.21,28585.1]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",340,90.31,30705.4]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",790,73.599999999999994,58144]
["1575000000-E","ASP FOR PLANT MIX","","",85,651,55335]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",50,157.29,7864.5]
["2022000000-E","SUBDRAIN EXCAVATION","","",45,23.61,1062.45]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",200,3.17,634]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",34,52.37,1780.58]
["2044000000-E","6\" PERF SUBDRN PIPE","","",200,13.61,2722]
["2070000000-N","SUBDRN PIPE OUTLET","","",1,292.55,292.55]
["2077000000-E","6\" OUTLET PIPE","","",6,11.35,68.099999999999994]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",14,1375.24,19253.36]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",5.3,234.539622641509,1243.06]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",2,551.92999999999995,1103.8599999999999]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",10,561.88,5618.8]
["2396000000-N","FRAME W/COVER STD 840.54","","",4,953.73,3814.92]
["2556000000-E","SHOULDER BERM GUTTER","","",100,42.83,4283]
["2619000000-E","4\" CONC PAVED DITCH","","",120,97.27,11672.4]
["2724000000-E","PC REINF BARRIER SNGL FC","","",265,93.27,24716.55]
["2905000000-N","CONVERT DI TO JB","","",2,854.59,1709.18]
["3030000000-E","STL BEAM GUARDRAIL","","",525,18.22,9565.5]
["3045000000-E","SBGR SHOP CURVED","","",12.5,18.5,231.25]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",10,32.64,326.39999999999998]
["3165500000-N","GR END UNIT TYPE **********","(AT-1)","",1,544.01,544.01]
["3215000000-N","GR ANCHOR TYPE III","","",3,1904.04,5712.12]
["3287000000-N","GR END TYPE TL-3","","",3,2937.67,8813.01]
["3317000000-N","GR ANCHOR TYPE B-77","","",1,1795.24,1795.24]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",510,1.0900000000000001,555.9]
["3380000000-E","TEMP STL BM GUARDRAIL","","",62.5,8.6999999999999993,543.75]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",2,1523.23,3046.46]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",2,1849.64,3699.28]
["3575000000-E","GENERIC FENCING ITEM (LF)","TEMPORARY 5 STRAND BARBED WIRE","FENCE WITH POSTS",400,9.25,3700]
["3628000000-E","RIP RAP, CLASS I","","",220,49.03,10786.6]
["3649000000-E","RIP RAP, CLASS B","","",55,45.17,2484.35]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",1650,2.42,3993]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",180,8.16,1468.8]
["4096000000-N","SIGN ERECTION, TYPE D","","",2,136.01,272.02]
["4102000000-N","SIGN ERECTION, TYPE E","","",11,136,1496]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",8,27.2,217.6]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",689,13.06,8998.34]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",144,11.11,1599.84]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",106,10.88,1153.28]
["4430000000-N","DRUMS","","",52,49.71,2584.92]
["4435000000-N","CONES","","",50,0.59,29.5]
["4445000000-E","BARRICADES (TYPE III)","","",64,35.090000000000003,2245.7600000000002]
["4455000000-N","FLAGGER","","",16,23.72,379.52]
["4465000000-N","TEMP CRASH CUSHIONS","","",2,5440.11,10880.22]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",215,43.52,9356.7999999999993]
["4650000000-N","TEMP RAISED PVMT MRKS","","",85,16.32,1387.2]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",4720,0.98,4625.6000000000004]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",4723.3999999999996,2.4500000000000002,11572.33]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",2060,0.92,1895.2]
["4900000000-N","PERM RAISED PVMT MARKERS","","",15,16.32,244.8]
["6000000000-E","TEMP SILT FENCE","","",4455,2.72,12117.6]
["6006000000-E","EROS CONTRL STONE CL A","","",90,34.6,3114]
["6009000000-E","EROS CONTRL STONE CL B","","",630,36.58,23045.4]
["6012000000-E","SEDIMENT CONTROL STONE","","",670,33.43,22398.1]
["6015000000-E","TEMP MULCHING","","",4,2170.6,8682.4]
["6018000000-E","SEED FOR TEMP SEEDING","","",300,3.86,1158]
["6021000000-E","FERT FOR TEMP SEEDING","","",1.5,1953,2929.5]
["6024000000-E","TEMP SLOPE DRAINS","","",200,8.42,1684]
["6029000000-E","SAFETY FENCE","","",2600,2.72,7072]
["6030000000-E","SILT EXCAVATION","","",360,9.74,3506.4]
["6036000000-E","MATTING FOR EROS CONTROL","","",7935,2.4900000000000002,19758.150000000001]
["6037000000-E","COIR FIBER MAT","","",100,8.65,865]
["6038000000-E","PERM SOIL REINF MAT","","",50,8.65,432.5]
["6042000000-E","1/4\" HARDWARE CLOTH","","",970,6.52,6324.4]
["6048000000-E","FLOAT TURBIDITY CURTAIN","","",2050,29.55,60577.5]
["6070000000-N","SPECIAL STILLING BASINS","","",12,245.98,2951.76]
["6071012000-E","COIR FIBER WATTLE","","",300,6.52,1956]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",215,5.71,1227.6500000000001]
["6071030000-E","COIR FIBER BAFFLE","","",105,8.6999999999999993,913.5]
["6084000000-E","SEEDING AND MULCHING","","",4,2915.9,11663.6]
["6087000000-E","MOWING","","",2,65.28,130.56]
["6090000000-E","SEED FOR REPAIR SEEDING","","",50,5.43,271.5]
["6093000000-E","FERT FOR REPAIR SEEDING","","",0.25,1604.84,401.21]
["6096000000-E","SEED FOR SUPP SEEDING","","",125,6.53,816.25]
["6108000000-E","FERTILIZER TOPDRESSING","","",3.25,1626.5907692307701,5286.42]
["6114500000-N","SPECIALIZED HAND MOWING","","",10,75.069999999999993,750.7]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",25,108.8,2720]
["6117500000-N","CONC WASHOUT STR","","",2,724.07,1448.14]
["6123000000-E","REFORESTATION","","",0.1,4896.1000000000004,489.61]
["8007000000-N","CM&R TEMP STR ***********","(19+77.50-LDET-)","",1,992282.95,992282.95]
["8017000000-N","CM&R TEMP ACCESS ***********","(19+78.50-L-)","",1,397578.9,397578.9]
["8035000000-N","REMV EXIST STR **********","(19+78.50-L-)","",1,148125.92000000001,148125.92000000001]
["8065000000-N","ASBESTOS ASSESSMENT","","",1,1033.6199999999999,1033.6199999999999]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",30.5,1064.77016393443,32475.49]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",28,2332.54,65311.12]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",30,244.8,7344]
["8115000000-N","CSL TESTING","","",1,2665.65,2665.65]
["8121000000-N","UNCL STR EXCAV STA *****","(19+78.50-L-)","",1,10684.66,10684.66]
["8147000000-E","REINF CONC DECK SLAB","","",10841,32.29,350055.89]
["8161000000-E","GROOVING BRIDGE FLOORS","","",9931,0.61,6057.91]
["8182000000-E","CLASS A CONC (BRIDGE)","","",177.1,892.19000564652697,158006.85]
["8210000000-N","BRG APPR SLAB ***********","(19+78.50-L-)","",1,30679.49,30679.49]
["8217000000-E","REINF STEEL (BRIDGE)","","",38527,1.1000000000000001,42379.7]
["8238000000-E","SPIRAL COL REINF STL BRG","","",3280,1.94,6363.2]
["8274000000-E","63\" MOD PRESTR CONC GIRDR","","",1239.5,298.49000403388499,369978.36]
["8475000000-E","TWO BAR METAL RAIL","","",611.13,108.910002781732,66558.17]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",641.97,112.549994548032,72253.72]
["8608000000-E","RIP RAP II (2'-0\")","","",2138,0.03,64.14]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2375,1.88,4465]
["8657000000-N","ELASTOMERIC BEARINGS","","",1,5661.58,5661.58]
["8692000000-N","FOAM JOINT SEALS","","",1,12378.41,12378.41]
["8801000000-E","MSE RETAIN WALL NO **","(1)","",1900,50.82,96558]
["8802010000-E","SOIL NAIL RETAINING WALLS","","",1617,102.95,166470.15]
["8802015100-N","SOIL NAIL VERIFICATION TESTS","","",2,652.82000000000005,1305.6400000000001]
["8802015110-N","SOIL NAIL PROOF TESTS","","",4,108.8,435.2]
["8897000000-N","GENERIC STR ITEM (EA)","9-5/8\" DIAMETER MICROPILES","",11,7329.7,80626.7]

{"sheet":"ITEMS - DIV 12","index":14,"n_rows":363,"n_cols":7,"rows_kept":363,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 12"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",10,524550,5245500]
["0000400000-N","CONST SURVEYING","","",3,118333.33333333299,355000]
["0000700000-N","FIELD OFFICE","","",1,58000,58000]
["0000996000-N","DESIGN AND CONST","","",1,260290000,260290000]
["0001000000-E","CLEARING & GRUBBING","","",1,100000,50000]
["0008000000-E","SUPP CLEARING & GRUBBING","","",1,100,100]
["0022000000-E","UNCLAS EXCAVATION","","",3500,8.71428571428571,30500]
["0029000000-N","TYPE III REINF APPR **********","(21+10.00 -L-)","",1,38000,38000]
["0036000000-E","UNDERCUT EXCAVATION","","",1930,30.233160621761701,58350]
["0043000000-N","GRADING","","",1,2885000,2885000]
["0050000000-E","SUPP CLEARING & GRUBBING","","",2,10500,21000]
["0057000000-E","UNDERCUT EXCAVATION","","",5250,27.35,143587.5]
["0106000000-E","BORROW EXCAVATION","","",22500,4.6719999999999997,105120]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",3665,17.2538199181446,63235.25]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",2050,7,14350]
["0163000000-E","REMOVAL OF EXT CONC PVMT","","",46,50,2300]
["0170000000-E","REMOVAL OF CONC PVMT SLBS","","",4600,100,460000]
["0192000000-N","PROOF ROLLING","","",60,175,10500]
["0195000000-E","SELECT GRANULAR MAT'L","","",5750,48.739130434782602,280250]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",24330,3.3281956432388,80975]
["0199000000-E","TEMP SHORING","","",1153,45,51885]
["0223000000-E","ROCK PLATING","","",525,77.349999999999994,40608.75]
["0225000000-E","REINF SOIL SLOPES","","",2000,70,140000]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETR-","OLEUM CONTAMINATED SOIL",100,114,11400]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",1098,36.775956284152997,40380]
["0320000000-E","FND CONDIT GEOTEXTILE","","",3430,2.72361516034985,9342]
["0335200000-E","15\" DRAINAGE PIPE","","",136,45,6120]
["0335300000-E","18\" DRAINAGE PIPE","","",60,50,3000]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",4,300,1200]
["0343000000-E","15\" SIDE DRAIN PIPE","","",1468,68.8,100998.39999999999]
["0344000000-E","18\" SIDE DRAIN PIPE","","",464,72.650000000000006,33709.599999999999]
["0366000000-E","15\" RC PIPE CULV III","","",4824,58.107172470978398,280309]
["0372000000-E","18\" RC PIPE CULV III","","",1592,67.701633165829193,107781]
["0378000000-E","24\" RC PIPE CULV III","","",492,82.635772357723596,40656.800000000003]
["0384000000-E","30\" RC PIPE CULV III","","",60,166,9960]
["0390000000-E","36\" RC PIPE CULV III","","",20,237,4740]
["0402000000-E","48\" RC PIPE CULV III","","",88,252,22176]
["0448200000-E","15\" RCP CULV CLASS IV","","",364,62.026373626373598,22577.599999999999]
["0448300000-E","18\" RCP CULV CLASS IV","","",80,78.8,6304]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",532,68.75,36575]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",128,75.8,9702.4]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",12,195,2340]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",16,675,10800]
["0995000000-E","PIPE REMOVAL","","",3550,28.3867605633803,100773]
["0996000000-N","PIPE CLEAN OUT","","",9,4600,41400]
["1011000000-N","FINE GRADING","","",2,397500,795000]
["1044000000-E","LIME TRTD SOIL (SLURRY)","","",95520,3.1,296112]
["1066000000-E","LIME FOR LIME TREATED SOIL","","",960,185.48,178060.79999999999]
["1099500000-E","SHALLOW UNDERCUT","","",3890,34.949871465295601,135955]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",10800,36.2222222222222,391200]
["1110000000-E","STABILIZER AGGREGATE","","",765,23,17595]
["1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",87700,2,175400]
["1121000000-E","AGGREGATE BASE COURSE","","",144630,22.038650349166801,3187450]
["1176000000-E","SOIL CEMENT BASE","","",143280,1.58,226382.4]
["1187000000-E","PC FOR SOIL CEMENT BASE","","",3950,170.14,672053]
["1209000000-E","ASPHALT CURING SEAL","","",35820,2.2999999999999998,82386]
["1220000000-E","INCIDENTAL STONE BASE","","",10867,26.4610288027975,287552]
["1231000000-E","SHOULDER BORROW","","",10000,0.01,100]
["1245000000-E","SHOULDER RECONST","","",391.32,2271.0028365531998,888688.83]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",53697,24.086205933292401,1293357]
["1264000000-E","DITCHING","","",50,15,750]
["1275000000-E","PRIME COAT","","",96880,2.54190751445087,246260]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",44400,1.75,77700]
["","","(1-1/2\")","",428736,1.7987080627705601,771170.9]
["","","(2\")","",349150,2.75,960162.5]
["","","(2-5/8\")","",281600,2.95,830720]
["","","(5-1/2\")","",144040,3.25,468130]
["","","(5/8\")","",309760,2.4500000000000002,758912]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",65803,1.95699238636536,128775.97]
["","","(0\" TO 3\")","",730,10.95,7993.5]
["","","(1-1/2\" TO 3\")","",16052,2.1,33709.199999999997]
["1330000000-E","INCIDENTAL MILLING","","",34691,11.3850710558935,394959.5]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",72825,57.608554754548599,4195343]
["1498000000-E","ASP CONC INTR CRS I19.0B","","",7200,50,360000]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",64060,50.840699344364701,3256855.2]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",52910,49.030686070686102,2594213.6]
["1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",4245,48.682685512367499,206658]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",301232,45.408308214266697,13678435.5]
["1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",21074,43.413898642877498,914904.5]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",101060,54,5457240]
["1575000000-E","ASP FOR PLANT MIX","","",29639,500.38445966463098,14830895]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",6595,700,4616500]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",100,125,12500]
["1704000000-E","PATCHING EXIST PVMT","","",44164,103.392355764876,4566220]
["1771000000-E","AST, MAT COAT, 6M STONE","","",282104,1,282104]
["1838000000-E","EMULSION FOR AST","","",112842,2,225684]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",15990,125,1998750]
["1840000000-E","MILLED RUMBLE STRIPS","","",610169,0.16113337452411,98318.59]
["1881000000-E","GENERIC PAVING ITEM (LF)","MILLED RUMBLE STRIPS, ASPHALT","CONCRETE (CENTERLINE)",11088,0.22,2439.36]
["2022000000-E","SUBDRAIN EXCAVATION","","",706,26.133711048158599,18450.400000000001]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",3100,2,6200]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",521,60.792706333973101,31673]
["2044000000-E","6\" PERF SUBDRN PIPE","","",3100,5.6451612903225801,17500]
["2070000000-N","SUBDRN PIPE OUTLET","","",7,342.857142857143,2400]
["2077000000-E","6\" OUTLET PIPE","","",42,17.285714285714299,726]
["2143000000-E","BLOTTING SAND","","",31,75,2325]
["2209000000-E","ENDWALLS","","",15.4,1600,24640]
["2253000000-E","PIPE COLLARS","","",17.940000000000001,1230,22066.2]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",77,1208.4415584415599,93050]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",22.5,262.66666666666703,5910]
["2354200000-N","FRAME W/GRATE 840.24 STD","","",1,465,465]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",15,552,8280]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",1,1000,1000]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",16,624.5,9992]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",25,585.32000000000005,14633]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",2,791,1582]
["","","(F)","",10,615.79999999999995,6158]
["","","(G)","",5,689.6,3448]
["2396000000-N","FRAME W/COVER STD 840.54","","",4,825,3300]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",11,885,9735]
["2473000000-N","GENERIC DRAINAGE ITEM (EA)","ADJUSTMENT OF JUNCTION BOXES","",2,2000,4000]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",6645,20.009932279909702,132966]
["2556000000-E","SHOULDER BERM GUTTER","","",5810,21.137779690189301,122810.5]
["2577000000-E","CONC EXPRESSWAY GUTTER","","",11050,26.345927601810001,291122.5]
["2600000000-N","RETROFIT EXT CURB RAMPS","","",86,875.34883720930202,75280]
["2605000000-N","CONC CURB RAMPS","","",58,2886.2068965517201,167400]
["2612000000-E","6\" CONC DRIVEWAY","","",1090,108.02752293578,117750]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",3400,45.35,154190]
["2724000000-E","PC REINF BARRIER SNGL FC","","",1378,242.92452830188699,334750]
["2738000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE ISLAND CAP","",170,350,59500]
["2738100000-E","GENERIC PAVING ITEM (SF)","PATCHING CONCRETE PAVEMENT SPALLS","",11000,199,2189000]
["2800000000-N","ADJ CATCH BASINS","","",3,1133.3333333333301,3400]
["2815000000-N","ADJ DROP INLETS","","",20,1623.75,32475]
["2830000000-N","ADJ MANHOLES","","",194,1157.0876288659799,224475]
["2845000000-N","ADJ METER OR VALVE BOXES","","",194,965.46391752577301,187300]
["2995000000-N","GENERIC DRAINAGE ITEM (EA)","ADJUSTMENT OF COMMUNICATION/","OVERSIZE MANHOLES",10,2150,21500]
["","","ADJUSTMENT OF OVERSIZED","MANHOLES",3,3200,9600]
["3000000000-N","IMPACT ATTEN TYPE 350","","",20,23400,468000]
["3030000000-E","STL BEAM GUARDRAIL","","",189125,17.2088037012558,3254615]
["3045000000-E","SBGR SHOP CURVED","","",37.5,21.1,791.25]
["3075000000-E","TRIPLE CORRUGATED SBGR","","",500,29.4,14700]
["3135000000-N","W-TR SBGR TRANS SECTIONS","","",51,157.5,8032.5]
["3145000000-E","EX LENGTH GR POST ** STL","(8')","",30,58,1740]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",80,34.462499999999999,2757]
["3165500000-N","GR END UNIT TYPE **********","(BIC)","",1,2100,2100]
["3195000000-N","GR END TYPE AT-1","","",1,580,580]
["3210000000-N","GR END TYPE CAT-1","","",92,689.02173913043498,63390]
["3215000000-N","GR ANCHOR TYPE III","","",4,1850,7400]
["3287000000-N","GR END TYPE TL-3","","",190,2933.2368421052602,557315]
["3317000000-N","GR ANCHOR TYPE B-77","","",80,1603.5,128280]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",75,12,900]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",120106,2.09995837010641,252217.60000000001]
["3365000000-E","REMOVE EXISTING GUIDERAIL","","",3000,1.05,3150]
["3380000000-E","TEMP STL BM GUARDRAIL","","",325,12,3900]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(III)","",2,1100,2200]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",2,2900,5800]
["3389400000-E","DBL FACED CABLE GUIDERAIL","","",26500,6.75,178875]
["3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",60,42.1666666666667,2530]
["3389600000-N","CBL GUIDERAIL ANCH UNIT","","",71,1687.60563380282,119820]
["3575000000-E","GENERIC FENCING ITEM (LF)","TEMPORARY 72\" CHAIN LINK FENCE","WITH POSTS",286,18,5148]
["3628000000-E","RIP RAP, CLASS I","","",562,62.213523131672602,34964]
["3635000000-E","RIP RAP, CLASS II","","",740,50,37000]
["3649000000-E","RIP RAP, CLASS B","","",1142,68.019001751313496,77677.7]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",9355,2.5034206306787801,23419.5]
["3659000000-N","PREFORMED SCOUR HOLES","","",3,4500,13500]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(A)","",3156,17,53652]
["","","(B)","",419,17,7123]
["","","(D)","",184,17.244565217391301,3173]
["","","(E)","",1400,16.7042857142857,23386]
["","","(F)","",86,16.665697674418599,1433.25]
["4048000000-E","REINF CONC FOUNDTN","","",22,950,20900]
["4054000000-E","PLN CONC FOUNDTN","","",2,400,800]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",11855,5.5,65202.5]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",9349,5.5,51419.5]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",4676,7.0045979469632202,32753.5]
["4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",12,55,660]
["4096000000-N","SIGN ERECTION, TYPE D","","",23,153.04347826086999,3520]
["4102000000-N","SIGN ERECTION, TYPE E","","",177,73.336158192090394,12980.5]
["4108000000-N","SIGN ERECTION, TYPE F","","",10,144.6,1446]
["4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",8,950,7600]
["","","(B)","",2,450,900]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",23,650,14950]
["","","(B)","",15,275,4125]
["4114000000-N","SIGN ERECTION, MILEMARKERS","","",12,100,1200]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(F)","",1,250,250]
["","","(MILEMARKER)","",2,100,200]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",50,7.04,352]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",23,7.5869565217391299,174.5]
["4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",1,1.5,1.5]
["4237000000-N","STOCKPILE SIGN, D, E, F","","",28,10.6,296.8]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",2330,12.409484978540799,28914.1]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",1109,9.0692515779981999,10057.799999999999]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",329,9.7234042553191493,3199]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",31085,11.671610101335,362812]
["4415000000-N","FLASHING ARROW BOARD","","",7,728.57142857142901,5100]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",4,8200,32800]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",76,60,4560]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",4,6825,27300]
["4424000000-N","WZ PRESENCE LIGHTING","","",15,4725,70875]
["4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",1,12000,12000]
["4430000000-N","DRUMS","","",716,42.229050279329599,30236]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",16,131.25,2100]
["4435000000-N","CONES","","",145,17.724137931034502,2570]
["4445000000-E","BARRICADES (TYPE III)","","",459,25.620915032679701,11760]
["4455000000-N","FLAGGER","","",1795,394.99164345403898,709010]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",4,192875,771500]
["4465000000-N","TEMP CRASH CUSHIONS","","",6,6543.3333333333303,39260]
["4470000000-N","REM & RES CRASH CUSHION","","",4,2500,10000]
["4480000000-N","TMA","","",5,9080,45400]
["4485000000-E","PORT CONC BARRIER","","",345,19.5,6727.5]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",815,35,28525]
["4505000000-E","REM & RES PORT CONC BARR, ANCH","","",150,15,2250]
["4508000000-E","REM & RES H2O FILL BARR","","",820,50,41000]
["4510000000-N","LAW ENFORCEMENT","","",1849,57.677122769064397,106645]
["4516000000-N","SKINNY DRUM","","",158,27.867088607594901,4403]
["4520000000-N","TUBULAR MARKERS (FIXED)","","",15,65,975]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","LANE CLOSURE","",590,3412.5,2013375]
["","","RAMP/LOOP CLOSURE","",40,3412.5,136500]
["4650000000-N","TEMP RAISED PVMT MRKS","","",187,13.9304812834225,2605]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",96071,0.84350147286902,81036.03]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",117758,0.86794731568131001,102207.74]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",3898,2.5990251410980001,10131]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",4022,2.9210591745400301,11748.5]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",7875,3.2223492063492101,25376]
["4705000000-E","THERMO LINES 16\" 120MILS","","",1000,7.05,7050]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",10102,10.596901603642801,107049.9]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",216,130.09259259259301,28100]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",950,145.19999999999999,137940]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",1050,2,2100]
["","","(III)","",988,8,7904]
["","","(IV)","",1351,3.5903034789045201,4850.5]
["4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(III)","",125,16,2000]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",7280339,0.13382269973967001,974274.62]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",808590,0.27258175342261998,220406.88]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",1012,1,1012]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",28566,0.69624728698452998,19889]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",2542,3,7626]
["4840000000-N","PAINT PVT MKG CHARACTER","","",24,55,1320]
["4845000000-N","PAINT PVT MKG SYMBOL","","",403,67.116625310173703,27048]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",940,4.3600000000000003,4098.3999999999996]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",144444,0.92,132888.48000000001]
["4847040000-E","POLYUREA LINES (6\", 30 MILS)","","",511576,1.6,818521.59999999998]
["4847070000-E","POLYUREA LINES (12\", 20 MILS)","","",4717,1.75,8254.75]
["4847080000-E","POLYUREA LINES (12\", 30 MILS)","","",14000,3.62,50680]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",17291,0.92630559250476996,16016.75]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",19890,0.86273504273503998,17159.8]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",400,2,800]
["4865000000-E","LINE REMOVAL 12\" WIDE","","",1950,4,7800]
["4900000000-N","PERM RAISED PVMT MARKERS","","",4499,11.2589508779729,50654.02]
["4905000000-N","SNOWPLB PVMT MRKER","","",15159,25.938617323042401,393203.5]
["4935000000-N","FLEX DELINATR (CRYSTAL)","","",154,55,8470]
["4940000000-N","FLEX DELINATR (YELLOW)","","",134,55,7370]
["4945000000-N","FLEX DELINATR (CRY & RED)","","",15,55,825]
["4950000000-N","FLEX DELINATR (YEL & RED)","","",15,55,825]
["5255000000-N","PORTABLE LIGHTING","","",5,383200,1916000]
["6000000000-E","TEMP SILT FENCE","","",25110,3.9667463162086798,99605]
["6006000000-E","EROS CONTRL STONE CL A","","",2325,38.723440860215,90032]
["6009000000-E","EROS CONTRL STONE CL B","","",11880,38.111531986532,452765]
["6012000000-E","SEDIMENT CONTROL STONE","","",5380,38.879182156133801,209170]
["6015000000-E","TEMP MULCHING","","",57.5,1263.04347826087,72625]
["6018000000-E","SEED FOR TEMP SEEDING","","",2900,3.1379310344827598,9100]
["6021000000-E","FERT FOR TEMP SEEDING","","",17,644.41176470588198,10955]
["6024000000-E","TEMP SLOPE DRAINS","","",4285,13.36756126021,57280]
["6029000000-E","SAFETY FENCE","","",1800,2.8,5040]
["6030000000-E","SILT EXCAVATION","","",22630,12.3923994697304,280440]
["6036000000-E","MATTING FOR EROS CONTROL","","",115700,1.3465427830596399,155795]
["6037000000-E","COIR FIBER MAT","","",2660,3.6964285714285698,9832.5]
["6038000000-E","PERM SOIL REINF MAT","","",2160,4.8370370370370397,10448]
["6042000000-E","1/4\" HARDWARE CLOTH","","",6660,4.4677177177177203,29755]
["6070000000-N","SPECIAL STILLING BASINS","","",20,250,5000]
["6071010000-E","WATTLE","","",1450,7.6551724137930997,11100]
["6071012000-E","COIR FIBER WATTLE","","",120,15.85,1902]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1935,9.8488372093023298,19057.5]
["6071030000-E","COIR FIBER BAFFLE","","",2105,6.5655581947743498,13820.5]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",16,1162.5,18600]
["","","(2\")","",1,1250,1250]
["6084000000-E","SEEDING AND MULCHING","","",49,1985,97265]
["6087000000-E","MOWING","","",48,78.0625,3747]
["6090000000-E","SEED FOR REPAIR SEEDING","","",750,6.6566666666666698,4992.5]
["6093000000-E","FERT FOR REPAIR SEEDING","","",2,1062.5,2125]
["6096000000-E","SEED FOR SUPP SEEDING","","",1150,4.6934782608695702,5397.5]
["6108000000-E","FERTILIZER TOPDRESSING","","",33.5,631.23134328358196,21146.25]
["6111000000-E","IMPERVIOUS DIKE","","",275,42.25,11618.75]
["6114500000-N","SPECIALIZED HAND MOWING","","",70,86.428571428571402,6050]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",128,291.40625,37300]
["6117500000-N","CONC WASHOUT STR","","",33,1106.8181818181799,36525]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",12,200,2400]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",4,200,800]
["6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","REMOVAL OF EROSION CONTROL DEVICES","",1,65000,65000]
["7060000000-E","SIGNAL CABLE","","",1850,2.48648648648649,4600]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",13,925.38461538461502,12030]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",3,1130,3390]
["7252000000-E","MESSENGER CABLE (1/4\")","","",1900,2,3800]
["7264000000-E","MESSENGER CABLE (3/8\")","","",300,3.5,1050]
["7279000000-E","TRACER WIRE","","",5100,0.6,3060]
["7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",225,28,6300]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",5075,6.9660098522167502,35352.5]
["","","(3, 2\")","",10,11.5,115]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",670,18.089552238806,12120]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",26,356.730769230769,9275]
["7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",24,680,16320]
["7360000000-N","WOOD POLE","","",10,1036.5,10365]
["7372000000-N","GUY ASSEMBLY","","",11,390.90909090909099,4300]
["7408000000-E","1\" RISER WITH WEATHERHEAD","","",1,425,425]
["7420000000-E","2\" RISER WITH WEATHERHEAD","","",4,525,2100]
["7432000000-E","2\" RISER WITH TUBING","","",4,642,2568]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",27114,7.6757025890683801,208119]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",12820,2.1396255850234001,27430]
["7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(24)","",7800,2.06,16068]
["7528000000-E","DROP CABLE","","",410,1.85,758.5]
["7540000000-N","SPLICE ENCLOSURE","","",5,1420,7100]
["7552000000-N","INTERCONNECT CENTER","","",5,1520,7600]
["7566000000-N","DELINEATOR MARKER","","",3,123,369]
["7636000000-N","SIGN FOR SIGNALS","","",2,425,850]
["7684000000-N","SIGNAL CABINET FOUND","","",1,1200,1200]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",3,13708.333333333299,41125]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",13,145.38461538461499,1890]
["7901000000-N","CABINET BASE EXTENDER","","",3,353.33333333333297,1060]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","CCTV CAMERA ASSEMBLY","",3,2900,8700]
["","","ETHERNET EDGE SWITCH","",5,1395,6975]
["","","JUNCTION BOX MARKER","",21,64,1344]
["","","MICROWAVE VEHICLE DETECTOR -","SINGLE ZONE",1,900,900]
["8017000000-N","CM&R TEMP ACCESS ***********","(21+10.00 -L-)","",1,79000,79000]
["8035000000-N","REMV EXIST STR **********","(21+10.00 -L-)","",1,70000,70000]
["8065000000-N","ASBESTOS ASSESSMENT","","",1,1500,1500]
["8096000000-E","PILE EXCAVATION IN SOIL","","",70,50,3500]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",40,190,7600]
["8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",135.5,1220,165310]
["8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",88,1220,107360]
["8111400000-E","PERM STL CASING FOR 3'-6\" PIER","","",105,280,29400]
["8115000000-N","CSL TESTING","","",1,3500,3500]
["8121000000-N","UNCL STR EXCAV STA *****","(21+10.00 -L-)","",1,8000,8000]
["8126000000-N","CULV EXCAV @ ************","(324+60.00-L-)","",1,10550,10550]
["","","(42+19.00-L-)","",1,10550,10550]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",87,53,4611]
["8147000000-E","REINF CONC DECK SLAB","","",13068,28,365904]
["8161000000-E","GROOVING BRIDGE FLOORS","","",19331,0.76163416274378004,14723.15]
["8182000000-E","CLASS A CONC (BRIDGE)","","",371.8,800,297440]
["8196000000-E","CLASS A CONC (CULV)","","",174.1,845,147114.5]
["8210000000-N","BRG APPR SLAB ***********","(21+10.00 -L-)","",1,68000,68000]
["8217000000-E","REINF STEEL (BRIDGE)","","",68630,1.07,73434.100000000006]
["8238000000-E","SPIRAL COL REINF STL BRG","","",7045,2.5,17612.5]
["8245000000-E","REINF STEEL (CULVERT)","","",22579,1.6,36126.400000000001]
["8262000000-E","45\" PRESTR CONC GIRDR","","",1660,255,423300]
["8296000000-N","POLLUTION CONTROL","","",1,2725,2725]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",34,450,15300]
["8364000000-E","HP12X53 PILES","","",805,35,28175]
["8475000000-E","TWO BAR METAL RAIL","","",406.8,112,45561.599999999999]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 3'-3\")","",441.4,100,44140]
["8559000000-E","SURFACE PREP, CLASS II","","",8,300,2400]
["8566000000-E","SURFACE PREP, CLASS III","","",2,600,1200]
["8608000000-E","RIP RAP II (2'-0\")","","",887,50,44350]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",985,2,1970]
["8657000000-N","ELASTOMERIC BEARINGS","","",1,25000,25000]
["8660000000-E","CONC REPAIRS","","",7.64,750,5730]
["8664000000-E","SHOTCRETE REPAIRS","","",158.5,750,118875]
["8678000000-E","EPOXY RESIN INJECTION","","",21.36,35,747.6]
["8706000000-N","EXPANSION JOINT SEALS","","",1,90000,90000]
["8860000000-N","GENERIC STR ITEM (LS)","PAINTING CONTAINMENT","FOR BRIDGE NO 39",1,8175,8175]
["","","VOLUMETRIC MIXER","",1,1000,1000]
["8867000000-E","GENERIC STR ITEM (LF)","FOAM JOINT SEALS FOR","PRESERVATION",80.400000000000006,72,5788.8]
["8881000000-E","GENERIC STR ITEM (CY)","LATEX MODIFIED CONC. OVERLAY-","VERY EARLY STRENGTH",21.3,1200,25560]
["8882000000-E","GENERIC STR ITEM (CF)","CONCRETE FOR DECK REPAIR","",208.3,25,5207.5]
["","","ELASTOMERIC CONCRETE FOR","PRESERVATION",20.100000000000001,525,10552.5]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",80.400000000000006,40,3216]
["","","EPOXY COATING","",450.4,32,14412.8]
["8893000000-E","GENERIC STR ITEM (SY)","HYDRO-DEMOLITION OF BRIDGE","DECK",624,68.319999999999993,42631.68]
["","","PLACING & FINISHING OF LATEX MODIFIED","CONC OVERLAY-VERY EARLY STRENGTH",614.4,75,46080]
["","","SCARIFYING BRIDGE DECK","",624,32.659999999999997,20379.84]
["8897000000-N","GENERIC STR ITEM (EA)","CLEANING & PAINTING EXISTING","BEARINGS WITH HRSCA BRIDGE NO 39",32,817.5,26160]
["","","TYPE I BRIDGE JACKING BRIDGE NO 39","",7,2000,14000]

{"sheet":"ITEMS - DIV 13","index":15,"n_rows":541,"n_cols":7,"rows_kept":541,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 13"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",16,406023.44374999998,6496375.0999999996]
["0000400000-N","CONST SURVEYING","","",5,18695,93475]
["0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN & CONSTRUCTION OF","BRIDGES",2,1860900,3721800]
["","","MOBILIZATION","",1,449500,449500]
["0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","END BENTS STRUCTURE 100088","",2,62000,124000]
["","","END BENTS STRUCTURE 100099","",2,45000,90000]
["","","END BENTS STRUCTURE 100100","",2,42000,84000]
["","","END BENTS STRUCTURE 110126","",2,30000,60000]
["","","END BENTS STRUCTURE 580108","",2,36000,72000]
["","","END BENTS STRUCTURE 600157","",2,70000,140000]
["","","END BENTS STRUCTURE 800058","",2,31000,62000]
["","","END BENTS STRUCTURE 800088","",2,41000,82000]
["","","END BENTS STRUCTURE 800265","",2,28500,57000]
["","","INTERIOR BENT CAPS STRUCTURE 580108","",2,36000,72000]
["","","INTERIOR BENT CAPS STRUCTURE 800058","",1,34000,34000]
["","","RIGHT OF WAY ACQUISITION","",18,4088.8888888888901,73600]
["0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT 1 STRUCTURE 100088",10,4500,45000]
["","","","BENT 1 STRUCTURE 100099",28,0.01,0.28000000000000003]
["","","","BENT 1 STRUCTURE 100100",19,0.01,0.19]
["","","","BENT 1 STRUCTURE 110126",35,190,6650]
["","","","BENT 1 STRUCTURE 580108",11,2675,29425]
["","","","BENT 1 STRUCTURE 600157",20,0.01,0.2]
["","","","BENT 1 STRUCTURE 800058",14,252.5,3535]
["","","","BENT 1 STRUCTURE 800088",30,175,5250]
["","","","BENT 1 STRUCTURE 800265",18,255,4590]
["","","","BENT 2 STRUCTURE 100088",26,0.01,0.26]
["","","","BENT 2 STRUCTURE 100099",33,0.01,0.33]
["","","","BENT 2 STRUCTURE 100100",15,0.01,0.15]
["","","","BENT 2 STRUCTURE 110126",27,190,5130]
["","","","BENT 2 STRUCTURE 580108",27,320,8640]
["","","","BENT 2 STRUCTURE 600157",29,0.01,0.28999999999999998]
["","","","BENT 2 STRUCTURE 800058",20,252.5,5050]
["","","","BENT 2 STRUCTURE 800088",17,217,3689]
["","","","BENT 2 STRUCTURE 800265",17,252.5,4292.5]
["","","AVE FOUNDATION LENGTH AT INTE-","RIOR BENT 1 STRUCTURE 580108",29,3000,87000]
["","","","RIOR BENT 1 STRUCTURE 800058",27,2285,61695]
["","","","RIOR BENT 2 STRUCTURE 580108",29,3000,87000]
["","","BRIDGE LENGTH STRUCTURE 100088","",70,3005,210350]
["","","BRIDGE LENGTH STRUCTURE 100099","",50,3000,150000]
["","","BRIDGE LENGTH STRUCTURE 100100","",70,3100,217000]
["","","BRIDGE LENGTH STRUCTURE 110126","",60,1555,93300]
["","","BRIDGE LENGTH STRUCTURE 580108","",170,1730,294100]
["","","BRIDGE LENGTH STRUCTURE 600157","",50,2800,140000]
["","","BRIDGE LENGTH STRUCTURE 800058","",120,2215,265800]
["","","BRIDGE LENGTH STRUCTURE 800088","",100,2750,275000]
["","","BRIDGE LENGTH STRUCTURE 800265","",60,1455,87300]
["0028000000-N","TYPE I STANDARD APPR **********","(14+21.00)","",1,11800,11800]
["","","(28+26.49 WB)","",1,140000,140000]
["","","(28+45.42 EB)","",1,140000,140000]
["0030000000-N","TYPE II MOD APPR **********","(10+53.50)","",1,24000,24000]
["","","(15+54.50 -L-)","",1,15000,15000]
["0036000000-E","UNDERCUT EXCAVATION","","",1295,27.895752895752899,36125]
["0043000000-N","GRADING","","",5,241478.43799999999,1207392.19]
["0050000000-E","SUPP CLEARING & GRUBBING","","",6,2458.3150000000001,14749.89]
["0057000000-E","UNDERCUT EXCAVATION","","",1550,15.2645161290323,23660]
["0063000000-N","GRADING","","",1,1860657,1860657]
["0106000000-E","BORROW EXCAVATION","","",1300,56,72800]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",1815,12.9029752066116,23418.9]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",400,34.875,13950]
["0195000000-E","SELECT GRANULAR MAT'L","","",1400,50.8642857142857,71210]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",8075,4.1157894736842104,33235]
["0199000000-E","TEMP SHORING","","",7153,58.314693135747198,417125]
["0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,77.5,3875]
["","","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",50,150,7500]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",1351,35.687490747594403,48213.8]
["0320000000-E","FND CONDIT GEOTEXTILE","","",4180,2.9072966507176998,12152.5]
["0335200000-E","15\" DRAINAGE PIPE","","",1096,45.893284671532797,50299.040000000001]
["0335300000-E","18\" DRAINAGE PIPE","","",68,65,4420]
["0335400000-E","24\" DRAINAGE PIPE","","",84,67.7542857142857,5691.36]
["0335500000-E","30\" DRAINAGE PIPE","","",52,74.510000000000005,3874.52]
["0343000000-E","15\" SIDE DRAIN PIPE","","",56,44,2464]
["0366000000-E","15\" RC PIPE CULV III","","",60,30,1800]
["0372000000-E","18\" RC PIPE CULV III","","",396,48.813131313131301,19330]
["0378000000-E","24\" RC PIPE CULV III","","",56,45,2520]
["0384000000-E","30\" RC PIPE CULV III","","",32,55,1760]
["0390000000-E","36\" RC PIPE CULV III","","",68,120,8160]
["0396000000-E","42\" RC PIPE CULV III","","",76,175,13300]
["0408000000-E","54\" RC PIPE CULV III","","",144,1048.23,150945.12]
["0448200000-E","15\" RCP CULV CLASS IV","","",2780,44.836345323741,124645.04]
["0448300000-E","18\" RCP CULV CLASS IV","","",1192,60.6122483221477,72249.8]
["0448400000-E","24\" RCP CULV CLASS IV","","",1192,66.077651006711406,78764.56]
["0448500000-E","30\" RCP CULV CLASS IV","","",992,101.485322580645,100673.44]
["0448600000-E","36\" RCP CULV CLASS IV","","",192,135,25920]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",646,50.311764705882297,32501.4]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",40,60,2400]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",112,78,8736]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",128,105,13440]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",9,250,2250]
["","","(24\", 0.064\")","",4,350,1400]
["","","(30\", 0.079\")","",2,850,1700]
["0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(24\", 0.375\")","",83,255,21165]
["","","(30\", 0.375\")","",205,305,62525]
["0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(24\", 0.375\")","",83,1450,120350]
["","","(30\", 0.375\")","",205,1450,297250]
["0995000000-E","PIPE REMOVAL","","",6213,15.4814952518912,96186.53]
["1000000000-E","6\" SLOPE PROTECTION","","",240,95,22800]
["1099500000-E","SHALLOW UNDERCUT","","",850,11.4117647058823,9700]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",1550,27.5045161290323,42632]
["1121000000-E","AGGREGATE BASE COURSE","","",3752,29.368603411513899,110191]
["1220000000-E","INCIDENTAL STONE BASE","","",9228,29.052015604681401,268092]
["1245000000-E","SHOULDER RECONST","","",308.69,4193.3719913181503,1294452]
["1260000000-E","AGGREGATE SHOULDER BORROW","","",35997,16.991054810123099,611627]
["1275000000-E","PRIME COAT","","",942,16.471868365180502,15516.5]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",2500,4,10000]
["","","(1-1/2\")","",343966,2.7665301221632399,951592.3]
["","","(1-1/4\")","",187,5.95,1112.6500000000001]
["","","(1/2\")","",20850,5.75,119887.5]
["","","(2\")","",213211,2.9,618311.9]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",43416,4.6151027271052101,200369.3]
["","","(0\" TO 4\")","",8037,30,241110]
["1330000000-E","INCIDENTAL MILLING","","",52391,9.2469908953827904,484459.1]
["1489000000-E","ASP CONC BASE CRS B25.0B","","",1200,102.425,122910]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",24130,68.702279320348097,1657786]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",15305,68.158314276380295,1043163]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",112964,49.707136786941,5615117]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",98419,55.913837775226298,5502984]
["1524200000-E","ASP CONC SURF CRS S9.5D","","",42324,57.140251394008096,2418404]
["1525000000-E","ASP CONC SURF CRS SF9.5A","","",1060,111.811320754717,118520]
["1575000000-E","ASP FOR PLANT MIX","","",15744,615.06972815040604,9683657.8000000007]
["1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",5027,721.88084344539504,3628895]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",310,239.712903225806,74311]
["1704000000-E","PATCHING EXIST PVMT","","",49731,140.12577667853,6968595]
["1735000000-E","REP JNT CONC PVT SLABS","","",3975,465,1848375]
["1736000000-E","SELECT MAT'L, CLASS IV","","",1900,45,85500]
["1737000000-E","PATCHING CONC PVMT SPALLS","","",1000,150,150000]
["1803500000-E","AST, DOUBLE SEAL","","",662323,1.5154067275332399,1003688.73]
["1820000000-E","AST, FOG SEAL","","",662323,0.53568112537236001,354793.93]
["1838000000-E","EMULSION FOR AST","","",364348,2.0513094898284101,747390.51]
["1838500000-N","VACUUM TRUCK","","",26,4911.5384615384601,127700]
["1839140000-E","ULTRATHIN BOND WEAR CRS","","",54000,122,6588000]
["1840000000-E","MILLED RUMBLE STRIPS","","",770893,0.16467072602812999,126943.51]
["1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR,","AND SEALING",1047712,2,2095424]
["1891000000-E","GENERIC PAVING ITEM (SY)","DIAMOND GRINDING PCC PAVEMENT","",654820,4.49,2940141.8]
["","","FINE MILLING (1-1/2\")","",760000,2.15,1634000]
["","","FINE MILLING (5/8\")","",605000,2.0499999999999998,1240250]
["","","LATEX MODIFIED MICRO-SURFACING","TYPE III",118720,3.06335865902965,363681.94]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",129,190.13302325581401,24527.16]
["2022000000-E","SUBDRAIN EXCAVATION","","",292.2,27.1267282683094,7926.43]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",1300,3.1,4030]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",219.4,54.997082953509597,12066.36]
["2044000000-E","6\" PERF SUBDRN PIPE","","",1300,14.4384615384615,18770]
["2070000000-N","SUBDRN PIPE OUTLET","","",6,313.65166666666698,1881.91]
["2077000000-E","6\" OUTLET PIPE","","",36,33.5566666666667,1208.04]
["2165000000-E","12\" FUNNEL DRAIN PIPE","","",30,93,2790]
["2190000000-N","TEMP STL PLT COVER FOR MDS","","",2,1136.5450000000001,2273.09]
["2209000000-E","ENDWALLS","","",4.5,1200,5400]
["2253000000-E","PIPE COLLARS","","",0.39900000000000002,1524.4611528822099,608.26]
["2264000000-E","PIPE PLUGS","","",0.497,851.16700201207198,423.03]
["2275000000-E","FLOWABLE FILL","","",91,385.63626373626403,35092.9]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",117,1674.2897435897401,195891.9]
["2297000000-E","MASNRY DRAINAGE STRUCT","","",24.22,898.36994219653195,21758.52]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",36.700000000000003,374.32425068119898,13737.7]
["2355000000-N","FRAME W/GRATE 840.29 STD","","",4,600,2400]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",16,553.34375,8853.5]
["2364200000-N","FRAME W/2GRTS 840.20 STD","","",5,750,3750]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",22,738.88,16255.36]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",7,1015.0514285714301,7105.36]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",3,657.50333333333299,1972.51]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",7,630.57000000000005,4413.99]
["","","(F)","",17,630.57000000000005,10719.69]
["","","(G)","",22,630.57000000000005,13872.54]
["2396000000-N","FRAME W/COVER STD 840.54","","",9,500,4500]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",2,2215,4430]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",1,487.55,487.55]
["2473000000-N","GENERIC DRAINAGE ITEM (EA)","DRAINAGE STRUCTURE CLEANOUT","",10,550,5500]
["","","REMOVE AND REPLACE CONCRETE APRON","",70,2424.6428571428601,169725]
["","","REMOVE AND REPLACE METAL FUN- NELS","",1,2270,2270]
["2484000000-E","GENERIC DRAINAGE ITEM (LF)","MODIFIED SHOULDER BERM GUTTER","",28,83.5,2338]
["2489000000-E","GENERIC DRAINAGE ITEM (SY)","REMOVE & REPLACE 4\" CONC PAVEDDITCH","",2000,100,200000]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",690,20.27,13986.3]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",6780,21.28,144278.39999999999]
["2556000000-E","SHOULDER BERM GUTTER","","",270,30,8100]
["2570000000-N","MOD CONC FLUME","","",2,2500,5000]
["2591000000-E","4\" CONC SIDEWALK","","",3390,39.69,134549.1]
["2605000000-N","CONC CURB RAMPS","","",166,2492.7987951807199,413804.6]
["2612000000-E","6\" CONC DRIVEWAY","","",6000,46,276000]
["2613000000-N","REM & REP CURB RAMPS","","",1,1807.09,1807.09]
["2619000000-E","4\" CONC PAVED DITCH","","",15603,89.998192655258606,1404241.8]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",60,72.09,4325.3999999999996]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",270,88.502222222222201,23895.599999999999]
["2738000000-E","GENERIC PAVING ITEM (SY)","REMOVE AND REPLACE 4\" CONCRETE","PAVED DITCH",577,92,53084]
["2752000000-E","GENERIC PAVING ITEM (LF)","MODIFIED SHOULDER BERM","GUTTER",135,40,5400]
["2815000000-N","ADJ DROP INLETS","","",15,950,14250]
["2830000000-N","ADJ MANHOLES","","",166,1105.6680722891599,183540.9]
["2845000000-N","ADJ METER OR VALVE BOXES","","",158,934.90727848101301,147715.35]
["2905000000-N","CONVERT DI TO JB","","",2,905.01,1810.02]
["2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXT DROP INLET TO TB","DROP INLET",1,4470,4470]
["3030000000-E","STL BEAM GUARDRAIL","","",142887.5,16.3473676843671,2335834.5]
["3045000000-E","SBGR SHOP CURVED","","",350,25.741085714285699,9009.3799999999992]
["3060000000-E","SBGR DOUBLE FACED","","",155550,22.024590163934398,3425925]
["3075000000-E","TRIPLE CORRUGATED SBGR","","",262.5,124.571428571429,32700]
["3120000000-E","20\"TUBULAR 3C GUARDRAIL","","",3622,178.60298177802301,646900]
["3145000000-E","EX LENGTH GR POST ** STL","(8')","",16,147.76,2364.16]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",45,30.5622222222222,1375.3]
["3180000000-N","GR ANCHOR TYPE **********","(B-83, SHOP CURVED)","",3,2100,6300]
["","","(III MOD)","",6,1950,11700]
["","","(III, SHOP CURVED)","",2,1850,3700]
["3195000000-N","GR END TYPE AT-1","","",8,713.75,5710]
["3210000000-N","GR END TYPE CAT-1","","",238,551.99579831932795,131375]
["3215000000-N","GR ANCHOR TYPE III","","",51,1034.7058823529401,52770]
["3287000000-N","GR END TYPE TL-3","","",245,2984.6938775510198,731250]
["3288000000-N","GR END TYPE TL-2","","",8,3075,24600]
["3317000000-N","GR ANCHOR TYPE B-77","","",60,1920,115200]
["3319000000-N","GR ANCHOR TYPE B-83","","",16,1650,26400]
["3345000000-E","REMOVE & RESET GUARDRAIL","","",1615,19,30685]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",214193,2.49135125797762,533630]
["3380000000-E","TEMP STL BM GUARDRAIL","","",4612.5,12.139295392953899,55992.5]
["3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",87.5,14.214285714285699,1243.75]
["3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",12,950,11400]
["","","(B-83)","",4,950,3800]
["","","(III)","",8,825,6600]
["","","(III-MODIFIED)","",2,1250,2500]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",8,2875,23000]
["","","(TL-3)","",1,2800,2800]
["3420000000-E","GENERIC GUARDRAIL ITEM (LF)","REMOVE AND REPLACE EXISTING GUARDRAIL","",87703,16.2,1420788.6]
["3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY ADDITIONAL GUARDRAILPOSTS","",5,22.5,112.5]
["","","TEMPORARY GUARDRAIL END","UNITS, TYPE AT-1",1,325,325]
["","","TEMPORARY GUARDRAIL END UNITS,TYPE AT-1","",1,400,400]
["","","TEMPORARY GUARDRAIL END UNITS,TYPE CAT-1","",2,300,600]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",750,4.0999999999999996,3075]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",46,18,828]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",15,32,480]
["3533000000-E","CHN LK FENCE **\" FABRIC","(60\")","",16,47.29,756.64]
["3539000000-E","MET LINE PST **\" CL FEN","(60\")","",2,236.42,472.84]
["3545000000-E","MET TERM PST **\" CL FEN","(60\")","",2,472.82,945.64]
["3628000000-E","RIP RAP, CLASS I","","",383,75.652741514360301,28975]
["3635000000-E","RIP RAP, CLASS II","","",680,45.654411764705898,31045]
["3649000000-E","RIP RAP, CLASS B","","",463,61.169330453563703,28321.4]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",6004,2.99045636242505,17954.7]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(D)","",7.5,17.5,131.25]
["","","(E)","",250.25,17.484115884115901,4375.3999999999996]
["","","(F)","",28.19,19.1411848173111,539.59]
["4048000000-E","REINF CONC FOUNDTN","","",11,806.45,8870.9500000000007]
["4054000000-E","PLN CONC FOUNDTN","","",1,537.63,537.63]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",4896,4.84,23696.639999999999]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",3653,3.76,13735.28]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",1498,8.7088451268357794,13045.85]
["4096000000-N","SIGN ERECTION, TYPE D","","",8,93.987499999999997,751.9]
["4102000000-N","SIGN ERECTION, TYPE E","","",84,81.477738095238095,6844.13]
["4108000000-N","SIGN ERECTION, TYPE F","","",8,36.020000000000003,288.16000000000003]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",6,806.45,4838.7]
["","","(B)","",4,806.45,3225.8]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",3,488.44,1465.32]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",6,215.05,1290.3]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",83,33.782168674698802,2803.92]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",8,25.14875,201.19]
["4237000000-N","STOCKPILE SIGN, D, E, F","","",8,41.37,330.96]
["4238000000-N","DISPOSE SIGN, D, E, F","","",1,53.76,53.76]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",4037,12.892878375031,52048.55]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",2063,13.309646146388801,27457.8]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",334,10.0213173652695,3347.12]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",25333,11.6881893182805,296096.90000000002]
["4415000000-N","FLASHING ARROW BOARD","","",30,2219.0796666666702,66572.39]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",34,7656.8873529411803,260334.17]
["4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",215,123.255813953488,26500]
["4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",18,10043.608888888901,180784.96]
["4424000000-N","WZ PRESENCE LIGHTING","","",75,7700,577500]
["4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",5,29200,146000]
["4430000000-N","DRUMS","","",1668,50.673411270983202,84523.25]
["4432000000-N","HIGH VISIBILITY DRUMS","","",250,62.37,15592.5]
["4434000000-N","SEQ FLASH WARN LIGHTS","","",62,246.29435483871001,15270.25]
["4435000000-N","CONES","","",253,25.865612648221301,6544]
["4445000000-E","BARRICADES (TYPE III)","","",556,33.001870503597097,18349.04]
["4455000000-N","FLAGGER","","",2040,83.767156862745097,170885]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",4,347625,1390500]
["4465000000-N","TEMP CRASH CUSHIONS","","",18,4003.6072222222201,72064.929999999993]
["4470000000-N","REM & RES CRASH CUSHION","","",5,2835.5160000000001,14177.58]
["4480000000-N","TMA","","",19,10124.9278947368,192373.63]
["4485000000-E","PORT CONC BARRIER","","",3395,29.666686303387301,100718.39999999999]
["4490000000-E","PORT CONC BARRIER(ANCHRD)","","",120,60,7200]
["4500000000-E","REM & RES PORT CONC BARRIER","","",5725,6.3223493449781696,36195.449999999997]
["4507000000-E","WATER FILLED BARRIER","","",1207,74.821872410936194,90310]
["4508000000-E","REM & RES H2O FILL BARR","","",1200,4.9733333333333301,5968]
["4510000000-N","LAW ENFORCEMENT","","",1996,53.4068136272545,106600]
["4516000000-N","SKINNY DRUM","","",699,45.431330472102999,31756.5]
["4595000000-E","GENERIC TRAFFIC CONTROL ITEM (SF)","HIGH VISIBILITY RIGID PORTABLE","WORK ZONE SIGNS",482,10.16,4897.12]
["","","HIGH VISIBILITY STATIONARY","WORK ZONE SIGNS",1143,15.91,18185.13]
["4650000000-N","TEMP RAISED PVMT MRKS","","",628,10.181210191082799,6393.8]
["4687000000-E","THERMO PVT MKG LINES 4\"240","","",300,2.4500000000000002,735]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",3305,1.87456883509834,6195.45]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",1770,1.96107344632768,3471.1]
["4705000000-E","THERMO LINES 16\" 120MILS","","",426,5.8075117370892002,2474]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",4164,9.7801392891450494,40724.5]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",225,227.52657777777799,51193.48]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",581,158.03352839931199,91817.48]
["4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(IV)","",3730,2.25,8392.5]
["4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",20,25,500]
["","","(IV)","",91,29.945054945054899,2725]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",6550021,0.11958541354295001,783286.97]
["4815000000-E","PAINT PVMT MARKINGS 6\"","","",1358020,0.25477091648134997,345984]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",6314,0.37847640164712998,2389.6999999999998]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",60000,0.75,45000]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",41,11.5,471.5]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",1130,4.5724778761061904,5166.8999999999996]
["4840000000-N","PAINT PVT MKG CHARACTER","","",10,87.28,872.8]
["4845000000-N","PAINT PVT MKG SYMBOL","","",488,58.923155737704903,28754.5]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",1326992.8999999999,0.84221123564414002,1117608.33]
["4847030000-E","POLYUREA LINES (6\", 20 MILS)","","",865164,1.1341141448326599,981194.73]
["4847050000-E","POLYUREA LINES (8\", 20 MILS)","","",1210,11.645619834710701,14091.2]
["4847070000-E","POLYUREA LINES (12\", 20 MILS)","","",37688,2.9890999787730799,112653.2]
["4847400000-E","WZ PERF PVMT MKG LINES 4\"","","",4614,0.65,2999.1]
["4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",89032,0.85,75677.2]
["4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",5660,2.5499999999999998,14433]
["4848000000-E","WZ TRAF PATTERN MASKING","","",40080,0.85,34068]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",265248,0.46506032090722998,123356.32]
["4855000000-E","LINE REMOVAL 6\" WIDE","","",2716,0.90144329896907005,2448.3200000000002]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",48,8,384]
["4895000000-N","GENERIC PVMT MARKING ITEM (EA)","IN LANE ROUTE SHIELDS","",2,5000,10000]
["4900000000-N","PERM RAISED PVMT MARKERS","","",236,50.580508474576298,11937]
["4905000000-N","SNOWPLB PVMT MRKER","","",13289,26.921033185341301,357753.61]
["5255000000-N","PORTABLE LIGHTING","","",6,442196.71500000003,2653180.29]
["5319000000-E","CL B CONC FOR ENCAS LINE","","",3,414.27,1242.81]
["5325800000-E","8\" WATER LINE","","",197,51.03,10052.91]
["5326200000-E","12\" WATER LINE","","",1430,64.069999999999993,91620.1]
["5326600000-E","16\" WATER LINE","","",125,89.28,11160]
["5329000000-E","DI H2O PIPE FITTINGS","","",6700,4.33,29011]
["5546000000-E","8\" VALVE","","",2,1420.96,2841.92]
["5558000000-E","12\" VALVE","","",4,2654.25,10617]
["5558600000-E","16\" VALVE","","",1,7112.93,7112.93]
["5648000000-N","RELOCATE WATER METER","","",19,681.83,12954.77]
["5649000000-N","RECONNECT WATER METER","","",3,622.44000000000005,1867.32]
["5672000000-N","RELOCATE FIRE HYDRANT","","",3,2412.25,7236.75]
["5673000000-E","FIRE HYDRANT LEG","","",55,51.91,2855.05]
["5686000000-E","**\" H2O SERVICE LINE","(2\")","",120,33.08,3969.6]
["5686500000-E","WATER SERVICE LINE","","",760,24.19,18384.400000000001]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",72,84.97,6117.84]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",1066,104.01,110874.66]
["5775000000-E","4' DIA UTILITY MANHOLE","","",7,1761.93,12333.51]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",22.5,268.150222222222,6033.38]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",1460,15.02,21929.200000000001]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",70,20.23,1416.1]
["5816000000-N","ABANDON UTILITY MANHOLE","","",2,2051.73,4103.46]
["5828000000-N","REMOVE UTILITY MANHOLE","","",3,1362.16,4086.48]
["5888000000-E","GENERIC UTILITY ITEM (LF)","POLYETHYLENE ENCASEMENT","",100,17.420000000000002,1742]
["6000000000-E","TEMP SILT FENCE","","",18165,2.8682466281310202,52101.7]
["6006000000-E","EROS CONTRL STONE CL A","","",1345,40.155724907063203,54009.45]
["6009000000-E","EROS CONTRL STONE CL B","","",3855,45.196523994811898,174232.6]
["6012000000-E","SEDIMENT CONTROL STONE","","",2835,38.114638447971799,108055]
["6015000000-E","TEMP MULCHING","","",43.3,1142.1219399538099,49453.88]
["6018000000-E","SEED FOR TEMP SEEDING","","",2900,4.2103448275862103,12210]
["6021000000-E","FERT FOR TEMP SEEDING","","",17.5,1192.3245714285699,20865.68]
["6024000000-E","TEMP SLOPE DRAINS","","",1400,16.205714285714301,22688]
["6029000000-E","SAFETY FENCE","","",2000,2.8570000000000002,5714]
["6030000000-E","SILT EXCAVATION","","",3450,13.4399420289855,46367.8]
["6036000000-E","MATTING FOR EROS CONTROL","","",34575,1.8175054229934899,62840.25]
["6037000000-E","COIR FIBER MAT","","",760,5.7144736842105299,4343]
["6038000000-E","PERM SOIL REINF MAT","","",1715,4.0466472303207004,6940]
["6042000000-E","1/4\" HARDWARE CLOTH","","",5355,4.1507936507936503,22227.5]
["6045000000-E","**\" TEMP PIPE","(30\")","",245,45,11025]
["6070000000-N","SPECIAL STILLING BASINS","","",12,575,6900]
["6071010000-E","WATTLE","","",5850,7.8954871794871799,46188.6]
["6071012000-E","COIR FIBER WATTLE","","",1800,8.06666666666667,14520]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",190,10,1900]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",1610,8.8004968944099407,14168.8]
["6071030000-E","COIR FIBER BAFFLE","","",455,6.8125274725274698,3099.7]
["6071050000-E","**\" SKIMMER","(1-1/2\")","",6,1023.33333333333,6140]
["6084000000-E","SEEDING AND MULCHING","","",45.05,1942.4079911209799,87505.48]
["6087000000-E","MOWING","","",23.9,162.98577405857699,3895.36]
["6090000000-E","SEED FOR REPAIR SEEDING","","",600,6.63,3978]
["6093000000-E","FERT FOR REPAIR SEEDING","","",2.25,1601.14222222222,3602.57]
["6096000000-E","SEED FOR SUPP SEEDING","","",1125,4.6068888888888901,5182.75]
["6108000000-E","FERTILIZER TOPDRESSING","","",30,1267.626,38028.78]
["6111000000-E","IMPERVIOUS DIKE","","",300,70.8333333333333,21250]
["6114500000-N","SPECIALIZED HAND MOWING","","",60,48.948333333333302,2936.9]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",124,186.989919354839,23186.75]
["6117500000-N","CONC WASHOUT STR","","",16,2335.62,37369.919999999998]
["6123000000-E","REFORESTATION","","",0.4,4625,1850]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",26,254.14,6607.64]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",13,254.14,3303.82]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",4,1063.8499999999999,4255.3999999999996]
["7060000000-E","SIGNAL CABLE","","",2950,5.91,17434.5]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",6,1182.06,7092.36]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",1,1418.48,1418.48]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",2,1891.3,3782.6]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",960,12.41,11913.6]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",230,20.09,4620.7]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",12,472.82,5673.84]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",23679,9.8310845052578202,232790.25]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",4700,2.95,13865]
["","","(3/8\")","",200,6,1200]
["7575200000-N","GPS UNIT","","",1,1182.06,1182.06]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",1,14184.75,14184.75]
["7590000000-N","DBL MAST ARM WITH METAL POLE","","",1,21277.13,21277.13]
["7613000000-N","SOIL TEST","","",2,1182.06,2364.12]
["7614100000-E","DRILLED PIER FOUND","","",16,1063.8499999999999,17021.599999999999]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",2,118.21,236.42]
["7636000000-N","SIGN FOR SIGNALS","","",7,531.92999999999995,3723.51]
["7642200000-N","TYPE II PED W/ FOUND","","",4,2364.12,9456.48]
["7684000000-N","SIGNAL CABINET FOUND","","",1,1182.06,1182.06]
["7696000000-N","CONTLRS WITH CBNT (**************)","(2070, BASE MOUNTED)","",1,15366.81,15366.81]
["7708000000-N","DETECTOR CARD (***********)","(2070)","",5,236.42,1182.0999999999999]
["7901000000-N","CABINET BASE EXTENDER","","",1,591.03,591.03]
["7960000000-N","METAL POLE FOUND REMVL","","",2,2364.12,4728.24]
["7972000000-N","METAL POLE REMOVAL","","",2,2364.12,4728.24]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","MULTIZONE MICROWAVE VEHICLE","DETECTION SYSTEM-MULTIPLE ZONES",1,29551.56,29551.56]
["","","POWDER COAT FOR DUAL MAST ARM POLE","",1,4137.22,4137.22]
["","","POWDER COAT FOR SIGNAL PEDESTAL","",2,177.31,354.62]
["","","POWDER COAT FOR SINGLE MAST ARM POLE","",1,2955.15,2955.15]
["8007000000-N","CM&R TEMP STR ***********","(12+71.50 -DET-)","",1,120000,120000]
["","","(14+40.00 -DET-)","",1,150000,150000]
["","","(28+45.42-EBL-)","",1,550000,550000]
["8017000000-N","CM&R TEMP ACCESS ***********","(15+54.50 -L-)","",1,10000,10000]
["8021000000-N","REMV EXIST STR **********","(10+53.50-L-)","",1,6000,6000]
["","","(15+54.50 -L-)","",1,50000,50000]
["8035000000-N","REMV EXIST STR **********","(13+07.00 -L-)","",1,25000,25000]
["","","(14+21.00 -L-)","",1,38000,38000]
["","","(28+26.49-WBL-)","",1,130019,130019]
["","","(28+45.42-EBL-)","",1,130019,130019]
["8065000000-N","ASBESTOS ASSESSMENT","","",5,1249,6245]
["8096000000-E","PILE EXCAVATION IN SOIL","","",155,377.12258064516101,58454]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",91,212.25274725274701,19315]
["8121000000-N","UNCL STR EXCAV STA *****","(14+21.00 -L-)","",1,7630,7630]
["","","(15+54.50 -L-)","",1,7500,7500]
["","","(28+26.49-WBL-)","",1,30000,30000]
["","","(28+45.42-EBL-)","",1,30000,30000]
["8126000000-N","CULV EXCAV @ ************","(13+07.00 -L-)","",1,75990,75990]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",179,37.75,6757.25]
["8147000000-E","REINF CONC DECK SLAB","","",8898,44,391512]
["8156000000-E","CONC WEARING SURFACE","","",2589,18,46602]
["8161000000-E","GROOVING BRIDGE FLOORS","","",291971,0.55380739868001005,161695.70000000001]
["8175000000-E","CLASS AA CONC (BRIDGE)","","",0.9,645,580.5]
["8182000000-E","CLASS A CONC (BRIDGE)","","",320.5,1217.08892355694,390077]
["8196000000-E","CLASS A CONC (CULV)","","",250.6,835,209251]
["8210000000-N","BRG APPR SLAB ***********","(10+53.50-L-)","",1,27000,27000]
["","","(14+21.00 -L-)","",1,34750,34750]
["","","(15+54.50 -L-)","",1,45000,45000]
["","","(28+26.49-WBL-)","",1,51000,51000]
["","","(28+45.42-EBL-)","",1,51000,51000]
["8217000000-E","REINF STEEL (BRIDGE)","","",40662,1.62171068811175,65942]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",91,2.75,250.25]
["8245000000-E","REINF STEEL (CULVERT)","","",30958,1,30958]
["8280000000-E","STRUCTURAL STEEL","","",270343,3.6065294829161498,975000]
["8296000000-N","POLLUTION CONTROL","","",3,89000,267000]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",46,823.47826086956502,37880]
["","","(HP12 X 53)","",12,500,6000]
["","","(HP12X53)","",10,1,10]
["8364000000-E","HP12X53 PILES","","",2195,56.5831435079727,124200]
["8391000000-N","STEEL PILE POINTS","","",19,227.36842105263199,4320]
["8484000000-E","42\" OREGON RAIL","","",100,500,50000]
["8503000000-E","CONC BARRIER RAIL","","",393.2,125,49150]
["8505000000-E","VERT CONC BARRIER RAIL","","",260.5,142.5,37121.25]
["8531000000-E","4\" SLOPE PROTECTION","","",364,85,30940]
["8559000000-E","SURFACE PREP, CLASS II","","",568.4,324.76249120337798,184595]
["8566000000-E","SURFACE PREP, CLASS III","","",21.1,683.41232227488103,14420]
["8608000000-E","RIP RAP II (2'-0\")","","",984,54.194613821138198,53327.5]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",1094,4.0877513711151696,4472]
["8629000000-E","EROS CONTRL STONE CL B","","",1,550,550]
["8657000000-N","ELASTOMERIC BEARINGS","","",5,6270,31350]
["8660000000-E","CONC REPAIRS","","",31.1,900,27990]
["8664000000-E","SHOTCRETE REPAIRS","","",3979.3,556.93488804563594,2216211]
["8678000000-E","EPOXY RESIN INJECTION","","",6626.9,84.911723430261503,562701.5]
["8692000000-N","FOAM JOINT SEALS","","",4,34875,139500]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",700,169,118300]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",1560,181.666666666667,283400]
["8801000000-E","MSE RETAIN WALL NO **","(-WL1-)","",2855,120,342600]
["","","(-WL2-)","",2600,120,312000]
["8802031000-E","PRECAST GRAVITY RETAINING WALLS","","",680,82.6,56168]
["8847000000-E","GENERIC RET WALL ITEM (SF)","TEMPORARY SHORING FOR","RETAINING WALL NO 1",410,70.92,29077.200000000001]
["8860000000-N","GENERIC STR ITEM (LS)","CLEANING & PAINTING EXISTING WEATHERING","STEEL FOR BRIDGE 560093",1,100000,100000]
["","","","STEEL FOR BRIDGE 560113",1,100000,100000]
["","","","STEEL FOR BRIDGE 600247",1,100000,100000]
["","","CLEANING AND REPAINTING OF","BRIDGE 358",1,100000,100000]
["","","","BRIDGE 366",1,100000,100000]
["","","","BRIDGE 369",1,100000,100000]
["","","","BRIDGE 374",1,100000,100000]
["","","","BRIDGE 377",1,220000,220000]
["","","","BRIDGE 378",1,220000,220000]
["","","FIELD MEASURING","",1,30000,30000]
["","","MOLDED RUBBER SEGMENTAL","EXPANSION JOINT",1,450000,450000]
["","","PAINTING CONTAINMENT FOR","BRIDGE 358",1,30000,30000]
["","","","BRIDGE 366",1,30000,30000]
["","","","BRIDGE 369",1,30000,30000]
["","","","BRIDGE 374",1,30000,30000]
["","","","BRIDGE 377",1,75000,75000]
["","","","BRIDGE 378",1,75000,75000]
["","","","BRIDGE 560093",1,15000,15000]
["","","","BRIDGE 560113",1,15000,15000]
["","","","BRIDGE 600247",1,15000,15000]
["","","PAINTING CONTAINMENT FOR ZONE","PAINTING, BRIDGE 334",1,10000,10000]
["","","","PAINTING, BRIDGE 339",1,10000,10000]
["","","","PAINTING, BRIDGE 344",1,20000,20000]
["","","","PAINTING, BRIDGE 347",1,20000,20000]
["","","PARTIAL REMOVAL OF EXISTING","STRUCTURE 369",1,20000,20000]
["","","PREFORMED SILICONE EXPANSION","JOINT SEALS",1,12000,12000]
["","","REPAIR OF EXISTING DECK DRAINS","",1,10500,10500]
["","","SPOT PAINTING OF STEEL STRUCTURE","REPAIR AREAS",1,75000,75000]
["","","UNDER STRUCTURE WORK PLATFORM","",1,575000,575000]
["","","VOLUMETRIC MIXER","",3,38083.333333333299,114250]
["","","ZONE PAINTING OF EXISTING","STRUCTURE, BRIDGE 334",1,25000,25000]
["","","","STRUCTURE, BRIDGE 339",1,30000,30000]
["","","","STRUCTURE, BRIDGE 344",1,60000,60000]
["","","","STRUCTURE, BRIDGE 347",1,60000,60000]
["8867000000-E","GENERIC STR ITEM (LF)","EXPANSION JOINT SEAL REPAIR","",38,95,3610]
["","","REMOVE AND RESET BRIDGE DECK","MOUNTED GUARDRAIL FOR BRIDGE 358",242,140,33880]
["","","","MOUNTED GUARDRAIL FOR BRIDGE 366",242,140,33880]
["","","","MOUNTED GUARDRAIL FOR BRIDGE 369",270,130,35100]
["","","","MOUNTED GUARDRAIL FOR BRIDGE 374",270,130,35100]
["","","SILICONE JOINT SEALANT","",650,72,46800]
["8881000000-E","GENERIC STR ITEM (CY)","LATEX MODIFIED CONCRETE-EARLY","STRENGTH",438.3,1450,635535]
["","","LATEX MODIFIED CONCRETE-VERY","EARLY STRENGTH",614.70000000000005,1269.31836668293,780250]
["","","PPC MATERIALS","",725.1,3500,2537850]
["8882000000-E","GENERIC STR ITEM (CF)","CONCRETE FOR DECK REPAIR","",208.5,62.949640287769803,13125]
["","","ELASTOMERIC CONCRETE","",575,472.93913043478301,271940]
["","","REPAIRS TO REINFORCED CONCRETE","DECK GIRDERS",29.5,1050,30975]
["8889000000-E","GENERIC STR ITEM (LB)","BEAM PLATED REPAIR","",1155.9000000000001,30,34677]
["","","BEAM PLATING REPAIR","",169,150,25350]
["","","BEAM REPAIR","",1283,130,166790]
["","","BEAM SECTION REPLACEMENT AND","STIFFENER/CONNECTOR PLATE REPAIR",37850,16,605600]
["","","STEEL CONNECTION HARDWARE","",300,5,1500]
["","","STEEL DIAPHRAGM REPLACEMENT","",2295,24,55080]
["8892000000-E","GENERIC STR ITEM (SF)","ANCHORED VENEER","",17075,118,2014850]
["","","BRIDGE JOINT DEMOLITION","",2151,61.066945606694603,131355]
["","","CONCRETE WORK FOR JOINT","REPLACEMENT",240,170,40800]
["","","EPOXY COATING","",9042.4,11.798714942935501,106688.7]
["","","EPOXY COATING AND DEBRIS","REMOVAL",1159,51,59109]
["8893000000-E","GENERIC STR ITEM (SY)","CONCRETE DECK REPAIR FOR PPC","OVERLAY",62.4,550,34320]
["","","HYDRO-DEMOLITION OF BRIDGE","DECK",13624,54.908543746329997,748074]
["","","HYDRO-DEMOLITION OF BRIDGE DECK","",4548,110,500280]
["","","PLACING & FINISHING LATEX MODIFIED","CONC. OVERLAY-VERY EARLY STRENGTH",4548,30,136440]
["","","PLACING & FINISHING OF LATEX","MOD CONC OVERLAY-VERY EARLY STRENGTH",6226,30,186780]
["","","PLACING AND FINISHING LATEX MODIFIED","CONC. OVERLAY-EARLY STRENGTH",7398,40,295920]
["","","PLACING AND FINISHING PPC OVERLAY","",14988,40,599520]
["","","SCARIFYING BRIDGE DECK","",33160,28.4500603136309,943404]
["","","SHOTBLASTING BRIDGE DECK","",14988,7.5,112410]
["8897000000-N","GENERIC STR ITEM (EA)","BRIDGE JACKING","",160,1000,160000]
["","","ELASTOMERIC BEARING, MODIFIED","TYPE I-A",64,160,10240]
["","","","TYPE I-B",48,170,8160]
["","","","TYPE I-C",16,180,2880]
["","","GUARDRAIL ANCHOR UNIT REPAIR","",4,600,2400]
["","","OVERHANG DIAPHRAGM REMOVAL","",20,850,17000]
["","","STEEL KEEPER ANGLE ASSEMBLY","",80,1000,80000]
["","","STEEL KEEPER ASSEMBLY","",3,4000,12000]
["","","STEEL PLATE BEARING","",1,500,500]
["","","STUB COLUMN ASSEMBLY","",34,2800,95200]
["","","TYPE I BRIDGE JACKING","BRIDGE 560113",28,3500,98000]
["","","","BRIDGE 600247",2,7200,14400]
["","","","",6,6000,36000]
["","Not assigned","","",null,null,0]
["Overall Result","","","",19208853.646000002,6.7883431105818897,130396289.31]

{"sheet":"ITEMS - DIV 14","index":16,"n_rows":457,"n_cols":7,"rows_kept":457,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["2018 BID AVERAGES - DIVISION 14"]
["Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
["0000100000-N","MOBILIZATION","","",10,281080.7,2810807]
["0000400000-N","CONST SURVEYING","","",7,56721.428571428602,397050]
["0001010000-N","SELECT TREE REMOVAL","","",1,5000,5000]
["0015000000-N","SEALING ABANDONED WELLS","","",1,2303.66,2303.66]
["0030000000-N","TYPE II MOD APPR **********","(13+52 -L-)","",1,7500,7500]
["","","(13+86 -L-)","",1,18500,18500]
["","","(14+27 -L-)","",1,22000,22000]
["","","(14+94.00 -L-)","",1,15000,15000]
["0036000000-E","UNDERCUT EXCAVATION","","",200,15,3000]
["0043000000-N","GRADING","","",7,499793.28571428597,3498553]
["0050000000-E","SUPP CLEARING & GRUBBING","","",8,3133.125,25065]
["0057000000-E","UNDERCUT EXCAVATION","","",4200,19.625,82425]
["0134000000-E","DRAINAGE DITCH EXCAVATION","","",4575,20.256393442623001,92673]
["0141000000-E","BERM DITCH CONST","","",430,5,2150]
["0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",426.6,15,6399]
["0177000000-E","BREAKING OF EXT ASPH PVMT","","",426.6,15,6399]
["0194000000-E","SELECT GRANULAR MATL, CLASS III","","",200,36.25,7250]
["0195000000-E","SELECT GRANULAR MAT'L","","",6000,46.9166666666667,281500]
["0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",8100,1.9814814814814801,16050]
["0199000000-E","TEMP SHORING","","",5476,53.224981738495302,291460]
["0223000000-E","ROCK PLATING","","",200,72,14400]
["0225000000-E","REINF SOIL SLOPES","","",130,190,24700]
["0318000000-E","FND CONDIT MATL MINOR STRS","","",3406,39.415149735760401,134248]
["0320000000-E","FND CONDIT GEOTEXTILE","","",11769,3.2429263318888601,38166]
["0335200000-E","15\" DRAINAGE PIPE","","",708,63.324293785310701,44833.599999999999]
["0335300000-E","18\" DRAINAGE PIPE","","",80,69.599999999999994,5568]
["0335400000-E","24\" DRAINAGE PIPE","","",28,75,2100]
["0335500000-E","30\" DRAINAGE PIPE","","",112,92.3,10337.6]
["0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",4,397.5,1590]
["0343000000-E","15\" SIDE DRAIN PIPE","","",24,50,1200]
["0344000000-E","18\" SIDE DRAIN PIPE","","",78,55.076923076923102,4296]
["0345000000-E","24\" SIDE DRAIN PIPE","","",28,70,1960]
["0366000000-E","15\" RC PIPE CULV III","","",3524,67.157207718501695,236662]
["0372000000-E","18\" RC PIPE CULV III","","",1352,71.538461538461505,96720]
["0378000000-E","24\" RC PIPE CULV III","","",92,85.260869565217405,7844]
["0384000000-E","30\" RC PIPE CULV III","","",112,105,11760]
["0390000000-E","36\" RC PIPE CULV III","","",88,109,9592]
["0396000000-E","42\" RC PIPE CULV III","","",136,120,16320]
["0402000000-E","48\" RC PIPE CULV III","","",608,182,110656]
["0448000000-E","***\" RCP CULV CLASS IV","(48\")","",92,340,31280]
["0448200000-E","15\" RCP CULV CLASS IV","","",6556,84.321293471629005,552810.4]
["0448300000-E","18\" RCP CULV CLASS IV","","",1648,94.019417475728204,154944]
["0448400000-E","24\" RCP CULV CLASS IV","","",1692,120.66028368794299,204157.2]
["0448500000-E","30\" RCP CULV CLASS IV","","",1852,142.63174946004301,264154]
["0448600000-E","36\" RCP CULV CLASS IV","","",904,172.843362831858,156250.4]
["0448700000-E","42\" RCP CULV CLASS IV","","",428,184.76635514018699,79080]
["0576000000-E","**\" CS PIPE CULV *****\"","(48\", 0.109\")","",32,275,8800]
["0582000000-E","15\" CS PIPE CULV 0.064\"","","",368,68.369565217391298,25160]
["0588000000-E","18\" CS PIPE CULV 0.064\"","","",218,76.023853211009197,16573.2]
["0594000000-E","24\" CS PIPE CULV 0.064\"","","",12,168,2016]
["0600000000-E","30\" CS PIPE CULV 0.079\"","","",28,100,2800]
["0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",2,250,500]
["","","(18\", 0.064\")","",3,360,1080]
["0986000000-E","GENERIC PIPE ITEM (LF)","15\" CURED IN PLACE PIPE","",106,132,13992]
["","","18\" CURED IN PLACE PIPE","",255,177,45135]
["","","24\" CURED IN PLACE PIPE","",155,268,41540]
["","","30\" CURED IN PLACE PIPE","",185,285,52725]
["0995000000-E","PIPE REMOVAL","","",5466,13.4705085986096,73629.8]
["1077000000-E","57 STONE","","",100,26,2600]
["1099500000-E","SHALLOW UNDERCUT","","",1050,13.604761904761901,14285]
["1099700000-E","CLASS IV SUBGRD STABILIZATION","","",2010,31.233830845771099,62780]
["1121000000-E","AGGREGATE BASE COURSE","","",13376,31.825956937798999,425704]
["1220000000-E","INCIDENTAL STONE BASE","","",3700,42.148648648648702,155950]
["1245000000-E","SHOULDER RECONST","","",81.17,7060.4798570900602,573099.15]
["1275000000-E","PRIME COAT","","",175,30,5250]
["1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",319769,2.84778027263431,910631.85]
["","","(2-1/2\")","",22090,3.7,81733]
["","","(4-1/2\")","",226982,5,1134910]
["1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",11223,8.7028281208233107,97671.84]
["1330000000-E","INCIDENTAL MILLING","","",11687.6,13.210068790855299,154394]
["1491000000-E","ASP CONC BASE CRS B25.0C","","",11820,108.72250423011801,1285100]
["1503000000-E","ASP CONC INTR CRS I19.0C","","",58757,74.280204911755206,4364482]
["1519000000-E","ASP CONC SURF CRS S9.5B","","",10181,77.466358903840501,788685]
["1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",8160,72.529411764705898,591840]
["1523000000-E","ASP CONC SURF CRS S9.5C","","",111846,74.038749709421893,8280938]
["1575000000-E","ASP FOR PLANT MIX","","",11796,690.22634791454698,8141910]
["1693000000-E","ASPH PLT MIX PVMT REPAIR","","",1820,175.57802197802201,319552]
["1704000000-E","PATCHING EXIST PVMT","","",2832,175.328389830508,496530]
["1840000000-E","MILLED RUMBLE STRIPS","","",267484,0.13,34772.92]
["1869000000-E","******\"PCC PVMT MISC","(12\")","",1220,125,152500]
["1880000000-E","GENERIC PAVING ITEM (TON)","ASPHALT FOR PAVEMENT INTERLAYER","",893,91,81263]
["1891000000-E","GENERIC PAVING ITEM (SY)","PAVEMENT INTERLAYER (HIGH STRENGTH)","",91225,5.95,542788.75]
["","","PAVEMENT INTERLAYER (REGULAR)","",91225,4,364900]
["2000000000-N","RIGHT-OF-WAY MARKERS","","",91,232.89450549450501,21193.4]
["2022000000-E","SUBDRAIN EXCAVATION","","",246.6,18.9752635847526,4679.3]
["2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",1000,4.5350000000000001,4535]
["2036000000-E","SUBDRAIN COARSE AGGREGATE","","",169.4,59.190082644628099,10026.799999999999]
["2044000000-E","6\" PERF SUBDRN PIPE","","",1000,12.194000000000001,12194]
["2070000000-N","SUBDRN PIPE OUTLET","","",6,377.83333333333297,2267]
["2077000000-E","6\" OUTLET PIPE","","",36,23.1666666666667,834]
["2209000000-E","ENDWALLS","","",9,1500,13500]
["2253000000-E","PIPE COLLARS","","",6.2380000000000004,1785.82879127926,11140]
["2264000000-E","PIPE PLUGS","","",0.13,13152,1709.76]
["2275000000-E","FLOWABLE FILL","","",90,300.444444444444,27040]
["2286000000-N","MASNRY DRAINAGE STRUCT","","",287,2071.5484320557498,594534.40000000002]
["2308000000-E","MASNRY DRAINAGE STRUCT","","",177.8,289.13644544431901,51408.46]
["2364000000-N","FRAME W/2GRTS 840.16 STD","","",47,642.31914893617,30189]
["2365000000-N","FRAME W/2GRTS 840.22 STD","","",1,1000,1000]
["2366000000-N","FRAME W/2GRTS 840.24 STD","","",17,587.67058823529396,9990.4]
["2367000000-N","FRAME W/2GRTS 840.29 STD","","",7,628.57142857142901,4400]
["2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",15,726.78666666666697,10901.8]
["","","(F)","",74,612.92432432432395,45356.4]
["","","(G)","",84,635.41428571428605,53374.8]
["2396000000-N","FRAME W/COVER STD 840.54","","",31,499.37419354838698,15480.6]
["2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",16,1500,24000]
["2418000000-E","FRM W/GRATES, DRIVEWY DI","","",65,290.89999999999998,18908.5]
["2451000000-N","CONC TRANS SECT FOR DROP INLET","","",34,1144.11764705882,38900]
["2535000000-E","**\"X**\" CONC CURB","(8\" X 12\")","",190,26,4940]
["","","(8\" X 18\")","",580,28,16240]
["2538000000-E","**'-**\" CONC CURB & GUTTER","(2'-9\")","",460,34.200000000000003,15732]
["2542000000-E","1'-6\" CONC CURB & GUTTER","","",4150,24.625060240963901,102194]
["2549000000-E","2'-6\" CONC CURB & GUTTER","","",27080,28.618537666174301,774990]
["2556000000-E","SHOULDER BERM GUTTER","","",113,69.203539823008896,7820]
["2570000000-N","MOD CONC FLUME","","",2,1562.5,3125]
["2580000000-E","CONC VALLEY GUTTER","","",300,26.3,7890]
["2591000000-E","4\" CONC SIDEWALK","","",7460,48.818498659517402,364186]
["2605000000-N","CONC CURB RAMPS","","",98,2054.8979591836701,201380]
["2612000000-E","6\" CONC DRIVEWAY","","",1244,73.258038585208993,91133]
["2619000000-E","4\" CONC PAVED DITCH","","",240,82.6041666666667,19825]
["2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",120,78.8,9456]
["2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",2560,74.0625,189600]
["2657000000-E","**\" MONO CONC MEDIAN (*****)","(5-1/2\", KEYED IN)","",20,85,1700]
["2738000000-E","GENERIC PAVING ITEM (SY)","REINFORCED CONCRETE DRIVEWAY","",259,90,23310]
["2761000000-E","GENERIC PAVING ITEM 848 (SY)","8\" CONCRETE DRIVEWAY","",90,120,10800]
["2800000000-N","ADJ CATCH BASINS","","",10,1000,10000]
["2815000000-N","ADJ DROP INLETS","","",1,2500,2500]
["2830000000-N","ADJ MANHOLES","","",23,1589.8,36565.4]
["2845000000-N","ADJ METER OR VALVE BOXES","","",17,1278.88823529412,21741.1]
["2860000000-N","CONVERT CB TO JB","","",1,2200,2200]
["2905000000-N","CONVERT DI TO JB","","",5,2080,10400]
["2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION BOX",2,1700,3400]
["3030000000-E","STL BEAM GUARDRAIL","","",2712.5,18.7299539170507,50805]
["3045000000-E","SBGR SHOP CURVED","","",337.5,21.040740740740699,7101.25]
["3150000000-N","ADDIT GUARDRAIL POSTS","","",40,33.931249999999999,1357.25]
["3195000000-N","GR END TYPE AT-1","","",6,688.1,4128.6000000000004]
["3210000000-N","GR END TYPE CAT-1","","",6,700,4200]
["3215000000-N","GR ANCHOR TYPE III","","",19,1815.78947368421,34500]
["3287000000-N","GR END TYPE TL-3","","",12,3248.9333333333302,38987.199999999997]
["3288000000-N","GR END TYPE TL-2","","",13,3436.9230769230799,44680]
["3360000000-E","REMOVE EXISTING GUARDRAIL","","",1930,1.1402849740932599,2200.75]
["3380000000-E","TEMP STL BM GUARDRAIL","","",287.5,13.6,3910]
["3389150000-N","TEMP GDRL END UNITS *****","(TL-3)","",1,3700,3700]
["3435000000-N","GENERIC GUARDRAIL ITEM (EA)","GUARDRAIL POST CAPS","",161,45.4,7309.4]
["3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",310,6,1860]
["3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",20,24,480]
["3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",20,40,800]
["3533000000-E","CHN LK FENCE **\" FABRIC","(60\")","",73,20.45,1492.85]
["3536000000-E","CHN LK FENCE 48\" FABRIC","","",382,15.9,6073.8]
["3539000000-E","MET LINE PST **\" CL FEN","(60\")","",7,85.5,598.5]
["3542000000-E","MET LINE PST 48\" CL FEN","","",32,73.75,2360]
["3545000000-E","MET TERM PST **\" CL FEN","(60\")","",4,230,920]
["3548000000-E","MET TERM PST 48\" CL FEN","","",4,170,680]
["3557000000-E","ADDITIONAL BARBED WIRE","","",50,1.9,95]
["3559000000-E","** STRAND BW FENCE W/ POSTS","(3)","",100,6,600]
["","","(4)","",280,7.5,2100]
["3563000000-E","TEMP **\" WW FENCE W/POSTS","(47\")","",310,10,3100]
["3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 12')","",1,600,600]
["3575000000-E","GENERIC FENCING ITEM (LF)","BLACK VINYL COATED CHAIN LINK","FENCE, 48\" FABRIC",510,14.8,7548]
["","","RETAINING WALL ALUMINUM PICKETFENCE","",745,71,52895]
["","","WALL MOUNTED PEDESTRIAN HANDRAIL","",182,170,30940]
["3578000000-N","GENERIC FENCING ITEM (EA)","BLACK VINYL COATED METAL","TERMINAL POST FOR 48\" CHAIN LINK FENCE",6,159.1,954.6]
["","","BLACK VINYL COATED METAL LINE","POST FOR 48\" CHAIN LINK FENCE",42,79.5,3339]
["3628000000-E","RIP RAP, CLASS I","","",1641,70.611212675198004,115873]
["3635000000-E","RIP RAP, CLASS II","","",640,53.03125,33940]
["3642000000-E","RIP RAP, CLASS A","","",17,35,595]
["3649000000-E","RIP RAP, CLASS B","","",626,66.581469648562305,41680]
["3656000000-E","GEOTEXTILE FOR DRAINGE","","",9701,3.2900474177919801,31916.75]
["4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",154,14,2156]
["4048000000-E","REINF CONC FOUNDTN","","",3,735,2205]
["4054000000-E","PLN CONC FOUNDTN","","",1,735,735]
["4057000000-E","OVERHEAD FOOTING","","",49,1155,56595]
["4060000000-E","SUPPORT, BREAKAWAY STL BM","","",3159,6.3,19901.7]
["4066000000-E","SUPPORTS, SIMPLE STL BM","","",415,6.3,2614.5]
["4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",4476,8.44994191242181,37821.94]
["4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",30,68.900000000000006,2067]
["4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(13+25 -LPD-)","",1,85000,85000]
["","","(69+00 -L-)","",1,75000,75000]
["4096000000-N","SIGN ERECTION, TYPE D","","",28,138.392857142857,3875]
["4102000000-N","SIGN ERECTION, TYPE E","","",318,113.58805031446499,36121]
["4108000000-N","SIGN ERECTION, TYPE F","","",25,152.6,3815]
["4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",4,735,2940]
["4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",1,735,735]
["","","(B)","",6,580.83333333333303,3485]
["","","(D)","",2,116,232]
["","","(E)","",3,125.333333333333,376]
["","","(F)","",2,165,330]
["4138000000-N","DISPOSE SUPPORT, STL BM","","",1,210,210]
["4152000000-N","DISPOSE SIGN SYST STL BM","","",1,230,230]
["4155000000-N","DISPOSE SIGN SYST U-CHAN","","",161,11.2708074534162,1814.6]
["4192000000-N","DISPOSE SUPPORT, U-CHAN","","",1,1.1499999999999999,1.1499999999999999]
["4360000000-N","GENERIC SIGNING ITEM (EA)","DISPOSAL OF SIGN SYSTEM ON SPAN WIRE","",1,2300,2300]
["4370000000-N","GENERIC SIGNING ITEM (LS)","DISPOSAL OF FLASHER SYSTEM","",1,2000,2000]
["4400000000-E","WORK ZONE SIGNS (STAT)","","",3673,11.561873128233,42466.76]
["4405000000-E","WORK ZONE SIGNS (PORT)","","",1200,21.271999999999998,25526.400000000001]
["4410000000-E","WORK ZONE SIGNS (BARR)","","",1027,9.6420642648490702,9902.4]
["4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",7869,13.2712161646969,104431.2]
["4415000000-N","FLASHING ARROW BOARD","","",5,2475.6799999999998,12378.4]
["4420000000-N","PORTABLE CHANGE MSG SIGN","","",12,7648.6333333333296,91783.6]
["4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",2,16500,33000]
["4430000000-N","DRUMS","","",1226,53.851876019575897,66022.399999999994]
["4435000000-N","CONES","","",187,21.310160427807499,3985]
["4445000000-E","BARRICADES (TYPE III)","","",982,29.947861507128302,29408.799999999999]
["4455000000-N","FLAGGER","","",216,160.71111111111099,34713.599999999999]
["4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",2,515000,1030000]
["4465000000-N","TEMP CRASH CUSHIONS","","",8,4946.7,39573.599999999999]
["4480000000-N","TMA","","",3,20000,60000]
["4485000000-E","PORT CONC BARRIER","","",634,31.845425867507899,20190]
["4507000000-E","WATER FILLED BARRIER","","",1152,84.0069444444444,96776]
["4510000000-N","LAW ENFORCEMENT","","",112,50.535714285714299,5660]
["4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","WARNING FLAGS","",2,500,1000]
["4650000000-N","TEMP RAISED PVMT MRKS","","",103,22.7669902912621,2345]
["4685000000-E","THERMO PVT MKG LINES 4\"90","","",15276,1.7073121235925599,26080.9]
["4686000000-E","THERMO PVT MKG LINES 4\"120","","",42080,2.11110979087452,88835.5]
["4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",975,3.4,3315]
["4690000000-E","THERMO PVT MKG LINES 6\"120 MILS","","",419,3.7,1550.3]
["4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",10549,2.2372926343729298,23601.200000000001]
["4697000000-E","THERMO PVT MKG LINE 8\"120 MILS","","",2583,3.6456445993031399,9416.7000000000007]
["4700000000-E","12\"WIDE THERMO 90 MILS","","",265,3,795]
["4705000000-E","THERMO LINES 16\" 120MILS","","",100,11.4,1140]
["4710000000-E","24\"WIDE THERMO 120 MILS","","",3837,18.610789679437101,71409.600000000006]
["4721000000-E","THERMO PVT MKG CHARACTER 120","","",54,140.014814814815,7560.8]
["4725000000-E","THERMO PVT SYMBOL 90MILS","","",425,143.66823529411801,61059]
["4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",52,370,19240]
["4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(IV)","",4684,3.4269854824935999,16052]
["4810000000-E","PAINT PVMT MARKINGS 4\"","","",1602508,0.14455992107372001,231658.43]
["4820000000-E","PAINT PVMT MARKINGS 8\"","","",8165,1.3163808940600099,10748.25]
["4825000000-E","PAINT PVMT MARKINGS 12\"","","",956,1.25,1195]
["4830000000-E","PAINT PVT MKGS LINES 16\"","","",308,2.7,831.6]
["4835000000-E","PAINT PVT MKG LINES 24\"","","",4346,8.0829958582604693,35128.699999999997]
["4840000000-N","PAINT PVT MKG CHARACTER","","",27,71.7222222222222,1936.5]
["4845000000-N","PAINT PVT MKG SYMBOL","","",279,75.018996415770602,20930.3]
["4847010000-E","POLYUREA LINES (4\", 20 MILS)","","",3042,2.75,8365.5]
["4850000000-E","LINE REMOVAL 4\" WIDE","","",46167,0.71475729417115996,32998.199999999997]
["4860000000-E","LINE REMOVAL 8\" WIDE","","",1331,1.2,1597.2]
["4870000000-E","LINE REMOVAL 24\" WIDE","","",383,4.2,1608.6]
["4875000000-N","REMOVAL OF SYMBL & CHARAC","","",47,101.16170212766001,4754.6000000000004]
["4890000000-E","GENERIC PVMT MARKING ITEM (LF)","THERMOPLASTIC PAVEMENT MARKING","LINES, 50 MILS, 4\"",291132,0.48,139743.35999999999]
["4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (50 MIL)",386877,0.46,177963.42]
["4895000000-N","GENERIC PVMT MARKING ITEM (EA)","IN LANE ROUTE SHIELD","",1,4000,4000]
["4900000000-N","PERM RAISED PVMT MARKERS","","",136,40.735294117647101,5540]
["4905000000-N","SNOWPLB PVMT MRKER","","",5802,25.797354360565301,149676.25]
["4915000000-E","7' U-CHANNEL POSTS","","",11,75,825]
["4957000000-N","OBJECT MARKERS (TYPE **)","(1)","",13,100,1300]
["5160000000-E","ELECT DUCT JA, SIZE *****","(2\" HDPE)","",1229,22,27038]
["5240000000-N","ELEC JB ************","(STANDARD SIZE)","",18,450,8100]
["5255000000-N","PORTABLE LIGHTING","","",3,98666.666666666701,296000]
["5325600000-E","6\" WATER LINE","","",412,192.14126213592201,79162.2]
["5325800000-E","8\" WATER LINE","","",2584,88.917724458204304,229763.4]
["5326000000-E","10\" WATER LINE","","",2646,113.230045351474,299606.7]
["5326200000-E","12\" WATER LINE","","",2808,149.58066239316199,420022.5]
["5326600000-E","16\" WATER LINE","","",945,147.1,139009.5]
["5329000000-E","DI H2O PIPE FITTINGS","","",39910,7.2785266850413404,290486]
["5538000000-E","4\" VALVE","","",1,1260.5,1260.5]
["5540000000-E","6\" VALVE","","",9,1473.86666666667,13264.8]
["5546000000-E","8\" VALVE","","",10,2140.7199999999998,21407.200000000001]
["5552000000-E","10\" VALVE","","",8,2518.0500000000002,20144.400000000001]
["5558000000-E","12\" VALVE","","",8,3775,30200]
["5571000000-E","**\" TAPPING SLEEVE & VALVE","(1\")","",15,710,10650]
["5588000000-E","*\" AIR RELEASE VALVE","(12\")","",2,6750,13500]
["5600000000-E","**\" BLOW OFF","(1\")","",1,3151.2,3151.2]
["5648000000-N","RELOCATE WATER METER","","",18,2625.6,47260.800000000003]
["5649000000-N","RECONNECT WATER METER","","",9,3151.2,28360.799999999999]
["5666000000-N","FIRE HYDRANT","","",11,4800.7272727272702,52808]
["5672000000-N","RELOCATE FIRE HYDRANT","","",1,2300,2300]
["5673000000-E","FIRE HYDRANT LEG","","",110,124.6,13706]
["5678600000-E","8\" LINE STOP","","",1,14705.6,14705.6]
["5686000000-E","**\" H2O SERVICE LINE","(2\")","",33,105,3465]
["","","(4\")","",31,210.1,6513.1]
["5686500000-E","WATER SERVICE LINE","","",537,32.908752327746697,17672]
["5691100000-E","4\" SANITARY GRAVITY SEWER","","",160,100.8125,16130]
["5691200000-E","6\" SANITARY GRAVITY SEWER","","",35,105,3675]
["5691300000-E","8\" SANITARY GRAVITY SEWER","","",4725,158.08482539682501,746950.8]
["5691500000-E","12\" SANITARY GRAVITY SEWER","","",2496,220,549120]
["5691600000-E","16\" SANITARY GRAVITY SEWER","","",185,290,53650]
["5768000000-N","SANITARY SEWER CLEAN-OUT","","",9,1366.75555555556,12300.8]
["5768500000-E","SEWER SERVICE LINE","","",185,60.010810810810803,11102]
["5775000000-E","4' DIA UTILITY MANHOLE","","",144,3683.7055555555598,530453.6]
["5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",60,329.36,19761.599999999999]
["5800000000-E","ABANDON 6\" UTILITY PIPE","","",4482,12.939402052655099,57994.400000000001]
["5801000000-E","ABANDON 8\" UTILITY PIPE","","",2199,13.4160982264666,29502]
["5802000000-E","ABANDON 10\" UTILITY PIPE","","",4254,21.356488011283499,90850.5]
["5804000000-E","ABANDON 12\" UTILITY PIPE","","",2510,19.408764940238999,48716]
["5810000000-E","ABANDON 16\" UTILITY PIPE","","",1070,67.763551401869194,72507]
["5815000000-N","REMOVE WATER METER","","",2,1680.6,3361.2]
["5815500000-N","REMOVE FIRE HYDRANT","","",7,2743.6571428571401,19205.599999999999]
["5816000000-N","ABANDON UTILITY MANHOLE","","",22,1963.6363636363601,43200]
["5835700000-E","16\" ENCASEMENT PIPE","","",170,153.929411764706,26168]
["5835900000-E","20\" ENCASEMENT PIPE","","",248,210.1,52104.800000000003]
["5836000000-E","24\" ENCASEMENT PIPE","","",89,190,16910]
["5872500000-E","BORE & JACK **\"","(16\")","",90,740,66600]
["","","(20\")","",85,420.2,35717]
["","","(24\")","",89,820,72980]
["5882000000-N","GENERIC UTILITY ITEM (EA)","16\" BUTTERFLY VALVE","",2,9453.6,18907.2]
["","","16\" INSERT VALVE","",1,36764,36764]
["5912000000-N","GENERIC UTILITY ITEM (LS)","TEMPORARY SANITARY SEWER BY-","PASS PUMPING",1,34000,34000]
["6000000000-E","TEMP SILT FENCE","","",30410,2.67728543242354,81416.25]
["6006000000-E","EROS CONTRL STONE CL A","","",2275,54.471208791208802,123922]
["6009000000-E","EROS CONTRL STONE CL B","","",3565,51.103927068723699,182185.5]
["6012000000-E","SEDIMENT CONTROL STONE","","",3835,47.865449804432899,183564]
["6015000000-E","TEMP MULCHING","","",28,1020.22321428571,28566.25]
["6018000000-E","SEED FOR TEMP SEEDING","","",2200,2.8,6160]
["6021000000-E","FERT FOR TEMP SEEDING","","",11,1063.8181818181799,11702]
["6024000000-E","TEMP SLOPE DRAINS","","",1600,12.7125,20340]
["6029000000-E","SAFETY FENCE","","",1800,2.0388888888888901,3670]
["6030000000-E","SILT EXCAVATION","","",4400,13.1134090909091,57699]
["6036000000-E","MATTING FOR EROS CONTROL","","",64650,1.6990719257540601,109845]
["6037000000-E","COIR FIBER MAT","","",2245,6.3576837416481098,14273]
["6038000000-E","PERM SOIL REINF MAT","","",1400,4.6428571428571397,6500]
["6042000000-E","1/4\" HARDWARE CLOTH","","",10915,5.6530691708657796,61703.25]
["6045000000-E","**\" TEMP PIPE","(18\")","",80,39,3120]
["","","(24\")","",270,76.244444444444397,20586]
["6069000000-E","STILLING BASINS","","",135,20,2700]
["6070000000-N","SPECIAL STILLING BASINS","","",10,309.63,3096.3]
["6071012000-E","COIR FIBER WATTLE","","",1090,10.249541284403699,11172]
["6071014000-E","COIR FIBER WATTLE BARRIER","","",740,14.4864864864865,10720]
["6071020000-E","POLYACRYLAMIDE (PAM)","","",805,13.5484472049689,10906.5]
["6071030000-E","COIR FIBER BAFFLE","","",510,10.281862745098,5243.75]
["6084000000-E","SEEDING AND MULCHING","","",34,2090.8529411764698,71089]
["6087000000-E","MOWING","","",22.5,195.62666666666701,4401.6000000000004]
["6090000000-E","SEED FOR REPAIR SEEDING","","",550,3.30909090909091,1820]
["6093000000-E","FERT FOR REPAIR SEEDING","","",2,996.57500000000005,1993.15]
["6096000000-E","SEED FOR SUPP SEEDING","","",775,4.82258064516129,3737.5]
["6108000000-E","FERTILIZER TOPDRESSING","","",18.5,1090.56756756757,20175.5]
["6111000000-E","IMPERVIOUS DIKE","","",725,64.110344827586204,46480]
["6114500000-N","SPECIALIZED HAND MOWING","","",80,51.625,4130]
["6117000000-N","RESPONSE FOR EROS CONTROL","","",164,150.01524390243901,24602.5]
["6117500000-N","CONC WASHOUT STR","","",38,1171.87368421053,44531.199999999997]
["6123000000-E","REFORESTATION","","",5.5,3469.3636363636401,19081.5]
["6126000000-E","STREAMBANK REFORESTATION","","",0.31,3450,1069.5]
["6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",86,185,15910]
["","","FABRIC INSERT INLET PROTECTIONDEVICE","",43,265,11395]
["7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",21,981.8,20617.8]
["7060000000-E","SIGNAL CABLE","","",17890,3.5900223588597,64225.5]
["7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",62,970.72741935483896,60185.1]
["7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",13,1096.24615384615,14251.2]
["7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",14,1550,21700]
["7264000000-E","MESSENGER CABLE (3/8\")","","",1800,5.0287499999999996,9051.75]
["7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",4620,8.1063311688311703,37451.25]
["7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",235,15.8,3713]
["","","(2, 2\")","",1905,18.75,35718.75]
["7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",74,402.95675675675699,29818.799999999999]
["7360000000-N","WOOD POLE","","",4,1110,4440]
["7372000000-N","GUY ASSEMBLY","","",7,570,3990]
["7444000000-E","INDUCTIVE LOOP SAWCUT","","",9443,9.2770729641003893,87603.4]
["7456000000-E","LEAD-IN CABLE(********)","(14-2)","",28140,2.2058280028429298,62072]
["7481000000-N","SITE SURVEY","","",3,851,2553]
["7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",12,740,8880]
["7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",12,3350,40200]
["7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",3,9550,28650]
["7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",9,910,8190]
["7528000000-E","DROP CABLE","","",20,2.8,56]
["7540000000-N","SPLICE ENCLOSURE","","",1,1470.6,1470.6]
["7552000000-N","INTERCONNECT CENTER","","",1,1785.7,1785.7]
["7564100000-N","FIBER-OPTIC TRANS SELF HEAL","","",1,1575.6,1575.6]
["7574000000-N","FURN FIB-OPT TRANSCEIVER","","",1,1575.6,1575.6]
["7575142000-N","900MHZ SPECTRUM RADIO","","",4,3600,14400]
["7576000000-N","METAL STRAIN SIGNAL POLE","","",5,6565,32825]
["7588000000-N","SGNL MAST ARM WITH METAL POLE","","",16,19900,318400]
["7613000000-N","SOIL TEST","","",21,1456.6428571428601,30589.5]
["7614100000-E","DRILLED PIER FOUND","","",174,972.46551724137896,169209]
["7630000000-N","METAL STRAIN POLE DESIGN","","",5,105,525]
["7631000000-N","MAST ARM W/ MTL POLE DES","","",16,400,6400]
["7636000000-N","SIGN FOR SIGNALS","","",22,512.76363636363601,11280.8]
["7642100000-N","TYPE I POST W/ FOUND","","",4,1260.5,5042]
["7642200000-N","TYPE II PED W/ FOUND","","",19,1849.6842105263199,35144]
["7675000000-N","LED BLANKOUT SIGN","","",2,3676.4,7352.8]
["7684000000-N","SIGNAL CABINET FOUND","","",6,1260.13333333333,7560.8]
["7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070E, BASE MOUNTED)","",4,15000,60000]
["7744000000-N","DETECTOR CARD (TYPE 170)","","",34,130,4420]
["7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",2,12079.6,24159.200000000001]
["7780000000-N","DETECTOR CARD (TYPE 2070L)","","",28,157.6,4412.8]
["7901000000-N","CABINET BASE EXTENDER","","",6,591.73333333333301,3550.4]
["7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,12000,12000]
["7960000000-N","METAL POLE FOUND REMVL","","",2,2200.4,4400.8]
["7972000000-N","METAL POLE REMOVAL","","",2,1375.2,2750.4]
["7980000000-N","GENERIC SIGNAL ITEM (EA)","ETHERNET EDGE SWITCH","",1,1313,1313]
["","","PROTECTIVE COATING FOR","PUSHBUTTON POST (BLACK)",14,230,3220]
["","","PROTECTIVE COATING FOR SINGLE","MAST ARM POLE (BLACK)",16,2850,45600]
["8017000000-N","CM&R TEMP ACCESS ***********","(14+94.00 -L-)","",1,62500,62500]
["8035000000-N","REMV EXIST STR **********","(13+52.00-L-)","",1,12000,12000]
["","","(14+27.00-L-)","",1,25000,25000]
["","","(14+94.00 -L-)","",1,49600,49600]
["","","(17+23.00-L-)","",1,65000,65000]
["8049000000-N","REMV EXIST STR **********","(13+86.00-L-)","",1,50000,50000]
["8056000000-N","REMV EXIST STR **********","(22+17.00-Y7)","",1,11880,11880]
["8065000000-N","ASBESTOS ASSESSMENT","","",6,1496.8333333333301,8981]
["8096000000-E","PILE EXCAVATION IN SOIL","","",77,200,15400]
["8097000000-E","PILE EXCAVATION NOT IN SOIL","","",133,302.59398496240601,40245]
["8121000000-N","UNCL STR EXCAV STA *****","(13+52.00-L-)","",1,7500,7500]
["","","(13+86.00-L-)","",1,25000,25000]
["","","(14+27.00-L-)","",1,75000,75000]
["","","(14+94.00 -L-)","",1,10000,10000]
["8126000000-N","CULV EXCAV @ ************","(17+23.00-L-)","",1,60000,60000]
["","","(19+20.00 -L-)","",1,11000,11000]
["","","(22+17.00-Y7)","",1,21384,21384]
["8133000000-E","FND CONDIT MAT, BOX CULV","","",215,50.1100465116279,10773.66]
["8161000000-E","GROOVING BRIDGE FLOORS","","",34904,0.85,29668.400000000001]
["8175000000-E","CLASS AA CONC (BRIDGE)","","",43.7,851,37188.699999999997]
["8182000000-E","CLASS A CONC (BRIDGE)","","",203.2,892.46751968503895,181349.4]
["8196000000-E","CLASS A CONC (CULV)","","",203.6,1181.9253438113899,240640]
["8210000000-N","BRG APPR SLAB ***********","(13+52.00-L-)","",1,20000,20000]
["","","(13+86.00-L-)","",1,28000,28000]
["","","(14+27.00-L-)","",1,37000,37000]
["","","(14+94.00 -L-)","",1,29500,29500]
["8217000000-E","REINF STEEL (BRIDGE)","","",29302,1.56764043410006,45935]
["8224000000-E","EPOXY COAT REINF STL BRDG","","",1092,1.7,1856.4]
["8245000000-E","REINF STEEL (CULVERT)","","",23636,1.6165467930275901,38208.699999999997]
["8296000000-N","POLLUTION CONTROL","","",1,35000,35000]
["8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",28,480,13440]
["","","(HP12X53)","",28,1,28]
["8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(PP 18 X 0.50)","",7,600,4200]
["8364000000-E","HP12X53 PILES","","",2225,68.085393258427004,151490]
["8387000000-E","PP18X0.50 GALV STL PILE","","",490,85,41650]
["8391000000-N","STEEL PILE POINTS","","",14,120,1680]
["8475000000-E","TWO BAR METAL RAIL","","",205.25,130,26682.5]
["8482000000-E","THREE BAR METAL RAIL","","",92.2,295,27199]
["8505000000-E","VERT CONC BARRIER RAIL","","",100,182,18200]
["8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-9 1/2\")","",480.25,131.317022384175,63065]
["8559000000-E","SURFACE PREP, CLASS II","","",22.8,130,2964]
["8566000000-E","SURFACE PREP, CLASS III","","",5,525,2625]
["8573000000-E","LATEX MOD CONC OVERLAY","","",158.6,2000,317200]
["8580000000-E","PLACING LATEX MOD CONC","","",4572,30,137160]
["8608000000-E","RIP RAP II (2'-0\")","","",1156,50.297577854671303,58144]
["8622000000-E","GEOTEXTILE FOR DRAINAGE","","",1346,4.1560178306092102,5594]
["8657000000-N","ELASTOMERIC BEARINGS","","",4,3750,15000]
["8660000000-E","CONC REPAIRS","","",26.7,1150,30705]
["8664000000-E","SHOTCRETE REPAIRS","","",232.3,1050,243915]
["8678000000-E","EPOXY RESIN INJECTION","","",175.5,150,26325]
["8753200000-E","3'-0\"X 3'-3\" PRESTR BOX BEAM","","",1100,329,361900]
["8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",440,135,59400]
["8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",2200,178.65,393030]
["8801000000-E","MSE RETAIN WALL NO **","(W3)","",1084,98.2,106448.8]
["","","(W4)","",682,108.1,73724.2]
["8802014000-E","SOLDIER PILE RETAINING WALLS","","",3495,137.03862660944199,478950]
["8802030000-E","SEGMENTAL GRAVITY RETAIN WALLS","","",2243,50.941729826125702,114262.3]
["8804000000-N","GENERIC CULVERT ITEM (LS)","ALUMINUM STRUCTURAL PLATE ARCH","CULVERT",1,170332.1,170332.1]
["8818000000-E","GENERIC CULVERT ITEM (TON)","CULVERT BACKFILL","",320,40.1,12832]
["8860000000-N","GENERIC STR ITEM (LS)","CLEANING & REPAINTING OF BRIDGE 31","",1,230000,230000]
["","","CLEANING & REPAINTING OF BRIDGE 33","",1,230000,230000]
["","","PAINTING CONTAINMENT FOR BRIDGE 31","",1,135000,135000]
["","","PAINTING CONTAINMENT FOR BRIDGE 33","",1,135000,135000]
["","","VOLUMETRIC MIXER","",1,1000,1000]
["8867000000-E","GENERIC STR ITEM (LF)","ANODIZED TWO BAR METAL RAIL","",229.4,220.422842197036,50565]
["","","FOAM JOINT SEALS FOR PRESERVA-TION","",184.8,60,11088]
["","","POURABLE SILICONE JOINT SEAL- ANT","",184.8,40,7392]
["8882000000-E","GENERIC STR ITEM (CF)","CONCRETE FOR DECK REPAIR","",87.9,10,879]
["","","ELASTOMERIC CONCRETE FOR PRES-ERVATION","",46.4,400,18560]
["8889000000-E","GENERIC STR ITEM (LB)","BEAM REPAIR","",1875.9,50,93795]
["8892000000-E","GENERIC STR ITEM (SF)","BRIDGE JOINT DEMOLITION","",184.8,24,4435.2]
["","","CONCRETE WORK FOR JOINT RE- PLACEMENT","",184.8,100,18480]
["","","EPOXY COATING","",2399.6,24,57590.400000000001]
["8893000000-E","GENERIC STR ITEM (SY)","HYDRO-DEMOLITION OF BRIDGE DECK","",4572,52,237744]
["","","SCARIFYING BRIDGE DECK","",4572,20,91440]
["8897000000-N","GENERIC STR ITEM (EA)","TYPE I BRIDGE JACKING BRIDGE 31","",3,10000,30000]
["","","TYPE I BRIDGE JACKING BRIDGE 33","",3,10000,30000]