{"text_format":"1","workbook":"xlsx","n_sheets":18,"sheets":["BExRepositorySheet","SUMMARY - STATEWIDE","ITEMS - STATEWIDE","ITEMS - DIV 01","ITEMS - DIV 02","ITEMS - DIV 03","ITEMS - DIV 04","ITEMS - DIV 05","ITEMS - DIV 06","ITEMS - DIV 07","ITEMS - DIV 08","ITEMS - DIV 09","ITEMS - DIV 10","ITEMS - DIV 11","ITEMS - DIV 12","ITEMS - DIV 13","ITEMS - DIV 14","Graph"],"not_rendered":{"charts":1,"images":18,"macros":1,"external_links":3,"defined_names":67,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BExRepositorySheet","index":0,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
[7]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Filter"]

{"sheet":"SUMMARY - STATEWIDE","index":1,"n_rows":817,"n_cols":25,"rows_kept":817,"cut":false,"hidden":false,"merged":[[0,1,0,24]]}
[null,"NORTH CAROLINA DEPARTMENT OF TRANSPORTATION     2021 BID AVERAGES"]
[null,"LET DATE","RPN","TIP","CONTRACT","PROJECT","CAT","COUNTY","VENDOR NAME","$TOTAL","JOB","FED WRK ","PROJ LGTH (MI)"," LN / CVT FILL DPTH","CVT CODE OVR/UND RET WLL X-SECT","BOX LTH /WLL HT (FT)","BOX SPAN (FT)","BRG SUP STR","SUB STR"," SPAN","CURB-CURB BRG WDTH (FT)","BRG LTH (FT)","AREA","DIV","LOC"]
[null,"1/19/2021","2","BR-0122","C204524","C204514B-EC","1","SAMPSON","S T WOOTEN CORPORATION",29173,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204514B-RW","1","SAMPSON","S T WOOTEN CORPORATION",175929.8,"RW1","I000",6.7000000000000004E-2,2,"B810",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204514B-SI","1","SAMPSON","S T WOOTEN CORPORATION",2330,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204514B-ST","1","SAMPSON","S T WOOTEN CORPORATION",324065.5,"BR01","X080",1.2999999999999999E-2,null,"15",null,33,"722","A",1,30.833300000000001,67.25,"COAST","3","(16+08.00-L-)"]
[null,"","","","","C204514B-TC","1","SAMPSON","S T WOOTEN CORPORATION",3630,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204514B-UT","1","SAMPSON","S T WOOTEN CORPORATION",97025.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","",null,null,null,null,"Result",632153.80000000005]
[null,"","3","BR-0113","C204531","C204531-EC","1","HALIFAX","S T WOOTEN CORPORATION",46639,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204531-RW","1","HALIFAX","S T WOOTEN CORPORATION",207253.2,"RW1","I000",9.5000000000000001E-2,2,"B810",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204531-SI","1","HALIFAX","S T WOOTEN CORPORATION",2400,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204531-ST","1","HALIFAX","S T WOOTEN CORPORATION",430190.75,"BR01","X080",1.7000000000000001E-2,null,"15",null,33,"721","",2,30.833300000000001,92.375,"PDMT","4","(16+10.00-L-)"]
[null,"","","","","C204531-TC","1","HALIFAX","S T WOOTEN CORPORATION",5450,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",691932.95,"","",0.112," ","",null,null,null,null,null,null,null,"","",""]
[null,"","4","","C204599","C204599-RW","1","PERSON","CAROLINA ROAD SOLUTIONS LLC",338714.08,"RW1","",8.07,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",338714.08,"","",8.07,2,"",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204598","C204598-RW","1","FRANKLIN","WHITEHURST PAVING CO INC",663670.67000000004,"RW1","",17.884,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",663670.67000000004,"","",17.884," ","",null,null,"","",null,null,null,"","",""]
[null,"","6","","C204597","C204597A-RW","1","GRANVILLE","FSC II LLC DBA FRED SMITH COMPANY",444976.05,"RW1","",9.19,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204597B-RW","1","VANCE","FSC II LLC DBA FRED SMITH COMPANY",230203,"RW1","",6.4850000000000003,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204597C-RW","1","WARREN","FSC II LLC DBA FRED SMITH COMPANY",25235.599999999999,"RW1","",0.61799999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",700414.65,"","",16.292999999999999," ","",null,null,"","",null,null,null,"","",""]
[null,"","7","","C204595","C204595A-RW","1","GRANVILLE","S T WOOTEN CORPORATION",2751823.07,"RW1","",27.8,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204595B-RW","1","VANCE","S T WOOTEN CORPORATION",12425.05,"RW1","",0.1,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2764248.12,"","",27.9," ","",null,null,"","",null,null,null,"","",""]
[null,"","8","BR-0126","C204487","C204487-EC","1","WILKES","EASTERN STRUCTURES LLC",50785,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204487-RW","1","WILKES","EASTERN STRUCTURES LLC",424685,"RW1","I000",0.159,2,"B801",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204487-ST","1","WILKES","EASTERN STRUCTURES LLC",574241,"BR01","X080",2.1000000000000001E-2,null,"15",null,39,"722","Q",2,36.833300000000001,112.375,"MTN","11","(16+62.00 -L-)"]
[null,"","","","","C204487-TC","1","WILKES","EASTERN STRUCTURES LLC",64301.2,"RW1","I000",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","","","","Result",1114012.2,"","",0.18," ","",null,null,null,null,null,null,null,"","",""]
[null,"","9","","C204590","C204590-RW","1","JACKSON","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",7985479.2800000003,"RW1","",6.4,4,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",7985479.2800000003,"","",6.4," ","",null,null,"","",null,null,null,"","",""]
[null,"2/16/2021","1","R-5740","C204593","C204344-EC","1","PERQUIMANS","BARNHILL CONTRACTING CO",371539,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204344-RW","1","PERQUIMANS","BARNHILL CONTRACTING CO",3102781,"RW1","",4.3769999999999998,2,"D300",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204344-SI","1","PERQUIMANS","BARNHILL CONTRACTING CO",44796,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204344-ST","1","PERQUIMANS","BARNHILL CONTRACTING CO",311784.3,"CV01","Y007",6.0000000000000001E-3,5.67,"C005",55.75,32.916699999999999,"","",null,null,null,"COAST","1","(79+82.10-L-)"]
[null,"","","","","","2","PERQUIMANS","BARNHILL CONTRACTING CO",338770,"CV02","Y007",8.9999999999999993E-3,4.83,"C005",52.75,44,"","",null,null,null,"COAST","1","(132+88.62-L-)"]
[null,"","","","","C204344-TC","1","PERQUIMANS","BARNHILL CONTRACTING CO",15103.2,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204344-UT","1","PERQUIMANS","BARNHILL CONTRACTING CO",848801.98,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","","2","PERQUIMANS","BARNHILL CONTRACTING CO",45263.27,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","","","","Result",5078838.75,"","",4.3920000000000003,22.5,"",108.5,76.916700000000006,"","",null,null,null,"","",""]
[null,"","2","B-4484","C204434","C204434-EC","1","CRAVEN","SANFORD CONTRACTORS INC",532196.5,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204434-RW","1","CRAVEN","SANFORD CONTRACTORS INC",4597059.55,"RW1","",0.51200000000000001,2,"B801",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204434-SI","1","CRAVEN","SANFORD CONTRACTORS INC",45787,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204434-ST","1","CRAVEN","SANFORD CONTRACTORS INC",529627.4,"WL1","Y007",null,null,"W001",44.75,null,"","",null,null,null,"COAST","2","(10+00.00-RETWL1-)"]
[null,"","","","","","2","CRAVEN","SANFORD CONTRACTORS INC",780258.45,"WL2","Y007",null,null,"W001",33.9,null,"","",null,null,null,"COAST","2","(10+00.00-RETWL2-)"]
[null,"","","","","","3","CRAVEN","SANFORD CONTRACTORS INC",4219207.91,"BR01","X281",0.113,null,"15",null,32.25,"854","E",6,30,600,"COAST","2","(25+06.00-L1-)"]
[null,"","","","","","4","CRAVEN","SANFORD CONTRACTORS INC",2193745.17,"BR02","X281",7.5999999999999998E-2,null,"15",null,32.25,"854","E",4,31,400,"COAST","2"," (41+45.00-L1-)"]
[null,"","","","","C204434-TC","1","CRAVEN","SANFORD CONTRACTORS INC",191395.02,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204434-UT","1","CRAVEN","SANFORD CONTRACTORS INC",760223,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",13849500,"","",0.70099999999999996," ","",null,null,null,null,null,null,null,"","",""]
[null,"","3","","C204449","C204449-ST","1","PENDER","BUCKEYE BRIDGE LLC",526825.4,"BR01","X281",3.6999999999999998E-2,null,"11",null,32.833300000000001,"745","I",4,30,194.33330000000001,"COAST","3","BRIDGE NO. 300433"]
[null,"","","","","","2","PENDER","BUCKEYE BRIDGE LLC",305434.3,"BR02","X231",4.7E-2,null,"11",null,46.833300000000001,"564","I",2,44,250.66669999999999,"COAST","3","BRIDGE NO. 700219"]
[null,"","","","","C204449-TC","1","PENDER","BUCKEYE BRIDGE LLC",94166,"0","",null,2,"M720",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",926425.7,"","",8.4000000000000005E-2," ","",null,null,null,null,null,null,null,"","",""]
[null,"","4","B-5639","C204535","C204535-EC","1","DUPLIN","S T WOOTEN CORPORATION",190199.7,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204535-RW","1","DUPLIN","S T WOOTEN CORPORATION",1189086.2,"RW1","",0.29599999999999999,2,"B812",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204535-SI","1","DUPLIN","S T WOOTEN CORPORATION",9777.6,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204535-ST","1","DUPLIN","S T WOOTEN CORPORATION",1427144,"BR01","X080",3.3000000000000002E-2,null,"15",null,36,"722","E",3,33.833300000000001,172.5,"PDMT","3","(23+55.00-L-)"]
[null,"","","","","C204535-TC","1","DUPLIN","S T WOOTEN CORPORATION",39346,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204535-UT","1","DUPLIN","S T WOOTEN CORPORATION",120340,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","","","","Result",2975893.5,"","",0.32900000000000001," ","",null,null,null,null,null,null,null,"","",""]
[null,"","5","B-5534","C204534","C204534-EC","1","DUPLIN","S T WOOTEN CORPORATION",163557,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204534-RW","1","DUPLIN","S T WOOTEN CORPORATION",1121113,"RW1","",0.28299999999999997,2,"B801",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204534-SI","1","DUPLIN","S T WOOTEN CORPORATION",1040,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204534-ST","1","DUPLIN","S T WOOTEN CORPORATION",875198.72,"BR01","X081",0.02,null,"15",null,43.25,"836","A",3,40,105,"PDMT","3","(21+68.50-L-)"]
[null,"","","","","C204534-TC","1","DUPLIN","S T WOOTEN CORPORATION",69828,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204534-UT","1","DUPLIN","S T WOOTEN CORPORATION",95088.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","","","","Result",2325825.2200000002,"","",0.30299999999999999," ","",null,null,null,null,null,null,null,"","",""]
[null,"","6","B-5662","C204489","C204489-EC","1","HALIFAX","NATIONAL BRIDGE BUILDERS LLC",76225,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204489-RW","1","HALIFAX","NATIONAL BRIDGE BUILDERS LLC",632941.1,"RW1","I000",0.17599999999999999,2,"B812",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204489-SI","1","HALIFAX","NATIONAL BRIDGE BUILDERS LLC",20557.900000000001,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204489-ST","1","HALIFAX","NATIONAL BRIDGE BUILDERS LLC",1163969.3999999999,"BR01","X080",2.1000000000000001E-2,null,"15",null,35.25,"836","E",2,32,110,"PDMT","4","(15+61.00-L-)"]
[null,"","","","","C204489-TC","1","HALIFAX","NATIONAL BRIDGE BUILDERS LLC",86102,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204489-UT","1","HALIFAX","NATIONAL BRIDGE BUILDERS LLC",264654,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",2244449.4,"","",0.19700000000000001,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","7","B-5671","C204517","C204517B-EC","1","EDGECOMBE","NATIONAL BRIDGE BUILDERS LLC",63930.25,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204517B-RW","1","EDGECOMBE","NATIONAL BRIDGE BUILDERS LLC",455471.35,"RW1","",0.151,2,"B810",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204517B-SI","1","EDGECOMBE","NATIONAL BRIDGE BUILDERS LLC",900,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204517B-ST","1","EDGECOMBE","NATIONAL BRIDGE BUILDERS LLC",1223927,"BR01","X081",3.7999999999999999E-2,null,"15",null,35.25,"854","E",2,32,200,"PDMT","4","(17+00.00-L-)"]
[null,"","","","","C204517B-TC","1","EDGECOMBE","NATIONAL BRIDGE BUILDERS LLC",17810,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204517B-UT","1","EDGECOMBE","NATIONAL BRIDGE BUILDERS LLC",219336.2,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",1981374.8,"","",0.189," ","",null,null,null,null,null,null,null,"","",""]
[null,"","8","","C204602","C204602-RW","1","GRANVILLE","BOXLEY MATERIALS COMPANY",643370.55000000005,"RW1","",11.942,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",643370.55000000005,"","",11.942," ","",null,null,"","",null,null,null,"","",""]
[null,"","9","","C204606","C204606A-RW","1","RANDOLPH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2341151.08,"RW1","",5.92,4,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204606B-RW","1","RANDOLPH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2111037.14,"RW1","",17.440000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",4452188.22,"","",23.36,null,"",null,null,"","",null,null,null,"","",""]
[null,"","10","","C204601","C204601-RW","1","MOORE","FSC II LLC DBA FRED SMITH COMPANY",1169406.05,"RW1","",2.2480000000000002,5,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",1169406.05,"","",2.2480000000000002,null,"",null,null,"","",null,null,null,"","",""]
[null,"","11","","C204607","C204607-RW","1","RANDOLPH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",3157460.86,"RW1","",18.914000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",3157460.86,"","",18.914000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","12","","C204608","C204608-RW","1","RANDOLPH","BLYTHE CONSTRUCTION INC",3091982.31,"RW1","",23.105,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",3091982.31,"","",23.105,null,"",null,null,"","",null,null,null,"","",""]
[null,"","13","B-5825","C204490","C204490-EC","1","YADKIN","SMITH-ROWE, LLC",283449.2,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","11",""]
[null,"","","","","C204490-RW","1","YADKIN","SMITH-ROWE, LLC",3395061.16,"RW1","",0.55600000000000005,2,"B801",null,null,"","",null,null,null,"PDMT","11",""]
[null,"","","","","C204490-SI","1","YADKIN","SMITH-ROWE, LLC",30929,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","11",""]
[null,"","","","","C204490-ST","1","YADKIN","SMITH-ROWE, LLC",142201.82999999999,"CV01","Y007",null,13.45,"C201",102.08,9,"","",null,null,null,"PDMT","11","(46+80.60-L-)"]
[null,"","","","","","2","YADKIN","SMITH-ROWE, LLC",276316.68,"CV02","Y007",null,19.100000000000001,"C001",150,9,"","",null,null,null,"PDMT","11","(19+90.69-Y2-)"]
[null,"","","","","","3","YADKIN","SMITH-ROWE, LLC",5131153.1100000003,"BR01","X081",0.20200000000000001,null,"15",null,35.35,"873","Q",9,32,1066.6667,"PDMT","11","(34+65.50-L-)"]
[null,"","","","","C204490-TC","1","YADKIN","SMITH-ROWE, LLC",72572.55,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","11",""]
[null,"","","","","C204490-UT","1","YADKIN","SMITH-ROWE, LLC",246144.93,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","11",""]
[null,"","","","","","","","Result",9577828.4600000009,"","",0.75800000000000001,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","14","BR-0047","C204394","C204394-EC","1","STOKES","SMITH-ROWE, LLC",78864.83,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204394-RW","1","STOKES","SMITH-ROWE, LLC",1718084.48,"RW1","I000",0.25900000000000001,2,"B811",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204394-SI","1","STOKES","SMITH-ROWE, LLC",16966.900000000001,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204394-ST","1","STOKES","SMITH-ROWE, LLC",271348,"WL1","Y007",null,null,"W001",16.59,null,"","",null,null,null,"PDMT","9","(13+57.28-Y2-)"]
[null,"","","","","","2","STOKES","SMITH-ROWE, LLC",214274.34,"WL2","Y007",null,null,"W001",14.52,null,"","",null,null,null,"PDMT","9","(13+57.28-Y2-)"]
[null,"","","","","","3","STOKES","SMITH-ROWE, LLC",1762309.18,"BR01","X231",0.04,null,"11",null,54.083300000000001,"638","I",2,46,210.5,"PDMT","9","(18+27.98-L-)"]
[null,"","","","","C204394-TC","1","STOKES","SMITH-ROWE, LLC",184933.9,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204394-UT","1","STOKES","SMITH-ROWE, LLC",481379.14,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",4728160.7699999996,"","",0.29899999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","15","","C204604","C204604-RW","1","DAVIDSON","BLYTHE CONSTRUCTION INC",4150984.76,"RW1","",28.6,4,"R000",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",4150984.76,"","",28.6," ","",null,null,"","",null,null,null,"","",""]
[null,"","16","","C204304","C204304-RW","1","BUNCOMBE","NHM CONSTRUCTORS LLC",290797.56,"RW1","",null,5,"M720",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204304-ST","1","BUNCOMBE","NHM CONSTRUCTORS LLC",561526.57999999996,"BR01","X231",4.3999999999999997E-2,null,"11",null,66,"336","I",4,64,233,"MTN","13","BRIDGE NO. 481"]
[null,"","","","","","2","BUNCOMBE","NHM CONSTRUCTORS LLC",652365.6,"BR02","X231",4.2000000000000003E-2,null,"11",null,70,"572","I",3,68,220.5,"MTN","13","BRIDGE NO. 495"]
[null,"","","","","","3","BUNCOMBE","NHM CONSTRUCTORS LLC",2940009.58,"BR03","X331",0.18,null,"17",null,67.2,"571","N",7,54.7,952.58,"MTN","13","BRIDGE NO. 705"]
[null,"","","","","C204304-TC","1","BUNCOMBE","NHM CONSTRUCTORS LLC",145715.6,"RW1","",null,5,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","","","Result",4590414.92,"","",0.26600000000000001,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","17","BR-0009","C204386","C204386-EC","1","BUNCOMBE","BUCKEYE BRIDGE LLC",63756.25,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204386-RW","1","BUNCOMBE","BUCKEYE BRIDGE LLC",345787.02,"RW1","",0.105,2,"B801",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204386-SI","1","BUNCOMBE","BUCKEYE BRIDGE LLC",7967,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204386-ST","1","BUNCOMBE","BUCKEYE BRIDGE LLC",548007.16,"BR01","X080",1.2999999999999999E-2,null,"15",null,36,"722","A",1,33.5,67.604200000000006,"MTN","13","(12+94.70-L-)"]
[null,"","","","","C204386-TC","1","BUNCOMBE","BUCKEYE BRIDGE LLC",31492.7,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","","","Result",997010.13,"","",0.11799999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","18","","C204600","C204600-RW","1","HENDERSON","ROGERS GROUP INC",4059703.98,"RW1","",5.81,4,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",4059703.98,"","",5.81," ","",null,null,"","",null,null,null,"","",""]
[null,"","19","","C204605","C204605-RW","1","CHEROKEE","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",10546245.939999999,"RW1","",8.1,4,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",10546245.939999999,"","",8.1," ","",null,null,"","",null,null,null,"","",""]
[null,"3/16/2021","1","W-5600","C204359","C204359-EC","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",2482760.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204359-RW","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",42843090.560000002,"RW1","I000",4.9589999999999996,4,"D311",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204359-SG","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",675604.25,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204359-SI","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",490867.63,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204359-ST","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",189057.85,"CV01","Y007",null,10,"C203",92.58,5.6665999999999999,"","",null,null,null,"PDMT","4","(45+66.22-L-)"]
[null,"","","","","","2","JOHNSTON","FLATIRON CONSTRUCTORS INC",38637.75,"CV02","Y007",null,2.69,"C202",8,10,"","",null,null,null,"PDMT","4","(155+30.40-L-)"]
[null,"","","","","","3","JOHNSTON","FLATIRON CONSTRUCTORS INC",502358.3,"CV03","Y007",null,30.12,"C002",151,22.416699999999999,"","",null,null,null,"PDMT","4","(28+84.00-Y7-)"]
[null,"","","","","","4","JOHNSTON","FLATIRON CONSTRUCTORS INC",1038582,"WL1","Y007",null,null,"W001",null,null,"","",null,null,null,"PDMT","4","(10+00.00-WL1-)"]
[null,"","","","","","5","JOHNSTON","FLATIRON CONSTRUCTORS INC",1164993,"WL2","Y007",null,null,"W001",null,null,"","",null,null,null,"PDMT","4","(10+00.00-WL2-)"]
[null,"","","","","","6","JOHNSTON","FLATIRON CONSTRUCTORS INC",873525,"BR01","X281",1.9E-2,null,"11",null,47.25,"754","A",1,44,97.447000000000003,"PDMT","4","(217+31.76-L-) LT"]
[null,"","","","","","7","JOHNSTON","FLATIRON CONSTRUCTORS INC",510933.45,"BR02","X281",null,null,"11",null,47.25,"754","A",1,44,97.552099999999996,"PDMT","4","(217+31.76-L-) RT"]
[null,"","","","","","8","JOHNSTON","FLATIRON CONSTRUCTORS INC",1763226.15,"BR03","X281",null,null,"11",null,56.093299999999999,"854","Q",2,53.5,194.5,"PDMT","4","(27+01.91-Y7-)"]
[null,"","","","","C204359-TC","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",3457740.62,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204359-UT","1","JOHNSTON","FLATIRON CONSTRUCTORS INC",2832625.07,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",58864002.130000003,"","",4.9779999999999998,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","2","","C204202","C204202-EC","1","HENDERSON","FLATIRON CONSTRUCTORS INC",248818.25,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204202-RW","1","HENDERSON","FLATIRON CONSTRUCTORS INC",5684442.4500000002,"RW1","",0.53400000000000003,4,"M720",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204202-SG","1","HENDERSON","FLATIRON CONSTRUCTORS INC",1301264.75,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204202-SI","1","HENDERSON","FLATIRON CONSTRUCTORS INC",46753.599999999999,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204202-ST","1","HENDERSON","FLATIRON CONSTRUCTORS INC",18824074.5,"BR01","X031",0.20899999999999999,null,"15",null,89.416700000000006,"430","O",5,86.166600000000003,1049.75,"VERY MTN","14","(35+30.22-L-)"]
[null,"","","","","C204202-TC","1","HENDERSON","FLATIRON CONSTRUCTORS INC",865277.66,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",26970631.210000001,"","",0.74299999999999999,20,"",null,89.416700000000006,"","",5,86.166600000000003,1049.75,"","",""]
[null,"","3","BR-0119","C204521","C204515B-EC","1","PITT","SANFORD CONTRACTORS INC",50158.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515B-RW","1","PITT","SANFORD CONTRACTORS INC",309901.55,"RW1","I000",0.10199999999999999,2,"B810",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515B-SI","1","PITT","SANFORD CONTRACTORS INC",5040,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515B-ST","1","PITT","SANFORD CONTRACTORS INC",520755.7,"BR01","X080",1.7000000000000001E-2,null,"15",null,33,"729","A",1,30.833300000000001,92.25,"COAST","2","(13+34.00 -L-)"]
[null,"","","","","C204515B-TC","1","PITT","SANFORD CONTRACTORS INC",3482,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515B-UT","1","PITT","SANFORD CONTRACTORS INC",22956,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","2","PITT","SANFORD CONTRACTORS INC",22956,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",935250,"","",0.11899999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","4","","C204618","C204618A-RW","1","VANCE","CAROLINA SUNROCK LLC",999428.91,"RW1","",3.2709999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204618B-RW","1","VANCE","CAROLINA SUNROCK LLC",2833584.69,"RW1","",22.93,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204618C-RW","1","VANCE","CAROLINA SUNROCK LLC",68187.95,"RW1","",0.71399999999999997,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",3901201.55,"","",26.914999999999999," ","",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204610","C204610-RW","1","PERSON","CAROLINA SUNROCK LLC",2976291.35,"RW1","",27.032,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2976291.35,"","",27.032," ","",null,null,"","",null,null,null,"","",""]
[null,"","6","","C204616","C204616A-RW","1","VANCE","CAROLINA SUNROCK LLC",485849.25,"RW1","",5.12,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204616B-RW","1","WARREN","CAROLINA SUNROCK LLC",2280669.48,"RW1","",18.526,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2766518.73,"","",23.646000000000001," ","",null,null,"","",null,null,null,"","",""]
[null,"","7","BR-0042","C204392","C204392-EC","1","ROCKINGHAM","SMITH-ROWE, LLC",112231.6,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204392-RW","1","ROCKINGHAM","SMITH-ROWE, LLC",1678123.6,"RW1","",0.29899999999999999,2,"B813",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204392-SI","1","ROCKINGHAM","SMITH-ROWE, LLC",23656.54,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204392-ST","1","ROCKINGHAM","SMITH-ROWE, LLC",162202.15,"WL1","Y007",null,null,"W005",19.329999999999998,null,"","",null,null,null,"PDMT","7","(1, 19+56.99 -L-)"]
[null,"","","","","","2","ROCKINGHAM","SMITH-ROWE, LLC",243300.42,"WL2","Y007",null,null,"W005",19.09,null,"","",null,null,null,"PDMT","7","(2, 19+56.99 -L-)"]
[null,"","","","","","3","ROCKINGHAM","SMITH-ROWE, LLC",1208681.47,"BR01","X281",3.9E-2,null,"11",null,39.25,"864","I",2,36,208,"PDMT","7","(19+56.99 -L-)"]
[null,"","","","","C204392-TC","1","ROCKINGHAM","SMITH-ROWE, LLC",248500.8,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",3676696.58,"","",0.33800000000000002,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","8","I-5711","C204603","C204352-EC","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",206599.11,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204352-LI","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",79160.66,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204352-RW","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",5388610.21,"RW1","I000",0.56299999999999994,8,"D344",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204352-SG","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",1172227.81,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204352-SI","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",419320.61,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204352-ST","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",98600,"WL1","Y007",null,null,"W001",8,null,"","",null,null,null,"PDMT","7","(34+82.39 -L-)"]
[null,"","","","","","2","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",29659.5,"WL2","Y007",null,null,"W001",6.5,null,"","",null,null,null,"PDMT","7","(19+70.65 -L-)"]
[null,"","","","","","3","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",4344967.01,"BR01","X231",4.2000000000000003E-2,null,"",null,71.083299999999994,"592","Q",4,57.5,221,"PDMT","7","(37+02.26 -L-)"]
[null,"","","","","C204352-TC","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",787587.8,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204352-UT","1","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",254250,"RW1","I000",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","2","ALAMANCE","ZACHRY CONSTRUCTION CORPORATION",84750,"RW1","NPAR",null,8,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",12865732.710000001,"","",0.60499999999999998,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","9","","C204612","C204612-RW","1","CHATHAM","FSC II LLC DBA FRED SMITH COMPANY",2501597.2000000002,"RW1","",27.77,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2501597.2000000002,"","",27.77," ","",null,null,"","",null,null,null,"","",""]
[null,"","10","","C204613","C204613-RW","1","CHATHAM","FSC II LLC DBA FRED SMITH COMPANY",2378351.36,"RW1","",26.475000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2378351.36,"","",26.475000000000001," ","",null,null,"","",null,null,null,"","",""]
[null,"","11","","C204619","C204619A-RW","1","RANDOLPH","FSC II LLC DBA FRED SMITH COMPANY",853411.79,"RW1","",2.12,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204619B-RW","1","RANDOLPH","FSC II LLC DBA FRED SMITH COMPANY",1173753.1499999999,"RW1","",9.7899999999999991,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2027164.94,"","",11.91," ","",null,null,"","",null,null,null,"","",""]
[null,"","12","","C204617","C204617A-RW","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",1079023.33,"RW1","",7.4740000000000002,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204617B-RW","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2028172.12,"RW1","",12.102,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",3107195.45,"","",19.576000000000001," ","",null,null,"","",null,null,null,"","",""]
[null,"","13","","C204614","C204614-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",1765276,"RW1","",7.04,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",1765276,"","",7.04," ","",null,null,"","",null,null,null,"","",""]
[null,"","14","","C204615","C204615A-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",571189.93000000005,"RW1","",2.54,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204615B-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",2868972.7,"RW1","",17.21,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204615C-RW","1","UNION","LYNCHES RIVER CONTRACTING INC",531150.05000000005,"RW1","",null,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",3971312.68,"","",19.75," ","",null,null,"","",null,null,null,"","",""]
[null,"","15","","C204609","C204609-RW","1","MACON","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",11767325.300000001,"RW1","",8.6300000000000008,5,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",11767325.300000001,"","",8.6300000000000008," ","",null,null,"","",null,null,null,"","",""]
[null,"3/26/2021","1","HO-0002A","C204556","C204556C-RW","1","BUNCOMBE","BROOKS BERRY HAYNIE & ASSOCIATES, INC.",17142200,"RW1","K000",130,null,"M713",null,null,"","",null,null,null,"MTN","4",""]
[null,"","","","","","","","Result",17142200,"","",130,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","HO-0002B","C204556","C204556D-RW","1","ANSON","BROOKS BERRY HAYNIE & ASSOCIATES, INC.",12856650,"RW1","K000",100,null,"M713",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",12856650,"","",100,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","HO-0002C","C204556","C204556E-RW","1","COLUMBUS","BROOKS BERRY HAYNIE & ASSOCIATES, INC.",12856650,"RW1","K000",70,null,"M713",null,null,"","",null,null,null,"COAST","4",""]
[null,"","","","","","","","Result",12856650,"","",70,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","I-5986C","C204556","C204556B-RW","1","CUMBERLAND","BROOKS BERRY HAYNIE & ASSOCIATES, INC.",25713300,"RW1","K000",181,null,"M713",null,null,"","",null,null,null,"COAST","4",""]
[null,"","","","","","","","Result",25713300,"","",181,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","R-5777D","C204556","C204556A-RW","1","CRAVEN","BROOKS BERRY HAYNIE & ASSOCIATES, INC.",17142200,"RW1","K000",119,null,"M713",null,null,"","",null,null,null,"COAST","4",""]
[null,"","","","","","","","Result",17142200,"","",119,null,"",null,null,"","",null,null,null,"","",""]
[null,"4/20/2021","2","B-4414","C204178","C204178-EC","1","BEAUFORT","S T WOOTEN CORPORATION",78105.25,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204178-RW","1","BEAUFORT","S T WOOTEN CORPORATION",571502,"RW1","",0.159,2,"B810",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204178-SI","1","BEAUFORT","S T WOOTEN CORPORATION",14259.8,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204178-ST","1","BEAUFORT","S T WOOTEN CORPORATION",1170875.44,"BR01","X081",0.03,null,"15",null,43.25,"836","A",3,40,157.04169999999999,"COAST","2","(24+78.90-L-)"]
[null,"","","","","C204178-TC","1","BEAUFORT","S T WOOTEN CORPORATION",5900,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",1840642.49,"","",0.189," ","",null,null,null,null,null,null,null,"","",""]
[null,"","3","B-5302","C204594","C204219A-ST","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",980225,"BR01","X031",0.23,null,"15",null,61.25,"430","E",35,52,1222.7969000000001,"COAST","2","BRIDGE NO. 25"]
[null,"","","","","C204219B-EC","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",196440,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204219B-RW","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",2676157,"RW1","",0.34499999999999997,4,"B810",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204219B-SG","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",84398.5,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204219B-SI","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",33953,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204219B-ST","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",4785854.9000000004,"BR01","X181",4.7E-2,null,"12",null,70.25,"854","E",3,68,245.75,"COAST","2","(28+85.96-L-)"]
[null,"","","","","C204219B-TC","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",53463.9,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204219B-UT","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",2375299.7999999998,"RW1","VREG",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",11185792.1,"","",0.622,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","","","C204594","C204219A-TC","1","BEAUFORT","CATON CONSTRUCTION GROUP INC",282552.2,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",282552.2,"","",null," ","",null,null,"","",null,null,null,"","",""]
[null,"","4","","C204630","C204630A-RW","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",5114473.1500000004,"RW1","",21.175000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204630B-RW","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",408912.45,"RW1","",4.149,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",5523385.5999999996,"","",25.324000000000002," ","",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204624","C204624A-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",4672846.33,"RW1","",8.1999999999999993,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204624B-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",1027036.74,"RW1","",3.48,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",5699883.0700000003,"","",11.68," ","",null,null,"","",null,null,null,"","",""]
[null,"","7","R-5797","C204571","C204571-EC","1","COLUMBUS","BMCO CONSTRUCTION, INC.",588790.75,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204571-RW","1","COLUMBUS","BMCO CONSTRUCTION, INC.",12314044.119999999,"RW1","",1.006,4,"I600",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204571-SG","1","COLUMBUS","BMCO CONSTRUCTION, INC.",401869.95,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204571-SI","1","COLUMBUS","BMCO CONSTRUCTION, INC.",113799.01,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204571-ST","1","COLUMBUS","BMCO CONSTRUCTION, INC.",211151.5,"WL1","Y007",null,null,"W001",8.15,null,"","",null,null,null,"COAST","6","(10+00.00-WALL1-"]
[null,"","","","","","2","COLUMBUS","BMCO CONSTRUCTION, INC.",227171,"WL2","Y007",null,null,"W001",6.9,null,"","",null,null,null,"COAST","6","(17+00.00-WALL2-)"]
[null,"","","","","","3","COLUMBUS","BMCO CONSTRUCTION, INC.",999722.44,"BR01","X281",null,null,"11",null,39.25,"854","I",2,36.666699999999999,200.5,"COAST","6","(30+65.33-Y1B-)"]
[null,"","","","","C204571-TC","1","COLUMBUS","BMCO CONSTRUCTION, INC.",780467.6,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204571-UT","1","COLUMBUS","BMCO CONSTRUCTION, INC.",554263,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",16191279.369999999,"","",1.006,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","8","BR-0014","C204483","C204483-EC","1","CUMBERLAND","S & C CONSTRUCTION LLC",60643,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204483-RW","1","CUMBERLAND","S & C CONSTRUCTION LLC",1502750.6,"RW1","",0.252,2,"B810",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204483-SI","1","CUMBERLAND","S & C CONSTRUCTION LLC",37313.1,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204483-ST","1","CUMBERLAND","S & C CONSTRUCTION LLC",570792.97,"BR01","X081",2.1000000000000001E-2,null,"15",null,36.25,"836","A",2,33,110,"COAST","6","(21+37.00 -L REV-)"]
[null,"","","","","C204483-TC","1","CUMBERLAND","S & C CONSTRUCTION LLC",71289.279999999999,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",2242788.9500000002,"","",0.27300000000000002,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","9","R-4707","C204499","C204499-EC","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2547001.13,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204499-LI","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",551383.91,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204499-RW","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",29053015.02,"RW1","",1.33,4,"I640",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204499-SG","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",550751.25,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204499-SI","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",754789.6,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204499-ST","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",1105002,"CV01","Y007",null,36.9,"C203",440.25,7,"","",null,null,null,"PDMT","7","(56+34.85 -L-)"]
[null,"","","","","","2","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",1549164.5,"CV02","Y007",null,37.99,"C004",378.08,8,"","",null,null,null,"PDMT","7","(46+07.79 -Y-)"]
[null,"","","","","","3","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",343634.5,"WL1","Y007",null,null,"W005",18.54,null,"","",null,null,null,"PDMT","7","(10+00.00 -W1-)"]
[null,"","","","","","4","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",331828.44,"WL2","Y007",null,null,"W005",17.96,null,"","",null,null,null,"PDMT","7","(10+00.00 -W2-)"]
[null,"","","","","","5","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2810106.75,"BR01","X281",null,null,"11",null,121.23,"854","I",2,118,157.5,"PDMT","7","(41+39.51 -Y-)"]
[null,"","","","","C204499-TC","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",1401321.31,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204499-UT","1","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",3158398.57,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","2","GUILFORD","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2226316.06,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",46382713.039999999,"","",1.33,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","10","","C204626","C204626A-RW","1","ALAMANCE","FSC II LLC DBA FRED SMITH COMPANY",3233469.69,"RW1","",25.568000000000001,6,"R000",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204626B-RW","1","GUILFORD","FSC II LLC DBA FRED SMITH COMPANY",116872.42,"RW1","",0.23,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204626C-RW","1","ALAMANCE","FSC II LLC DBA FRED SMITH COMPANY",1289228.26,"RW1","",3.2090000000000001,6,"R000",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",4639570.37,"","",29.007000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","11","U-2579BA","C204533","C204533-EC","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",2561326.21,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204533-RW","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",5609645.6100000003,"RW1","I000",0.97499999999999998,6,"M720",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204533-SI","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",45046.5,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204533-ST","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",341314,"CV01","Y007",null,5.5,"C203",35.58,8,"","",null,null,null,"PDMT","9","(45+66.21 -Y4-)"]
[null,"","","","","C204533-TC","1","FORSYTH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",876589.98,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",9433922.3000000007,"","",0.97499999999999998,null,null,null,null,"","",null,null,null,"","",""]
[null,"","14","BR-0011","C204387","C204387-EC","1","CHEROKEE","SUMMERS TAYLOR INC",122895.5,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204387-RW","1","CHEROKEE","SUMMERS TAYLOR INC",834223.6,"RW1","",0.21,2,"B812",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204387-SI","1","CHEROKEE","SUMMERS TAYLOR INC",10650.25,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204387-ST","1","CHEROKEE","SUMMERS TAYLOR INC",737255.3,"BR01","X080",1.4E-2,null,"15",null,42,"722","A",1,39.833300000000001,72.604200000000006,"VERY MTN","14","(15+45.00 -L-)"]
[null,"","","","","C204387-TC","1","CHEROKEE","SUMMERS TAYLOR INC",35601.4,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204387-UT","1","CHEROKEE","SUMMERS TAYLOR INC",101286.5,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",1841912.55,"","",0.224,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","15","","C204611","C204611-RW","1","ALLEGHANY","DANE CONSTRUCTION INC",4113382.5,"RW1","",0.28799999999999998,2,"M720",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","","","","Result",4113382.5,"","",0.28799999999999998,null,"",null,null,"","",null,null,null,"","",""]
[null,"5/18/2021","1","B-5619","C204475","C204475-EC","1","LENOIR","W C ENGLISH INCORPORATED",199157.85,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204475-RW","1","LENOIR","W C ENGLISH INCORPORATED",2459097.4,"RW1","I000",4.4160000000000004,2,"B810",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204475-SI","1","LENOIR","W C ENGLISH INCORPORATED",21279,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204475-ST","1","LENOIR","W C ENGLISH INCORPORATED",3700416.95,"BR01","X081",8.6999999999999994E-2,null,"15",null,38.25,"100","Q",5,35,461.58330000000001,"COAST","2","(30+80.00-L-)"]
[null,"","","","","","2","LENOIR","W C ENGLISH INCORPORATED",1453614.57,"BR02","X080",4.1000000000000002E-2,null,"15",null,39,"722","E",4,39,212.625,"COAST","2","(23+06.50-L-)"]
[null,"","","","","C204475-TC","1","LENOIR","W C ENGLISH INCORPORATED",140528.29999999999,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",7974094.0700000003,"","",4.5439999999999996,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","2","B-5626","C204476","C204476-EC","1","ONSLOW","CIVIL WORKS CONTRACTING LLC",55737.7,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204476-RW","1","ONSLOW","CIVIL WORKS CONTRACTING LLC",492741.99,"RW1","",0.154,2,"B810",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204476-ST","1","ONSLOW","CIVIL WORKS CONTRACTING LLC",747626.65,"BR01","X080",2.5999999999999999E-2,null,"15",null,36,"721","A",3,33,137.5,"COAST","3","(23+71.50 -L-)"]
[null,"","","","","C204476-TC","1","ONSLOW","CIVIL WORKS CONTRACTING LLC",35901.550000000003,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204476-UT","1","ONSLOW","CIVIL WORKS CONTRACTING LLC",158624.75,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",1490632.64,"","",0.18,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","3","B-4931","C204518","C204518A-EC","1","EDGECOMBE","SANFORD CONTRACTORS INC",82905,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204518A-RW","1","EDGECOMBE","SANFORD CONTRACTORS INC",405676.2,"RW1","",0.14000000000000001,2,"B810",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204518A-SI","1","EDGECOMBE","SANFORD CONTRACTORS INC",7198.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204518A-ST","1","EDGECOMBE","SANFORD CONTRACTORS INC",1131746.3,"BR01","X081",3.2000000000000001E-2,null,"15",null,35.25,"854","A",2,33.333300000000001,170,"PDMT","4","(16+99.00-L-)"]
[null,"","","","","C204518A-TC","1","EDGECOMBE","SANFORD CONTRACTORS INC",6545,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204518A-UT","1","EDGECOMBE","SANFORD CONTRACTORS INC",217229,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",1851300,"","",0.17199999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","4","","C204625","C204625A-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",845408.47,"RW1","",2.8,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204625B-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",2206781.35,"RW1","",11.57,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204625C-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",1062796.48,"RW1","",4.7530000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",4114986.3,"","",19.123000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204637","C204637A-RW","1","FRANKLIN","S T WOOTEN CORPORATION",3399465.75,"RW1","",27.417999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204637B-RW","1","GRANVILLE","S T WOOTEN CORPORATION",14834.22,"RW1","",5.1999999999999998E-2,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204637C-RW","1","WARREN","S T WOOTEN CORPORATION",25395.03,"RW1","",0.22500000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",3439695,"","",27.695,null,"",null,null,"","",null,null,null,"","",""]
[null,"","6","","C204636","C204636-RW","1","WAKE","S T WOOTEN CORPORATION",3266005,"RW1","",23.29,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",3266005,"","",23.29,null,"",null,null,"","",null,null,null,"","",""]
[null,"","7","","C204635","C204635A-RW","1","CASWELL","ADAMS CONSTRUCTION COMPANY",1563473.44,"RW1","",12.942,4,"R000",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204635B-RW","1","CASWELL","ADAMS CONSTRUCTION COMPANY",2292173.35,"RW1","",24.216000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",3855646.79,"","",37.158000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","8","","C204634","C204634A-RW","1","SCOTLAND","BARNHILL CONTRACTING CO",280614.34000000003,"RW1","",4.08,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204634B-RW","1","HOKE","BARNHILL CONTRACTING CO",440108.21,"RW1","",3.581,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204634C-RW","1","SCOTLAND","BARNHILL CONTRACTING CO",210464.04,"RW1","",2,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",931186.59,"","",9.6609999999999996,null,"",null,null,"","",null,null,null,"","",""]
[null,"","9","B-4407","C204469","C204469-EC","1","ANSON","REEVES CONSTRUCTION COMPANY",106706.2,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204469-RW","1","ANSON","REEVES CONSTRUCTION COMPANY",1904861.5,"RW1","I000",0.54800000000000004,2,"B801",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204469-SI","1","ANSON","REEVES CONSTRUCTION COMPANY",31459.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204469-ST","1","ANSON","REEVES CONSTRUCTION COMPANY",3105246.36,"BR01","X081",9.9000000000000005E-2,null,"15",null,37.083300000000001,"854","Q",5,33.833300000000001,525,"PDMT","10","(32+31.61-L-)"]
[null,"","","","","C204469-TC","1","ANSON","REEVES CONSTRUCTION COMPANY",143476,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",5291749.8099999996,"","",0.64700000000000002,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","10","B-5818","C204555","C204555-EC","1","ANSON","SMITH-ROWE, LLC",44891.25,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204555-RW","1","ANSON","SMITH-ROWE, LLC",1583848.3,"RW1","",0.46700000000000003,2,"B801",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204555-ST","1","ANSON","SMITH-ROWE, LLC",726496.55,"BR01","X081",2.5000000000000001E-2,null,"15",null,35.25,"772","A",1,32,130,"PDMT","10","27+79.00 -L-"]
[null,"","","","","C204555-TC","1","ANSON","SMITH-ROWE, LLC",50660,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204555-UT","1","ANSON","SMITH-ROWE, LLC",532794.98,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",2938691.08,"","",0.49199999999999999,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","11","U-5887","C204631","C204631-EC","1","HENDERSON","BUCHANAN AND SONS INC",417968,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204631-RW","1","HENDERSON","BUCHANAN AND SONS INC",3354668.85,"RW1","",1.0580000000000001,4,"D340",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204631-SG","1","HENDERSON","BUCHANAN AND SONS INC",162713,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204631-SI","1","HENDERSON","BUCHANAN AND SONS INC",67946.899999999994,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204631-ST","1","HENDERSON","BUCHANAN AND SONS INC",800705,"CV01","Y007",6.0000000000000001E-3,4.83,"C005",54,28,"","",null,null,null,"VERY MTN","14","(22+44.41 -L-)"]
[null,"","","","","","2","HENDERSON","BUCHANAN AND SONS INC",384664,"WL1","Y007",null,null,"W001",5,null,"","",null,null,null,"VERY MTN","14","(11+25.00 -L-)"]
[null,"","","","","C204631-TC","1","HENDERSON","BUCHANAN AND SONS INC",134638.5,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204631-UT","1","HENDERSON","BUCHANAN AND SONS INC",1350678.2,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",6673982.4500000002,"","",1.0640000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","12","B-6015","C204407","C204407-RW","1","BUNCOMBE","MOUNTAIN CREEK CONTRACTORS INC",1517675,"RW1","I000",7.5999999999999998E-2,2,"M720",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","","","Result",1517675,"","",7.5999999999999998E-2,null,"",null,null,"","",null,null,null,"","",""]
[null,"6/15/2021","1","U-5942","C204648","C204154-SG","1","PASQUOTANK","ALS OF NORTH CAROLINA LLC",4399018,"RW1","Y033",20,2,"M705",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","","","","Result",4399018,"","",20,null,"",null,null,"","",null,null,null,"","",""]
[null,"","2","I-5905","C204647","C204365-RW","1","MECKLENBURG","BOGGS CONTRACTING INC",15126678.41,"RW1","I000",6.08,8,"RH12",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204365-ST","1","MECKLENBURG","BOGGS CONTRACTING INC",168064.5,"BR01","X251",null,null,"11",null,41.082999999999998,"574","I",2,38,354.16699999999997,"PDMT","10",""]
[null,"","","","","","","","Result",15294742.91,"","",6.08,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","3","","C204646","C204622A-RW","1","MECKLENBURG","BOGGS CONTRACTING INC",2724083.26,"RW1","",9.7889999999999997,4,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204622B-RW","1","MECKLENBURG","BOGGS CONTRACTING INC",4015223.39,"RW1","",11.677,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",6739306.6500000004,"","",21.466000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","4","BR-0017","C204620","C204620-EC","1","DUPLIN","UNITED CONTRACTORS INC DBA UNITED CONTRA",83820.5,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204620-RW","1","DUPLIN","UNITED CONTRACTORS INC DBA UNITED CONTRA",718683.5,"RW1","",0.122,2,"B810",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204620-SI","1","DUPLIN","UNITED CONTRACTORS INC DBA UNITED CONTRA",11358.8,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204620-ST","1","DUPLIN","UNITED CONTRACTORS INC DBA UNITED CONTRA",1121795.1100000001,"BR01","X081",0.03,null,"15",null,42.25,"845","E",2,39,160,"PDMT","3","(18+27.00-L-)"]
[null,"","","","","C204620-TC","1","DUPLIN","UNITED CONTRACTORS INC DBA UNITED CONTRA",26601.9,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","C204620-UT","1","DUPLIN","UNITED CONTRACTORS INC DBA UNITED CONTRA",417524.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","3",""]
[null,"","","","","","","","Result",2379784.31,"","",0.152,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","5","B-5980","C204350","C204350-EC","1","NASH","BARNHILL CONTRACTING CO",571270.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350-LI","1","NASH","BARNHILL CONTRACTING CO",536267.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350-RW","1","NASH","BARNHILL CONTRACTING CO",10660902.789999999,"RW1","I000",0.69,4,"B801",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350-SG","1","NASH","BARNHILL CONTRACTING CO",90036,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350-SI","1","NASH","BARNHILL CONTRACTING CO",83763,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350-ST","1","NASH","BARNHILL CONTRACTING CO",1804649.45,"BR01","X231",null,null,"11",null,49.25,"864","D",2,46,232,"PDMT","4","(42+56.82 -Y1-)"]
[null,"","","","","C204350-TC","1","NASH","BARNHILL CONTRACTING CO",485796.02,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350-UT","2","NASH","BARNHILL CONTRACTING CO",60103.3,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",14292788.560000001,"","",0.69,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","","BR-0036","C204350","C204350B-EC","1","NASH","BARNHILL CONTRACTING CO",122436.5,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350B-RW","1","NASH","BARNHILL CONTRACTING CO",1987731.99,"0","",0.20699999999999999,2,"B810",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350B-SI","1","NASH","BARNHILL CONTRACTING CO",33115.199999999997,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350B-ST","1","NASH","BARNHILL CONTRACTING CO",2113412.33,"BR01","X231",4.2999999999999997E-2,null,"11",null,43.25,"642","D",2,40,226,"PDMT","4","(19+07.12 -L-)"]
[null,"","","","","C204350B-TC","1","NASH","BARNHILL CONTRACTING CO",158945.63,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",4415641.6500000004,"","",0.25,8,"",null,null,null,null,null,null,null,"","",""]
[null,"","","BR-0039","C204350","C204350C-EC","1","NASH","BARNHILL CONTRACTING CO",252121,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350C-RW","1","NASH","BARNHILL CONTRACTING CO",1669538.5,"0","",0.29199999999999998,2,"B810",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204350C-ST","1","NASH","BARNHILL CONTRACTING CO",2158121.3199999998,"BR01","X231",0.05,null,"11",null,37.25,"648","D",2,34,266,"PDMT","4","(28+02.81 -L-)"]
[null,"","","","","C204350C-TC","1","NASH","BARNHILL CONTRACTING CO",224342.75,"0","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",4304123.57,"","",0.34200000000000003,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","6","","C204643","C204643A-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",758230.25,"RW1","",1.6,5,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204643B-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",3479830.35,"RW1","",20.814,6,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",4238060.5999999996,"","",22.414000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","7","","C204640","C204640-RW","1","LEE","S T WOOTEN CORPORATION",1323015,"RW1","",6.87,4,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",1323015,"","",6.87,null,"",null,null,"","",null,null,null,"","",""]
[null,"","8","","C204641","C204641-RW","1","MOORE","FSC II LLC DBA FRED SMITH COMPANY",1414948.11,"RW1","",9.4600000000000009,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",1414948.11,"","",9.4600000000000009,null,"",null,null,"","",null,null,null,"","",""]
[null,"","9","","C204642","C204642-RW","1","RANDOLPH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",1536564.79,"RW1","",10.84,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",1536564.79,"","",10.84,null,"",null,null,"","",null,null,null,"","",""]
[null,"","10","","C204644","C204644A-RW","1","RICHMOND","BARNHILL CONTRACTING CO",4849407.5199999996,"RW1","",11.44,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204644B-RW","1","RICHMOND","BARNHILL CONTRACTING CO",650467.41,"RW1","",5.3239999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",5499874.9299999997,"","",16.763999999999999,null,"",null,null,"","",null,null,null,"","",""]
[null,"7/20/2021","1","B-4863","C204372","C204372-ST","1","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",5916354,"BR01","X081",null,null,"15",null,34.583300000000001,"800","I",28,32,3200,"COAST","2","(34+75.00-L-)"]
[null,"","","","","C204372B-EC","1","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",478097.25,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204372B-RW","1","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",5296208.74,"RW1","",0.247,2,"B801",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204372B-SI","1","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",52580.5,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204372B-ST","1","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",2950166,"WL1","Y007",null,null,"W001",13.12,null,"","",null,null,null,"COAST","2","(10+00.00-RETWL1-)"]
[null,"","","","","","2","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",918854,"WL2","Y007",null,null,"W001",9.4,null,"","",null,null,null,"COAST","2","(10+00.00-RETWL2-)"]
[null,"","","","","","3","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",43907827.789999999,"BR01","X081",0.60599999999999998,null,"15",null,34.583300000000001,"800","I",28,32,3200,"COAST","2","(34+75.00-L-)"]
[null,"","","","","","4","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",330030,"BR02","X081",null,null,"15",null,30,"721","A",13,26.25,587,"COAST","2","BRIDGE NO. 150096"]
[null,"","","","","C204372B-TC","1","CARTERET","BALFOUR BEATTY INFRASTRUCTURE INC",145627.68,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",59995745.960000001,"","",0.85299999999999998,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","2","I-5986B","C204543","C204543A-EC","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",8233206.75,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","C204543A-LI","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",2578907.2999999998,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","C204543A-RW","1","JOHNSTON","FLATIRON FRED SMITH COMPANY JV",164939707.41999999,"RW1","",8.7799999999999994,8,"D313",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","C204543A-SG","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",1938770.1,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","C204543A-SI","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",3321309.6,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","C204543A-ST","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",166649.5,"CV01","Y007",null,7.56,"C001",85.08,8,"","",null,null,null,"PDMT","6","(15+47.41-NBCD-)"]
[null,"","","","","","2","HARNETT","FLATIRON FRED SMITH COMPANY JV",957636,"CV02","Y007",6.0000000000000001E-3,8.89,"C003",222,8,"","",null,null,null,"PDMT","6","(1042+08.93-L-)"]
[null,"","","","","","3","HARNETT","FLATIRON FRED SMITH COMPANY JV",698645,"CV03","Y007",null,5.46,"C002",263.75,7,"","",null,null,null,"PDMT","6","(1220+34.00-L-)"]
[null,"","","","","","4","HARNETT","FLATIRON FRED SMITH COMPANY JV",189264,"CV04","Y007",null,4.72,"C002",60.33,6,"","",null,null,null,"PDMT","6","(35+91.00-Y33-)"]
[null,"","","","","","5","HARNETT","FLATIRON FRED SMITH COMPANY JV",592982,"WL1","Y007",null,null,"W001",13.6,null,"","",null,null,null,"PDMT","6","(971+41.06-L-)"]
[null,"","","","","","6","HARNETT","FLATIRON FRED SMITH COMPANY JV",317199.59999999998,"WL2","Y007",null,null,"W001",15.72,null,"","",null,null,null,"PDMT","6","(971+41.06-L-)"]
[null,"","","","","","7","HARNETT","FLATIRON FRED SMITH COMPANY JV",421649.4,"WL3","Y007",null,null,"W001",17.96,null,"","",null,null,null,"PDMT","6","(1002+79.68-LREV-)"]
[null,"","","","","","8","HARNETT","FLATIRON FRED SMITH COMPANY JV",368009.8,"WL4","Y007",null,null,"W001",15.93,null,"","",null,null,null,"PDMT","6","(1002+79.68-LREV-)"]
[null,"","","","","","9","HARNETT","FLATIRON FRED SMITH COMPANY JV",278932,"WL5","Y007",null,null,"W001",11.34,null,"","",null,null,null,"PDMT","6","(10+00.00-WL3-)"]
[null,"","","","","","10","HARNETT","FLATIRON FRED SMITH COMPANY JV",29260.799999999999,"WL6","Y007",null,null,"W005",2.99,null,"","",null,null,null,"PDMT","6","(10+00.00-WL4-)"]
[null,"","","","","","11","HARNETT","FLATIRON FRED SMITH COMPANY JV",74419.199999999997,"WL7","Y007",null,null,"W005",2.99,null,"","",null,null,null,"PDMT","6","(10+00.00-WL5-)"]
[null,"","","","","","12","HARNETT","FLATIRON FRED SMITH COMPANY JV",150879,"WL8","Y007",null,null,"W001",15,null,"","",null,null,null,"PDMT","6","(10+00.00-WL6-)"]
[null,"","","","","","13","HARNETT","FLATIRON FRED SMITH COMPANY JV",66891,"WL9","Y007",null,null,"W005",3.72,null,"","",null,null,null,"PDMT","6","(10+00.00-WL8-)"]
[null,"","","","","","14","HARNETT","FLATIRON FRED SMITH COMPANY JV",772500,"WL10","Y007",null,null,"W001",15,null,"","",null,null,null,"PDMT","6","(10+00.00-WL7-)"]
[null,"","","","","","15","HARNETT","FLATIRON FRED SMITH COMPANY JV",276058,"WL11","Y007",null,null,"W001",14.32,null,"","",null,null,null,"PDMT","6","(1101+61.98-L-)"]
[null,"","","","","","16","HARNETT","FLATIRON FRED SMITH COMPANY JV",247076,"WL12","Y007",null,null,"W001",13.01,null,"","",null,null,null,"PDMT","6","(1101+61.98-L-)"]
[null,"","","","","","17","HARNETT","FLATIRON FRED SMITH COMPANY JV",260876,"WL13","Y007",null,null,"W001",11.69,null,"","",null,null,null,"PDMT","6","(1206+59.51-L-)"]
[null,"","","","","","18","HARNETT","FLATIRON FRED SMITH COMPANY JV",271961,"WL14","Y007",null,null,"W001",12.24,null,"","",null,null,null,"PDMT","6","(1206+59.51-L-)"]
[null,"","","","","","19","HARNETT","FLATIRON FRED SMITH COMPANY JV",211033,"WL15","Y007",null,null,"W001",13.75,null,"","",null,null,null,"PDMT","6","(28+39.21-Y29-)"]
[null,"","","","","","20","HARNETT","FLATIRON FRED SMITH COMPANY JV",205661.2,"WL16","Y007",null,null,"W001",14.24,null,"","",null,null,null,"PDMT","6","(28+39.21-Y29-)"]
[null,"","","","","","21","HARNETT","FLATIRON FRED SMITH COMPANY JV",30597.599999999999,"WL17","Y007",null,null,"W001",3.44,null,"","",null,null,null,"PDMT","6","(10+00.00-W9-)"]
[null,"","","","","","22","HARNETT","FLATIRON FRED SMITH COMPANY JV",203760,"WL18","Y007",null,null,"W001",12.4,null,"","",null,null,null,"PDMT","6","(10+00.00-NW29-1-)"]
[null,"","","","","","24","HARNETT","FLATIRON FRED SMITH COMPANY JV",369900,"WL20","Y007",null,null,"W001",15.14,null,"","",null,null,null,"PDMT","6","(10+00.00-NW32-1-)"]
[null,"","","","","","25","HARNETT","FLATIRON FRED SMITH COMPANY JV",792540,"WL21","Y007",null,null,"W001",12.83,null,"","",null,null,null,"PDMT","6","(10+00.00-NW33-1-)"]
[null,"","","","","","26","HARNETT","FLATIRON FRED SMITH COMPANY JV",2148270.6,"BR01","X281",null,null,"11",null,45.583300000000001,"863","I",2,32,227,"PDMT","6","(26+05.28-Y14-)"]
[null,"","","","","","27","HARNETT","FLATIRON FRED SMITH COMPANY JV",2962008.87,"BR02","X281",0.02,null,"11",null,149.25,"100","A",1,146,104.75,"PDMT","6","(1002+79.68-LREV-)"]
[null,"","","","","","28","HARNETT","FLATIRON FRED SMITH COMPANY JV",2178930.67,"BR03","X281",null,null,"11",null,51.25,"854","I",2,48,189.5,"PDMT","6","(27+09.19-Y16-)"]
[null,"","","","","","29","HARNETT","FLATIRON FRED SMITH COMPANY JV",2299476.8199999998,"BR04","X281",null,null,"11",null,51.25,"863","I",2,48,213.5,"PDMT","6","(26+80.73-Y17-)"]
[null,"","","","","","30","HARNETT","FLATIRON FRED SMITH COMPANY JV",6576815.9199999999,"BR05","X281",4.7E-2,null,"11",null,148.25,"100","I",3,146,245.83330000000001,"PDMT","6","(1260+34.00-L-)"]
[null,"","","","","","31","HARNETT","FLATIRON FRED SMITH COMPANY JV",1171948.04,"BR06","X281",null,null,"11",null,33.25,"854","I",2,30,197.5,"PDMT","6","(28+39.21-Y29-)"]
[null,"","","","","","32","HARNETT","FLATIRON FRED SMITH COMPANY JV",3794684.76,"BR07","X281",0.02,null,"11",null,149.25,"100","A",1,146,105.91670000000001,"PDMT","6","(1391+19.65-L-)"]
[null,"","","","","","33","HARNETT","FLATIRON FRED SMITH COMPANY JV",853103.25,"BR08","X231",null,null,"11",null,75.458299999999994,"672","I",2,63,228.96879999999999,"PDMT","6","(25+31.59-Y18-)"]
[null,"","","","","C204543A-TC","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",16086867.66,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","C204543A-UT","1","HARNETT","FLATIRON FRED SMITH COMPANY JV",9270287.4000000004,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","","2","HARNETT","FLATIRON FRED SMITH COMPANY JV",151418.5,"RW1","",null,8,"",null,null,"","",null,null,null,"PDMT","6",""]
[null,"","","","","","","","Result",236460093.75999999,"","",8.8729999999999993,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","3","","C204519","C204519A-EC","1","NORTHAMPTON","DELLINGER INC",47520,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","1",""]
[null,"","","","","C204519A-RW","1","NORTHAMPTON","DELLINGER INC",352022,"RW1","",0.154,2,"B810",null,null,"","",null,null,null,"PDMT","1",""]
[null,"","","","","C204519A-SI","1","NORTHAMPTON","DELLINGER INC",8257.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","1",""]
[null,"","","","","C204519A-ST","1","NORTHAMPTON","DELLINGER INC",678878,"BR01","X080",0.02,null,"15",null,33,"721","A",2,30.833300000000001,107.39700000000001,"PDMT","1","(15+50.00-L-)"]
[null,"","","","","C204519A-TC","1","NORTHAMPTON","DELLINGER INC",5251.95,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","1",""]
[null,"","","","","C204519A-UT","1","NORTHAMPTON","DELLINGER INC",780,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","1",""]
[null,"","","","","","","","Result",1092709.45,"","",0.17399999999999999,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","4","","C204331","C204331-ST","1","NEW HANOVER","COASTAL GUNITE CONSTRUCTION COMPANY",3185192.15,"BR01","X081",0.16,null,"15",null,57.958300000000001,"845","E",14,47.833300000000001,869.25,"COAST","3","BRIDGE NO. 640021"]
[null,"","","","","C204331-TC","1","NEW HANOVER","COASTAL GUNITE CONSTRUCTION COMPANY",549919.21,"RW1","",5.0000000000000001E-3,4,"RH10",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",3735111.36,"","",0.16500000000000001,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","6","B-5666","C204536","C204536-EC","1","WILSON","W C ENGLISH INCORPORATED",170537.75,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204536-RW","1","WILSON","W C ENGLISH INCORPORATED",1812352.2,"RW1","",0.254,2,"B810",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204536-SI","1","WILSON","W C ENGLISH INCORPORATED",10307.58,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204536-ST","1","WILSON","W C ENGLISH INCORPORATED",1863837.16,"BR01","X181",3.5999999999999997E-2,null,"12",null,37.25,"854","E",3,34,190.5,"PDMT","4","(17+37.36-L-)"]
[null,"","","","","C204536-TC","1","WILSON","W C ENGLISH INCORPORATED",7854,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204536-UT","1","WILSON","W C ENGLISH INCORPORATED",20817.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",3885706.19,"","",0.28999999999999998,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","7","","C204550","C204550-EC","1","WILKES","SMITH-ROWE, LLC",28172.3,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204550-RW","1","WILKES","SMITH-ROWE, LLC",302086.40000000002,"RW1","",4.2999999999999997E-2,2,"B810",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204550-SI","1","WILKES","SMITH-ROWE, LLC",4004,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204550-ST","1","WILKES","SMITH-ROWE, LLC",302421.78999999998,"BR01","X080",1.4E-2,null,"15",null,30,"722","A",1,27.833300000000001,71.9375,"MTN","11","(15+23.00-L-)"]
[null,"","","","","C204550-TC","1","WILKES","SMITH-ROWE, LLC",3799,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","","","","Result",640483.49,"","",5.7000000000000002E-2,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","8","BR-0108","C204628","C204537-EC","1","WILKES","SMITH-ROWE, LLC",36978.75,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204537-RW","1","WILKES","SMITH-ROWE, LLC",315344.84999999998,"RW1","",8.3000000000000004E-2,2,"B810",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204537-SI","1","WILKES","SMITH-ROWE, LLC",6857.73,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","C204537-ST","1","WILKES","SMITH-ROWE, LLC",305297.36,"BR01","X080",1.4E-2,null,"15",null,30,"722","A",1,27.833300000000001,72.25,"MTN","11","(18+28.00-L-)"]
[null,"","","","","C204537-TC","1","WILKES","SMITH-ROWE, LLC",3238,"RW1","",null,2,"",null,null,"","",null,null,null,"MTN","11",""]
[null,"","","","","","","","Result",667716.68999999994,"","",9.7000000000000003E-2,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","9","BR-0107","C204627","C204516C-EC","1","IREDELL","SMITH-ROWE, LLC",21357.5,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
[null,"","","","","C204516C-RW","1","IREDELL","SMITH-ROWE, LLC",248460.35,"RW1","",7.9000000000000001E-2,2,"B810",null,null,"","",null,null,null,"PDMT","12",""]
[null,"","","","","C204516C-SI","1","IREDELL","SMITH-ROWE, LLC",6379.8,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
[null,"","","","","C204516C-ST","1","IREDELL","SMITH-ROWE, LLC",276318.78999999998,"BR01","X080",1.2999999999999999E-2,null,"15",null,30,"722","A",1,30,27.833300000000001,"PDMT","12","(17+68.00 -L-)"]
[null,"","","","","C204516C-TC","1","IREDELL","SMITH-ROWE, LLC",1732,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","12",""]
[null,"","","","","","","","Result",554248.43999999994,"","",9.1999999999999998E-2,null,"",null,null,null,null,null,null,null,"","",""]
[null,"8/17/2021","1","R-5020B","C204649","C204423-EC","1","COLUMBUS","HIGHLAND PAVING CO LLC",828135,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204423-RW","1","COLUMBUS","HIGHLAND PAVING CO LLC",20789190.899999999,"RW1","",2.1829999999999998,4,"D351",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204423-SG","1","COLUMBUS","HIGHLAND PAVING CO LLC",1237376.8500000001,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204423-SI","1","COLUMBUS","HIGHLAND PAVING CO LLC",199100.85,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204423-ST","1","COLUMBUS","HIGHLAND PAVING CO LLC",103476.3,"CV01","Y007",null,8.6,"C201",83.75,6,"","",null,null,null,"COAST","6","(172+34.91-L-)"]
[null,"","","","","","2","COLUMBUS","HIGHLAND PAVING CO LLC",17600,"WL1","Y007",null,null,"W001",6.98,null,"","",null,null,null,"COAST","6","(10+00.00-W1-)"]
[null,"","","","","","3","COLUMBUS","HIGHLAND PAVING CO LLC",92400,"WL2","Y007",null,null,"W001",6.28,null,"","",null,null,null,"COAST","6","(10+00.00-W2-)"]
[null,"","","","","C204423-TC","1","COLUMBUS","HIGHLAND PAVING CO LLC",963648.13,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204423-UT","1","COLUMBUS","HIGHLAND PAVING CO LLC",4018320,"RW1","",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",28249248.030000001,"","",2.1829999999999998,null,"",null,null,"","",null,null,null,"","",""]
[null,"","2","I-6048","C204441","C204441-RW","1","WAYNE","S T WOOTEN CORPORATION",5291972.3,"RW1","I000",14.74,4,"R000",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204441-SI","1","WAYNE","S T WOOTEN CORPORATION",455082.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204441-TC","1","WAYNE","S T WOOTEN CORPORATION",245953.41,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",5993008.21,"","",14.74,null,"",null,null,"","",null,null,null,"","",""]
[null,"","3","B-5703","C204430","C204430-EC","1","CUMBERLAND","SMITH-ROWE, LLC",59431.9,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204430-RW","1","CUMBERLAND","SMITH-ROWE, LLC",510532.19,"RW1","",0.13900000000000001,2,"B810",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204430-SI","1","CUMBERLAND","SMITH-ROWE, LLC",10720.8,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204430-ST","1","CUMBERLAND","SMITH-ROWE, LLC",1308248.06,"BR01","X281",3.6999999999999998E-2,null,"15",null,35.25,"854","E",3,32,197,"COAST","6","(16+92.70-L-)"]
[null,"","","","","C204430-TC","1","CUMBERLAND","SMITH-ROWE, LLC",8355,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204430-UT","1","CUMBERLAND","SMITH-ROWE, LLC",414695.33,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",2311983.2799999998,"","",0.17599999999999999,null,"",null,35.25,"","",3,32,197,"","",""]
[null,"","4","I-3306A","C204632","C204632-RW","1","ORANGE","THE LANE CONSTRUCTION CORPORATION",236457869,"RW1","I000",13,6,"M713",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",236457869,"","",13,null,"",null,null,"","",null,null,null,"","",""]
[null,"9/21/2021","1","U-4906","C203649","C203649-EC","1","ONSLOW","BARNHILL CONTRACTING CO",1376512.75,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C203649-RW","1","ONSLOW","BARNHILL CONTRACTING CO",8805185.5999999996,"RW1","I000",6.6050000000000004,2,"D300",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C203649-SG","1","ONSLOW","BARNHILL CONTRACTING CO",470629.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C203649-SI","1","ONSLOW","BARNHILL CONTRACTING CO",273615,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C203649-TC","1","ONSLOW","BARNHILL CONTRACTING CO",371065.9,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C203649-UT","1","ONSLOW","BARNHILL CONTRACTING CO",1839517.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","2","ONSLOW","BARNHILL CONTRACTING CO",728439,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",13864965.25,"","",6.6050000000000004,null,"",null,null,"","",null,null,null,"","",""]
[null,"","2","I-5932A","C204366","C204366-RW","1","HALIFAX","FSC II LLC DBA ROSE BROTHERS PAVING COMP",6331962.6100000003,"RW1","I000",7.1,4,"RH10",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",6331962.6100000003,"","",7.1,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","I-5932B","C204366","C204652-RW","1","HALIFAX","FSC II LLC DBA ROSE BROTHERS PAVING COMP",6243037.3899999997,"RW1","I000",6.7,4,"RH10",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",6243037.3899999997,"","",6.7,null,"",null,null,"","",null,null,null,"","",""]
[null,"","3","I-5936","C204653","C204653-EC","1","WILSON","S T WOOTEN CORPORATION",7767.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204653-RW","1","WILSON","S T WOOTEN CORPORATION",1883810,"RW1","I000",6.19,4,"RH10",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204653-SG","1","WILSON","S T WOOTEN CORPORATION",125500,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204653-SI","1","WILSON","S T WOOTEN CORPORATION",185326,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204653-TC","1","WILSON","S T WOOTEN CORPORATION",292022.69,"RW1","I000",null,4,"",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","C204653B-RW","1","JOHNSTON","S T WOOTEN CORPORATION",377822,"RW1","",0.4,4,"RH10",null,null,"","",null,null,null,"PDMT","4",""]
[null,"","","","","","","","Result",2872248.19,"","",6.59,null,"",null,null,"","",null,null,null,"","",""]
[null,"","4","","C204662","C204662-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",1825812,"RW1","",1.714,5,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",1825812,"","",1.714,null,"",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204663","C204663-RW","1","WAKE","FSC II LLC DBA FRED SMITH COMPANY",2444169.2599999998,"RW1","",8.5399999999999991,5,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2444169.2599999998,"","",8.5399999999999991,null,"",null,null,"","",null,null,null,"","",""]
[null,"","6","","C204664","C204664A-RW","1","PERSON","CAROLINA SUNROCK LLC",564638.77,"RW1","",3.24,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204664B-RW","1","PERSON","CAROLINA SUNROCK LLC",3333878.82,"RW1","",17.077999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",3898517.59,"","",20.318000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","7","R-5709A","C204661","C204661-EC","1","HOKE","FSC II LLC DBA FRED SMITH COMPANY",6650025.0999999996,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204661-RW","1","HOKE","FSC II LLC DBA FRED SMITH COMPANY",7854335,"RW1","",15.606999999999999,2,"M720",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204661-SI","1","HOKE","FSC II LLC DBA FRED SMITH COMPANY",21610,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204661-TC","1","HOKE","FSC II LLC DBA FRED SMITH COMPANY",800000,"RW1","",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",15325970.1,"","",15.606999999999999,null,"",null,null,"","",null,null,null,"","",""]
[null,"","8","I-6003","C204645","C204645-RW","1","DAVIE","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",6675172.7800000003,"RW1","I000",3.64,4,"RH10",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",6675172.7800000003,"","",3.64,null,"",null,null,"","",null,null,null,"","",""]
[null,"","10","I-5834A","C204651","C204651-RW","1","HAYWOOD","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",7744795.9199999999,"RW1","I000",3.02,4,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204651-SI","1","HAYWOOD","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",203178.5,"RW1","I000",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204651-TC","1","HAYWOOD","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",749484.6,"RW1","I000",null,4,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",8697459.0199999996,"","",3.02,null,"",null,null,"","",null,null,null,"","",""]
[null,"","11","I-6064A","C204596","C204596A-RW","1","ROBESON","FLATIRON UNITED",240488250,"RW1","K000",5.5,8,"M713",null,null,"","",null,null,null,"COAST","6","`"]
[null,"","","","","","","","Result",240488250,"","",5.5,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","I-6064B","C204596","C204596B-RW","1","ROBESON","FLATIRON UNITED",114376950,"RW1","",2.5,8,"M713",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",114376950,"","",2.5,null,"",null,null,"","",null,null,null,"","",""]
[null,"","","I-6064C","C204596","C204596C-RW","1","ROBESON","FLATIRON UNITED",77834800,"RW1","K000",null,8,"M713",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",77834800,"","",null,null,"",null,null,"","",null,null,null,"","",""]
[null,"10/4/2021","1","B-6054A","C204654","C204654-RW","1","HAYWOOD","KIEWIT INFRASTRUCTURE SOUTH CO",18945378.960000001,"RW1","",0.79,4,"M720",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",18945378.960000001,"","",0.79,null,"",null,null,"","",null,null,null,"","",""]
[null,"10/19/2021","2","","C204515","C204515D-EC","1","PITT","FSC II LLC DBA FRED SMITH COMPANY",22632.75,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515D-RW","1","PITT","FSC II LLC DBA FRED SMITH COMPANY",293036.90000000002,"RW1","",9.6000000000000002E-2,2,"B810",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515D-ST","1","PITT","FSC II LLC DBA FRED SMITH COMPANY",558581.56999999995,"BR01","X080",1.7000000000000001E-2,null,"15",null,33,"721","A",2,30,87.739599999999996,"COAST","2","(13+78.50-L-)"]
[null,"","","","","C204515D-TC","1","PITT","FSC II LLC DBA FRED SMITH COMPANY",2700,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","C204515D-UT","1","PITT","FSC II LLC DBA FRED SMITH COMPANY",73046,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","2",""]
[null,"","","","","","","","Result",949997.22,"","",0.113,null,"",null,null,null,null,null,null,null,"","",""]
[null,"","3","","C204666","C204666A-RW","1","FRANKLIN","CAROLINA SUNROCK LLC",193728.8,"RW1","",1.33,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204666B-RW","1","GRANVILLE","CAROLINA SUNROCK LLC",2372791.8199999998,"RW1","",15.528,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2566520.62,"","",16.858000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","4","","C204667","C204667A-RW","1","DURHAM","CAROLINA SUNROCK LLC",2062367.63,"RW1","",4.47,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204667B-RW","1","DURHAM","CAROLINA SUNROCK LLC",2987280.18,"RW1","",12.601000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",5049647.8099999996,"","",17.071000000000002,null,"",null,null,"","",null,null,null,"","",""]
[null,"","6","I-5939","C204639","C204639-RW","1","ROBESON","BARNHILL CONTRACTING CO",12109926.300000001,"RW1","I000",12.738,4,"RH10",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204639-SI","1","ROBESON","BARNHILL CONTRACTING CO",409053.86,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204639-ST","1","ROBESON","BARNHILL CONTRACTING CO",186500,"CV01","Y007",5.2999999999999999E-2,null,"C004",278,10,"","",null,null,null,"COAST","6","770089 (S5)"]
[null,"","","","","","2","ROBESON","BARNHILL CONTRACTING CO",28800,"CV02","Y007",7.6999999999999999E-2,null,"C002",405,10,"","",null,null,null,"COAST","6","770090 (S6)"]
[null,"","","","","","3","ROBESON","BARNHILL CONTRACTING CO",12000,"CV03","Y007",4.3999999999999997E-2,null,"C002",230.5,10,"","",null,null,null,"COAST","6","770098 (S8)"]
[null,"","","","","","4","ROBESON","BARNHILL CONTRACTING CO",1064497.1000000001,"BR01","X231",4.4999999999999998E-2,null,"11",null,42,"336","M",4,40,236,"COAST","6","770010 (S1)"]
[null,"","","","","","5","ROBESON","BARNHILL CONTRACTING CO",1214088.6000000001,"BR02","X231",null,null,"11",null,42,"336","M",4,40,236,"COAST","6","770012 (S2)"]
[null,"","","","","","6","ROBESON","BARNHILL CONTRACTING CO",163640.5,"BR03","X231",null,null,"11",null,70,"336","M",4,67.75,248.125,"COAST","6","770004 (S3)"]
[null,"","","","","","7","ROBESON","BARNHILL CONTRACTING CO",185556.5,"BR04","X231",null,null,"11",null,34,"400","M",4,32,269.52080000000001,"COAST","6","770086 (S4)"]
[null,"","","","","","8","ROBESON","BARNHILL CONTRACTING CO",88498,"BR05","X231",null,null,"11",null,34,"541","M",4,32,258.45310000000001,"COAST","6","770096 (S7)"]
[null,"","","","","","9","ROBESON","BARNHILL CONTRACTING CO",259611,"BR06","X231",null,null,"11",null,62,"642","M",4,60,294.375,"COAST","6","770104 (S9)"]
[null,"","","","","","10","ROBESON","BARNHILL CONTRACTING CO",74500,"BR07","X231",4.2999999999999997E-2,null,"11",null,42,"336","M",4,40,229.0052,"COAST","6","770106 (S10)"]
[null,"","","","","","11","ROBESON","BARNHILL CONTRACTING CO",59440,"BR08","X231",null,null,"11",null,42,"333","M",4,40,212.5104,"COAST","6","770107 (S11)"]
[null,"","","","","","12","ROBESON","BARNHILL CONTRACTING CO",161667,"BR09","X231",null,null,"11",null,38,"645","M",4,36,297.91669999999999,"COAST","6","770124 (S12)"]
[null,"","","","","","13","ROBESON","BARNHILL CONTRACTING CO",127907,"BR10","X230",null,null,"11",null,38,"652","M",2,36,241.60419999999999,"COAST","6","770130 (S13)"]
[null,"","","","","","14","ROBESON","BARNHILL CONTRACTING CO",326074,"BR11","X231",null,null,"11",null,38,"656","M",2,36,276.97919999999999,"COAST","6","770131 (S14)"]
[null,"","","","","C204639-TC","1","ROBESON","BARNHILL CONTRACTING CO",1079668.8999999999,"RW1","I000",null,4,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",17551428.760000002,"","",13,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","7","","C204303","C204303-ST","1","ROCKINGHAM","THE TRUESDELL CORPORATION",950903.4,"BR01","X081",9.8000000000000004E-2,null,"15",null,90.083299999999994,"754","Q",7,87,520,"PDMT","7","BRIDGE NO 780132"]
[null,"","","","","C204303-TC","1","ROCKINGHAM","THE TRUESDELL CORPORATION",230277.6,"RW1","",null,6,"RH11",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",1181181,"","",9.8000000000000004E-2,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","8","","C204668","C204668-RW","1","MOORE","FSC II LLC DBA FRED SMITH COMPANY",4178687.4,"RW1","",18.324999999999999,4,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",4178687.4,"","",18.324999999999999,4,"",null,null,"","",null,null,null,"","",""]
[null,"","9","","C204669","C204669-RW","1","RANDOLPH","APAC ATLANTIC INC THOMPSON ARTHUR DIVISI",3817411.02,"RW1","",21.44,4,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",3817411.02,"","",21.44,4,"",null,null,"","",null,null,null,"","",""]
[null,"","10","B-4626","C204446","C204446-EC","1","DAVIDSON","SMITH-ROWE, LLC",39645,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204446-RW","1","DAVIDSON","SMITH-ROWE, LLC",2173833.2000000002,"RW1","I000",0.92700000000000005,2,"B813",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204446-SI","1","DAVIDSON","SMITH-ROWE, LLC",73210,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204446-ST","1","DAVIDSON","SMITH-ROWE, LLC",10181974.890000001,"BR01","X531",0.20899999999999999,null,"14",null,39.25,"569","N",13,36,1101.9375,"PDMT","9","(45+22.65-EBL-)"]
[null,"","","","","","2","DAVIDSON","SMITH-ROWE, LLC",1221372.23,"BR02","X381",null,null,"17",null,34.583300000000001,"873","Q",12,31.5,1111.9583,"PDMT","9","BRIDGE NO. 780008"]
[null,"","","","","C204446-TC","1","DAVIDSON","SMITH-ROWE, LLC",87532.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",13777567.57,"","",1.1359999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","11","R-5737","C204399","C204399-EC","1","DAVIDSON","SMITH-ROWE, LLC",634391.9,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204399-LI","1","DAVIDSON","SMITH-ROWE, LLC",269730,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204399-RW","1","DAVIDSON","SMITH-ROWE, LLC",17279765.379999999,"RW1","",1.32,4,"I602",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204399-SI","1","DAVIDSON","SMITH-ROWE, LLC",244905,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204399-ST","1","DAVIDSON","SMITH-ROWE, LLC",1824508.35,"WL1","Y007",null,null,"W001",13.78,null,"","",null,null,null,"PDMT","9","(10+00.00 -RW2-)"]
[null,"","","","","","2","DAVIDSON","SMITH-ROWE, LLC",1068068.05,"WL2","Y007",null,null,"W001",10.89,null,"","",null,null,null,"PDMT","9","(10+00.00 -RW3-)"]
[null,"","","","","","3","DAVIDSON","SMITH-ROWE, LLC",353140.4,"WL3","Y007",null,null,"W001",6.29,null,"","",null,null,null,"PDMT","9","(10+00.00 -RW4-)"]
[null,"","","","","","4","DAVIDSON","SMITH-ROWE, LLC",1421260.69,"BR01","X281",4.2000000000000003E-2,null,"11",null,43.75,"863","Q",2,40.5,222.32400000000001,"PDMT","9","(61+02.86 -L- LT)"]
[null,"","","","","","5","DAVIDSON","SMITH-ROWE, LLC",1407400.39,"BR02","X281",null,null,"11",null,43.75,"863","Q",2,40.5,222.32400000000001,"PDMT","9","(61+02.86 -L- RT)"]
[null,"","","","","C204399-TC","1","DAVIDSON","SMITH-ROWE, LLC",971204.45,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204399-UT","1","DAVIDSON","SMITH-ROWE, LLC",418700.29,"RW1","",null,4,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",25893074.899999999,"","",1.3620000000000001,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","12","I-5746C","C204027","C204027-EC","1","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",76600,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204027-RW","1","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",6506444,"RW1","I000",0.91800000000000004,6,"M720",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204027-SG","1","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",4960,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204027-SI","1","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",86997,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204027-ST","1","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",174825.89,"BR01","X231",null,null,"11",null,45.5,"336","I",6,40,376.83330000000001,"PDMT","10","BRIDGE NO. 590044"]
[null,"","","","","","2","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",205819.64,"BR02","X231",null,null,"11",null,54.58,"336","I",6,40.167000000000002,400.5,"PDMT","10","BRIDGE NO. 590048"]
[null,"","","","","","3","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",581225.85,"BR03","X131",null,null,"12",null,62.08,"336","I",3,50,167.25,"PDMT","10","BRIDGE NO. 590138"]
[null,"","","","","","4","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",1332401.48,"BR04","X231",2.3E-2,null,"11",null,115.6887,"336","I",3,108.54,121.5,"PDMT","10","BRIDGE NO. 590320"]
[null,"","","","","","5","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",1110228.58,"BR05","X231",3.7999999999999999E-2,null,"11",null,113.63,"745","I",3,106,203,"PDMT","10","BRIDGE NO. 590322"]
[null,"","","","","","6","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",1104974.1599999999,"BR06","X231",2.5999999999999999E-2,null,"11",null,127.33,"336","I",3,121.83,138,"PDMT","10","BRIDGE NO. 590326"]
[null,"","","","","","7","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",1313650.06,"BR07","X231",3.5000000000000003E-2,null,"11",null,116,"336","I",3,110.83,186,"PDMT","10","BRIDGE NO. 590327"]
[null,"","","","","","8","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",739673.57,"BR08","X231",2.9000000000000001E-2,null,"11",null,109.167,"536","I",3,103.45,153,"PDMT","10","BRIDGE NO. 590328"]
[null,"","","","","","9","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",2096329.44,"BR09","X231",3.5999999999999997E-2,null,"11",null,131.874,"336","I",3,126.334,190,"PDMT","10","BRIDGE NO. 590330"]
[null,"","","","","","10","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",8565622.0800000001,"BR10","X231",0.22500000000000001,null,"11",null,62.083300000000001,"300","I",17,49.916600000000003,1189,"PDMT","10","BRIDGE NO. 590332"]
[null,"","","","","C204027-TC","1","MECKLENBURG","AMERICAN CIVIL CONSTRUCTORS WEST COAST L",2085248.25,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",25985000,"","",1.33,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","13","","C204657","C204638-RW","1","POLK","WATSON CONTRACTING INC",16495772.35,"RW1","",0.89200000000000002,4,"M720",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",16495772.35,"","",0.89200000000000002,null,"",null,null,"","",null,null,null,"","",""]
[null,"11/16/2021","2","U-4405A","C204404","C204404-EC","1","CUMBERLAND","HIGHLAND PAVING CO LLC",693235.05,"RW1","I000",null,6,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204404-RW","1","CUMBERLAND","HIGHLAND PAVING CO LLC",25928639.739999998,"RW1","I000",2.1019999999999999,6,"D352",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204404-SG","1","CUMBERLAND","HIGHLAND PAVING CO LLC",1511298.4,"RW1","I000",null,6,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204404-SI","1","CUMBERLAND","HIGHLAND PAVING CO LLC",212595.25,"RW1","",null,6,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204404-ST","1","CUMBERLAND","HIGHLAND PAVING CO LLC",24757.1,"WL1","Y007",null,null,"W001",7.83,null,"","",null,null,null,"COAST","6","(46+64.00-L-) RT"]
[null,"","","","","C204404-TC","1","CUMBERLAND","HIGHLAND PAVING CO LLC",236419,"RW1","I000",null,6,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","C204404-UT","1","CUMBERLAND","HIGHLAND PAVING CO LLC",1890091.32,"RW1","I000",null,6,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","2","CUMBERLAND","HIGHLAND PAVING CO LLC",5263964.93,"RW1","NPAR",null,6,"",null,null,"","",null,null,null,"COAST","6",""]
[null,"","","","","","","","Result",35761000.789999999,"","",2.1019999999999999,null,null,null,null,"","",null,null,null,"","",""]
[null,"","3","","C204671","C204671-RW","1","WARREN","S T WOOTEN CORPORATION",2103490,"RW1","",16.457999999999998,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2103490,"","",16.457999999999998,null,"",null,null,"","",null,null,null,"","",""]
[null,"","4","","C204670","C204670A-RW","1","VANCE","CAROLINA SUNROCK LLC",2564073.73,"RW1","",19.21,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204670B-RW","1","VANCE","CAROLINA SUNROCK LLC",183687.8,"RW1","",2.1539999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",2747761.53,"","",21.364000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204674","C204674A-RW","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",2555350.9500000002,"RW1","",12.863,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204674B-RW","1","DURHAM","FSC II LLC DBA FRED SMITH COMPANY",705649.41,"RW1","",3.4790000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204674C-RW","1","ORANGE","FSC II LLC DBA FRED SMITH COMPANY",31478.29,"RW1","",0.188,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204674D-RW","1","ORANGE","FSC II LLC DBA FRED SMITH COMPANY",16266.95,"RW1","",4.7E-2,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",3308745.6,"","",16.577000000000002,null,"",null,null,"","",null,null,null,"","",""]
[null,"","6","U-5754","C204665","C204295-EC","1","GUILFORD","BRANCH CIVIL INC",224525.5,"RW1","",null,3,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204295-LI","1","GUILFORD","BRANCH CIVIL INC",576737.5,"RW1","",null,3,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204295-RW","1","GUILFORD","BRANCH CIVIL INC",3243194.85,"RW1","",1.018,3,"M720",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204295-SI","1","GUILFORD","BRANCH CIVIL INC",680269.9,"RW1","",null,3,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","C204295-TC","1","GUILFORD","BRANCH CIVIL INC",420157.25,"RW1","",null,3,"",null,null,"","",null,null,null,"PDMT","7",""]
[null,"","","","","","","","Result",5144885,"","",1.018,null,"",null,null,"","",null,null,null,"","",""]
[null,"","7","I-5946B","C204660","C204660-RW","1","RICHMOND","FSC II LLC DBA FRED SMITH COMPANY",5302480.5,"RW1","I000",6.85,2,"RH10",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204660-SI","1","RICHMOND","FSC II LLC DBA FRED SMITH COMPANY",252204,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204660-ST","1","RICHMOND","FSC II LLC DBA FRED SMITH COMPANY",46989.32,"BR01","X281",2.3E-2,null,"11",null,42.453099999999999,"100","I",3,39.369799999999998,121.7188,"PDMT","8","BRIDGE NO 760183"]
[null,"","","","","","2","RICHMOND","FSC II LLC DBA FRED SMITH COMPANY",45229.36,"BR02","X281",2.1999999999999999E-2,null,"11",null,42.362499999999997,"100","I",3,39.369799999999998,113.51560000000001,"PDMT","8","BRIDGE NO 760184"]
[null,"","","","","C204660-TC","1","RICHMOND","FSC II LLC DBA FRED SMITH COMPANY",276476.65000000002,"RW1","I000",null,2,"",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",5923379.8300000001,"","",6.8949999999999996,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","9","","C204680","C204680A-RW","1","RANDOLPH","SHARPE BROTHERS A DIVISION OF VECELLIO &",1893905.46,"RW1","",10.54,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204680B-RW","1","RANDOLPH","SHARPE BROTHERS A DIVISION OF VECELLIO &",840122.59,"RW1","",6.11,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2734028.05,"","",16.649999999999999,null,"",null,null,"","",null,null,null,"","",""]
[null,"","10","","C204677","C204677A-RW","1","MOORE","S T WOOTEN CORPORATION",534627.76,"RW1","",2.92,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204677B-RW","1","MOORE","S T WOOTEN CORPORATION",3637062.24,"RW1","",27.972999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",4171690,"","",30.893000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","11","","C204676","C204676A-RW","1","MONTGOMERY","FSC II LLC DBA FRED SMITH COMPANY",1522093.59,"RW1","",6.556,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204676B-RW","1","MONTGOMERY","FSC II LLC DBA FRED SMITH COMPANY",688791.18,"RW1","",3.7869999999999999,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204676C-RW","1","MONTGOMERY","FSC II LLC DBA FRED SMITH COMPANY",162229.5,"RW1","",0.82899999999999996,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2373114.27,"","",11.172000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","12","","C204679","C204679-RW","1","RANDOLPH","SHARPE BROTHERS A DIVISION OF VECELLIO &",2864100.92,"RW1","",22.31,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2864100.92,"","",22.31,null,"",null,null,"","",null,null,null,"","",""]
[null,"","13","","C204678","C204678A-RW","1","ROWAN","NJR GROUP INC",1978636.09,"RW1","",9.5749999999999993,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204678B-RW","1","ROWAN","NJR GROUP INC",4521277.97,"RW1","",25.251000000000001,2,"R000",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",6499914.0599999996,"","",34.826000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","14","R-2566BA","C204355","C204355-EC","1","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",436132.5,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204355-RW","1","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",10011132.630000001,"RW1","",0.378,4,"B801",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204355-SG","1","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",202930,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204355-SI","1","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",40207.9,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204355-ST","1","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",420422.75,"WL1","Y007",null,null,"W001",11.2,null,"","",null,null,null,"VERY MTN","11","(19+40.00 -WALL 1-)"]
[null,"","","","","","2","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",8238148.8700000001,"BR01","X031",5.0999999999999997E-2,null,"15",null,101.58329999999999,"","Q",2,99,270,"VERY MTN","11","(164+30.00 -L-)"]
[null,"","","","","C204355-TC","1","WATAUGA","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",889221.4,"RW1","",null,4,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","","","","Result",20238196.050000001,"","",0.42899999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","15","BR-0002","C204682","C204482-EC","1","ASHE","JAMES R VANNOY & SONS CONSTRUCTION COMPA",347056,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204482-RW","1","ASHE","JAMES R VANNOY & SONS CONSTRUCTION COMPA",3866335.4,"RW1","",0.27700000000000002,2,"B801",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204482-SI","1","ASHE","JAMES R VANNOY & SONS CONSTRUCTION COMPA",21142.15,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","C204482-ST","1","ASHE","JAMES R VANNOY & SONS CONSTRUCTION COMPA",2190120,"WL1","Y007",null,null,"W001",12.48,null,"","",null,null,null,"VERY MTN","11","(14+99.33 -WALL 1-)"]
[null,"","","","","","2","ASHE","JAMES R VANNOY & SONS CONSTRUCTION COMPA",1592288.72,"BR01","X081",5.2999999999999999E-2,null,"15",null,38.25,"764","Q",3,35,280,"VERY MTN","11","(23+80.00 -L-)"]
[null,"","","","","C204482-TC","1","ASHE","JAMES R VANNOY & SONS CONSTRUCTION COMPA",262784.40000000002,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","11",""]
[null,"","","","","","","","Result",8279726.6699999999,"","",0.33,null,null,null,null,null,null,null,null,null,"","",""]
[null,"12/7/2021","1","R-5021","C204123","C204123-EC","1","BRUNSWICK","BARNHILL CONTRACTING CO",8844937.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204123-RW","1","BRUNSWICK","BARNHILL CONTRACTING CO",134590584.00999999,"RW1","I000",7.1580000000000004,2,"D320",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204123-ST","1","BRUNSWICK","BARNHILL CONTRACTING CO",292851.7,"CV01","X088",null,8.2100000000000009,"C001",136,10,"","",null,null,null,"COAST","3","(64+15.00 -L-)"]
[null,"","","","","","2","BRUNSWICK","BARNHILL CONTRACTING CO",375412.25,"CV02","X088",null,4.82,"C003",134,8,"","",null,null,null,"COAST","3","(83+76.00 -L-)"]
[null,"","","","","","3","BRUNSWICK","BARNHILL CONTRACTING CO",437721.95,"CV03","X088",null,6.6,"C002",134,9,"","",null,null,null,"COAST","3","(226+01.00 -L-)"]
[null,"","","","","","4","BRUNSWICK","BARNHILL CONTRACTING CO",379353.3,"CV04","X088",null,8.4600000000000009,"C002",148,7,"","",null,null,null,"COAST","3","(316+72.00 -L-)"]
[null,"","","","","","5","BRUNSWICK","BARNHILL CONTRACTING CO",102940.5,"WL1","Y007",null,null,"W001",5.27,null,"","",null,null,null,"COAST","3","(232+85.00 -L-)"]
[null,"","","","","","6","BRUNSWICK","BARNHILL CONTRACTING CO",24283.4,"WL2","Y007",null,null,"W001",5.1100000000000003,null,"","",null,null,null,"COAST","3","(232+85.00 -L-)"]
[null,"","","","","","7","BRUNSWICK","BARNHILL CONTRACTING CO",319570.59999999998,"WL3","Y007",null,null,"W001",20.399999999999999,null,"","",null,null,null,"COAST","3","(31+30.81 -Y REV-)"]
[null,"","","","","","8","BRUNSWICK","BARNHILL CONTRACTING CO",141835.85,"WL4","Y007",null,null,"W001",20.39,null,"","",null,null,null,"COAST","3","(31+30.81-YREV-)"]
[null,"","","","","","9","BRUNSWICK","BARNHILL CONTRACTING CO",441345.3,"WL5","Y007",null,null,"W001",23.05,null,"","",null,null,null,"COAST","3","(31+30.81-YREV-)"]
[null,"","","","","","10","BRUNSWICK","BARNHILL CONTRACTING CO",194628.35,"WL6","Y007",null,null,"W001",23.27,null,"","",null,null,null,"COAST","3","(31+30.81-YREV-)"]
[null,"","","","","","11","BRUNSWICK","BARNHILL CONTRACTING CO",581773.35,"WL7","Y007",null,null,"W001",8.61,null,"","",null,null,null,"COAST","3","(38+00.00-YREV-)"]
[null,"","","","","","12","BRUNSWICK","BARNHILL CONTRACTING CO",291062.65000000002,"WL8","Y007",null,null,"W001",19.350000000000001,null,"","",null,null,null,"COAST","3","(39+52.37-Y14A-)"]
[null,"","","","","","13","BRUNSWICK","BARNHILL CONTRACTING CO",1141021.8999999999,"WL9","Y007",null,null,"W001",20.79,null,"","",null,null,null,"COAST","3","(39+52.37-Y14A-)"]
[null,"","","","","","14","BRUNSWICK","BARNHILL CONTRACTING CO",677503.75,"WL10","Y007",null,null,"W001",22.38,null,"","",null,null,null,"COAST","3","(39+52.37-Y14A-)"]
[null,"","","","","","15","BRUNSWICK","BARNHILL CONTRACTING CO",1047403.2,"WL11","Y007",null,null,"W001",19.489999999999998,null,"","",null,null,null,"COAST","3","(39+52.37-Y14A-)"]
[null,"","","","","","16","BRUNSWICK","BARNHILL CONTRACTING CO",570510.94999999995,"WL12","Y007",null,null,"W001",12.1,null,"","",null,null,null,"COAST","3","(48+50.00-Y14A-)"]
[null,"","","","","","17","BRUNSWICK","BARNHILL CONTRACTING CO",335760.3,"WL13","Y007",null,null,"W001",10.68,null,"","",null,null,null,"COAST","3","(47+00.00-YREV-)"]
[null,"","","","","","18","BRUNSWICK","BARNHILL CONTRACTING CO",1145615.6200000001,"BR01","X081",null,null,"15",null,32.583300000000001,"836","C",3,30,139.95830000000001,"COAST","3","(369+42.00-L-) WBL"]
[null,"","","","","","19","BRUNSWICK","BARNHILL CONTRACTING CO",1236823.8600000001,"BR02","X081",2.7E-2,null,"15",null,32.583300000000001,"836","A",3,30,140.04169999999999,"COAST","3","(369+42.00-L-) EBL"]
[null,"","","","","","20","BRUNSWICK","BARNHILL CONTRACTING CO",2189504.9,"BR03","X081",null,null,"11",null,84.75,"873","A",1,81.5,140.66669999999999,"COAST","3","(31+30.81-YREV-)"]
[null,"","","","","","21","BRUNSWICK","BARNHILL CONTRACTING CO",1652223.64,"BR04","X281",null,null,"11",null,84.75,"873","A",1,81.5,140.66669999999999,"COAST","3","(39+52.37-Y14A-)"]
[null,"","","","","","22","BRUNSWICK","BARNHILL CONTRACTING CO",4467322.3899999997,"BR05","X281",null,null,"11",null,32.583300000000001,"854","A",3,30,311.41669999999999,"COAST","3","(390+15.00-L-) LT"]
[null,"","","","","","23","BRUNSWICK","BARNHILL CONTRACTING CO",2575179.38,"BR06","X081",5.8999999999999997E-2,null,"15",null,32.583300000000001,"854","A",3,30,311.58330000000001,"COAST","3","(390+15.00-L-) RT"]
[null,"","","","","C204123-UT","1","BRUNSWICK","BARNHILL CONTRACTING CO",44530435.299999997,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","2","BRUNSWICK","BARNHILL CONTRACTING CO",8672442.6999999993,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",217260048.59999999,"","",7.2439999999999998,null,null,null,null,null,null,null,null,null,"","",""]
[null,"12/21/2021","1","U-2579AB","C204633","C204633-EC","1","FORSYTH","WEBBER LLC",15489094.310000001,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204633-LI","1","FORSYTH","WEBBER LLC",469746.33,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204633-RW","1","FORSYTH","WEBBER LLC",133241370.79000001,"RW1","I000",2.722,6,"N212",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204633-SG","1","FORSYTH","WEBBER LLC",2723529.6,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204633-SI","1","FORSYTH","WEBBER LLC",5067989.62,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204633-ST","1","FORSYTH","WEBBER LLC",3112720.33,"CV01","Y007",5.0000000000000001E-3,20.170000000000002,"C002",564.33000000000004,12,"","",null,null,null,"PDMT","9","(768+62.23 -L-)"]
[null,"","","","","","2","FORSYTH","WEBBER LLC",458492.2,"CV02","Y007",null,19.760000000000002,"C001",320.5,6,"","",null,null,null,"PDMT","9","(792+88.12 -L-)"]
[null,"","","","","","3","FORSYTH","WEBBER LLC",399468.94,"CV03","Y007",null,40.35,"C001",357,5,"","",null,null,null,"PDMT","9","(43+66.60-Y15FLYCA-)"]
[null,"","","","","","4","FORSYTH","WEBBER LLC",560766.49,"CV04","Y007",null,26.33,"C001",330.75,8,"","",null,null,null,"PDMT","9","(30+13.47 -Y15REV-)"]
[null,"","","","","","5","FORSYTH","WEBBER LLC",468283.55,"CV05","Y007",null,10.43,"C003",78.75,12,"","",null,null,null,"PDMT","9","(18+22.67 -Y5B-)"]
[null,"","","","","","6","FORSYTH","WEBBER LLC",119120.7,"CV06","Y007",null,6.75,"C001",60.25,7,"","",null,null,null,"PDMT","9","(19+75.11 -Y5B-)"]
[null,"","","","","","7","FORSYTH","WEBBER LLC",329891.36,"CV07","Y007",null,27.65,"C001",215.67,6,"","",null,null,null,"PDMT","9","35+53.70-Y15RPDREV-"]
[null,"","","","","","8","FORSYTH","WEBBER LLC",402824.1,"WL1","Y007",null,null,"W001",19.66,null,"","",null,null,null,"PDMT","9","(29+93.81 -Y4-)"]
[null,"","","","","","9","FORSYTH","WEBBER LLC",317492.5,"WL2","Y007",null,null,"W001",14.38,null,"","",null,null,null,"PDMT","9","(31+41.50 -Y4-)"]
[null,"","","","","","10","FORSYTH","WEBBER LLC",1866479.08,"WL3","Y007",null,null,"W001",43.71,null,"","",null,null,null,"PDMT","9","(10+00.00 -NW11/13-)"]
[null,"","","","","","11","FORSYTH","WEBBER LLC",2803610.49,"WL4","Y007",null,null,"W001",42.82,null,"","",null,null,null,"PDMT","9","(10+00.00 -NW15/16-)"]
[null,"","","","","","12","FORSYTH","WEBBER LLC",2877061.11,"WL5","Y007",null,null,"W001",16.3,null,"","",null,null,null,"PDMT","9","(10+00 -NW17/18/19-)"]
[null,"","","","","","13","FORSYTH","WEBBER LLC",3577643.5,"WL6","Y007",null,null,"W001",27.7,null,"","",null,null,null,"PDMT","9","(10+00.00 -NW24/25-)"]
[null,"","","","","","14","FORSYTH","WEBBER LLC",3431832.32,"BR01","X231",null,null,"11",null,38.083300000000001,"678","A",2,30,355.79169999999999,"PDMT","9","(22+26.35 -Y1B-)"]
[null,"","","","","","15","FORSYTH","WEBBER LLC",2399331.1800000002,"BR02","X281",null,null,"11",null,116.25,"854","Q",2,113,164,"PDMT","9","(30+67.66 -Y4-)"]
[null,"","","","","","16","FORSYTH","WEBBER LLC",5172545.29,"BR03","X281",null,null,"11",null,151.25,"800","Q",2,148,245,"PDMT","9","(47+28.33 -Y15REV-)"]
[null,"","","","","","17","FORSYTH","WEBBER LLC",21312115.170000002,"BR04","X231",null,null,"11",null,43.25,"600","I",10,40,1883,"PDMT","9","(60+66.06-Y15FLYAC-)"]
[null,"","","","","","18","FORSYTH","WEBBER LLC",17390098.300000001,"BR05","X231",null,null,"11",null,43.25,"600","I",10,40,1883,"PDMT","9","(47+63.62-Y15FLYBD-)"]
[null,"","","","","","19","FORSYTH","WEBBER LLC",21009523.969999999,"BR06","X231",null,null,"11",null,43.25,"699","I",8,40,1717,"PDMT","9","(58+33.94-Y15FLYCA-)"]
[null,"","","","","","20","FORSYTH","WEBBER LLC",5264065.63,"BR07","X231",null,null,"11",null,38.083300000000001,"699","Q",4,28,476,"PDMT","9","(23+43.03 -Y16-)"]
[null,"","","","","C204633-TC","1","FORSYTH","WEBBER LLC",3407609.25,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","C204633-UT","1","FORSYTH","WEBBER LLC",4492653.2300000004,"RW1","I000",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","2","FORSYTH","WEBBER LLC",3598663.03,"RW1","NPAR",null,6,"",null,null,"","",null,null,null,"PDMT","9",""]
[null,"","","","","","","","Result",261764022.37,"","",2.7269999999999999,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","2","R-2233BB","C204397","C204397-EC","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",10374953.25,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204397-RW","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",71742089.069999993,"RW1","",5.1379999999999999,4,"N210",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204397-SG","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",858629.25,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204397-SI","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",885454.1,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204397-ST","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1390779.1,"CV01","Y007",null,88,"C001",464,10,"","",null,null,null,"MTN","13","(797+66.00 -L3-)"]
[null,"","","","","","2","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1028432.3,"CV02","Y007",null,57,"C001",543,8,"","",null,null,null,"MTN","13","(830+02.00 -L3-)"]
[null,"","","","","","3","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",832841.65,"CV03","Y007",7.0000000000000001E-3,19,"C003",201.5,10,"","",null,null,null,"MTN","13","(874+45.00 -L3-)"]
[null,"","","","","","4","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1686044.65,"CV04","Y007",null,85,"C001",514.75,10,"","",null,null,null,"MTN","13","(735+38.59 -L3-)"]
[null,"","","","","","5","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",601662.5,"WL1","Y007",null,null,"W001",16.809999999999999,null,"","",null,null,null,"MTN","13","(10+00.00-W1-)"]
[null,"","","","","","6","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",502860,"WL2","Y007",null,null,"W001",17.329999999999998,null,"","",null,null,null,"MTN","13","(10+00.00-W2-)"]
[null,"","","","","","7","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",592033,"WL3","Y007",null,null,"W001",16.02,null,"","",null,null,null,"MTN","13","(9+95.80-WALL6-)"]
[null,"","","","","","8","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",609745.6,"WL4","Y007",null,null,"W001",15.79,null,"","",null,null,null,"MTN","13","(10+00.00-NW5A-)"]
[null,"","","","","","9","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",352192.5,"WL5","Y007",null,null,"W001",16.09,null,"","",null,null,null,"MTN","13","(10+00.00-NW5B-)"]
[null,"","","","","","10","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",776652.7,"WL6","Y007",null,null,"W001",16.68,null,"","",null,null,null,"MTN","13","(10+00.00-NW8-)"]
[null,"","","","","","11","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",784883,"WL7","Y007",null,null,"W001",13.87,null,"","",null,null,null,"MTN","13","(10+00.00-NW11-)"]
[null,"","","","","","12","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1116144.1000000001,"WL8","Y007",null,null,"W001",16.36,null,"","",null,null,null,"MTN","13","(10+00.00-NW13-)"]
[null,"","","","","","13","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",314577.2,"WL9","Y007",null,null,"W001",12.82,null,"","",null,null,null,"MTN","13","(10+00.00-NW15-)"]
[null,"","","","","","14","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",787868.38,"BR01","X281",1.9E-2,null,"11",null,49.25,"754","A",1,46,103.5,"MTN","13","(774+41.49 -L3- LT)"]
[null,"","","","","","15","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",774750.48,"BR02","X281",null,null,"11",null,49.25,"754","A",1,46,103.5,"MTN","13","(774+41.49 -L3- RT)"]
[null,"","","","","","16","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",1280669.92,"BR03","X281",null,null,"11",null,44.583300000000001,"854","I",2,28,181.5,"MTN","13","(20+88.94-Y19-)"]
[null,"","","","","","17","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",2882713.95,"BR04","X281",null,null,"11",null,91.583299999999994,"873","Q",2,80,181.5,"MTN","13","(26+65.52-Y3-)"]
[null,"","","","","C204397-TC","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",795332.25,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","C204397-UT","1","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",7838328.3300000001,"RW1","",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","2","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",273330.12,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","3","RUTHERFORD","WRIGHT BROTHERS CONSTRUCTION COMPANY INC",154332.62,"RW1","NPAR",null,4,"",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","","","Result",109237300.02,"","",5.1639999999999997,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","4","R-5014","C204688","C204182-EC","1","DARE","FSC II LLC DBA FRED SMITH COMPANY",674611.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204182-RW","1","DARE","FSC II LLC DBA FRED SMITH COMPANY",13297866.65,"RW1","I000",4.2039999999999997,2,"D300",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204182-SG","1","DARE","FSC II LLC DBA FRED SMITH COMPANY",248362,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204182-SI","1","DARE","FSC II LLC DBA FRED SMITH COMPANY",159364.6,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204182-TC","1","DARE","FSC II LLC DBA FRED SMITH COMPANY",1121530.5,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","C204182-UT","1","DARE","FSC II LLC DBA FRED SMITH COMPANY",3948673.25,"RW1","I000",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","","2","DARE","FSC II LLC DBA FRED SMITH COMPANY",504591.75,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"COAST","1",""]
[null,"","","","","","","","Result",19955000,"","",4.2039999999999997,null,"",null,null,"","",null,null,null,"","",""]
[null,"","5","","C204685","C204685A-RW","1","BRUNSWICK","S T WOOTEN CORPORATION",3787339.52,"RW1","",3.9,4,"R000",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204685B-RW","1","BRUNSWICK","S T WOOTEN CORPORATION",992480.51,"RW1","",5.97,2,"R000",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",4779820.03,"","",9.8699999999999992,null,"",null,null,"","",null,null,null,"","",""]
[null,"","6","B-5642","C204623","C204623-EC","1","BRUNSWICK","ES WAGNER COMPANY LLC",50165.38,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204623-RW","1","BRUNSWICK","ES WAGNER COMPANY LLC",466803.33,"RW1","",0.14699999999999999,2,"B810",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204623-SI","1","BRUNSWICK","ES WAGNER COMPANY LLC",8281.7999999999993,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","C204623-ST","1","BRUNSWICK","ES WAGNER COMPANY LLC",626347.53,"BR01","X080",1.4E-2,null,"15",null,42,"722","A",1,39.833300000000001,72.25,"COAST","3","(18+30.00 -L-)"]
[null,"","","","","C204623-TC","1","BRUNSWICK","ES WAGNER COMPANY LLC",8017.2,"RW1","",null,2,"",null,null,"","",null,null,null,"COAST","3",""]
[null,"","","","","","","","Result",1159615.24,"","",0.161,null,null,null,null,null,null,null,null,null,"","",""]
[null,"","7","","C204687","C204687A-RW","1","WAKE","CAROLINA SUNROCK LLC",2210653.35,"RW1","",8.33,2,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","C204687B-RW","1","WAKE","CAROLINA SUNROCK LLC",2362479.2000000002,"RW1","",16.321999999999999,4,"R000",null,null,"","",null,null,null,"PDMT","5",""]
[null,"","","","","","","","Result",4573132.55,"","",24.652000000000001,null,"",null,null,"","",null,null,null,"","",""]
[null,"","8","","C204683","C204683A-RW","1","HOKE","HUDSON PAVING INC",736328.45,"RW1","",5.08,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204683B-RW","1","SCOTLAND","HUDSON PAVING INC",544933.9,"RW1","",2.93,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204683C-RW","1","HOKE","HUDSON PAVING INC",522776.57,"RW1","",5.18,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","C204683D-RW","1","SCOTLAND","HUDSON PAVING INC",335196.42,"RW1","",3.31,2,"R000",null,null,"","",null,null,null,"PDMT","8",""]
[null,"","","","","","","","Result",2139235.34,"","",16.5,null,"",null,null,"","",null,null,null,"","",""]
[null,"","9","","C204686","C204686A-RW","1","CABARRUS","NJR GROUP INC",346463.13,"RW1","",1.01,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204686B-RW","1","CABARRUS","NJR GROUP INC",4423428.38,"RW1","",20.65,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","C204686C-RW","1","CABARRUS","NJR GROUP INC",734877.82,"RW1","",null,2,"R000",null,null,"","",null,null,null,"PDMT","10",""]
[null,"","","","","","","","Result",5504769.3300000001,"","",21.66,null,"",null,null,"","",null,null,null,"","",""]
[null,"","10","","C204681","C204681A-RW","1","TRANSYLVANIA","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",626507.23,"RW1","",0.8,3,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204681B-RW","1","POLK","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",1299469.07,"RW1","",8.11,2,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204681C-RW","1","TRANSYLVANIA","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",1792351.43,"RW1","",9.8320000000000007,4,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204681D-RW","1","POLK","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",1045825.44,"RW1","",6.19,2,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204681E-RW","1","TRANSYLVANIA","APAC ATLANTIC INC DBA HARRISON CONSTRUCT",1279296.3799999999,"RW1","",8.23,2,"R000",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",6043449.5499999998,"","",33.161999999999999,null,"",null,null,"","",null,null,null,"","",""]
[null,"","11","U-5888","C204675","C204675-EC","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",368030,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204675-LI","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",127078.6,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","2","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",190420.4,"RW1","NPAR",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204675-RW","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",3471375.5,"RW1","",0.24,2,"C002",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204675-SG","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",17500,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204675-SI","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",46272.3,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204675-ST","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",662822,"CV01","Y007",null,5.19,"C002",89,11,"","",null,null,null,"VERY MTN","14","(14+99.00 -Y14-)"]
[null,"","","","","C204675-TC","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",244118.95,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","C204675-UT","1","HAYWOOD","IPC PAVING LLC IPC STRUCTURES LLC",771904.85,"RW1","",null,2,"",null,null,"","",null,null,null,"VERY MTN","14",""]
[null,"","","","","","","","Result",5899522.5999999996,"","",0.24,null,null,null,null,"","",null,null,null,"","",""]
[null,"","12","B-6011","C204406","C204406-RW","1","BUNCOMBE","R. E. BURNS & SONS CO., INC.",4200819,"RW1","K000",0.28100000000000003,2,"M713",null,null,"","",null,null,null,"MTN","13",""]
[null,"","","","","","","","Result",4200819,"","",0.28100000000000003,null,"",null,null,"","",null,null,null,"","",""]
[null,"Overall Result",null,null,null,null,null,null,null,2502166248.6700001]

{"sheet":"ITEMS - STATEWIDE","index":2,"n_rows":2289,"n_cols":8,"rows_kept":2289,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - STATEWIDE"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",132,666749.97666666703,88010996.920000002]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",56,359785.34625,20147979.390000001]
[null,"0000700000-N","FIELD OFFICE","","",2,862500,1725000]
[null,"0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN & CONSTRUCTION OF","BRIDGES",1,2082600,2082600]
[null,"","","DESIGN & CONSTRUCTION OF      BRIDGES","",1,2004595,2004595]
[null,"","","DESIGN & CONSTRUCTION OF CUL-","VERT #100536",1,809374,809374]
[null,"","","","VERT #110237",1,585301,585301]
[null,"","","DESIGN AND CONSTRUCTION","I-6064A",1,240488250,240488250]
[null,"","","","I-6064B",1,114376950,114376950]
[null,"","","","I-6064C / I-5879",1,77834800,77834800]
[null,"0000910000-N","GENERIC MISCELLANEOUS ITEM (HR)","EXPLORATORY EXCAVATION -      STANDARD","",1,500,500]
[null,"","","EXPLORATORY EXCAVATION -      VACUUM","",1,600,600]
[null,"0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","DRILLED ORIFICE PLATE AND     TRASH RACK","",1,555,555]
[null,"","","END BENTS STRUCTURE #020035","",2,110000,220000]
[null,"","","END BENTS STRUCTURE #020133","",2,40000,80000]
[null,"","","END BENTS STRUCTURE #100142","",2,35000,70000]
[null,"","","END BENTS STRUCTURE #110145","",2,32000,64000]
[null,"","","END BENTS STRUCTURE #580312","",2,47000,94000]
[null,"","","END BENTS STRUCTURE #600207","",2,35000,70000]
[null,"","","END BENTS STRUCTURE #960733","",2,85000,170000]
[null,"","","INTERIOR BENT CAPS STRUCTURE  #020133","",2,30000,60000]
[null,"","","INTERIOR BENT CAPS STRUCTURE  #580312","",1,30000,30000]
[null,"","","POLYMER CONCRETE CLEANOUT     BOXES","",1,975,975]
[null,"","","RIGHT OF WAY ACQUISITION","",18,7444.4444444444398,134000]
[null,"","","WILDLIFE GUARDS","",4,106451,425804]
[null,"","","WILDLIFE JUMP OUTS","",3,14245,42735]
[null,"0000920000-E","GENERIC MISCELLANEOUS ITEM (CY)","BIOSWALE FILTRATION MEDIA","",90,100,9000]
[null,"0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT #1 STRUCTURE #020035",21,600,12600]
[null,"","","","BENT #1 STRUCTURE #020133",13,750,9750]
[null,"","","","BENT #1 STRUCTURE #100142",13,4500,58500]
[null,"","","","BENT #1 STRUCTURE #110145",25,685,17125]
[null,"","","","BENT #1 STRUCTURE #580312",18,1,18]
[null,"","","","BENT #1 STRUCTURE #600207",30,960,28800]
[null,"","","","BENT #1 STRUCTURE #960733",22.5,640,14400]
[null,"","","","BENT #2 STRUCTURE #020035",12,1650,19800]
[null,"","","","BENT #2 STRUCTURE #020133",11,815,8965]
[null,"","","","BENT #2 STRUCTURE #100142",10,5800,58000]
[null,"","","","BENT #2 STRUCTURE #110145",22,780,17160]
[null,"","","","BENT #2 STRUCTURE #580312",16,1,16]
[null,"","","","BENT #2 STRUCTURE #600207",20,1000,20000]
[null,"","","","BENT #2 STRUCTURE #960733",20.5,615,12607.5]
[null,"","","AVE FOUNDATION LENGTH AT INT","BENT STRUCTURE #020133",29,6000,174000]
[null,"","","AVE FOUNDATION LENGTH AT INTE-","RIOR BENT #1 STRUCTURE #580312",28,5500,154000]
[null,"","","BIOSWALE UNDERDRAIN PIPE","",300,25,7500]
[null,"","","BRIDGE LENGTH STRUCTURE       #020035","",100,4250,425000]
[null,"","","BRIDGE LENGTH STRUCTURE       #020133","",150,3000,450000]
[null,"","","BRIDGE LENGTH STRUCTURE       #100142","",50,3300,165000]
[null,"","","BRIDGE LENGTH STRUCTURE       #110145","",70,3200,224000]
[null,"","","BRIDGE LENGTH STRUCTURE       #580312","",110,3300,363000]
[null,"","","BRIDGE LENGTH STRUCTURE       #600207","",55,3320,182600]
[null,"","","BRIDGE LENGTH STRUCTURE       #960733","",70,3000,210000]
[null,"0000950000-E","GENERIC MISCELLANEOUS ITEM (SF)","PERMANENT SHORING","",4200,200,840000]
[null,"0000960000-E","GENERIC MISCELLANEOUS ITEM (SY)","POLYPROPYLENE NONWOVEN GEO-","TEXTILE FABRIC",250,4,1000]
[null,"0000995000-E","GENERIC MISCELLANEOUS ITEM (TON)","NO 57 STONE, WASHED","",50,37,1850]
[null,"0000996000-N","DESIGN AND CONSTRUCTION","","",2,161084434.5,322168869]
[null,"0001000000-E","CLEARING & GRUBBING","","",385,161302.38888600399,62117549.960000001]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",39,7673.7951282051299,299278.01]
[null,"0015000000-N","SEALING ABANDONED WELLS","","",42,2373.07071428571,99668.97]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",7717530,6.2231808881857296,48027585.200000003]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(1260+34.00 -L-)","",1,75000,75000]
[null,"","","(1391+19.65 -L-)","",1,125000,125000]
[null,"","","(15+61.00 -L-)","",1,30000,30000]
[null,"","","(16+92.70 -L-)","",1,49200,49200]
[null,"","","(16+99.00 -L-)","",1,25000,25000]
[null,"","","(164+30.00 -L-)","",1,100000,100000]
[null,"","","(17+00.00-L-)","",1,33000,33000]
[null,"","","(17+37.36 -L-)","",1,24000,24000]
[null,"","","(18+27.00 -L-)","",1,33000,33000]
[null,"","","(20+88.94 -Y19-)","",1,43500,43500]
[null,"","","(21+37.00 -L REV-)","",1,15675,15675]
[null,"","","(21+68.50 -L-)","",1,48000,48000]
[null,"","","(22+26.35 -Y1B-)","",1,30500.41,30500.41]
[null,"","","(23+43.03 -Y16-)","",1,30689.69,30689.69]
[null,"","","(23+80.00 -L-)","",1,27320,27320]
[null,"","","(24+78.90)","",1,56000,56000]
[null,"","","(26+65.52 -Y3-)","",1,67600,67600]
[null,"","","(27+01.91 -Y7-)","",1,39000,39000]
[null,"","","(27+79.00 -L-)","",1,28959,28959]
[null,"","","(28+85.96-L-)","",1,100000,100000]
[null,"","","(30+65.33 -Y1B-)","",1,43641.94,43641.94]
[null,"","","(30+80.00 -L-)","",1,16600,16600]
[null,"","","(32+31.61 -L-)","",1,25000,25000]
[null,"","","(34+65.50 -L-)","",1,43756.35,43756.35]
[null,"","","(35+30.22 -L-)","",1,70000,70000]
[null,"","","(369+42.00 -L- EBL)","",1,50000,50000]
[null,"","","(369+42.00 -L- WBL)","",1,50000,50000]
[null,"","","(390+15.00 -L- LT)","",1,75000,75000]
[null,"","","(390+15.00 -L- RT)","",1,75000,75000]
[null,"","","(41+45 -L1-)","",1,26000,26000]
[null,"","","(42+56.82 -Y1-)","",1,46000,46000]
[null,"","","(45+22.65 -EBL-)","",1,25000,25000]
[null,"","","(47+28.33 -Y15REV-)","",1,91890.66,91890.66]
[null,"","","(47+63.62 -Y15FLYBD-)","",1,42821.42,42821.42]
[null,"","","(58+33.94 -Y15FLYCA-)","",1,52200.66,52200.66]
[null,"","","(60+66.06 -Y15FLYAC-)","",1,46435.4,46435.4]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(1002+79.68 -L REV-)","",1,105000,105000]
[null,"","","(18+27.98 -L-)","",1,53500,53500]
[null,"","","(19+56.99 -L-)","",1,50875,50875]
[null,"","","(217+31.76 -L- LT)","",1,65000,65000]
[null,"","","(217+31.76 -L- RT)","",1,31000,31000]
[null,"","","(26+05.28 -Y14-)","",1,100000,100000]
[null,"","","(26+80.73 -Y17-)","",1,65000,65000]
[null,"","","(27+09.19 -Y16-)","",1,75000,75000]
[null,"","","(28+39.21 -Y29-)","",1,35000,35000]
[null,"","","(28+62 -L-)","",1,284948,284948]
[null,"","","(30+67.66 -Y4-)","",1,123127.96,123127.96]
[null,"","","(31+30.81 -Y REV-)","",1,90000,90000]
[null,"","","(39+52.37 -Y14A-)","",1,75000,75000]
[null,"","","(41+39.51 -Y-)","",1,130000,130000]
[null,"","","(61+02.86 -L- LT)","",1,79900,79900]
[null,"","","(61+02.86 -L- RT)","",1,79900,79900]
[null,"","","(774+41.49 -L3- LT)","",1,93000,93000]
[null,"","","(774+41.49 -L3- RT)","",1,93000,93000]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(12+94.70 -L-)","",1,25000,25000]
[null,"","","(13+34.00 -L-)","",1,16036.8,16036.8]
[null,"","","(13+78.50 -L-)","",1,11620,11620]
[null,"","","(15+23 -L-)","",1,11800,11800]
[null,"","","(15+45.00 -L-)","",1,23200,23200]
[null,"","","(15+50.00 -L-)","",1,10000,10000]
[null,"","","(16+08.00 -L-)","",1,9000,9000]
[null,"","","(16+10.00 -L-)","",1,9000,9000]
[null,"","","(16+62.00 -L-)","",1,11000,11000]
[null,"","","(17+68.00 -L-)","",1,5275,5275]
[null,"","","(18+28.00 -L- )","",1,8400,8400]
[null,"","","(18+30 -L-)","",1,15500,15500]
[null,"","","(19+07.12 -L-)","",1,23000,23000]
[null,"","","(23+06.50 -L-)","",1,6500,6500]
[null,"","","(23+55.00 -L-)","",1,13000,13000]
[null,"","","(23+71.50 -L-)","",1,9000,9000]
[null,"","","(25+06 -L1-)","",1,16500,16500]
[null,"","","(27+02.26 -L-)","",1,40000,40000]
[null,"","","(28+02.81 -L-)","",1,24000,24000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",277330,9.8852873832618204,2741486.75]
[null,"0043000000-N","GRADING","","",37,457629.15027027001,16932278.559999999]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",38.1,3982.2102362204701,151722.21]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",12854,13.916407344017401,178881.5]
[null,"0063000000-N","GRADING","","",7,549851.08428571397,3848957.59]
[null,"0084000000-E","WICK DRAINS","","",205000,0.7,143500]
[null,"0098000000-E","PRE-SPLITTING OF ROCK","","",16300,41.618098159509202,678375]
[null,"0106000000-E","BORROW EXCAVATION","","",4290126,8.5763207607422292,36793496.68]
[null,"0127000000-N","EMBM'T SETTLEMENT GAUGE","","",27,1146.8518518518499,30965]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",359896,11.1906224298131,4027460.25]
[null,"0141000000-E","BERM DITCH CONSTRUCTION","","",12305,8.5077935798455897,104688.4]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",678492,9.2903559658772696,6303432.2000000002]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",96757,18.5842057938961,1798152]
[null,"0170000000-E","REMOVAL OF CONC PVMT SLBS","","",500,191,95500]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",156125,4.4716201761409096,698131.7]
[null,"0185000000-E","BREAKING OF EXT CONC PVMT","","",9630,6.07,58454.1]
[null,"0192000000-N","PROOF ROLLING","","",535,317.61682242990702,169925]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",166050,27.419626618488401,4553029]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",164130,16.603178882593099,2725079.75]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",1095657,1.8084532841938701,1981444.5]
[null,"0199000000-E","TEMPORARY SHORING","","",119139,56.004034782900703,6672264.7000000002]
[null,"0220000000-E","ROCK EMBANKMENTS","","",5775,58.233333333333299,336297.5]
[null,"0222000000-E","GEOTEXTILE ROCK EMBANK","","",4990,4.4104208416833703,22008]
[null,"0223000000-E","ROCK PLATING","","",24078,70.834363319212599,1705549.8]
[null,"0225000000-E","REINFORCED SOIL SLOPES","","",650,64.5,41925]
[null,"0234000000-E","GENERIC GRADING ITEM (CY)","REMOVAL AND HAULING OF DEEP","BROWNFIELDS SOIL",10000,4.95,49500]
[null,"","","STOCKPILED SOIL","",500,10.42,5210]
[null,"0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",2550,8.5166666666666693,21717.5]
[null,"","","GEOTEXTILE FOR WICK DRAINS","",10400,1.5,15600]
[null,"","","NONWOVEN GEOTEXTILE","",2850,3.01,8578.5]
[null,"","","ROCK PLATING","",2200,78.900000000000006,173580]
[null,"","","ROCK PLATING, DETAIL NO A","",2000,40.1,80200]
[null,"","","SOIL CEMENT BASE (FULL DEPTH","RECLAMATION)",161471,3.3717575911463999,544441.06999999995]
[null,"","","SOIL CEMENT BASE FULL DEPTH","RECLAMATION",8840,4.7,41548]
[null,"","","TYPE 2 WIRE MESH","",400,210,84000]
[null,"0245000000-E","GENERIC GRADING ITEM (GAL)","TRENCH DEWATERING","",10000,1.82,18200]
[null,"0248000000-N","GENERIC GRADING ITEM (LS)","DE-WATERING","",1,62950,62950]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",110,127.272727272727,14000]
[null,"","","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",50,49.92,2496]
[null,"","","HAULING AND DISPOSAL OF CONTA-","MINATED SOIL STOCKPILES",500,78.13,39065]
[null,"","","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",2200,106.734772727273,234816.5]
[null,"","","RIP RAP, CLASS 2","",150,65.5,9825]
[null,"","","RIP RAP, CLASS A","",260,42.9,11154]
[null,"","","RIP RAP, CLASS II","",925,51.7,47822.5]
[null,"0257000000-E","GENERIC GRADING ITEM (LF)","ANCHOR FOR WIRE MESH","",600,190,114000]
[null,"0262000000-N","GENERIC GRADING ITEM (EA)","HAULING NCDOT SUPPLIED        MATERIAL","",320,104,33280]
[null,"0264000000-E","GENERIC GRADING ITEM (SMI)","SHOULDER GRADING","",588.24,2679.9499184006499,1576453.74]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",59912,46.298527006275897,2773837.35]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",247051,3.4947132373477499,863372.4]
[null,"0331000000-E","GENERIC DRAINAGE ITEM (CY)","ANTI-SEEP COLLAR","",30,364.59,10937.7]
[null,"0335000000-E","**\" DRAINAGE PIPE","(4\")","",100,25,2500]
[null,"","","(54\")","",1116,340.78853046594998,380320]
[null,"","","(66\")","",52,650,33800]
[null,"0335100000-E","12\" DRAINAGE PIPE","","",52,145,7540]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",10150,67.357674876847298,683680.4]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",4668,76.727849185946894,358165.6]
[null,"0335400000-E","24\" DRAINAGE PIPE","","",3444,91.607433217189296,315496]
[null,"0335500000-E","30\" DRAINAGE PIPE","","",2544,130.45990566037699,331890]
[null,"0335600000-E","36\" DRAINAGE PIPE","","",1832,128.18493449781701,234834.8]
[null,"0335700000-E","42\" DRAINAGE PIPE","","",940,210.33829787234001,197718]
[null,"0335800000-E","48\" DRAINAGE PIPE","","",1216,265.15460526315798,322428]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(12\")","",2,304,608]
[null,"","","(15\")","",89,390.65617977528098,34768.400000000001]
[null,"","","(30\")","",4,710,2840]
[null,"0342000000-E","**\" SIDE DRAIN PIPE","(12\")","",20,40,800]
[null,"","","(30\")","",2064,91.814728682170497,189505.6]
[null,"","","(36\")","",768,119.927083333333,92104]
[null,"","","(42\")","",1320,144.993939393939,191392]
[null,"","","(48\")","",428,195.09345794392499,83500]
[null,"","","(54\")","",52,230,11960]
[null,"","","(60\")","",48,250,12000]
[null,"","","(66\")","",372,350,130200]
[null,"","","(84\")","",76,450,34200]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",24206,50.764749235726697,1228811.52]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",12248,60.746116917047701,744018.44]
[null,"0345000000-E","24\" SIDE DRAIN PIPE","","",8644,72.488014807959303,626586.4]
[null,"0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",50,335.66800000000001,16783.400000000001]
[null,"","","(18\")","",2,600,1200]
[null,"","","(24\")","",2,520.84,1041.68]
[null,"","","(8\")","",3,250,750]
[null,"0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",924,78.987012987013003,72984]
[null,"","","(18\", V)","",996,75.634538152610403,75332]
[null,"","","(24\", CLASS V)","",128,91,11648]
[null,"","","(24\", V)","",1584,85.273737373737404,135073.60000000001]
[null,"","","(30\", V)","",64,148,9472]
[null,"","","(36\", CLASS V)","",280,155,43400]
[null,"","","(36\", V)","",44,170,7480]
[null,"","","(42\", V)","",954,266.061740041929,253822.9]
[null,"","","(48\", V)","",48,290,13920]
[null,"","","(54\", V)","",1064,440.10868421052601,468275.64]
[null,"","","(60\", V)","",1032,539.61968992248103,556887.52]
[null,"","","(66\", V)","",100,1015,101500]
[null,"0360000000-E","12\" RC PIPE CULV III","","",124,52.06,6455.44]
[null,"0366000000-E","15\" RC PIPE CULV III","","",29448,58.586738657973399,1725262.28]
[null,"0372000000-E","18\" RC PIPE CULV III","","",24412,67.438664591184704,1646312.68]
[null,"0378000000-E","24\" RC PIPE CULV III","","",13704,90.548517221249298,1240876.8799999999]
[null,"0384000000-E","30\" RC PIPE CULV III","","",10350,115.774502415459,1198266.1000000001]
[null,"0390000000-E","36\" RC PIPE CULV III","","",6988,150.38751001717199,1050907.92]
[null,"0396000000-E","42\" RC PIPE CULV III","","",3928,205.01109979633401,805283.6]
[null,"0402000000-E","48\" RC PIPE CULV III","","",2088,243.12521072796901,507645.44]
[null,"0408000000-E","54\" RC PIPE CULV III","","",1448,369.69419889502802,535317.19999999995]
[null,"0414000000-E","60\" RC PIPE CULV III","","",1368,415.69403508771899,568669.43999999994]
[null,"0420000000-E","66\" RC PIPE CULV III","","",48,652,31296]
[null,"0426000000-E","72\" RC PIPE CULV III","","",524,588.289618320611,308263.76]
[null,"0438000000-E","84\" RC PIPE CULV III","","",208,550,114400]
[null,"0448000000-E","***\" RCP CULV CLASS IV","(12\")","",1408,68.323863636363598,96200]
[null,"","","(48\")","",3818,272.11830277632299,1038947.68]
[null,"","","(54\")","",2392,451.19215719063499,1079251.6399999999]
[null,"","","(60\")","",2388,455.14857621440501,1086894.8]
[null,"","","(66\")","",812,545.27093596059103,442760]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",88568,66.923858730015397,5927312.3200000003]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",31158,85.451865973425797,2662509.2400000002]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",27964,95.126748676870307,2660124.4]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",16166,144.31398738092301,2332979.92]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",10876,185.63593232806201,2018976.4]
[null,"0448700000-E","42\" RCP CULV CLASS IV","","",8228,224.78118619348601,1849499.6]
[null,"0453000000-E","**\" PIPE END SECTION","(15\")","",1,1650,1650]
[null,"0536000000-E","***\" HDPE PIPE CULVTS","(18\")","",20,44.5,890]
[null,"","","(8\")","",44,74.75,3289]
[null,"0542000000-E","**\" PVC PIPE CULVERTS","(6\")","",64,70,4480]
[null,"0546000000-E","**\" CAA PIPE CLVT *****\"","(15\", 0.064\")","",140,74.599999999999994,10444]
[null,"","","(18\", 0.105\")","",12,175,2100]
[null,"","","(36\", 0.135\")","",12,308.5,3702]
[null,"","","(42\", 0.135\")","",128,470,60160]
[null,"","","(48\", 0.164\")","",216,475,102600]
[null,"","","(54\", 0.109\")","",84,588,49392]
[null,"","","(60\", 0.164\")","",172,650,111800]
[null,"0564000000-E","**\" CAA PIPE ELBOW *****\"","(15\", 0.064\")","",8,610,4880]
[null,"0576000000-E","**\" CS PIPE CULV *****\"","(18\", 0.079\")","",340,190,64600]
[null,"","","(24\", 0.109\")","",156,250,39000]
[null,"","","(30\", 0.138\")","",1876,315,590940]
[null,"","","(36\", 0.079\")","",856,210.006074766355,179765.2]
[null,"","","(36\", 0.138\")","",1004,375,376500]
[null,"","","(42\", 0.109\")","",668,283.21556886227501,189188]
[null,"","","(60\", 0.138\")","",56,530,29680]
[null,"","","(84\", 0.168\")","",28,815,22820]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",8442,83.996984126984103,709102.54]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",4184,107.173068833652,448412.12]
[null,"0594000000-E","24\" CS PIPE CULV 0.064\"","","",1812,124.916534216336,226348.76]
[null,"0600000000-E","30\" CS PIPE CULV 0.079\"","","",1432,187.49092178770999,268487]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",322,551.93881987577595,177724.3]
[null,"","","(18\", 0.064\")","",47,610.93872340425503,28714.12]
[null,"","","(18\", 0.079\")","",4,2125,8500]
[null,"","","(18\". 0.064\")","",14,910,12740]
[null,"","","(24\", 0.064\")","",29,658.43448275862102,19094.599999999999]
[null,"","","(24\", 0.109\")","",3,2675,8025]
[null,"","","(30\", 0.079\")","",23,1000.51217391304,23011.78]
[null,"","","(30\", 0.138\")","",20,4000,80000]
[null,"","","(36\", 0.079\")","",2,1041.21,2082.42]
[null,"","","(36\", 0.138')","",15,4925,73875]
[null,"","","(42\", 0.109\")","",2,1561.82,3123.64]
[null,"0654000000-E","***X***\"CSP ARCH CULV *****","(42\" X 29\", 0.079\")","",176,275,48400]
[null,"","","(57\" X 38\", 0.109\")","",60,385,23100]
[null,"","","(95\" X 67\", 0.109\")","",84,922,77448]
[null,"0926000000-E","***\"CS STR PL PIPE ** GA","(60\", 12)","",152,402,61104]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\", 0.250\")","",95,535.78947368421098,50900]
[null,"","","(16\", 0.281\")","",318,355,112890]
[null,"","","(18\", 0.250\")","",482,483.68572614107899,233136.52]
[null,"","","(18\", 0.312\")","",258,410,105780]
[null,"","","(18\", 0.500\")","",576,401.840277777778,231460]
[null,"","","(20\", 0.500\")","",24,668.12,16034.88]
[null,"","","(24\", 0.250\")","",46,300,13800]
[null,"","","(24\", 0.375\")","",430,446.78716279069801,192118.48]
[null,"","","(24\", 0.500\")","",60,1005.54,60332.4]
[null,"","","(30\", 0.312\")","",364,350,127400]
[null,"","","(30\", 0.375\")","",102,130.15,13275.3]
[null,"","","(30\", 0.469\")","",290,516,149640]
[null,"","","(30\", 0.500\")","",592,480.89189189189199,284688]
[null,"","","(36\", 0.312\")","",106,400,42400]
[null,"","","(36\", 0.375\")","",96,589,56544]
[null,"","","(36\", 0.500\")","",406,860.46896551724103,349350.40000000002]
[null,"","","(36\", 0.532\")","",478,623,297794]
[null,"","","(42\", 0.375\")","",114,585,66690]
[null,"","","(42\", 0.500\")","",192,156.18,29986.560000000001]
[null,"","","(42\", 0.625\")","",804,827.34514925373105,665185.5]
[null,"","","(48\", 0.500\")","",198,423.09060606060598,83771.94]
[null,"","","(48\", 0.688\")","",910,868,789880]
[null,"","","(54\", 0.500\")","",122,975,118950]
[null,"","","(54\", 0.750\")","",218,2000,436000]
[null,"","","(54\", 0.781\")","",54,1150,62100]
[null,"","","(60\", 0.844\")","",884,1516.8390950226201,1340885.76]
[null,"","","(60\", 0.875\")","",88,2900,255200]
[null,"","","(66\", 0.875\")","",122,2040,248880]
[null,"","","(66\", 0.938\")","",466,1886,878876]
[null,"","","(72\", 0.625\")","",104,2300,239200]
[null,"","","(72\", 1.000\")","",84,5054,424536]
[null,"","","(84\", 1.000\")","",122,2370,289140]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\", 0.250\")","",95,0.37473684210525998,35.6]
[null,"","","(16\", 0.281\")","",318,0.01,3.18]
[null,"","","(18\", 0.250\")","",482,0.16609958506224001,80.06]
[null,"","","(18\", 0.312\")","",258,0.01,2.58]
[null,"","","(18\", 0.500\")","",52,3400,176800]
[null,"","","(20\", 0.500\")","",52,1765.06,91783.12]
[null,"","","(24\", 0.250\")","",46,0.01,0.46]
[null,"","","(24\", 0.375\")","",430,19.6220465116279,8437.48]
[null,"","","(24\", 0.500\")","",152,948.43815789473695,144162.6]
[null,"","","(30\", 0.312\")","",364,0.01,3.64]
[null,"","","(30\", 0.375\")","",102,182.21,18585.419999999998]
[null,"","","(30\", 0.469\")","",290,0.01,2.9]
[null,"","","(30\", 0.500\")","",592,1.0218243243243199,604.91999999999996]
[null,"","","(36\", 0.312\")","",106,0.01,1.06]
[null,"","","(36\", 0.375\")","",96,0.01,0.96]
[null,"","","(36\", 0.500\")","",406,2110.4546798029601,856844.6]
[null,"","","(36\", 0.532\")","",478,0.01,4.78]
[null,"","","(42\", 0.375\")","",114,0.01,1.1399999999999999]
[null,"","","(42\", 0.500\")","",192,208.24,39982.080000000002]
[null,"","","(42\", 0.625\")","",804,1063.135,854760.54]
[null,"","","(48\", 0.500\")","",198,149.873939393939,29675.040000000001]
[null,"","","(48\", 0.688\")","",910,0.01,9.1]
[null,"","","(54\", 0.500\")","",122,0.01,1.22]
[null,"","","(54\", 0.750\")","",218,3800,828400]
[null,"","","(54\", 0.781\")","",54,0.01,0.54]
[null,"","","(60\", 0.844\")","",636,0.01,6.36]
[null,"","","(60\", 0.875\")","",88,5100,448800]
[null,"","","(66\", 0.875\")","",122,2620,319640]
[null,"","","(66\", 0.938\")","",466,0.01,4.66]
[null,"","","(72\", 0.625\")","",104,0.01,1.04]
[null,"","","(72\", 1.000\")","",84,5054,424536]
[null,"","","(84\", 1.000\")","",122,0.01,1.22]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","15\" PIPE REHABILITATION CIPP  LINER","",92,245,22540]
[null,"","","16\" SEALED DIP, CLASS 250","",284,120,34080]
[null,"","","16\" SEALED DUCTILE IRON PIPE  CLASS 250","",880,188.54,165915.20000000001]
[null,"","","18\" DUCTILE IRON PIPE","",112,217,24304]
[null,"","","18\" PIPE REHABILITATION CIPP  LINER","",688,290,199520]
[null,"","","18\" PIPE REHABILITATION SMOOTH","WALL STEEL SLIP LINER",40,400,16000]
[null,"","","18\" SEALED DIP, CLASS 250","",216,150,32400]
[null,"","","24\" DUCTILE IRON PIPE","",202,227,45854]
[null,"","","24\" PIPE REHABILITATION CIPP  LINER","",364,400,145600]
[null,"","","24\" SEALED DUCTILE IRON PIPE  CLASS 200","",170,307.3,52241]
[null,"","","28\" X 20\" CAA PIPE ARCH","CULVERT, 0.135\" THICK",92,250,23000]
[null,"","","30\" DUCTILE IRON PIPE","",104,290,30160]
[null,"","","30\" PIPE REHABILITATION CIPP  LINER","",262,405,106110]
[null,"","","30\" SEALED DUCTILE IRON PIPE  CLASS 150","",120,536.47,64376.4]
[null,"","","35\" X 24\" CORRUGATED ALUMINUM","PIPE ARCH, 0.105\" THICK       (12 GAUGE)",72,225,16200]
[null,"","","36\" DUCTILE IRON PIPE, CLASS","150 (SEALED)",148,330,48840]
[null,"","","36\" PIPE REHABILITATION CIPP  LINER","",176,500,88000]
[null,"","","36\" SEALED DIP, CLASS 150","",704,220,154880]
[null,"","","36\" SEALED DUCTILE IRON PIPE  CLASS 150","",134,767.72,102874.48]
[null,"","","4\" PVC IRRIGATION CONDUIT","",1276,27,34452]
[null,"","","4\" PVC SLEEVE","",950,19.5,18525]
[null,"","","42\" DUCTILE IRON PIPE, CLASS","150 (SEALED)",188,499,93812]
[null,"","","42\" PIPE REHABILITATION","SOLID WALL THERMOPLASTIC SLIP LINER",604,325,196300]
[null,"","","42\" PIPE REHABILITATION CIPP  LINER","",140,850,119000]
[null,"","","42\" PIPE REHABILITATION SMOOTH","WALL STEEL SLIP LINER",88,994,87472]
[null,"","","42\" SEALED DUCTILE IRON PIPE  CLASS 150","",162,808.35,130952.7]
[null,"","","54\" PIPE REHABILITATION CIPP  LINER","",150,414,62100]
[null,"","","57\" X 38\" CORRUGATED ALUMINUM","ALLOY PIPE ARCH CULVERT 0.109\"THICK",348,916,318768]
[null,"","","60\" PIPE REHABILITATION CIPP  LINER","",212,562.76,119305.12]
[null,"","","60\" SEALED DIP, CLASS 150","",580,150,87000]
[null,"","","60\" X 38\" HORIZONTAL ELLIPTI- CAL RCP-IV","",452,1372,620144]
[null,"","","87\" X 63\" CAA PIPE ARCH","CULVERT, 0.135\" THICK",148,825,122100]
[null,"","","PIPE REHABILITATION CIPP LINER","(15\" ID HOST PIPE)",258,164,42312]
[null,"","","","(18\" ID HOST PIPE)",650,169,109850]
[null,"","","","(24\" ID HOST PIPE)",550,185,101750]
[null,"","","","(8\" ID HOST PIPE)",404,72,29088]
[null,"","","PRE INSTALLATION INSPECTION","",300,23.3966666666667,7019]
[null,"","","PRE-INSTALLATION INSPECTION","",2522,50,126100]
[null,"","","PREINSTALLATION INSPECTION","",1862,7,13034]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","18\" DUCTILE IRON PIPE ELBOW","",2,1477,2954]
[null,"","","24\" DUCTILE IRON PIPE ELBOW","",4,1983,7932]
[null,"","","30\" DUCTILE IRON PIPE ELBOW","",2,3027,6054]
[null,"","","ALUMINUM HEADWALL, 0.150\"","THICK (CONTRACTOR DESIGNED)",6,51500,309000]
[null,"","","BOOTS FOR SEALED DRAINAGE","STRUCTURES",9,725,6525]
[null,"","","BOOTS FOR SEALED DRAINAGE     STRUCTURES","",26,312.5,8125]
[null,"","","DE-WATERING","",2,11262.565000000001,22525.13]
[null,"","","REMOVE AND REPLACE FLARED END SECTION","",12,2650,31800]
[null,"","","STANDARD CAST IRON MANHOLE","FRAME AND VENTED MANHOLE GRATE",35,500,17500]
[null,"0995000000-E","PIPE REMOVAL","","",116756,26.029266076261599,3039072.99]
[null,"0996000000-N","PIPE CLEAN OUT","","",88,2387.3638636363598,210088.02]
[null,"1000000000-E","6\" SLOPE PROTECTION","","",786,119.656488549618,94050]
[null,"1011000000-N","FINE GRADING","","",16,2237571.8768750001,35801150.030000001]
[null,"1022000000-E","SEALING PVMT CRACKS","","",73440,3.5,257040]
[null,"1044000000-E","LIME TRTD SOIL (SLURRY)","","",249460,3.61713701595446,902331]
[null,"1066000000-E","LIME FOR LIME TREATED SOIL","","",3000,264.756666666667,794270]
[null,"1077000000-E","#57 STONE","","",4016,60.499950199203198,242967.8]
[null,"1099500000-E","SHALLOW UNDERCUT","","",269501,11.9934137535668,3232237]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",578453,28.445820922356699,16454570.449999999]
[null,"1110000000-E","STABILIZER AGGREGATE","","",3000,38.979999999999997,116940]
[null,"1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",105200,53.196482889733801,5596270]
[null,"1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",348688,4.2067756848529303,1466852.2]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",284774,38.8469916495186,11062613.199999999]
[null,"1165000000-E","PORT CEM FOR CEM TRTD BASE CRSE","","",315,215,67725]
[null,"1176000000-E","SOIL CEMENT BASE","","",249460,3.5467417622063699,884770.2]
[null,"1187000000-E","PC FOR SOIL CEMENT BASE","","",11653,205.52312537544,2394960.98]
[null,"1209000000-E","ASPHALT CURING SEAL","","",74850,2.7476272545090201,205659.9]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",73088,47.119977834938702,3443904.94]
[null,"1231000000-E","SHOULDER BORROW","","",62987,13.396198739422401,843786.37]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",804.95,2877.5037952667899,2316246.6800000002]
[null,"1260000000-E","AGGREGATE SHOULDER BORROW","(ASB)","",107,30,3210]
[null,"","","","",106319.25,20.172328059123799,2144706.79]
[null,"1264000000-E","DITCHING","","",15,21,315]
[null,"1275000000-E","PRIME COAT","","",61790,5.7266065706424998,353847.02]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",245,17,4165]
[null,"","","(1-1/2\")","",6696865,1.6403975546767,10985520.970000001]
[null,"","","(1-1/4\")","",151248,1.85951939860362,281248.59000000003]
[null,"","","(2\")","",1861106,1.96685325822387,3660522.4]
[null,"","","(2-1/2\")","",351930,2.3452938084278099,825379.25]
[null,"","","(2-3/4\")","",264940,1.7875179285875999,473585]
[null,"","","(3\")","",189851,3.1617731800201199,600265.80000000005]
[null,"","","(3-1/2\")","",2322,3.5,8127]
[null,"","","(3/4\")","",3540,28,99120]
[null,"","","(4\")","",150528,5.1954663584183702,782063.16]
[null,"","","(4-1/2\")","",21589,6.5,140328.5]
[null,"","","(5-1/4\")","",99218,8.5,843353]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1\")","",380,7.85,2983]
[null,"","","(0\" TO 1\"-1/2\")","",607,8.61,5226.2700000000004]
[null,"","","(0\" TO 1-1/2\")","",157356,2.99658341594855,471530.38]
[null,"","","(0\" TO 1-1/4\")","",1953,11.105222734254999,21688.5]
[null,"","","(0\" TO 2\")","",570,24,13680]
[null,"","","(0\" TO 2-1/2\")","",2000,4.8,9600]
[null,"","","(0\" TO 3\")","",59197,4.2641628798756699,252425.65]
[null,"","","(0\" TO 4-3/4\")","",640,6,3840]
[null,"","","(1-1/2\" TO 3\")","",29395,1.95,57320.25]
[null,"","","(2-1/2\" TO 4\")","",24800,2.6,64480]
[null,"","","(3/4\" TO 2-3/4\")","",525,12.95,6798.75]
[null,"1330000000-E","INCIDENTAL MILLING","","",516427.2,6.9636445756536398,3596215.47]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",1182050,55.443575948563897,65537078.950000003]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",815793,61.5459554078057,50208759.600000001]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",1158035,50.083532000328098,57998482.979999997]
[null,"1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",4845,73.242487100103205,354859.85]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",900139,58.122984883445802,52318765.490000002]
[null,"1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",9072,54.333815035273403,492916.37]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",543415,62.277889826375798,33842739.5]
[null,"1526000000-E","ASP CONC SURF CRS S4.75A","","",4154,55.808979297063097,231830.5]
[null,"1575000000-E","ASP FOR PLANT MIX","","",226384.5,483.99725096020302,109569475.66]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",36530,662.46405693950203,24199812]
[null,"1662000000-E","OG ASP FRICT FC-1 MOD","","",64761,83.378684702212794,5399687]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",28501.599999999999,193.167785317316,5505590.9500000002]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",139576,112.91919807130201,15760809.99]
[null,"1735000000-E","REP JNT CONC PVT SLABS","","",3520,471.44176136363598,1659475]
[null,"1736000000-E","SELECT MATERIAL, CLASS IV","","",4543,52.362645828747503,237883.5]
[null,"1737000000-E","PATCHING CONC PVMT SPALLS","","",1000,95,95000]
[null,"1775000000-E","AST, MAT COAT, #78M STONE","","",724799,0.48445942944182002,351135.71]
[null,"1775500000-E","AST, MAT COAT, #*** STONE","(67)","",226531,0.34772304894252998,78770.05]
[null,"","","(67)","",216189,0.77736767365591997,168058.34]
[null,"","","(67M)","",146731,1.24,181946.44]
[null,"","","(78M)","",54505,0.65,35428.25]
[null,"1803500000-E","AST, DOUBLE SEAL","","",676655,0.97888983307594002,662370.69999999995]
[null,"1814500000-E","AST, SINGLE SEAL","","",76279,0.6,45767.4]
[null,"1820000000-E","AST, FOG SEAL","","",381733,0.23202832870095,88572.87]
[null,"1838000000-E","EMULSION FOR AST","","",877538,1.85258792211847,1625716.3]
[null,"1838500000-N","VACUUM TRUCK","","",46,2068.1739130434798,95136]
[null,"1839140000-E","ULTRATHIN BOND WEAR CRS","","",34147,111.478753624037,3806665]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",2316986,0.22705584755368,526085.22]
[null,"1847000000-E","******\"PCC PVMT THRU LNS","(11\")","",6381,121,772101]
[null,"","","(12\")","",132215,73.42,9707225.3000000007]
[null,"1858000000-E","******\"PCC PVMT RAMPS","(11\")","",2836,212,601232]
[null,"","","(12\")","",9980,75.87,757182.6]
[null,"1869000000-E","******\"PCC PVMT MISC","(12\")","",3470,91.04,315908.8]
[null,"1880000000-E","GENERIC PAVING ITEM (TON)","PATCHING EXISTING PAVEMENT    (MILL)","",1894,125,236750]
[null,"","","SELECT MATERIAL, CLASS IV","",549,50,27450]
[null,"1881000000-E","GENERIC PAVING ITEM (LF)","12\" MILLED RUMBLE STRIPS","(ASPHALT CONCRETE)",33317,0.18,5997.06]
[null,"","","JOINT CONSTRUCTION, REPAIR ANDSEALING","",119664,2.9994885679903698,358930.8]
[null,"","","MILLED RUMBLE STRIPS (ASPHALT","CONCRETE)(12\")",106260,0.1,10626]
[null,"","","","CONCRETE)(8\")",9700,0.1,970]
[null,"1882000000-E","GENERIC PAVING ITEM (GAL)","STRUCTURAL FOAM VOID FILL/","STABILIZATION",400,150,60000]
[null,"1890000000-N","GENERIC PAVING ITEM (EA)","PRECAST CONCRETE PARKING CURB","",19,300,5700]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","11\" CONCRETE TRUCK APRON","",1571,76.5,120181.5]
[null,"","","12\" CONCRETE TRUCK APRON","",1755,105,184275]
[null,"","","4\" CONCRETE PAD FOR PIPES","UNDER FENCE",30,111,3330]
[null,"","","7\" CONCRETE TRUCK APRON","",3210,95.392523364485996,306210]
[null,"","","7\" JOINTED CONCRETE TRUCK","APRON",380,90.77,34492.6]
[null,"","","8\" CONTINUOUSLY REINFORCED","CONCRETE PAVEMENT REPAIR",817,650,531050]
[null,"","","DIAMOND GRINDING PCC PAVEMENT","",53730,5.6806607109622203,305221.90000000002]
[null,"","","FINE MILLING 5/8\" DEPTH","",43591,11,479501]
[null,"","","LATEX MODIFIED MICROSURFACING,","TYPE III",68228,2.93,199908.04]
[null,"","","LATEX MODIFIED MICROSURFACING,TYPE III","",140119,2.29,320872.51]
[null,"","","MULTI-USE PATH REPAIR","",15,112.25,1683.75]
[null,"1913000000-E","CONC SHLD ADJ ******\"PVMT","(12\")","",75440,64.56,4870406.4000000004]
[null,"1924000000-N","FIELD LAB RENTAL, PCCP","","",1,925000,925000]
[null,"1925000000-E","MILL RUMBLE STRPS (CONC SHLDR)","","",71241,2.4166056063222001,172161.4]
[null,"2000000000-N","RIGHT-OF-WAY MARKERS","","",1000,309.85115000000002,309851.15000000002]
[null,"2020000000-N","CONTROL-OF-ACCESS MARKERS","","",24,321.33333333333297,7712]
[null,"2021000000-N","GENERIC GRADING ITEM (EA)","RIGHT OF WAY MARKERS","",14,315,4410]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",49007.199999999997,26.8175190584241,1314251.52]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",145049.5,7.3413989706962104,1064866.25]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",2907.2,58.899559713814,171232.8]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",24378.7,67.579315139855694,1647495.85]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",162349.5,14.7409246717729,2393181.75]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",351,423.95501424501401,148808.21]
[null,"2077000000-E","6\" OUTLET PIPE","","",2106,39.343361823361803,82857.119999999995]
[null,"2099000000-E","SHOULDER DRAIN","","",152520,12.842225281930199,1958696.2]
[null,"2110000000-E","4\" SHOULDER DRAIN PIPE","","",152552,2.4340631391263301,371321.2]
[null,"2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",7686,15.993832943013301,122928.6]
[null,"2132000000-N","CONC PAD SHLDR DRN OUTLET","","",272,393.56764705882398,107050.4]
[null,"2143000000-E","BLOTTING SAND","","",145,60.615172413793097,8789.2000000000007]
[null,"2190000000-N","TEMP STL PLT COVER FOR MDS","","",108,1888.5185185185201,203960]
[null,"2209000000-E","ENDWALLS","","",805.66399999999999,1615.1405921078799,1301260.6299999999]
[null,"2220000000-E","REINFORCED ENDWALLS","","",541.89,1554.70038199635,842476.59]
[null,"2253000000-E","PIPE COLLARS","","",210.304,1497.1189801430301,314850.11]
[null,"2264000000-E","PIPE PLUGS","","",11.135,1771.4261338122999,19724.830000000002]
[null,"2275000000-E","FLOWABLE FILL","","",3972.7,323.53037480806501,1285289.1200000001]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",3906,3450.98554275474,13479549.529999999]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",663.43600000000004,2651.6061684925098,1759170.99]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",2823.44,574.298943841555,1621498.61]
[null,"2352000000-N","FRAME W/GRATE 840.***** STD","(840.16)","",81,730,59130]
[null,"","","(840.36)","",2,900,1800]
[null,"2354000000-N","FRAME W/GRATE 840.22 STD","","",6,743.506666666667,4461.04]
[null,"2354200000-N","FRAME W/GRATE 840.24 STD","","",4,810,3240]
[null,"2355000000-N","FRAME W/GRATE 840.29 STD","","",5,840,4200]
[null,"2363000000-N","FRAME W/2GRTS 840.***** STD","(840.15)","",6,700,4200]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",366,880.86404371584695,322396.24]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",591,921.69252115059203,544720.28]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",796,995.66982412060304,792553.18]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",109,871.124495412844,94952.57]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",215,733.822,157771.73000000001]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",155,991.05845161290301,153614.06]
[null,"","","(F)","",454,1000.22784140969,454103.44]
[null,"","","(G)","",441,1058.6811337868501,466878.38]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",296,770.18486486486495,227974.72]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",516,2347.7149806201601,1211420.93]
[null,"2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",3,1200,3600]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",272,1322.381875,359687.87]
[null,"2462000000-E","**\" SLUICE GATE","(8\")","",4,2565,10260]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","CONCRETE APRON FOR DROP INLET","",29,2300,66700]
[null,"","","DE-WATERING","",16,3200,51200]
[null,"","","DEWATERING","",2,12882.8,25765.599999999999]
[null,"","","ENERGY DISSIPATOR BASIN","",18,13944.4444444444,251000]
[null,"","","HINGED GRATE","",5,2500,12500]
[null,"","","OUTLET CONTROL STUCTURE","",2,52060.47,104120.94]
[null,"","","REMOVE AND REPLACE CONCRETE   APRON","",8,1500,12000]
[null,"","","SEALED PRECAST DRAINAGE       STRUCTURE","",5,3000,15000]
[null,"","","SEALED PRECAST DRAINAGE STRUC-TURE","",13,3020.88,39271.440000000002]
[null,"","","SEALED PRECAST DRAINAGE STRUC-TURES","",4,7950,31800]
[null,"","","SPECIAL DESIGN PIPE CONNECTION","",85,1800,153000]
[null,"","","TRASH GRATE FOR 24\" RCP FES","",1,10673.77,10673.77]
[null,"2484000000-E","GENERIC DRAINAGE ITEM (LF)","84\" PIPE REHABILITATION","",123,968.67,119146.41]
[null,"","","CONCRETE FLUME WITH GRATE","",100,82,8200]
[null,"","","PRE-INSTALLATION INSPECTION","",123,50,6150]
[null,"","","SEALED PRECAST DRAINAGE       STRUCTURE","",9.3000000000000007,650,6045]
[null,"","","SEALED PRECAST DRAINAGE STRUC-TURE","",17,364.59,6198.03]
[null,"","","SEALED PRECAST DRAINAGE STRUC-TURES","",4,625,2500]
[null,"2495000000-E","GENERIC DRAINAGE ITEM (CY)","SEALED PRECAST DRAINAGE       STRUCTURE","",25.1,2000,50200]
[null,"2529000000-E","GENERIC GRADING ITEM (SF)","ARTIFICIAL TURF","",9705,8,77640]
[null,"2535000000-E","**\"X**\" CONCRETE CURB","(8\" X 12\")","",750,22.292000000000002,16719]
[null,"","","(8\" X 18\")","",3815,25.339449541284399,96670]
[null,"","","(9\" X 12\")","",340,31,10540]
[null,"","","(9\" X 18\")","",1740,19.215517241379299,33435]
[null,"2538000000-E","**'-**\" CONCRETE CURB & GUTTER","(2'-9\")","",11070,35.292140921409199,390684]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",82395,20.168450755506999,1661779.5]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",179443,31.944085308426601,5732142.5]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",59235.5,37.9441458247166,2247640.4500000002]
[null,"2570000000-N","MODIFIED CONCRETE FLUME","","",2,2750,5500]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",13000,51.627576923076901,671158.5]
[null,"2580000000-E","CONCRETE VALLEY GUTTER","","",670,18,12060]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",49963,53.688947821387799,2682460.9]
[null,"2600000000-N","RETROFIT EXT CURB RAMPS","","",378,931.35317460317503,352051.5]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",540,2529.6796296296302,1366027]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",13004,94.540145339895403,1229400.05]
[null,"2613000000-N","REM & REP CURB RAMPS","","",716,2539.4553072625699,1818250]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",10287,117.482613978808,1208543.6499999999]
[null,"2627000000-E","4\" CONC ISLAND COVER","","",9321,57.763705610986001,538415.5]
[null,"2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",15510,73.481463571889094,1139697.5]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",31080,87.053088803088798,2705610]
[null,"2657000000-E","**\" MONO CONC MEDIAN (*****)","(8\", NON-MOUNTABLE)","",20,407.09,8141.8]
[null,"2703000000-E","CONC BARRIER TYPE ******","(III)","",3700,161.87027027027,598920]
[null,"","","(IV)","",1500,114.84,172260]
[null,"","","(SINGLE SLOPE)","",4157,191.333894635554,795375]
[null,"","","(T)","",58116,122.26730160368901,7105686.5]
[null,"","","(T1)","",20296,138.796437721719,2817012.5]
[null,"","","(T2)","",4891,340.814250664486,1666922.5]
[null,"","","(TI)","",809,193,156137]
[null,"2710000000-N","CONC BARRIER TRANS SECTN","","",24,22683.480416666702,544403.53]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",31519,96.746825724166399,3049363.2]
[null,"2738000000-E","GENERIC PAVING ITEM (SY)","12\" CONCRETE TRUCK APRON","",1715,120.37900874635601,206450]
[null,"","","6\" CONCRETE DRIVEWAY","",1915,224,428960]
[null,"","","6\" CONCRETE PAVED DITCH","",1220,175,213500]
[null,"","","9\" JOINTED CONCRETE TRUCK","APRON",1000,95,95000]
[null,"","","FILL AND CAP BEHIND BARRIER","",270,192,51840]
[null,"","","REMOVE AND REPLACE DRIVEWAY","APRON",1,100,100]
[null,"","","REMOVE AND REPLACE DRIVEWAY   APRON","",225,125,28125]
[null,"","","REMOVE CONCRETE ISLAND","",3,100,300]
[null,"","","REMOVE CONCRETE SIDEWALK","",64,43.90625,2810]
[null,"","","REMOVE SIDEWALK","",25,37,925]
[null,"2738100000-E","GENERIC PAVING ITEM (SF)","PERMEABLE PAVERS","",13104,5,65520]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","1'-6\" CONCRETE CURB & GUTTER","(11\" DEPTH)",1370,21.95,30071.5]
[null,"","","2\" ROLLED CONCRETE CURB","",720,16,11520]
[null,"","","2'-0\" MODIFIED VALLEY GUTTER","",590,70.4398305084746,41559.5]
[null,"","","2'-6\" CONCRETE CURB & GUTTER","(11\" THICK)",143,60,8580]
[null,"","","","(TINTED CONCRETE)",170,52.5,8925]
[null,"","","DDI BARRIER","",710,365.48,259490.8]
[null,"","","MEDIAN HAZARD PROTECTION","",1178,208.38285229202,245475]
[null,"","","MODIFIED VALLEY GUTTER","",1100,27,29700]
[null,"","","REMOVE 2'-6\" CURB AND GUTTER","",115,30,3450]
[null,"","","REMOVE AND REPLACE 2'-6\" CURB AND GUTTER","",869,68.273878020713497,59330]
[null,"2759000000-N","GENERIC PAVING ITEM (EA)","EMERGENCY VEHICLE ACCESS FOR","CONCRETE ISLAND",2,10000,20000]
[null,"","","MEDIAN HAZARD PROTECTION","",4,51624.37,206497.48]
[null,"","","REMOVE CURB RAMP","",123,974.47154471544695,119860]
[null,"","","REMOVE CURB RAMPS","",47,879.787234042553,41350]
[null,"","","VERTICAL CONCRETE BARRIER     TRANSITION","",2,5710,11420]
[null,"2766000000-N","GENERIC PAVING ITEM (LS)","42\" CONCRETE BARRIER WITH","MOMENT SLAB",1,323640.58,323640.58]
[null,"2800000000-N","ADJ CATCH BASINS","","",22,1773.17227272727,39009.79]
[null,"2815000000-N","ADJ DROP INLETS","","",53,1821.90924528302,96561.19]
[null,"2830000000-N","ADJ MANHOLES","","",1201,758.55693588676104,911026.88]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",1268,663.864589905363,841780.3]
[null,"2860000000-N","CONVERT CB TO JB","","",4,2926.5124999999998,11706.05]
[null,"2875000000-N","CONVERT CB TO DI","","",1,2000,2000]
[null,"2905000000-N","CONVERT DI TO JB","","",25,2772.4036000000001,69310.09]
[null,"2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION   BOX",1,10867,10867]
[null,"","","CONVERT EXISTING DROP INLET TO","TRAFFIC BEARING JUNCTION BOX",1,10867,10867]
[null,"","","CONVERT EXISTING OTCB TO      MEDIAN 2GI","",7,1798.67,12590.69]
[null,"","","REMOVE AND REPLACE DRAINAGE   STRUCTURES","",33,13000,429000]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",21,20253.670476190498,425327.08]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",266598.5,24.352273362378298,6492279.5499999998]
[null,"3045000000-E","SBGR SHOP CURVED","","",7100,25.483645070422501,180933.88]
[null,"3060000000-E","SBGR DOUBLE FACED","","",400,35,14000]
[null,"3105000000-N","SBGR TERM SECT","","",2,76,152]
[null,"3135000000-N","W-TR SBGR TRANS SECTIONS","","",6,250,1500]
[null,"3140000000-E","25' CLR SPAN GR SECTIONS","","",3,2266.6666666666702,6800]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",1058,95.457759924385599,100994.31]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",625,38.733280000000001,24208.3]
[null,"3180000000-N","GR ANCHOR TYPE **********","(B-77 MODIFIED)","",2,2397.5,4795]
[null,"","","(III SHOP CURVED)","",2,2355,4710]
[null,"","","(III, SHOP CURVED)","",2,2800,5600]
[null,"3195000000-N","GR END TYPE AT-1","","",55,793.35636363636399,43634.6]
[null,"3210000000-N","GR END TYPE CAT-1","","",219,944.76255707762596,206903]
[null,"3215000000-N","GR ANCHOR TYPE III","","",172,1866.4613953488399,321031.36]
[null,"3287000000-N","GR END TYPE TL-3","","",517,3103.9514506769801,1604742.9]
[null,"3288000000-N","GR END TYPE TL-2","","",94,2522.4680851063799,237112]
[null,"3289000000-N","GR END TYPE MEDIAN TL-3","","",3,3607,10821]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",276,2200.4610869565199,607327.26]
[null,"3345000000-E","REMOVE & RESET GUARDRAIL","","",10682,5.5249485115147001,59017.5]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",214827.5,1.20992749997091,259925.7]
[null,"3365000000-E","REMOVE EXISTING GUIDERAIL","","",37090,1.65678080345106,61450]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",22749.5,7.9600268137761301,181086.63]
[null,"3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",781.25,14.3248,11191.25]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",24,1469.5833333333301,35270]
[null,"","","(III MOD)","",2,1800,3600]
[null,"","","(III MODIFIED)","",1,2360,2360]
[null,"","","(III)","",12,1030,12360]
[null,"","","(THRIE-BEAM)","",2,2300,4600]
[null,"","","(W-BEAM)","",1,1680,1680]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(AT-1)","",10,600,6000]
[null,"","","(TL-2)","",18,2281.1111111111099,41060]
[null,"","","(TL-3)","",45,2186.55044444444,98394.77]
[null,"3389200000-E","CABLE GUIDERAIL","","",7400,7.9560810810810798,58875]
[null,"3389400000-E","DBL FACED CABLE GUIDERAIL","","",35415,9.4749399971763406,335555]
[null,"3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",47,90.138297872340402,4236.5]
[null,"3389600000-N","CBL GUIDERAIL ANCH UNIT","","",85,1881.4117647058799,159920]
[null,"3420000000-E","GENERIC GUARDRAIL ITEM (LF)","POWDER COATED GALVANIZED","STEEL BEAM GUARDRAIL",1925,45,86625]
[null,"","","","STEEL BEAM GUARDRAIL, SHOP    CURVED",162.5,47,7637.5]
[null,"","","REMOVE AND REPLACE EXISTING   GUARDRAIL","",325,30,9750]
[null,"","","REMOVE AND TRANSPORT EXISTING","GUARDRAIL",350,10,3500]
[null,"","","REMOVE, STOCKPILE, AND DELIVER","EXISTING GUARDRAIL",530,5,2650]
[null,"3435000000-N","GENERIC GUARDRAIL ITEM (EA)","GUARDRAIL PRE-FAB POSTS","",4,550,2200]
[null,"","","PERMANENT BOLLARDS","",6,500,3000]
[null,"","","POWDER COATED GALVANIZED","25' CLEAR SPAN GUARDRAIL      SECTIONS",1,4170,4170]
[null,"","","","ADDITIONAL GUARDRAIL POSTS",10,90,900]
[null,"","","","GUARDRAIL ANCHOR UNITS,       TYPE III",1,3315,3315]
[null,"","","","GUARDRAIL END UNITS, TYPE AT-1",3,1145,3435]
[null,"","","","GUARDRAIL END UNITS, TYPE TL-2",4,4175,16700]
[null,"","","REMOVABLE BOLLARDS","",3,1060,3180]
[null,"","","TEMPORARY GUARDRAIL END UNITS,TYPE TL-3","",2,3750,7500]
[null,"","","TEMPORARY IMPACT ATTENUATOR","UNITS, TYPE TL-3",1,32666.77,32666.77]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNIT","TYPE AT-1",2,311,622]
[null,"","","TEMPORARY GUARDRAIL END UNITS,","TYPE CAT-1",2,275,550]
[null,"","","TEMPORARY GUARDRAIL END UNITS,TYPE AT-1","",3,396.48333333333301,1189.45]
[null,"","","TEMPORARY GUARDRAIL END UNITS,TYPE CAT-1","",2,500,1000]
[null,"3500000000-E","WOVEN WIRE FENCE **\" FAB","(48\")","",220,8.5,1870]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",291445,3.4918852613700699,1017692.5]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",18143,21.387904425949401,388040.75]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",5011,30.977250049890198,155227]
[null,"3533000000-E","CHN LK FENCE **\" FABRIC","(60\")","",9460,14.5,137170]
[null,"3536000000-E","CHN LK FENCE 48\" FABRIC","","",15390,6.3116959064327496,97137]
[null,"3539000000-E","MET LINE PST **\" CL FEN","(60\")","",946,75,70950]
[null,"3542000000-E","MET LINE PST 48\" CL FEN","","",1287,69.342657342657304,89244]
[null,"3545000000-E","MET TERM PST **\" CL FEN","(60\")","",237,250,59250]
[null,"3548000000-E","MET TERM PST 48\" CL FEN","","",88,124.545454545455,10960]
[null,"3557000000-E","ADDITIONAL BARBED WIRE","","",410,1,410]
[null,"3559000000-E","** STRAND BW FENCE W/ POSTS","(4)","",500,10,5000]
[null,"","","(5)","",3430,14.591836734693899,50050]
[null,"","","(6)","",200,15,3000]
[null,"3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 12')","",6,3000,18000]
[null,"3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 7'-6\", 15')","",2,1100,2200]
[null,"","","(47\", 8', 16')","",1,2020,2020]
[null,"3566000000-E","WOVEN WIRE FENCE RESET","","",5434,6.5605447184394601,35650]
[null,"3572000000-E","CHAIN LINK FENCE RESET","","",1010,23.980198019802,24220]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","36\" VINYL FENCE RESET","",185,55,10175]
[null,"","","BIKE AND PEDESTRIAN SAFETY    RAIL","",810,170,137700]
[null,"","","ORNAMENTAL WOOD FENCE","",100,140,14000]
[null,"","","PEDESTRIAN SAFETY RAIL","",60,175,10500]
[null,"","","STEEL PIPE HANDRAIL","",50,225,11250]
[null,"","","TEMPORARY 3 STRAND BARBED WIRE","FENCE WITH POSTS",500,5,2500]
[null,"","","WILDLIFE FENCE","",3880,22,85360]
[null,"3578000000-N","GENERIC FENCING ITEM (EA)","RESET EXISTING GATE","",3,1133.3333333333301,3400]
[null,"","","STEEL BOLLARDS","",9,1650,14850]
[null,"","","WILDLIFE DOUBLE GATES 9' HIGH, 6' WIDE,","12' OPENING",1,5550,5550]
[null,"","","WILDLIFE FENCE POST 4\", 13'","",221,53,11713]
[null,"","","WILDLIFE FENCE POST 5\", 13'","",108,139,15012]
[null,"3595000000-E","RELAPPING GUARDRAIL","","",450,4,1800]
[null,"3628000000-E","RIP RAP, CLASS I","","",28932,63.567166113645797,1839125.25]
[null,"3635000000-E","RIP RAP, CLASS II","","",17876,69.779575967778001,1247379.7]
[null,"3642000000-E","RIP RAP, CLASS A","","",3015,93.702155887230504,282512]
[null,"3649000000-E","RIP RAP, CLASS B","","",30381,56.035777624173001,1702422.96]
[null,"3651000000-E","BOULDERS","","",1279,138.193901485536,176750]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",226032,3.49330559389821,789598.85]
[null,"3659000000-N","PREFORMED SCOUR HOLES","","",20,4772.1030000000001,95442.06]
[null,"3678000000-E","GENERIC EROSION CONTROL ITEM (SF)","PRECAST GRAVITY RETAINING     WALLS","",850,75.400000000000006,64090]
[null,"3684000000-E","GENERIC EROSION CONTROL ITEM (TON)","RIP RAP, CLASS A","",375,57.6,21600]
[null,"","","RIP RAP, CLASS B","",375,65.25,24468.75]
[null,"3691000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",15,444,6660]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",15,222,3330]
[null,"3984000000-E","GENERIC WALL ITEM (SF)","TIMBER RETAINING WALL (# 1)","",200,237.5,47500]
[null,"","","TIMBER RETAINING WALL (# 2)","",600,121,72600]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(A)","",1161,31.212144702842402,36237.300000000003]
[null,"","","(B)","",165,34.51,5694.15]
[null,"","","(D)","",597,15.8088777219431,9437.9]
[null,"","","(E)","",1556.6,13.3806372863934,20828.3]
[null,"","","(F)","",462.5,12.259027027027001,5669.8]
[null,"","","(MILEMARKER)","",12,14.86,178.32]
[null,"4048000000-E","REINF CONC FOUNDTN","","",104,875.85,91088.4]
[null,"4054000000-E","PLN CONC FOUNDTN","","",23,585.30565217391302,13462.03]
[null,"4057000000-E","OVERHEAD FOOTING","","",1382,808.85785094066603,1117841.55]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",107379,6.5418339712606697,702455.59]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",20643,6.6016218572881797,136277.28]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",49596,7.7804887490926697,385881.12]
[null,"4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",34,87.631764705882304,2979.48]
[null,"4079000000-N","SUPPORT, BARR SMALL","","",2,500,1000]
[null,"4082000000-E","SUPPORT, WOOD","","",2063,12.326708676684399,25430]
[null,"4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(1019+50 -L-)","",1,40000,40000]
[null,"","","(1034+40 -L-)","",1,47000,47000]
[null,"","","(1044+00 -L-)","",1,49000,49000]
[null,"","","(1060+60 -L-)","",1,47000,47000]
[null,"","","(1070+50 -L-)","",1,48000,48000]
[null,"","","(1087+00 -L-)","",1,43000,43000]
[null,"","","(1117+00 -L-)","",1,40000,40000]
[null,"","","(1136+00 -L-)","",1,43500,43500]
[null,"","","(1141+00 -L-)","",1,44000,44000]
[null,"","","(1162+00 -L-)","",1,41000,41000]
[null,"","","(1167+00 -L-)","",1,44000,44000]
[null,"","","(1188+75 -L-)","",1,48000,48000]
[null,"","","(12+69 -Y2-)","",1,69500,69500]
[null,"","","(1220+56 -L-)","",1,57000,57000]
[null,"","","(1247+00 -L-)","",1,44000,44000]
[null,"","","(1272+50 -L-)","",1,51000,51000]
[null,"","","(1278+50 -L-)","",1,54000,54000]
[null,"","","(1305+00 -L-)","",1,54000,54000]
[null,"","","(1331+50 -L-)","",1,101000,101000]
[null,"","","(1351+00 -L-)","",1,58000,58000]
[null,"","","(1367+00 -L-)","",1,58000,58000]
[null,"","","(1377+00 -L-)","",1,54000,54000]
[null,"","","(1393+50 -L-)","",1,96000,96000]
[null,"","","(155+88 -Y15-)","",1,117938.14,117938.14]
[null,"","","(16+86 -Y1RP-)","",1,200000,200000]
[null,"","","(160+00 -Y15-)","",1,102391.75,102391.75]
[null,"","","(160+85 -Y15-)","",1,102391.75,102391.75]
[null,"","","(17+50 -Y15REV-)","",1,101855.67,101855.67]
[null,"","","(20+87 -Y4-)","",1,192989.69,192989.69]
[null,"","","(23+15 -L-)","",1,139050,139050]
[null,"","","(23+61 -Y2-)","",1,49000,49000]
[null,"","","(233+00 -L-)","",1,51100,51100]
[null,"","","(24+50 -Y15-)","",1,101855.67,101855.67]
[null,"","","(26+00 -Y4-)","",1,160824.74,160824.74]
[null,"","","(26+37 -Y15FLYBD-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(29+41 -Y4-)","",1,84164.95,84164.95]
[null,"","","(30+75 -L-)","",1,103000,103000]
[null,"","","(31+94 -Y4-)","",1,84164.95,84164.95]
[null,"","","(32+00 -Y15-)","",1,92742.27,92742.27]
[null,"","","(32+00 -Y15FLYAC-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(33+50.00 -Y-)","",1,105000,105000]
[null,"","","(34+68 -Y15FLYCA-)","",1,171546.39,171546.39]
[null,"","","(40+24.00 -Y-)","",1,57500,57500]
[null,"","","(42+44.00 -Y-)","",1,47500,47500]
[null,"","","(46+80.00 -Y-)","",1,91000,91000]
[null,"","","(47+00 -Y15FLYAC-)","",1,83628.87,83628.87]
[null,"","","(47+08.00 -L-)","",1,55500,55500]
[null,"","","(49+43 -Y2-)","",1,49000,49000]
[null,"","","(50+46 -Y15-)","",1,160824.74,160824.74]
[null,"","","(52+00 -Y15FLYCA-)","",1,84701.03,84701.03]
[null,"","","(56+00 -Y15REV-)","",1,92206.19,92206.19]
[null,"","","(666+00 -L-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(686+00 -L-)","",1,109896.91,109896.91]
[null,"","","(702+30 -L-)","",1,167793.81,167793.81]
[null,"","","(706+00 -L-)","",1,102927.84,102927.84]
[null,"","","(737+50 -L- EB)","",1,102927.84,102927.84]
[null,"","","(737+50 -L- WB)","",1,134020.62,134020.62]
[null,"","","(757+00 -L-)","",1,92206.19,92206.19]
[null,"","","(76+25 -Y15FLYBD-)","",1,85237.11,85237.11]
[null,"","","(763+84 -L-)","",1,134020.62,134020.62]
[null,"","","(78+18.00 -L-)","",1,75000,75000]
[null,"","","(794+00 -L-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(819+00 -L-)","",1,134020.62,134020.62]
[null,"","","(826+00 -L-)","",1,122226.8,122226.8]
[null,"","","(835+50 -L-)","",1,134020.62,134020.62]
[null,"","","(861+15 -L3-)","",1,204900,204900]
[null,"","","(89+70 -Y15REV-)","",1,112577.32,112577.32]
[null,"","","(91+50 -Y15REV-)","",1,134020.62,134020.62]
[null,"","","(956+67 -L-)","",1,44000,44000]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",197,137.12558375634501,27013.74]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",2584,84.449980650154799,218218.75]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",433,118.40817551963001,51270.74]
[null,"4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",115,416.22513043478301,47865.89]
[null,"","","(B)","",68,229.91441176470599,15634.18]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",160,760.48362499999996,121677.38]
[null,"","","(B)","",76,496.58499999999998,37740.46]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",71,80.454366197183106,5712.26]
[null,"4115000000-N","SIGN ERECTION, OVERLAY (OVRHD)","","",7,585,4095]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",55,779.35199999999998,42864.36]
[null,"","","(B)","",2,300,600]
[null,"","","(D)","",59,208.16949152542401,12282]
[null,"","","(E)","",62,186.41935483871001,11558]
[null,"","","(F)","",11,237.363636363636,2611]
[null,"","","(GM RESTAURANT LOGO SIGNS)","",1,515,515]
[null,"","","(WOOD)","",6,250,1500]
[null,"4138000000-N","DISPOSE SUPPORT, STL BM","","",56,517.58000000000004,28984.48]
[null,"4141000000-N","DISPOSE SUPPORT, WOOD","","",11,25.272727272727298,278]
[null,"4149000000-N","DISPOSE SIGN SYST OVRHD","","",7,8029.2857142857101,56205]
[null,"4151000000-N","STOCKPILE SIGN SYST STL BM","","",4,515,2060]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",118,573.68135593220302,67694.399999999994]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",1603,14.521684341859,23278.26]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",128,16.377656250000001,2096.34]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",109,3.4946788990825701,380.92]
[null,"4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",21,89.047619047619094,1870]
[null,"4236000000-N","DISPOSE SIGN, A & B (GRD MTD)","","",66,63.575757575757599,4196]
[null,"4238000000-N","DISPOSE SIGN, D, E, F","","",104,3.1033653846153801,322.75]
[null,"4238500000-N","DISPOSE SIGN, MILEMKR","","",4,1,4]
[null,"4241000000-N","DISPOSE SIGN, OVERLAY OVRHD","","",3,58,174]
[null,"4251000000-N","DISPOSE LIGHT SYSTEM","","",6,540.83333333333303,3245]
[null,"4263000000-N","DISPOSE WALKWAY","","",4,745,2980]
[null,"4360000000-N","GENERIC SIGNING ITEM (EA)","ADVANCE WARNING FLASHING BEA-","CON ASSEMBLY",3,8610,25830]
[null,"","","CUTTING OF SIGN HANGERS, OVER-HEAD","",4,245,980]
[null,"","","RRFB ASSEMBLY","",4,9380,37520]
[null,"","","VERTICAL PANEL, TYPE 3 OBJECT","MARKERS # OM3-C",19,150,2850]
[null,"","","","MARKERS # OM3-L",44,150,6600]
[null,"4370000000-N","GENERIC SIGNING ITEM (LS)","DISPOSAL OF FLASHER SYSTEM","",1,1600,1600]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",42885.5,7.06906250364342,303160.28000000003]
[null,"4402000000-E","HIGH VISIBILITY STAT SIGNS","","",12445,14.9051619124146,185494.74]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",15581,16.734552981195101,260741.07]
[null,"4407000000-E","HIGH VISIBILITY PORT SIGNS","","",4801,15.4688148302437,74265.78]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",11778,8.2099210392256694,96696.45]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",130769,5.8943269429298999,770795.24]
[null,"4415000000-N","FLASHING ARROW BOARD","","",128,2799.3469531249998,358316.41]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",169,9242.3934911242595,1561964.5]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",1204,75.291528239202705,90651]
[null,"4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",80,4443.0625,355445]
[null,"4424000000-N","WZ PRESENCE LIGHTING","","",248,2062.27419354839,511444]
[null,"4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",8,21175.125,169401]
[null,"4430000000-N","DRUMS","","",12693,52.5261167572678,666714]
[null,"4432000000-N","HIGH VISIBILITY DRUMS","","",6585,55.664236902050099,366549]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",964,128.52230290456399,123895.5]
[null,"4435000000-N","CONES","","",2446,28.4681316434996,69633.05]
[null,"4445000000-E","BARRICADES (TYPE III)","","",13590,36.245415746872702,492575.2]
[null,"4447000000-E","PED CHANNEL DEVICES","","",3672,30.845247821350799,113263.75]
[null,"4455000000-N","FLAGGER","","",9968,432.65273675762398,4312682.4800000004]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",62,108773.21661290299,6743939.4299999997]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",205,9042.6810243902401,1853749.61]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",104,3054.95423076923,317715.24]
[null,"4480000000-N","TMA","","",95,20337.6884210526,1932080.4]
[null,"4485000000-E","PORT CONC BARRIER","","",256379,40.787779849363602,10457130.210000001]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",118454,70.594402046363996,8362189.2999999998]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",310430,7.0380949006217204,2184835.7999999998]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",40186,14.1600557408053,569036]
[null,"4507000000-E","WATER FILLED BARRIER","","",10124,56.581884630580802,572835]
[null,"4508000000-E","REM & RES H2O FILL BARR","","",6700,7.2067164179104504,48285]
[null,"4510000000-N","LAW ENFORCEMENT","","",37225,61.291745601074602,2281585.23]
[null,"4516000000-N","SKINNY DRUM","","",3325,45.161112781954898,150160.70000000001]
[null,"4520000000-N","TUBULAR MARKERS (FIXED)","","",94,83.829787234042598,7880]
[null,"4570000000-E","TEMPORARY GLARE SCREEN","","",14445,19.371973001038398,279828.15000000002]
[null,"4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","DYNAMIC ZIPPER MERGE SYSTEM","DEPLOYMENT",1,50000,50000]
[null,"","","DYNAMIC ZIPPER MERGE SYSTEM   DEPLOYMENT","",3,17690.333333333299,53071]
[null,"","","PROTECTIVE CANOPY","",1,5000,5000]
[null,"","","TRAFFIC CONTROL","",1,800000,800000]
[null,"4595000000-E","GENERIC TRAFFIC CONTROL ITEM (SF)","TEMPORARY TYPE A AND B SIGNS","",405,47,19035]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICE","",43,183.37209302325601,7885]
[null,"","","AUDIBLE WARNING DEVICES","",87,296.41379310344797,25788]
[null,"","","CONNECTED LANE CLOSURE DEVICE","",42,1944.3333333333301,81662]
[null,"","","CONNECTED LANE CLOSURE DEVICES","",2,2400,4800]
[null,"","","COVER AND RELOCATE GROUND","MOUNTED GUIDE SIGNS",1,1000,1000]
[null,"","","DOUBLE LANE CLOSURE","",150,2000,300000]
[null,"","","DYNAMIC ZIPPER MERGE SYSTEM","RELOCATION",3,2500,7500]
[null,"","","FLASHING BEACON AND DETECTION SYSTEM","",2,38496,76992]
[null,"","","HIGH VISIBILITY SKINNY DRUMS","",100,90,9000]
[null,"","","INTERSTATE LANE CLOSURE","",612,1800,1101600]
[null,"","","PEDESTRIAN TRANSPORT SERVICE  (PER TRIP)","",1804,17.641352549889099,31825]
[null,"","","PORTABLE CCTV CAMERA ASSEMBLY","",16,21821,349136]
[null,"","","PORTABLE FLASHING BEACONS &","DETECTION SYSTEM",2,16500,33000]
[null,"","","RAMP / LOOP CLOSURE DETOUR    (TYPE A)","",80,1000,80000]
[null,"","","RAMP / LOOP CLOSURE DETOUR    (TYPE B)","",8,1000,8000]
[null,"","","RAMP/LOOP CLOSURE","",140,1341.24285714286,187774]
[null,"","","RAMP/LOOP CLOSURES","",32,1043.25,33384]
[null,"","","RAMP/LOOP TRAFFIC CONTROL","",30,1663.86666666667,49916]
[null,"","","SIGNS, COVERING","",7,1057.5085714285699,7402.56]
[null,"","","SINGLE LANE CLOSURE","",669,1729.7458893871501,1157200]
[null,"","","SOLAR-POWERED FLASHING BEACON","",3,5000,15000]
[null,"","","STREET LANE CLOSURE","",62,1300,80600]
[null,"","","TEMPORARY CURB RAMPS","",16,1674.6875,26795]
[null,"","","TRIPLE LANE CLOSURE","",50,2200,110000]
[null,"","","WARNING FLAGS","",8,17.600000000000001,140.80000000000001]
[null,"4609000000-N","GENERIC TRAFFIC CONTROL ITEM (DAY)","DYNAMIC ZIPPER MERGE SYSTEM","",667,157.27136431784101,104900]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",34944,5.4802770146520103,191502.8]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",12408331,0.53136153685777998,6593309.8300000001]
[null,"4687000000-E","THERMO PVT MKG LINES 4\"240","","",220,1.21,266.2]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",3126323,0.86140029677036001,2693015.56]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",178674,2.24414744170948,400970.8]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",136442,2.33889667404465,319123.74]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",1947,96.856445814072899,188579.5]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",8712,130.02654958677701,1132791.3]
[null,"4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",204,328.553921568627,67025]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",36894,2.7920003252561401,103008.06]
[null,"","","(IV)","",28061,2.6294679448344702,73785.5]
[null,"4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",5252,6.6762185833967997,35063.5]
[null,"","","(IV)","",1948,7.8782854209445601,15346.9]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",1580,6.3264556962025296,9995.7999999999993]
[null,"","","(IV)","",642,6.3037383177570101,4047]
[null,"4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",227,11.9165198237885,2705.05]
[null,"","","(IV)","",1632,13.2,21542.400000000001]
[null,"4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",436,25.2385321100917,11004]
[null,"","","(IV)","",80,28.35,2268]
[null,"4800000000-N","COLD APP PLAS CHAR TYPE *","(II)","",52,103.605769230769,5387.5]
[null,"","","(IV)","",24,115,2760]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(I)","",2,1410,2820]
[null,"","","(II)","",111,253.66621621621599,28156.95]
[null,"","","(IV)","",15,218.2,3273]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",10950512,0.17462526866323999,1912236.1]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",4095147,0.25706549484059998,1052720.99]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",213331,0.55194509939951997,117747]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",234967,0.83004847489222,195034]
[null,"4830000000-E","PAINT PVT MKGS LINES 16\"","","",2057,1.8107438016528901,3724.7]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",56884,2.5234505309049999,143543.96]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",1157,40.774330164217801,47175.9]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",7276,37.251010170423299,271038.34999999998]
[null,"4847400000-E","WZ PERF PVMT MKG LINES 4\"","","",854425,0.35444521169206999,302846.84999999998]
[null,"4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",2131687,0.62442410166219997,1331076.74]
[null,"4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",119613,1.05997675837911,126787]
[null,"4848000000-E","WZ TRAF PATTERN MASKING","","",86280,0.65,56082]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",698903,0.62781307277262,438780.44]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",1199215,0.44229564340006,530407.56999999995]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",15619,1.34550547410206,21015.45]
[null,"4865000000-E","LINE REMOVAL 12\" WIDE","","",65836,0.95616167446382005,62949.86]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",4181,4.5504113848361598,19025.27]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",579,56.735751295336797,32850]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","CONTRAST COLD APPLIED PLASTIC","PAVEMENT MARKING LINES, TYPE  II (9\")",2873,9,25857]
[null,"","","HOT SPRAY PLASTIC PAVEMENT","MARKING LINES (4\", 50 MILS)",3210,0.72,2311.1999999999998]
[null,"","","HOT SPRAY THERMOPLASTIC","PAVEMENT MARKING LINES, 4\", 50 MILS",186560,0.56000000000000005,104473.60000000001]
[null,"","","HOT SPRAY THERMOPLASTIC       PAVEMENT","MARKING LINES (4\", 50 MILS)",431715,0.24028317292658,103733.85]
[null,"","","","MARKING LINES (6\", 50 MILS)",616,0.5,308]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES (4\",       50 MILS)",341150,0.24091836435586,82189.3]
[null,"","","","MENT MARKING LINES (6\",       50 MILS)",570,0.34,193.8]
[null,"","","","MENT MARKING LINES(4\", 50MILS)",2914,1.5,4371]
[null,"","","","MENT MARKING LINES, (4\",      50 MILS)",19801,1.0104984596737501,20008.88]
[null,"","","","MENT MARKING LINES, 4\",       50 MILS",1300,1,1300]
[null,"","","","MENT MARKING LINES, 4\",       50MILS",2764,1.5,4146]
[null,"","","HOT SPRAY THERMOPLASTIC PAVEM-","ENT MARKING LINES (4\", 50MILS)",192780,0.72,138801.60000000001]
[null,"","","","ENT MARKING LINES, 4\", 50 MIL",531374,0.28075524959821002,149186.04]
[null,"","","","ENT MARKING LINES, 4\", 50 MILS",337133,0.3,101139.9]
[null,"","","POLYUREA  PAVEMENT MARKING    LINES,","12\", 20 MILS (STANDARD GLASS  BEADS)",100,11,1100]
[null,"","","POLYUREA  PAVEMENT MARKING    LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",6646,2.6508877520312999,17617.8]
[null,"","","POLYUREA  PAVEMENT MARKING    LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",1450,3.55,5147.5]
[null,"","","POLYUREA PAVEMENT MARKING     LINES","(4\", 20 MILS) (STANDARD GLASS BEADS)",1710,3.8888888888888902,6650]
[null,"","","","(6\", 20 MILS) (STANDARD GLASS BEADS)",1440,2.58,3715.2]
[null,"","","POLYUREA PAVEMENT MARKING     LINES,","(4\", 20MILS) (STANDARD GLASS  BEADS)",21440,1,21440]
[null,"","","","12\", 20 MILS (STD GLASS BEADS)",256,8,2048]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 12\"","20 MILS (STANDARD GLASS BEADS)",12474,2.1580808080808098,26919.9]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",23680,2.1235929054054101,50286.68]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\"","20 MILS (STANDARD GLASS BEADS)",29895,3.3689780899816002,100715.6]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",137859,1.7464659543446599,240766.05]
[null,"","","","20 MILS (STANDARD GLASSBEADS)",800,4.0999999999999996,3280]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",4479,2.15,9629.85]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\"","20 MILS (STANDARD GLASS BEADS)",28514,1.05591989899698,30108.5]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",226718,1.0251592727529399,232422.06]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",189693,1.6333679682434199,309838.46999999997]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 8\"","20 MILS (STANDARD GLASS BEADS)",245,15,3675]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 8\",","20 MILS (STANDARD GLASS BEADS)",1844,3.25,5993]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",124,14.15,1754.6]
[null,"","","POLYUREA PAVEMENT MARKING     LINES,12\",","20 MILS (STANDARD GLASS BEADS)",2025,1.55,3138.75]
[null,"","","THERMOPLASTIC PAVEMENT MARKING","LINES (4\", 90 MILS) (HRM)",10740,1.95,20943]
[null,"","","WORK ZONE PERFORMANCE PAVEMENT","MARKING LINES, 24\"",5755,1.02,5870.1]
[null,"","","","MARKING LINES, 8\"",2722,1.02,2776.44]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",3249,8.6243336411203408,28020.46]
[null,"","","","LINES (16\", 90MILS)",230,6.3478260869565197,1460]
[null,"","","","LINES (24\", 90 MILS)",71547,10.0441685884803,718630.13]
[null,"","","","LINES (24\", 90MILS)",1879,8.5293773283661505,16026.7]
[null,"","","","LINES (24', 90 MILS)",1127,8.5,9579.5]
[null,"","","THERMOPLASTIC PAVMENT MARKING","LINES (24\", 90 MILS)",2122,11.329877474081099,24042]
[null,"4892000000-N","GENERIC PVMT MARKING ITEM (EA) 1205","HEATED-IN-PLACE THERMOPLASTIC PAVE-","MENT MARKING CHARACTER (90    MILS)",78,175,13650]
[null,"","","THERMOPLASTIC PAVEMENT MARKING","CHARACTER (90 MILS)",20,80,1600]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","IN LANE ROUTE SHIELDS","",6,2000,12000]
[null,"","","NON-CAST IRON SNOW-","PLOWABLE PAVEMENT MARKER",992,40,39680]
[null,"","","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",45675,39.122456486042701,1786918.2]
[null,"","","","PAVEMENT MARKERS",22956,34.4342132775745,790471.8]
[null,"","","","PAVMENT MARKER",445,64,28480]
[null,"","","WORK ZONE PERFORMANCE PAVEMENT","MARKING CHARACTER",560,15.5,8680]
[null,"","","","MARKING SYMBOL",303,15.5,4696.5]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",15086,5.8237306111626701,87856.8]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",12085,32.2288374017377,389485.5]
[null,"4915000000-E","7' U-CHANNEL POSTS","","",137,65.014598540145997,8907]
[null,"4940000000-N","FLEX DELINATR (YELLOW)","","",20,55,1100]
[null,"4955000000-N","OBJECT MARKERS (END OF RD)","","",63,111.97619047619,7054.5]
[null,"4957000000-N","OBJECT MARKERS (TYPE **)","(I)","",4,300,1200]
[null,"","","(III)","",2,162,324]
[null,"5005000000-E","80' HIGH MOUNT STANDARD","","",2,26500,53000]
[null,"5010000000-E","100' HIGH MOUNT STANDARD","","",13,30554.545384615401,397209.09]
[null,"5015000000-E","120' HIGH MOUNT STANDARD","","",24,33322.916666666701,799750]
[null,"5020000000-N","PORTABLE DRIVE UNIT","","",5,9300.2720000000008,46501.36]
[null,"5025000000-E","HIGH MOUNT FOUNDATIONS","","",316,1204.93136075949,380758.31]
[null,"5030000000-N","HM LUMINAIRE ************","(560W LED)","",30,1720.9079999999999,51627.24]
[null,"5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",36,4562.6841666666696,164256.63]
[null,"","","(45' TA, 15' ARM)","",35,4902.4685714285697,171586.4]
[null,"5070000000-N","STD FOUNDAT ***********","(R1)","",22,831.81818181818198,18300]
[null,"","","(R2)","",3,925,2775]
[null,"","","(TYPE M1)","",18,1500,27000]
[null,"","","(TYPE M2)","",6,1850,11100]
[null,"","","(TYPE R1)","",74,1540.4562162162199,113993.76]
[null,"","","(TYPE R2)","",9,1605.3088888888899,14447.78]
[null,"5080000000-N","LITE STD LUM ************","(RDW, 185W LED)","",17,1200,20400]
[null,"","","(RDW, 285W LED)","",35,816.38199999999995,28573.37]
[null,"5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",10,2321.1869999999999,23211.87]
[null,"","","(30', CLASS 4)","",1,3500,3500]
[null,"5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",250,39.549999999999997,9887.5]
[null,"","","(3 1/0 USE)","",25,50.51,1262.75]
[null,"5145000000-N","LITE CNTRL RW************","(240/480 V)","",2,17213.384999999998,34426.769999999997]
[null,"5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",18716,8.5582576405214805,160176.35]
[null,"","","(3\")","",485,19,9215]
[null,"","","(4\")","",423,28,11844]
[null,"5160000000-E","ELECT DUCT JA, SIZE *****","(2\")","",486,16.5,8019]
[null,"","","(3\")","",4284,19.763235294117599,84665.7]
[null,"","","(4\")","",2539,23.8703032690035,60606.7]
[null,"","","(6\")","",215,41,8815]
[null,"5170000000-E","**-#8 W/G FEEDER CIRCUIT","(2)","",12803,4.6075763492931303,58990.8]
[null,"5175000000-E","**-#6 W/G FEEDER CIRCUIT","(2)","",3639,3.8169826875515298,13890]
[null,"5180000000-E","**-#4 W/G FEEDER CIRCUIT","(2)","",13248,7.9087484903381604,104775.1]
[null,"5185000000-E","**-#2 W/G FEEDER CIRCUIT","(2)","",530,7.4984905660377397,3974.2]
[null,"5205000000-E","**-#8 W/G FEEDR N *****\"","(2, 1.5\")","",34217,9.9955855276616905,342018.95]
[null,"5210000000-E","**-#6 W/G FEEDR N *****\"","(2, 1.5\")","",13684,10.488113855597801,143519.35]
[null,"5215000000-E","**-#4 W/G FEEDER N *****\"","(2, 1.5\")","",19307,12.032855958978599,232318.35]
[null,"5220000000-E","**-#2 W/G FEEDER N *****\"","(2, 1.5\")","",2730,15.940329670329699,43517.1]
[null,"5240000000-N","ELEC JB ************","(BR18)","",8,3500,28000]
[null,"","","(CS36)","",12,1057.1341666666699,12685.61]
[null,"","","(HM18)","",37,375.98297297297302,13911.37]
[null,"","","(HM30)","",1,610,610]
[null,"","","(HM36)","",2,922.5,1845]
[null,"","","(IG18)","",115,484.350434782609,55700.3]
[null,"","","(IG30)","",16,627.83437500000002,10045.35]
[null,"","","(IG36)","",16,1143.75,18300]
[null,"","","(LS18)","",73,565.18958904109604,41258.839999999997]
[null,"","","(LS30)","",2,707.07,1414.14]
[null,"","","(TYPE IG, 13\"W x 24\"L x 18\"D)","",21,750,15750]
[null,"5252000000-N","UNDERPASS LUMINARIES *****","(TYPE WM, 70W MAX LED)","",6,800,4800]
[null,"","","(WM)","",8,780,6240]
[null,"5253000000-N","UNDERPASS CIRCUITRY *************","(UPL-1)","",2,8750,17500]
[null,"","","(UPL-2)","",2,8750,17500]
[null,"5255000000-N","PORTABLE LIGHTING","","",37,96163.862702702696,3558062.92]
[null,"5260000000-N","GENERIC LIGHTING ITEM (LS)","EQUIPMENT STORAGE","",1,750,750]
[null,"","","LUMINAIRE STORAGE","",3,3925,11775]
[null,"","","TEMPORARY PORTABLE LIGHTING","",1,18000,18000]
[null,"5265000000-E","GENERIC LIGHTING ITEM (LF)","STREET LIGHTING CONDUIT IN-","STALLATION (2\" PVC)",4320,7.5,32400]
[null,"5270000000-N","GENERIC LIGHTING ITEM (EA)","100' HIGH MOUNT LUMINAIRE -   LED","",36,1650,59400]
[null,"","","100A 6-POSITION MAIN CB PANEL","",1,450,450]
[null,"","","120' HIGH MOUNT LUMINAIRE -   LED","",160,1800,288000]
[null,"","","80' HIGH MOUNT LUMINAIRE - LED","",16,1700,27200]
[null,"","","CCTV SERVICE DISCONNECT","",1,895,895]
[null,"","","COMMUNICATION GATEWAY","",5,6017,30085]
[null,"","","CONTROL NODE","",261,264.92337164751001,69145]
[null,"","","DECORATIVE ROADWAY LUMINAIRE","(118W LED)",5,300,1500]
[null,"","","","(140W LED)",9,300,2700]
[null,"","","","(174W LED)",12,300,3600]
[null,"","","","(57W LED)",11,300,3300]
[null,"","","DECORATIVE ROADWAY POLE (22'","MH, DOUBLE 30\" ARM)",1,1000,1000]
[null,"","","","MH, SINGLE 30\" ARM)",1,950,950]
[null,"","","DECORATIVE ROADWAY POLE (25'","MH, DOUBLE 30\" ARM)",2,1000,2000]
[null,"","","","MH, SINGLE 30\" ARM)",30,950,28500]
[null,"","","LIGHT CONTROL EQUIPMENT, TYPE","RW, 120/240V",3,17500,52500]
[null,"","","","RW, 240/480V",5,13360,66800]
[null,"","","LIGHT STANDARD, 45' SA, 15'   ARM","",17,4575,77775]
[null,"","","LIGHTING CONTROL CENTER","",1,15000,15000]
[null,"","","LIGHTING CONTROL SYSTEM","",1,14000,14000]
[null,"","","REFURBISH SINGLE ARM LIGHT STAN- DARD","",7,1250,8750]
[null,"","","REINSTALL COBRAHEAD LUMINAIRE","",30,181.666666666667,5450]
[null,"","","REINSTALL COMMUNICATION GATE- WAY","",2,1037.5,2075]
[null,"","","REINSTALL HIGH MAST LUMINAIRE","",32,475,15200]
[null,"","","RELOCATE CONTROL SYSTEM","",1,5100,5100]
[null,"","","RELOCATE LIGHT STANDARD","",1,1818,1818]
[null,"","","RELOCATE SINGLE ARM LIGHT     STANDARD","",7,1400,9800]
[null,"","","REMOVE 100' HIGH MAST STAND-","ARD FOUNDATION",2,2600,5200]
[null,"","","REMOVE 100' HIGH MAST STANDARD","",4,4337.5,17350]
[null,"","","REMOVE 100' HIGH MAST STANDARDFOUNDATION","",2,2300,4600]
[null,"","","REMOVE 120' HIGH MAST STANDARD","",3,6260,18780]
[null,"","","REMOVE 120' HIGH MAST STANDARDFOUNDATION","",3,2300,6900]
[null,"","","REMOVE CONTROL SYSTEM","",1,100,100]
[null,"","","REMOVE CONTROL SYSTEM -       DISPOSE","",2,1150,2300]
[null,"","","REMOVE CONTROL SYSTEM -       SALVAGE","",1,980,980]
[null,"","","REMOVE HIGH MOUNT LIGHT       STANDARD","",3,4000,12000]
[null,"","","REMOVE HIGH MOUNT STANDARD    FOUNDATION","",3,2000,6000]
[null,"","","REMOVE LIGHT STANDARD","",19,400,7600]
[null,"","","REMOVE LIGHT STANDARD FOUND-  ATION","",20,510,10200]
[null,"","","REMOVE LIGHT STANDARD FOUNDA- TION","",25,536.36,13409]
[null,"","","REMOVE SINGLE ARM LIGHT       STANDARD","",1,606,606]
[null,"","","REMOVE SINGLE ARM LIGHT STAND-","ARD - DISPOSE",11,290.90909090909099,3200]
[null,"","","","ARD - SALVAGE",11,245.45454545454501,2700]
[null,"","","REMOVE TWIN ARM LIGHT STANDARD","- DISPOSE",4,515,2060]
[null,"","","ROADWAY LIGHT STANDARD LUMI-","NAIRE - 285W LED",28,1265,35420]
[null,"","","ROADWAY LIGHT STANDARD LUMIN-","AIRE - 185W LED",21,875,18375]
[null,"5319000000-E","CL B CONC FOR ENCAS LINE","","",6,495,2970]
[null,"5325000000-E","**\" WATER LINE","(1-1/2\")","",30,45,1350]
[null,"","","(14\")","",1922,128.324661810614,246640]
[null,"","","(18\")","",8926,306.86847412054698,2739108]
[null,"","","(36\")","",1303,917.59,1195619.77]
[null,"5325200000-E","2\" WATER LINE","","",3874,43.675418172431598,169198.57]
[null,"5325400000-E","4\" WATER LINE","","",499,89.168336673346701,44495]
[null,"5325600000-E","6\" WATER LINE","","",59088,56.539096770918,3340782.15]
[null,"5325800000-E","8\" WATER LINE","","",42391,55.689507914415799,2360733.9300000002]
[null,"5326000000-E","10\" WATER LINE","","",11573,107.281690140845,1241571]
[null,"5326200000-E","12\" WATER LINE","","",66137,106.57910367872699,7048822.1799999997]
[null,"5326600000-E","16\" WATER LINE","","",12758,130.140598056122,1660333.75]
[null,"5327000000-E","20\" WATER LINE","","",2012,214.59,431755.08]
[null,"5327400000-E","24\" WATER LINE","","",19044,278.24217601344299,5298844]
[null,"5328000000-E","30\" WATER LINE","","",55,432.3,23776.5]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",574086,12.824985542235799,7362644.6500000004]
[null,"5534000000-E","**\" VALVE","(14\")","",2,14525,29050]
[null,"","","(18\")","",6,12000,72000]
[null,"5536000000-E","2\" VALVE","","",24,1340.4037499999999,32169.69]
[null,"5538000000-E","4\" VALVE","","",8,2236.25,17890]
[null,"5540000000-E","6\" VALVE","","",375,1872.55149333333,702206.81]
[null,"5546000000-E","8\" VALVE","","",86,2588.8897674418599,222644.52]
[null,"5552000000-E","10\" VALVE","","",42,3998.9523809523798,167956]
[null,"5558000000-E","12\" VALVE","","",102,4448.3269607843104,453729.35]
[null,"5558600000-E","16\" VALVE","","",13,10574.9230769231,137474]
[null,"5559000000-E","20\" VALVE","","",5,20828.43,104142.15]
[null,"5559400000-E","24\" VALVE","","",23,23773.304347826099,546786]
[null,"5571000000-E","**\" TAPPING SLEEVE & VALVE","(2\")","",1,7500,7500]
[null,"","","(2-1/2\")","",1,8100,8100]
[null,"","","(3\")","",3,8200,24600]
[null,"5571400000-E","4\" TAPPING SLEEVE & VALVE","","",3,5500,16500]
[null,"5571600000-E","6\" TAPPING SLEEVE & VALVE","","",28,6599.9271428571401,184797.96]
[null,"5571800000-E","8\" TAPPING SLEEVE & VALVE","","",12,6617.6666666666697,79412]
[null,"5572000000-E","10\" TAPPING SLEEVE & VALVE","","",2,12674,25348]
[null,"5572200000-E","12\" TAPPING SLEEVE & VALVE","","",21,8279.9047619047597,173878]
[null,"5572600000-E","16\" TAPPING SLEEVE & VALVE","","",1,18950,18950]
[null,"5573000000-E","20\" TAPPING SLEEVE & VALVE","","",2,46100,92200]
[null,"5573400000-E","24\" TAPPING SLEEVE & VALVE","","",5,59468,297340]
[null,"5589100000-E","1\" AIR RELEASE VALVE","","",23,3572.3913043478301,82165]
[null,"5589200000-E","2\" AIR RELEASE VALVE","","",29,12343.7493103448,357968.73]
[null,"5600000000-E","**\" BLOW OFF","(1-1/2\")","",1,3125.05,3125.05]
[null,"","","(3/4\")","",1,1715.58,1715.58]
[null,"5606000000-E","2\" BLOW OFF","","",15,9210.2886666666709,138154.32999999999]
[null,"5606600000-E","6\" BLOW OFF","","",6,16500,99000]
[null,"5643000000-E","**\" WATER METER","(1\")","",4,2875,11500]
[null,"","","(2\")","",1,3000,3000]
[null,"","","(5/8\")","",2,2700,5400]
[null,"5643100000-E","3/4\" WATER METER","","",21,2502.8571428571399,52560]
[null,"5643150000-E","1-1/2\" WATER METER","","",6,7533,45198]
[null,"5643200000-E","2\" WATER METER","","",5,10000,50000]
[null,"5648000000-N","RELOCATE WATER METER","","",292,1620.89712328767,473301.96]
[null,"5649000000-N","RECONNECT WATER METER","","",237,1386.3087763713099,328555.18]
[null,"5653100000-E","RELC **\" DCV BACKFLOW PREVNT A","(1\")","",3,3250,9750]
[null,"","","(2\")","",3,3500,10500]
[null,"5653210000-E","RELC 2\" DCV BACKFLOW PREVNT A","","",2,15000,30000]
[null,"5656000000-E","**\" RPZ BACKFLOW PREVNT ASMBLY","(1\")","",1,2280,2280]
[null,"","","(1-1/2\")","",6,5072,30432]
[null,"","","(2\")","",1,3300,3300]
[null,"5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1\")","",3,6500,19500]
[null,"","","(3/4\")","",33,5000,165000]
[null,"5656200000-E","2\" RPZ BACKFLOW PREVNT ASMBLY","","",2,2100,4200]
[null,"5656210000-E","RELC 2\" RPZ BACKFLOW PREVNT A","","",1,15000,15000]
[null,"5666000000-N","FIRE HYDRANT","","",108,5806.3978703703697,627090.97]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",85,3294.5985882352902,280040.88]
[null,"5673000000-E","FIRE HYDRANT LEG","","",2240.9,81.741510107546105,183174.55]
[null,"5678400000-E","6\" LINE STOP","","",7,8627.2071428571398,60390.45]
[null,"5678600000-E","8\" LINE STOP","","",10,16104,161040]
[null,"5679000000-E","12\" LINE STOP","","",18,15008.4311111111,270151.76]
[null,"5679200000-E","16\" LINE STOP","","",6,40000,240000]
[null,"5679400000-E","20\" LINE STOP","","",6,20791.866666666701,124751.2]
[null,"5679600000-E","24\" LINE STOP","","",5,51000,255000]
[null,"5684000000-E","**\" LINE STOP W/ BYPASS","(14\")","",1,70000,70000]
[null,"5684400000-E","6\" LINE STOP W/ BYPASS","","",1,42300,42300]
[null,"5684800000-E","10\" LINE STOP W/ BYPASS","","",1,64000,64000]
[null,"5686000000-E","**\" H2O SERVICE LINE","(1\")","",70,60,4200]
[null,"","","(2\")","",1302.7,69.592177784601205,90657.73]
[null,"","","(2-1/2\")","",35,40,1400]
[null,"5686500000-E","WATER SERVICE LINE","","",12550,22.227144223107601,278950.65999999997]
[null,"5691000000-E","**\" SANITARY GRAVITY SEWER","(15\")","",360,181.111111111111,65200]
[null,"","","(36\")","",1848,505.22,933646.56]
[null,"","","(8\")","",5592,213,1191096]
[null,"5691200000-E","6\" SANITARY GRAVITY SEWER","","",10,300,3000]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",28753.23,163.857682076066,4711437.62]
[null,"5691400000-E","10\" SANITARY GRAVITY SEWER","","",2846.1,194.90987667334201,554733]
[null,"5691500000-E","12\" SANITARY GRAVITY SEWER","","",5169.25,145.658461092035,752945]
[null,"5691600000-E","16\" SANITARY GRAVITY SEWER","","",5578,181.65074220150601,1013247.84]
[null,"5691700000-E","18\" SANITARY GRAVITY SEWER","","",1560,209.13653846153801,326253]
[null,"5709000000-E","**\" FORCE MAIN SEWER","(2\")","",69,110,7590]
[null,"","","(3\")","",287,43,12341]
[null,"5709100000-E","2\" FORCE MAIN SEWER","","",1131,26.262599469495999,29703]
[null,"5709200000-E","4\" FORCE MAIN SEWER","","",5535,209.41300813008101,1159101]
[null,"5709300000-E","6\" FORCE MAIN SEWER","","",6822,56.2078569334506,383450]
[null,"5709400000-E","8\" FORCE MAIN SEWER","","",7534,89.634058932837803,675303]
[null,"5709500000-E","10\" FORCE MAIN SEWER","","",7648,60.316684100418399,461302]
[null,"5709600000-E","12\" FORCE MAIN SEWER","","",1392,253.717672413793,353175]
[null,"5709700000-E","16\" FORCE MAIN SEWER","","",20555,228,4686540]
[null,"5709800000-E","20\" FORCE MAIN SEWER","","",988,48,47424]
[null,"5709900000-E","24\" FORCE MAIN SEWER","","",34740,399.5,13878630]
[null,"5768000000-N","SANITARY SEWER CLEAN-OUT","","",99,853.90323232323203,84536.42]
[null,"5768500000-E","SEWER SERVICE LINE","","",4685,43.474706510138702,203679]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",113330,15.9068825553693,1802727]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",266,5711.8012030075197,1519339.12]
[null,"5776000000-E","5' DIA UTILITY MANHOLE","","",50,7654.8191999999999,382740.96]
[null,"5777000000-E","6' DIA UTILITY MANHOLE","","",8,9104.4,72835.199999999997]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",993.4,409.26713307831699,406565.97]
[null,"5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",440.4,603.79468664850106,265911.18]
[null,"5783000000-E","UTILITY MANHOLE WALL 6' DIA","","",50,466.59120000000001,23329.56]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(1-1/2\")","",157,15,2355]
[null,"","","(15\")","",5218,14.8851763127635,77670.850000000006]
[null,"","","(2\")","",2400,8.2844583333333297,19882.7]
[null,"","","(36\")","",590,99.542203389830505,58729.9]
[null,"","","(4\")","",3807,9.5275545048594701,36271.4]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",64749.5,7.7831543100718896,503955.35]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",48901.3,14.707018218329599,719192.31]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",15662,18.101711786489599,283509.01]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",35529,15.2615592895944,542227.93999999994]
[null,"5805000000-E","ABANDON 14\" UTILITY PIPE","","",1627,25.998770743700099,42300]
[null,"5810000000-E","ABANDON 16\" UTILITY PIPE","","",63367,24.1466695598656,1530102.01]
[null,"5811000000-E","ABANDON 18\" UTILITY PIPE","","",1415,43.5102756183746,61567.040000000001]
[null,"5812000000-E","ABANDON 20\" UTILITY PIPE","","",2685,19.068513966480399,51198.96]
[null,"5813000000-E","ABANDON 24\" UTILITY PIPE","","",25642,40.540480461742398,1039539]
[null,"5814000000-E","ABANDON 30\" UTILITY PIPE","","",1754,29.892565564424199,52431.56]
[null,"5815000000-N","REMOVE WATER METER","","",435,217.682459770115,94691.87]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",75,1022.38613333333,76678.960000000006]
[null,"5816000000-N","ABANDON UTILITY MANHOLE","","",184,997.58494565217404,183555.63]
[null,"5828000000-N","REMOVE UTILITY MANHOLE","","",46,3988.7141304347801,183480.85]
[null,"5835000000-E","**\" ENCASEMENT PIPE","(14\")","",898,122.495545657016,110001]
[null,"","","(22\")","",165,195,32175]
[null,"","","(26\")","",488,155,75640]
[null,"","","(32\")","",521,830,432430]
[null,"","","(48\")","",743,1265,939895]
[null,"","","(54\")","",330,884.42,291858.59999999998]
[null,"","","(60\")","",1040,1143.77,1189520.8]
[null,"5835400000-E","6\" ENCASEMENT PIPE","","",216,139,30024]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",2592,191.11358024691401,495366.40000000002]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",3897.3,189.50432863777499,738555.22]
[null,"5835900000-E","20\" ENCASEMENT PIPE","","",1225,190.15755102040799,232943]
[null,"5836000000-E","24\" ENCASEMENT PIPE","","",4792,207.33681969949899,993558.04]
[null,"5836200000-E","30\" ENCASEMENT PIPE","","",1405,192.25622775800699,270120]
[null,"5836400000-E","36\" ENCASEMENT PIPE","","",1621,198.39851943244901,321604]
[null,"5872500000-E","BORE & JACK **\"","(14\")","",646,184.12369969040199,118943.91]
[null,"","","(16\")","",1238,410.31906300484701,507975]
[null,"","","(18\")","",1461.3,623.38173544104598,910947.73]
[null,"","","(2\")","",75,26,1950]
[null,"","","(20\")","",739,266.40216508795697,196871.2]
[null,"","","(22\")","",165,300,49500]
[null,"","","(24\")","",2135,393.38875878220102,839885]
[null,"","","(26\")","",180,281.97000000000003,50754.6]
[null,"","","(30\")","",550,391,215050]
[null,"","","(32\")","",235,590,138650]
[null,"","","(36\")","",1070,684.27141121495299,732170.41]
[null,"","","(48\")","",271,845,228995]
[null,"5872600000-E","DIRECT DRILL **\"","(10\")","",5432,63.465942562591998,344747]
[null,"","","(12\")","",5745,126.28407310705001,725502]
[null,"","","(14\")","",1850,107.318918918919,198540]
[null,"","","(16\")","",8336,267.18507077735097,2227254.75]
[null,"","","(18\")","",7105,278.975369458128,1982120]
[null,"","","(20\")","",899,434,390166]
[null,"","","(24\")","",17863,371,6627173]
[null,"","","(3\")","",287,39,11193]
[null,"","","(6\")","",3212,84.0644458281445,270015]
[null,"","","(8\")","",3229,86.434422421802395,279096.75]
[null,"5872700000-E","TUNNELING **\"","(60\")","",670,1895.86,1270226.2]
[null,"5876000000-N","STEEL PILE PIERS","","",6,84,504]
[null,"5882000000-N","GENERIC UTILITY ITEM (EA)","10\" INSERTION VALVE","",2,22000,44000]
[null,"","","12\" CHECK VALVE AND VAULT","",1,100000,100000]
[null,"","","12\" INSERT VALVE","",6,18566.666666666701,111400]
[null,"","","12\" INSERTION VALVE","",7,25291.428571428602,177040]
[null,"","","12\" SEWER VALVE","",1,10000,10000]
[null,"","","16\" NITRILE PIPE GASKET","",3,221,663]
[null,"","","16\" SEWER VALVE","",3,16000,48000]
[null,"","","2\" AIR AND VACUUM RELEASE     VALVE","",25,12800,320000]
[null,"","","2\" CHECK VALVE","",4,2600,10400]
[null,"","","2\" COMBINATION AIR RELEASE    VALVE","",1,12919,12919]
[null,"","","24\" NITRILE PIPE GASKET","",20,350,7000]
[null,"","","24\" PRESSURE SUSTAINING VALVE ASSEMBLY","",1,350000,350000]
[null,"","","24\" SEWER VALVE","",30,40000,1200000]
[null,"","","36\" X 6\" TAPPING SLEEVE AND   VALVE","",1,13567.84,13567.84]
[null,"","","4\" COMBINATION AIR VALVE IN   MH","",1,80804.02,80804.02]
[null,"","","6\" INSERT VALVE","",6,9100,54600]
[null,"","","6\" INSERTION VALVE","",33,12866.666666666701,424600]
[null,"","","6\" SEWER VALVE","",2,5500,11000]
[null,"","","6' DIA POLYMER CONCRETE UTILI-","TY MANHOLE",9,30000.43,270003.87]
[null,"","","8\" INSERT VALVE","",4,10500,42000]
[null,"","","8\" INSERTION VALVE","",8,12250,98000]
[null,"","","8\" PRESSURE RELIEF VALVE IN 7'","DIA MANHOLE",1,35417.18,35417.18]
[null,"","","8\" SEWER VALVE","",2,7000,14000]
[null,"","","ABANDON UTILITY VAULT","",5,6500,32500]
[null,"","","ADJUST SANITARY SEWER CLEAN-","OUT TO FINISH GRADE",4,2500,10000]
[null,"","","ADJUSTABLE  HYDRAULIC JACK","",1,2750,2750]
[null,"","","ADJUSTMENT OF BRICK AND MORTARMANHOLES","",2,803,1606]
[null,"","","ADJUSTMENT OF PRECAST MANHOLES","",5,803,4015]
[null,"","","CONCRETE ANTI-SEEP PIPE       COLLARS","",6,1770.86,10625.16]
[null,"","","FLOW METER VAULT","",1,112000,112000]
[null,"","","RECONNECT FORCE MAIN","",12,11500,138000]
[null,"","","RELOCATE YARD HYDRANT","",1,8000,8000]
[null,"","","REMOVE EXISTING VAULT, BYPASS","AND STOCKPILE VALVES",1,5200,5200]
[null,"","","REMOVE UTILITY VAULT","",3,6500,19500]
[null,"","","STEEL PILE PIER","",3,10653.27,31959.81]
[null,"","","WATER METER BOX","",2,200,400]
[null,"5888000000-E","GENERIC UTILITY ITEM (LF)","6\" SEWER SERVICE LINE","",299,40,11960]
[null,"","","MAJOR DRAINAGE STRUCTURES AND","BRICK AND MORTAR MANHOLES",3.5,960,3360]
[null,"","","","PRECAST MANHOLES",2,563,1126]
[null,"","","POLYETHYLENE ENCASEMENT ON 16\"DIA MAIN","",101,12,1212]
[null,"","","POLYETHYLENE ENCASEMENT ON 24\"DIA MAIN","",340,9,3060]
[null,"","","POLYETHYLENE ENCASEMENT WATER LINE","",100,175,17500]
[null,"","","POLYMER CONCRETE UTILITY MAN-","HOLE WALL, 6' DIA",92,416.67,38333.64]
[null,"5894000000-E","GENERIC UTILITY ITEM (CY)","REINFORCED CONCRETE ENCASEMENT","AND SUPPORTS",50,400,20000]
[null,"5912000000-N","GENERIC UTILITY ITEM (LS)","DEWATERING","",1,225000,225000]
[null,"","","PUMP STATION","",1,775000,775000]
[null,"","","RELOCATE MASTER METER AND","INSTALL NEW VAULT",1,52200,52200]
[null,"","","REMOVE EXISTING PUMP STATION","",1,100000,100000]
[null,"","","UTILITY COORDINATOR","",1,745200,745200]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",1793210,2.0341563118653099,3647669.44]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",52460,52.899616850934002,2775113.9]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",223821,46.758115413656398,10465448.15]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",145602,43.039211343250798,6266595.25]
[null,"6015000000-E","TEMPORARY MULCHING","","",5434.91,935.82619031409899,5086131.12]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",223443,3.53288981977507,789399.5]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",1146.48,975.33294082757698,1118199.71]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",121062,13.877134856519801,1679993.7]
[null,"6029000000-E","SAFETY FENCE","","",163464,2.39370258894925,391284.2]
[null,"6030000000-E","SILT EXCAVATION","","",1036810,4.4754374475554801,4640178.3]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",3523050,1.47275260072948,5188581.05]
[null,"6037000000-E","COIR FIBER MAT","","",241008,5.6378234332470303,1358760.55]
[null,"6038000000-E","PERM SOIL REINF MAT","","",72580,4.5775661339211897,332239.75]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",248928,5.3016619263401497,1319732.1000000001]
[null,"6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",12755,4.8790121520972196,62231.8]
[null,"6045000000-E","**\" TEMPORARY PIPE","(15\")","",1265,72.284584980237199,91440]
[null,"","","(18\")","",1769,57.518371961560199,101750]
[null,"","","(24\")","",740,99.704054054054097,73781]
[null,"","","(30\")","",735,102.772108843537,75537.5]
[null,"","","(36\")","",1575,114.62222222222201,180530]
[null,"","","(42\")","",390,156.02564102564099,60850]
[null,"","","(48\")","",1200,90,108000]
[null,"","","(54\")","",431,148.097447795824,63830]
[null,"6046000000-E","TEMP PIPE FOR STREAM CROSS","","",300,78.228333333333296,23468.5]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",16012,28.885145515863101,462508.95]
[null,"6069000000-E","STILLING BASINS","","",2138,18.520579981290901,39597]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",310,887.83064516129002,275227.5]
[null,"6071010000-E","WATTLE","","",77593,6.4972679236529096,504142.51]
[null,"6071012000-E","COIR FIBER WATTLE","","",153200,9.8648994778067909,1511302.6]
[null,"6071013000-E","WATTLE BARRIER","","",60878,12.8777440126154,783971.3]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",9101,11.798330952642599,107376.61]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",112029,6.7659736318274701,757985.26]
[null,"6071030000-E","COIR FIBER BAFFLE","","",173465,5.5678136799930797,965820.8]
[null,"6071050000-E","**\" SKIMMER","(1\")","",1,900,900]
[null,"","","(1-1/2\")","",359,2222.15554317549,797753.84]
[null,"","","(2\")","",133,2518.2544360902298,334927.84000000003]
[null,"","","(2-1/2\")","",63,3718.6834920634901,234277.06]
[null,"","","(3\")","",29,2537.0365517241398,73574.06]
[null,"","","(4\")","",5,3528.8980000000001,17644.490000000002]
[null,"6078000000-E","SELECT UNDERGRTH REMOVAL","","",0.1,10000,1000]
[null,"6084000000-E","SEEDING AND MULCHING","","",3720.33,2182.4616069004601,8119477.3899999997]
[null,"6087000000-E","MOWING","","",2776.72,154.450531562419,428865.88]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",57043,7.8672142068264304,448769.5]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",165.73,1359.2376153985399,225266.45]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",83875,5.7691654247392004,483888.75]
[null,"6102000000-E","SODDING","","",3875,9.1354838709677395,35400]
[null,"6105000000-E","WATER","","",28,857.142857142857,24000]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",2500.0500000000002,1030.95449691006,2577437.79]
[null,"6111000000-E","IMPERVIOUS DIKE","","",12779,183.566707097582,2345798.9500000002]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",1455,119.591065292096,174005]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",3716,184.42105220667401,685308.63]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",400,1034.7139999999999,413885.6]
[null,"6120000000-E","CULVERT DIVERSION CHANNEL","","",7437,16.778405270942599,124781]
[null,"6123000000-E","REFORESTATION","","",34.119999999999997,3379.8027549824201,115318.87]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",12.9,4419.0697674418598,57006]
[null,"6129000000-E","WETLAND REFORESTATION","","",0.27200000000000002,4000,1088]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",382,318.69136125654501,121740.1]
[null,"","","","DEVICE CLEANOUT",1804,189.97246119733899,342710.32]
[null,"","","FABRIC INSERT INLET PROTECTION DEVICE","",55,79.545454545454504,4375]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",130,240.869230769231,31313]
[null,"","","SIGN","",88,71.25,6270]
[null,"6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","CONSTRUCTION, MAINTENANCE, &  REMOVAL OF","TEMP ACCESS AT STA 66+62-Y4-RT",1,275000,275000]
[null,"","","PUMP-AROUND OPERATION","",1,50900,50900]
[null,"","","REMOVAL OF JAPANESE KNOTWEED","",1,25000,25000]
[null,"","","STREAM INTAKE VAULT","",1,53429.41,53429.41]
[null,"","","SURVEYING FOR MITIGATION","",1,19095,19095]
[null,"6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","COMPOST BLANKET","",5,20335,101675]
[null,"","","DISKING","",0.27200000000000002,1000,272]
[null,"","","RIPPING","",0.27200000000000002,1000,272]
[null,"","","WETLAND GRASS PLANTING","",0.38,4000,1520]
[null,"6138000000-E","GENERIC EROSION CONTROL ITEM (CY)","ASTM C-33 FINE AGGREGATE","",36,155,5580]
[null,"","","BLANKET DRAIN","",1350,66.400000000000006,89640]
[null,"","","BORROW FOR STREAM RELOCATION","",25000,18.100000000000001,452500]
[null,"","","DAM EMBANKMENT EARTH FILL","",4850,22.45,108882.5]
[null,"","","IMPERVIOUS SELECT MATERIAL","",700,58.15,40705]
[null,"","","SHREDDED HARDWOOD MULCH","",9,135,1215]
[null,"","","UNCLASSIFIED FOR STREAM","RELOCATION",34000,13.35,453900]
[null,"","","UNDERCUT FOR STREAM RELOCATION","",13000,27.2,353600]
[null,"6141000000-E","GENERIC EROSION CONTROL ITEM (SY)","EXCELSIOR NATURAL FIBER MAT-  TING","",3722,2.5,9305]
[null,"","","TYPE 2 GEOTEXTILE","",1050,2.23,2341.5]
[null,"6147000000-E","GENERIC EROSION CONTROL ITEM (LF)","SAFETY FENCE FOR MONITORING","WELL PROTECTION",880,6.5,5720]
[null,"","","TOE WOOD PROTECTION","",400,111.36,44544]
[null,"","","TREE PROTECTION FENCE","",1700,2.5,4250]
[null,"6900000000-E","TOPSOIL","","",3730,26.3270777479893,98200]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",226,904.73,204468.98]
[null,"7060000000-E","SIGNAL CABLE","","",221785,3.0703438014293098,680956.2]
[null,"7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",28,493.21428571428601,13810]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",894,804.38302013422799,719118.42]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",164,996.637804878049,163448.6]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",105,1353.16571428571,142082.4]
[null,"7180000000-N","BACKPLATE","","",176,102.329545454545,18010]
[null,"7216000000-N","MODIFY EXT VEHIC SIGNL HD","","",4,330,1320]
[null,"7229000000-N","APS DETECTOR STATION","","",8,808,6464]
[null,"7230000000-N","CENT CONT UNIT APS DETECT STA","","",1,1818,1818]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",36203,3.2989241223103098,119430.95]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",34150,4.2929721815519803,146605]
[null,"7279000000-E","TRACER WIRE","","",138128,0.79460833429861999,109757.66]
[null,"7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",975,28.092564102564101,27390.25]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 1\")","",20,10.3,206]
[null,"","","(1, 2\")","",36051,8.4724964633435995,305441.96999999997]
[null,"","","(2, 2\")","",52037,8.9279356995983594,464582.99]
[null,"","","(3, 2\")","",14575,8.1478010291595204,118754.2]
[null,"","","(4, 2\")","",1010,18.312673267326701,18495.8]
[null,"7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",5580,4.2455197132616496,23690]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",6955,19.903709561466599,138430.29999999999]
[null,"","","(2, 2\")","",48464,19.856062644437099,962304.22]
[null,"","","(3, 2\")","",2454,23.4082314588427,57443.8]
[null,"","","(4, 2\")","",275,39.700000000000003,10917.5]
[null,"","","(5, 2\")","",150,47.5,7125]
[null,"7312000000-N","JUNCTION BOX (***************)","(SPECIAL OVER-SIZED HEAVY     DUTY)","",4,750,3000]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",623,340.17691813804203,211930.22]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",358,681.83589385474897,244097.25]
[null,"7360000000-N","WOOD POLE","","",153,1041.9675163398699,159421.03]
[null,"7372000000-N","GUY ASSEMBLY","","",408,607.71661764705902,247948.38]
[null,"7384000000-E","***\" RISER WITH **************","(1-1/2\", WEATHERHEAD)","",16,485.38687499999997,7766.19]
[null,"","","(1-1/4\", WEATHERHEAD)","",12,607,7284]
[null,"7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",37,491.79459459459503,18196.400000000001]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",62,434.37548387096803,26931.279999999999]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",132,706.37484848484803,93241.48]
[null,"7430000000-N","HEAT SHRINK TUB KIT","","",10,110.5,1105]
[null,"7432000000-E","2\" RISER WITH TUBING","","",70,780.12285714285701,54608.6]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",274473,7.2250379454445399,1983077.84]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",279051,1.7696974746551699,493835.85]
[null,"7481000000-N","SITE SURVEY","","",27,1223.7596296296299,33041.51]
[null,"7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",47,260.30297872340401,12234.24]
[null,"7481220000-N","CAMERA W/ INT LOOP EMUL PROCESS","","",14,1500,21000]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",59,3784.4501694915298,223282.56]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",18,6240.40333333333,112327.26]
[null,"7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",63,319.94190476190499,20156.34]
[null,"7485000000-N","WRLESS MAGN SENSOR DET SYS","","",1,10327,10327]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",20210,2.4785254824344398,50091]
[null,"","","(144)","",49114,3.5148401677729399,172627.86]
[null,"","","(24)","",31755,2.7151598173516001,86219.9]
[null,"","","(36)","",5425,3.03,16437.75]
[null,"","","(48)","",132439,3.1550147615128501,417847]
[null,"","","(72)","",21055,3.28,69060.399999999994]
[null,"7528000000-E","DROP CABLE","","",30788,2.6731658438352599,82301.429999999993]
[null,"7540000000-N","SPLICE ENCLOSURE","","",110,1693.1328181818201,186244.61]
[null,"7541000000-N","MOD SPLICE ENCLOSURE","","",10,805.75,8057.5]
[null,"7552000000-N","INTERCONNECT CENTER","","",116,1794.07017241379,208112.14]
[null,"7566000000-N","DELINEATOR MARKER","","",246,113.26073170731701,27862.14]
[null,"7574550000-N","FURN WRLESS LIGHTNING ARSTR","","",1,208,208]
[null,"7575000000-N","FIBER-OPTIC TRAINING","","",1,7000,7000]
[null,"7575142000-N","900MHZ SPECTRUM RADIO","","",5,5101.2,25506]
[null,"7575142010-N","900MHZ SER/ETH SPEC RADIO","","",31,4414.3870967741896,136846]
[null,"7575142060-N","MOD RADIO INSTALL","","",14,1240.0314285714301,17360.439999999999]
[null,"7575142200-N","NEW ELECTRICAL SERVICE","","",10,1800,18000]
[null,"7575160000-E","REM EXT COMM CABLE","","",33638,0.93955496759616997,31604.75]
[null,"7575180000-N","CABLE TRANSFER","","",11,364,4004]
[null,"7575200000-N","GPS UNIT","","",2,1305,2610]
[null,"7576000000-N","METAL STRAIN SIGNAL POLE","","",75,12835.0314666667,962627.36]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",59,29489.757966101701,1739895.72]
[null,"7590000000-N","DBL MAST ARM WITH METAL POLE","","",6,37233.333333333299,223400]
[null,"7613000000-N","SOIL TEST","","",159,1156.1756603773599,183831.93]
[null,"7614100000-E","DRILLED PIER FOUND","","",1058.3,1124.79537938203,1190370.95]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",69,161.66057971014499,11154.58]
[null,"7636000000-N","SIGN FOR SIGNALS","","",349,403.97068767908303,140985.76999999999]
[null,"7642100000-N","TYPE I POST W/ FOUNDATION","","",24,1377.5,33060]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",185,1945.65189189189,359945.6]
[null,"7642300000-N","TYPE III PED W/ FOUNDATION","","",14,4990.7142857142899,69870]
[null,"7648000000-N","RELOCATE EXISTING SIGN","","",1,303,303]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",64,1796.765625,114993]
[null,"7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",32,664.21875,21255]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(2070E, BASE MOUNTED)","",6,17550,105300]
[null,"","","(2070LX, 332)","",9,14417,129753]
[null,"","","(2070LX, 336S)","",6,15950,95700]
[null,"","","(TYPE 2070E, BASE MOUNTED)","",8,15173.95,121391.6]
[null,"","","(TYPE 2070E, BASE-MOUNTED)","",13,16355,212615]
[null,"","","(TYPE 2070E, POLE MOUNTED)","",2,13000,26000]
[null,"","","(TYPE 2070E, POLE-MOUNTED)","",1,14500,14500]
[null,"","","(TYPE 2070LX, BASE MOUNTED)","",17,13751.588235294101,233777]
[null,"","","(TYPE 2070LX, POLE MOUNTED)","",1,14810,14810]
[null,"7708000000-N","DETECTOR CARD (***********)","(2070E)","",165,120,19800]
[null,"","","(MODEL 222)","",282,90,25380]
[null,"","","(TYPE 2070E)","",19,125,2375]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",355,127.33160563380299,45202.720000000001]
[null,"7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",2,15700,31400]
[null,"7780000000-N","DETECTOR CARD (TYPE 2070L)","","",9,121,1089]
[null,"7901000000-N","CABINET BASE EXTENDER","","",90,531.10988888888903,47799.89]
[null,"7912000000-N","BEACON CNTRL ASSM & CBNT *****","(F3)","",2,3875,7750]
[null,"","","(TYPE F3)","",1,6600,6600]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",7,8757.9214285714297,61305.45]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",35,2748.9142857142901,96212]
[null,"7972000000-N","METAL POLE REMOVAL","","",35,932.57142857142901,32640]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","2070E CONTROLLER","",6,4640,27840]
[null,"","","5/8\" X 10' GROUNDING ELEC-    TRODES","",5,180.25,901.25]
[null,"","","5/8\" X 10' GROUNDING ELECTRODE","",116,249.93086206896601,28991.98]
[null,"","","5/8\"X10' GROUNDING ELECTRODES","",30,91,2730]
[null,"","","CCTV CAMERA  ASSEMBLY","",20,4900,98000]
[null,"","","CCTV CAMERA  LOWERING SYSTEM","",1,6263,6263]
[null,"","","CCTV CAMERA ASSEMBLY","",1,4253,4253]
[null,"","","CCTV EXTENSION POLE","",2,2380,4760]
[null,"","","CCTV FIELD EQUIPMENT CABINET","",20,5450,109000]
[null,"","","CCTV METAL POLE (60')","",8,15017.42,120139.36]
[null,"","","CCTV WOOD POLE","",27,2745.9629629629599,74141]
[null,"","","CONTRACTOR FURNISHED CONTROL-","LER (2070LX)",4,2605,10420]
[null,"","","CONTROLLER (TYPE 2070E)","",3,4495,13485]
[null,"","","CONTROLLER WITH CABINET WITH","AUX FILE (2070LX, 332)",44,12500,550000]
[null,"","","DECORATIVE METAL POLE WITH","SINGLE MAST ARM",4,34000,136000]
[null,"","","DIGITAL CCTV CAMERA  ASSEMBLY","",8,6176.875,49415]
[null,"","","DIGITAL CCTV CAMERA ASSEMBLY","",38,4187.0073684210502,159106.28]
[null,"","","DIGITAL DISPLAY MONITOR","",1,3800,3800]
[null,"","","DMS ACCESS LADDER","",14,7482.8071428571402,104759.3]
[null,"","","DMS ELECTRICAL SERVICE","",2,1850,3700]
[null,"","","DMS PEDESTAL STRUCTURE","",14,51943.0964285714,727203.35]
[null,"","","DMS STRUCTURE","",1,51888,51888]
[null,"","","DMS STRUCTURE (BACK-TO-BACK","PEDESTAL)",2,50000,100000]
[null,"","","DUAL DMS MOUNTED BACK TO BACK","",1,181999,181999]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE 1C)","",4,103000,412000]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE 2C)","",13,117933.846153846,1533140]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE-2C)","",5,75757.58,378787.9]
[null,"","","ELECTRICAL SERVICE FOR ITS","DEVICE",8,1510,12080]
[null,"","","ELECTRONIC MARKER BALL","",47,43,2021]
[null,"","","EQUIPMENT CABINET DISCONNECT","",39,1226.83153846154,47846.43]
[null,"","","ETHERNET CORE SWITCH","",1,55451.95,55451.95]
[null,"","","ETHERNET EDGE SWITCH","",142,1798.0320422535201,255320.55]
[null,"","","EXISTING CCTV CAMERA REMOVAL","",6,305,1830]
[null,"","","FIELD EQUIPMENT CABINET","",14,5697.24285714286,79761.399999999994]
[null,"","","FIREWALL","",1,5000,5000]
[null,"","","FURNISH 2018 ENHANCED CONFLICTMONITOR","",3,1200,3600]
[null,"","","FURNISH 2070 CONTROLLER TESTER","",1,8000,8000]
[null,"","","FURNISH 2070LX CONTROLLER","",3,1800,5400]
[null,"","","FURNISH 332 CABINET WITH AUX  FILE","",3,9000,27000]
[null,"","","FURNISH CCTV CAMERA  ASSEMBLY","",2,3500,7000]
[null,"","","FURNISH CONFLICT MONITOR TEST-ER","",1,27000,27000]
[null,"","","FURNISH ETHERNET EDGE SWITCH","",4,1715,6860]
[null,"","","GROUNDING SYSTEM","",1,2177,2177]
[null,"","","GUY ASSEMBLY - AERIAL","",1,1000,1000]
[null,"","","GUY ASSEMBLY - SIDEWALK","",8,950,7600]
[null,"","","HEAT SHRINK TUBING KIT","",12,150,1800]
[null,"","","HUB CABINET","",1,24747.47,24747.47]
[null,"","","HUB CABINET BASE EXTENDER","",1,1262.6300000000001,1262.6300000000001]
[null,"","","HUB CABINET FOUNDATION","",1,2525.25,2525.25]
[null,"","","ITS SERVER","",3,10000,30000]
[null,"","","JUNCTION BOX (SPECIAL OVER-","SIZED HEAVY DUTY)",24,1750,42000]
[null,"","","JUNCTION BOX (SPECIAL OVER-   SIZED)","",12,1515.15,18181.8]
[null,"","","JUNCTION BOX (SPECIAL-SIZED)","",15,950,14250]
[null,"","","JUNCTION BOX MARKER","",92,106.360869565217,9785.2000000000007]
[null,"","","KVM SWITCH","",1,3400,3400]
[null,"","","LIMITED ACCESS FACILITIES - JBW/CONCRETE","COLLAR (OVERSIZED)",22,1860,40920]
[null,"","","","COLLAR (SPECIAL OVERSIZED)",7,2650,18550]
[null,"","","","COLLAR (STANDARD SIZE)",18,930,16740]
[null,"","","LUMINAIRE MAST ARM","",2,2030,4060]
[null,"","","METER BASE/DISCONNECT","COMBINATION PANEL",2,1215,2430]
[null,"","","METER BASE/DISCONNECT COMBI-","NATION PANEL",1,912,912]
[null,"","","METER BASE/DISCONNECT COMBINA-","TION PANEL",21,1614.2857142857099,33900]
[null,"","","METER BASE/DISCONNECT COMBINA-TION PANEL","",11,2323.23,25555.53]
[null,"","","METER/BASE DISCONNECT","COMBINATION PANEL",1,1236,1236]
[null,"","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",15,38696.666666666701,580450]
[null,"","","MODIFY COMMUNICATIONS RACK","",1,6000,6000]
[null,"","","MODIFY EXISTING ELECTRICAL","SERVICE EQUIPMENT",4,777.5,3110]
[null,"","","MODIFY EXISTING ELECTRICAL    SERVICE","",8,500,4000]
[null,"","","MODIFY FOUNDATION FOR CONTROL-","LER CABINET",6,1250,7500]
[null,"","","PCMS (IM)","",3,22100,66300]
[null,"","","POLE GROUNDING SYSTEM","",71,280,19880]
[null,"","","PORTABLE CCTV CAMERA  ASSEMBLY","",3,28300,84900]
[null,"","","POWDER COAT FOR STRAIN POLE","(BLACK)",2,1001,2002]
[null,"","","PROTECTIVE COATING FOR DUAL","MAST ARM POLE (BLACK)",2,2090,4180]
[null,"","","PROTECTIVE COATING FOR SIGNAL","PEDESTAL (BLACK)",7,110,770]
[null,"","","PROTECTIVE COATING FOR SINGLE","MAST ARM POLE (BLACK)",14,1594.2857142857099,22320]
[null,"","","","MAST ARM POLE (BROWN)",2,2900,5800]
[null,"","","","PEDESTAL (BROWN)",2,260,520]
[null,"","","PTZ JOYSTICK","",1,1200,1200]
[null,"","","RELOCATE ETHERNET EDGE SWITCH","",2,250,500]
[null,"","","RELOCATE EXISTING CABINET","EQUIPMENT",30,100,3000]
[null,"","","REMOVAL AND DISPOSAL OF","EXISTING DMS COMPONENTS",2,5500,11000]
[null,"","","REMOVAL OF QUEUE BACKUP WARN- ING SYSTEM","",1,4500,4500]
[null,"","","REMOVE 900 MHZ RADIO","",5,52,260]
[null,"","","REMOVE 900MHZ RADIO","",10,350,3500]
[null,"","","REMOVE RADIO INSTALLATION","",8,656.5,5252]
[null,"","","SIGNAL SYSTEM SUPERVISOR'S","COMPUTER SYSTEM",1,6500,6500]
[null,"","","SOIL TEST","",1,3400,3400]
[null,"","","SOIL TEST FOR DMS FOUNDATION","",1,3500,3500]
[null,"","","SOLAR POWER ASSEMBLY","",3,12773.063333333301,38319.19]
[null,"","","SPAN TRANSFER","",69,60,4140]
[null,"","","TYPE 332 TEST CONTROLLER WITH CABINET","",1,15000,15000]
[null,"","","UPS IN COMMUNICATIONS RACK","",1,8300,8300]
[null,"","","VARIABLE SPEED DRILL","",1,1900,1900]
[null,"","","WOOD PEDESTAL","",14,222.49785714285699,3114.97]
[null,"","","WOOD POLE FOR SIGNALS","",9,1500,13500]
[null,"","","WOOD POLE FOR SIGNALS WITH    CCTV","",13,3700,48100]
[null,"7985000000-N","GENERIC SIGNAL ITEM (LS)","CCTV SOFTWARE","",1,14000,14000]
[null,"","","NETWORK MANAGEMENT SOFTWARE","",1,16650,16650]
[null,"","","REMOVE DMS AND STRUCTURE AT","I-40 MM 324",1,5200,5200]
[null,"","","","I-40 MM 331",1,5200,5200]
[null,"","","","I-95 MM 78",1,5200,5200]
[null,"","","SIGNAL SYSTEM SOFTWARE","",1,285000,285000]
[null,"","","SYSTEM SUPPORT SOFTWARE &     DEVICES","",1,28000,28000]
[null,"","","TMC BUILDING MODIFICATIONS","",1,32260.6,32260.6]
[null,"","","TRAINING","",1,71507,71507]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","#4 SOLID BARE COPPER GROUNDING","CONDUCTOR",350,6.4671428571428597,2263.5]
[null,"","","#4 SOLID BARE COPPER GROUNDINGCONDUCTOR","",660,10.61,7002.6]
[null,"","","#4 SOLID BARE GROUNDING","CONDUCTOR",750,9.1,6825]
[null,"","","#4 SOLID BARE GROUNDING       CONDUCTOR","",2000,6.5,13000]
[null,"","","3 WIRE COPPER FEEDER CON-     DUCTORS","",430,3,1290]
[null,"","","3-WIRE COPPER FEEDER","CONDUCTORS",775,10.1,7827.5]
[null,"","","3-WIRE COPPER FEEDER CONDUC-","TORS",500,5,2500]
[null,"","","3-WIRE COPPER FEEDER CONDUC-  TORS","",7825,4.7269009584664499,36988]
[null,"","","3-WIRE COPPER SERVICE","ENTRANCE CONDUCTORS",30,16.48,494.4]
[null,"","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",130,9.6538461538461497,1255]
[null,"","","4-WIRE COPPER FEEDER","CONDUCTORS",2090,15.9401913875598,33315]
[null,"","","4-WIRE COPPER FEEDER CONDUC-","TORS",400,6,2400]
[null,"","","4-WIRE COPPER FEEDER CONDUC-  TORS","",3670,6.2354768392370596,22884.2]
[null,"","","AERIAL CABLE PROTECTOR","",75,20,1500]
[null,"","","BACK PULL FIBER OPTIC CABLE","",1235,2.7210526315789498,3360.5]
[null,"","","BRIDGE MOUNTED CONDUIT","",1115,122,136030]
[null,"","","CONDUIT THROUGH ROCK","(1 CONDUIT, 2\")",384,46,17664]
[null,"","","","(2 CONDUITS, 2\")",6,56,336]
[null,"","","","(3 CONDUITS, 2\")",2341,61,142801]
[null,"","","ETHERNET CABLE","",3887,4.4511191149987104,17301.5]
[null,"","","UNDERGROUND CONDUIT (1, 1\")","",185,10.5,1942.5]
[null,"","","UNDERGROUND CONDUIT (1, 2\")","",1955,10.5,20527.5]
[null,"","","UNDERGROUND CONDUIT (2, 2\")","",24158,9.5,229501]
[null,"","","UNDERGROUND CONDUIT (3, 2\")","",40,40,1600]
[null,"7991000000-E","GENERIC SIGNAL ITEM (SF)","BRICK PAVERS","",8,340,2720]
[null,"7992000000-E","GENERIC SIGNAL ITEM (CY)","DMS FOUNDATION","",15,1125,16875]
[null,"","","DRILLED PIER FOUNDATION","",6,1100,6600]
[null,"","","METAL POLE FOUNDATION","",36,1200,43200]
[null,"","","OVERHEAD FOOTINGS","",32,1013.5,32432]
[null,"8007000000-N","CM&R TEMP STR ***********","(13+24.00 -DET-)","",1,175000,175000]
[null,"","","(15+60.50-DET-)","",1,350000,350000]
[null,"","","(53+43.00 -DET-)","",1,124000,124000]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(15+61.00-L-)","",1,40000,40000]
[null,"","","(16+99.00 -L-)","",1,81817.240000000005,81817.240000000005]
[null,"","","(164+30.00 -L-)","",1,326500,326500]
[null,"","","(17+00.00-L-)","",1,50000,50000]
[null,"","","(23+80.00 -L-)","",1,37700,37700]
[null,"","","(25+06.00 -L1-)","",1,1334494.45,1334494.45]
[null,"","","(30+80.00-L-)","",1,885000,885000]
[null,"","","(32+31.61 -L-)","",1,260000,260000]
[null,"","","(34+65.50 -L-)","",1,472950,472950]
[null,"","","(34+75.00 -L-)","",1,14392000,14392000]
[null,"","","(390+15.00 -L- LT)","",1,2245000,2245000]
[null,"","","(41+45.00 -L1-)","",1,519160.26,519160.26]
[null,"","","(45+22.65 -EBL-)","",1,1,1]
[null,"8021000000-N","REMV EXIST STR **********","(18+27.98 -L-)","",1,145457.97,145457.97]
[null,"","","(19+07.12 -L-)","",1,180000,180000]
[null,"","","(23+80.00 -L-)","",1,88330,88330]
[null,"","","(25+06.00 -L1-)","",1,234449.33,234449.33]
[null,"","","(28+02.81 -L-)","",1,183000,183000]
[null,"","","(34+65.50 -L-)","",1,608438.31000000006,608438.31000000006]
[null,"8035000000-N","REMV EXIST STR **********","(12+94.70 -L-)","",1,20000,20000]
[null,"","","(1260+34.00 -L-)","",1,115000,115000]
[null,"","","(13+34.00 -L-)","",1,55000,55000]
[null,"","","(13+78.50 -L-)","",1,54000,54000]
[null,"","","(1391+19.65 -L-)","",1,90000,90000]
[null,"","","(15+23.00 -L-)","",1,33750,33750]
[null,"","","(15+45.00 -L-)","",1,48705,48705]
[null,"","","(15+50.00 -L-)","",1,35000,35000]
[null,"","","(15+61.00-L-)","",1,110000,110000]
[null,"","","(16+08.00 -L-)","",1,21000,21000]
[null,"","","(16+10.00 -L-)","",1,45000,45000]
[null,"","","(16+62.00-L-)","",1,50000,50000]
[null,"","","(16+92.70 -L-)","",1,162620.93,162620.93]
[null,"","","(16+99.00 -L-)","",1,165000,165000]
[null,"","","(164+30.00 -L-)","",1,250000,250000]
[null,"","","(17+00.00-L-)","",1,100000,100000]
[null,"","","(17+07.50 -Y2-)","",1,212000,212000]
[null,"","","(17+37.36 -L-)","",1,512000,512000]
[null,"","","(17+68.00 -L-)","",1,44850,44850]
[null,"","","(18+27.00 -L-)","",1,140000,140000]
[null,"","","(18+28.00 -L-)","",1,52350,52350]
[null,"","","(18+30.00 -L-)","",1,30000,30000]
[null,"","","(19+56.99 -L-)","",1,120000,120000]
[null,"","","(21+37.00 -L REV-)","",1,44000,44000]
[null,"","","(21+68.50 -L-)","",1,135000,135000]
[null,"","","(23+06.50-L-)","",1,195000,195000]
[null,"","","(23+55.00 -L-)","",1,105000,105000]
[null,"","","(23+71.50 -L-)","",1,29000,29000]
[null,"","","(24+78.90 -L-)","",1,72500,72500]
[null,"","","(25+31.59 -Y18-)","",1,140000,140000]
[null,"","","(26+05.28 -Y14-)","",1,115000,115000]
[null,"","","(26+80.73 -Y17-)","",1,175000,175000]
[null,"","","(27+02.26 -L-)","",1,125000,125000]
[null,"","","(27+09.19 -Y16-)","",1,105000,105000]
[null,"","","(27+79.00 -L-)","",1,87550,87550]
[null,"","","(28+85.96 -L-)","",1,156500,156500]
[null,"","","(30+68.60 -L-)","",1,686359,686359]
[null,"","","(30+80.00-L-)","",1,293000,293000]
[null,"","","(32+31.61 -L-)","",1,275000,275000]
[null,"","","(34+75.00 -L-)","",1,2000000,2000000]
[null,"","","(35+30.22 -L-)","",1,948000,948000]
[null,"","","(369+42.00 -L- EBL)","",1,92000,92000]
[null,"","","(390+15.00 -L- RT)","",1,350000,350000]
[null,"","","(41+39.51 -Y-)","",1,155938.01999999999,155938.01999999999]
[null,"","","(41+45.00 -L1-)","",1,87032.19,87032.19]
[null,"","","(42+87.26 -Y1-)","",1,168000,168000]
[null,"","","(45+22.65 -EBL-)","",1,4105318.81,4105318.81]
[null,"8042000000-N","REMV EXIST STRS *********","(1002+79.68 -L REV-)","",1,190000,190000]
[null,"8056000000-N","REMV EXIST STR **********","(1042+08.93 -L-)","",1,125000,125000]
[null,"","","(14+99.00 -Y4-)","",1,55000,55000]
[null,"","","(22+44.41 -L-)","",1,23300,23300]
[null,"","","(226+01.00 -L-)","",1,19575,19575]
[null,"","","(28+84.00 -Y7-)","",1,22000,22000]
[null,"","","(30+13.47 -Y115REV-)","",1,30332.48,30332.48]
[null,"","","(316+72.00 -L-)","",1,19575,19575]
[null,"","","(64+15.00 -L-)","",1,22750,22750]
[null,"","","(83+76.00 -L-)","",1,19575,19575]
[null,"","","(874+45.00 -L3-)","",1,38600,38600]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",45,5360.5555555555602,241225]
[null,"8070000000-E","FOUNDATION EXCAVATION BRIDGE","","",629,32.5,20442.5]
[null,"8084000000-N","FND EXCAV EB** STA*******","(1, 35+30.22.-L-)","",1,16000,16000]
[null,"","","(2, 35+30.22-L-)","",1,16000,16000]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 18+27.98 -L-)","",1,8600,8600]
[null,"","","(1, 19+07.12 -L-)","",1,13500,13500]
[null,"","","(1, 19+56.99 -L-)","",1,75175,75175]
[null,"","","(1, 20+88.94 -Y19-)","",1,22200,22200]
[null,"","","(1, 22+26.35 -Y1B-)","",1,15082.44,15082.44]
[null,"","","(1, 26+05.28 -Y14-)","",1,8000,8000]
[null,"","","(1, 26+80.73 -Y17-)","",1,9000,9000]
[null,"","","(1, 27+09.19 -Y16-)","",1,7000,7000]
[null,"","","(1, 28+39.21 -Y29-)","",1,5000,5000]
[null,"","","(1, 30+12.56 -L-)","",1,162480,162480]
[null,"","","(1, 30+65.33 -Y1B-)","",1,10000,10000]
[null,"","","(1, 41+39.51 -Y-)","",1,53490.21,53490.21]
[null,"","","(1, 42+88.27 -Y1-)","",1,39500,39500]
[null,"","","(1, 58+33.94 -Y15FLYCA-)","",1,35948.28,35948.28]
[null,"","","(1, 60+66.06 -Y15FLYAC-)","",1,27643.26,27643.26]
[null,"","","(2, 47+63.62 -Y15FLYBD-)","",1,17732.189999999999,17732.189999999999]
[null,"","","(2, 60+66.06 -Y15FLYAC-)","",1,15528.2,15528.2]
[null,"","","(3, 47+63.62 -Y15FLYBD-)","",1,23622.65,23622.65]
[null,"","","(3, 58+33.94 -Y15FLYCA-)","",1,27245.15,27245.15]
[null,"","","(3, 60+66.06 -Y15FLYAC-)","",1,13683.43,13683.43]
[null,"","","(4, 47+63.62 -Y15FLYBD-)","",1,18719.59,18719.59]
[null,"","","(4, 58+33.94 -Y15FLYCA-)","",1,33346.97,33346.97]
[null,"","","(4, 60+66.06 -Y15FLYAC-)","",1,13681.42,13681.42]
[null,"","","(5, 47+63.62 -Y15FLYBD-)","",1,27212.12,27212.12]
[null,"","","(5, 58+33.94 -Y15FLYCA-)","",1,15879.52,15879.52]
[null,"","","(5, 60+66.06 -Y15FLYAC-)","",1,21367.7,21367.7]
[null,"","","(6, 47+63.62 -Y15FLYBD-)","",1,19829.21,19829.21]
[null,"","","(6, 58+33.94 -Y15FLYCA-)","",1,37299.519999999997,37299.519999999997]
[null,"","","(6, 60+66.06 -Y15FLYAC-)","",1,19923.3,19923.3]
[null,"","","(7, 58+33.94 -Y15FLYCA-)","",1,14083.78,14083.78]
[null,"","","(8, 60+66.06 -Y15FLYAC-)","",1,6194.44,6194.44]
[null,"","","(9, 60+66.06-Y15FLYAC-)","",1,22168.42,22168.42]
[null,"8096000000-E","PILE EXCAVATION IN SOIL","","",560,214.78419642857099,120279.15]
[null,"8097000000-E","PILE EXCAVATION NOT IN SOIL","","",435,333.551379310345,145094.85]
[null,"8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",192.8,630.716182572614,121602.08]
[null,"","","(5'-0\")","",320.32,1401.3437812187799,448878.44]
[null,"","","(6'-0\")","",47,1272.93,59827.71]
[null,"8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",81,1313.46913580247,106391]
[null,"8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",110,1249.72727272727,137470]
[null,"8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",234.7,944.00345121431599,221557.61]
[null,"8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",264,1488.03818181818,392842.08]
[null,"","","(5'-0\")","",317,1361.78567823344,431686.06]
[null,"","","(5'-6\")","",140,1279.33,179106.2]
[null,"8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",91,1289.16483516484,117314]
[null,"8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",242.6,1535.61158285243,372539.37]
[null,"8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",278,1039.76086330935,289053.52]
[null,"8108000000-E","**'-**\" DIA DRILLD PIERS","(4'-6\")","",729,760,554040]
[null,"8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",202.4,393.36462450592899,79617]
[null,"","","(5'-0\")","",146.32,574.15848824494299,84010.87]
[null,"8111200000-E","PERM STL CASING FOR 3' PIER","","",26,240,6240]
[null,"8112730000-N","PDA TESTING","","",97,3335.7982474226801,323572.43]
[null,"8113000000-N","SID INSPECTIONS","","",26,643.11538461538498,16721]
[null,"8114000000-N","SPT TESTING","","",22,909.12,20000.64]
[null,"8115000000-N","CSL TESTING","","",25,2947.5632000000001,73689.08]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(12+94.70 -L-)","",1,10000,10000]
[null,"","","(1260+34.00 -L-)","",1,80000,80000]
[null,"","","(13+34.00 -L-)","",1,9000,9000]
[null,"","","(13+78.50 -L-)","",1,10000,10000]
[null,"","","(1391+19.65 -L-)","",1,75000,75000]
[null,"","","(15+23.00 -L-)","",1,2700,2700]
[null,"","","(15+45.00 -L-)","",1,11500,11500]
[null,"","","(15+50.00 -L-)","",1,15000,15000]
[null,"","","(15+61.00-L-)","",1,40000,40000]
[null,"","","(16+08.00 -L-)","",1,15000,15000]
[null,"","","(16+10.00 -L-)","",1,16000,16000]
[null,"","","(16+62.00-L-)","",1,5000,5000]
[null,"","","(16+92.70 -L-)","",1,12000,12000]
[null,"","","(16+99.00 -L-)","",1,5000,5000]
[null,"","","(164+30.00 -L-)","",1,14900,14900]
[null,"","","(17+00.00-L-)","",1,40000,40000]
[null,"","","(17+37.36 -L-)","",1,24000,24000]
[null,"","","(17+68.00 -L-)","",1,2000,2000]
[null,"","","(18+27.00-L-)","",1,12500,12500]
[null,"","","(18+28.00 -L-)","",1,2500,2500]
[null,"","","(18+30.00 -L-)","",1,8500,8500]
[null,"","","(19+07.12 -L-)","",1,42500,42500]
[null,"","","(21+37.00 -L REV-)","",1,11000,11000]
[null,"","","(22+44.41 -L-)","",1,140000,140000]
[null,"","","(23+06.50-L-)","",1,8000,8000]
[null,"","","(23+55.00 -L-)","",1,30000,30000]
[null,"","","(23+71.50 -L-)","",1,3000,3000]
[null,"","","(23+80.00 -L-)","",1,6790,6790]
[null,"","","(24+78.90 -L-)","",1,15000,15000]
[null,"","","(25+06.00 -L1-)","",1,1611.47,1611.47]
[null,"","","(26+05.28 -Y14-)","",1,6000,6000]
[null,"","","(26+80.73 -Y17-)","",1,5000,5000]
[null,"","","(28+02.81 -L-)","",1,48000,48000]
[null,"","","(28+85.96 -L-)","",1,110000,110000]
[null,"","","(30+68.60 -L-)","",1,261923,261923]
[null,"","","(30+80.00-L-)","",1,8000,8000]
[null,"","","(32+31.61 -L-)","",1,52000,52000]
[null,"","","(369+42.00 -L- EBL)","",1,11000,11000]
[null,"","","(390+15.00 -L- LT)","",1,10000,10000]
[null,"","","(390+15.00 -L- RT)","",1,10000,10000]
[null,"","","(45+22.65 -EBL-)","",1,2300,2300]
[null,"8126000000-N","CULV EXCAV @ ************","(1042+08.93 -L-)","",1,80000,80000]
[null,"","","(1220+34.00 -L-)","",1,200000,200000]
[null,"","","(132+88.62 -L-)","",1,37890,37890]
[null,"","","(14+99.00 -Y4-)","",1,66450,66450]
[null,"","","(15+47.41 -NBCD-)","",1,30000,30000]
[null,"","","(155+30.40 -L-)","",1,5100,5100]
[null,"","","(172+34.91 -L-)","",1,10400,10400]
[null,"","","(18+22.67 -Y5B-)","",1,91946.9,91946.9]
[null,"","","(19+75.11 -Y5B-)","",1,34773.54,34773.54]
[null,"","","(19+90.69 -Y2-)","",1,19250,19250]
[null,"","","(226+01.00 -L-)","",1,56795,56795]
[null,"","","(28+84.00 -Y7-)","",1,36000,36000]
[null,"","","(30+13.47 -Y115REV-)","",1,127508.06,127508.06]
[null,"","","(316+72.00 -L-)","",1,63595,63595]
[null,"","","(35+53.70 -Y15RPDREV-)","",1,74937.38,74937.38]
[null,"","","(35+91.00 -Y33-)","",1,35000,35000]
[null,"","","(43+66.60 -Y15FLYCA-)","",1,63865.88,63865.88]
[null,"","","(45+66.21 -Y4-)","",1,150000,150000]
[null,"","","(45+66.22 -L-)","",1,15700,15700]
[null,"","","(46+07.79 -Y-)","",1,75000,75000]
[null,"","","(46+80.60 -L-)","",1,13400,13400]
[null,"","","(56+34.85 -L-)","",1,130000,130000]
[null,"","","(64+15.00 -L-)","",1,53490,53490]
[null,"","","(735+38.59 -L3-)","",1,247200,247200]
[null,"","","(768+62.23 -L-)","",1,268837.09999999998,268837.09999999998]
[null,"","","(79+82.10 -L-)","",1,29600,29600]
[null,"","","(792+88.12 -L-)","",1,96061.66,96061.66]
[null,"","","(797+66.00 -L3-)","",1,130100,130100]
[null,"","","(83+76.00 -L-)","",1,71560,71560]
[null,"","","(830+02.00 -L3-)","",1,278700,278700]
[null,"","","(874+45.00 -L3-)","",1,92100,92100]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",13636,68.832498533294199,938599.95]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",920849,45.456215850807197,41858310.909999996]
[null,"8154000000-E","REINF CONC DECK SLAB,LTWT","","",110595,100,11059500]
[null,"8156000000-E","CONCRETE WEARING SURFACE","","",2789,18.5,51596.5]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",1542406.8,0.83668641761692997,1290510.82]
[null,"8175000000-E","CLASS AA CONC (BRIDGE)","","",12001.1,1244.5563323362001,14936045]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",12602.2,1094.6094840583401,13794487.640000001]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",18993.900000000001,543.555713676496,10324242.869999999]
[null,"8203000000-E","CLASS A CONCRETE RET WALL","","",28,718,20104]
[null,"8210000000-N","BRG APPR SLAB ***********","(1002+79.68 -L REV-)","",1,220000,220000]
[null,"","","(12+94.70 -L-)","",1,38000,38000]
[null,"","","(1260+34.00 -L-)","",1,220000,220000]
[null,"","","(13+34.00 -L-)","",1,37000,37000]
[null,"","","(13+78.50 -L-)","",1,37000,37000]
[null,"","","(1391+19.65 -L-)","",1,220000,220000]
[null,"","","(15+23.00 -L-)","",1,27350,27350]
[null,"","","(15+45.00 -L-)","",1,48700,48700]
[null,"","","(15+50.00 -L-)","",1,25000,25000]
[null,"","","(15+61.00-L-)","",1,35000,35000]
[null,"","","(16+08.00 -L-)","",1,31500,31500]
[null,"","","(16+10.00 -L-)","",1,25000,25000]
[null,"","","(16+62.00-L-)","",1,25000,25000]
[null,"","","(16+92.70 -L-)","",1,47100,47100]
[null,"","","(16+99.00 -L-)","",1,51000,51000]
[null,"","","(164+30.00 -L-)","",1,204500,204500]
[null,"","","(17+00.00-L-)","",1,45000,45000]
[null,"","","(17+37.36 -L-)","",1,50000,50000]
[null,"","","(17+68.00 -L-)","",1,25200,25200]
[null,"","","(18+27.00 -L-)","",1,44000,44000]
[null,"","","(18+27.98 -L-)","",1,58550,58550]
[null,"","","(18+28.00 -L-)","",1,25150,25150]
[null,"","","(18+30.00 -L-)","",1,34000,34000]
[null,"","","(19+07.12 -L-)","",1,41000,41000]
[null,"","","(19+56.99 -L-)","",1,33850,33850]
[null,"","","(20+88.94 -Y19-)","",1,55100,55100]
[null,"","","(21+37.00 -L REV-)","",1,27940,27940]
[null,"","","(21+68.50 -L-)","",1,55000,55000]
[null,"","","(217+31.76 -L-) LT","",1,70000,70000]
[null,"","","(217+31.76 -L-) RT","",1,64000,64000]
[null,"","","(22+26.35 -Y1B-)","",1,40455.980000000003,40455.980000000003]
[null,"","","(23+06.50-L-)","",1,26000,26000]
[null,"","","(23+43.03 -Y16-)","",1,38428.32,38428.32]
[null,"","","(23+55.00 -L-)","",1,25000,25000]
[null,"","","(23+71.50 -L-)","",1,32690,32690]
[null,"","","(23+80.00 -L-)","",1,36770,36770]
[null,"","","(24+78.90 -L-)","",1,70000,70000]
[null,"","","(25+06.00 -L1-)","",1,41341.58,41341.58]
[null,"","","(26+05.28 -Y14-)","",1,95000,95000]
[null,"","","(26+65.52 -Y3-)","",1,110600,110600]
[null,"","","(26+80.73 -Y17-)","",1,55000,55000]
[null,"","","(27+01.91 -Y7-)","",1,46000,46000]
[null,"","","(27+02.26 -L-)","",1,55000,55000]
[null,"","","(27+09.19 -Y16-)","",1,87000,87000]
[null,"","","(27+79.00 -L-)","",1,30175,30175]
[null,"","","(28+02.81 -L-)","",1,39000,39000]
[null,"","","(28+39.21 -Y29-)","",1,34000,34000]
[null,"","","(28+85.96 -L-)","",1,135000,135000]
[null,"","","(30+65.33 -Y1B-)","",1,29406.240000000002,29406.240000000002]
[null,"","","(30+67.66 -Y4-)","",1,144311.93,144311.93]
[null,"","","(30+68.60 -L-)","",1,267425,267425]
[null,"","","(30+80.00-L-)","",1,28000,28000]
[null,"","","(31+30.81 -Y REV-)","",1,125000,125000]
[null,"","","(32+31.61 -L-)","",1,51354.93,51354.93]
[null,"","","(34+65.50 -L-)","",1,42525,42525]
[null,"","","(34+75.00 -L-)","",1,100000,100000]
[null,"","","(369+42.00 -L- EBL)","",1,52000,52000]
[null,"","","(369+42.00 -L- WBL)","",1,52000,52000]
[null,"","","(39+52.37 -Y14A-)","",1,110000,110000]
[null,"","","(390+15.00 -L- LT)","",1,52000,52000]
[null,"","","(390+15.00 -L- RT)","",1,52000,52000]
[null,"","","(41+39.51 -Y-)","",1,179585.72,179585.72]
[null,"","","(41+45.00 -L1-)","",1,29840.7,29840.7]
[null,"","","(42+56.82 -Y1-)","",1,64000,64000]
[null,"","","(45+22.65 -EBL-)","",1,58850,58850]
[null,"","","(47+28.33 -Y15REV-)","",1,233807.08,233807.08]
[null,"","","(47+63.62 -Y15FLYBD-)","",1,55192.76,55192.76]
[null,"","","(58+33.94 -Y15FLYCA-)","",1,55355.53,55355.53]
[null,"","","(60+66.06 -Y15FLYAC-)","",1,55871.19,55871.19]
[null,"","","(61+02.86 -L- LT)","",1,65155,65155]
[null,"","","(61+02.86 -L- RT)","",1,65155,65155]
[null,"","","(774+41.49 -L3- LT)","",1,66200,66200]
[null,"","","(774+41.49 -L3- RT)","",1,66200,66200]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",3909406,1.3602230645780999,5317664.21]
[null,"8224000000-E","EPOXY COAT REINF STL BRDG","","",85413,1.8142665636378501,154961.95000000001]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",159370,2.71803520110435,433173.27]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",2795837,1.6504350790121201,4614347.46]
[null,"8248000000-E","EPOXY COAT REINF STEEL","","",396,2.8,1108.8]
[null,"8252000000-E","REINF STEEL (RET WALL)","","",3002,1.55,4653.1000000000004]
[null,"8259000000-E","36\" PRESTR CONCRETE GIRDR","","",3503.38,254.838841347499,892797.3]
[null,"8262000000-E","45\" PRESTR CONCRETE GIRDR","","",786.88,255,200654.4]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",24210.11,335.31083460587303,8117912.1900000004]
[null,"8274000000-E","63\" MOD PRESTR CONC GIRDR","","",7662.84,393.170254109442,3012800.75]
[null,"8277000000-E","72\" MOD PRESTR CONC GIRDR","","",9081.81,378.00185315482298,3432941.01]
[null,"8280000000-E","STRUCTURAL STEEL","","",17429841,2.87675028131352,50141300]
[null,"8296000000-N","POLLUTION CONTROL","","",5,41085.127999999997,205425.64]
[null,"8328000000-E","PILE DRV EQUIP SETUP * PRESTR CONC PILES","(16\")","",42,2733.3333333333298,114800]
[null,"","","(24\" CARBON FIBER REINFORCED","POLYMER)",212,10000,2120000]
[null,"","","(24\")","",24,4300,103200]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",1294,1273.88485316847,1648407]
[null,"","","(HP 14 X 73)","",974,2092.2970020533899,2037897.28]
[null,"","","(HP12 X 53)","",50,1665.7239999999999,83286.2]
[null,"","","(HP12X53)","",129,968.80279069767403,124975.56]
[null,"8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",29,2730.12413793103,79173.600000000006]
[null,"","","(HP 14 X 89)","",16,550,8800]
[null,"","","(HP14X73)","",12,1750,21000]
[null,"","","(PP 18 X 0.50)","",47,2870.2127659574498,134900]
[null,"","","(PP 24 X 0.50)","",21,4069.5642857142898,85460.85]
[null,"","","(PP 30 X 0.50)","",55,8780.4887272727301,482926.88]
[null,"","","(PP 30 X 0.500)","",22,3650,80300]
[null,"","","(PP 36 X 0.50)","",20,6334.36,126687.2]
[null,"","","(PP 36 X 0.625)","",5,2500,12500]
[null,"8333000000-E","16\" PRESTR CONC PILES","","",2310,153.21212121212099,353920]
[null,"8350000000-E","24\" PRESTR CONC PILES","","",2520,200,504000]
[null,"8355000000-E","HP**X** PILES","(HP 14 X 73)","",355,68.59,24349.45]
[null,"8356000000-E","HP**X** GALV PILES","(HP 14 X 89)","",800,125,100000]
[null,"8364000000-E","HP12X53 PILES","","",82491,72.814146149276894,6006511.7300000004]
[null,"8384000000-E","HP14X73 PILES","","",47248,72.341910133762298,3418010.57]
[null,"8384200000-E","HP14X73 GALV PILES","","",2500,77.518720000000002,193796.8]
[null,"8385200000-E","PP**X**** GALV STL PILE","(24 X 0.50)","",480,139,66720]
[null,"","","(30 X 0.50)","",1790,232.66388268156399,416468.35]
[null,"","","(36 x 0.625)","",550,350,192500]
[null,"","","(PP 24 X 0.50)","",1450,126.89,183990.5]
[null,"","","(PP 30 X 0.50)","",2560,330,844800]
[null,"","","(PP 30 X 0.500)","",2530,325,822250]
[null,"","","(PP 36 X 0.50)","",2060,203.58,419374.8]
[null,"8386000000-E","PP18X0.50 STL PILE","","",525,145,76125]
[null,"8387000000-E","PP18X0.50 GALV STL PILE","","",2800,146.02857142857101,408880]
[null,"8391000000-N","STEEL PILE POINTS","","",508,256.870767716535,130490.35]
[null,"8392000000-N","PIPE PILE PLATES","","",82,358.42682926829298,29391]
[null,"8392500000-E","PREDRILLING FOR PILES","","",947,116.910073917635,110713.84]
[null,"8393000000-N","PILE REDRIVES","","",808,445.00396039603999,359563.2]
[null,"8475000000-E","TWO BAR METAL RAIL","","",12443.13,121.366086346442,1510173.99]
[null,"8482000000-E","THREE BAR METAL RAIL","","",1197.42,182.51069800070201,218541.96]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",28177.67,92.906181029162497,2617879.71]
[null,"8504000000-E","CONC BARR RAIL MOMENT SLAB","","",3316.74,388.48402346882801,1288500.5]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",6443.13,126.86748055680999,817423.67]
[null,"8510000000-E","CONCRETE MEDIAN BARRIER","","",1174.9000000000001,129.86489914035201,152578.26999999999]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-3 1/2\")","",354.1,77.160011296243994,27322.36]
[null,"","","(1'-2\" X 2'-6\")","",10682.47,102.702943233166,1097121.1100000001]
[null,"","","(1'-2\" X 2'-8 1/2\")","",207.43,120.699995179097,25036.799999999999]
[null,"","","(1'-2\" X 2'-9 1/2\")","",130,200,26000]
[null,"","","(1'-2\" X 3'-3 3/4\")","",481.4,99.490008309098499,47894.49]
[null,"","","(1'-2\" X 3'-3\")","",385.55,180,69399]
[null,"","","(1'-2\" X 3'-7\")","",453.67,176,79845.919999999998]
[null,"","","(1'-3\" X 2'-6\")","",36,225,8100]
[null,"8524000000-E","**\" CHAIN LINK FENCE","(104\")","",427.83,152,65030.16]
[null,"","","(72\")","",264,180,47520]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",14794.4,92.912406045530702,1374583.3]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",1022.4,91.125361893583701,93166.57]
[null,"8566000000-E","SURFACE PREP, CLASS III","","",316.8,530.571338383838,168085]
[null,"8590000000-E","RIP RAP, CLASS **","(A)","",85,81.92,6963.2]
[null,"","","(II)","",32,72.75,2328]
[null,"8594000000-E","RIP RAP B","","",120,74.0683333333333,8888.2000000000007]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",21859,56.472953932018797,1234442.3]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",28614,3.6603022995736398,104735.89]
[null,"8654000000-N","DISC BEARINGS","","",4,302730.92749999999,1210923.71]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",46,30354.808043478301,1396321.17]
[null,"8660000000-E","CONCRETE REPAIRS","","",776,826.98814432989695,641742.80000000005]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",4819.12,658.51256245953596,3173451.06]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",7371.3,98.985402846173699,729651.1]
[null,"8692000000-N","FOAM JOINT SEALS","","",11,27524.337272727302,302767.71000000002]
[null,"8706000000-N","EXPANSION JOINT SEALS","","",5,457697.728,2288488.64]
[null,"8713000000-N","MODULAR EXP JOINT SEALS","","",1,400140.2,400140.2]
[null,"8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(26+05.28 -Y14-)","",1,67000,67000]
[null,"","","(26+80.73 -Y17-)","",1,66000,66000]
[null,"","","(27+02.26 -L-)","",1,55550,55550]
[null,"","","(27+09.19 -Y16-)","",1,65000,65000]
[null,"","","(28+39.21 -Y29-)","",1,65000,65000]
[null,"","","(390+15.00 -L- LT)","",1,74500,74500]
[null,"","","(390+15.00 -L- RT)","",1,74500,74500]
[null,"8741000000-N","STR DRN SYS ************","(34+75.00 -L-)","",1,587880,587880]
[null,"8744000000-N","SOLAR ARRAY SUPPT PLTFORM","","",1,26000,26000]
[null,"8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",990,236.46,234095.4]
[null,"8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",5220,181.72988505747099,948630]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",11185,197.61528833258799,2210327]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",49811,77.551188492501694,3862902.25]
[null,"","","(10)","",9625,70.39,677503.75]
[null,"","","(11)","",14880,70.39,1047403.2]
[null,"","","(12)","",8105,70.39,570510.94999999995]
[null,"","","(13)","",4770,70.39,335760.3]
[null,"","","(2)","",66362,64.954918477441893,4310538.3]
[null,"","","(3)","",15382,62.2207905343909,957080.2]
[null,"","","(4)","",2015,70.39,141835.85]
[null,"","","(5)","",6270,70.39,441345.3]
[null,"","","(6)","",7430,89.608795423956906,665793.35]
[null,"","","(7)","",8265,70.39,581773.35]
[null,"","","(8)","",4135,70.39,291062.65000000002]
[null,"","","(9)","",16210,70.39,1141021.8999999999]
[null,"","","(W3)","",4063,64,260032]
[null,"","","(W6)","",791,66,52206]
[null,"","","(W8)","",917,69,63273]
[null,"","","(W9)","",316,93,29388]
[null,"","","W1-1 (I-5878)","",8300,67,556100]
[null,"","","W1-1 (I-5883)","",3800,68,258400]
[null,"","","W1-2 (I-5878)","",4275,70,299250]
[null,"","","W1-2 (I-5883)","",3400,68,231200]
[null,"","","W2-1 (I-5878)","",5750,69,396750]
[null,"","","W2-1 (I-5883)","",3500,70,245000]
[null,"","","W2-1 (I-5986B)","",2830,70,198100]
[null,"","","W2-2 (I-5878)","",4880,71,346480]
[null,"","","W2-2 (I-5883)","",3800,67,254600]
[null,"","","W2-2 (I-5986B)","",2770,70,193900]
[null,"8802010000-E","SOIL NAIL RETAINING WALLS","","",2672,123.1,328923.2]
[null,"8802014000-E","SOLDIER PILE RETAINING WALLS","","",1955,200,391000]
[null,"8802015100-N","SOIL NAIL VERIFICATION TESTS","","",2,1670,3340]
[null,"8802015110-N","SOIL NAIL PROOF TESTS","","",10,725,7250]
[null,"8802016000-E","ANCHORED RETAINING WALLS","","",6330,271,1715430]
[null,"8802030000-E","SEGMENTAL GRAVITY RETAIN WALLS","","",450,225,101250]
[null,"8802040000-E","CIP GRAVITY RETAINING WALLS","","",6505,123.31429669485,802159.5]
[null,"8804000000-N","GENERIC CULVERT ITEM (LS)","ALUMINUM BOX CULVERT @","STA 132+88.62 -L-",1,253470,253470]
[null,"","","","STA 79+82.10 -L-",1,248220,248220]
[null,"","","ASBESTO ASSESSMENT","",1,4500,4500]
[null,"","","ASBESTOS ASSESSMENT","",1,6000,6000]
[null,"","","CHANNEL SUBSTRATE MATERIALS","",1,35000,35000]
[null,"","","PRECAST REINFORCED CONCRETE   THREE","SIDED CULVERT @ STA 22+44.41 L",1,200000,200000]
[null,"8811000000-E","GENERIC CULVERT ITEM (LF)","ANODIZED TWO BAR METAL RAIL","",28.5,165,4702.5]
[null,"","","GALVANIZED RAILS","",164.88,150,24732]
[null,"","","MOMENT SLAB","",166,362,60092]
[null,"8821000000-E","GENERIC CULVERT ITEM (SF)","18\" STEEL SHEET PILES","",440,97,42680]
[null,"","","ARCHITECTURAL SURFACE TREAT-  MENT","",1274,46,58604]
[null,"8839000000-E","GENERIC RET WALL ITEM (LF)","ANODIZED TWO BAR METAL RAIL","",188,165,31020]
[null,"","","CONCRETE SHEET PILE RETAINING WALL","",660.5,4760,3143980]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL CONCRETE SURFACE","TREATMENT",41169,5.4,222312.6]
[null,"","","","TREATMENT (WALL)",33833,5.0999999999999996,172548.3]
[null,"","","ARCHITECTURAL CONCRETE SURFACETREATMENT","",5445,1,5445]
[null,"","","ARCHITECTURAL SURFACE         TREATMENT","",37450,3,112350]
[null,"","","ARCHITECTURAL SURFACE TREAT-  MENT","",708339,2.3116708948681399,1637446.65]
[null,"","","CIP CANTILEVER RETAINING WALLS","",978,268,262104]
[null,"","","REINFORCED RETAINING WALL     BACKFILL","",7315,44.77,327492.55]
[null,"","","REINFORCED RETAINING WALL BACKFILL","",8056,90,725040]
[null,"","","SHEET PILE CUTOFF WALL","",5730,53,303690]
[null,"","","SHEET PILE RETAINING WALL","",28945,33.94,982393.3]
[null,"","","SOUND BARRIER WALL 1","",56818,29.41,1671017.38]
[null,"","","SOUND BARRIER WALL 2","",85427,29.37,2508990.9900000002]
[null,"","","SOUND BARRIER WALL 3","",87297,29.53,2577880.41]
[null,"","","SOUND BARRIER WALL 4","",108020,29.63,3200632.6]
[null,"","","SOUND BARRIER WALL NO -NW11-","",18303,39.1,715647.3]
[null,"","","SOUND BARRIER WALL NO -NW13-","",26005,39.1,1016795.5]
[null,"","","SOUND BARRIER WALL NO -NW15-","",7308,39.299999999999997,287204.40000000002]
[null,"","","SOUND BARRIER WALL NO -NW5A-","",14210,39.1,555611]
[null,"","","SOUND BARRIER WALL NO -NW5B-","",8208,39.1,320932.8]
[null,"","","SOUND BARRIER WALL NO -NW8-","",18010,39.299999999999997,707793]
[null,"","","SOUND BARRIER WALL NO. NW29-1","",3720,50,186000]
[null,"","","SOUND BARRIER WALL NO. NW32-1","",7570,45,340650]
[null,"","","SOUND BARRIER WALL NO. NW33-1","",16160,45,727200]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","ACCESS & FALL PROTECTION","",1,800000,800000]
[null,"","","BEARING REPAIRS","",1,12000,12000]
[null,"","","BRIDGE DECK DE-ICING SYSTEM","",1,795000,795000]
[null,"","","CLEANING & PAINTING EXISTING","WEATHERING STEEL",1,828000,828000]
[null,"","","CLEANING & PAINTING OF EXIST-","ING WEATHING STEEL FOR BRIDGE #495",1,123000,123000]
[null,"","","CLEANING & REPAINTING OF","BRIDGE #320",1,400000,400000]
[null,"","","","BRIDGE #330",1,600000,600000]
[null,"","","","BRIDGE #705",1,1025045.4,1025045.4]
[null,"","","CLEANING AND PAINTING EXISTING","WEATHERING STEEL FOR BRIDGE   NO 500051",1,104114.72,104114.72]
[null,"","","CONST, MAINT, & REM OF TEMP   STRUCTURE","AT STA 18+76.04-L_DET-",1,470000,470000]
[null,"","","CONTAINMENT OVER CHARLOTTE","AREA TRANSIT SYSTEM RAIL LINE",1,67000,67000]
[null,"","","FIELD MEASURING","",1,8450,8450]
[null,"","","GUSSET PLATE RETROFIT","",1,55000,55000]
[null,"","","HEAT STRAIGHTENING STEEL BEAM","REPAIR, BRIDGE #770012",1,90000,90000]
[null,"","","MOLDED RUBBER SEGMENTAL EXPAN-","SION JOINTS",1,600000,600000]
[null,"","","MOLDED RUBBER SEGMENTAL EXPAN-SION JOINT","",1,150000,150000]
[null,"","","MURAL PAINT REPAIR","",1,50000,50000]
[null,"","","PAINTING CONTAINMENT","",1,72000,72000]
[null,"","","PAINTING CONTAINMENT FOR","BRIDGE #320",1,60000,60000]
[null,"","","","BRIDGE #322",1,25000,25000]
[null,"","","","BRIDGE #326",1,40000,40000]
[null,"","","","BRIDGE #327",1,40000,40000]
[null,"","","","BRIDGE #328",1,40000,40000]
[null,"","","","BRIDGE #330",1,75000,75000]
[null,"","","","BRIDGE #332",1,30000,30000]
[null,"","","","BRIDGE #481",1,10302,10302]
[null,"","","","BRIDGE #495",1,51510,51510]
[null,"","","","BRIDGE #640021",1,110000,110000]
[null,"","","","BRIDGE #705",1,412080,412080]
[null,"","","","BRIDGE #770010",1,15000,15000]
[null,"","","","BRIDGE #770012",1,15000,15000]
[null,"","","","BRIDGE NO 500051",1,85184.77,85184.77]
[null,"","","PLASTIC LUMBER FENDER BOARDS","AT CHANNEL BENTS",1,55000,55000]
[null,"","","POLLUTION CONTROL","",1,212000,212000]
[null,"","","POST TENSIONING ENCASEMENT","",1,62639.48,62639.48]
[null,"","","POST TENSIONING TENDONS","",1,41963.519999999997,41963.519999999997]
[null,"","","POST-TENSIONING ANCHORAGE","",1,750000,750000]
[null,"","","POST-TENSIONING BARS","",1,120000,120000]
[null,"","","SPOT PAINTING OF STEEL STRUC-","TURE REPAIR AREAS",2,252953,505906]
[null,"","","STRIP SEAL EXPANSION JOINTS","",3,96450,289350]
[null,"","","TRAFFIC SIGNAL EXTENSION","",1,5500,5500]
[null,"","","VOLUMETRIC MIXER","",4,22750,91000]
[null,"","","WELD REPAIR W1","",1,130,130]
[null,"","","WELD REPAIR W2","",1,210,210]
[null,"","","WELD REPAIR W3","",1,130,130]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","24\" CARBON FIBER REINFORCED     POLYMER","PRESTRESSED CONCRETE PILES",20970,89.5,1876815]
[null,"","","3'-0\" X 2'-6\" PRESTRESSED","CONCRETE BENT CAPS",153.32,925,141821]
[null,"","","36\" FLORIDA I-BEAM","(FIB) GIRDERS",1833.33,315,577498.94999999995]
[null,"","","36\" FLORIDA I-BEAM CONCRETE   GIRDER","",745,651,484995]
[null,"","","4 BAR METAL RAIL","",1158,285,330030]
[null,"","","45\" PREST CONC FLORIDA        I-BEAM","",7090.17,475,3367830.75]
[null,"","","54\" CARBON FIBER REINFORCED     POLYMER","F.I.B. PRESTRESSED CONCRETE      GIRDERS",5579.64,460,2566634.4]
[null,"","","54\" FLORIDA I-BEAM CONCRETE   GIRDER","",962,807,776334]
[null,"","","63\" PRESTRESSED CONCRETE","FLORIDA I-BEAM GIRDERS",4566.33,338.03000002189901,1543556.53]
[null,"","","72\" CARBON FIBER REINFORCED      POLYMER","F.I.B. PRESTRESSED CONCRETE      GIRDERS",5707.35,410,2340013.5]
[null,"","","78\" CARBON FIBER REINFORCED      POLYMER","F.I.B. PRESTRESSED CONCRETE      GIRDERS",1815.18,515,934817.7]
[null,"","","ASPHALT JOINT REPAIR/REPLACE-","MENT (20\" WIDE, W/PLATE)",1716,150,257400]
[null,"","","ASPHALT PLUG JOINT REPAIR/RE-","PLACEMENT (18\"-24\" WIDE, W/ PLATE)",1660,185,307100]
[null,"","","","PLACEMENT (18\"-24\" WIDE, WITH PLATE)",250,195,48750]
[null,"","","CARBON FIBER REINFORCED","POLYMER (CFRP) STRAND",986059,6,5916354]
[null,"","","CLEAN BRIDGE DECK DRAINAGE    SYSTEM","",900,36.729999999999997,33057]
[null,"","","CONCRETE BARRIER RAIL","(ALL-LIGHTWEIGHT CONCRETE)",2208,149,328992]
[null,"","","CONCRETE MEDIAN BARRIER","(ALL-LIGHTWEIGHT CONCRETE)",1097,170,186490]
[null,"","","FIBER OPTIC CONDUIT SYSTEM","WITH HANGERS",832,122,101504]
[null,"","","","",3306.03,40.470280064004299,133795.96]
[null,"","","FOAM JOINT SEALS FOR","PRESERVATION",3936.9,52.895501536742103,208244.3]
[null,"","","FOAM JOINT SEALS FOR PRESER-  VATION","",1135,175,198625]
[null,"","","FOAM JOINT SEALS FOR PRESERVA-TION","",1807.9,78.946916311742896,142728.13]
[null,"","","GALVANIC CATHODIC PROTECTION","INTEGRAL PILE JACKET (MONI-   TORING)",40.5,1950,78975]
[null,"","","","INTEGRAL PILE JACKET (NON-MON-ITORING)",67.25,1935,130128.75]
[null,"","","GALVANIZED PEDESTRIAN SAFETY  RAIL","",869.25,115,99963.75]
[null,"","","GLASS FIBER REINFORCED POLYMER","(GFRP) BAR",199245.43,2.2500000125473401,448302.22]
[null,"","","PILE EXC FOR 24\" CARBON FIBER REINFORCED","POLYMER PRESTRESSED CONCRETE  PILES",7211,120,865320]
[null,"","","POURABLE SILICONE JOINT","SEALANT",98.2,45,4419]
[null,"","","POURABLE SILICONE JOINT       SEALANT","",491.87,51.179376664565801,25173.599999999999]
[null,"","","POURABLE SILICONE JOINT SEAL- ANT","",174.9,15,2623.5]
[null,"","","RAIL REPAIRS FOR ONE BAR METAL RAIL","",30,300,9000]
[null,"","","RAIL RETROFIT (2-BAR METAL    RAIL)","",2079,150,311850]
[null,"","","RAIL RETROFIT (3-BAR METAL    RAIL)","",360,265,95400]
[null,"","","SILICONE JOINT SEALANT","",365,70,25550]
[null,"","","SILICONE JOINT SEALANT FOR","SLOPE PROTECTION",743,80,59440]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","6000 PSI CONCRETE","",95.2,1637.66995798319,155906.18]
[null,"","","ASPHALT JOINT REPAIR/REPLACE-","MENT (18\"-24\" WIDE, W/ PLATE)",6,10395,62370]
[null,"","","EPOXY POLYMER CONCRETE","MATERIAL (ALTERNATE)",null,null,0]
[null,"","","","MATERIALS",null,null,0]
[null,"","","EPOXY POLYMER CONCRETE        MATERIALS","",149.80000000000001,4592.3481308411201,687933.75]
[null,"","","LATEX MODIFIED CONCRETE","OVERLAY-EARLY STRENGTH",102,1925,196350]
[null,"","","LATEX MODIFIED CONCRETE OVER-","LAY - EARLY STRENGTH",477.3,1182.0452545568801,564190.19999999995]
[null,"","","","LAY - VERY EARLY STRENGTH",116.8,1700,198560]
[null,"","","POLYESTER POLYMER CONCRETE    MATERIALS","",2559.4,2647.2767054778501,6775440]
[null,"8882000000-E","GENERIC STRUCTURE ITEM (CF)","CONCRETE FOR DECK REPAIR","",1793.6,15.2583574933095,27367.39]
[null,"","","ELASTOMERIC CONCRETE FOR","PRESERVATION",227.7,409.74931927975399,93299.92]
[null,"","","ELASTOMERIC CONCRETE FOR PRES-ERVATION","",414.1,596.66264187394302,247078]
[null,"","","ELASTOMETRIC CONCRETE FOR","PRESERVATION",77.400000000000006,325,25155]
[null,"","","PRESTRESSED CONCRETE GIRDER   REPAIR","",136.5,975,133087.5]
[null,"8889000000-E","GENERIC STRUCTURE ITEM (LB)","BEAM REPAIR","",745.1,60,44706]
[null,"","","BEAM REPAIR CUT-OUT","",5040,110,554400]
[null,"","","BEAM REPAIR PLATING","",4016,70,281120]
[null,"","","BOLTED BEAM REPAIR","",226.1,185,41828.5]
[null,"","","SLOPE PROTECTION VOID FILLING","",1500,10,15000]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","18\" GALVANIZED STEEL SHEET    PILES","",3592,55,197560]
[null,"","","ARCHITECTURAL CONCRETE SURFACE","TREATMENT (BRIDGE)",1246.4000000000001,45.990003209242602,57321.94]
[null,"","","BEAM END EPOXY COATING","",272.5,87,23707.5]
[null,"","","BRIDGE JOINT DEMOLITION","",2751.3,57.918969214553101,159352.46]
[null,"","","CATHODIC PROTECTION OF PILE","CAP (MONITORING)",888,176,156288]
[null,"","","","CAP (NON-MONITORING)",4179,125,522375]
[null,"","","CONCRETE DECK REPAIR FOR EPOXYOVERLAY","",0.2,1200,240]
[null,"","","CONCRETE FILLED GRID DECK","REPAIR FOR EPOXY OVERLAY",88,232,20416]
[null,"","","EPOXY COATING","",40407,8.7650374935036002,354168.87]
[null,"","","EPOXY COATING AND DEBRIS      REMOVAL","",2862,16,45792]
[null,"","","EPOXY OVERLAY SYSTEM I","",2229,53.978465679677001,120318]
[null,"","","EPOXY OVERLAY SYSTEM II","",44252,10,442520]
[null,"","","FIBER REINFORCED CONCRETE     DECKSLAB","(ALL-LIGHTWEIGHT CONCRETE)",75343,48,3616464]
[null,"","","JOINT REPAIR","",373,275,102575]
[null,"","","PRESTRESSED CONC GIRDERS WITH","THERMAL SPRAY ANODE (NON-MONI-TORING)",35966,45.15,1623864.9]
[null,"","","SILANE BARRIER RAIL TREATMENT","",2557,2.5,6392.5]
[null,"","","SILANE RAIL TREATMENTS","",2828,10,28280]
[null,"","","SILANE TREATMENTS","",3800,16.2,61560]
[null,"","","SURFACE PREPARATION FOR","CONCRETE BARRIER",2557,5,12785]
[null,"","","SURFACE PREPARATION FOR SILANE","RAIL TREATMENT",2828,15,42420]
[null,"","","","",3800,6.75,25650]
[null,"","","TOP OF CAP EPOXY COATINGS","",494,20.27,10013.379999999999]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","CONCRETE DECK REPAIR FOR","POLYESTER POLYMER CONCRETE OVERLAY",4.2,150,630]
[null,"","","","POLYMER CONCRETE OVERLAY",7.3,1013.32054794521,7397.24]
[null,"","","CONCRETE DECK REPAIR FOR POLY-","MER CONCRETE OVERLAY",82.8,85,7038]
[null,"","","HYDRO-DEMOLITION OF BRIDGE","DECK",2028.2,70,141974]
[null,"","","HYDRO-DEMOLITION OF BRIDGE    DECK","",12516.2,94.065259423786799,1177339.6000000001]
[null,"","","PLACING & FINISHING LATEX","MODIFIED CONC OVERLAY-EARLY   STRENGTH",2028.2,28,56789.599999999999]
[null,"","","PLACING & FINISHING LATEX MOD-","IFIED CONCRETE OVERLAY - EARLYSTRENGTH",10418.200000000001,40.927991399665999,426396]
[null,"","","PLACING & FINISHING PC OVERLAY","",1156,72,83232]
[null,"","","PLACING & FINISHING POLYESTER","POLYMER CONCRETE OVERLAY",12484.5,21.106732348111699,263507]
[null,"","","PLACING & FINISHING POLYMER","CONCRETE OVERLAY",39400,77.195925126903504,3041519.45]
[null,"","","PLACING AND FINISHING OF LATEXMODIFIED","CONCRETE OVERLAY-VERY EARLY   STRENGTH",2098,260,545480]
[null,"","","PLACING AND FINISHING POLYMER","CONCRETE OVERLAY",554,185,102490]
[null,"","","SCARIFYING BRIDGE DECK","",57118.9,29.141985927600199,1664558.18]
[null,"","","SHOTBLASTING BRIDGE DECK","",62916.5,6.3807810351815499,401456.41]
[null,"","","SILANE DECK TREATMENT","",8251,20.8736177433038,172228.22]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","9-5/8\" DIA MICROPILES","",196,10765.31,2110000.7599999998]
[null,"","","9-5/8\" DIAMETER MICROPILES","",10,34805,348050]
[null,"","","BEAM END EPOXY COATINGS","",30,1125,33750]
[null,"","","BEARING KEEPER PLATE","",10,5515,55150]
[null,"","","BEARING PLATE REPOSITIONING","",1,4000,4000]
[null,"","","BEARING REPLACEMENT","",2,4500,9000]
[null,"","","BRIDGE JACKING TYPE I","BRIDGE #640021",1,7500,7500]
[null,"","","BRIDGE WASHING","",30,3000,90000]
[null,"","","BULK ANODE","",8,850,6800]
[null,"","","CFRP PEDESTAL REPAIRS AND","BEARING RETROFIT",16,3000,48000]
[null,"","","CLEANING & PAINTING OF EXT    BEARINGS","WITH HIGH RATIO CALCIUM SULF-   ONATE",196,575,112700]
[null,"","","CLEANING AND PAINTING EXISTING","BEARINGS WITH HRSCA",72,1000,72000]
[null,"","","CLEANING AND PAINTING EXISTINGBEARINGS","WITH HIGH RATIO CALCIUM       SULFONATE",1336,800,1068800]
[null,"","","DEMONSTRATION MICROPILES","",1,26734.69,26734.69]
[null,"","","HOLE REPAIR TYPE I","",12,125,1500]
[null,"","","HOLE REPAIR TYPE II","",3,195,585]
[null,"","","HOLE REPAIR TYPE III","",1,250,250]
[null,"","","MICROPILE PROOF TESTS","",8,4591.84,36734.720000000001]
[null,"","","MICROPILE VERIFICATION TESTS","",1,20408.16,20408.16]
[null,"","","PACK RUST REPAIR TYPE I","",17,400,6800]
[null,"","","PACK RUST REPAIR TYPE II","",6,500,3000]
[null,"","","REMOVE AND RESET BEARINGS","",1,2000,2000]
[null,"","","STEEL BEARING KEEPER ANGLE    ASSEMBLY","",37,1800,66600]
[null,"","","TOP PIPE PILE PLATES","",35,107,3745]
[null,"","","TYPE I BRIDGE JACKING","BRIDGE #138",1,15000,15000]
[null,"","","","BRIDGE #320",1,15000,15000]
[null,"","","","BRIDGE #326",1,15000,15000]
[null,"","","","BRIDGE #327",1,15000,15000]
[null,"","","","BRIDGE #328",1,15000,15000]
[null,"","","","BRIDGE #330",1,15000,15000]
[null,"","","","BRIDGE #332",7,15000,105000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE","NO. 300433",3,7500,22500]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  #481","",7,3700,25900]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  #495","",2,3700,7400]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  #770010","",8,7000,56000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  #770012","",8,7000,56000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  NO 780132","",6,7500,45000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  NO 790008","",10,7881.41,78814.100000000006]
[null,"","","WELD REPAIR W4","",5,500,2500]

{"sheet":"ITEMS - DIV 01","index":3,"n_rows":341,"n_cols":8,"rows_kept":341,"cut":false,"hidden":false,"merged":[[8,1,8,7]]}
[]
[null,"Information"]
[null,"Author","PHIGGINS",null,"Last Refreshed","3/9/2022 13:28:02"]
[null,"Current User","HLUCAS",null,"Key Date","3/9/2022"]
[null,"Last Changed by","PHIGGINS",null,"Changed At","8/23/2013 10:16:36"]
[null,"InfoProvider","ZSPCI_C01",null,"Status of Data","3/1/2022 23:17:51"]
[null,"Query Technical Name","Y_SPX_ITEMLISTSUPPDESCSDIV",null,"Relevance of Data (Date)","3/1/2022"]
[null,"Query Description","Item List with Supplemental Descriptions (Bid Averages)",null,"Relevance of Data (Time)","23:17:51"]
[null,"2021 BID AVERAGES - DIVISION 01"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",4,443366,1773464]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",3,128833.55,386500.65]
[null,"0001000000-E","CLEARING & GRUBBING","","",3,560000,1680000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",2,250.5,501]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",37470,7.10008006405124,266040]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(15+50.00 -L-)","",1,10000,10000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",11980,23.101836393989998,276760]
[null,"0043000000-N","GRADING","","",1,128000,128000]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",1,1,1]
[null,"0106000000-E","BORROW EXCAVATION","","",21480,24.8417597765363,533601]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",1380,11.986231884058,16541]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",9120,5.2697368421052602,48060]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",410,2.25,922.5]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",5000,14.7,73500]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",9480,24.778481012658201,234900]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",25200,2.50595238095238,63150]
[null,"0199000000-E","TEMPORARY SHORING","","",343,100,34300]
[null,"0222000000-E","GEOTEXTILE ROCK EMBANK","","",600,3.25,1950]
[null,"0223000000-E","ROCK PLATING","","",1280,110,140800]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",100,95,9500]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",2360,49.639830508474603,117150]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",4610,1.2086767895878501,5572]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",40,50,2000]
[null,"0335600000-E","36\" DRAINAGE PIPE","","",52,62.9,3270.8]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",2,450,900]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",260,33.6,8736]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",484,36.200000000000003,17520.8]
[null,"0345000000-E","24\" SIDE DRAIN PIPE","","",464,48.35,22434.400000000001]
[null,"0354000000-E","***\" RC PIPE CULV *****","(24\", V)","",312,96.3,30045.599999999999]
[null,"0378000000-E","24\" RC PIPE CULV III","","",80,54.5,4360]
[null,"0448000000-E","***\" RCP CULV CLASS IV","(12\")","",1332,68,90576]
[null,"","","(48\")","",96,237,22752]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",3508,61.9288483466363,217246.4]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",2336,61.965667808219202,144751.79999999999]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",1332,79.632432432432395,106070.39999999999]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",628,114.484076433121,71896]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",344,136.4,46921.599999999999]
[null,"0546000000-E","**\" CAA PIPE CLVT *****\"","(18\", 0.105\")","",12,175,2100]
[null,"","","(36\", 0.135\")","",12,308.5,3702]
[null,"","","(42\", 0.135\")","",128,470,60160]
[null,"","","(48\", 0.164\")","",216,475,102600]
[null,"","","(60\", 0.164\")","",172,650,111800]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","35\" X 24\" CORRUGATED ALUMINUM","PIPE ARCH, 0.105\" THICK       (12 GAUGE)",72,225,16200]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","ALUMINUM HEADWALL, 0.150\"","THICK (CONTRACTOR DESIGNED)",6,51500,309000]
[null,"0995000000-E","PIPE REMOVAL","","",5432,17.089874815905699,92832.2]
[null,"0996000000-N","PIPE CLEAN OUT","","",6,800,4800]
[null,"1011000000-N","FINE GRADING","","",2,689104.5,1378209]
[null,"1077000000-E","#57 STONE","","",240,65,15600]
[null,"1099500000-E","SHALLOW UNDERCUT","","",5500,25,137500]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",10945,52,569140]
[null,"1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",5000,40,200000]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",40,46,1840]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",3305,59.104387291981901,195340]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 3\")","",1130,14,15820]
[null,"1330000000-E","INCIDENTAL MILLING","","",2815,20.230905861456499,56950]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",23450,96.276673773987199,2257688]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",9000,93.632222222222197,842690]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",21830,75.987081997251494,1658798]
[null,"1575000000-E","ASP FOR PLANT MIX","","",2960,507.46097972973001,1502084.5]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",2650,150.641509433962,399200]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",493,18.2657200811359,9005]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2200,2.3636363636363602,5200]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",370,54.578378378378403,20194]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",2200,11,24200]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",5,360.2,1801]
[null,"2077000000-E","6\" OUTLET PIPE","","",30,20.2,606]
[null,"2209000000-E","ENDWALLS","","",30,1920,57600]
[null,"2253000000-E","PIPE COLLARS","","",4.0599999999999996,800,3248]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",39,2550.1282051282101,99455]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",27,647.22222222222194,17475]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",4,675,2700]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",4,637.5,2550]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",1,725,725]
[null,"","","(F)","",1,750,750]
[null,"","","(G)","",1,750,750]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",1,600,600]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",1,1000,1000]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",440,29,12760]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",31,30,930]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",410,137.02439024390199,56180]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",5,3000,15000]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",2715,68.209208103130806,185188]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",80,53.5,4280]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",100,64.5,6450]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",114,65,7410]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",3950,29.9873417721519,118450]
[null,"3045000000-E","SBGR SHOP CURVED","","",125,32,4000]
[null,"3140000000-E","25' CLR SPAN GR SECTIONS","","",2,2500,5000]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",25,70,1750]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",15,24,360]
[null,"3180000000-N","GR ANCHOR TYPE **********","(III, SHOP CURVED)","",2,2800,5600]
[null,"3195000000-N","GR END TYPE AT-1","","",3,800,2400]
[null,"3215000000-N","GR ANCHOR TYPE III","","",4,1950,7800]
[null,"3287000000-N","GR END TYPE TL-3","","",23,3323.9130434782601,76450]
[null,"3288000000-N","GR END TYPE TL-2","","",8,3450,27600]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",2878,1,2878]
[null,"3628000000-E","RIP RAP, CLASS I","","",450,66.47,29911.5]
[null,"3635000000-E","RIP RAP, CLASS II","","",450,107,48150]
[null,"3642000000-E","RIP RAP, CLASS A","","",220,100,22000]
[null,"3649000000-E","RIP RAP, CLASS B","","",541,81.419593345656196,44048]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",3300,2.77651515151515,9162.5]
[null,"3984000000-E","GENERIC WALL ITEM (SF)","TIMBER RETAINING WALL ( 1)","",200,237.5,47500]
[null,"","","TIMBER RETAINING WALL ( 2)","",600,121,72600]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",20,12.5,250]
[null,"4082000000-E","SUPPORT, WOOD","","",1400,11.5,16100]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",2,150,300]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",90,75,6750]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(B)","",1,225,225]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(B)","",1,250,250]
[null,"","","(D)","",2,200,400]
[null,"","","(E)","",5,100,500]
[null,"4141000000-N","DISPOSE SUPPORT, WOOD","","",6,25,150]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",73,25,1825]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",653,11.4501531393568,7476.95]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",709,28.500705218617799,20207]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",166,9.8373493975903603,1633]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",514,5.8,2981.2]
[null,"4415000000-N","FLASHING ARROW BOARD","","",3,7666.6666666666697,23000]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",1,15000,15000]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",40,325,13000]
[null,"4430000000-N","DRUMS","","",210,54.142857142857103,11370]
[null,"4435000000-N","CONES","","",140,40.714285714285701,5700]
[null,"4445000000-E","BARRICADES (TYPE III)","","",412,33.203883495145597,13680]
[null,"4447000000-E","PED CHANNEL DEVICES","","",30,55,1650]
[null,"4455000000-N","FLAGGER","","",1422,758.22784810126598,1078200]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",1,2844,2844]
[null,"4480000000-N","TMA","","",2,17500,35000]
[null,"4507000000-E","WATER FILLED BARRIER","","",301,70,21070]
[null,"4510000000-N","LAW ENFORCEMENT","","",490,80.408163265306101,39400]
[null,"4516000000-N","SKINNY DRUM","","",80,40,3200]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",8,1400,11200]
[null,"","","TEMPORARY CURB RAMPS","",4,3500,14000]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",285,10,2850]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",194571,0.53294478622200003,103695.6]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",1680,2.5,4200]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",16,173.75,2780]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",92,196.95652173913001,18120]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",8000,2.5,20000]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",375555,0.1,37555.5]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",1410,1,1410]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",2286,3,6858]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",36,45,1620]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",93,45,4185]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",8160,0.89215686274509998,7280]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",590,5.75,3392.5]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",7,190,1330]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",3670,2.25,8257.5]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (24\", 90 MILS)",4270,12.1569086651054,51910]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",652,10.2223926380368,6665]
[null,"5325200000-E","2\" WATER LINE","","",93,51.505376344086002,4790]
[null,"5325400000-E","4\" WATER LINE","","",255,45.980392156862699,11725]
[null,"5325600000-E","6\" WATER LINE","","",690,95.869565217391298,66150]
[null,"5325800000-E","8\" WATER LINE","","",22779,26.5171868826551,604035]
[null,"5326000000-E","10\" WATER LINE","","",826,26,21476]
[null,"5326200000-E","12\" WATER LINE","","",15500,150,2325000]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",58095,14.451351235045999,839551.25]
[null,"5536000000-E","2\" VALVE","","",5,1545,7725]
[null,"5538000000-E","4\" VALVE","","",4,1637.5,6550]
[null,"5540000000-E","6\" VALVE","","",27,1929.62962962963,52100]
[null,"5546000000-E","8\" VALVE","","",21,1971.42857142857,41400]
[null,"5558000000-E","12\" VALVE","","",30,4950,148500]
[null,"5572200000-E","12\" TAPPING SLEEVE & VALVE","","",1,4000,4000]
[null,"5589100000-E","1\" AIR RELEASE VALVE","","",10,2100,21000]
[null,"5643000000-E","**\" WATER METER","(1\")","",1,2500,2500]
[null,"5643100000-E","3/4\" WATER METER","","",18,2450,44100]
[null,"5648000000-N","RELOCATE WATER METER","","",18,1411.1111111111099,25400]
[null,"5649000000-N","RECONNECT WATER METER","","",126,1355.1587301587299,170750]
[null,"5666000000-N","FIRE HYDRANT","","",10,7040,70400]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",15,7733.3333333333303,116000]
[null,"5673000000-E","FIRE HYDRANT LEG","","",100,45,4500]
[null,"5678600000-E","8\" LINE STOP","","",1,21000,21000]
[null,"5686500000-E","WATER SERVICE LINE","","",536,22,11792]
[null,"5709300000-E","6\" FORCE MAIN SEWER","","",100,116.5,11650]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(4\")","",200,8,1600]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",24300,2.5925925925925899,63000]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",2566,19.8908807482463,51040]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",1270,25,31750]
[null,"5815000000-N","REMOVE WATER METER","","",18,500,9000]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",2,1500,3000]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",330,475,156750]
[null,"5872600000-E","DIRECT DRILL **\"","(10\")","",826,56,46256]
[null,"5888000000-E","GENERIC UTILITY ITEM (LF)","POLYETHYLENE ENCASEMENT WATER LINE","",100,175,17500]
[null,"5894000000-E","GENERIC UTILITY ITEM (CY)","REINFORCED CONCRETE ENCASEMENT","AND SUPPORTS",50,400,20000]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",43625,2.7385386819484201,119468.75]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",990,52.5,51975]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",2155,50.703016241299302,109265]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",1190,40.231092436974798,47875]
[null,"6015000000-E","TEMPORARY MULCHING","","",29,765.94827586206895,22212.5]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",1900,3.5710526315789499,6785]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",9.5,1028.94736842105,9775]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",985,16.5228426395939,16275]
[null,"6029000000-E","SAFETY FENCE","","",10070,2.24230387288977,22580]
[null,"6030000000-E","SILT EXCAVATION","","",2710,5,13550]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",72120,1.4672767609539701,105820]
[null,"6037000000-E","COIR FIBER MAT","","",1880,3.9361702127659601,7400]
[null,"6038000000-E","PERM SOIL REINF MAT","","",100,4.75,475]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",1385,6.6967509025270804,9275]
[null,"6045000000-E","**\" TEMPORARY PIPE","(24\")","",85,88.6,7531]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",810,59.370370370370402,48090]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",7,820,5740]
[null,"6071012000-E","COIR FIBER WATTLE","","",9810,10.1148623853211,99226.8]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",250,9,2250]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",2380,9.1155462184873901,21695]
[null,"6071030000-E","COIR FIBER BAFFLE","","",190,7.5263157894736796,1430]
[null,"6084000000-E","SEEDING AND MULCHING","","",29,2151.03448275862,62380]
[null,"6087000000-E","MOWING","","",19,228.947368421053,4350]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",350,12.285714285714301,4300]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",1.25,1000,1250]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",700,5.21428571428571,3650]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",20.25,850.246913580247,17217.5]
[null,"6111000000-E","IMPERVIOUS DIKE","","",798,294.54724310776902,235048.7]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",30,60,1800]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",57,337.71929824561403,19250]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",12,861.66666666666697,10340]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",63,992.06349206349205,62500]
[null,"7060000000-E","SIGNAL CABLE","","",24830,3.6207813129279098,89904]
[null,"7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",2,710,1420]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",116,831.89655172413802,96500]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",27,1105.55555555556,29850]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",11,1510.9090909090901,16620]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",25058,3.4,85197.2]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",2630,5.5,14465]
[null,"7279000000-E","TRACER WIRE","","",44687,0.75,33515.25]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",1760,7,12320]
[null,"","","(2, 2\")","",39,14,546]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",425,19.4352941176471,8260]
[null,"","","(2, 2\")","",19235,17.225734338445498,331337]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",65,294,19110]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",114,565,64410]
[null,"7372000000-N","GUY ASSEMBLY","","",116,725,84100]
[null,"7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",12,700,8400]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",1,665.2,665.2]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",26,750,19500]
[null,"7432000000-E","2\" RISER WITH TUBING","","",38,900,34200]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",7550,8.2814569536423797,62525]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",53495,2.1071782409570998,112723.5]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",14785,2.5,36962.5]
[null,"","","(48)","",91379,3,274137]
[null,"7528000000-E","DROP CABLE","","",9537,2.4,22888.799999999999]
[null,"7540000000-N","SPLICE ENCLOSURE","","",38,1500,57000]
[null,"7552000000-N","INTERCONNECT CENTER","","",44,1525,67100]
[null,"7566000000-N","DELINEATOR MARKER","","",67,95,6365]
[null,"7575142200-N","NEW ELECTRICAL SERVICE","","",10,1800,18000]
[null,"7575160000-E","REM EXT COMM CABLE","","",13318,1,13318]
[null,"7575180000-N","CABLE TRANSFER","","",10,360,3600]
[null,"7576000000-N","METAL STRAIN SIGNAL POLE","","",2,17150,34300]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",3,22141,66423]
[null,"7613000000-N","SOIL TEST","","",5,2490,12450]
[null,"7614100000-E","DRILLED PIER FOUND","","",68.3,1354.0995607613499,92485]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",3,750,2250]
[null,"7636000000-N","SIGN FOR SIGNALS","","",5,574,2870]
[null,"7642100000-N","TYPE I POST W/ FOUNDATION","","",4,1700,6800]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",27,2007.4074074074099,54200]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",9,2316.6666666666702,20850]
[null,"7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",19,600,11400]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(2070E, BASE MOUNTED)","",1,19000,19000]
[null,"7708000000-N","DETECTOR CARD (***********)","(MODEL 222)","",282,90,25380]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",17,165,2805]
[null,"7901000000-N","CABINET BASE EXTENDER","","",45,504.222222222222,22690]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",2,2550,5100]
[null,"7972000000-N","METAL POLE REMOVAL","","",2,575,1150]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","CCTV CAMERA  ASSEMBLY","",20,4900,98000]
[null,"","","CONTROLLER WITH CABINET WITH","AUX FILE (2070LX, 332)",44,12500,550000]
[null,"","","DIGITAL DISPLAY MONITOR","",1,3800,3800]
[null,"","","ETHERNET CORE SWITCH","",1,55451.95,55451.95]
[null,"","","ETHERNET EDGE SWITCH","",44,1700,74800]
[null,"","","FIREWALL","",1,5000,5000]
[null,"","","FURNISH 2018 ENHANCED CONFLICTMONITOR","",3,1200,3600]
[null,"","","FURNISH 2070 CONTROLLER TESTER","",1,8000,8000]
[null,"","","FURNISH 2070LX CONTROLLER","",3,1800,5400]
[null,"","","FURNISH 332 CABINET WITH AUX  FILE","",3,9000,27000]
[null,"","","FURNISH CCTV CAMERA  ASSEMBLY","",2,3500,7000]
[null,"","","FURNISH CONFLICT MONITOR TEST-ER","",1,27000,27000]
[null,"","","FURNISH ETHERNET EDGE SWITCH","",3,1700,5100]
[null,"","","GUY ASSEMBLY - AERIAL","",1,1000,1000]
[null,"","","GUY ASSEMBLY - SIDEWALK","",8,950,7600]
[null,"","","HEAT SHRINK TUBING KIT","",12,150,1800]
[null,"","","ITS SERVER","",3,10000,30000]
[null,"","","JUNCTION BOX (SPECIAL-SIZED)","",15,950,14250]
[null,"","","JUNCTION BOX MARKER","",46,60,2760]
[null,"","","KVM SWITCH","",1,3400,3400]
[null,"","","MODIFY COMMUNICATIONS RACK","",1,6000,6000]
[null,"","","MODIFY EXISTING ELECTRICAL    SERVICE","",8,500,4000]
[null,"","","MODIFY FOUNDATION FOR CONTROL-","LER CABINET",6,1250,7500]
[null,"","","POLE GROUNDING SYSTEM","",71,280,19880]
[null,"","","POWDER COAT FOR STRAIN POLE","(BLACK)",2,1001,2002]
[null,"","","PTZ JOYSTICK","",1,1200,1200]
[null,"","","RELOCATE EXISTING CABINET","EQUIPMENT",30,100,3000]
[null,"","","SIGNAL SYSTEM SUPERVISOR'S","COMPUTER SYSTEM",1,6500,6500]
[null,"","","SPAN TRANSFER","",69,60,4140]
[null,"","","TYPE 332 TEST CONTROLLER WITH CABINET","",1,15000,15000]
[null,"","","UPS IN COMMUNICATIONS RACK","",1,8300,8300]
[null,"","","WOOD POLE FOR SIGNALS","",9,1500,13500]
[null,"","","WOOD POLE FOR SIGNALS WITH    CCTV","",13,3700,48100]
[null,"7985000000-N","GENERIC SIGNAL ITEM (LS)","CCTV SOFTWARE","",1,14000,14000]
[null,"","","NETWORK MANAGEMENT SOFTWARE","",1,16650,16650]
[null,"","","SIGNAL SYSTEM SOFTWARE","",1,285000,285000]
[null,"","","SYSTEM SUPPORT SOFTWARE &     DEVICES","",1,28000,28000]
[null,"","","TMC BUILDING MODIFICATIONS","",1,32260.6,32260.6]
[null,"","","TRAINING","",1,71507,71507]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","AERIAL CABLE PROTECTOR","",75,20,1500]
[null,"","","ETHERNET CABLE","",3787,4.5,17041.5]
[null,"","","UNDERGROUND CONDUIT (1, 1\")","",185,10.5,1942.5]
[null,"","","UNDERGROUND CONDUIT (1, 2\")","",1955,10.5,20527.5]
[null,"","","UNDERGROUND CONDUIT (2, 2\")","",24158,9.5,229501]
[null,"","","UNDERGROUND CONDUIT (3, 2\")","",40,40,1600]
[null,"7991000000-E","GENERIC SIGNAL ITEM (SF)","BRICK PAVERS","",8,340,2720]
[null,"8035000000-N","REMV EXIST STR **********","(15+50.00 -L-)","",1,35000,35000]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",1,1560,1560]
[null,"8112730000-N","PDA TESTING","","",1,2610,2610]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(15+50.00 -L-)","",1,15000,15000]
[null,"8126000000-N","CULV EXCAV @ ************","(132+88.62 -L-)","",1,37890,37890]
[null,"","","(79+82.10 -L-)","",1,29600,29600]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",321,66.3,21282.3]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",53.9,1500,80850]
[null,"8210000000-N","BRG APPR SLAB ***********","(15+50.00 -L-)","",1,25000,25000]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",7408,2,14816]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",14,3500,49000]
[null,"8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",8,5000,40000]
[null,"8364000000-E","HP12X53 PILES","","",1015,40,40600]
[null,"8384200000-E","HP14X73 GALV PILES","","",720,70,50400]
[null,"8393000000-N","PILE REDRIVES","","",12,1,12]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",210.5,150,31575]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",240,65,15600]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",267,5,1335]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",1,6000,6000]
[null,"8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",1155,228,263340]
[null,"8804000000-N","GENERIC CULVERT ITEM (LS)","ALUMINUM BOX CULVERT @","STA 132+88.62 -L-",1,253470,253470]
[null,"","","","STA 79+82.10 -L-",1,248220,248220]
[null,"8811000000-E","GENERIC CULVERT ITEM (LF)","MOMENT SLAB","",166,362,60092]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FIBER OPTIC CONDUIT SYSTEM","",206,30,6180]

{"sheet":"ITEMS - DIV 02","index":4,"n_rows":364,"n_cols":8,"rows_kept":364,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 02"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",7,689748.21428571397,4828237.5]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",7,111865,783055]
[null,"0000910000-N","GENERIC MISCELLANEOUS ITEM (HR)","EXPLORATORY EXCAVATION -      STANDARD","",1,500,500]
[null,"","","EXPLORATORY EXCAVATION -      VACUUM","",1,600,600]
[null,"0000950000-E","GENERIC MISCELLANEOUS ITEM (SF)","PERMANENT SHORING","",4200,200,840000]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(24+78.90)","",1,56000,56000]
[null,"","","(28+85.96-L-)","",1,100000,100000]
[null,"","","(30+80.00 -L-)","",1,16600,16600]
[null,"","","(41+45 -L1-)","",1,26000,26000]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(13+34.00 -L-)","",1,16036.8,16036.8]
[null,"","","(13+78.50 -L-)","",1,11620,11620]
[null,"","","(23+06.50 -L-)","",1,6500,6500]
[null,"","","(25+06 -L1-)","",1,16500,16500]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",2700,14.05,37935]
[null,"0043000000-N","GRADING","","",4,299875,1199500]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",6.1,13580.0163934426,82838.100000000006]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",4250,11.5,48875]
[null,"0063000000-N","GRADING","","",3,699935.86333333305,2099807.59]
[null,"0106000000-E","BORROW EXCAVATION","","",90340,9.3389417755147193,843680]
[null,"0127000000-N","EMBM'T SETTLEMENT GAUGE","","",11,815,8965]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",470,33.808510638297903,15890]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",1450,96,139200]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",7500,9.9600000000000009,74700]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",10625,3.2451764705882402,34480]
[null,"0199000000-E","TEMPORARY SHORING","","",2440,80.883688524590198,197356.2]
[null,"0220000000-E","ROCK EMBANKMENTS","","",3850,56.35,216947.5]
[null,"0222000000-E","GEOTEXTILE ROCK EMBANK","","",2300,6,13800]
[null,"0223000000-E","ROCK PLATING","","",723,98.374827109266903,71125]
[null,"0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",650,12.95,8417.5]
[null,"","","NONWOVEN GEOTEXTILE","",2850,3.01,8578.5]
[null,"","","ROCK PLATING","",2200,78.900000000000006,173580]
[null,"","","ROCK PLATING, DETAIL NO A","",2000,40.1,80200]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,110,5500]
[null,"","","RIP RAP, CLASS 2","",150,65.5,9825]
[null,"0262000000-N","GENERIC GRADING ITEM (EA)","HAULING NCDOT SUPPLIED        MATERIAL","",320,104,33280]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",361,46.980609418282498,16960]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",1584,4.2791035353535403,6778.1]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",282,59.3829787234043,16746]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",156,45,7020]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",16,488.125,7810]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",152,54.1394736842105,8229.2000000000007]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",64,52,3328]
[null,"0366000000-E","15\" RC PIPE CULV III","","",428,47.15,20180.2]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",144,72.75,10476]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",768,79.764479166666703,61259.12]
[null,"0546000000-E","**\" CAA PIPE CLVT *****\"","(15\", 0.064\")","",140,74.599999999999994,10444]
[null,"0564000000-E","**\" CAA PIPE ELBOW *****\"","(15\", 0.064\")","",8,610,4880]
[null,"0576000000-E","**\" CS PIPE CULV *****\"","(84\", 0.168\")","",28,815,22820]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",460,50,23000]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",22,430,9460]
[null,"0995000000-E","PIPE REMOVAL","","",943,10.6086956521739,10004]
[null,"1077000000-E","#57 STONE","","",2235,58.583892617449699,130935]
[null,"1099500000-E","SHALLOW UNDERCUT","","",325,13.384615384615399,4350]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",640,37.0625,23720]
[null,"1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",200,49,9800]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",2151,54.540678754067898,117317]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",1073,46.345293569431497,49728.5]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",8.52,5970,50864.4]
[null,"1275000000-E","PRIME COAT","","",818,20,16360]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",480,13.64,6547.2]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 2-1/2\")","",2000,4.8,9600]
[null,"","","(0\" TO 3\")","",840,12.16,10214.4]
[null,"1330000000-E","INCIDENTAL MILLING","","",9551,6.9939273374515798,66799]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",12315,59.095294356475797,727758.55]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",12010,51.951032472939197,623931.9]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",4205,78.954411414982204,332003.3]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",8140,56.834914004913998,462636.2]
[null,"1575000000-E","ASP FOR PLANT MIX","","",1908.6,461.08152572566303,880020.2]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",100,95,9500]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",150,205,30750]
[null,"1890000000-N","GENERIC PAVING ITEM (EA)","PRECAST CONCRETE PARKING CURB","",19,300,5700]
[null,"2000000000-N","RIGHT-OF-WAY MARKERS","","",35,346.01171428571399,12110.41]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",493.2,16.636820762368199,8205.2800000000007]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2200,3.6554545454545502,8042]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",370.4,41.406263498920097,15336.88]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",2200,7.4772727272727302,16450]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",8,260.70249999999999,2085.62]
[null,"2077000000-E","6\" OUTLET PIPE","","",48,24.614999999999998,1181.52]
[null,"2209000000-E","ENDWALLS","","",1,3950,3950]
[null,"2220000000-E","REINFORCED ENDWALLS","","",19.100000000000001,1629.02984293194,31114.47]
[null,"2253000000-E","PIPE COLLARS","","",4.3,3159.9,13587.57]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",46,1986.19565217391,91365]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",3.4,330,1122]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",42,650.95238095238096,27340]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",4,557.5,2230]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","DEWATERING","",2,12882.8,25765.599999999999]
[null,"2484000000-E","GENERIC DRAINAGE ITEM (LF)","84\" PIPE REHABILITATION","",123,968.67,119146.41]
[null,"","","PRE-INSTALLATION INSPECTION","",123,50,6150]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",5568,34.8150502873563,193850.2]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",50,72,3600]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",650,81.95,53267.5]
[null,"2738100000-E","GENERIC PAVING ITEM (SF)","PERMEABLE PAVERS","",13104,5,65520]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",1,1500,1500]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",10212.5,18.513121175030602,189065.25]
[null,"3045000000-E","SBGR SHOP CURVED","","",250,21.795000000000002,5448.75]
[null,"3135000000-N","W-TR SBGR TRANS SECTIONS","","",4,250,1000]
[null,"3140000000-E","25' CLR SPAN GR SECTIONS","","",1,1800,1800]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",22,66.569999999999993,1464.54]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",40,26.672499999999999,1066.9000000000001]
[null,"3195000000-N","GR END TYPE AT-1","","",5,712.42,3562.1]
[null,"3210000000-N","GR END TYPE CAT-1","","",2,3000,6000]
[null,"3215000000-N","GR ANCHOR TYPE III","","",28,1761.76285714286,49329.36]
[null,"3287000000-N","GR END TYPE TL-3","","",33,2827.28484848485,93300.4]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",12,1695.8333333333301,20350]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",5342,1.07383938599775,5736.45]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",662.5,7.5652830188679197,5012]
[null,"3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",50,12.1,605]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-3)","",5,2312.9540000000002,11564.77]
[null,"3420000000-E","GENERIC GUARDRAIL ITEM (LF)","REMOVE, STOCKPILE, AND DELIVER","EXISTING GUARDRAIL",530,5,2650]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNITS,TYPE AT-1","",1,403.45,403.45]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",30,30,900]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1,100,100]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",2,150,300]
[null,"3578000000-N","GENERIC FENCING ITEM (EA)","RESET EXISTING GATE","",2,800,1600]
[null,"","","STEEL BOLLARDS","",9,1650,14850]
[null,"3628000000-E","RIP RAP, CLASS I","","",233,72.141630901287598,16809]
[null,"3635000000-E","RIP RAP, CLASS II","","",419,81.565632458233907,34176]
[null,"3649000000-E","RIP RAP, CLASS B","","",120,96.658333333333303,11599]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",7893,2.53683643734955,20023.25]
[null,"3659000000-N","PREFORMED SCOUR HOLES","","",2,2161,4322]
[null,"3684000000-E","GENERIC EROSION CONTROL ITEM (TON)","RIP RAP, CLASS A","",375,57.6,21600]
[null,"","","RIP RAP, CLASS B","",375,65.25,24468.75]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(D)","",12,25,300]
[null,"","","(E)","",144,17.9444444444444,2584]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",170,7.8823529411764701,1340]
[null,"4082000000-E","SUPPORT, WOOD","","",140,10.6071428571429,1485]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",4,156.5,626]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",21,122.142857142857,2565]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",1,125,125]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",1,125,125]
[null,"4141000000-N","DISPOSE SUPPORT, WOOD","","",1,8,8]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",2,500,1000]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",6,4.1666666666666696,25]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",41,5.3170731707317103,218]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",2975,6.2015798319327704,18449.7]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",654,14.5981651376147,9547.2000000000007]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",442,5.6131221719457001,2481]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",480,6.15,2952]
[null,"4415000000-N","FLASHING ARROW BOARD","","",2,2800,5600]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",7,7400,51800]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",72,40.125,2889]
[null,"4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",3,16000,48000]
[null,"4430000000-N","DRUMS","","",526,87.461977186311799,46005]
[null,"4435000000-N","CONES","","",20,28.83,576.6]
[null,"4445000000-E","BARRICADES (TYPE III)","","",448,65.839285714285694,29496]
[null,"4447000000-E","PED CHANNEL DEVICES","","",8,140,1120]
[null,"4455000000-N","FLAGGER","","",354,467.96610169491498,165660]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",3,44533.333333333299,133600]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",6,6703.84666666667,40223.08]
[null,"4480000000-N","TMA","","",3,7333.3333333333303,22000]
[null,"4485000000-E","PORT CONC BARRIER","","",608,78.706447368421095,47853.52]
[null,"4510000000-N","LAW ENFORCEMENT","","",48,104.166666666667,5000]
[null,"4516000000-N","SKINNY DRUM","","",10,33.17,331.7]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","WARNING FLAGS","",8,17.600000000000001,140.80000000000001]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",127,10,1270]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",30672,1.6556892279603499,50783.3]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",190,4,760]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",9,175,1575]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(IV)","",8400,2.25,18900]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",80790,0.52014729545736005,42022.7]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",298,3,894]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",19908,0.73146473779385002,14562]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",72,3.3,237.6]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES","(4\", 20 MILS) (STANDARD GLASS BEADS)",1330,4.5,5985]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",19876,3.4570336083719102,68712]
[null,"","","THERMOPLASTIC PAVEMENT MARKING","LINES (4\", 90 MILS) (HRM)",10740,1.95,20943]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (24\", 90 MILS)",70,16.785714285714299,1175]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",121,10.3719008264463,1255]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",127,89.055118110236194,11310]
[null,"5260000000-N","GENERIC LIGHTING ITEM (LS)","TEMPORARY PORTABLE LIGHTING","",1,18000,18000]
[null,"5325000000-E","**\" WATER LINE","(14\")","",1620,87,140940]
[null,"5325400000-E","4\" WATER LINE","","",192,75,14400]
[null,"5325600000-E","6\" WATER LINE","","",300,40,12000]
[null,"5325800000-E","8\" WATER LINE","","",180,155,27900]
[null,"5326000000-E","10\" WATER LINE","","",1164,90,104760]
[null,"5326200000-E","12\" WATER LINE","","",2827,116.040325433322,328046]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",6391,10.785792520732301,68932]
[null,"5546000000-E","8\" VALVE","","",8,1650,13200]
[null,"5552000000-E","10\" VALVE","","",7,3150,22050]
[null,"5558000000-E","12\" VALVE","","",2,2800,5600]
[null,"5571400000-E","4\" TAPPING SLEEVE & VALVE","","",2,4000,8000]
[null,"5589200000-E","2\" AIR RELEASE VALVE","","",8,5900,47200]
[null,"5648000000-N","RELOCATE WATER METER","","",1,750,750]
[null,"5649000000-N","RECONNECT WATER METER","","",1,500,500]
[null,"5686500000-E","WATER SERVICE LINE","","",118,7,826]
[null,"5709400000-E","8\" FORCE MAIN SEWER","","",1000,112,112000]
[null,"5709500000-E","10\" FORCE MAIN SEWER","","",3250,46,149500]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",2800,10.75,30100]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(4\")","",469,15,7035]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",4275,12.776608187134499,54620]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",3560,10,35600]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",2040,11.6,23664]
[null,"5835000000-E","**\" ENCASEMENT PIPE","(22\")","",165,195,32175]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",330,185,61050]
[null,"5835900000-E","20\" ENCASEMENT PIPE","","",62,200,12400]
[null,"5872500000-E","BORE & JACK **\"","(18\")","",330,295,97350]
[null,"","","(22\")","",165,300,49500]
[null,"5872600000-E","DIRECT DRILL **\"","(10\")","",3250,66,214500]
[null,"","","(12\")","",2311,142,328162]
[null,"","","(14\")","",1620,97,157140]
[null,"","","(6\")","",300,80,24000]
[null,"5912000000-N","GENERIC UTILITY ITEM (LS)","DEWATERING","",1,225000,225000]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",35515,3.6562016049556498,129850]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",650,64.553076923076901,41959.5]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",2240,64.274553571428598,143975]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",2980,51.533724832214801,153570.5]
[null,"6015000000-E","TEMPORARY MULCHING","","",25.5,922.94117647058795,23535]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",1600,3.8125,6100]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",8,948,7584]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",3375,14.807481481481499,49975.25]
[null,"6029000000-E","SAFETY FENCE","","",22530,2.5289613848202399,56977.5]
[null,"6030000000-E","SILT EXCAVATION","","",2100,8.0815714285714293,16971.3]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",17415,1.86060867068619,32402.5]
[null,"6037000000-E","COIR FIBER MAT","","",1400,4.57,6398]
[null,"6038000000-E","PERM SOIL REINF MAT","","",85,5.5,467.5]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",2105,5.7967933491686496,12202.25]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",10065,29.050099354197702,292389.25]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",51,904.46078431372598,46127.5]
[null,"6071012000-E","COIR FIBER WATTLE","","",3205,11.0787831513261,35507.5]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",4159,15.0624549170474,62644.75]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",645,11.9476744186047,7706.25]
[null,"6071030000-E","COIR FIBER BAFFLE","","",645,5.8062015503876001,3745]
[null,"6084000000-E","SEEDING AND MULCHING","","",35.090000000000003,2445.47734397264,85811.8]
[null,"6087000000-E","MOWING","","",20.65,311.23486682808698,6427]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",450,8.43333333333333,3795]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",1.75,955,1671.25]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",750,5.1166666666666698,3837.5]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",19.5,937.17948717948696,18275]
[null,"6111000000-E","IMPERVIOUS DIKE","","",397,398.06234256927002,158030.75]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",70,70.8857142857143,4962]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",429,150.34090909090901,64496.25]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",15,1359.4666666666701,20392]
[null,"6123000000-E","REFORESTATION","","",2.5,5420,13550]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",0.04,100,4]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",60,247.76666666666699,14866]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",30,251.833333333333,7555]
[null,"6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","WETLAND GRASS PLANTING","",0.38,4000,1520]
[null,"7060000000-E","SIGNAL CABLE","","",1920,3,5760]
[null,"7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",4,575,2300]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",14,850,11900]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",2,975,1950]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",450,2,900]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",1375,7,9625]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",11,235,2585]
[null,"7360000000-N","WOOD POLE","","",4,900,3600]
[null,"7372000000-N","GUY ASSEMBLY","","",8,450,3600]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",1,423.5,423.5]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",3,500,1500]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",1120,7,7840]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",4800,2,9600]
[null,"7636000000-N","SIGN FOR SIGNALS","","",2,600,1200]
[null,"7642300000-N","TYPE III PED W/ FOUNDATION","","",1,4200,4200]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",1,880,880]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(2070E, BASE MOUNTED)","",1,15500,15500]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",5,132,660]
[null,"7901000000-N","CABINET BASE EXTENDER","","",1,375,375]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(25+06.00 -L1-)","",1,1334494.45,1334494.45]
[null,"","","(30+80.00-L-)","",1,885000,885000]
[null,"","","(34+75.00 -L-)","",1,14392000,14392000]
[null,"","","(41+45.00 -L1-)","",1,519160.26,519160.26]
[null,"8021000000-N","REMV EXIST STR **********","(25+06.00 -L1-)","",1,234449.33,234449.33]
[null,"8035000000-N","REMV EXIST STR **********","(13+34.00 -L-)","",1,55000,55000]
[null,"","","(13+78.50 -L-)","",1,54000,54000]
[null,"","","(23+06.50-L-)","",1,195000,195000]
[null,"","","(24+78.90 -L-)","",1,72500,72500]
[null,"","","(28+85.96 -L-)","",1,156500,156500]
[null,"","","(30+80.00-L-)","",1,293000,293000]
[null,"","","(34+75.00 -L-)","",1,2000000,2000000]
[null,"","","(41+45.00 -L1-)","",1,87032.19,87032.19]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",7,3275,22925]
[null,"8108000000-E","**'-**\" DIA DRILLD PIERS","(4'-6\")","",729,760,554040]
[null,"8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",167,375,62625]
[null,"8112730000-N","PDA TESTING","","",33,3054.3406060606098,100793.24]
[null,"8113000000-N","SID INSPECTIONS","","",2,1070,2140]
[null,"8114000000-N","SPT TESTING","","",3,1070,3210]
[null,"8115000000-N","CSL TESTING","","",4,2675,10700]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(13+34.00 -L-)","",1,9000,9000]
[null,"","","(13+78.50 -L-)","",1,10000,10000]
[null,"","","(23+06.50-L-)","",1,8000,8000]
[null,"","","(24+78.90 -L-)","",1,15000,15000]
[null,"","","(25+06.00 -L1-)","",1,1611.47,1611.47]
[null,"","","(28+85.96 -L-)","",1,110000,110000]
[null,"","","(30+80.00-L-)","",1,8000,8000]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",73860,45.075334687246098,3329264.22]
[null,"8154000000-E","REINF CONC DECK SLAB,LTWT","","",110595,100,11059500]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",163496,0.78071108773303,127643.14]
[null,"8175000000-E","CLASS AA CONC (BRIDGE)","","",1910.2,1487.1217673542001,2840700]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",1200,1275.2848166666699,1530341.78]
[null,"8210000000-N","BRG APPR SLAB ***********","(13+34.00 -L-)","",1,37000,37000]
[null,"","","(13+78.50 -L-)","",1,37000,37000]
[null,"","","(23+06.50-L-)","",1,26000,26000]
[null,"","","(24+78.90 -L-)","",1,70000,70000]
[null,"","","(25+06.00 -L1-)","",1,41341.58,41341.58]
[null,"","","(28+85.96 -L-)","",1,135000,135000]
[null,"","","(30+80.00-L-)","",1,28000,28000]
[null,"","","(34+75.00 -L-)","",1,100000,100000]
[null,"","","(41+45.00 -L1-)","",1,29840.7,29840.7]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",246453,1.1535713097426299,284301.11]
[null,"8224000000-E","EPOXY COAT REINF STL BRDG","","",13094,1.5,19641]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",23994,1.73,41509.620000000003]
[null,"8259000000-E","36\" PRESTR CONCRETE GIRDR","","",770,230,177100]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",5860.66,333.68537502602101,1955616.53]
[null,"8328000000-E","PILE DRV EQUIP SETUP * PRESTR CONC PILES","(16\")","",14,2800,39200]
[null,"","","(24\" CARBON FIBER REINFORCED","POLYMER)",212,10000,2120000]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",130,1403.45769230769,182449.5]
[null,"8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",8,2134.1999999999998,17073.599999999999]
[null,"","","(PP 18 X 0.50)","",24,3100,74400]
[null,"","","(PP 24 X 0.50)","",15,4697.3900000000003,70460.850000000006]
[null,"","","(PP 30 X 0.500)","",22,3650,80300]
[null,"","","(PP 36 X 0.50)","",20,6334.36,126687.2]
[null,"8333000000-E","16\" PRESTR CONC PILES","","",595,76,45220]
[null,"8364000000-E","HP12X53 PILES","","",9068,61.285763123070097,555739.30000000005]
[null,"8384200000-E","HP14X73 GALV PILES","","",640,96.37,61676.800000000003]
[null,"8385200000-E","PP**X**** GALV STL PILE","(PP 24 X 0.50)","",1450,126.89,183990.5]
[null,"","","(PP 30 X 0.500)","",2530,325,822250]
[null,"","","(PP 36 X 0.50)","",2060,203.58,419374.8]
[null,"8387000000-E","PP18X0.50 GALV STL PILE","","",2040,152,310080]
[null,"8391000000-N","STEEL PILE POINTS","","",34,847.29411764705901,28808]
[null,"8392000000-N","PIPE PILE PLATES","","",37,78.675675675675706,2911]
[null,"8393000000-N","PILE REDRIVES","","",264,721.17045454545496,190389]
[null,"8475000000-E","TWO BAR METAL RAIL","","",6380.5,120,765660]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",1230.1300000000001,96.605757115101696,118837.64]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",3287.72,116.322332802063,382435.26]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",6396.69,97.8899993590435,626171.98]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",1340,120,160800]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",2926,62.391524265208503,182557.6]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",3242,3.3516347933374502,10866]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",7,45386.064285714303,317702.45]
[null,"8660000000-E","CONCRETE REPAIRS","","",111,725,80475]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",18,725,13050]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",122,92,11224]
[null,"8692000000-N","FOAM JOINT SEALS","","",3,24517.57,73552.710000000006]
[null,"8706000000-N","EXPANSION JOINT SEALS","","",1,230000,230000]
[null,"8741000000-N","STR DRN SYS ************","(34+75.00 -L-)","",1,587880,587880]
[null,"8744000000-N","SOLAR ARRAY SUPPT PLTFORM","","",1,26000,26000]
[null,"8753100000-E","3'-0\"X 2'-9\" PRESTR BOX BEAM","","",990,236.46,234095.4]
[null,"8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",935,188,175780]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",2730,197,537810]
[null,"8839000000-E","GENERIC RET WALL ITEM (LF)","CONCRETE SHEET PILE RETAINING WALL","",660.5,4760,3143980]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","REINFORCED RETAINING WALL     BACKFILL","",7315,44.77,327492.55]
[null,"","","REINFORCED RETAINING WALL BACKFILL","",8056,90,725040]
[null,"","","SHEET PILE RETAINING WALL","",28945,33.94,982393.3]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","PLASTIC LUMBER FENDER BOARDS","AT CHANNEL BENTS",1,55000,55000]
[null,"","","TRAFFIC SIGNAL EXTENSION","",1,5500,5500]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","24\" CARBON FIBER REINFORCED     POLYMER","PRESTRESSED CONCRETE PILES",20970,89.5,1876815]
[null,"","","36\" FLORIDA I-BEAM","(FIB) GIRDERS",1833.33,315,577498.94999999995]
[null,"","","4 BAR METAL RAIL","",1158,285,330030]
[null,"","","54\" CARBON FIBER REINFORCED     POLYMER","F.I.B. PRESTRESSED CONCRETE      GIRDERS",5579.64,460,2566634.4]
[null,"","","72\" CARBON FIBER REINFORCED      POLYMER","F.I.B. PRESTRESSED CONCRETE      GIRDERS",5707.35,410,2340013.5]
[null,"","","78\" CARBON FIBER REINFORCED      POLYMER","F.I.B. PRESTRESSED CONCRETE      GIRDERS",1815.18,515,934817.7]
[null,"","","ASPHALT JOINT REPAIR/REPLACE-","MENT (20\" WIDE, W/PLATE)",1716,150,257400]
[null,"","","CARBON FIBER REINFORCED","POLYMER (CFRP) STRAND",986059,6,5916354]
[null,"","","FIBER OPTIC CONDUIT SYSTEM","",342.28,45.556328152389902,15593.02]
[null,"","","GLASS FIBER REINFORCED POLYMER","(GFRP) BAR",199245.43,2.2500000125473401,448302.22]
[null,"","","PILE EXC FOR 24\" CARBON FIBER REINFORCED","POLYMER PRESTRESSED CONCRETE  PILES",7211,120,865320]
[null,"","","RAIL RETROFIT (2-BAR METAL    RAIL)","",2079,150,311850]
[null,"","","RAIL RETROFIT (3-BAR METAL    RAIL)","",360,265,95400]
[null,"","","SILICONE JOINT SEALANT","",365,70,25550]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","CONCRETE FILLED GRID DECK","REPAIR FOR EPOXY OVERLAY",88,232,20416]
[null,"","","EPOXY COATING AND DEBRIS      REMOVAL","",2862,16,45792]
[null,"","","EPOXY OVERLAY SYSTEM I","",2184,52,113568]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","TOP PIPE PILE PLATES","",35,107,3745]

{"sheet":"ITEMS - DIV 03","index":5,"n_rows":640,"n_cols":8,"rows_kept":640,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 03"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",11,1159683.7954545501,12756521.75]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",6,876208.33333333302,5257250]
[null,"0000700000-N","FIELD OFFICE","","",1,1500000,1500000]
[null,"0001000000-E","CLEARING & GRUBBING","","",26,576923.07692307699,15000000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",3,15000,45000]
[null,"0015000000-N","SEALING ABANDONED WELLS","","",8,1200,9600]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",90000,10,900000]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(18+27.00 -L-)","",1,33000,33000]
[null,"","","(21+68.50 -L-)","",1,48000,48000]
[null,"","","(369+42.00 -L- EBL)","",1,50000,50000]
[null,"","","(369+42.00 -L- WBL)","",1,50000,50000]
[null,"","","(390+15.00 -L- LT)","",1,75000,75000]
[null,"","","(390+15.00 -L- RT)","",1,75000,75000]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(31+30.81 -Y REV-)","",1,90000,90000]
[null,"","","(39+52.37 -Y14A-)","",1,75000,75000]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(16+08.00 -L-)","",1,9000,9000]
[null,"","","(18+30 -L-)","",1,15500,15500]
[null,"","","(23+55.00 -L-)","",1,13000,13000]
[null,"","","(23+71.50 -L-)","",1,9000,9000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",58100,11.372685025817599,660753]
[null,"0043000000-N","GRADING","","",7,332785.38571428601,2329497.7000000002]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",7,3312.5728571428599,23188.01]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",300,2.5,750]
[null,"0106000000-E","BORROW EXCAVATION","","",1201026,8.0130788675682307,9623916.0600000005]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",63115,9.5020121999524694,599719.5]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",19500,15.1,294450]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",63810,5.8,370098]
[null,"0192000000-N","PROOF ROLLING","","",100,365,36500]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",500,0.01,5]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",57400,9.7829268292682894,561540]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",49440,2.0840210355987101,103034]
[null,"0199000000-E","TEMPORARY SHORING","","",33566,78.960257403324803,2650380]
[null,"0223000000-E","ROCK PLATING","","",4825,81.022279792746104,390932.5]
[null,"0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR EMBANKMENT","STABILIZATION",1900,7,13300]
[null,"0248000000-N","GENERIC GRADING ITEM (LS)","DE-WATERING","",1,62950,62950]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",150,182.666666666667,27400]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",8500,48.631823529411797,413370.5]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",67059,4.8409684009603504,324630.5]
[null,"0335000000-E","**\" DRAINAGE PIPE","(54\")","",288,432,124416]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",2236,84.364937388193198,188640]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",1508,82.145623342175099,123875.6]
[null,"0335400000-E","24\" DRAINAGE PIPE","","",1004,97.752988047808799,98144]
[null,"0335500000-E","30\" DRAINAGE PIPE","","",588,114.734693877551,67464]
[null,"0335600000-E","36\" DRAINAGE PIPE","","",604,141,85164]
[null,"0335800000-E","48\" DRAINAGE PIPE","","",636,264,167904]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",20,360.42,7208.4]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",40,80,3200]
[null,"0448000000-E","***\" RCP CULV CLASS IV","(12\")","",76,74,5624]
[null,"","","(48\")","",1154,307.92201039861402,355342]
[null,"","","(54\")","",488,634,309392]
[null,"","","(60\")","",1240,469,581560]
[null,"","","(66\")","",408,600,244800]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",15860,67.980832282471596,1078176]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",4858,88.421572663647595,429552]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",3676,97.068552774755204,356824]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",5130,151.53294346978601,777364]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",3460,221.32369942196499,765780]
[null,"0448700000-E","42\" RCP CULV CLASS IV","","",1144,330,377520]
[null,"0546000000-E","**\" CAA PIPE CLVT *****\"","(54\", 0.109\")","",84,588,49392]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",632,53,33496]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",52,52,2704]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",30,428,12840]
[null,"","","(18\", 0.064\")","",2,871,1742]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","18\" DUCTILE IRON PIPE","",112,217,24304]
[null,"","","24\" DUCTILE IRON PIPE","",202,227,45854]
[null,"","","28\" X 20\" CAA PIPE ARCH","CULVERT, 0.135\" THICK",92,250,23000]
[null,"","","30\" DUCTILE IRON PIPE","",104,290,30160]
[null,"","","57\" X 38\" CORRUGATED ALUMINUM","ALLOY PIPE ARCH CULVERT 0.109\"THICK",348,916,318768]
[null,"","","60\" X 38\" HORIZONTAL ELLIPTI- CAL RCP-IV","",452,1372,620144]
[null,"","","87\" X 63\" CAA PIPE ARCH","CULVERT, 0.135\" THICK",148,825,122100]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","18\" DUCTILE IRON PIPE ELBOW","",2,1477,2954]
[null,"","","24\" DUCTILE IRON PIPE ELBOW","",4,1983,7932]
[null,"","","30\" DUCTILE IRON PIPE ELBOW","",2,3027,6054]
[null,"0995000000-E","PIPE REMOVAL","","",18302,46.9173860780243,858682]
[null,"0996000000-N","PIPE CLEAN OUT","","",5,5000,25000]
[null,"1011000000-N","FINE GRADING","","",1,10771738,10771738]
[null,"1099500000-E","SHALLOW UNDERCUT","","",2100,27.6666666666667,58100]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",3900,60.512820512820497,236000]
[null,"1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",90000,54.9,4941000]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",29742,58.069968394862499,1727117]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",7697,71.975164349746606,553992.84]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",30.02,3813.3800799466999,114477.67]
[null,"1275000000-E","PRIME COAT","","",21954,6,131724]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",241178,2.0505965718266199,494558.78]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",710,10,7100]
[null,"","","(0\" TO 3\")","",290,18,5220]
[null,"1330000000-E","INCIDENTAL MILLING","","",12204,14.7500213044903,180009.26]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",190940,77.914789986383198,14877050]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",123845,81.838830796560202,10135330]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",52782,88.930101170853703,4693908.5999999996]
[null,"1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",200,85,17000]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",89030,80.879338425249898,7200687.5]
[null,"1575000000-E","ASP FOR PLANT MIX","","",23468,507.53408897221698,11910810]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",7441,212.423061416476,1580640]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",100,121.72,12172]
[null,"1880000000-E","GENERIC PAVING ITEM (TON)","PATCHING EXISTING PAVEMENT    (MILL)","",1894,125,236750]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","7\" CONCRETE TRUCK APRON","",580,125,72500]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",5555.8,35.351605529356704,196406.45]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",21550,5.7437122969837597,123777]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",3624.6,69.4592893008884,251762.14]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",21550,11.538375870069601,248652]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",47,462.25553191489399,21726.01]
[null,"2077000000-E","6\" OUTLET PIPE","","",282,44.819361702127701,12639.06]
[null,"2190000000-N","TEMP STL PLT COVER FOR MDS","","",75,1674,125550]
[null,"2209000000-E","ENDWALLS","","",145.9,1782.07539410555,260004.8]
[null,"2220000000-E","REINFORCED ENDWALLS","","",77.69,2610.3374951731198,202797.12]
[null,"2253000000-E","PIPE COLLARS","","",3.556,2027.2750281214801,7208.99]
[null,"2275000000-E","FLOWABLE FILL","","",152,406.427631578947,61777]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",485,3189.0059793814398,1546667.9]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",90.611000000000004,3812.8262572976801,345484]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",177.5,297.02084507042298,52721.2]
[null,"2355000000-N","FRAME W/GRATE 840.29 STD","","",1,1200,1200]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",95,1031.93684210526,98034]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",125,1259,157375]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",10,1199.4000000000001,11994]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",10,1144.2,11442]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",22,912.03636363636394,20064.8]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",30,1359,40770]
[null,"","","(F)","",65,1406.4,91416]
[null,"","","(G)","",80,1639.8625,131189]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",24,895.625,21495]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",42,2311,97062]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",97,1200,116400]
[null,"2535000000-E","**\"X**\" CONCRETE CURB","(8\" X 18\")","",1580,25,39500]
[null,"","","(9\" X 18\")","",350,30,10500]
[null,"2538000000-E","**'-**\" CONCRETE CURB & GUTTER","(2'-9\")","",10300,35,360500]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",46660,18,839880]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",28220,30.6888731396173,866040]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",8809.5,30.030535217662699,264554]
[null,"2570000000-N","MODIFIED CONCRETE FLUME","","",1,3700,3700]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",340,60,20400]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",2870,54,154980]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",37,3500,129500]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",380,123.147368421053,46796]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",110,135,14850]
[null,"2627000000-E","4\" CONC ISLAND COVER","","",580,54,31320]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",15845,95,1505275]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",350,150,52500]
[null,"2759000000-N","GENERIC PAVING ITEM (EA)","EMERGENCY VEHICLE ACCESS FOR","CONCRETE ISLAND",2,10000,20000]
[null,"2800000000-N","ADJ CATCH BASINS","","",14,1696,23744]
[null,"2815000000-N","ADJ DROP INLETS","","",1,1693,1693]
[null,"2830000000-N","ADJ MANHOLES","","",15,2059,30885]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",5,1538.6,7693]
[null,"2875000000-N","CONVERT CB TO DI","","",1,2000,2000]
[null,"2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXISTING CATCH BASIN","TO TRAFFIC BEARING JUNCTION   BOX",1,10867,10867]
[null,"","","CONVERT EXISTING DROP INLET TO","TRAFFIC BEARING JUNCTION BOX",1,10867,10867]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",3,25500,76500]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",23400,26.2975427350427,615362.5]
[null,"3045000000-E","SBGR SHOP CURVED","","",1650,28.159090909090899,46462.5]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",25,100,2500]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",211,49.075829383886301,10355]
[null,"3195000000-N","GR END TYPE AT-1","","",20,807.5,16150]
[null,"3210000000-N","GR END TYPE CAT-1","","",31,1059.6774193548399,32850]
[null,"3215000000-N","GR ANCHOR TYPE III","","",32,1953.75,62520]
[null,"3287000000-N","GR END TYPE TL-3","","",53,3158.4905660377399,167400]
[null,"3288000000-N","GR END TYPE TL-2","","",3,3000,9000]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",21,2433.3333333333298,51100]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",6570,1.4261796042618,9370]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",4475,9.11173184357542,40775]
[null,"3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",637.5,15,9562.5]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",12,1583.3333333333301,19000]
[null,"","","(III MOD)","",2,1800,3600]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(AT-1)","",10,600,6000]
[null,"","","(TL-3)","",26,2269.23076923077,59000]
[null,"3420000000-E","GENERIC GUARDRAIL ITEM (LF)","REMOVE AND REPLACE EXISTING   GUARDRAIL","",325,30,9750]
[null,"3435000000-N","GENERIC GUARDRAIL ITEM (EA)","GUARDRAIL PRE-FAB POSTS","",4,550,2200]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",61000,2.8,170800]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",3699,16.25,60108.75]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",1213,25,30325]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","36\" VINYL FENCE RESET","",185,55,10175]
[null,"3628000000-E","RIP RAP, CLASS I","","",3875,99.24,384555]
[null,"3635000000-E","RIP RAP, CLASS II","","",450,82,36900]
[null,"3642000000-E","RIP RAP, CLASS A","","",41,69.609756097561004,2854]
[null,"3649000000-E","RIP RAP, CLASS B","","",1333,93.587396849212297,124752]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",20975,2.60865315852205,54716.5]
[null,"3659000000-N","PREFORMED SCOUR HOLES","","",3,3300,9900]
[null,"4048000000-E","REINF CONC FOUNDTN","","",14,950,13300]
[null,"4054000000-E","PLN CONC FOUNDTN","","",1,10,10]
[null,"4057000000-E","OVERHEAD FOOTING","","",16,1500,24000]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",15793,6,94758]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",1958,6,11748]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",9230,8.0599458288190693,74393.3]
[null,"4082000000-E","SUPPORT, WOOD","","",58,15,870]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",25,108.44,2711]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",454,96.290748898678402,43716]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",82,104.53658536585399,8572]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",18,750,13500]
[null,"","","(B)","",1,350,350]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",1,750,750]
[null,"","","(B)","",1,350,350]
[null,"","","(D)","",18,197.833333333333,3561]
[null,"","","(F)","",2,150,300]
[null,"4138000000-N","DISPOSE SUPPORT, STL BM","","",2,500,1000]
[null,"4141000000-N","DISPOSE SUPPORT, WOOD","","",2,50,100]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",4,500,2000]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",243,5.3555555555555596,1301.4000000000001]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",26,5.6769230769230798,147.6]
[null,"4360000000-N","GENERIC SIGNING ITEM (EA)","VERTICAL PANEL, TYPE 3 OBJECT","MARKERS  OM3-C",19,150,2850]
[null,"","","","MARKERS  OM3-L",44,150,6600]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",6958,8.3154642138545594,57859]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",2747,15.8450309428467,43526.3]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",2592,6.9030671296296298,17892.75]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",1543,6.75,10415.25]
[null,"4415000000-N","FLASHING ARROW BOARD","","",25,2318.5304000000001,57963.26]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",24,7597.875,182349]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",157,105.414012738854,16550]
[null,"4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",1,5000,5000]
[null,"4430000000-N","DRUMS","","",3252,54.355781057810603,176765]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",109,46.838532110091698,5105.3999999999996]
[null,"4435000000-N","CONES","","",270,39.814814814814802,10750]
[null,"4445000000-E","BARRICADES (TYPE III)","","",2008,31.755776892430301,63765.599999999999]
[null,"4447000000-E","PED CHANNEL DEVICES","","",1010,18.861386138613899,19050]
[null,"4455000000-N","FLAGGER","","",1350,521.181481481481,703595]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",1,204026.17,204026.17]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",27,10513.703703703701,283870]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",9,2950,26550]
[null,"4480000000-N","TMA","","",13,6319.0769230769201,82148]
[null,"4485000000-E","PORT CONC BARRIER","","",4522,45.940070765148199,207741]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",2442,68.849999999999994,168131.7]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",1072,6.15,6592.8]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",404,25,10100]
[null,"4507000000-E","WATER FILLED BARRIER","","",300,160,48000]
[null,"4510000000-N","LAW ENFORCEMENT","","",3860,78.601554404145105,303402]
[null,"4516000000-N","SKINNY DRUM","","",573,55.588132635252997,31852]
[null,"4520000000-N","TUBULAR MARKERS (FIXED)","","",10,150,1500]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",1,1025,1025]
[null,"","","CONNECTED LANE CLOSURE DEVICE","",8,100,800]
[null,"","","TEMPORARY CURB RAMPS","",1,2845,2845]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",9667,4.9307954898107003,47666]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",472960,0.69518629482409,328795.31]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",22838,2.4155552149925601,55166.45]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",7261,4.0811596198870701,29633.3]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",52,78.846153846153896,4100]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",914,140.052516411379,128008]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",712,4.0283146067415698,2868.16]
[null,"4800000000-N","COLD APP PLAS CHAR TYPE *","(II)","",14,31.25,437.5]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",7,31.25,218.75]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",1870445,0.18265263613739,341641.71]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",104318,0.40338196667880999,42080]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",13774,1.6216131842602,22336.1]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",14657,3.0876850651565801,45256.2]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",1861,26.028264373992499,48438.6]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",106108,0.70221095487616003,74510.2]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",8000,0.75,6000]
[null,"4865000000-E","LINE REMOVAL 12\" WIDE","","",1000,1,1000]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",2156,2.61873840445269,5646]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",322,48.695652173912997,15680]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES, 4\"","20 MILS (STANDARD GLASS BEADS)",2979,10,29790]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",3290,7.1428571428571397,23500]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 8\"","20 MILS (STANDARD GLASS BEADS)",245,15,3675]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (24\", 90 MILS)",6001,9.2311948008665201,55396.4]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",5265,44.707692307692298,235386]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",995,10.44,10387.799999999999]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",33,99.143939393939405,3271.75]
[null,"4915000000-E","7' U-CHANNEL POSTS","","",2,32.5,65]
[null,"4957000000-N","OBJECT MARKERS (TYPE **)","(III)","",2,162,324]
[null,"5255000000-N","PORTABLE LIGHTING","","",3,201937.49,605812.47]
[null,"5325000000-E","**\" WATER LINE","(14\")","",302,350,105700]
[null,"","","(18\")","",8926,306.86847412054698,2739108]
[null,"5325400000-E","4\" WATER LINE","","",52,353.269230769231,18370]
[null,"5325600000-E","6\" WATER LINE","","",6291,92.064854554124906,579180]
[null,"5325800000-E","8\" WATER LINE","","",4646,95.570167886353801,444019]
[null,"5326000000-E","10\" WATER LINE","","",1865,119.988203753351,223778]
[null,"5326200000-E","12\" WATER LINE","","",4896,172.90032679738599,846520]
[null,"5326600000-E","16\" WATER LINE","","",2723,225.61696658097699,614355]
[null,"5327400000-E","24\" WATER LINE","","",11108,275,3054700]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",137711,11.9234048115256,1641984]
[null,"5534000000-E","**\" VALVE","(14\")","",2,14525,29050]
[null,"","","(18\")","",6,12000,72000]
[null,"5536000000-E","2\" VALVE","","",2,1200,2400]
[null,"5538000000-E","4\" VALVE","","",4,2835,11340]
[null,"5540000000-E","6\" VALVE","","",40,2656.5,106260]
[null,"5546000000-E","8\" VALVE","","",11,4234.1818181818198,46576]
[null,"5552000000-E","10\" VALVE","","",8,4600,36800]
[null,"5558000000-E","12\" VALVE","","",11,5599.0909090909099,61590]
[null,"5558600000-E","16\" VALVE","","",6,11500,69000]
[null,"5559400000-E","24\" VALVE","","",12,18500,222000]
[null,"5571000000-E","**\" TAPPING SLEEVE & VALVE","(2-1/2\")","",1,8100,8100]
[null,"","","(3\")","",3,8200,24600]
[null,"5571400000-E","4\" TAPPING SLEEVE & VALVE","","",1,8500,8500]
[null,"5571800000-E","8\" TAPPING SLEEVE & VALVE","","",2,9317,18634]
[null,"5572200000-E","12\" TAPPING SLEEVE & VALVE","","",2,14900,29800]
[null,"5589200000-E","2\" AIR RELEASE VALVE","","",11,13395.4545454545,147350]
[null,"5606000000-E","2\" BLOW OFF","","",1,3400,3400]
[null,"5606600000-E","6\" BLOW OFF","","",6,16500,99000]
[null,"5643000000-E","**\" WATER METER","(1\")","",3,3000,9000]
[null,"","","(5/8\")","",2,2700,5400]
[null,"5643100000-E","3/4\" WATER METER","","",3,2820,8460]
[null,"5643200000-E","2\" WATER METER","","",5,10000,50000]
[null,"5648000000-N","RELOCATE WATER METER","","",85,2648.4705882352901,225120]
[null,"5649000000-N","RECONNECT WATER METER","","",26,2261.5384615384601,58800]
[null,"5653210000-E","RELC 2\" DCV BACKFLOW PREVNT A","","",2,15000,30000]
[null,"5656100000-E","RELC **\" RPZ BACKFLOW PREVNT A","(1\")","",3,6500,19500]
[null,"","","(3/4\")","",33,5000,165000]
[null,"5656210000-E","RELC 2\" RPZ BACKFLOW PREVNT A","","",1,15000,15000]
[null,"5666000000-N","FIRE HYDRANT","","",22,7136.3636363636397,157000]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",6,6956.6666666666697,41740]
[null,"5673000000-E","FIRE HYDRANT LEG","","",363,73.140495867768607,26550]
[null,"5678600000-E","8\" LINE STOP","","",5,22000,110000]
[null,"5679000000-E","12\" LINE STOP","","",5,24000,120000]
[null,"5679200000-E","16\" LINE STOP","","",6,40000,240000]
[null,"5679600000-E","24\" LINE STOP","","",5,51000,255000]
[null,"5684000000-E","**\" LINE STOP W/ BYPASS","(14\")","",1,70000,70000]
[null,"5684400000-E","6\" LINE STOP W/ BYPASS","","",1,42300,42300]
[null,"5684800000-E","10\" LINE STOP W/ BYPASS","","",1,64000,64000]
[null,"5686000000-E","**\" H2O SERVICE LINE","(2\")","",171,35,5985]
[null,"","","(2-1/2\")","",35,40,1400]
[null,"5686500000-E","WATER SERVICE LINE","","",4018,20.052762568441999,80572]
[null,"5691000000-E","**\" SANITARY GRAVITY SEWER","(8\")","",5592,213,1191096]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",116,295,34220]
[null,"5691700000-E","18\" SANITARY GRAVITY SEWER","","",135,430,58050]
[null,"5709000000-E","**\" FORCE MAIN SEWER","(2\")","",69,110,7590]
[null,"","","(3\")","",287,43,12341]
[null,"5709100000-E","2\" FORCE MAIN SEWER","","",102,39,3978]
[null,"5709200000-E","4\" FORCE MAIN SEWER","","",60,215,12900]
[null,"5709300000-E","6\" FORCE MAIN SEWER","","",2053,101,207353]
[null,"5709400000-E","8\" FORCE MAIN SEWER","","",2627,109,286343]
[null,"5709500000-E","10\" FORCE MAIN SEWER","","",228,310,70680]
[null,"5709600000-E","12\" FORCE MAIN SEWER","","",1392,253.717672413793,353175]
[null,"5709700000-E","16\" FORCE MAIN SEWER","","",20555,228,4686540]
[null,"5709900000-E","24\" FORCE MAIN SEWER","","",34740,399.5,13878630]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",97660,16.356389514642601,1597365]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",37,13089.189189189199,484300]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",177.1,682.76397515527901,120917.5]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(2\")","",380,2,760]
[null,"","","(36\")","",180,150,27000]
[null,"","","(4\")","",237,41.7848101265823,9903]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",10924,12.7308678139875,139072]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",16669,14.5275061491391,242159]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",1065,68.488262910798099,72940]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",5766,26.7082032604925,153999.5]
[null,"5805000000-E","ABANDON 14\" UTILITY PIPE","","",292,90,26280]
[null,"5810000000-E","ABANDON 16\" UTILITY PIPE","","",54047,27.159564823209401,1467893]
[null,"5811000000-E","ABANDON 18\" UTILITY PIPE","","",895,50.0536312849162,44798]
[null,"5813000000-E","ABANDON 24\" UTILITY PIPE","","",19242,49,942858]
[null,"5814000000-E","ABANDON 30\" UTILITY PIPE","","",65,130,8450]
[null,"5815000000-N","REMOVE WATER METER","","",11,1458.6363636363601,16045]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",9,4000,36000]
[null,"5816000000-N","ABANDON UTILITY MANHOLE","","",1,675,675]
[null,"5828000000-N","REMOVE UTILITY MANHOLE","","",36,4619.4444444444398,166300]
[null,"5835000000-E","**\" ENCASEMENT PIPE","(14\")","",139,360,50040]
[null,"","","(32\")","",521,830,432430]
[null,"","","(48\")","",743,1265,939895]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",214,371.44859813084099,79490]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",108,275,29700]
[null,"5835900000-E","20\" ENCASEMENT PIPE","","",301,406.56146179401998,122375]
[null,"5836000000-E","24\" ENCASEMENT PIPE","","",330,650,214500]
[null,"5872500000-E","BORE & JACK **\"","(14\")","",139,330,45870]
[null,"","","(16\")","",120,375,45000]
[null,"","","(18\")","",58,500,29000]
[null,"","","(20\")","",135,442.222222222222,59700]
[null,"","","(24\")","",170,460,78200]
[null,"","","(32\")","",235,590,138650]
[null,"","","(48\")","",271,845,228995]
[null,"5872600000-E","DIRECT DRILL **\"","(10\")","",1098,64.275956284152997,70575]
[null,"","","(12\")","",1144,169.42307692307699,193820]
[null,"","","(14\")","",230,180,41400]
[null,"","","(16\")","",7293,263,1918059]
[null,"","","(18\")","",6805,284,1932620]
[null,"","","(24\")","",17863,371,6627173]
[null,"","","(3\")","",287,39,11193]
[null,"","","(6\")","",901,57.513873473917897,51820]
[null,"","","(8\")","",1800,78.84375,141918.75]
[null,"5882000000-N","GENERIC UTILITY ITEM (EA)","12\" CHECK VALVE AND VAULT","",1,100000,100000]
[null,"","","12\" SEWER VALVE","",1,10000,10000]
[null,"","","16\" SEWER VALVE","",3,16000,48000]
[null,"","","2\" AIR AND VACUUM RELEASE     VALVE","",25,12800,320000]
[null,"","","2\" CHECK VALVE","",4,2600,10400]
[null,"","","24\" PRESSURE SUSTAINING VALVE ASSEMBLY","",1,350000,350000]
[null,"","","24\" SEWER VALVE","",30,40000,1200000]
[null,"","","6\" INSERTION VALVE","",2,8300,16600]
[null,"","","6\" SEWER VALVE","",2,5500,11000]
[null,"","","8\" INSERTION VALVE","",2,16000,32000]
[null,"","","8\" SEWER VALVE","",2,7000,14000]
[null,"","","ADJUST SANITARY SEWER CLEAN-","OUT TO FINISH GRADE",4,2500,10000]
[null,"","","FLOW METER VAULT","",1,112000,112000]
[null,"","","RECONNECT FORCE MAIN","",12,11500,138000]
[null,"","","RELOCATE YARD HYDRANT","",1,8000,8000]
[null,"5912000000-N","GENERIC UTILITY ITEM (LS)","PUMP STATION","",1,775000,775000]
[null,"","","REMOVE EXISTING PUMP STATION","",1,100000,100000]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",291495,0.36347518825365999,105951.2]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",4160,83.734531250000003,348335.65]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",18807,58.131275588876498,1093274.8999999999]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",13762,49.847747420433102,686004.7]
[null,"6015000000-E","TEMPORARY MULCHING","","",926.01,1447.11104631699,1340039.3]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",36193,2.1289061420716702,77051.5]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",183.48,626.95389143230898,115033.5]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",20385,5.6426293843512401,115025]
[null,"6029000000-E","SAFETY FENCE","","",39800,2.2537688442211099,89700]
[null,"6030000000-E","SILT EXCAVATION","","",54460,6.4959786999632803,353771]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",201770,1.71197402983595,345425]
[null,"6037000000-E","COIR FIBER MAT","","",185805,5.9691208525066601,1109092.5]
[null,"6038000000-E","PERM SOIL REINF MAT","","",1705,11.8403225806452,20187.75]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",31848,8.8524554132127609,281933]
[null,"6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",1800,4.9583333333333304,8925]
[null,"6045000000-E","**\" TEMPORARY PIPE","(18\")","",24,100,2400]
[null,"","","(24\")","",155,100,15500]
[null,"","","(30\")","",275,112.5,30937.5]
[null,"","","(42\")","",265,140,37100]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",1310,40.259541984732799,52740]
[null,"6069000000-E","STILLING BASINS","","",135,35,4725]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",50,1010.6,50530]
[null,"6071010000-E","WATTLE","","",150,16,2400]
[null,"6071012000-E","COIR FIBER WATTLE","","",24185,18.322741368616899,443135.5]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",770,13.146103896103901,10122.5]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",8730,10.7784650630011,94096]
[null,"6071030000-E","COIR FIBER BAFFLE","","",12190,6.3997128794093499,78012.5]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",28,1138.7857142857099,31886]
[null,"","","(2\")","",5,1470,7350]
[null,"","","(2-1/2\")","",3,1687,5061]
[null,"","","(3\")","",1,2182,2182]
[null,"6084000000-E","SEEDING AND MULCHING","","",638.85,2580.0320889097602,1648253.5]
[null,"6087000000-E","MOWING","","",313.07,237.13865908582699,74241]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",9943,5.9636427637533904,59296.5]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",30.98,1345.2969657843801,41677.300000000003]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",14025,6.1889483065953703,86800]
[null,"6102000000-E","SODDING","","",175,12,2100]
[null,"6105000000-E","WATER","","",3,500,1500]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",418.55,946.053040258034,395970.5]
[null,"6111000000-E","IMPERVIOUS DIKE","","",3699,370.38659097053301,1370060]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",260,130.38461538461499,33900]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",328,228.976006097561,75104.13]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",47,965.95744680851101,45400]
[null,"6123000000-E","REFORESTATION","","",1.74,4735.6321839080501,8240]
[null,"6129000000-E","WETLAND REFORESTATION","","",0.27200000000000002,4000,1088]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",20,426,8520]
[null,"","","","DEVICE CLEANOUT",60,197,11820]
[null,"6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","DISKING","",0.27200000000000002,1000,272]
[null,"","","RIPPING","",0.27200000000000002,1000,272]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",12,933,11196]
[null,"7060000000-E","SIGNAL CABLE","","",55735,2.7365928052390802,152524]
[null,"7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",4,500,2000]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",249,829.27710843373495,206490]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",54,985.555555555556,53220]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",31,1330.16129032258,41235]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",3020,3.7238410596026501,11246]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",6500,4.9000000000000004,31850]
[null,"7279000000-E","TRACER WIRE","","",39410,0.8,31528]
[null,"7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",160,21,3360]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",7810,9.4641485275288098,73915]
[null,"","","(2, 2\")","",18200,10.0175824175824,182320]
[null,"","","(3, 2\")","",80,19,1520]
[null,"","","(4, 2\")","",190,21.947368421052602,4170]
[null,"7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",10,15,150]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",1670,17,28390]
[null,"","","(2, 2\")","",24480,22.005821078431399,538702.5]
[null,"","","(3, 2\")","",1330,23.845864661654101,31715]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",138,335.97101449275402,46364]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",87,754.77011494252895,65665]
[null,"7360000000-N","WOOD POLE","","",42,1050,44100]
[null,"7372000000-N","GUY ASSEMBLY","","",91,642.36263736263697,58455]
[null,"7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",10,460,4600]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",31,830,25730]
[null,"7432000000-E","2\" RISER WITH TUBING","","",4,895,3580]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",28245,7.7409807045494796,218644]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",36180,1.6939192924267601,61286]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(48)","",41060,3.5,143710]
[null,"7528000000-E","DROP CABLE","","",4740,2.7,12798]
[null,"7540000000-N","SPLICE ENCLOSURE","","",21,1755,36855]
[null,"7541000000-N","MOD SPLICE ENCLOSURE","","",1,1582,1582]
[null,"7552000000-N","INTERCONNECT CENTER","","",22,1565,34430]
[null,"7566000000-N","DELINEATOR MARKER","","",49,145,7105]
[null,"7574550000-N","FURN WRLESS LIGHTNING ARSTR","","",1,208,208]
[null,"7575142010-N","900MHZ SER/ETH SPEC RADIO","","",10,4100,41000]
[null,"7575142060-N","MOD RADIO INSTALL","","",6,1210,7260]
[null,"7575160000-E","REM EXT COMM CABLE","","",4650,0.8,3720]
[null,"7575200000-N","GPS UNIT","","",2,1305,2610]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",34,36264.705882352901,1233000]
[null,"7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,49950,99900]
[null,"7613000000-N","SOIL TEST","","",40,1111.75,44470]
[null,"7614100000-E","DRILLED PIER FOUND","","",204,1400,285600]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",40,120.485,4819.3999999999996]
[null,"7636000000-N","SIGN FOR SIGNALS","","",121,451.21487603305798,54597]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",20,2172.35,43447]
[null,"7642300000-N","TYPE III PED W/ FOUNDATION","","",9,5050,45450]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",16,1788.125,28610]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070E, BASE MOUNTED)","",3,14115,42345]
[null,"","","(TYPE 2070E, BASE-MOUNTED)","",13,16355,212615]
[null,"","","(TYPE 2070E, POLE-MOUNTED)","",1,14500,14500]
[null,"7708000000-N","DETECTOR CARD (***********)","(2070E)","",165,120,19800]
[null,"","","(TYPE 2070E)","",19,125,2375]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",1,178,178]
[null,"7901000000-N","CABINET BASE EXTENDER","","",16,585.875,9374]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",2,19000,38000]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",23,2523.47826086957,58040]
[null,"7972000000-N","METAL POLE REMOVAL","","",23,513.91304347826099,11820]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","CCTV WOOD POLE","",6,2600,15600]
[null,"","","CONTROLLER (TYPE 2070E)","",3,4495,13485]
[null,"","","DECORATIVE METAL POLE WITH","SINGLE MAST ARM",4,34000,136000]
[null,"","","DIGITAL CCTV CAMERA ASSEMBLY","",7,4525,31675]
[null,"","","DMS STRUCTURE (BACK-TO-BACK","PEDESTAL)",2,50000,100000]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE 1C)","",4,103000,412000]
[null,"","","ELECTRICAL SERVICE FOR ITS","DEVICE",8,1510,12080]
[null,"","","ETHERNET EDGE SWITCH","",20,2200,44000]
[null,"","","FIELD EQUIPMENT CABINET","",3,7035,21105]
[null,"","","FURNISH ETHERNET EDGE SWITCH","",1,1760,1760]
[null,"","","JUNCTION BOX (SPECIAL OVER-","SIZED HEAVY DUTY)",24,1750,42000]
[null,"","","JUNCTION BOX MARKER","",19,100,1900]
[null,"","","LUMINAIRE MAST ARM","",2,2030,4060]
[null,"","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",14,40482.142857142899,566750]
[null,"","","PROTECTIVE COATING FOR SINGLE","MAST ARM POLE (BLACK)",4,2130,8520]
[null,"","","RELOCATE ETHERNET EDGE SWITCH","",2,250,500]
[null,"","","REMOVE 900MHZ RADIO","",10,350,3500]
[null,"","","WOOD PEDESTAL","",3,205,615]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","BACK PULL FIBER OPTIC CABLE","",310,3.4,1054]
[null,"7992000000-E","GENERIC SIGNAL ITEM (CY)","METAL POLE FOUNDATION","",36,1200,43200]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(390+15.00 -L- LT)","",1,2245000,2245000]
[null,"8035000000-N","REMV EXIST STR **********","(16+08.00 -L-)","",1,21000,21000]
[null,"","","(18+27.00 -L-)","",1,140000,140000]
[null,"","","(18+30.00 -L-)","",1,30000,30000]
[null,"","","(21+68.50 -L-)","",1,135000,135000]
[null,"","","(23+55.00 -L-)","",1,105000,105000]
[null,"","","(23+71.50 -L-)","",1,29000,29000]
[null,"","","(369+42.00 -L- EBL)","",1,92000,92000]
[null,"","","(390+15.00 -L- RT)","",1,350000,350000]
[null,"8056000000-N","REMV EXIST STR **********","(226+01.00 -L-)","",1,19575,19575]
[null,"","","(316+72.00 -L-)","",1,19575,19575]
[null,"","","(64+15.00 -L-)","",1,22750,22750]
[null,"","","(83+76.00 -L-)","",1,19575,19575]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",7,1521.42857142857,10650]
[null,"8112730000-N","PDA TESTING","","",17,2535.2941176470599,43100]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(16+08.00 -L-)","",1,15000,15000]
[null,"","","(18+27.00-L-)","",1,12500,12500]
[null,"","","(18+30.00 -L-)","",1,8500,8500]
[null,"","","(23+55.00 -L-)","",1,30000,30000]
[null,"","","(23+71.50 -L-)","",1,3000,3000]
[null,"","","(369+42.00 -L- EBL)","",1,11000,11000]
[null,"","","(390+15.00 -L- LT)","",1,10000,10000]
[null,"","","(390+15.00 -L- RT)","",1,10000,10000]
[null,"8126000000-N","CULV EXCAV @ ************","(226+01.00 -L-)","",1,56795,56795]
[null,"","","(316+72.00 -L-)","",1,63595,63595]
[null,"","","(64+15.00 -L-)","",1,53490,53490]
[null,"","","(83+76.00 -L-)","",1,71560,71560]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",807,80,64560]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",61037,66.137416648917906,4036829.5]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",80040.800000000003,0.80380468461084997,64337.17]
[null,"8175000000-E","CLASS AA CONC (BRIDGE)","","",399.9,1500,599850]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",583,952.48713550600303,555300]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",887.2,950,842840]
[null,"8210000000-N","BRG APPR SLAB ***********","(16+08.00 -L-)","",1,31500,31500]
[null,"","","(18+27.00 -L-)","",1,44000,44000]
[null,"","","(18+30.00 -L-)","",1,34000,34000]
[null,"","","(21+68.50 -L-)","",1,55000,55000]
[null,"","","(23+55.00 -L-)","",1,25000,25000]
[null,"","","(23+71.50 -L-)","",1,32690,32690]
[null,"","","(31+30.81 -Y REV-)","",1,125000,125000]
[null,"","","(369+42.00 -L- EBL)","",1,52000,52000]
[null,"","","(369+42.00 -L- WBL)","",1,52000,52000]
[null,"","","(39+52.37 -Y14A-)","",1,110000,110000]
[null,"","","(390+15.00 -L- LT)","",1,52000,52000]
[null,"","","(390+15.00 -L- RT)","",1,52000,52000]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",90662,1.46096766010015,132454.25]
[null,"8224000000-E","EPOXY COAT REINF STL BRDG","","",61921,1.7,105265.7]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",119524,2.0499999999999998,245024.2]
[null,"8259000000-E","36\" PRESTR CONCRETE GIRDR","","",1873.38,275.398904653621,515926.8]
[null,"8262000000-E","45\" PRESTR CONCRETE GIRDR","","",786.88,255,200654.4]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",2455.63,350,859470.5]
[null,"8277000000-E","72\" MOD PRESTR CONC GIRDR","","",2068.1999999999998,500,1034100]
[null,"8296000000-N","POLLUTION CONTROL","","",1,43750,43750]
[null,"8328000000-E","PILE DRV EQUIP SETUP * PRESTR CONC PILES","(16\")","",28,2700,75600]
[null,"","","(24\")","",24,4300,103200]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",162,1745.0617283950601,282700]
[null,"","","(HP12 X 53)","",14,770,10780]
[null,"","","(HP12X53)","",12,1650,19800]
[null,"8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 89)","",16,550,8800]
[null,"","","(HP14X73)","",12,1750,21000]
[null,"","","(PP 18 X 0.50)","",23,2630.4347826087001,60500]
[null,"8333000000-E","16\" PRESTR CONC PILES","","",1715,180,308700]
[null,"8350000000-E","24\" PRESTR CONC PILES","","",2520,200,504000]
[null,"8356000000-E","HP**X** GALV PILES","(HP 14 X 89)","",800,125,100000]
[null,"8364000000-E","HP12X53 PILES","","",12606,99.654331270823405,1256242.5]
[null,"8384200000-E","HP14X73 GALV PILES","","",810,74,59940]
[null,"8386000000-E","PP18X0.50 STL PILE","","",525,145,76125]
[null,"8387000000-E","PP18X0.50 GALV STL PILE","","",760,130,98800]
[null,"8391000000-N","STEEL PILE POINTS","","",166,157.490963855422,26143.5]
[null,"8392000000-N","PIPE PILE PLATES","","",7,240,1680]
[null,"8392500000-E","PREDRILLING FOR PILES","","",352,100,35200]
[null,"8393000000-N","PILE REDRIVES","","",206,429.36932038834999,88450.08]
[null,"8475000000-E","TWO BAR METAL RAIL","","",1730.95,128,221561.60000000001]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",1038.92,133.440351518885,138633.85]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",881.75,169.997164729232,149895]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",1792.19,120,215062.8]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",119,110,13090]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",38.799999999999997,125,4850]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",3868,75.049896587383699,290293]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",4302,1.86163412366341,8008.75]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",7,20213.571428571398,141495]
[null,"8660000000-E","CONCRETE REPAIRS","","",44.2,800.11312217194597,35365]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",483.4,689.84795200661995,333472.5]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",32,90,2880]
[null,"8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(390+15.00 -L- LT)","",1,74500,74500]
[null,"","","(390+15.00 -L- RT)","",1,74500,74500]
[null,"8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",1620,180,291600]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",3735,199.31325301204799,744435]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",1950,52.79,102940.5]
[null,"","","(10)","",9625,70.39,677503.75]
[null,"","","(11)","",14880,70.39,1047403.2]
[null,"","","(12)","",8105,70.39,570510.94999999995]
[null,"","","(13)","",4770,70.39,335760.3]
[null,"","","(2)","",460,52.79,24283.4]
[null,"","","(3)","",4540,70.39,319570.59999999998]
[null,"","","(4)","",2015,70.39,141835.85]
[null,"","","(5)","",6270,70.39,441345.3]
[null,"","","(6)","",2765,70.39,194628.35]
[null,"","","(7)","",8265,70.39,581773.35]
[null,"","","(8)","",4135,70.39,291062.65000000002]
[null,"","","(9)","",16210,70.39,1141021.8999999999]
[null,"8804000000-N","GENERIC CULVERT ITEM (LS)","ASBESTOS ASSESSMENT","",1,6000,6000]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","CONST, MAINT, & REM OF TEMP   STRUCTURE","AT STA 18+76.04-L_DET-",1,470000,470000]
[null,"","","PAINTING CONTAINMENT FOR","BRIDGE 640021",1,110000,110000]
[null,"","","VOLUMETRIC MIXER","",1,1000,1000]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","3'-0\" X 2'-6\" PRESTRESSED","CONCRETE BENT CAPS",153.32,925,141821]
[null,"","","FIBER OPTIC CONDUIT SYSTEM","",665.42,37.840311382284902,25179.7]
[null,"","","FOAM JOINT SEALS FOR PRESERVA-TION","",267.10000000000002,43.285286409584401,11561.5]
[null,"","","GALVANIC CATHODIC PROTECTION","INTEGRAL PILE JACKET (MONI-   TORING)",40.5,1950,78975]
[null,"","","","INTEGRAL PILE JACKET (NON-MON-ITORING)",67.25,1935,130128.75]
[null,"","","GALVANIZED PEDESTRIAN SAFETY  RAIL","",869.25,115,99963.75]
[null,"","","POURABLE SILICONE JOINT       SEALANT","",58,125,7250]
[null,"","","POURABLE SILICONE JOINT SEAL- ANT","",174.9,15,2623.5]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","LATEX MODIFIED CONCRETE","OVERLAY-EARLY STRENGTH",102,1925,196350]
[null,"8882000000-E","GENERIC STRUCTURE ITEM (CF)","ELASTOMETRIC CONCRETE FOR","PRESERVATION",77.400000000000006,325,25155]
[null,"","","PRESTRESSED CONCRETE GIRDER   REPAIR","",136.5,975,133087.5]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","18\" GALVANIZED STEEL SHEET    PILES","",3592,55,197560]
[null,"","","BEAM END EPOXY COATING","",272.5,87,23707.5]
[null,"","","BRIDGE JOINT DEMOLITION","",278.10000000000002,25,6952.5]
[null,"","","CATHODIC PROTECTION OF PILE","CAP (MONITORING)",888,176,156288]
[null,"","","","CAP (NON-MONITORING)",4179,125,522375]
[null,"","","EPOXY COATING","",3287.2,16.334889875882201,53696.05]
[null,"","","EPOXY OVERLAY SYSTEM I","",45,150,6750]
[null,"","","PRESTRESSED CONC GIRDERS WITH","THERMAL SPRAY ANODE (NON-MONI-TORING)",35966,45.15,1623864.9]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","HYDRO-DEMOLITION OF BRIDGE","DECK",2028.2,70,141974]
[null,"","","PLACING & FINISHING LATEX","MODIFIED CONC OVERLAY-EARLY   STRENGTH",2028.2,28,56789.599999999999]
[null,"","","SCARIFYING BRIDGE DECK","",2028.2,20,40564]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","BRIDGE JACKING TYPE I","BRIDGE #640021",1,7500,7500]
[null,"","","BULK ANODE","",8,850,6800]
[null,"","","CLEANING & PAINTING OF EXT    BEARINGS","WITH HIGH RATIO CALCIUM SULF-   ONATE",196,575,112700]
[null,"","","REMOVE AND RESET BEARINGS","",1,2000,2000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE","NO. 300433",3,7500,22500]

{"sheet":"ITEMS - DIV 04","index":6,"n_rows":590,"n_cols":8,"rows_kept":590,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 04"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",10,565006.5,5650065]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",8,122712.535,981700.28]
[null,"0000996000-N","DESIGN AND CONSTRUCTION","","",1,85711000,85711000]
[null,"0001000000-E","CLEARING & GRUBBING","","",47,73707.627118644101,3479000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",6,9850,59100]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",321840,7.4004791200596598,2381770.2000000002]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(15+61.00 -L-)","",1,30000,30000]
[null,"","","(16+99.00 -L-)","",1,25000,25000]
[null,"","","(17+00.00-L-)","",1,33000,33000]
[null,"","","(17+37.36 -L-)","",1,24000,24000]
[null,"","","(27+01.91 -Y7-)","",1,39000,39000]
[null,"","","(42+56.82 -Y1-)","",1,46000,46000]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(217+31.76 -L- LT)","",1,65000,65000]
[null,"","","(217+31.76 -L- RT)","",1,31000,31000]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(16+10.00 -L-)","",1,9000,9000]
[null,"","","(19+07.12 -L-)","",1,23000,23000]
[null,"","","(28+02.81 -L-)","",1,24000,24000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",21650,7.8810623556581998,170625]
[null,"0043000000-N","GRADING","","",4,107408.75,429635]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",5,100.8,504]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",400,15,6000]
[null,"0063000000-N","GRADING","","",1,490000,490000]
[null,"0084000000-E","WICK DRAINS","","",205000,0.7,143500]
[null,"0106000000-E","BORROW EXCAVATION","","",761820,7.7693680922002599,5918860]
[null,"0127000000-N","EMBM'T SETTLEMENT GAUGE","","",8,1250,10000]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",42265,7.0545131905832204,298159]
[null,"0141000000-E","BERM DITCH CONSTRUCTION","","",830,4,3320]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",107180,7.0332338122784099,753822]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",12550,18.5,232175]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",17090,3.7308367466354602,63760]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",13600,23.7,322320]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",19800,10.6111111111111,210100]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",40850,1.76223990208078,71987.5]
[null,"0199000000-E","TEMPORARY SHORING","","",3070,29.7,91179]
[null,"0223000000-E","ROCK PLATING","","",11660,61.672384219553997,719100]
[null,"0241000000-E","GENERIC GRADING ITEM (SY)","GEOTEXTILE FOR WICK DRAINS","",10400,1.5,15600]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,63,3150]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",4101,41.8513045598635,171632.2]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",17586,2.3597634481974299,41498.800000000003]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",884,58.192760180995499,51442.400000000001]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",30,348,10440]
[null,"0342000000-E","**\" SIDE DRAIN PIPE","(30\")","",496,110,54560]
[null,"","","(36\")","",172,137,23564]
[null,"","","(42\")","",824,148,121952]
[null,"","","(48\")","",172,225,38700]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",2626,72,189072]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",2152,78,167856]
[null,"0345000000-E","24\" SIDE DRAIN PIPE","","",1844,86,158584]
[null,"0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",10,550,5500]
[null,"","","(18\")","",2,600,1200]
[null,"0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",744,86,63984]
[null,"","","(18\", V)","",696,84.528735632183896,58832]
[null,"","","(24\", V)","",140,107,14980]
[null,"","","(30\", V)","",64,148,9472]
[null,"","","(54\", V)","",256,300,76800]
[null,"0366000000-E","15\" RC PIPE CULV III","","",1600,70.793499999999995,113269.6]
[null,"0372000000-E","18\" RC PIPE CULV III","","",2692,75.222882615155996,202500]
[null,"0378000000-E","24\" RC PIPE CULV III","","",244,105.377049180328,25712]
[null,"0384000000-E","30\" RC PIPE CULV III","","",1044,109.547892720307,114368]
[null,"0390000000-E","36\" RC PIPE CULV III","","",956,134.06694560669499,128168]
[null,"0396000000-E","42\" RC PIPE CULV III","","",704,153.31818181818201,107936]
[null,"0402000000-E","48\" RC PIPE CULV III","","",356,202.797752808989,72196]
[null,"0408000000-E","54\" RC PIPE CULV III","","",100,285.60000000000002,28560]
[null,"0426000000-E","72\" RC PIPE CULV III","","",404,509,205636]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",2432,70.759868421052602,172088]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",712,82,58384]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",416,80.201923076923094,33364]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",280,114.428571428571,32040]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",1196,149.11371237458201,178340]
[null,"0542000000-E","**\" PVC PIPE CULVERTS","(6\")","",64,70,4480]
[null,"0576000000-E","**\" CS PIPE CULV *****\"","(36\", 0.079\")","",20,201,4020]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",592,68.216216216216196,40384]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",40,110,4400]
[null,"0594000000-E","24\" CS PIPE CULV 0.064\"","","",32,145,4640]
[null,"0600000000-E","30\" CS PIPE CULV 0.079\"","","",32,170,5440]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",12,641.66666666666697,7700]
[null,"","","(18\", 0.064\")","",2,650,1300]
[null,"0654000000-E","***X***\"CSP ARCH CULV *****","(42\" X 29\", 0.079\")","",176,275,48400]
[null,"","","(57\" X 38\", 0.109\")","",60,385,23100]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\", 0.250\")","",60,265,15900]
[null,"","","(18\", 0.250\")","",406,340,138040]
[null,"","","(24\", 0.250\")","",46,300,13800]
[null,"","","(30\", 0.312\")","",364,350,127400]
[null,"","","(30\", 0.500\")","",592,480.89189189189199,284688]
[null,"","","(36\", 0.312\")","",106,400,42400]
[null,"","","(36\", 0.375\")","",96,589,56544]
[null,"","","(42\", 0.375\")","",114,585,66690]
[null,"","","(48\", 0.500\")","",84,750,63000]
[null,"","","(54\", 0.500\")","",122,975,118950]
[null,"","","(72\", 0.625\")","",104,2300,239200]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\", 0.250\")","",60,0.01,0.6]
[null,"","","(18\", 0.250\")","",406,0.01,4.0599999999999996]
[null,"","","(24\", 0.250\")","",46,0.01,0.46]
[null,"","","(30\", 0.312\")","",364,0.01,3.64]
[null,"","","(30\", 0.500\")","",592,1.0218243243243199,604.91999999999996]
[null,"","","(36\", 0.312\")","",106,0.01,1.06]
[null,"","","(36\", 0.375\")","",96,0.01,0.96]
[null,"","","(42\", 0.375\")","",114,0.01,1.1399999999999999]
[null,"","","(48\", 0.500\")","",84,0.01,0.84]
[null,"","","(54\", 0.500\")","",122,0.01,1.22]
[null,"","","(72\", 0.625\")","",104,0.01,1.04]
[null,"0995000000-E","PIPE REMOVAL","","",4039,25.406164892300101,102615.5]
[null,"1000000000-E","6\" SLOPE PROTECTION","","",345,130,44850]
[null,"1011000000-N","FINE GRADING","","",3,1187214.66666667,3561644]
[null,"1099500000-E","SHALLOW UNDERCUT","","",3250,12.036923076923101,39120]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",6200,28.387096774193601,176000]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",2144,34.281716417910502,73500]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",5170,42.579303675048401,220135]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",2.8,6000,16800]
[null,"1260000000-E","AGGREGATE SHOULDER BORROW","","",44,35,1540]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",701100,1.21071402082442,848831.6]
[null,"","","(2\")","",263030,1.45874424970536,383693.5]
[null,"","","(2-1/2\")","",136200,1.75,238350]
[null,"","","(2-3/4\")","",264940,1.7875179285875999,473585]
[null,"","","(3\")","",190,15,2850]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",560,26.95,15092]
[null,"","","(0\" TO 3\")","",220,43.8,9636]
[null,"","","(2-1/2\" TO 4\")","",24800,2.6,64480]
[null,"","","(3/4\" TO 2-3/4\")","",525,12.95,6798.75]
[null,"1330000000-E","INCIDENTAL MILLING","","",27340,7.8061356986100998,213419.75]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",176300,45.075801191151399,7946863.75]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",91065,43.953247680228401,4002602.5]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",27375,49.108694063926897,1344350.5]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",8915,67.918171620863703,605490.5]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",168000,51.570550595238103,8663852.5]
[null,"1575000000-E","ASP FOR PLANT MIX","","",14717,452.08814636135099,6653381.25]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",11063,618.26385248124404,6839853]
[null,"1662000000-E","OG ASP FRICT FC-1 MOD","","",22880,54.75,1252680]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",890,123.876404494382,110250]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",585190,0.17473299270322001,102252]
[null,"1847000000-E","******\"PCC PVMT THRU LNS","(11\")","",6381,121,772101]
[null,"1881000000-E","GENERIC PAVING ITEM (LF)","MILLED RUMBLE STRIPS (ASPHALT","CONCRETE)(12\")",106260,0.1,10626]
[null,"","","","CONCRETE)(8\")",9700,0.1,970]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","11\" CONCRETE TRUCK APRON","",1571,76.5,120181.5]
[null,"2000000000-N","RIGHT-OF-WAY MARKERS","","",11,375,4125]
[null,"2020000000-N","CONTROL-OF-ACCESS MARKERS","","",16,375,6000]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",3315.2,17.5675675675676,58240]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2800,6.3928571428571397,17900]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",2016,63,127008]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",470.4,60,28224]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",14800,7.75,114700]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",32,445.71875,14263]
[null,"2077000000-E","6\" OUTLET PIPE","","",192,23.421875,4497]
[null,"2099000000-E","SHOULDER DRAIN","","",80,80,6400]
[null,"2110000000-E","4\" SHOULDER DRAIN PIPE","","",80,55,4400]
[null,"2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",90,55,4950]
[null,"2132000000-N","CONC PAD SHLDR DRN OUTLET","","",2,550,1100]
[null,"2209000000-E","ENDWALLS","","",100.29,1291.95034400239,129569.7]
[null,"2220000000-E","REINFORCED ENDWALLS","","",40.9,1381.3936430317799,56499]
[null,"2253000000-E","PIPE COLLARS","","",121.23,1304.87090654129,158189.5]
[null,"2275000000-E","FLOWABLE FILL","","",555,267.32432432432398,148365]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",265,4064.50188679245,1077093]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",30.4,1600,48640]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",165,592.97878787878801,97841.5]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",3,900,2700]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",65,883.87692307692305,57452]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",136,1500.9264705882399,204126]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",5,725.8,3629]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",21,663.66666666666697,13937]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",1,978,978]
[null,"","","(F)","",11,939.45454545454595,10334]
[null,"","","(G)","",1,1000,1000]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",20,691.15,13823]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",4,1965,7860]
[null,"2440000000-N","CONC TRANS SECT FOR CATCH BASIN","","",3,1200,3600]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",7,1065,7455]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","CONCRETE APRON FOR DROP INLET","",29,2300,66700]
[null,"","","TRASH GRATE FOR 24\" RCP FES","",1,10673.77,10673.77]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",860,19.25,16555]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",2035,27,54945]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",5078,25.894042930287501,131489.95000000001]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",330,50,16500]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",4,2200,8800]
[null,"2613000000-N","REM & REP CURB RAMPS","","",7,2000,14000]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",1130,74.783185840708001,84505]
[null,"2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",3010,74.055647840531606,222907.5]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",360,65.25,23490]
[null,"2703000000-E","CONC BARRIER TYPE ******","(T)","",12300,132,1623600]
[null,"2710000000-N","CONC BARRIER TRANS SECTN","","",3,25400,76200]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",130,100,13000]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","1'-6\" CONCRETE CURB & GUTTER","(11\" DEPTH)",1370,21.95,30071.5]
[null,"2815000000-N","ADJ DROP INLETS","","",25,2400,60000]
[null,"2905000000-N","CONVERT DI TO JB","","",1,3250,3250]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",2,12800,25600]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",30325,19.805441055235001,600600]
[null,"3045000000-E","SBGR SHOP CURVED","","",675,23,15525]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",60,39.203333333333298,2352.1999999999998]
[null,"3210000000-N","GR END TYPE CAT-1","","",18,602.5,10845]
[null,"3215000000-N","GR ANCHOR TYPE III","","",13,1648.0769230769199,21425]
[null,"3287000000-N","GR END TYPE TL-3","","",116,2860.43103448276,331810]
[null,"3288000000-N","GR END TYPE TL-2","","",5,2700,13500]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",41,1728.9024390243901,70885]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",38052,1.2458044255229701,47405.35]
[null,"3365000000-E","REMOVE EXISTING GUIDERAIL","","",15500,1.05,16275]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",212.5,12,2550]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(III)","",4,1100,4400]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-3)","",4,1600,6400]
[null,"3389400000-E","DBL FACED CABLE GUIDERAIL","","",19625,8.2377070063694298,161665]
[null,"3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",12,102,1224]
[null,"3389600000-N","CBL GUIDERAIL ANCH UNIT","","",22,1695.45454545455,37300]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",28850,2.7845753899480101,80335]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1794,18.356744704570801,32932]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",495,25.909090909090899,12825]
[null,"3557000000-E","ADDITIONAL BARBED WIRE","","",350,1,350]
[null,"3566000000-E","WOVEN WIRE FENCE RESET","","",50,15,750]
[null,"3628000000-E","RIP RAP, CLASS I","","",2526,56.649643705463198,143097]
[null,"3635000000-E","RIP RAP, CLASS II","","",70,70,4900]
[null,"3642000000-E","RIP RAP, CLASS A","","",227,73.127753303964795,16600]
[null,"3649000000-E","RIP RAP, CLASS B","","",7660,50.424608355091401,386252.5]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",28785,2.8613166579815901,82363]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(A)","",626,35,21910]
[null,"","","(D)","",422,14,5908]
[null,"","","(E)","",397,14,5558]
[null,"","","(F)","",203,14,2842]
[null,"","","(MILEMARKER)","",4,25,100]
[null,"4048000000-E","REINF CONC FOUNDTN","","",15,663.33333333333303,9950]
[null,"4054000000-E","PLN CONC FOUNDTN","","",2,182.5,365]
[null,"4057000000-E","OVERHEAD FOOTING","","",44,910,40040]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",14908,5.0116447544942302,74713.600000000006]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",2681,2.75,7372.75]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",7233,6.4563915387805899,46699.08]
[null,"4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(233+00 -L-)","",1,51100,51100]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",50,129.4,6470]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",263,39.178707224334602,10304]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",131,85.118320610686993,11150.5]
[null,"4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",4,649.5,2598]
[null,"","","(B)","",2,49,98]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",53,832.45283018867894,44120]
[null,"","","(B)","",47,452.531914893617,21269]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",22,20.909090909090899,460]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",7,115,805]
[null,"","","(E)","",4,120,480]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",10,1011,10110]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",239,7.1359832635983302,1705.5]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",4,1,4]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",43,1.31395348837209,56.5]
[null,"4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",5,150,750]
[null,"4236000000-N","DISPOSE SIGN, A & B (GRD MTD)","","",66,63.575757575757599,4196]
[null,"4238000000-N","DISPOSE SIGN, D, E, F","","",90,3.1555555555555599,284]
[null,"4238500000-N","DISPOSE SIGN, MILEMKR","","",4,1,4]
[null,"4251000000-N","DISPOSE LIGHT SYSTEM","","",5,500,2500]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",8648,6.1070305272895498,52813.599999999999]
[null,"4402000000-E","HIGH VISIBILITY STAT SIGNS","","",314,8.8000000000000007,2763.2]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",928,18.620689655172399,17280]
[null,"4407000000-E","HIGH VISIBILITY PORT SIGNS","","",400,34.5,13800]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",1163,9.1447119518486701,10635.3]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",803,7.5,6022.5]
[null,"4415000000-N","FLASHING ARROW BOARD","","",8,381.26249999999999,3050.1]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",26,4650.9230769230799,120924]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",104,83.451923076923094,8679]
[null,"4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",23,3313.2608695652202,76205]
[null,"4424000000-N","WZ PRESENCE LIGHTING","","",72,1154.7777777777801,83144]
[null,"4430000000-N","DRUMS","","",1250,51.380800000000001,64226]
[null,"4432000000-N","HIGH VISIBILITY DRUMS","","",110,104,11440]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",104,154.538461538462,16072]
[null,"4445000000-E","BARRICADES (TYPE III)","","",1528,25.790575916230399,39408]
[null,"4447000000-E","PED CHANNEL DEVICES","","",50,30,1500]
[null,"4455000000-N","FLAGGER","","",633,346.63349131121601,219419]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",1,155860.91,155860.91]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",26,6336.09,164738.34]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",14,2940.9628571428598,41173.480000000003]
[null,"4480000000-N","TMA","","",13,11769.2307692308,153000]
[null,"4485000000-E","PORT CONC BARRIER","","",50188,40.633904519008503,2039334.4]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",1020,55.75,56865]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",54604,13.9958720972823,764230.6]
[null,"4510000000-N","LAW ENFORCEMENT","","",4904,54.099510603588897,265304]
[null,"4516000000-N","SKINNY DRUM","","",500,44.88,22440]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","CONNECTED LANE CLOSURE DEVICE","",4,1900.5,7602]
[null,"","","RAMP/LOOP CLOSURE","",2,587,1174]
[null,"","","RAMP/LOOP CLOSURES","",16,802.5,12840]
[null,"","","RAMP/LOOP TRAFFIC CONTROL","",18,1906.44444444444,34316]
[null,"","","SINGLE LANE CLOSURE","",240,2116.6666666666702,508000]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",3186,5.3737602008788397,17120.8]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",182403,0.85653185528747,156233.98000000001]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",967930,0.93127560877336002,901409.6]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",1489,2.64942914707858,3945]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",17421,2.0384019287067301,35511]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",36,125,4500]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",444,155.736486486486,69147]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",2411,2.8129821650767299,6782.1]
[null,"","","(IV)","",1672,2.4174641148325402,4042]
[null,"4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",215,25,5375]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",12,475,5700]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",41090,1.0044512046726699,41272.9]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",815515,0.20596157029607001,167964.75]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",620,1.0322580645161299,640]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",9945,0.52745098039215998,5245.5]
[null,"4830000000-E","PAINT PVT MKGS LINES 16\"","","",460,2,920]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",2276,3.0799648506151098,7010]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",28,25,700]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",479,29.302713987473901,14036]
[null,"4847400000-E","WZ PERF PVMT MKG LINES 4\"","","",185613,0.55000000000000004,102087.15]
[null,"4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",265551,0.67064895255525003,178091.5]
[null,"4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",4900,0.8,3920]
[null,"4848000000-E","WZ TRAF PATTERN MASKING","","",86280,0.65,56082]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",61190,0.51197091027945996,31327.5]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",13060,1.5,19590]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",160,3.1,496]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",3,100,300]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES,","12\", 20 MILS (STD GLASS BEADS)",256,8,2048]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",5819,3,17457]
[null,"","","","20 MILS (STANDARD GLASSBEADS)",800,4.0999999999999996,3280]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",16885,2.8397986378442401,47950]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",460,12,5520]
[null,"","","","LINES (24\", 90 MILS)",1954,11.823439099283499,23103]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",3030,37.233003300329997,112816]
[null,"","","","PAVEMENT MARKERS",4066,35.359075258239102,143770]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",4347,5.1964113181504503,22588.799999999999]
[null,"4940000000-N","FLEX DELINATR (YELLOW)","","",20,55,1100]
[null,"4955000000-N","OBJECT MARKERS (END OF RD)","","",6,180,1080]
[null,"5005000000-E","80' HIGH MOUNT STANDARD","","",2,26500,53000]
[null,"5010000000-E","100' HIGH MOUNT STANDARD","","",5,29680,148400]
[null,"5020000000-N","PORTABLE DRIVE UNIT","","",1,3815,3815]
[null,"5025000000-E","HIGH MOUNT FOUNDATIONS","","",48,1450,69600]
[null,"5070000000-N","STD FOUNDAT ***********","(R1)","",6,850,5100]
[null,"","","(R2)","",1,875,875]
[null,"5120000000-N","SERVICE POLE ************","(30', CLASS 4)","",1,3500,3500]
[null,"5125000000-E","SERVICE LATERAL *********","(3 1/0 USE)","",25,40,1000]
[null,"5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",370,6,2220]
[null,"5160000000-E","ELECT DUCT JA, SIZE *****","(3\")","",530,17,9010]
[null,"","","(4\")","",260,21,5460]
[null,"5170000000-E","**-#8 W/G FEEDER CIRCUIT","(2)","",320,2.5,800]
[null,"5175000000-E","**-#6 W/G FEEDER CIRCUIT","(2)","",420,3,1260]
[null,"5180000000-E","**-#4 W/G FEEDER CIRCUIT","(2)","",320,4,1280]
[null,"5205000000-E","**-#8 W/G FEEDR N *****\"","(2, 1.5\")","",2385,8,19080]
[null,"5210000000-E","**-#6 W/G FEEDR N *****\"","(2, 1.5\")","",3535,8.65,30577.75]
[null,"5215000000-E","**-#4 W/G FEEDER N *****\"","(2, 1.5\")","",2315,9.65,22339.75]
[null,"5240000000-N","ELEC JB ************","(CS36)","",1,950,950]
[null,"","","(HM18)","",7,350,2450]
[null,"","","(HM36)","",1,950,950]
[null,"","","(IG18)","",9,350,3150]
[null,"","","(IG36)","",6,950,5700]
[null,"","","(LS18)","",8,350,2800]
[null,"5255000000-N","PORTABLE LIGHTING","","",3,121771.23,365313.69]
[null,"5260000000-N","GENERIC LIGHTING ITEM (LS)","EQUIPMENT STORAGE","",1,750,750]
[null,"5270000000-N","GENERIC LIGHTING ITEM (EA)","100' HIGH MOUNT LUMINAIRE -   LED","",18,1500,27000]
[null,"","","80' HIGH MOUNT LUMINAIRE - LED","",16,1700,27200]
[null,"","","CONTROL NODE","",34,200,6800]
[null,"","","LIGHTING CONTROL SYSTEM","",1,14000,14000]
[null,"","","REFURBISH SINGLE ARM LIGHT STAN- DARD","",7,1250,8750]
[null,"","","REINSTALL COMMUNICATION GATE- WAY","",1,1600,1600]
[null,"","","RELOCATE SINGLE ARM LIGHT     STANDARD","",7,1400,9800]
[null,"","","REMOVE CONTROL SYSTEM","",1,100,100]
[null,"","","REMOVE HIGH MOUNT LIGHT       STANDARD","",3,4000,12000]
[null,"","","REMOVE HIGH MOUNT STANDARD    FOUNDATION","",3,2000,6000]
[null,"","","REMOVE LIGHT STANDARD","",19,400,7600]
[null,"","","REMOVE LIGHT STANDARD FOUNDA- TION","",19,400,7600]
[null,"5325200000-E","2\" WATER LINE","","",875,12,10500]
[null,"5325600000-E","6\" WATER LINE","","",3209,38.3072608289187,122928]
[null,"5325800000-E","8\" WATER LINE","","",408,75.647058823529406,30864]
[null,"5326200000-E","12\" WATER LINE","","",8854,52.175400948723698,461961]
[null,"5326600000-E","16\" WATER LINE","","",8480,91,771680]
[null,"5327400000-E","24\" WATER LINE","","",1520,151,229520]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",58003,6.7221781631984596,389906.5]
[null,"5536000000-E","2\" VALVE","","",1,1040,1040]
[null,"5540000000-E","6\" VALVE","","",8,1391.25,11130]
[null,"5546000000-E","8\" VALVE","","",6,1785,10710]
[null,"5558000000-E","12\" VALVE","","",5,3350,16750]
[null,"5558600000-E","16\" VALVE","","",5,8690,43450]
[null,"5589200000-E","2\" AIR RELEASE VALVE","","",2,3105,6210]
[null,"5648000000-N","RELOCATE WATER METER","","",3,980,2940]
[null,"5649000000-N","RECONNECT WATER METER","","",7,680,4760]
[null,"5666000000-N","FIRE HYDRANT","","",10,4316,43160]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",4,470,1880]
[null,"5673000000-E","FIRE HYDRANT LEG","","",125,73.400000000000006,9175]
[null,"5686500000-E","WATER SERVICE LINE","","",243,23.039506172839499,5598.6]
[null,"5691500000-E","12\" SANITARY GRAVITY SEWER","","",412,62,25544]
[null,"5709200000-E","4\" FORCE MAIN SEWER","","",2358,15.5,36549]
[null,"5709300000-E","6\" FORCE MAIN SEWER","","",2061,21,43281]
[null,"5709400000-E","8\" FORCE MAIN SEWER","","",1052,20,21040]
[null,"5709500000-E","10\" FORCE MAIN SEWER","","",1247,41,51127]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",5610,10.203208556149701,57240]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",3,3610,10830]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(2\")","",999,4.5999999999999996,4595.3999999999996]
[null,"","","(4\")","",2218,4.3,9537.4]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",4732,5.4841081994928098,25950.799999999999]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",1871,17.680277926242599,33079.800000000003]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",1279,5,6395]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",8112,9.0031434911242592,73033.5]
[null,"5810000000-E","ABANDON 16\" UTILITY PIPE","","",7813,5.15,40236.949999999997]
[null,"5813000000-E","ABANDON 24\" UTILITY PIPE","","",602,6.5,3913]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",2,1200,2400]
[null,"5835000000-E","**\" ENCASEMENT PIPE","(14\")","",759,79,59961]
[null,"","","(26\")","",488,155,75640]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",247,83,20501]
[null,"5835900000-E","20\" ENCASEMENT PIPE","","",454,111,50394]
[null,"5836400000-E","36\" ENCASEMENT PIPE","","",239,250,59750]
[null,"5872500000-E","BORE & JACK **\"","(14\")","",507,144.13,73073.91]
[null,"","","(16\")","",247,255,62985]
[null,"","","(20\")","",311,163.19999999999999,50755.199999999997]
[null,"","","(26\")","",180,281.97000000000003,50754.6]
[null,"","","(36\")","",199,323.08999999999997,64294.91]
[null,"5872600000-E","DIRECT DRILL **\"","(12\")","",2290,88.873362445414898,203520]
[null,"","","(18\")","",300,165,49500]
[null,"","","(6\")","",631,65,41015]
[null,"","","(8\")","",829,75,62175]
[null,"5882000000-N","GENERIC UTILITY ITEM (EA)","12\" INSERTION VALVE","",3,20316.666666666701,60950]
[null,"","","6\" INSERTION VALVE","",2,1000,2000]
[null,"","","8\" INSERTION VALVE","",2,1000,2000]
[null,"","","ADJUSTABLE  HYDRAULIC JACK","",1,2750,2750]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",167765,2.1200637796918298,355672.5]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",3990,37.741854636591498,150590]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",19225,30.654356306892101,589330]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",13480,26.7006676557864,359925]
[null,"6015000000-E","TEMPORARY MULCHING","","",396,779.35606060606096,308625]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",16600,3.37861445783133,56085]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",88,879.80681818181802,77423]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",11687,12.392102335928801,144826.5]
[null,"6029000000-E","SAFETY FENCE","","",19672,2.1437322082147201,42171.5]
[null,"6030000000-E","SILT EXCAVATION","","",85040,4.0510348071500002E-2,3445]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",170120,1.41130672466494,240091.5]
[null,"6037000000-E","COIR FIBER MAT","","",2995,6.1561769616026698,18437.75]
[null,"6038000000-E","PERM SOIL REINF MAT","","",3730,4.6777479892761402,17448]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",23190,4.8514877102199199,112506]
[null,"6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",1750,4.2428571428571402,7425]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",1370,17.578467153284699,24082.5]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",24,713.16666666666697,17116]
[null,"6071010000-E","WATTLE","","",5270,6.3449715370019,33438]
[null,"6071012000-E","COIR FIBER WATTLE","","",13440,4.8656249999999996,65394]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",12785,3.77219397731717,48227.5]
[null,"6071030000-E","COIR FIBER BAFFLE","","",23865,4.4580452545568798,106391.25]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",81,866.79012345678996,70210]
[null,"","","(2\")","",6,1128.3333333333301,6770]
[null,"","","(2-1/2\")","",3,1100,3300]
[null,"6084000000-E","SEEDING AND MULCHING","","",288.2,1949.34247050659,561800.5]
[null,"6087000000-E","MOWING","","",285.5,108.83362521891399,31072]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",4200,10.8059523809524,45385]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",13,1159.3269230769199,15071.25]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",6550,5.0782442748091601,33262.5]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",193.75,836.27741935483903,162028.75]
[null,"6111000000-E","IMPERVIOUS DIKE","","",1210,59.421487603305799,71900]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",90,94.2222222222222,8480]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",525,135.95238095238099,71375]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",45,828.88888888888903,37300]
[null,"6120000000-E","CULVERT DIVERSION CHANNEL","","",631,40.923930269413603,25823]
[null,"6123000000-E","REFORESTATION","","",2.1,3476.1904761904798,7300]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",2.15,10200,21930]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",16,242,3872]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",8,242,1936]
[null,"7060000000-E","SIGNAL CABLE","","",15430,2.0715489306545698,31964]
[null,"7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",8,355,2840]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",21,646.61904761904805,13579]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",2,864,1728]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",3,1171,3513]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",1715,2.9674927113702601,5089.25]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",1310,6.4839694656488502,8494]
[null,"","","(3, 2\")","",40,10.7,428]
[null,"7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",5200,4.0999999999999996,21320]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",760,21.6184210526316,16430]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",26,393.461538461538,10230]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",7,501,3507]
[null,"7360000000-N","WOOD POLE","","",9,1215,10935]
[null,"7372000000-N","GUY ASSEMBLY","","",14,394,5516]
[null,"7384000000-E","***\" RISER WITH **************","(1-1/2\", WEATHERHEAD)","",3,610,1830]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",2,1215,2430]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",14,511.357142857143,7159]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",11430,5.9122922134733198,67577.5]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",18790,1.3499201703033501,25365]
[null,"7481000000-N","SITE SURVEY","","",1,1492,1492]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",2,4240,8480]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",1,4942,4942]
[null,"7636000000-N","SIGN FOR SIGNALS","","",5,307.8,1539]
[null,"7642300000-N","TYPE III PED W/ FOUNDATION","","",4,5055,20220]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",1,783,783]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070E, BASE MOUNTED)","",1,13188,13188]
[null,"","","(TYPE 2070E, POLE MOUNTED)","",2,13000,26000]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",14,130,1820]
[null,"7780000000-N","DETECTOR CARD (TYPE 2070L)","","",9,121,1089]
[null,"7901000000-N","CABINET BASE EXTENDER","","",1,335,335]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","5/8\"X10' GROUNDING ELECTRODES","",30,91,2730]
[null,"","","CCTV CAMERA  LOWERING SYSTEM","",1,6263,6263]
[null,"","","CCTV CAMERA ASSEMBLY","",1,4253,4253]
[null,"","","CCTV EXTENSION POLE","",1,4245,4245]
[null,"","","CCTV METAL POLE (60')","",1,16200,16200]
[null,"","","CCTV WOOD POLE","",2,4170.5,8341]
[null,"","","DIGITAL CCTV CAMERA  ASSEMBLY","",3,6100,18300]
[null,"","","DMS ACCESS LADDER","",2,5900,11800]
[null,"","","DMS PEDESTAL STRUCTURE","",2,48500,97000]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE 2C)","",4,123250,493000]
[null,"","","EQUIPMENT CABINET DISCONNECT","",4,1550,6200]
[null,"","","ETHERNET EDGE SWITCH","",1,1423,1423]
[null,"","","FIELD EQUIPMENT CABINET","",3,5006.6666666666697,15020]
[null,"","","GROUNDING SYSTEM","",1,2177,2177]
[null,"","","METER BASE/DISCONNECT COMBI-","NATION PANEL",1,912,912]
[null,"","","METER BASE/DISCONNECT COMBINA-","TION PANEL",4,2100,8400]
[null,"","","REMOVAL AND DISPOSAL OF","EXISTING DMS COMPONENTS",2,5500,11000]
[null,"","","SOIL TEST","",1,3400,3400]
[null,"","","VARIABLE SPEED DRILL","",1,1900,1900]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","4 SOLID BARE COPPER GROUNDING","CONDUCTOR",300,6,1800]
[null,"","","3 WIRE COPPER FEEDER CON-     DUCTORS","",430,3,1290]
[null,"","","3-WIRE COPPER FEEDER CONDUC-","TORS",500,5,2500]
[null,"","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",90,3.5,315]
[null,"","","4-WIRE COPPER FEEDER CONDUC-","TORS",400,6,2400]
[null,"","","ETHERNET CABLE","",100,2.6,260]
[null,"7992000000-E","GENERIC SIGNAL ITEM (CY)","DRILLED PIER FOUNDATION","",6,1100,6600]
[null,"","","OVERHEAD FOOTINGS","",16,1100,17600]
[null,"8007000000-N","CM&R TEMP STR ***********","(15+60.50-DET-)","",1,350000,350000]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(15+61.00-L-)","",1,40000,40000]
[null,"","","(16+99.00 -L-)","",1,81817.240000000005,81817.240000000005]
[null,"","","(17+00.00-L-)","",1,50000,50000]
[null,"8021000000-N","REMV EXIST STR **********","(19+07.12 -L-)","",1,180000,180000]
[null,"","","(28+02.81 -L-)","",1,183000,183000]
[null,"8035000000-N","REMV EXIST STR **********","(15+61.00-L-)","",1,110000,110000]
[null,"","","(16+10.00 -L-)","",1,45000,45000]
[null,"","","(16+99.00 -L-)","",1,165000,165000]
[null,"","","(17+00.00-L-)","",1,100000,100000]
[null,"","","(17+07.50 -Y2-)","",1,212000,212000]
[null,"","","(17+37.36 -L-)","",1,512000,512000]
[null,"","","(42+87.26 -Y1-)","",1,168000,168000]
[null,"8056000000-N","REMV EXIST STR **********","(28+84.00 -Y7-)","",1,22000,22000]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",7,1945.7142857142901,13620]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 19+07.12 -L-)","",1,13500,13500]
[null,"","","(1, 42+88.27 -Y1-)","",1,39500,39500]
[null,"8096000000-E","PILE EXCAVATION IN SOIL","","",201,270,54270]
[null,"8097000000-E","PILE EXCAVATION NOT IN SOIL","","",31,260,8060]
[null,"8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",45,1466,65970]
[null,"8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",86.2,725,62495]
[null,"8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",51,1466,74766]
[null,"8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",16,725,11600]
[null,"8112730000-N","PDA TESTING","","",15,2529.3333333333298,37940]
[null,"8113000000-N","SID INSPECTIONS","","",2,650,1300]
[null,"8114000000-N","SPT TESTING","","",1,800,800]
[null,"8115000000-N","CSL TESTING","","",2,5000,10000]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(15+61.00-L-)","",1,40000,40000]
[null,"","","(16+10.00 -L-)","",1,16000,16000]
[null,"","","(16+99.00 -L-)","",1,5000,5000]
[null,"","","(17+00.00-L-)","",1,40000,40000]
[null,"","","(17+37.36 -L-)","",1,24000,24000]
[null,"","","(19+07.12 -L-)","",1,42500,42500]
[null,"","","(28+02.81 -L-)","",1,48000,48000]
[null,"8126000000-N","CULV EXCAV @ ************","(155+30.40 -L-)","",1,5100,5100]
[null,"","","(28+84.00 -Y7-)","",1,36000,36000]
[null,"","","(45+66.22 -L-)","",1,15700,15700]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",486,51,24786]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",74623,39.089650643903298,2916987]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",76851,1.0183928641136699,78264.509999999995]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",1185.5,1044.2746520455501,1237987.6000000001]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",858.7,570,489459]
[null,"8210000000-N","BRG APPR SLAB ***********","(15+61.00-L-)","",1,35000,35000]
[null,"","","(16+10.00 -L-)","",1,25000,25000]
[null,"","","(16+99.00 -L-)","",1,51000,51000]
[null,"","","(17+00.00-L-)","",1,45000,45000]
[null,"","","(17+37.36 -L-)","",1,50000,50000]
[null,"","","(19+07.12 -L-)","",1,41000,41000]
[null,"","","(217+31.76 -L-) LT","",1,70000,70000]
[null,"","","(217+31.76 -L-) RT","",1,64000,64000]
[null,"","","(27+01.91 -Y7-)","",1,46000,46000]
[null,"","","(28+02.81 -L-)","",1,39000,39000]
[null,"","","(42+56.82 -Y1-)","",1,64000,64000]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",189930,1.4256163849839401,270767.32]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",9843,2.5401554404145101,25002.75]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",100414,1.35,135558.9]
[null,"8259000000-E","36\" PRESTR CONCRETE GIRDR","","",431,250,107750]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",4290.68,342.64056746249997,1470161.03]
[null,"8274000000-E","63\" MOD PRESTR CONC GIRDR","","",1143.33,385,440182.05]
[null,"8280000000-E","STRUCTURAL STEEL","","",896000,2.0457589285714302,1833000]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",199,995.47738693467295,198100]
[null,"","","(HP 14 X 73)","",11,2000,22000]
[null,"","","(HP12X53)","",24,2500,60000]
[null,"8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",8,1250,10000]
[null,"","","(PP 24 X 0.50)","",6,2500,15000]
[null,"","","(PP 30 X 0.50)","",15,4000,60000]
[null,"","","(PP 36 X 0.625)","",5,2500,12500]
[null,"8364000000-E","HP12X53 PILES","","",11994,51.9092796398199,622599.9]
[null,"8384000000-E","HP14X73 PILES","","",1152,73.7152777777778,84920]
[null,"8385200000-E","PP**X**** GALV STL PILE","(24 X 0.50)","",480,139,66720]
[null,"","","(30 X 0.50)","",1300,228.507884615385,297060.25]
[null,"","","(36 x 0.625)","",550,350,192500]
[null,"8391000000-N","STEEL PILE POINTS","","",35,173.57142857142901,6075]
[null,"8392000000-N","PIPE PILE PLATES","","",6,400,2400]
[null,"8393000000-N","PILE REDRIVES","","",82,121.342682926829,9950.1]
[null,"8475000000-E","TWO BAR METAL RAIL","","",369.44,110,40638.400000000001]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",3245.45,105.06498328428999,340983.15]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",180.5,130,23465]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 3'-3\")","",385.55,180,69399]
[null,"8524000000-E","**\" CHAIN LINK FENCE","(72\")","",264,180,47520]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",4569,106.913219522872,488486.5]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",2606,58.1582003069839,151560.26999999999]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2837,3.01824109975326,8562.75]
[null,"8654000000-N","DISC BEARINGS","","",1,38000,38000]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",7,12100,84700]
[null,"8692000000-N","FOAM JOINT SEALS","","",2,30900,61800]
[null,"8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",990,145,143550]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",19233,54,1038582]
[null,"","","(2)","",21981,53,1164993]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FIBER OPTIC CONDUIT SYSTEM","WITH HANGERS",832,122,101504]
[null,"","","","",1477.78,42.464703812475499,62753.49]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","ASPHALT JOINT REPAIR/REPLACE-","MENT (18\"-24\" WIDE, W/ PLATE)",6,10395,62370]

{"sheet":"ITEMS - DIV 05","index":7,"n_rows":118,"n_cols":8,"rows_kept":118,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 05"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",23,123895.43478260899,2849595]
[null,"0106000000-E","BORROW EXCAVATION","","",14704,32.670403971708403,480385.62]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",195,13,2535]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",30,91,2730]
[null,"0170000000-E","REMOVAL OF CONC PVMT SLBS","","",500,191,95500]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",250,5,1250]
[null,"0264000000-E","GENERIC GRADING ITEM (SMI)","SHOULDER GRADING","",588.24,2679.9499184006499,1576453.74]
[null,"1099500000-E","SHALLOW UNDERCUT","","",84,37.5,3150]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",173,39.5,6833.5]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",150,64.5,9675]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",13507,50.835910268749501,686640.64000000001]
[null,"1260000000-E","AGGREGATE SHOULDER BORROW","(ASB)","",107,30,3210]
[null,"","","","",39403,18.523970256071902,729900]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",1790887,1.50470216713841,2694751.55]
[null,"","","(1-1/4\")","",28213,2.6895012937298399,75878.899999999994]
[null,"","","(2\")","",244389,1.5420957162556399,376871.23]
[null,"","","(2-1/2\")","",34203,2.4,82087.199999999997]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1\")","",380,7.85,2983]
[null,"","","(0\" TO 1\"-1/2\")","",607,8.61,5226.2700000000004]
[null,"","","(0\" TO 1-1/2\")","",15902,4.7969538422839904,76281.16]
[null,"","","(0\" TO 1-1/4\")","",1378,12.4807692307692,17198.5]
[null,"","","(1-1/2\" TO 3\")","",29395,1.95,57320.25]
[null,"1330000000-E","INCIDENTAL MILLING","","",128864,7.4151895021107501,955550.98]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",200,208,41600]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",4943,40,197720]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",390870,41.553063934300397,16241846.1]
[null,"1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",398,144.339824120603,57447.25]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",131193,38.771849107803,5086595.2]
[null,"1575000000-E","ASP FOR PLANT MIX","","",34764.9,432.30155127729398,15028920.199999999]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",82107,107.49503708575401,8826095.0099999998]
[null,"1803500000-E","AST, DOUBLE SEAL","","",489562,0.75240847941628997,368350.6]
[null,"1820000000-E","AST, FOG SEAL","","",381733,0.23202832870095,88572.87]
[null,"1838000000-E","EMULSION FOR AST","","",269262,1.65774613573397,446368.04]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",35805,0.2,7161]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","LATEX MODIFIED MICROSURFACING,TYPE III","",140119,2.29,320872.51]
[null,"","","MULTI-USE PATH REPAIR","",15,112.25,1683.75]
[null,"2484000000-E","GENERIC DRAINAGE ITEM (LF)","CONCRETE FLUME WITH GRATE","",100,82,8200]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",10491,54.729387093699401,574166]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",1269,59.184003152088302,75104.5]
[null,"2600000000-N","RETROFIT EXT CURB RAMPS","","",268,544.02985074626895,145800]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",46,2341.3043478260902,107700]
[null,"2613000000-N","REM & REP CURB RAMPS","","",545,2346.9724770642201,1279100]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",180,62,11160]
[null,"2738000000-E","GENERIC PAVING ITEM (SY)","REMOVE AND REPLACE DRIVEWAY","APRON",1,100,100]
[null,"","","REMOVE AND REPLACE DRIVEWAY   APRON","",225,125,28125]
[null,"","","REMOVE CONCRETE ISLAND","",3,100,300]
[null,"","","REMOVE CONCRETE SIDEWALK","",64,43.90625,2810]
[null,"","","REMOVE SIDEWALK","",25,37,925]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","REMOVE 2'-6\" CURB AND GUTTER","",115,30,3450]
[null,"","","REMOVE AND REPLACE 2'-6\" CURB AND GUTTER","",769,67.3992197659298,51830]
[null,"2759000000-N","GENERIC PAVING ITEM (EA)","REMOVE CURB RAMP","",120,925.08333333333303,111010]
[null,"","","REMOVE CURB RAMPS","",47,879.787234042553,41350]
[null,"2800000000-N","ADJ CATCH BASINS","","",2,750,1500]
[null,"2815000000-N","ADJ DROP INLETS","","",5,750,3750]
[null,"2830000000-N","ADJ MANHOLES","","",418,572.53588516746402,239320]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",324,556.85185185185196,180420]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",27,18.3888888888889,496.5]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",48,6.484375,311.25]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",29,119.827586206897,3475]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",2,135,270]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(E)","",5,420,2100]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",46946,5.9073179823627102,277324.95]
[null,"4447000000-E","PED CHANNEL DEVICES","","",1296,35.848765432098801,46460]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",23,88708.772173913094,2040301.76]
[null,"4510000000-N","LAW ENFORCEMENT","","",4160,53.221153846153797,221400]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICE","",40,167.5,6700]
[null,"","","AUDIBLE WARNING DEVICES","",19,276.31578947368399,5250]
[null,"","","PEDESTRIAN TRANSPORT SERVICE  (PER TRIP)","",254,95.708661417322801,24310]
[null,"","","TEMPORARY CURB RAMPS","",3,1500,4500]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",6098488,0.48382659767469999,2950610.7]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",51250,1.05326341463415,53979.75]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",55811,1.82885094336242,102070]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",12884,2.5742781744799799,33167]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",804,91.330845771144297,73430]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",2400,126.60625,303855]
[null,"4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",79,279.49367088607602,22080]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",2927,3.1212845917321501,9136]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",300,9.5,2850]
[null,"4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",191,25.151832460733001,4804]
[null,"4800000000-N","COLD APP PLAS CHAR TYPE *","(II)","",14,147.857142857143,2070]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",26,217.69230769230799,5660]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",1080176,0.12127258891143999,130995.74]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",50626,0.20141231778138,10196.700000000001]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",27290,0.51398497618174999,14026.65]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",8340,0.62901678657074001,5246]
[null,"4830000000-E","PAINT PVT MKGS LINES 16\"","","",450,1.1111111111111101,500]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",10154,2.1490299389403198,21821.25]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",305,29.386885245901599,8963]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",1191,30.5037783375315,36330]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",275574,0.21567143489589,59433.440000000002]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",1128,2.4698581560283701,2786]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",55,3.83636363636364,211]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",14,30.6071428571429,428.5]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","HOT SPRAY PLASTIC PAVEMENT","MARKING LINES (4\", 50 MILS)",3210,0.72,2311.1999999999998]
[null,"","","HOT SPRAY THERMOPLASTIC       PAVEMENT","MARKING LINES (4\", 50 MILS)",1470,3.25,4777.5]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES (4\",       50 MILS)",480,7.99,3835.2]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES(4\", 50MILS)",2914,1.5,4371]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES, (4\",      50 MILS)",7297,1.50829107852542,11006]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES, 4\",       50 MILS",1300,1,1300]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES, 4\",       50MILS",2764,1.5,4146]
[null,"","","HOT SPRAY THERMOPLASTIC PAVEM-","ENT MARKING LINES, 4\", 50 MIL",531374,0.28075524959821002,149186.04]
[null,"","","","ENT MARKING LINES, 4\", 50 MILS",337133,0.3,101139.9]
[null,"","","POLYUREA  PAVEMENT MARKING    LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",1490,3,4470]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",1172,6.8319112627986298,8007]
[null,"","","","LINES (16\", 90MILS)",80,7,560]
[null,"","","","LINES (24\", 90 MILS)",25522,9.6734777838727393,246886.5]
[null,"","","","LINES (24\", 90MILS)",672,7.4229166666666702,4988.2]
[null,"","","THERMOPLASTIC PAVMENT MARKING","LINES (24\", 90 MILS)",50,25,1250]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",13566,31.745540321391701,430660]
[null,"5255000000-N","PORTABLE LIGHTING","","",3,31750,95250]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",21303,2.8444115852227401,60594.5]
[null,"6071010000-E","WATTLE","","",53454,6.0538219777752804,323601]
[null,"6084000000-E","SEEDING AND MULCHING","","",203.79,2315.0179105942402,471777.5]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",159,277.35849056603797,44100]
[null,"6900000000-E","TOPSOIL","","",130,70,9100]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",108850,6.5412395957739999,712013.93]

{"sheet":"ITEMS - DIV 06","index":8,"n_rows":884,"n_cols":8,"rows_kept":884,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 06"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",7,2412509.0428571398,16887563.300000001]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",7,497985.71428571403,3485900]
[null,"0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN AND CONSTRUCTION","I-6064A",1,240488250,240488250]
[null,"","","","I-6064B",1,114376950,114376950]
[null,"","","","I-6064C / I-5879",1,77834800,77834800]
[null,"0001000000-E","CLEARING & GRUBBING","","",29,414448.27586206899,12019000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",7,5143.4285714285697,36004]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",543000,9.0317127071823204,4904220]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(1260+34.00 -L-)","",1,75000,75000]
[null,"","","(1391+19.65 -L-)","",1,125000,125000]
[null,"","","(16+92.70 -L-)","",1,49200,49200]
[null,"","","(21+37.00 -L REV-)","",1,15675,15675]
[null,"","","(30+65.33 -Y1B-)","",1,43641.94,43641.94]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(1002+79.68 -L REV-)","",1,105000,105000]
[null,"","","(26+05.28 -Y14-)","",1,100000,100000]
[null,"","","(26+80.73 -Y17-)","",1,65000,65000]
[null,"","","(27+09.19 -Y16-)","",1,75000,75000]
[null,"","","(28+39.21 -Y29-)","",1,35000,35000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",110000,9.1814545454545495,1009960]
[null,"0043000000-N","GRADING","","",2,174535,349070]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",2,1.05,2.1]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",600,18.0833333333333,10850]
[null,"0063000000-N","GRADING","","",1,781000,781000]
[null,"0106000000-E","BORROW EXCAVATION","","",1489290,8.8411659247023699,13167060]
[null,"0127000000-N","EMBM'T SETTLEMENT GAUGE","","",4,2000,8000]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",40645,17.692766637962901,719122.5]
[null,"0141000000-E","BERM DITCH CONSTRUCTION","","",2055,8,16440]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",348960,11.194146893626799,3906309.5]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",630,11,6930]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",44225,3,132675]
[null,"0192000000-N","PROOF ROLLING","","",175,225,39375]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",64900,12.9876733436056,842900]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",34150,6.0281844802342599,205862.5]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",743050,1.5192046295673201,1128845]
[null,"0199000000-E","TEMPORARY SHORING","","",45642,45.530125761360203,2078086]
[null,"0220000000-E","ROCK EMBANKMENTS","","",1925,62,119350]
[null,"0222000000-E","GEOTEXTILE ROCK EMBANK","","",2090,2.99425837320574,6258]
[null,"0225000000-E","REINFORCED SOIL SLOPES","","",650,64.5,41925]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",900,79.5555555555556,71600]
[null,"","","RIP RAP, CLASS A","",260,42.9,11154]
[null,"","","RIP RAP, CLASS II","",925,51.7,47822.5]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",21717,46.711101901736001,1014425]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",79499,2.8372822299651599,225561.1]
[null,"0335000000-E","**\" DRAINAGE PIPE","(4\")","",100,25,2500]
[null,"","","(54\")","",828,309.06280193236699,255904]
[null,"","","(66\")","",52,650,33800]
[null,"0335100000-E","12\" DRAINAGE PIPE","","",52,145,7540]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",3300,69.477575757575806,229276]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",980,92.942857142857093,91084]
[null,"0335400000-E","24\" DRAINAGE PIPE","","",1036,92.729729729729698,96068]
[null,"0335500000-E","30\" DRAINAGE PIPE","","",920,138.77608695652199,127674]
[null,"0335600000-E","36\" DRAINAGE PIPE","","",252,148.76190476190499,37488]
[null,"0335700000-E","42\" DRAINAGE PIPE","","",908,211.442731277533,191990]
[null,"0335800000-E","48\" DRAINAGE PIPE","","",580,266.420689655172,154524]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(12\")","",2,304,608]
[null,"","","(15\")","",10,430,4300]
[null,"","","(30\")","",4,710,2840]
[null,"0342000000-E","**\" SIDE DRAIN PIPE","(12\")","",20,40,800]
[null,"","","(30\")","",1128,89.971631205673802,101488]
[null,"","","(36\")","",596,115,68540]
[null,"","","(42\")","",496,140,69440]
[null,"","","(48\")","",256,175,44800]
[null,"","","(54\")","",52,230,11960]
[null,"","","(60\")","",48,250,12000]
[null,"","","(66\")","",372,350,130200]
[null,"","","(84\")","",76,450,34200]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",16456,47.255590666018499,777638]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",8292,57.276410998552798,474936]
[null,"0345000000-E","24\" SIDE DRAIN PIPE","","",5356,71.940253920836497,385312]
[null,"0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",14,350,4900]
[null,"0354000000-E","***\" RC PIPE CULV *****","(15\", V)","",180,50,9000]
[null,"","","(18\", V)","",300,55,16500]
[null,"","","(24\", CLASS V)","",128,91,11648]
[null,"","","(24\", V)","",1068,80,85440]
[null,"","","(36\", CLASS V)","",280,155,43400]
[null,"","","(36\", V)","",44,170,7480]
[null,"","","(42\", V)","",592,190,112480]
[null,"","","(48\", V)","",48,290,13920]
[null,"","","(54\", V)","",164,320,52480]
[null,"","","(66\", V)","",100,1015,101500]
[null,"0366000000-E","15\" RC PIPE CULV III","","",720,77.405555555555594,55732]
[null,"0372000000-E","18\" RC PIPE CULV III","","",1172,65.938566552900994,77280]
[null,"0378000000-E","24\" RC PIPE CULV III","","",212,113.39622641509401,24040]
[null,"0384000000-E","30\" RC PIPE CULV III","","",1604,93.411471321695799,149832]
[null,"0390000000-E","36\" RC PIPE CULV III","","",1312,112.673780487805,147828]
[null,"0396000000-E","42\" RC PIPE CULV III","","",112,145,16240]
[null,"0402000000-E","48\" RC PIPE CULV III","","",484,207.06611570247901,100220]
[null,"0408000000-E","54\" RC PIPE CULV III","","",300,284.66000000000003,85398]
[null,"0414000000-E","60\" RC PIPE CULV III","","",520,166.461538461538,86560]
[null,"0420000000-E","66\" RC PIPE CULV III","","",48,652,31296]
[null,"0426000000-E","72\" RC PIPE CULV III","","",40,718,28720]
[null,"0438000000-E","84\" RC PIPE CULV III","","",208,550,114400]
[null,"0448000000-E","***\" RCP CULV CLASS IV","(48\")","",1804,261.749445676275,472196]
[null,"","","(54\")","",1612,373.84615384615398,602640]
[null,"","","(60\")","",776,350,271600]
[null,"","","(66\")","",404,490,197960]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",44432,67.709985595966899,3008490.08]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",12228,74.070657507360195,905736]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",17360,89.518433179723502,1554040]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",5536,118.114161849711,653880]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",4224,167.197916666667,706244]
[null,"0448700000-E","42\" RCP CULV CLASS IV","","",5036,167.79189833200999,845000]
[null,"0453000000-E","**\" PIPE END SECTION","(15\")","",1,1650,1650]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",100,71.012799999999999,7101.28]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",94,653.55808510638303,61434.46]
[null,"","","(18\", 0.064\")","",9,650,5850]
[null,"","","(24\", 0.064\")","",6,450,2700]
[null,"","","(30\", 0.079\")","",4,900,3600]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(16\", 0.281\")","",318,355,112890]
[null,"","","(18\", 0.312\")","",258,410,105780]
[null,"","","(18\", 0.500\")","",524,340,178160]
[null,"","","(24\", 0.375\")","",376,496,186496]
[null,"","","(30\", 0.469\")","",290,516,149640]
[null,"","","(36\", 0.532\")","",478,623,297794]
[null,"","","(42\", 0.625\")","",394,735,289590]
[null,"","","(48\", 0.688\")","",910,868,789880]
[null,"","","(54\", 0.781\")","",54,1150,62100]
[null,"","","(60\", 0.844\")","",636,1235,785460]
[null,"","","(66\", 0.938\")","",466,1886,878876]
[null,"","","(72\", 1.000\")","",84,5054,424536]
[null,"","","(84\", 1.000\")","",122,2370,289140]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(16\", 0.281\")","",318,0.01,3.18]
[null,"","","(18\", 0.312\")","",258,0.01,2.58]
[null,"","","(24\", 0.375\")","",376,0.01,3.76]
[null,"","","(24\", 0.500\")","",92,363,33396]
[null,"","","(30\", 0.469\")","",290,0.01,2.9]
[null,"","","(36\", 0.532\")","",478,0.01,4.78]
[null,"","","(42\", 0.625\")","",394,0.01,3.94]
[null,"","","(48\", 0.688\")","",910,0.01,9.1]
[null,"","","(54\", 0.781\")","",54,0.01,0.54]
[null,"","","(60\", 0.844\")","",636,0.01,6.36]
[null,"","","(66\", 0.938\")","",466,0.01,4.66]
[null,"","","(72\", 1.000\")","",84,5054,424536]
[null,"","","(84\", 1.000\")","",122,0.01,1.22]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","16\" SEALED DIP, CLASS 250","",284,120,34080]
[null,"","","18\" SEALED DIP, CLASS 250","",216,150,32400]
[null,"","","36\" DUCTILE IRON PIPE, CLASS","150 (SEALED)",148,330,48840]
[null,"","","36\" SEALED DIP, CLASS 150","",704,220,154880]
[null,"","","4\" PVC IRRIGATION CONDUIT","",1276,27,34452]
[null,"","","4\" PVC SLEEVE","",950,19.5,18525]
[null,"","","42\" DUCTILE IRON PIPE, CLASS","150 (SEALED)",188,499,93812]
[null,"","","60\" SEALED DIP, CLASS 150","",580,150,87000]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","BOOTS FOR SEALED DRAINAGE","STRUCTURES",9,725,6525]
[null,"","","REMOVE AND REPLACE FLARED END SECTION","",12,2650,31800]
[null,"0995000000-E","PIPE REMOVAL","","",53437,24.776465744708702,1323980]
[null,"0996000000-N","PIPE CLEAN OUT","","",1,4500,4500]
[null,"1000000000-E","6\" SLOPE PROTECTION","","",131,120,15720]
[null,"1011000000-N","FINE GRADING","","",4,3325950,13303800]
[null,"1022000000-E","SEALING PVMT CRACKS","","",73440,3.5,257040]
[null,"1077000000-E","#57 STONE","","",1085,53.559907834101402,58112.5]
[null,"1099500000-E","SHALLOW UNDERCUT","","",227000,10.5933524229075,2404691]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",385650,23.550700116686102,9082327.5]
[null,"1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",500,50,25000]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",105746,40.246704367068297,4255928]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",11100,49.756756756756801,552300]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",10.7,3861.4953271027998,41318]
[null,"1260000000-E","AGGREGATE SHOULDER BORROW","","",300,42.5,12750]
[null,"1275000000-E","PRIME COAT","","",29540,5,147700]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",135590,1.92222140275832,260634]
[null,"","","(2\")","",549120,2.5499999999999998,1400256]
[null,"","","(3\")","",24050,1.95,46897.5]
[null,"1330000000-E","INCIDENTAL MILLING","","",25967,9.3055859359956905,241638.15]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",476555,45.257623569157801,21567746.800000001]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",275380,55.566811315273398,15301988.5]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",41950,65.220679380214506,2736007.5]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",123830,58.087410159089103,7192964]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",172655,63.104398945874699,10895290]
[null,"1575000000-E","ASP FOR PLANT MIX","","",45227,463.57087359320798,20965919.899999999]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",9832,676.89015459723396,6655184]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",9002,243.561430793157,2192540]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",100,240,24000]
[null,"1735000000-E","REP JNT CONC PVT SLABS","","",60,200,12000]
[null,"1736000000-E","SELECT MATERIAL, CLASS IV","","",20,35,700]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",426040,0.19821800769881001,84448.8]
[null,"1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR ANDSEALING","",6120,2.99,18298.8]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","12\" CONCRETE TRUCK APRON","",1755,105,184275]
[null,"","","DIAMOND GRINDING PCC PAVEMENT","",8000,9.4,75200]
[null,"2021000000-N","GENERIC GRADING ITEM (EA)","RIGHT OF WAY MARKERS","",14,315,4410]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",28263.200000000001,30.379065357072101,858609.6]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",83749.5,9.3438796649532208,782545.25]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",336,22.5,7560]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",14070.3,60.0171353844623,844459.1]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",85749.5,16.065012040886501,1377566.75]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",174,343.13850574712598,59706.1]
[null,"2077000000-E","6\" OUTLET PIPE","","",1044,41.604022988505697,43434.6]
[null,"2099000000-E","SHOULDER DRAIN","","",107780,14.4698459825571,1559560]
[null,"2110000000-E","4\" SHOULDER DRAIN PIPE","","",107780,2.5987938393022798,280098]
[null,"2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",3750,15.22,57075]
[null,"2132000000-N","CONC PAD SHLDR DRN OUTLET","","",190,354,67260]
[null,"2190000000-N","TEMP STL PLT COVER FOR MDS","","",25,2720,68000]
[null,"2209000000-E","ENDWALLS","","",370.3,1513.4485552254901,560430]
[null,"2220000000-E","REINFORCED ENDWALLS","","",298.10000000000002,1083.27742368333,322925]
[null,"2253000000-E","PIPE COLLARS","","",32.274000000000001,1121.2319514159999,36186.639999999999]
[null,"2264000000-E","PIPE PLUGS","","",6.5330000000000004,1644.09153528241,10740.85]
[null,"2275000000-E","FLOWABLE FILL","","",2414,306.03148301574203,738760]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",1387,2984.3713626532099,4139323.08]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",315.733,2176.0839063385802,687061.5]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",655.5,546.70327993897797,358364]
[null,"2352000000-N","FRAME W/GRATE 840.***** STD","(840.16)","",81,730,59130]
[null,"2354200000-N","FRAME W/GRATE 840.24 STD","","",3,900,2700]
[null,"2355000000-N","FRAME W/GRATE 840.29 STD","","",4,750,3000]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",129,838.75968992248102,108200]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",129,886.04651162790697,114300]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",175,935.857142857143,163775]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",32,922.65625,29525]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",77,820.231688311688,63157.84]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",72,892.29166666666697,64245]
[null,"","","(F)","",188,922.473404255319,173425]
[null,"","","(G)","",189,955.06878306878298,180508]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",100,727.4,72740]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",304,2200,668800]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",105,1135.06666666667,119182]
[null,"2462000000-E","**\" SLUICE GATE","(8\")","",2,2050,4100]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","REMOVE AND REPLACE CONCRETE   APRON","",8,1500,12000]
[null,"","","SEALED PRECAST DRAINAGE       STRUCTURE","",5,3000,15000]
[null,"","","SEALED PRECAST DRAINAGE STRUC-TURES","",4,7950,31800]
[null,"2484000000-E","GENERIC DRAINAGE ITEM (LF)","SEALED PRECAST DRAINAGE       STRUCTURE","",9.3000000000000007,650,6045]
[null,"","","SEALED PRECAST DRAINAGE STRUC-TURES","",4,625,2500]
[null,"2495000000-E","GENERIC DRAINAGE ITEM (CY)","SEALED PRECAST DRAINAGE       STRUCTURE","",25.1,2000,50200]
[null,"2529000000-E","GENERIC GRADING ITEM (SF)","ARTIFICIAL TURF","",9705,8,77640]
[null,"2535000000-E","**\"X**\" CONCRETE CURB","(8\" X 12\")","",440,17.5,7700]
[null,"","","(8\" X 18\")","",1915,25.0078328981723,47890]
[null,"","","(9\" X 12\")","",340,31,10540]
[null,"","","(9\" X 18\")","",1390,16.5,22935]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",23565,22.842647994907701,538287]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",67570,32.006963149326602,2162710.5]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",9560,35.475418410041797,339145]
[null,"2570000000-N","MODIFIED CONCRETE FLUME","","",1,1800,1800]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",2190,43.963470319634702,96280]
[null,"2580000000-E","CONCRETE VALLEY GUTTER","","",670,18,12060]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",23855,50.397631523789599,1202235.5]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",252,2153.4722222222199,542675]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",2809,64.887878248486999,182270.05]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",1400,218.5,305900]
[null,"2627000000-E","4\" CONC ISLAND COVER","","",2451,5.5,13480.5]
[null,"2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",3090,75,231750]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",8485,74.401296405421306,631295]
[null,"2703000000-E","CONC BARRIER TYPE ******","(T)","",35754,113,4040202]
[null,"","","(T1)","",18446,135,2490210]
[null,"","","(T2)","",2141,300,642300]
[null,"2710000000-N","CONC BARRIER TRANS SECTN","","",8,25000,200000]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",4599,85,390915]
[null,"2738000000-E","GENERIC PAVING ITEM (SY)","12\" CONCRETE TRUCK APRON","",1270,110,139700]
[null,"","","6\" CONCRETE DRIVEWAY","",1915,224,428960]
[null,"","","9\" JOINTED CONCRETE TRUCK","APRON",1000,95,95000]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","2\" ROLLED CONCRETE CURB","",720,16,11520]
[null,"","","MEDIAN HAZARD PROTECTION","",928,179.256465517241,166350]
[null,"2800000000-N","ADJ CATCH BASINS","","",3,2250,6750]
[null,"2815000000-N","ADJ DROP INLETS","","",3,1450,4350]
[null,"2830000000-N","ADJ MANHOLES","","",19,1115.78947368421,21200]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",51,1250,63750]
[null,"2860000000-N","CONVERT CB TO JB","","",3,2166.6666666666702,6500]
[null,"2905000000-N","CONVERT DI TO JB","","",2,1100,2200]
[null,"2995000000-N","GENERIC DRAINAGE ITEM (EA)","REMOVE AND REPLACE DRAINAGE   STRUCTURES","",33,13000,429000]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",4,16150,64600]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",49750,23.722804020100501,1180209.5]
[null,"3045000000-E","SBGR SHOP CURVED","","",1075,24.095934883720901,25903.13]
[null,"3060000000-E","SBGR DOUBLE FACED","","",400,35,14000]
[null,"3105000000-N","SBGR TERM SECT","","",2,76,152]
[null,"3135000000-N","W-TR SBGR TRANS SECTIONS","","",2,250,500]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",55,65,3575]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",119,41.621848739495803,4953]
[null,"3180000000-N","GR ANCHOR TYPE **********","(B-77 MODIFIED)","",1,1895,1895]
[null,"3195000000-N","GR END TYPE AT-1","","",4,680,2720]
[null,"3210000000-N","GR END TYPE CAT-1","","",59,808.305084745763,47690]
[null,"3215000000-N","GR ANCHOR TYPE III","","",51,2002.35294117647,102120]
[null,"3287000000-N","GR END TYPE TL-3","","",103,3129.6116504854399,322350]
[null,"3288000000-N","GR END TYPE TL-2","","",20,2830,56600]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",62,2166.77419354839,134340]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",90809.5,1.1985364967321701,108838.5]
[null,"3365000000-E","REMOVE EXISTING GUIDERAIL","","",5700,1,5700]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",1777,7.4276871131119897,13199]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",6,1450,8700]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-3)","",4,2062.5,8250]
[null,"3389200000-E","CABLE GUIDERAIL","","",7400,7.9560810810810798,58875]
[null,"3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",10,75,750]
[null,"3389600000-N","CBL GUIDERAIL ANCH UNIT","","",14,1915.7142857142901,26820]
[null,"3420000000-E","GENERIC GUARDRAIL ITEM (LF)","REMOVE AND TRANSPORT EXISTING","GUARDRAIL",350,10,3500]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNITS,","TYPE CAT-1",1,250,250]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",68775,2.5523446019629201,175537.5]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",4396,18.936760691537799,83246]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",950,25.574736842105299,24296]
[null,"3536000000-E","CHN LK FENCE 48\" FABRIC","","",600,6.6,3960]
[null,"3542000000-E","MET LINE PST 48\" CL FEN","","",47,52,2444]
[null,"3548000000-E","MET TERM PST 48\" CL FEN","","",8,120,960]
[null,"3566000000-E","WOVEN WIRE FENCE RESET","","",5184,6.0378086419753103,31300]
[null,"3572000000-E","CHAIN LINK FENCE RESET","","",30,50,1500]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","PEDESTRIAN SAFETY RAIL","",60,175,10500]
[null,"3628000000-E","RIP RAP, CLASS I","","",3730,74.211796246648802,276810]
[null,"3635000000-E","RIP RAP, CLASS II","","",6550,85.830534351145005,562190]
[null,"3642000000-E","RIP RAP, CLASS A","","",650,100,65000]
[null,"3649000000-E","RIP RAP, CLASS B","","",4170,68.944844124700197,287500]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",29676,3.3548810486588501,99559.45]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(A)","",535,26.78,14327.3]
[null,"","","(B)","",165,34.51,5694.15]
[null,"","","(D)","",115,22.66,2605.9]
[null,"","","(E)","",450,10.3,4635]
[null,"","","(F)","",170,9.7899999999999991,1664.3]
[null,"","","(MILEMARKER)","",8,9.7899999999999991,78.319999999999993]
[null,"4048000000-E","REINF CONC FOUNDTN","","",33,845.60606060606096,27905]
[null,"4054000000-E","PLN CONC FOUNDTN","","",12,804.77499999999998,9657.2999999999993]
[null,"4057000000-E","OVERHEAD FOOTING","","",344,1550,533200]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",47635,6.1270517476645301,291862.11]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",2517,3.35,8431.9500000000007]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",13693,6.7915905937340204,92997.25]
[null,"4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",2,51.5,103]
[null,"4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(1019+50 -L-)","",1,40000,40000]
[null,"","","(1034+40 -L-)","",1,47000,47000]
[null,"","","(1044+00 -L-)","",1,49000,49000]
[null,"","","(1060+60 -L-)","",1,47000,47000]
[null,"","","(1070+50 -L-)","",1,48000,48000]
[null,"","","(1087+00 -L-)","",1,43000,43000]
[null,"","","(1117+00 -L-)","",1,40000,40000]
[null,"","","(1136+00 -L-)","",1,43500,43500]
[null,"","","(1141+00 -L-)","",1,44000,44000]
[null,"","","(1162+00 -L-)","",1,41000,41000]
[null,"","","(1167+00 -L-)","",1,44000,44000]
[null,"","","(1188+75 -L-)","",1,48000,48000]
[null,"","","(1220+56 -L-)","",1,57000,57000]
[null,"","","(1247+00 -L-)","",1,44000,44000]
[null,"","","(1272+50 -L-)","",1,51000,51000]
[null,"","","(1278+50 -L-)","",1,54000,54000]
[null,"","","(1305+00 -L-)","",1,54000,54000]
[null,"","","(1331+50 -L-)","",1,101000,101000]
[null,"","","(1351+00 -L-)","",1,58000,58000]
[null,"","","(1367+00 -L-)","",1,58000,58000]
[null,"","","(1377+00 -L-)","",1,54000,54000]
[null,"","","(1393+50 -L-)","",1,96000,96000]
[null,"","","(956+67 -L-)","",1,44000,44000]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",68,119.17647058823501,8104]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",689,71.675907111756203,49384.7]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",100,128.05500000000001,12805.5]
[null,"4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",25,928,23200]
[null,"","","(B)","",24,516,12384]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",28,486.28571428571399,13616]
[null,"","","(B)","",6,309,1854]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",20,74.965000000000003,1499.3]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",51,778.47058823529403,39702]
[null,"","","(D)","",27,238.888888888889,6450]
[null,"","","(E)","",4,268.5,1074]
[null,"4138000000-N","DISPOSE SUPPORT, STL BM","","",48,516,24768]
[null,"4149000000-N","DISPOSE SIGN SYST OVRHD","","",4,7750,31000]
[null,"4151000000-N","STOCKPILE SIGN SYST STL BM","","",4,515,2060]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",76,516,39216]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",601,2.8558735440931802,1716.38]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",4,1.65,6.6]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",27,4.7777777777777803,129]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",4904,6.7172614192495903,32941.449999999997]
[null,"4402000000-E","HIGH VISIBILITY STAT SIGNS","","",7483,16.5,123469.5]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",2492,12.0653611556982,30066.880000000001]
[null,"4407000000-E","HIGH VISIBILITY PORT SIGNS","","",2791,13.1,36562.1]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",3019,11.7275587943027,35405.5]
[null,"4415000000-N","FLASHING ARROW BOARD","","",22,3472.7272727272698,76400]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",34,12341.1764705882,419600]
[null,"4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",23,6760.8695652173901,155500]
[null,"4424000000-N","WZ PRESENCE LIGHTING","","",42,2550,107100]
[null,"4430000000-N","DRUMS","","",2215,35.992099322799099,79722.5]
[null,"4432000000-N","HIGH VISIBILITY DRUMS","","",4143,39,161577]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",124,142.98387096774201,17730]
[null,"4435000000-N","CONES","","",1165,24.378755364806899,28401.25]
[null,"4445000000-E","BARRICADES (TYPE III)","","",3942,47.441400304414003,187014]
[null,"4447000000-E","PED CHANNEL DEVICES","","",212,38.981132075471699,8264]
[null,"4455000000-N","FLAGGER","","",2280,365.811403508772,834050]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",65,9546.1538461538494,620500]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",12,3000,36000]
[null,"4480000000-N","TMA","","",14,36464.285714285703,510500]
[null,"4485000000-E","PORT CONC BARRIER","","",124361,43.260218235620499,5379884]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",79428,75,5957100]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",158004,5,790020]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",16701,9,150309]
[null,"4507000000-E","WATER FILLED BARRIER","","",8000,48.6,388800]
[null,"4508000000-E","REM & RES H2O FILL BARR","","",6000,6,36000]
[null,"4510000000-N","LAW ENFORCEMENT","","",3484,54.408725602755503,189560]
[null,"4516000000-N","SKINNY DRUM","","",1396,40.906160458452703,57105]
[null,"4570000000-E","TEMPORARY GLARE SCREEN","","",6148,25,153700]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",37,125.40540540540501,4640]
[null,"","","CONNECTED LANE CLOSURE DEVICE","",8,3810,30480]
[null,"","","PORTABLE FLASHING BEACONS &","DETECTION SYSTEM",2,16500,33000]
[null,"","","RAMP/LOOP CLOSURES","",16,1284,20544]
[null,"","","SINGLE LANE CLOSURE","",87,2300,200100]
[null,"","","TEMPORARY CURB RAMPS","",6,475,2850]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",12133,4.1441028599686804,50280.4]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",434501,0.81296498742235002,353234.1]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",654281,0.91212202402331999,596784.11]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",24010,3.2669512703040402,78439.5]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",20483,2.2659766635746701,46414]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",92,100.04347826087,9204]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",657,146.01826484018301,95934]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",788,2.85,2245.8000000000002]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",28,254,7112]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",916860,0.16871042471042,154683.84]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",1514554,0.2224107559057,336853.1]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",25779,0.59583730943791002,15360.09]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",99176,0.76,75373.759999999995]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",5044,1.4969865186360001,7550.8]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",83,15.5,1286.5]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",815,23.655214723926399,19279]
[null,"4847400000-E","WZ PERF PVMT MKG LINES 4\"","","",632260,0.25393429918072002,160552.5]
[null,"4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",1550357,0.52749969200642,817812.84]
[null,"4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",102672,0.87670367773102997,90012.92]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",54660,0.62772045371386997,34311.199999999997]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",743244,0.36,267567.84000000003]
[null,"4865000000-E","LINE REMOVAL 12\" WIDE","","",49586,0.71,35206.06]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",53,5.0999999999999996,270.3]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",27,51,1377]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA  PAVEMENT MARKING    LINES,","12\", 20 MILS (STANDARD GLASS  BEADS)",100,11,1100]
[null,"","","POLYUREA  PAVEMENT MARKING    LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",5156,2.5499999999999998,13147.8]
[null,"","","POLYUREA  PAVEMENT MARKING    LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",1450,3.55,5147.5]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\"","20 MILS (STANDARD GLASS BEADS)",17488,2.9,50715.199999999997]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\"","20 MILS (STANDARD GLASS BEADS)",1864,4,7456]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",920,1.25,1150]
[null,"","","WORK ZONE PERFORMANCE PAVEMENT","MARKING LINES, 24\"",5755,1.02,5870.1]
[null,"","","","MARKING LINES, 8\"",2722,1.02,2776.44]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (24\", 90 MILS)",3400,12.417941176470601,42221]
[null,"","","THERMOPLASTIC PAVMENT MARKING","LINES (24\", 90 MILS)",2072,11,22792]
[null,"4892000000-N","GENERIC PVMT MARKING ITEM (EA) 1205","THERMOPLASTIC PAVEMENT MARKING","CHARACTER (90 MILS)",20,80,1600]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",2600,39,101400]
[null,"","","","PAVEMENT MARKERS",12000,32,384000]
[null,"","","WORK ZONE PERFORMANCE PAVEMENT","MARKING CHARACTER",560,15.5,8680]
[null,"","","","MARKING SYMBOL",303,15.5,4696.5]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",8420,4.8242399049881204,40620.1]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",935,38.248663101604301,35762.5]
[null,"4915000000-E","7' U-CHANNEL POSTS","","",80,60,4800]
[null,"5010000000-E","100' HIGH MOUNT STANDARD","","",3,33500,100500]
[null,"5015000000-E","120' HIGH MOUNT STANDARD","","",17,34250,582250]
[null,"5020000000-N","PORTABLE DRIVE UNIT","","",1,28000,28000]
[null,"5025000000-E","HIGH MOUNT FOUNDATIONS","","",204,1100,224400]
[null,"5050000000-N","LIT STD MTLT ************","(45' TA, 15' ARM)","",24,4800,115200]
[null,"5070000000-N","STD FOUNDAT ***********","(TYPE M1)","",18,1500,27000]
[null,"","","(TYPE M2)","",6,1850,11100]
[null,"5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",5,3100,15500]
[null,"5125000000-E","SERVICE LATERAL *********","(3 #1/0 USE)","",125,51,6375]
[null,"5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",14418,8.1,116785.8]
[null,"","","(3\")","",485,19,9215]
[null,"","","(4\")","",423,28,11844]
[null,"5160000000-E","ELECT DUCT JA, SIZE *****","(3\")","",1236,24,29664]
[null,"","","(4\")","",809,27,21843]
[null,"","","(6\")","",215,41,8815]
[null,"5170000000-E","**-#8 W/G FEEDER CIRCUIT","(2)","",2603,3,7809]
[null,"5175000000-E","**-#6 W/G FEEDER CIRCUIT","(2)","",2619,4,10476]
[null,"5180000000-E","**-#4 W/G FEEDER CIRCUIT","(2)","",759,7,5313]
[null,"5205000000-E","**-#8 W/G FEEDR N *****\"","(2, 1.5\")","",15362,11,168982]
[null,"5210000000-E","**-#6 W/G FEEDR N *****\"","(2, 1.5\")","",7109,12,85308]
[null,"5215000000-E","**-#4 W/G FEEDER N *****\"","(2, 1.5\")","",5407,12.5,67587.5]
[null,"5240000000-N","ELEC JB ************","(BR18)","",8,3500,28000]
[null,"","","(CS36)","",5,895,4475]
[null,"","","(HM18)","",18,325,5850]
[null,"","","(HM30)","",1,610,610]
[null,"","","(HM36)","",1,895,895]
[null,"","","(IG18)","",44,365,16060]
[null,"","","(IG30)","",10,556,5560]
[null,"","","(IG36)","",6,1100,6600]
[null,"5255000000-N","PORTABLE LIGHTING","","",3,253666.66666666701,761000]
[null,"5260000000-N","GENERIC LIGHTING ITEM (LS)","LUMINAIRE STORAGE","",1,6100,6100]
[null,"5265000000-E","GENERIC LIGHTING ITEM (LF)","STREET LIGHTING CONDUIT IN-","STALLATION (2\" PVC)",4320,7.5,32400]
[null,"5270000000-N","GENERIC LIGHTING ITEM (EA)","100' HIGH MOUNT LUMINAIRE -   LED","",18,1800,32400]
[null,"","","120' HIGH MOUNT LUMINAIRE -   LED","",128,1800,230400]
[null,"","","COMMUNICATION GATEWAY","",4,6100,24400]
[null,"","","CONTROL NODE","",174,305,53070]
[null,"","","LIGHT CONTROL EQUIPMENT, TYPE","RW, 240/480V",4,14200,56800]
[null,"","","REINSTALL COBRAHEAD LUMINAIRE","",20,155,3100]
[null,"","","REINSTALL HIGH MAST LUMINAIRE","",8,175,1400]
[null,"","","RELOCATE CONTROL SYSTEM","",1,5100,5100]
[null,"","","REMOVE 100' HIGH MAST STAND-","ARD FOUNDATION",2,2600,5200]
[null,"","","REMOVE 100' HIGH MAST STANDARD","",2,2900,5800]
[null,"","","REMOVE LIGHT STANDARD FOUND-  ATION","",20,510,10200]
[null,"","","REMOVE SINGLE ARM LIGHT STAND-","ARD - DISPOSE",10,280,2800]
[null,"","","","ARD - SALVAGE",10,230,2300]
[null,"","","ROADWAY LIGHT STANDARD LUMI-","NAIRE - 285W LED",28,1265,35420]
[null,"5325000000-E","**\" WATER LINE","(1-1/2\")","",30,45,1350]
[null,"5325200000-E","2\" WATER LINE","","",187,10,1870]
[null,"5325600000-E","6\" WATER LINE","","",38990,35.938214926904301,1401231]
[null,"5325800000-E","8\" WATER LINE","","",4907,57.418993274913397,281755]
[null,"5326000000-E","10\" WATER LINE","","",504,61,30744]
[null,"5326200000-E","12\" WATER LINE","","",25339,80.221650420300705,2032736.4]
[null,"5326600000-E","16\" WATER LINE","","",1555,176.397909967846,274298.75]
[null,"5327400000-E","24\" WATER LINE","","",6416,314,2014624]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",205077,14.9244810485818,3060667.8]
[null,"5536000000-E","2\" VALVE","","",3,1270,3810]
[null,"5540000000-E","6\" VALVE","","",197,1623.20812182741,319772]
[null,"5546000000-E","8\" VALVE","","",27,2668.74074074074,72056]
[null,"5552000000-E","10\" VALVE","","",4,2950,11800]
[null,"5558000000-E","12\" VALVE","","",38,3821.1578947368398,145204]
[null,"5558600000-E","16\" VALVE","","",2,12512,25024]
[null,"5559400000-E","24\" VALVE","","",11,29526,324786]
[null,"5571600000-E","6\" TAPPING SLEEVE & VALVE","","",23,6701.3043478260897,154130]
[null,"5571800000-E","8\" TAPPING SLEEVE & VALVE","","",8,6224.75,49798]
[null,"5572200000-E","12\" TAPPING SLEEVE & VALVE","","",18,7782.1111111111104,140078]
[null,"5573000000-E","20\" TAPPING SLEEVE & VALVE","","",2,46100,92200]
[null,"5573400000-E","24\" TAPPING SLEEVE & VALVE","","",5,59468,297340]
[null,"5589200000-E","2\" AIR RELEASE VALVE","","",7,18500,129500]
[null,"5606000000-E","2\" BLOW OFF","","",8,15075,120600]
[null,"5643000000-E","**\" WATER METER","(2\")","",1,3000,3000]
[null,"5643150000-E","1-1/2\" WATER METER","","",6,7533,45198]
[null,"5648000000-N","RELOCATE WATER METER","","",102,688.30392156862695,70207]
[null,"5649000000-N","RECONNECT WATER METER","","",40,1275.3499999999999,51014]
[null,"5656000000-E","**\" RPZ BACKFLOW PREVNT ASMBLY","(1\")","",1,2280,2280]
[null,"","","(1-1/2\")","",6,5072,30432]
[null,"","","(2\")","",1,3300,3300]
[null,"5656200000-E","2\" RPZ BACKFLOW PREVNT ASMBLY","","",2,2100,4200]
[null,"5666000000-N","FIRE HYDRANT","","",21,6890.4761904761899,144700]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",38,2213.71052631579,84121]
[null,"5673000000-E","FIRE HYDRANT LEG","","",448,79.3388392857143,35543.800000000003]
[null,"5678400000-E","6\" LINE STOP","","",6,7050,42300]
[null,"5678600000-E","8\" LINE STOP","","",4,7510,30040]
[null,"5679000000-E","12\" LINE STOP","","",12,10400,124800]
[null,"5679400000-E","20\" LINE STOP","","",2,21750,43500]
[null,"5686000000-E","**\" H2O SERVICE LINE","(2\")","",942,73.805626326963903,69524.899999999994]
[null,"5686500000-E","WATER SERVICE LINE","","",4124,16.469859359844801,67921.7]
[null,"5691000000-E","**\" SANITARY GRAVITY SEWER","(15\")","",360,181.111111111111,65200]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",9347,89.784636781855099,839217]
[null,"5691400000-E","10\" SANITARY GRAVITY SEWER","","",958,125.75156576200401,120470]
[null,"5691500000-E","12\" SANITARY GRAVITY SEWER","","",3420,111.028070175439,379716]
[null,"5691600000-E","16\" SANITARY GRAVITY SEWER","","",3992,84,335328]
[null,"5691700000-E","18\" SANITARY GRAVITY SEWER","","",1352,171,231192]
[null,"5709100000-E","2\" FORCE MAIN SEWER","","",1029,25,25725]
[null,"5709300000-E","6\" FORCE MAIN SEWER","","",1863,41.044551798175,76466]
[null,"5709400000-E","8\" FORCE MAIN SEWER","","",2545,36,91620]
[null,"5709500000-E","10\" FORCE MAIN SEWER","","",2923,65,189995]
[null,"5709800000-E","20\" FORCE MAIN SEWER","","",988,48,47424]
[null,"5768000000-N","SANITARY SEWER CLEAN-OUT","","",76,693.68421052631595,52720]
[null,"5768500000-E","SEWER SERVICE LINE","","",3389,26.241369135438202,88932]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",4840,16.709607438016501,80874.5]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",121,4393.5371900826403,531618]
[null,"5776000000-E","5' DIA UTILITY MANHOLE","","",5,5100,25500]
[null,"5777000000-E","6' DIA UTILITY MANHOLE","","",4,6450,25800]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",385.5,232.088197146563,89470]
[null,"5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",20,200,4000]
[null,"5783000000-E","UTILITY MANHOLE WALL 6' DIA","","",38,195,7410]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(1-1/2\")","",157,15,2355]
[null,"","","(15\")","",3653,13.5121817684095,49360]
[null,"","","(2\")","",652,10,6520]
[null,"","","(4\")","",683,12,8196]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",17157,12,205884]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",8046,14.030822769077799,112892]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",3533,16.084347579960401,56826]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",15586,14.189736301809299,221161.23]
[null,"5805000000-E","ABANDON 14\" UTILITY PIPE","","",1335,12,16020]
[null,"5812000000-E","ABANDON 20\" UTILITY PIPE","","",947,12,11364]
[null,"5813000000-E","ABANDON 24\" UTILITY PIPE","","",5798,16,92768]
[null,"5815000000-N","REMOVE WATER METER","","",6,366,2196]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",4,1781,7124]
[null,"5816000000-N","ABANDON UTILITY MANHOLE","","",72,1356.25,97650]
[null,"5828000000-N","REMOVE UTILITY MANHOLE","","",2,1163.5,2327]
[null,"5835400000-E","6\" ENCASEMENT PIPE","","",216,139,30024]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",1327,85,112795]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",248,97,24056]
[null,"5835900000-E","20\" ENCASEMENT PIPE","","",408,117.093137254902,47774]
[null,"5836000000-E","24\" ENCASEMENT PIPE","","",2747,98.642155078267194,270970]
[null,"5836200000-E","30\" ENCASEMENT PIPE","","",1045,138,144210]
[null,"5836400000-E","36\" ENCASEMENT PIPE","","",982,149.96945010183299,147270]
[null,"5872500000-E","BORE & JACK **\"","(16\")","",800,208,166400]
[null,"","","(18\")","",125,257,32125]
[null,"","","(20\")","",293,294.93515358361799,86416]
[null,"","","(24\")","",1765,365.385269121813,644905]
[null,"","","(30\")","",550,391,215050]
[null,"","","(36\")","",646,752.68266253870001,486233]
[null,"5872600000-E","DIRECT DRILL **\"","(16\")","",1043,296.448465963567,309195.75]
[null,"","","(20\")","",899,434,390166]
[null,"","","(6\")","",1380,111,153180]
[null,"","","(8\")","",600,125.005,75003]
[null,"5876000000-N","STEEL PILE PIERS","","",6,84,504]
[null,"5882000000-N","GENERIC UTILITY ITEM (EA)","10\" INSERTION VALVE","",2,22000,44000]
[null,"","","12\" INSERT VALVE","",4,15350,61400]
[null,"","","12\" INSERTION VALVE","",4,29022.5,116090]
[null,"","","16\" NITRILE PIPE GASKET","",3,221,663]
[null,"","","2\" COMBINATION AIR RELEASE    VALVE","",1,12919,12919]
[null,"","","24\" NITRILE PIPE GASKET","",20,350,7000]
[null,"","","6\" INSERT VALVE","",6,9100,54600]
[null,"","","6\" INSERTION VALVE","",29,14000,406000]
[null,"","","8\" INSERT VALVE","",4,10500,42000]
[null,"","","8\" INSERTION VALVE","",4,16000,64000]
[null,"","","ABANDON UTILITY VAULT","",5,6500,32500]
[null,"","","ADJUSTMENT OF BRICK AND MORTARMANHOLES","",2,803,1606]
[null,"","","ADJUSTMENT OF PRECAST MANHOLES","",5,803,4015]
[null,"","","REMOVE EXISTING VAULT, BYPASS","AND STOCKPILE VALVES",1,5200,5200]
[null,"","","REMOVE UTILITY VAULT","",3,6500,19500]
[null,"","","WATER METER BOX","",2,200,400]
[null,"5888000000-E","GENERIC UTILITY ITEM (LF)","6\" SEWER SERVICE LINE","",299,40,11960]
[null,"","","MAJOR DRAINAGE STRUCTURES AND","BRICK AND MORTAR MANHOLES",3.5,960,3360]
[null,"","","","PRECAST MANHOLES",2,563,1126]
[null,"","","POLYETHYLENE ENCASEMENT ON 16\"DIA MAIN","",101,12,1212]
[null,"","","POLYETHYLENE ENCASEMENT ON 24\"DIA MAIN","",340,9,3060]
[null,"5912000000-N","GENERIC UTILITY ITEM (LS)","RELOCATE MASTER METER AND","INSTALL NEW VAULT",1,52200,52200]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",260845,2.25637255841592,588563.5]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",9730,51.924717368962,505227.5]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",29300,59.977952218429998,1757354]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",28750,49.310608695652199,1417680]
[null,"6015000000-E","TEMPORARY MULCHING","","",525,1024.9047619047601,538075]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",25600,1.4931640625,38225]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",133,896.82330827067699,119277.5]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",21685,20.698178464376301,448840]
[null,"6029000000-E","SAFETY FENCE","","",19840,2.0349798387096798,40374]
[null,"6030000000-E","SILT EXCAVATION","","",148980,6.59620083232649,982702]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",691490,1.40425385761182,971027.5]
[null,"6037000000-E","COIR FIBER MAT","","",3325,4.1721804511278204,13872.5]
[null,"6038000000-E","PERM SOIL REINF MAT","","",605,6.4975206611570204,3931]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",62205,3.9876014789807899,248048.75]
[null,"6043000000-E","LOW PERMEABILITY GEOTEXTILE","","",9205,4.9844432373709902,45881.8]
[null,"6045000000-E","**\" TEMPORARY PIPE","(18\")","",390,50,19500]
[null,"","","(24\")","",150,70,10500]
[null,"","","(30\")","",360,85,30600]
[null,"","","(36\")","",120,115,13800]
[null,"","","(48\")","",1200,90,108000]
[null,"","","(54\")","",391,130,50830]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",1092,26.584249084249102,29030]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",50,892,44600]
[null,"6071010000-E","WATTLE","","",640,15,9600]
[null,"6071012000-E","COIR FIBER WATTLE","","",51830,6.9019100906810698,357726]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",26390,4.4560117468738198,117594.15]
[null,"6071030000-E","COIR FIBER BAFFLE","","",28505,4.7115769163304702,134303.5]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",19,939.47368421052602,17850]
[null,"","","(2\")","",31,1125.8064516129,34900]
[null,"","","(2-1/2\")","",18,1200,21600]
[null,"","","(3\")","",10,1480,14800]
[null,"6078000000-E","SELECT UNDERGRTH REMOVAL","","",0.1,10000,1000]
[null,"6084000000-E","SEEDING AND MULCHING","","",447.75,2020.6783919597999,904758.75]
[null,"6087000000-E","MOWING","","",278.55,142.028361155986,39562]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",5400,8.3870370370370395,45290]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",17.75,1072.88732394366,19043.75]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",10700,6.4204439252336396,68698.75]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",319.25,908.14800313234105,289926.25]
[null,"6111000000-E","IMPERVIOUS DIKE","","",2193,50.435476516187897,110605]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",185,103.70810810810799,19186]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",510,236.71568627451001,120725]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",50,1310.4000000000001,65520]
[null,"6120000000-E","CULVERT DIVERSION CHANNEL","","",130,18.2846153846154,2377]
[null,"6123000000-E","REFORESTATION","","",0.25,12500,3125]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",420,136.42857142857099,57300]
[null,"","","FABRIC INSERT INLET PROTECTION DEVICE","",55,79.545454545454504,4375]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",35,150,5250]
[null,"6147000000-E","GENERIC EROSION CONTROL ITEM (LF)","TREE PROTECTION FENCE","",1700,2.5,4250]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",82,801.78048780487802,65746]
[null,"7060000000-E","SIGNAL CABLE","","",63220,3.7674659917747499,238179.20000000001]
[null,"7108000000-E","VEHICLE SIGNAL HD (12\", 1 SECT)","","",10,525,5250]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",205,758.90243902438999,155575]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",33,927.27272727272702,30600]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",29,1231.89655172414,35725]
[null,"7180000000-N","BACKPLATE","","",176,102.329545454545,18010]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",2520,2.8626984126984101,7214]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",12020,4.2558652246256203,51155.5]
[null,"7279000000-E","TRACER WIRE","","",3830,1.1419060052219301,4373.5]
[null,"7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",190,27.684210526315798,5260]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",14030,9.4808980755523908,133017]
[null,"","","(2, 2\")","",2740,14.917518248175201,40874]
[null,"","","(3, 2\")","",120,20,2400]
[null,"","","(4, 2\")","",70,24,1680]
[null,"7300100000-E","UNPAVED TRENCH TEMP LEADIN","","",370,6,2220]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",1920,24.719166666666698,47460.800000000003]
[null,"","","(2, 2\")","",170,32,5440]
[null,"7312000000-N","JUNCTION BOX (***************)","(SPECIAL OVER-SIZED HEAVY     DUTY)","",4,750,3000]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",199,334.90954773869299,66647]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",25,615.12,15378]
[null,"7360000000-N","WOOD POLE","","",39,957.74358974358995,37352]
[null,"7372000000-N","GUY ASSEMBLY","","",78,461.29487179487199,35981]
[null,"7384000000-E","***\" RISER WITH **************","(1-1/2\", WEATHERHEAD)","",2,607,1214]
[null,"","","(1-1/4\", WEATHERHEAD)","",12,607,7284]
[null,"7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",13,350,4550]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",45,384.6,17307]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",20,705,14100]
[null,"7430000000-N","HEAT SHRINK TUB KIT","","",5,120,600]
[null,"7432000000-E","2\" RISER WITH TUBING","","",25,588.30399999999997,14707.6]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",19195,7.1141677520187496,136556.45000000001]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",65930,1.74617928105567,115125.6]
[null,"7481000000-N","SITE SURVEY","","",9,1000,9000]
[null,"7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",32,39.0625,1250]
[null,"7481220000-N","CAMERA W/ INT LOOP EMUL PROCESS","","",14,1500,21000]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",18,3948,71064]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",5,5800,29000]
[null,"7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",21,250,5250]
[null,"7485000000-N","WRLESS MAGN SENSOR DET SYS","","",1,10327,10327]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(24)","",30925,2.7,83497.5]
[null,"7528000000-E","DROP CABLE","","",10120,2.6980237154150202,27304]
[null,"7540000000-N","SPLICE ENCLOSURE","","",23,1759.1304347826101,40460]
[null,"7541000000-N","MOD SPLICE ENCLOSURE","","",6,650,3900]
[null,"7552000000-N","INTERCONNECT CENTER","","",19,1594.7368421052599,30300]
[null,"7566000000-N","DELINEATOR MARKER","","",3,183.333333333333,550]
[null,"7575000000-N","FIBER-OPTIC TRAINING","","",1,7000,7000]
[null,"7575142000-N","900MHZ SPECTRUM RADIO","","",2,4128,8256]
[null,"7575142010-N","900MHZ SER/ETH SPEC RADIO","","",3,4100,12300]
[null,"7575142060-N","MOD RADIO INSTALL","","",7,1350,9450]
[null,"7575160000-E","REM EXT COMM CABLE","","",7595,0.90862409479921002,6901]
[null,"7576000000-N","METAL STRAIN SIGNAL POLE","","",42,13966.5238095238,586594]
[null,"7613000000-N","SOIL TEST","","",50,1230.8,61540]
[null,"7614100000-E","DRILLED PIER FOUND","","",401,1052.8678304239399,422200]
[null,"7636000000-N","SIGN FOR SIGNALS","","",73,313.84931506849301,22911]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",78,1811.5384615384601,141300]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",13,1638.4615384615399,21300]
[null,"7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",3,760,2280]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(2070LX, 332)","",9,14417,129753]
[null,"","","(2070LX, 336S)","",6,15950,95700]
[null,"","","(TYPE 2070LX, BASE MOUNTED)","",5,14785,73925]
[null,"","","(TYPE 2070LX, POLE MOUNTED)","",1,14810,14810]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",145,115.862068965517,16800]
[null,"7901000000-N","CABINET BASE EXTENDER","","",5,608,3040]
[null,"7912000000-N","BEACON CNTRL ASSM & CBNT *****","(F3)","",2,3875,7750]
[null,"","","(TYPE F3)","",1,6600,6600]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,10500,10500]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",5,3500,17500]
[null,"7972000000-N","METAL POLE REMOVAL","","",5,2500,12500]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","5/8\" X 10' GROUNDING ELEC-    TRODES","",5,180.25,901.25]
[null,"","","5/8\" X 10' GROUNDING ELECTRODE","",17,230,3910]
[null,"","","CCTV EXTENSION POLE","",1,515,515]
[null,"","","CCTV FIELD EQUIPMENT CABINET","",17,5300,90100]
[null,"","","CCTV WOOD POLE","",16,2500,40000]
[null,"","","CONTRACTOR FURNISHED CONTROL-","LER (2070LX)",4,2605,10420]
[null,"","","DIGITAL CCTV CAMERA  ASSEMBLY","",2,5657.5,11315]
[null,"","","DIGITAL CCTV CAMERA ASSEMBLY","",23,4100,94300]
[null,"","","DMS ACCESS LADDER","",6,7021.6666666666697,42130]
[null,"","","DMS ELECTRICAL SERVICE","",2,1850,3700]
[null,"","","DMS PEDESTAL STRUCTURE","",6,42228.333333333299,253370]
[null,"","","DMS STRUCTURE","",1,51888,51888]
[null,"","","DUAL DMS MOUNTED BACK TO BACK","",1,181999,181999]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE 2C)","",6,114856.66666666701,689140]
[null,"","","EQUIPMENT CABINET DISCONNECT","",20,1188.3,23766]
[null,"","","ETHERNET EDGE SWITCH","",45,1820.1111111111099,81905]
[null,"","","EXISTING CCTV CAMERA REMOVAL","",6,305,1830]
[null,"","","JUNCTION BOX MARKER","",21,195,4095]
[null,"","","METER BASE/DISCONNECT COMBINA-","TION PANEL",17,1500,25500]
[null,"","","METER/BASE DISCONNECT","COMBINATION PANEL",1,1236,1236]
[null,"","","MICROWAVE VEHICLE DETECTION","SYSTEM - MULTIPLE ZONES",1,13700,13700]
[null,"","","MODIFY EXISTING ELECTRICAL","SERVICE EQUIPMENT",2,1100,2200]
[null,"","","REMOVAL OF QUEUE BACKUP WARN- ING SYSTEM","",1,4500,4500]
[null,"","","REMOVE 900 MHZ RADIO","",5,52,260]
[null,"","","SOIL TEST FOR DMS FOUNDATION","",1,3500,3500]
[null,"7985000000-N","GENERIC SIGNAL ITEM (LS)","REMOVE DMS AND STRUCTURE AT","I-40 MM 324",1,5200,5200]
[null,"","","","I-40 MM 331",1,5200,5200]
[null,"","","","I-95 MM 78",1,5200,5200]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","#4 SOLID BARE COPPER GROUNDING","CONDUCTOR",50,9.27,463.5]
[null,"","","#4 SOLID BARE GROUNDING       CONDUCTOR","",2000,6.5,13000]
[null,"","","3-WIRE COPPER FEEDER CONDUC-  TORS","",6150,4.5,27675]
[null,"","","3-WIRE COPPER SERVICE","ENTRANCE CONDUCTORS",30,16.48,494.4]
[null,"","","4-WIRE COPPER FEEDER","CONDUCTORS",700,25.75,18025]
[null,"","","4-WIRE COPPER FEEDER CONDUC-  TORS","",100,12.5,1250]
[null,"","","BACK PULL FIBER OPTIC CABLE","",500,2.25,1125]
[null,"7992000000-E","GENERIC SIGNAL ITEM (CY)","DMS FOUNDATION","",15,1125,16875]
[null,"","","OVERHEAD FOOTINGS","",16,927,14832]
[null,"8035000000-N","REMV EXIST STR **********","(1260+34.00 -L-)","",1,115000,115000]
[null,"","","(1391+19.65 -L-)","",1,90000,90000]
[null,"","","(16+92.70 -L-)","",1,162620.93,162620.93]
[null,"","","(21+37.00 -L REV-)","",1,44000,44000]
[null,"","","(25+31.59 -Y18-)","",1,140000,140000]
[null,"","","(26+05.28 -Y14-)","",1,115000,115000]
[null,"","","(26+80.73 -Y17-)","",1,175000,175000]
[null,"","","(27+09.19 -Y16-)","",1,105000,105000]
[null,"8042000000-N","REMV EXIST STRS *********","(1002+79.68 -L REV-)","",1,190000,190000]
[null,"8056000000-N","REMV EXIST STR **********","(1042+08.93 -L-)","",1,125000,125000]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",3,3925,11775]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 26+05.28 -Y14-)","",1,8000,8000]
[null,"","","(1, 26+80.73 -Y17-)","",1,9000,9000]
[null,"","","(1, 27+09.19 -Y16-)","",1,7000,7000]
[null,"","","(1, 28+39.21 -Y29-)","",1,5000,5000]
[null,"","","(1, 30+65.33 -Y1B-)","",1,10000,10000]
[null,"8112730000-N","PDA TESTING","","",19,5120.8521052631604,97296.19]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(1260+34.00 -L-)","",1,80000,80000]
[null,"","","(1391+19.65 -L-)","",1,75000,75000]
[null,"","","(16+92.70 -L-)","",1,12000,12000]
[null,"","","(21+37.00 -L REV-)","",1,11000,11000]
[null,"","","(26+05.28 -Y14-)","",1,6000,6000]
[null,"","","(26+80.73 -Y17-)","",1,5000,5000]
[null,"8126000000-N","CULV EXCAV @ ************","(1042+08.93 -L-)","",1,80000,80000]
[null,"","","(1220+34.00 -L-)","",1,200000,200000]
[null,"","","(15+47.41 -NBCD-)","",1,30000,30000]
[null,"","","(172+34.91 -L-)","",1,10400,10400]
[null,"","","(35+91.00 -Y33-)","",1,35000,35000]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",1075,74.626046511627905,80223]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",122936,44.8597485683608,5514878.0499999998]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",167878,1.1719041804167301,196736.93]
[null,"8175000000-E","CLASS AA CONC (BRIDGE)","","",205.7,550,113135]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",2715.6,947.61240241567202,2573336.2400000002]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",1410.2,907.38703729967403,1279597.2]
[null,"8203000000-E","CLASS A CONCRETE RET WALL","","",28,718,20104]
[null,"8210000000-N","BRG APPR SLAB ***********","(1002+79.68 -L REV-)","",1,220000,220000]
[null,"","","(1260+34.00 -L-)","",1,220000,220000]
[null,"","","(1391+19.65 -L-)","",1,220000,220000]
[null,"","","(16+92.70 -L-)","",1,47100,47100]
[null,"","","(21+37.00 -L REV-)","",1,27940,27940]
[null,"","","(26+05.28 -Y14-)","",1,95000,95000]
[null,"","","(26+80.73 -Y17-)","",1,55000,55000]
[null,"","","(27+09.19 -Y16-)","",1,87000,87000]
[null,"","","(28+39.21 -Y29-)","",1,34000,34000]
[null,"","","(30+65.33 -Y1B-)","",1,29406.240000000002,29406.240000000002]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",431679,1.5672223341881399,676536.97]
[null,"8224000000-E","EPOXY COAT REINF STL BRDG","","",9487,3,28461]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",6068,2.8362310481212898,17210.25]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",180138,1.5041279463522399,270950.59999999998]
[null,"8252000000-E","REINF STEEL (RET WALL)","","",3002,1.55,4653.1000000000004]
[null,"8259000000-E","36\" PRESTR CONCRETE GIRDR","","",429,214.5,92020.5]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",3436.6,374.63044869929598,1287455]
[null,"8274000000-E","63\" MOD PRESTR CONC GIRDR","","",2137.5,450,961875]
[null,"8296000000-N","POLLUTION CONTROL","","",2,5038.07,10076.14]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",429,1129.13902097902,484400.64000000001]
[null,"8328400000-E","PILE DRV EQUIP SETUP ** GALV STEEL PILES","(HP 14 X 73)","",5,2420,12100]
[null,"","","(PP 30 X 0.50)","",40,10573.172,422926.88]
[null,"8364000000-E","HP12X53 PILES","","",29546,84.791613077912402,2505253]
[null,"8384200000-E","HP14X73 GALV PILES","","",330,66,21780]
[null,"8385200000-E","PP**X**** GALV STL PILE","(30 X 0.50)","",490,243.69,119408.1]
[null,"","","(PP 30 X 0.50)","",2560,330,844800]
[null,"8392000000-N","PIPE PILE PLATES","","",32,700,22400]
[null,"8393000000-N","PILE REDRIVES","","",244,290.00827868852502,70762.02]
[null,"8475000000-E","TWO BAR METAL RAIL","","",819.12,133.84844711397599,109637.94]
[null,"8482000000-E","THREE BAR METAL RAIL","","",431,210,90510]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",2895.08,121.652496649488,352193.71]
[null,"8504000000-E","CONC BARR RAIL MOMENT SLAB","","",158.74,600,95244]
[null,"8510000000-E","CONCRETE MEDIAN BARRIER","","",599.20000000000005,93,55725.599999999999]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",397.47,116.06999270385199,46134.34]
[null,"","","(1'-2\" X 3'-7\")","",453.67,176,79845.919999999998]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",780,89.573974358974397,69867.7]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",1.6,400,640]
[null,"8566000000-E","SURFACE PREP, CLASS III","","",301.89999999999998,500,150950]
[null,"8594000000-E","RIP RAP B","","",35,55,1925]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",3591,64.244486215538899,230701.95]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",3971,3.3417527071266702,13270.1]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",4,35579.154999999999,142316.62]
[null,"8660000000-E","CONCRETE REPAIRS","","",18.399999999999999,850,15640]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",117.32,800,93856]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",3955.7,89.365346209267599,353502.5]
[null,"8692000000-N","FOAM JOINT SEALS","","",1,35000,35000]
[null,"8706000000-N","EXPANSION JOINT SEALS","","",1,1150000,1150000]
[null,"8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(26+05.28 -Y14-)","",1,67000,67000]
[null,"","","(26+80.73 -Y17-)","",1,66000,66000]
[null,"","","(27+09.19 -Y16-)","",1,65000,65000]
[null,"","","(28+39.21 -Y29-)","",1,65000,65000]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",3023,74.802679457492602,226128.5]
[null,"","","(2)","",4922,64.353718000812705,316749]
[null,"","","(W3)","",4063,64,260032]
[null,"","","(W6)","",791,66,52206]
[null,"","","(W8)","",917,69,63273]
[null,"","","(W9)","",316,93,29388]
[null,"","","W1-1 (I-5878)","",8300,67,556100]
[null,"","","W1-1 (I-5883)","",3800,68,258400]
[null,"","","W1-2 (I-5878)","",4275,70,299250]
[null,"","","W1-2 (I-5883)","",3400,68,231200]
[null,"","","W2-1 (I-5878)","",5750,69,396750]
[null,"","","W2-1 (I-5883)","",3500,70,245000]
[null,"","","W2-1 (I-5986B)","",2830,70,198100]
[null,"","","W2-2 (I-5878)","",4880,71,346480]
[null,"","","W2-2 (I-5883)","",3800,67,254600]
[null,"","","W2-2 (I-5986B)","",2770,70,193900]
[null,"8802030000-E","SEGMENTAL GRAVITY RETAIN WALLS","","",450,225,101250]
[null,"8802040000-E","CIP GRAVITY RETAINING WALLS","","",6180,125,772500]
[null,"8804000000-N","GENERIC CULVERT ITEM (LS)","ASBESTO ASSESSMENT","",1,4500,4500]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL CONCRETE SURFACE","TREATMENT",41169,5.4,222312.6]
[null,"","","ARCHITECTURAL CONCRETE SURFACETREATMENT","",5445,1,5445]
[null,"","","ARCHITECTURAL SURFACE         TREATMENT","",37450,3,112350]
[null,"","","SOUND BARRIER WALL NO. NW29-1","",3720,50,186000]
[null,"","","SOUND BARRIER WALL NO. NW32-1","",7570,45,340650]
[null,"","","SOUND BARRIER WALL NO. NW33-1","",16160,45,727200]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","CLEANING AND PAINTING EXISTING","WEATHERING STEEL FOR BRIDGE   NO 500051",1,104114.72,104114.72]
[null,"","","HEAT STRAIGHTENING STEEL BEAM","REPAIR, BRIDGE #770012",1,90000,90000]
[null,"","","PAINTING CONTAINMENT FOR","BRIDGE #770010",1,15000,15000]
[null,"","","","BRIDGE #770012",1,15000,15000]
[null,"","","","BRIDGE NO 500051",1,85184.77,85184.77]
[null,"","","VOLUMETRIC MIXER","",1,5000,5000]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","45\" PREST CONC FLORIDA        I-BEAM","",7090.17,475,3367830.75]
[null,"","","FOAM JOINT SEALS FOR PRESER-  VATION","",1135,175,198625]
[null,"","","POURABLE SILICONE JOINT       SEALANT","",149.47,40,5978.8]
[null,"","","RAIL REPAIRS FOR ONE BAR METAL RAIL","",30,300,9000]
[null,"","","SILICONE JOINT SEALANT FOR","SLOPE PROTECTION",743,80,59440]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","EPOXY POLYMER CONCRETE","MATERIAL (ALTERNATE)",null,null,0]
[null,"","","EPOXY POLYMER CONCRETE        MATERIALS","",30.8,4500,138600]
[null,"","","LATEX MODIFIED CONCRETE OVER-","LAY - VERY EARLY STRENGTH",116.8,1700,198560]
[null,"","","POLYESTER POLYMER CONCRETE    MATERIALS","",32,2050,65600]
[null,"8882000000-E","GENERIC STRUCTURE ITEM (CF)","ELASTOMERIC CONCRETE FOR PRES-ERVATION","",279,750,209250]
[null,"8889000000-E","GENERIC STRUCTURE ITEM (LB)","SLOPE PROTECTION VOID FILLING","",1500,10,15000]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","BRIDGE JOINT DEMOLITION","",1124,50,56200]
[null,"","","CONCRETE DECK REPAIR FOR EPOXYOVERLAY","",0.2,1200,240]
[null,"","","EPOXY COATING","",6869.9,10.010131151836299,68768.600000000006]
[null,"","","EPOXY OVERLAY SYSTEM II","",44252,10,442520]
[null,"","","SILANE RAIL TREATMENTS","",2828,10,28280]
[null,"","","SURFACE PREPARATION FOR SILANE","RAIL TREATMENT",2828,15,42420]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","HYDRO-DEMOLITION OF BRIDGE    DECK","",2098,260,545480]
[null,"","","PLACING & FINISHING PC OVERLAY","",1156,72,83232]
[null,"","","PLACING AND FINISHING OF LATEXMODIFIED","CONCRETE OVERLAY-VERY EARLY   STRENGTH",2098,260,545480]
[null,"","","PLACING AND FINISHING POLYMER","CONCRETE OVERLAY",554,185,102490]
[null,"","","SCARIFYING BRIDGE DECK","",3808,63.464285714285701,241672]
[null,"","","SHOTBLASTING BRIDGE DECK","",3712,18.073275862069,67088]
[null,"","","SILANE DECK TREATMENT","",1966,20,39320]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","CFRP PEDESTAL REPAIRS AND","BEARING RETROFIT",16,3000,48000]
[null,"","","CLEANING AND PAINTING EXISTING","BEARINGS WITH HRSCA",72,1000,72000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  770010","",8,7000,56000]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  770012","",8,7000,56000]

{"sheet":"ITEMS - DIV 07","index":9,"n_rows":574,"n_cols":8,"rows_kept":574,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 07"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",7,513089.258571429,3591624.81]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",3,152933.33333333299,458800]
[null,"0000700000-N","FIELD OFFICE","","",1,225000,225000]
[null,"0000996000-N","DESIGN AND CONSTRUCTION","","",1,236457869,236457869]
[null,"0001000000-E","CLEARING & GRUBBING","","",22,52272.727272727301,1150000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",2,1041.68,2083.36]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",225000,8.39,1887750]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(19+56.99 -L-)","",1,50875,50875]
[null,"","","(41+39.51 -Y-)","",1,130000,130000]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(27+02.26 -L-)","",1,40000,40000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",43425,5.7966033390903897,251717.5]
[null,"0043000000-N","GRADING","","",3,611577.92333333299,1834733.77]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",2,4000.5,8001]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",450,42,18900]
[null,"0106000000-E","BORROW EXCAVATION","","",680000,7.99,5433200]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",13088,9.3919582823960894,122921.95]
[null,"0141000000-E","BERM DITCH CONSTRUCTION","","",580,7.29,4228.2]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",56500,6.33,357645]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",4200,5.73,24066]
[null,"0192000000-N","PROOF ROLLING","","",20,187.5,3750]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",48500,27.66,1341510]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",2625,31.8857142857143,83700]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",48925,2.07967807869188,101748.25]
[null,"0199000000-E","TEMPORARY SHORING","","",3670,30.5103542234332,111973]
[null,"0223000000-E","ROCK PLATING","","",525,125,65625]
[null,"0234000000-E","GENERIC GRADING ITEM (CY)","REMOVAL AND HAULING OF DEEP","BROWNFIELDS SOIL",10000,4.95,49500]
[null,"","","STOCKPILED SOIL","",500,10.42,5210]
[null,"0245000000-E","GENERIC GRADING ITEM (GAL)","TRENCH DEWATERING","",10000,1.82,18200]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",60,150,9000]
[null,"","","HAULING AND DISPOSAL OF CONTA-","MINATED SOIL STOCKPILES",500,78.13,39065]
[null,"","","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,78.13,3906.5]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",2373,33.644719764011803,79838.92]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",8710,2.5479334098737101,22192.5]
[null,"0331000000-E","GENERIC DRAINAGE ITEM (CY)","ANTI-SEEP COLLAR","",30,364.59,10937.7]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",96,51,4896]
[null,"0342000000-E","**\" SIDE DRAIN PIPE","(30\")","",440,76.040000000000006,33457.599999999999]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",2900,46.966055172413803,136201.56]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",444,52.145945945945897,23152.799999999999]
[null,"0345000000-E","24\" SIDE DRAIN PIPE","","",980,61.485714285714302,60256]
[null,"0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(15\")","",26,245.51538461538499,6383.4]
[null,"","","(24\")","",2,520.84,1041.68]
[null,"0354000000-E","***\" RC PIPE CULV *****","(60\", V)","",412,380.21,156646.51999999999]
[null,"0366000000-E","15\" RC PIPE CULV III","","",408,45.83,18698.64]
[null,"0372000000-E","18\" RC PIPE CULV III","","",84,59.38,4987.92]
[null,"0378000000-E","24\" RC PIPE CULV III","","",168,76.083809523809506,12782.08]
[null,"0384000000-E","30\" RC PIPE CULV III","","",80,93.75,7500]
[null,"0390000000-E","36\" RC PIPE CULV III","","",72,114.59,8250.48]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",7536,55.841295116772798,420820]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",1096,62.608759124087598,68619.199999999997]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",1216,85.102763157894699,103484.96]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",584,88.54,51707.360000000001]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",160,119.79,19166.400000000001]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",668,67.868263473053901,45336]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",80,62.85,5028]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",24,253.65,6087.6]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(15\", 0.250\")","",35,1000,35000]
[null,"","","(60\", 0.844\")","",248,2239.62,555425.76]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(15\", 0.250\")","",35,1,35]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","16\" SEALED DUCTILE IRON PIPE  CLASS 250","",880,188.54,165915.20000000001]
[null,"","","24\" SEALED DUCTILE IRON PIPE  CLASS 200","",170,307.3,52241]
[null,"","","30\" SEALED DUCTILE IRON PIPE  CLASS 150","",120,536.47,64376.4]
[null,"","","36\" SEALED DUCTILE IRON PIPE  CLASS 150","",134,767.72,102874.48]
[null,"","","42\" SEALED DUCTILE IRON PIPE  CLASS 150","",162,808.35,130952.7]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","BOOTS FOR SEALED DRAINAGE     STRUCTURES","",26,312.5,8125]
[null,"0995000000-E","PIPE REMOVAL","","",5031,12.819409660107301,64494.45]
[null,"1011000000-N","FINE GRADING","","",1,750000,750000]
[null,"1044000000-E","LIME TRTD SOIL (SLURRY)","","",48000,4.05,194400]
[null,"1066000000-E","LIME FOR LIME TREATED SOIL","","",580,200.5,116290]
[null,"1077000000-E","#57 STONE","","",40,39.06,1562.4]
[null,"1099500000-E","SHALLOW UNDERCUT","","",3400,16.6926470588235,56755]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",20950,30.026730310262501,629060]
[null,"1110000000-E","STABILIZER AGGREGATE","","",500,40.9,20450]
[null,"1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",29135,3.33,97019.55]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",620,33.83,20974.6]
[null,"1176000000-E","SOIL CEMENT BASE","","",48000,3.87,185760]
[null,"1187000000-E","PC FOR SOIL CEMENT BASE","","",1320,191.75,253110]
[null,"1209000000-E","ASPHALT CURING SEAL","","",14400,2.5,36000]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",7693,40.107318341349298,308545.59999999998]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",250679,1.3524100542925399,339020.79999999999]
[null,"","","(1-1/4\")","",5855,2.95,17272.25]
[null,"","","(2-1/2\")","",250,23.35,5837.5]
[null,"","","(3\")","",19150,3,57450]
[null,"1330000000-E","INCIDENTAL MILLING","","",35297,7.4744272884381102,263824.86]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",68420,54.036831335866701,3697200]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",34850,54.618938307030099,1903470]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",79696,38.099296075085299,3036361.5]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",39523,49.369025630645503,1951212]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",7720,101.743523316062,785460]
[null,"1575000000-E","ASP FOR PLANT MIX","","",12617,439.40051359277197,5543916.2800000003]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",670,741.64179104477603,496900]
[null,"1662000000-E","OG ASP FRICT FC-1 MOD","","",3710,89.959568733153603,333750]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",2850,129.82456140350899,370000]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",562,193,108466]
[null,"1775000000-E","AST, MAT COAT, #78M STONE","","",583616,0.35520504921043999,207303.35]
[null,"1775500000-E","AST, MAT COAT, #*** STONE","(#67)","",183288,0.3,54986.400000000001]
[null,"1838000000-E","EMULSION FOR AST","","",262137,1.8943293010906499,496573.8]
[null,"1838500000-N","VACUUM TRUCK","","",14,500,7000]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",52095,0.91033688453785999,47424]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",218.4,48.271794871794903,10542.56]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",1000,9.2149999999999999,9215]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",168,122.75,20622]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",1000,15.35,15350]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",4,686.2,2744.8]
[null,"2077000000-E","6\" OUTLET PIPE","","",24,42.8125,1027.5]
[null,"2099000000-E","SHOULDER DRAIN","","",1800,17,30600]
[null,"2110000000-E","4\" SHOULDER DRAIN PIPE","","",1800,2,3600]
[null,"2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",30,25,750]
[null,"2143000000-E","BLOTTING SAND","","",10,131.96,1319.6]
[null,"2209000000-E","ENDWALLS","","",7.6,1666.68947368421,12666.84]
[null,"2253000000-E","PIPE COLLARS","","",4.9480000000000004,2641.3257881972499,13069.28]
[null,"2264000000-E","PIPE PLUGS","","",2.9000000000000001E-2,5500,159.5]
[null,"2275000000-E","FLOWABLE FILL","","",10.7,429.672897196262,4597.5]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",227,2331.5488986784098,529261.6]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",13.731999999999999,1562.2997378386301,21453.5]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",84.6,235.652245862884,19936.18]
[null,"2354000000-N","FRAME W/GRATE 840.22 STD","","",1,729.18,729.18]
[null,"2363000000-N","FRAME W/2GRTS 840.***** STD","(840.15)","",6,700,4200]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",23,606.07130434782596,13939.64]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",34,740.32823529411803,25171.16]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",54,979.99407407407398,52919.68]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",1,911.47,911.47]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",8,600.005,4800.04]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",12,793.75333333333299,9525.0400000000009]
[null,"","","(F)","",43,803.05581395348804,34531.4]
[null,"","","(G)","",46,803.49130434782603,36960.6]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",24,617.59749999999997,14822.34]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",9,4160,37440]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",20,1765.5435,35310.870000000003]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","SEALED PRECAST DRAINAGE STRUC-TURE","",13,3020.88,39271.440000000002]
[null,"2484000000-E","GENERIC DRAINAGE ITEM (LF)","SEALED PRECAST DRAINAGE STRUC-TURE","",17,364.59,6198.03]
[null,"2535000000-E","**\"X**\" CONCRETE CURB","(8\" X 12\")","",30,26,780]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",6800,19.03,129404]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",17870,22.850279798544999,408334.5]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",3110,30.6752411575563,95400]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",1980,71.992424242424207,142545]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",6760,45.743343195266299,309225]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",81,2066.6666666666702,167400]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",190,74.631578947368396,14180]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",103,86.407766990291293,8900]
[null,"2627000000-E","4\" CONC ISLAND COVER","","",270,44.5,12015]
[null,"2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",140,71.5,10010]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",2600,62.653846153846203,162900]
[null,"2703000000-E","CONC BARRIER TYPE ******","(III)","",900,91,81900]
[null,"2710000000-N","CONC BARRIER TRANS SECTN","","",2,2500,5000]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",2140,107.048598130841,229084]
[null,"2766000000-N","GENERIC PAVING ITEM (LS)","42\" CONCRETE BARRIER WITH","MOMENT SLAB",1,323640.58,323640.58]
[null,"2800000000-N","ADJ CATCH BASINS","","",1,4500,4500]
[null,"2815000000-N","ADJ DROP INLETS","","",12,1341.6783333333301,16100.14]
[null,"2830000000-N","ADJ MANHOLES","","",209,882.89473684210498,184525]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",189,875,165375]
[null,"2905000000-N","CONVERT DI TO JB","","",12,2247.5916666666699,26971.1]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",6,26444.5133333333,158667.07999999999]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",14825,19.4305396290051,288057.75]
[null,"3045000000-E","SBGR SHOP CURVED","","",950,19.4455263157895,18473.25]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",41,65.97,2704.77]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",25,17.204000000000001,430.1]
[null,"3195000000-N","GR END TYPE AT-1","","",5,504.5,2522.5]
[null,"3210000000-N","GR END TYPE CAT-1","","",11,777.27272727272702,8550]
[null,"3215000000-N","GR ANCHOR TYPE III","","",2,1725.5,3451]
[null,"3287000000-N","GR END TYPE TL-3","","",23,2839.6739130434798,65312.5]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",25,1886.0103999999999,47150.26]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",9235,1.0905305901461799,10071.049999999999]
[null,"3365000000-E","REMOVE EXISTING GUIDERAIL","","",500,2,1000]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",11300,7,79100]
[null,"3389400000-E","DBL FACED CABLE GUIDERAIL","","",1290,7.6046511627906996,9810]
[null,"3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",10,90,900]
[null,"3389600000-N","CBL GUIDERAIL ANCH UNIT","","",8,2225,17800]
[null,"3435000000-N","GENERIC GUARDRAIL ITEM (EA)","TEMPORARY GUARDRAIL END UNITS,TYPE TL-3","",2,3750,7500]
[null,"","","TEMPORARY IMPACT ATTENUATOR","UNITS, TYPE TL-3",1,32666.77,32666.77]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNITS,TYPE CAT-1","",2,500,1000]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",16800,2.9583333333333299,49700]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",1065,17.248826291079801,18370]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",278,28.683453237410099,7974]
[null,"3557000000-E","ADDITIONAL BARBED WIRE","","",60,1,60]
[null,"3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 7'-6\", 15')","",2,1100,2200]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","STEEL PIPE HANDRAIL","",50,225,11250]
[null,"3628000000-E","RIP RAP, CLASS I","","",500,50,25000]
[null,"3635000000-E","RIP RAP, CLASS II","","",650,57.29,37238.5]
[null,"3642000000-E","RIP RAP, CLASS A","","",10,62.5,625]
[null,"3649000000-E","RIP RAP, CLASS B","","",2717,46.782480677217499,127108]
[null,"3651000000-E","BOULDERS","","",100,156.25,15625]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",13933,2.61823010119859,36479.800000000003]
[null,"3659000000-N","PREFORMED SCOUR HOLES","","",4,3125.05,12500.2]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",119,18,2142]
[null,"4048000000-E","REINF CONC FOUNDTN","","",6,335.16666666666703,2011]
[null,"4054000000-E","PLN CONC FOUNDTN","","",3,117.083333333333,351.25]
[null,"4057000000-E","OVERHEAD FOOTING","","",213,1287.60563380282,274260]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",4966,6.4053705195328199,31809.07]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",761,13.968515111695099,10630.04]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",3175,6.3266141732283501,20087]
[null,"4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",4,55,220]
[null,"4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(12+69 -Y2-)","",1,69500,69500]
[null,"","","(16+86 -Y1RP-)","",1,200000,200000]
[null,"","","(23+15 -L-)","",1,139050,139050]
[null,"","","(23+61 -Y2-)","",1,49000,49000]
[null,"","","(30+75 -L-)","",1,103000,103000]
[null,"","","(33+50.00 -Y-)","",1,105000,105000]
[null,"","","(40+24.00 -Y-)","",1,57500,57500]
[null,"","","(42+44.00 -Y-)","",1,47500,47500]
[null,"","","(46+80.00 -Y-)","",1,91000,91000]
[null,"","","(47+08.00 -L-)","",1,55500,55500]
[null,"","","(49+43 -Y2-)","",1,49000,49000]
[null,"","","(78+18.00 -L-)","",1,75000,75000]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",4,103,412]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",195,70.328717948717994,13714.1]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",9,79.1111111111111,712]
[null,"4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",27,794.96740740740699,21464.12]
[null,"","","(B)","",11,258.09090909090901,2839]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",15,623,9345]
[null,"","","(B)","",4,352.625,1410.5]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",4,50,200]
[null,"4115000000-N","SIGN ERECTION, OVERLAY (OVRHD)","","",7,585,4095]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(E)","",8,110,880]
[null,"","","(GM RESTAURANT LOGO SIGNS)","",1,515,515]
[null,"4149000000-N","DISPOSE SIGN SYST OVRHD","","",3,8401.6666666666697,25205]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",18,501.38888888888903,9025]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",163,2.6777300613496902,436.47]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",2,4.12,8.24]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",1,4.12,4.12]
[null,"4234000000-N","DISPOSE SIGN, A OR B (OVRHD)","","",16,70,1120]
[null,"4238000000-N","DISPOSE SIGN, D, E, F","","",1,1.1499999999999999,1.1499999999999999]
[null,"4241000000-N","DISPOSE SIGN, OVERLAY OVRHD","","",3,58,174]
[null,"4251000000-N","DISPOSE LIGHT SYSTEM","","",1,745,745]
[null,"4263000000-N","DISPOSE WALKWAY","","",4,745,2980]
[null,"4360000000-N","GENERIC SIGNING ITEM (EA)","CUTTING OF SIGN HANGERS, OVER-HEAD","",4,245,980]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",2951.5,9.2206200237167497,27214.66]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",2355,13.3994904458599,31555.8]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",552,5.6253623188405797,3105.2]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",7277,5.5902294901745204,40680.1]
[null,"4415000000-N","FLASHING ARROW BOARD","","",20,3409,68180]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",18,10366.666666666701,186600]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",200,55.89,11178]
[null,"4430000000-N","DRUMS","","",1337,58.649962602842201,78415]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",101,137.50495049505,13888]
[null,"4435000000-N","CONES","","",310,40.403225806451601,12525]
[null,"4445000000-E","BARRICADES (TYPE III)","","",1184,20.896959459459499,24742]
[null,"4447000000-E","PED CHANNEL DEVICES","","",88,38.636363636363598,3400]
[null,"4455000000-N","FLAGGER","","",1515,300.825082508251,455750]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",2,159450,318900]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",23,6738.2608695652198,154980]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",28,2822.5,79030]
[null,"4480000000-N","TMA","","",14,17325,242550]
[null,"4485000000-E","PORT CONC BARRIER","","",26895,34.926064324223802,939336.5]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",1350,63.8888888888889,86250]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",34350,5.0324890829694304,172866]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",410,9,3690]
[null,"4510000000-N","LAW ENFORCEMENT","","",306,60.980392156862699,18660]
[null,"4516000000-N","SKINNY DRUM","","",136,65,8840]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",8,181.25,1450]
[null,"","","PEDESTRIAN TRANSPORT SERVICE  (PER TRIP)","",1550,4.8483870967741902,7515]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",2842,6.8124912033778999,19361.099999999999]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",209524,0.50551087226283997,105916.66]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",354953,0.67082627840869002,238111.8]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",11560,2.0840683391003498,24091.83]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",9142,2.3681382629621499,21649.52]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",188,93.138297872340402,17510]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",595,109.685714285714,65263]
[null,"4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",48,265,12720]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",4682,2.8941691584792801,13550.5]
[null,"","","(IV)","",721,2.6449375866851601,1907]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",103,4,412]
[null,"","","(IV)","",102,3.5,357]
[null,"4800000000-N","COLD APP PLAS CHAR TYPE *","(II)","",24,120,2880]
[null,"","","(IV)","",24,115,2760]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",13,211.538461538462,2750]
[null,"","","(IV)","",5,294,1470]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",220922,0.26043300350350002,57535.38]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",333329,0.26763851930075,89211.68]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",15028,0.87071333510780002,13085.08]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",35768,1.13174625363453,40480.300000000003]
[null,"4830000000-E","PAINT PVT MKGS LINES 16\"","","",150,2.5,375]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",5646,1.9426142401700299,10968]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",204,40.882352941176499,8340]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",765,41.235294117647101,31545]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",20127,0.80621801560092998,16226.75]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",66553,0.70210884558172004,46727.45]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",1193,1.33528918692372,1593]
[null,"4865000000-E","LINE REMOVAL 12\" WIDE","","",9315,1.18510466988728,11039.25]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",180,3.5,630]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",77,41.487012987013003,3194.5]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","HOT SPRAY THERMOPLASTIC       PAVEMENT","MARKING LINES (4\", 50 MILS)",430245,0.23,98956.35]
[null,"","","","MARKING LINES (6\", 50 MILS)",616,0.5,308]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES (4\",       50 MILS)",340670,0.23,78354.100000000006]
[null,"","","","MENT MARKING LINES (6\",       50 MILS)",570,0.34,193.8]
[null,"","","POLYUREA PAVEMENT MARKING     LINES","(4\", 20 MILS) (STANDARD GLASS BEADS)",380,1.75,665]
[null,"","","","(6\", 20 MILS) (STANDARD GLASS BEADS)",1440,2.58,3715.2]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 12\"","30 MILS (STANDARD GLASS BEADS)",4736,2.5,11840]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\"","20 MILS (STANDARD GLASS BEADS)",1200,4.5,5400]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",2888,5.8,16750.400000000001]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","30 MILS (STANDARD GLASS BEADS)",17545,2.0499999999999998,35967.25]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",450,9.7777777777777803,4400]
[null,"","","","LINES (24\", 90 MILS)",8584,8.3802714352283303,71936.25]
[null,"4892000000-N","GENERIC PVMT MARKING ITEM (EA) 1205","HEATED-IN-PLACE THERMOPLASTIC PAVE-","MENT MARKING CHARACTER (90    MILS)",78,175,13650]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",940,35,32900]
[null,"","","","PAVMENT MARKER",445,64,28480]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",73,15.579452054794499,1137.3]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",2122,31.189443920829401,66184]
[null,"5010000000-E","100' HIGH MOUNT STANDARD","","",2,28700,57400]
[null,"5015000000-E","120' HIGH MOUNT STANDARD","","",7,31071.428571428602,217500]
[null,"5020000000-N","PORTABLE DRIVE UNIT","","",2,5525,11050]
[null,"5025000000-E","HIGH MOUNT FOUNDATIONS","","",43,1475,63425]
[null,"5030000000-N","HM LUMINAIRE ************","(560W LED)","",12,1575,18900]
[null,"5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",23,4286.95652173913,98600]
[null,"","","(45' TA, 15' ARM)","",3,4250,12750]
[null,"5070000000-N","STD FOUNDAT ***********","(R1)","",16,825,13200]
[null,"","","(R2)","",2,950,1900]
[null,"","","(TYPE R1)","",9,877.41666666666697,7896.75]
[null,"","","(TYPE R2)","",2,1410,2820]
[null,"5080000000-N","LITE STD LUM ************","(RDW, 285W LED)","",6,1125,6750]
[null,"5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",3,941.66666666666697,2825]
[null,"5125000000-E","SERVICE LATERAL *********","(3 #1/0 USE)","",75,16.8333333333333,1262.5]
[null,"5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",850,11.5795882352941,9842.65]
[null,"5160000000-E","ELECT DUCT JA, SIZE *****","(3\")","",1018,15.8503438113949,16135.65]
[null,"","","(4\")","",650,22.3519230769231,14528.75]
[null,"5170000000-E","**-#8 W/G FEEDER CIRCUIT","(2)","",595,5.1462184873949601,3062]
[null,"5180000000-E","**-#4 W/G FEEDER CIRCUIT","(2)","",1055,9.4549763033175402,9975]
[null,"5185000000-E","**-#2 W/G FEEDER CIRCUIT","(2)","",530,7.4984905660377397,3974.2]
[null,"5205000000-E","**-#8 W/G FEEDR N *****\"","(2, 1.5\")","",8445,8.4533747779751298,71388.75]
[null,"5215000000-E","**-#4 W/G FEEDER N *****\"","(2, 1.5\")","",8950,12.7122905027933,113775]
[null,"5220000000-E","**-#2 W/G FEEDER N *****\"","(2, 1.5\")","",2730,15.940329670329699,43517.1]
[null,"5240000000-N","ELEC JB ************","(CS36)","",4,1087.5,4350]
[null,"","","(HM18)","",9,497.222222222222,4475]
[null,"","","(IG18)","",30,502.92599999999999,15087.78]
[null,"","","(IG30)","",1,950,950]
[null,"","","(IG36)","",4,1500,6000]
[null,"","","(LS18)","",29,583.02689655172401,16907.78]
[null,"5252000000-N","UNDERPASS LUMINARIES *****","(WM)","",8,780,6240]
[null,"5253000000-N","UNDERPASS CIRCUITRY *************","(UPL-1)","",1,6500,6500]
[null,"","","(UPL-2)","",1,6500,6500]
[null,"5255000000-N","PORTABLE LIGHTING","","",4,34002.54,136010.16]
[null,"5260000000-N","GENERIC LIGHTING ITEM (LS)","LUMINAIRE STORAGE","",2,2837.5,5675]
[null,"5270000000-N","GENERIC LIGHTING ITEM (EA)","100A 6-POSITION MAIN CB PANEL","",1,450,450]
[null,"","","120' HIGH MOUNT LUMINAIRE -   LED","",32,1800,57600]
[null,"","","CCTV SERVICE DISCONNECT","",1,895,895]
[null,"","","COMMUNICATION GATEWAY","",1,5685,5685]
[null,"","","CONTROL NODE","",53,175,9275]
[null,"","","LIGHT CONTROL EQUIPMENT, TYPE","RW, 120/240V",3,17500,52500]
[null,"","","","RW, 240/480V",1,10000,10000]
[null,"","","REINSTALL COBRAHEAD LUMINAIRE","",10,235,2350]
[null,"","","REINSTALL COMMUNICATION GATE- WAY","",1,475,475]
[null,"","","REINSTALL HIGH MAST LUMINAIRE","",24,575,13800]
[null,"","","RELOCATE LIGHT STANDARD","",1,1818,1818]
[null,"","","REMOVE 100' HIGH MAST STANDARD","",2,5775,11550]
[null,"","","REMOVE 100' HIGH MAST STANDARDFOUNDATION","",2,2300,4600]
[null,"","","REMOVE 120' HIGH MAST STANDARD","",3,6260,18780]
[null,"","","REMOVE 120' HIGH MAST STANDARDFOUNDATION","",3,2300,6900]
[null,"","","REMOVE CONTROL SYSTEM -       DISPOSE","",2,1150,2300]
[null,"","","REMOVE CONTROL SYSTEM -       SALVAGE","",1,980,980]
[null,"","","REMOVE LIGHT STANDARD FOUNDA- TION","",6,968.16666666666697,5809]
[null,"","","REMOVE SINGLE ARM LIGHT       STANDARD","",1,606,606]
[null,"","","REMOVE SINGLE ARM LIGHT STAND-","ARD - DISPOSE",1,400,400]
[null,"","","","ARD - SALVAGE",1,400,400]
[null,"","","REMOVE TWIN ARM LIGHT STANDARD","- DISPOSE",4,515,2060]
[null,"","","ROADWAY LIGHT STANDARD LUMIN-","AIRE - 185W LED",21,875,18375]
[null,"5325600000-E","6\" WATER LINE","","",60,104.17,6250.2]
[null,"5325800000-E","8\" WATER LINE","","",156,73.9583333333333,11537.5]
[null,"5326200000-E","12\" WATER LINE","","",524,144.667061068702,75805.539999999994]
[null,"5327000000-E","20\" WATER LINE","","",2012,214.59,431755.08]
[null,"5328000000-E","30\" WATER LINE","","",55,432.3,23776.5]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",31235,8.7998463262365902,274863.2]
[null,"5540000000-E","6\" VALVE","","",3,1875.02,5625.06]
[null,"5546000000-E","8\" VALVE","","",4,2398.46,9593.84]
[null,"5558000000-E","12\" VALVE","","",5,4708.3440000000001,23541.72]
[null,"5559000000-E","20\" VALVE","","",5,20828.43,104142.15]
[null,"5571000000-E","**\" TAPPING SLEEVE & VALVE","(2\")","",1,7500,7500]
[null,"5589200000-E","2\" AIR RELEASE VALVE","","",1,27708.73,27708.73]
[null,"5600000000-E","**\" BLOW OFF","(1-1/2\")","",1,3125.05,3125.05]
[null,"5648000000-N","RELOCATE WATER METER","","",10,2937.5140000000001,29375.14]
[null,"5649000000-N","RECONNECT WATER METER","","",2,2000,4000]
[null,"5653100000-E","RELC **\" DCV BACKFLOW PREVNT A","(1\")","",3,3250,9750]
[null,"","","(2\")","",3,3500,10500]
[null,"5666000000-N","FIRE HYDRANT","","",5,4531.32,22656.6]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",4,3927.1025,15708.41]
[null,"5673000000-E","FIRE HYDRANT LEG","","",208,115.384615384615,24000]
[null,"5679400000-E","20\" LINE STOP","","",4,20312.8,81251.199999999997]
[null,"5686000000-E","**\" H2O SERVICE LINE","(1\")","",70,60,4200]
[null,"","","(2\")","",95,65,6175]
[null,"5686500000-E","WATER SERVICE LINE","","",28,52.08,1458.24]
[null,"5691000000-E","**\" SANITARY GRAVITY SEWER","(36\")","",1848,505.22,933646.56]
[null,"5691200000-E","6\" SANITARY GRAVITY SEWER","","",10,300,3000]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",634,210.52798107255501,133474.74]
[null,"5768000000-N","SANITARY SEWER CLEAN-OUT","","",2,3645.89,7291.78]
[null,"5768500000-E","SEWER SERVICE LINE","","",50,62.5,3125]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",870,12.5,10875]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",5,6008.3519999999999,30041.759999999998]
[null,"5776000000-E","5' DIA UTILITY MANHOLE","","",3,4140.68,12422.04]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",8,234.38,1875.04]
[null,"5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",6,338.55,2031.3]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",350,18.529599999999999,6485.36]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",232,8.33,1932.56]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",394,12.5,4925]
[null,"5810000000-E","ABANDON 16\" UTILITY PIPE","","",1507,14.58,21972.06]
[null,"5812000000-E","ABANDON 20\" UTILITY PIPE","","",1738,22.92,39834.959999999999]
[null,"5814000000-E","ABANDON 30\" UTILITY PIPE","","",1689,26.04,43981.56]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",5,729.18,3645.9]
[null,"5816000000-N","ABANDON UTILITY MANHOLE","","",6,1041.68,6250.08]
[null,"5828000000-N","REMOVE UTILITY MANHOLE","","",2,4500,9000]
[null,"5835000000-E","**\" ENCASEMENT PIPE","(60\")","",1040,1143.77,1189520.8]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",340,133.34,45335.6]
[null,"5836400000-E","36\" ENCASEMENT PIPE","","",400,286.45999999999998,114584]
[null,"5872500000-E","BORE & JACK **\"","(36\")","",225,807.3,181642.5]
[null,"5872700000-E","TUNNELING **\"","(60\")","",670,1895.86,1270226.2]
[null,"5882000000-N","GENERIC UTILITY ITEM (EA)","12\" INSERT VALVE","",2,25000,50000]
[null,"","","6' DIA POLYMER CONCRETE UTILI-","TY MANHOLE",9,30000.43,270003.87]
[null,"","","8\" PRESSURE RELIEF VALVE IN 7'","DIA MANHOLE",1,35417.18,35417.18]
[null,"","","CONCRETE ANTI-SEEP PIPE       COLLARS","",6,1770.86,10625.16]
[null,"5888000000-E","GENERIC UTILITY ITEM (LF)","POLYMER CONCRETE UTILITY MAN-","HOLE WALL, 6' DIA",92,416.67,38333.64]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",56810,2.2779123393768699,129408.2]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",3630,44.159779614325103,160300]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",16400,43.666082317073197,716123.75]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",8765,38.3654877353109,336273.5]
[null,"6015000000-E","TEMPORARY MULCHING","","",140.5,921.78170818505305,129510.33]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",7200,2.7993055555555602,20155]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",38,782.18263157894705,29722.94]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",2510,19.844721115537901,49810.25]
[null,"6029000000-E","SAFETY FENCE","","",7200,2.5988888888888901,18712]
[null,"6030000000-E","SILT EXCAVATION","","",70340,6.0150184816605101,423096.4]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",131500,1.4485368821292799,190482.6]
[null,"6037000000-E","COIR FIBER MAT","","",550,8.2763636363636408,4552]
[null,"6038000000-E","PERM SOIL REINF MAT","","",8750,4,35000]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",14800,3.87936486486486,57414.6]
[null,"6045000000-E","**\" TEMPORARY PIPE","(36\")","",170,95,16150]
[null,"6069000000-E","STILLING BASINS","","",777,8,6216]
[null,"6071010000-E","WATTLE","","",270,7.75,2092.5]
[null,"6071012000-E","COIR FIBER WATTLE","","",4230,8.2497163120567407,34896.300000000003]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",192,8.33,1599.36]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",4340,7.8383870967741904,34018.6]
[null,"6071030000-E","COIR FIBER BAFFLE","","",13530,4.0605949741315603,54939.85]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",10,1284.01,12840.1]
[null,"","","(2\")","",10,1458.35,14583.5]
[null,"","","(2-1/2\")","",3,1770.86,5312.58]
[null,"","","(3\")","",7,1875.03,13125.21]
[null,"6084000000-E","SEEDING AND MULCHING","","",127,2010.7286614173199,255362.54]
[null,"6087000000-E","MOWING","","",113,138.79044247787601,15683.32]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",1450,10.393448275862101,15070.5]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",5,776.36400000000003,3881.82]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",3050,4.8538524590163901,14804.25]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",91.25,835.15167123287699,76207.59]
[null,"6111000000-E","IMPERVIOUS DIKE","","",895,25,22375]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",80,145.22125,11617.7]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",250,144.32300000000001,36080.75]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",44,640.19545454545505,28168.6]
[null,"6120000000-E","CULVERT DIVERSION CHANNEL","","",3016,15,45240]
[null,"6123000000-E","REFORESTATION","","",0.1,15000,1500]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",0.5,7000,3500]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",53,147.088679245283,7795.7]
[null,"","","","DEVICE CLEANOUT",124,166.5,20646]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",47,982.60638297872299,46182.5]
[null,"7060000000-E","SIGNAL CABLE","","",34300,2.29142857142857,78596]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",158,730.21835443038003,115374.5]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",26,895.32692307692298,23278.5]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",10,1337.8,13378]
[null,"7216000000-N","MODIFY EXT VEHIC SIGNL HD","","",4,330,1320]
[null,"7229000000-N","APS DETECTOR STATION","","",8,808,6464]
[null,"7230000000-N","CENT CONT UNIT APS DETECT STA","","",1,1818,1818]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",925,2.83,2617.75]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",6350,3.4145669291338598,21682.5]
[null,"7279000000-E","TRACER WIRE","","",2500,0.76,1900]
[null,"7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",300,28.28,8484]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",3025,6.6284297520661202,20051]
[null,"","","(2, 2\")","",1835,8.4311716621253403,15471.2]
[null,"","","(3, 2\")","",100,18.18,1818]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",380,19.511842105263199,7414.5]
[null,"","","(2, 2\")","",1525,17.544262295082,26755]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",56,306.205357142857,17147.5]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",38,830.05263157894694,31542]
[null,"7360000000-N","WOOD POLE","","",26,1034.23076923077,26890]
[null,"7372000000-N","GUY ASSEMBLY","","",57,620.82456140350905,35387]
[null,"7396000000-E","1/2\" RISER WITH WEATHERHEAD","","",2,323.2,646.4]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",8,361.5625,2892.5]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",28,595.18928571428603,16665.3]
[null,"7430000000-N","HEAT SHRINK TUB KIT","","",5,101,505]
[null,"7432000000-E","2\" RISER WITH TUBING","","",3,707,2121]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",26317,8.6515431090169894,227682.66]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",39675,1.1026275992438599,43746.75]
[null,"7481000000-N","SITE SURVEY","","",8,1055.53125,8444.25]
[null,"7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",6,860,5160]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",22,3477.7272727272698,76510]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",7,6042.8571428571404,42300]
[null,"7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",26,304.696153846154,7922.1]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(12)","",5425,2.42,13128.5]
[null,"7528000000-E","DROP CABLE","","",450,2.88,1296]
[null,"7540000000-N","SPLICE ENCLOSURE","","",5,2121,10605]
[null,"7541000000-N","MOD SPLICE ENCLOSURE","","",3,858.5,2575.5]
[null,"7552000000-N","INTERCONNECT CENTER","","",6,1504.9,9029.4]
[null,"7566000000-N","DELINEATOR MARKER","","",11,65,715]
[null,"7575142000-N","900MHZ SPECTRUM RADIO","","",3,5750,17250]
[null,"7575142010-N","900MHZ SER/ETH SPEC RADIO","","",8,4368.25,34946]
[null,"7575142060-N","MOD RADIO INSTALL","","",1,650.44000000000005,650.44000000000005]
[null,"7575160000-E","REM EXT COMM CABLE","","",3175,1.01,3206.75]
[null,"7575180000-N","CABLE TRANSFER","","",1,404,404]
[null,"7576000000-N","METAL STRAIN SIGNAL POLE","","",20,8080,161600]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",4,17300,69200]
[null,"7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,34250,68500]
[null,"7613000000-N","SOIL TEST","","",26,747.76923076923094,19442]
[null,"7614100000-E","DRILLED PIER FOUND","","",176,916.06818181818198,161228]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",6,65,390]
[null,"7636000000-N","SIGN FOR SIGNALS","","",97,380.05948453608198,36865.769999999997]
[null,"7642100000-N","TYPE I POST W/ FOUNDATION","","",20,1313,26260]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",31,1974.03225806452,61195]
[null,"7648000000-N","RELOCATE EXISTING SIGN","","",1,303,303]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",11,1275.3636363636399,14029]
[null,"7686000000-N","CONDUIT ENTR INTO EXT FOUND","","",10,757.5,7575]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070LX, BASE MOUNTED)","",12,13321,159852]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",109,107.238532110092,11689]
[null,"7901000000-N","CABINET BASE EXTENDER","","",12,510.1875,6122.25]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,3000,3000]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",1,1212,1212]
[null,"7972000000-N","METAL POLE REMOVAL","","",1,1010,1010]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","ETHERNET EDGE SWITCH","",9,1515,13635]
[null,"","","JUNCTION BOX MARKER","",6,171.7,1030.2]
[null,"","","REMOVE RADIO INSTALLATION","",8,656.5,5252]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","BACK PULL FIBER OPTIC CABLE","",425,2.78,1181.5]
[null,"8035000000-N","REMV EXIST STR **********","(19+56.99 -L-)","",1,120000,120000]
[null,"","","(27+02.26 -L-)","",1,125000,125000]
[null,"","","(41+39.51 -Y-)","",1,155938.01999999999,155938.01999999999]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",2,3275,6550]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 19+56.99 -L-)","",1,75175,75175]
[null,"","","(1, 41+39.51 -Y-)","",1,53490.21,53490.21]
[null,"8105540000-E","3'-6\" DRILLD PIER IN SOIL","","",65,1100,71500]
[null,"8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",124,1100,136400]
[null,"8112730000-N","PDA TESTING","","",4,2708.75,10835]
[null,"8113000000-N","SID INSPECTIONS","","",3,600,1800]
[null,"8114000000-N","SPT TESTING","","",6,600,3600]
[null,"8115000000-N","CSL TESTING","","",3,1500,4500]
[null,"8126000000-N","CULV EXCAV @ ************","(46+07.79 -Y-)","",1,75000,75000]
[null,"","","(56+34.85 -L-)","",1,130000,130000]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",1937,55,106535]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",42449,49.169055808146197,2087177.25]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",98734.6,0.87344416243140999,86239.16]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",873.9,1090.6833962696001,953148.22]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",4445.8,335,1489343]
[null,"8210000000-N","BRG APPR SLAB ***********","(19+56.99 -L-)","",1,33850,33850]
[null,"","","(27+02.26 -L-)","",1,55000,55000]
[null,"","","(41+39.51 -Y-)","",1,179585.72,179585.72]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",139103,1.3493599706692201,187700.02]
[null,"8224000000-E","EPOXY COAT REINF STL BRDG","","",911,1.75,1594.25]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",11448,2.4964544025157198,28579.41]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",535871,1.5,803806.5]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",1694,307.56,521006.64]
[null,"8274000000-E","63\" MOD PRESTR CONC GIRDR","","",808.67,337.08999962902101,272594.57]
[null,"8280000000-E","STRUCTURAL STEEL","","",441500,3.17100792751982,1400000]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",100,1242.2456,124224.56]
[null,"","","(HP 14 X 73)","",36,514.59,18525.240000000002]
[null,"8364000000-E","HP12X53 PILES","","",3831,46.050031323414302,176417.67]
[null,"8384000000-E","HP14X73 PILES","","",2472,63.08,155933.76000000001]
[null,"8391000000-N","STEEL PILE POINTS","","",100,197.25,19725]
[null,"8482000000-E","THREE BAR METAL RAIL","","",422.5,150,63375]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",761.2,114.213189700473,86939.08]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",410.6,100.560009741841,41289.94]
[null,"8524000000-E","**\" CHAIN LINK FENCE","(104\")","",427.83,152,65030.16]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",741.2,99.294306529951399,73596.94]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",4.2,600,2520]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",3,43264.0133333333,129792.04]
[null,"8660000000-E","CONCRETE REPAIRS","","",1.2,1660,1992]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",91.4,1062.2538293216601,97090]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",1557.5,138.083467094703,215065]
[null,"8692000000-N","FOAM JOINT SEALS","","",2,30212.5,60425]
[null,"8706000000-N","EXPANSION JOINT SEALS","","",1,166554.37,166554.37]
[null,"8727000000-N","ELEC CONDUIT SYS SIGNAL ******","(27+02.26 -L-)","",1,55550,55550]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",8145,74.209533456108005,604436.65]
[null,"","","(2)","",7981,72.062255356471596,575128.86]
[null,"8802040000-E","CIP GRAVITY RETAINING WALLS","","",325,91.26,29659.5]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FOAM JOINT SEALS FOR PRESERVA-TION","",712,75,53400]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","POLYESTER POLYMER CONCRETE    MATERIALS","",244.5,2653.9877300613498,648900]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","EPOXY COATING","",3137.8,18.5672764357193,58260.4]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","CONCRETE DECK REPAIR FOR","POLYESTER POLYMER CONCRETE OVERLAY",4.2,150,630]
[null,"","","PLACING & FINISHING POLYESTER","POLYMER CONCRETE OVERLAY",2234.5,56,125132]
[null,"","","PLACING & FINISHING POLYMER","CONCRETE OVERLAY",5242,28,146776]
[null,"","","SCARIFYING BRIDGE DECK","",6706.5,18.126519048684099,121565.5]
[null,"","","SHOTBLASTING BRIDGE DECK","",7476.5,5,37382.5]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","TYPE I BRIDGE JACKING BRIDGE  NO 780132","",6,7500,45000]

{"sheet":"ITEMS - DIV 08","index":10,"n_rows":149,"n_cols":8,"rows_kept":149,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 08"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",21,146161.502857143,3069391.56]
[null,"0001000000-E","CLEARING & GRUBBING","","",130,51578.137028483397,6700000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",5,7000,35000]
[null,"0015000000-N","SEALING ABANDONED WELLS","","",21,3000,63000]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",17500,3,52500]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",1165,75.064377682403403,87450]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",421.6,1984.40372390892,836624.61]
[null,"1260000000-E","AGGREGATE SHOULDER BORROW","","",66572.25,21.037546274911801,1400516.79]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",1601611,1.3452954369069601,2154639.9700000002]
[null,"","","(1-1/4\")","",36512,1.06435254163015,38861.64]
[null,"","","(2\")","",24962,2.8720242769008899,71691.47]
[null,"","","(2-1/2\")","",59767,2.15,128499.05]
[null,"","","(3\")","",37834,1.79132526299096,67773]
[null,"","","(3-1/2\")","",2322,3.5,8127]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",36719,2.3859982570331399,87611.47]
[null,"","","(0\" TO 1-1/4\")","",520,8,4160]
[null,"","","(0\" TO 3\")","",37883,1.75,66295.25]
[null,"","","(0\" TO 4-3/4\")","",640,6,3840]
[null,"1330000000-E","INCIDENTAL MILLING","","",158044,5.7713131153349702,912121.41]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",6354,57.477101038715801,365209.5]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",14803,45.579409579139401,674712]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",312797,47.108960699751002,14735541.58]
[null,"1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",625,41.76,26100]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",99697,45.283798409179802,4514658.8499999996]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",63314,51.789762137915801,3279017]
[null,"1526000000-E","ASP CONC SURF CRS S4.75A","","",4154,55.808979297063097,231830.5]
[null,"1575000000-E","ASP FOR PLANT MIX","","",28269,433.13066185574303,12244170.68]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",4561,609.34992326244196,2779245]
[null,"1662000000-E","OG ASP FRICT FC-1 MOD","","",9347,71,663637]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",500,240,120000]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",22475,124.144693214683,2790151.98]
[null,"1775500000-E","AST, MAT COAT, #*** STONE","(67)","",43243,0.55000000000000004,23783.65]
[null,"","","(67)","",216189,0.77736767365591997,168058.34]
[null,"","","(78M)","",54505,0.65,35428.25]
[null,"1803500000-E","AST, DOUBLE SEAL","","",27244,1.0792596535016901,29403.35]
[null,"1838000000-E","EMULSION FOR AST","","",138689,1.87043240631917,259408.4]
[null,"1838500000-N","VACUUM TRUCK","","",19,2007.15789473684,38136]
[null,"1839140000-E","ULTRATHIN BOND WEAR CRS","","",7370,110,810700]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",356777,0.16741608904161001,59730.21]
[null,"1881000000-E","GENERIC PAVING ITEM (LF)","12\" MILLED RUMBLE STRIPS","(ASPHALT CONCRETE)",33317,0.18,5997.06]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","LATEX MODIFIED MICROSURFACING,","TYPE III",68228,2.93,199908.04]
[null,"2143000000-E","BLOTTING SAND","","",75,58.4613333333333,4384.6000000000004]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",250,56.6,14150]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",625,66.590400000000002,41619]
[null,"2600000000-N","RETROFIT EXT CURB RAMPS","","",60,816.66666666666697,49000]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",9,2233.3333333333298,20100]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",50,70,3500]
[null,"2613000000-N","REM & REP CURB RAMPS","","",115,3298.6956521739098,379350]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","REMOVE AND REPLACE 2'-6\" CURB AND GUTTER","",100,75,7500]
[null,"2759000000-N","GENERIC PAVING ITEM (EA)","REMOVE CURB RAMP","",3,2950,8850]
[null,"2815000000-N","ADJ DROP INLETS","","",2,800,1600]
[null,"2830000000-N","ADJ MANHOLES","","",250,894.56039999999996,223640.1]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",188,801.69468085106405,150718.6]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",1000,6,6000]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",62,30,1860]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",18,40,720]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",5850,4.5,26325]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",304,6.9,2097.6]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",40579,5.9951684368762201,243277.94]
[null,"4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",10,2990,29900]
[null,"4447000000-E","PED CHANNEL DEVICES","","",230,36.956521739130402,8500]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",19,70137.61,1332614.5900000001]
[null,"4510000000-N","LAW ENFORCEMENT","","",3292,50.606925880923399,166598]
[null,"4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","TRAFFIC CONTROL","",1,800000,800000]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","CONNECTED LANE CLOSURE DEVICE","",4,1280,5120]
[null,"","","RAMP/LOOP CLOSURE","",8,1200,9600]
[null,"","","SINGLE LANE CLOSURE","",148,700,103600]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",1863398,0.53273017895263997,992688.35]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",360704,0.85660885379702001,308982.24]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",9164,2.6070875163684,23891.35]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",20148,2.4795791145523101,49958.559999999998]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",290,86.2068965517241,25000]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",1255,110.718725099602,138952]
[null,"4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",66,327.27272727272702,21600]
[null,"4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",570,3,1710]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",1579758,0.13584336968067001,214599.65]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",276892,0.16428614766767999,45489.52]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",13906,0.46858909823097999,6516.2]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",15974,0.73585388756729997,11754.53]
[null,"4830000000-E","PAINT PVT MKGS LINES 16\"","","",470,2.68085106382979,1260]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",6249,2.6468714994399098,16540.3]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",184,46.841304347826103,8618.7999999999993]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",813,39.7514760147602,32317.95]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",9041,1.00713416657449,9105.5]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",51556,0.29681938086741,15302.82]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",73,3.9691780821917799,289.75]
[null,"4865000000-E","LINE REMOVAL 12\" WIDE","","",1966,1,1966]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",12,75,900]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",636,10.288679245282999,6543.6]
[null,"","","","LINES (24\", 90 MILS)",7034,10.2560776229741,72141.25]
[null,"","","","LINES (24', 90 MILS)",1127,8.5,9579.5]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","IN LANE ROUTE SHIELDS","",6,2000,12000]
[null,"","","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",5094,37.7540243423636,192319]
[null,"","","","PAVEMENT MARKERS",1590,36,57240]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",38,10,380]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",7063,28.338949454905901,200158]
[null,"5255000000-N","PORTABLE LIGHTING","","",7,11471.5714285714,80301]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",350175,1.75062468765617,613025]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",3500,43,150500]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",27800,34,945200]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",13200,31,409200]
[null,"6015000000-E","TEMPORARY MULCHING","","",1138,650,739700]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",43900,1.66,72874]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",221,900,198900]
[null,"6029000000-E","SAFETY FENCE","","",200,5,1000]
[null,"6030000000-E","SILT EXCAVATION","","",180100,0.01,1801]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",253220,1.33,336782.6]
[null,"6037000000-E","COIR FIBER MAT","","",1850,6,11100]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",25300,2.5,63250]
[null,"6045000000-E","**\" TEMPORARY PIPE","(15\")","",1100,60,66000]
[null,"","","(18\")","",575,80,46000]
[null,"","","(24\")","",350,115,40250]
[null,"","","(30\")","",100,140,14000]
[null,"","","(36\")","",50,150,7500]
[null,"","","(42\")","",125,190,23750]
[null,"","","(54\")","",40,325,13000]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",2,2000,4000]
[null,"6071012000-E","COIR FIBER WATTLE","","",18600,9,167400]
[null,"6071013000-E","WATTLE BARRIER","","",650,12,7800]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",19125,5,95625]
[null,"6071030000-E","COIR FIBER BAFFLE","","",31000,5,155000]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",71,1800,127800]
[null,"","","(2\")","",30,2000,60000]
[null,"","","(2-1/2\")","",13,2150,27950]
[null,"","","(3\")","",5,2700,13500]
[null,"","","(4\")","",4,3400,13600]
[null,"6084000000-E","SEEDING AND MULCHING","","",650.65,1876.8731268731301,1221187.5]
[null,"6087000000-E","MOWING","","",500,100,50000]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",11500,8,92000]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",32,1045,33440]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",16075,8,128600]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",485,790,383150]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",10,135,1350]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",156,416.82692307692298,65025]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","SIGN","",88,71.25,6270]
[null,"6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","REMOVAL OF JAPANESE KNOTWEED","",1,25000,25000]
[null,"6147000000-E","GENERIC EROSION CONTROL ITEM (LF)","SAFETY FENCE FOR MONITORING","WELL PROTECTION",880,6.5,5720]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",40960,6.3460595703124998,259934.6]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",25600,1.6910937500000001,43292]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",1,136000,136000]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",1.8,2125,3825]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FOAM JOINT SEALS FOR PRESERVA-TION","",188,90.43,17000.84]
[null,"","","POURABLE SILICONE JOINT","SEALANT",98.2,45,4419]
[null,"8882000000-E","GENERIC STRUCTURE ITEM (CF)","ELASTOMERIC CONCRETE FOR","PRESERVATION",47.2,216.1,10199.92]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","BRIDGE JOINT DEMOLITION","",188,36.17,6799.96]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","SHOTBLASTING BRIDGE DECK","",1286,10.09,12975.74]
[null,"","","SILANE DECK TREATMENT","",1286,28.77,36998.22]

{"sheet":"ITEMS - DIV 09","index":11,"n_rows":753,"n_cols":8,"rows_kept":753,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 09"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",9,1918100,17262900]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",5,1098650,5493250]
[null,"0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","DRILLED ORIFICE PLATE AND     TRASH RACK","",1,555,555]
[null,"","","POLYMER CONCRETE CLEANOUT     BOXES","",1,975,975]
[null,"0000920000-E","GENERIC MISCELLANEOUS ITEM (CY)","BIOSWALE FILTRATION MEDIA","",90,100,9000]
[null,"0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","BIOSWALE UNDERDRAIN PIPE","",300,25,7500]
[null,"0000960000-E","GENERIC MISCELLANEOUS ITEM (SY)","POLYPROPYLENE NONWOVEN GEO-","TEXTILE FABRIC",250,4,1000]
[null,"0000995000-E","GENERIC MISCELLANEOUS ITEM (TON)","NO 57 STONE, WASHED","",50,37,1850]
[null,"0001000000-E","CLEARING & GRUBBING","","",10,1569743.996,15697439.960000001]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",7,8324.9500000000007,58274.65]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",3414300,4.9933822452625698,17048905]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(22+26.35 -Y1B-)","",1,30500.41,30500.41]
[null,"","","(23+43.03 -Y16-)","",1,30689.69,30689.69]
[null,"","","(45+22.65 -EBL-)","",1,25000,25000]
[null,"","","(47+28.33 -Y15REV-)","",1,91890.66,91890.66]
[null,"","","(47+63.62 -Y15FLYBD-)","",1,42821.42,42821.42]
[null,"","","(58+33.94 -Y15FLYCA-)","",1,52200.66,52200.66]
[null,"","","(60+66.06 -Y15FLYAC-)","",1,46435.4,46435.4]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(18+27.98 -L-)","",1,53500,53500]
[null,"","","(30+67.66 -Y4-)","",1,123127.96,123127.96]
[null,"","","(61+02.86 -L- LT)","",1,79900,79900]
[null,"","","(61+02.86 -L- RT)","",1,79900,79900]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",12725,10.5655206286837,134446.25]
[null,"0043000000-N","GRADING","","",2,317163.09999999998,634326.19999999995]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",1,1,1]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",1221,18.398034398034401,22464]
[null,"0106000000-E","BORROW EXCAVATION","","",25147,23.9321589056349,601822]
[null,"0127000000-N","EMBM'T SETTLEMENT GAUGE","","",4,1000,4000]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",164380,12.1060968487651,1990000.2]
[null,"0141000000-E","BERM DITCH CONSTRUCTION","","",7030,9.9603413940255994,70021.2]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",87037,8.5686627526224495,745790.7]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",75947,19.671626265685301,1494001]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",23090,5.0097964486790802,115676.2]
[null,"0185000000-E","BREAKING OF EXT CONC PVMT","","",9630,6.07,58454.1]
[null,"0192000000-N","PROOF ROLLING","","",140,467.857142857143,65500]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",30250,59.839471074380199,1810144]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",13525,33.702569316081302,455827.25]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",89632,2.9999414271688698,268890.75]
[null,"0199000000-E","TEMPORARY SHORING","","",1605,46.5,74632.5]
[null,"0223000000-E","ROCK PLATING","","",3750,65.61,246037.5]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",600,139.26666666666699,83560]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",8996,57.008551578479299,512848.93]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",32049,3.1225217635495599,100073.7]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",1548,60.808759689922503,94131.96]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",600,70.299733333333293,42179.839999999997]
[null,"0348000000-E","**\" SIDE DRAIN PIPE ELBOW","(8\")","",3,250,750]
[null,"0354000000-E","***\" RC PIPE CULV *****","(42\", V)","",362,390.45,141342.9]
[null,"","","(54\", V)","",292,572.66999999999996,167219.64000000001]
[null,"","","(60\", V)","",620,645.54999999999995,400241]
[null,"0360000000-E","12\" RC PIPE CULV III","","",124,52.06,6455.44]
[null,"0366000000-E","15\" RC PIPE CULV III","","",10160,54.113598425196798,549794.16]
[null,"0372000000-E","18\" RC PIPE CULV III","","",13152,68.064762773722606,895187.76]
[null,"0378000000-E","24\" RC PIPE CULV III","","",6656,92.690925480769195,616950.80000000005]
[null,"0384000000-E","30\" RC PIPE CULV III","","",3838,124.95,479558.1]
[null,"0390000000-E","36\" RC PIPE CULV III","","",2832,187.42,530773.43999999994]
[null,"0396000000-E","42\" RC PIPE CULV III","","",1756,255.1,447955.6]
[null,"0402000000-E","48\" RC PIPE CULV III","","",704,312.36,219901.44]
[null,"0408000000-E","54\" RC PIPE CULV III","","",212,520.6,110367.2]
[null,"0414000000-E","60\" RC PIPE CULV III","","",848,568.52528301886798,482109.44]
[null,"0426000000-E","72\" RC PIPE CULV III","","",56,1041.21,58307.76]
[null,"0448000000-E","***\" RCP CULV CLASS IV","(48\")","",764,246.93413612565399,188657.68]
[null,"","","(54\")","",292,572.66999999999996,167219.64000000001]
[null,"","","(60\")","",360,624.73,224902.8]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",10528,62.828647416413403,661460]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",5948,78.448197713517104,466609.88]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",1868,104.418286937901,195053.36]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",452,124.417168141593,56236.56]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",908,190.63718061674001,173098.56]
[null,"0448700000-E","42\" RCP CULV CLASS IV","","",748,226.630481283422,169519.6]
[null,"0576000000-E","**\" CS PIPE CULV *****\"","(36\", 0.079\")","",164,260.3,42689.2]
[null,"","","(42\", 0.109\")","",80,343.6,27488]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",2582,92.920224632068198,239920.02]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",1432,99.752709497206695,142845.88]
[null,"0594000000-E","24\" CS PIPE CULV 0.064\"","","",892,113.952421524664,101645.56]
[null,"0600000000-E","30\" CS PIPE CULV 0.079\"","","",664,221.16716867469901,146855]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",94,523.26723404255301,49187.12]
[null,"","","(18\", 0.064\")","",34,583.00352941176504,19822.12]
[null,"","","(24\", 0.064\")","",20,624.73,12494.6]
[null,"","","(30\", 0.079\")","",18,1041.21,18741.78]
[null,"","","(36\", 0.079\")","",2,1041.21,2082.42]
[null,"","","(42\", 0.109\")","",2,1561.82,3123.64]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(18\", 0.250\")","",76,1251.27,95096.52]
[null,"","","(20\", 0.500\")","",24,668.12,16034.88]
[null,"","","(24\", 0.375\")","",54,104.12,5622.48]
[null,"","","(30\", 0.375\")","",102,130.15,13275.3]
[null,"","","(42\", 0.500\")","",192,156.18,29986.560000000001]
[null,"","","(48\", 0.500\")","",114,182.21,20771.939999999999]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(18\", 0.250\")","",76,1,76]
[null,"","","(20\", 0.500\")","",52,1765.06,91783.12]
[null,"","","(24\", 0.375\")","",54,156.18,8433.7199999999993]
[null,"","","(30\", 0.375\")","",102,182.21,18585.419999999998]
[null,"","","(42\", 0.500\")","",192,208.24,39982.080000000002]
[null,"","","(48\", 0.500\")","",114,260.3,29674.2]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","60\" PIPE REHABILITATION CIPP  LINER","",212,562.76,119305.12]
[null,"","","PRE INSTALLATION INSPECTION","",212,30.95,6561.4]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","DE-WATERING","",1,15265.13,15265.13]
[null,"0995000000-E","PIPE REMOVAL","","",16869,16.265970715513699,274390.65999999997]
[null,"0996000000-N","PIPE CLEAN OUT","","",21,5861.3342857142898,123088.02]
[null,"1011000000-N","FINE GRADING","","",3,1613419.67666667,4840259.03]
[null,"1044000000-E","LIME TRTD SOIL (SLURRY)","","",16520,5.35,88382]
[null,"1066000000-E","LIME FOR LIME TREATED SOIL","","",200,293,58600]
[null,"1077000000-E","57 STONE","","",410,86.287560975609793,35377.9]
[null,"1099500000-E","SHALLOW UNDERCUT","","",11100,10.6873873873874,118630]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",106815,41.959738332631197,4481929.45]
[null,"1110000000-E","STABILIZER AGGREGATE","","",1000,38.44,38440]
[null,"1111000000-E","CLASS IV AGGREGATE STABILIZATION","","",9500,44.26,420470]
[null,"1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",190353,4.3116349624119401,820732.65]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",40290,39.302745098039203,1583507.6]
[null,"1165000000-E","PORT CEM FOR CEM TRTD BASE CRSE","","",315,215,67725]
[null,"1176000000-E","SOIL CEMENT BASE","","",16520,4.8099999999999996,79461.2]
[null,"1209000000-E","ASPHALT CURING SEAL","","",4960,3.44,17062.400000000001]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",5795,30.0912182916307,174378.61]
[null,"1231000000-E","SHOULDER BORROW","","",24437,13.472045259238,329216.37]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",151.32,2176.9230769230799,329412]
[null,"1264000000-E","DITCHING","","",15,21,315]
[null,"1275000000-E","PRIME COAT","","",8896,5.6524280575539603,50284]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",813617,1.4348525411833799,1167420.42]
[null,"","","(2\")","",7500,2.25,16875]
[null,"","","(3\")","",107127,3.9,417795.3]
[null,"","","(4\")","",12444,2.34,29118.959999999999]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",57743,2.26920579117815,131030.75]
[null,"","","(0\" TO 3\")","",1400,7.35,10290]
[null,"1330000000-E","INCIDENTAL MILLING","","",74975,4.6447315771923998,348238.75]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",163630,55.850944203385701,9138890]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",124193,55.806949667050503,6930832.5]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",143248,50.801248324583902,7277177.2199999997]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",96649,53.864529793376001,5205952.9400000004]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",25710,72,1851120]
[null,"1575000000-E","ASP FOR PLANT MIX","","",28739,511.27683635477899,14693585]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",1485,898.23232323232298,1333875]
[null,"1662000000-E","OG ASP FRICT FC-1 MOD","","",240,180,43200]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",2648,102.41878776435,271204.95]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",2520,140.972222222222,355250]
[null,"1735000000-E","REP JNT CONC PVT SLABS","","",1250,451.66,564575]
[null,"1736000000-E","SELECT MATERIAL, CLASS IV","","",50,1165.27,58263.5]
[null,"1775000000-E","AST, MAT COAT, #78M STONE","","",90867,0.98,89049.66]
[null,"1775500000-E","AST, MAT COAT, #*** STONE","(67M)","",146731,1.24,181946.44]
[null,"1814500000-E","AST, SINGLE SEAL","","",76279,0.6,45767.4]
[null,"1838000000-E","EMULSION FOR AST","","",102900,1.90441749271137,195964.56]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",156270,0.28846675625520002,45078.7]
[null,"1847000000-E","******\"PCC PVMT THRU LNS","(12\")","",132215,73.42,9707225.3000000007]
[null,"1858000000-E","******\"PCC PVMT RAMPS","(12\")","",9980,75.87,757182.6]
[null,"1869000000-E","******\"PCC PVMT MISC","(12\")","",3470,91.04,315908.8]
[null,"1880000000-E","GENERIC PAVING ITEM (TON)","SELECT MATERIAL, CLASS IV","",549,50,27450]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","7\" CONCRETE TRUCK APRON","",2040,82.75,168810]
[null,"","","7\" JOINTED CONCRETE TRUCK","APRON",380,90.77,34492.6]
[null,"","","8\" CONTINUOUSLY REINFORCED","CONCRETE PAVEMENT REPAIR",817,650,531050]
[null,"","","DIAMOND GRINDING PCC PAVEMENT","",45730,5.03,230021.9]
[null,"1913000000-E","CONC SHLD ADJ ******\"PVMT","(12\")","",75440,64.56,4870406.4000000004]
[null,"1924000000-N","FIELD LAB RENTAL, PCCP","","",1,925000,925000]
[null,"1925000000-E","MILL RUMBLE STRPS (CONC SHLDR)","","",60580,2.66590293826345,161500.4]
[null,"2000000000-N","RIGHT-OF-WAY MARKERS","","",325,129.58689230769201,42115.74]
[null,"2020000000-N","CONTROL-OF-ACCESS MARKERS","","",8,214,1712]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",7251.2,16.8976169461606,122528]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",21000,3.6458571428571398,76563]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",135,65,8775]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",3529.8,90.001711145107393,317688.03999999998]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",21800,19.453119266055101,424078]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",45,557.51066666666702,25087.98]
[null,"2077000000-E","6\" OUTLET PIPE","","",270,33.416444444444402,9022.44]
[null,"2099000000-E","SHOULDER DRAIN","","",22060,7.27,160376.20000000001]
[null,"2110000000-E","4\" SHOULDER DRAIN PIPE","","",22060,2.12,46767.199999999997]
[null,"2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",1780,16.98,30224.400000000001]
[null,"2132000000-N","CONC PAD SHLDR DRN OUTLET","","",40,626.26,25050.400000000001]
[null,"2143000000-E","BLOTTING SAND","","",40,35.75,1430]
[null,"2209000000-E","ENDWALLS","","",84.873999999999995,1910.67099465089,162166.29]
[null,"2220000000-E","REINFORCED ENDWALLS","","",50,2082.42,104121]
[null,"2253000000-E","PIPE COLLARS","","",30.526,1895.53167791391,57863]
[null,"2264000000-E","PIPE PLUGS","","",0.998,4316.8737474949903,4308.24]
[null,"2275000000-E","FLOWABLE FILL","","",102,690.72176470588204,70453.62]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",696,4028.6817528735601,2803962.5]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",104.24,3697.5094973138898,385428.39]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",788.8,802.94089756592302,633359.78]
[null,"2354000000-N","FRAME W/GRATE 840.22 STD","","",5,746.37199999999996,3731.86]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",28,787.41428571428605,22047.599999999999]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",157,759.24917197452203,119202.12]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",213,768.33173708920197,163654.66]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",6,754.8,4528.8]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",5,519.67999999999995,2598.4]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",18,908.39,16351.02]
[null,"","","(F)","",66,995.25818181818204,65687.039999999994]
[null,"","","(G)","",62,926.69,57454.78]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",58,735.42499999999995,42654.65]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",106,2773.8578301886801,294028.93]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",6,4750,28500]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","ENERGY DISSIPATOR BASIN","",1,4500,4500]
[null,"","","OUTLET CONTROL STUCTURE","",2,52060.47,104120.94]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",3290,29.75,97877.5]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",22470,32.567890520694299,731800.5]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",13369,50.420267035679601,674068.55]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",7610,48.4406701708279,368633.5]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",3870,81.987054263565895,317289.90000000002]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",44,5484.25,241307]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",1200,260.83,312996]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",540,110.25166666666701,59535.9]
[null,"2627000000-E","4\" CONC ISLAND COVER","","",6020,80,481600]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",3000,108.9975,326992.5]
[null,"2657000000-E","**\" MONO CONC MEDIAN (*****)","(8\", NON-MOUNTABLE)","",20,407.09,8141.8]
[null,"2703000000-E","CONC BARRIER TYPE ******","(III)","",2800,184.65,517020]
[null,"","","(IV)","",1500,114.84,172260]
[null,"","","(T)","",9670,143.15,1384260.5]
[null,"","","(T1)","",1850,176.65,326802.5]
[null,"","","(T2)","",2750,372.59,1024622.5]
[null,"2710000000-N","CONC BARRIER TRANS SECTN","","",11,23927.593636363599,263203.53000000003]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",18570,94.123004846526698,1747864.2]
[null,"2738000000-E","GENERIC PAVING ITEM (SY)","FILL AND CAP BEHIND BARRIER","",270,192,51840]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","2'-0\" MODIFIED VALLEY GUTTER","",230,92.65,21309.5]
[null,"","","DDI BARRIER","",710,365.48,259490.8]
[null,"","","MEDIAN HAZARD PROTECTION","",250,316.5,79125]
[null,"","","MODIFIED VALLEY GUTTER","",1100,27,29700]
[null,"2759000000-N","GENERIC PAVING ITEM (EA)","MEDIAN HAZARD PROTECTION","",4,51624.37,206497.48]
[null,"2800000000-N","ADJ CATCH BASINS","","",1,1015.79,1015.79]
[null,"2815000000-N","ADJ DROP INLETS","","",3,1356.0166666666701,4068.05]
[null,"2830000000-N","ADJ MANHOLES","","",159,884.56339622641497,140645.57999999999]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",193,814.30051813471505,157160]
[null,"2860000000-N","CONVERT CB TO JB","","",1,5206.05,5206.05]
[null,"2905000000-N","CONVERT DI TO JB","","",10,3688.8989999999999,36888.99]
[null,"2995000000-N","GENERIC DRAINAGE ITEM (EA)","CONVERT EXISTING OTCB TO      MEDIAN 2GI","",7,1798.67,12590.69]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",3,20500,61500]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",71225,26.799754299754301,1908812.5]
[null,"3045000000-E","SBGR SHOP CURVED","","",200,27,5400]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",40,17.502500000000001,700.1]
[null,"3180000000-N","GR ANCHOR TYPE **********","(B-77 MODIFIED)","",1,2900,2900]
[null,"3195000000-N","GR END TYPE AT-1","","",1,500,500]
[null,"3210000000-N","GR END TYPE CAT-1","","",62,1026.61290322581,63650]
[null,"3215000000-N","GR ANCHOR TYPE III","","",12,1900,22800]
[null,"3287000000-N","GR END TYPE TL-3","","",75,3138.6666666666702,235400]
[null,"3288000000-N","GR END TYPE TL-2","","",21,3152.38095238095,66200]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",45,2662.1111111111099,119795]
[null,"3345000000-E","REMOVE & RESET GUARDRAIL","","",10600,5.5,58300]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",20541,1.15722214108369,23770.5]
[null,"3365000000-E","REMOVE EXISTING GUIDERAIL","","",15390,2.5,38475]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",3050,9.8688524590163897,30100]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",4,1350,5400]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",11,2500,27500]
[null,"","","(TL-3)","",1,2500,2500]
[null,"3389400000-E","DBL FACED CABLE GUIDERAIL","","",1300,13,16900]
[null,"3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",5,100,500]
[null,"3389600000-N","CBL GUIDERAIL ANCH UNIT","","",1,4000,4000]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",54030,6.3935591338145503,345444]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",3386,31.769639692852898,107572]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",875,44.714285714285701,39125]
[null,"3536000000-E","CHN LK FENCE 48\" FABRIC","","",14790,6.3,93177]
[null,"3542000000-E","MET LINE PST 48\" CL FEN","","",1240,70,86800]
[null,"3548000000-E","MET TERM PST 48\" CL FEN","","",80,125,10000]
[null,"3559000000-E","** STRAND BW FENCE W/ POSTS","(5)","",3230,15,48450]
[null,"3564000000-E","SGL GATE **HIGH, **WIDE, **OPEN","(47\", 12', 12')","",6,3000,18000]
[null,"3595000000-E","RELAPPING GUARDRAIL","","",450,4,1800]
[null,"3628000000-E","RIP RAP, CLASS I","","",10050,54.217910447761199,544890]
[null,"3635000000-E","RIP RAP, CLASS II","","",776,66.473195876288699,51583.199999999997]
[null,"3642000000-E","RIP RAP, CLASS A","","",1810,92.816574585635394,167998]
[null,"3649000000-E","RIP RAP, CLASS B","","",5552,52.866950648414999,293517.31]
[null,"3651000000-E","BOULDERS","","",1040,130.67307692307699,135900]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",46365,3.2585872964520699,151084.4]
[null,"3659000000-N","PREFORMED SCOUR HOLES","","",11,6247.26,68719.86]
[null,"3678000000-E","GENERIC EROSION CONTROL ITEM (SF)","PRECAST GRAVITY RETAINING     WALLS","",850,75.400000000000006,64090]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(E)","",42,12,504]
[null,"4048000000-E","REINF CONC FOUNDTN","","",22,980.83636363636401,21578.400000000001]
[null,"4054000000-E","PLN CONC FOUNDTN","","",3,1018.56,3055.68]
[null,"4057000000-E","OVERHEAD FOOTING","","",727,321.64999999999998,233839.55]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",17813,7.74631505080559,137985.10999999999]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",5778,6.0345690550363402,34867.74]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",7063,8.6477898909811692,61079.34]
[null,"4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",14,107.22,1501.08]
[null,"4079000000-N","SUPPORT, BARR SMALL","","",2,500,1000]
[null,"4082000000-E","SUPPORT, WOOD","","",415,15,6225]
[null,"4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(155+88 -Y15-)","",1,117938.14,117938.14]
[null,"","","(160+00 -Y15-)","",1,102391.75,102391.75]
[null,"","","(160+85 -Y15-)","",1,102391.75,102391.75]
[null,"","","(17+50 -Y15REV-)","",1,101855.67,101855.67]
[null,"","","(20+87 -Y4-)","",1,192989.69,192989.69]
[null,"","","(24+50 -Y15-)","",1,101855.67,101855.67]
[null,"","","(26+00 -Y4-)","",1,160824.74,160824.74]
[null,"","","(26+37 -Y15FLYBD-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(29+41 -Y4-)","",1,84164.95,84164.95]
[null,"","","(31+94 -Y4-)","",1,84164.95,84164.95]
[null,"","","(32+00 -Y15-)","",1,92742.27,92742.27]
[null,"","","(32+00 -Y15FLYAC-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(34+68 -Y15FLYCA-)","",1,171546.39,171546.39]
[null,"","","(47+00 -Y15FLYAC-)","",1,83628.87,83628.87]
[null,"","","(50+46 -Y15-)","",1,160824.74,160824.74]
[null,"","","(52+00 -Y15FLYCA-)","",1,84701.03,84701.03]
[null,"","","(56+00 -Y15REV-)","",1,92206.19,92206.19]
[null,"","","(666+00 -L-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(686+00 -L-)","",1,109896.91,109896.91]
[null,"","","(702+30 -L-)","",1,167793.81,167793.81]
[null,"","","(706+00 -L-)","",1,102927.84,102927.84]
[null,"","","(737+50 -L- EB)","",1,102927.84,102927.84]
[null,"","","(737+50 -L- WB)","",1,134020.62,134020.62]
[null,"","","(757+00 -L-)","",1,92206.19,92206.19]
[null,"","","(76+25 -Y15FLYBD-)","",1,85237.11,85237.11]
[null,"","","(763+84 -L-)","",1,134020.62,134020.62]
[null,"","","(794+00 -L-)","",1,144742.26999999999,144742.26999999999]
[null,"","","(819+00 -L-)","",1,134020.62,134020.62]
[null,"","","(826+00 -L-)","",1,122226.8,122226.8]
[null,"","","(835+50 -L-)","",1,134020.62,134020.62]
[null,"","","(89+70 -Y15REV-)","",1,112577.32,112577.32]
[null,"","","(91+50 -Y15REV-)","",1,134020.62,134020.62]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",20,137.53700000000001,2750.74]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",372,75.677956989247306,28152.2]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",18,138.93,2500.7399999999998]
[null,"4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",56,10.72,600.32000000000005]
[null,"","","(B)","",29,10.72,310.88]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",26,713.24538461538498,18544.38]
[null,"","","(B)","",6,394.16,2364.96]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",12,160.83000000000001,1929.96]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(A)","",3,804.12,2412.36]
[null,"","","(E)","",2,337.5,675]
[null,"4138000000-N","DISPOSE SUPPORT, STL BM","","",6,536.08000000000004,3216.48]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",5,536.08000000000004,2680.4]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",143,5.8584615384615404,837.76]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",3,2,6]
[null,"4238000000-N","DISPOSE SIGN, D, E, F","","",1,10,10]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",4711,7.3544088303969399,34646.620000000003]
[null,"4402000000-E","HIGH VISIBILITY STAT SIGNS","","",2660,13.401142857142901,35647.040000000001]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",2311,15.566092600605799,35973.24]
[null,"4407000000-E","HIGH VISIBILITY PORT SIGNS","","",270,12.0284444444444,3247.68]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",1053,6.1052231718898398,6428.8]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",17008,5.1025252822201299,86783.75]
[null,"4415000000-N","FLASHING ARROW BOARD","","",23,2630.6,60503.8]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",29,9800.9655172413804,284228]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",401,34.314214463840401,13760]
[null,"4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",15,3940,59100]
[null,"4424000000-N","WZ PRESENCE LIGHTING","","",70,2420,169400]
[null,"4430000000-N","DRUMS","","",1739,58.421219091431901,101594.5]
[null,"4432000000-N","HIGH VISIBILITY DRUMS","","",960,86.931250000000006,83454]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",132,160.48560606060599,21184.1]
[null,"4435000000-N","CONES","","",219,40.133333333333297,8789.2000000000007]
[null,"4445000000-E","BARRICADES (TYPE III)","","",1784,20.873542600896901,37238.400000000001]
[null,"4447000000-E","PED CHANNEL DEVICES","","",69,44.260869565217398,3054]
[null,"4455000000-N","FLAGGER","","",407,415.77022113022099,169218.48]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",3,133000,399000]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",28,9638.0782142857206,269866.19]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",22,2871.48909090909,63172.76]
[null,"4480000000-N","TMA","","",21,19730.0952380952,414332]
[null,"4485000000-E","PORT CONC BARRIER","","",43181,36.4422845696024,1573614.29]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",14604,52.106107915639498,760957.6]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",60560,7.2167503302509903,437046.4]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",4536,20,90720]
[null,"4510000000-N","LAW ENFORCEMENT","","",929,60.1972335844995,55923.23]
[null,"4516000000-N","SKINNY DRUM","","",325,40,13000]
[null,"4570000000-E","TEMPORARY GLARE SCREEN","","",8297,15.201657225503199,126128.15]
[null,"4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","DYNAMIC ZIPPER MERGE SYSTEM","DEPLOYMENT",1,50000,50000]
[null,"4595000000-E","GENERIC TRAFFIC CONTROL ITEM (SF)","TEMPORARY TYPE A AND B SIGNS","",405,47,19035]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",9,172,1548]
[null,"","","CONNECTED LANE CLOSURE DEVICE","",10,2340,23400]
[null,"","","COVER AND RELOCATE GROUND","MOUNTED GUIDE SIGNS",1,1000,1000]
[null,"","","DYNAMIC ZIPPER MERGE SYSTEM","RELOCATION",3,2500,7500]
[null,"","","FLASHING BEACON AND DETECTION SYSTEM","",2,38496,76992]
[null,"","","HIGH VISIBILITY SKINNY DRUMS","",100,90,9000]
[null,"","","SIGNS, COVERING","",3,300,900]
[null,"","","SOLAR-POWERED FLASHING BEACON","",3,5000,15000]
[null,"4609000000-N","GENERIC TRAFFIC CONTROL ITEM (DAY)","DYNAMIC ZIPPER MERGE SYSTEM","",90,330,29700]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",3708,6.3212513484358102,23439.200000000001]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",1893091,0.46583959777950001,881876.75]
[null,"4687000000-E","THERMO PVT MKG LINES 4\"240","","",220,1.21,266.2]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",156846,0.75,117634.5]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",10854,2.05645107794362,22320.720000000001]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",18845,1.64502838949323,31000.560000000001]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",215,123.320930232558,26514]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",728,131.383653846154,95647.3]
[null,"4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",6,1725,10350]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",4928,2.5,12320]
[null,"","","(IV)","",7493,2.5,18732.5]
[null,"4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(IV)","",1646,7.7,12674.2]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(IV)","",360,4.5,1620]
[null,"4785000000-E","12\" COLD PLSTIC LINES TYPE **","(IV)","",1632,13.2,21542.400000000001]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",1186248,0.21012736797027001,249263.17]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",110318,0.27623397813592998,30473.58]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",20173,0.93575819164229002,18877.05]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",2539,1.1917132729421001,3025.76]
[null,"4830000000-E","PAINT PVT MKGS LINES 16\"","","",527,1.2707779886148001,669.7]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",7094,2.4268720045108498,17216.23]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",145,61.155862068965497,8867.6]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",759,66.111725955204193,50178.8]
[null,"4847400000-E","WZ PERF PVMT MKG LINES 4\"","","",36552,1.1000000000000001,40207.199999999997]
[null,"4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",268270,1.0900000000000001,292414.3]
[null,"4847600000-E","WZ PERF PVMT MKG LINES 12\"","","",12041,2.7285175649863,32854.080000000002]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",67171,1.6465863244554899,110602.85]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",297895,0.47972090837376002,142906.46]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",3425,1.97567883211679,6766.7]
[null,"4865000000-E","LINE REMOVAL 12\" WIDE","","",3969,3.4614638447971799,13738.55]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",519,8.2311560693641592,4271.97]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",66,70.560606060606105,4657]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES, 12\"","20 MILS (STANDARD GLASS BEADS)",2280,1.3,2964]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",13967,2.04,28492.68]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",8591,1.59759050168781,13724.9]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",4479,2.15,9629.85]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\"","20 MILS (STANDARD GLASS BEADS)",26650,0.85,22652.5]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",91399,0.78900710073414004,72114.460000000006]
[null,"","","","30 MILS (STANDARD GLASS BEADS)",138443,1.54,213202.22]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 8\",","30 MILS (STANDARD GLASS BEADS)",124,14.15,1754.6]
[null,"","","POLYUREA PAVEMENT MARKING     LINES,12\",","20 MILS (STANDARD GLASS BEADS)",2025,1.55,3138.75]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",427,6.38,2724.26]
[null,"","","","LINES (16\", 90MILS)",150,6,900]
[null,"","","","LINES (24\", 90 MILS)",3830,8.3969399477806803,32160.28]
[null,"","","","LINES (24\", 90MILS)",1077,9,9693]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",5807,45.603788531083197,264821.2]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",258,9.3255813953488396,2406]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",1724,37.731583526682101,65049.25]
[null,"5010000000-E","100' HIGH MOUNT STANDARD","","",3,30303.03,90909.09]
[null,"5020000000-N","PORTABLE DRIVE UNIT","","",1,3636.36,3636.36]
[null,"5025000000-E","HIGH MOUNT FOUNDATIONS","","",21,1111.1099999999999,23333.31]
[null,"5030000000-N","HM LUMINAIRE ************","(560W LED)","",18,1818.18,32727.24]
[null,"5050000000-N","LIT STD MTLT ************","(45' SA, 15' ARM)","",13,5050.51,65656.63]
[null,"","","(45' TA, 15' ARM)","",8,5454.55,43636.4]
[null,"5070000000-N","STD FOUNDAT ***********","(TYPE R1)","",34,932.26499999999999,31697.01]
[null,"","","(TYPE R2)","",4,994.44500000000005,3977.78]
[null,"5080000000-N","LITE STD LUM ************","(RDW, 185W LED)","",17,1200,20400]
[null,"","","(RDW, 285W LED)","",29,752.53,21823.37]
[null,"5120000000-N","SERVICE POLE ************","(30' CLASS 4)","",2,2443.4349999999999,4886.87]
[null,"5125000000-E","SERVICE LATERAL *********","(3 #1/0 USE)","",25,50,1250]
[null,"","","(3 1/0 USE)","",25,50.51,1262.75]
[null,"5145000000-N","LITE CNTRL RW************","(240/480 V)","",2,17213.384999999998,34426.769999999997]
[null,"5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",1010,10.5424752475248,10647.9]
[null,"5160000000-E","ELECT DUCT JA, SIZE *****","(3\")","",1500,19.904033333333299,29856.05]
[null,"","","(4\")","",820,22.896280487804901,18774.95]
[null,"5170000000-E","**-#8 W/G FEEDER CIRCUIT","(2)","",620,3.6480645161290299,2261.8000000000002]
[null,"5175000000-E","**-#6 W/G FEEDER CIRCUIT","(2)","",600,3.59,2154]
[null,"5180000000-E","**-#4 W/G FEEDER CIRCUIT","(2)","",190,4.29,815.1]
[null,"5205000000-E","**-#8 W/G FEEDR N *****\"","(2, 1.5\")","",8025,10.2888722741433,82568.2]
[null,"5210000000-E","**-#6 W/G FEEDR N *****\"","(2, 1.5\")","",3040,9.09,27633.599999999999]
[null,"5215000000-E","**-#4 W/G FEEDER N *****\"","(2, 1.5\")","",2635,10.86,28616.1]
[null,"5240000000-N","ELEC JB ************","(CS36)","",2,1455.3050000000001,2910.61]
[null,"","","(HM18)","",3,378.79,1136.3699999999999]
[null,"","","(IG18)","",32,668.82875000000001,21402.52]
[null,"","","(IG30)","",5,707.07,3535.35]
[null,"","","(LS18)","",36,598.64055555555603,21551.06]
[null,"","","(LS30)","",2,707.07,1414.14]
[null,"5252000000-N","UNDERPASS LUMINARIES *****","(TYPE WM, 70W MAX LED)","",6,800,4800]
[null,"5253000000-N","UNDERPASS CIRCUITRY *************","(UPL-1)","",1,11000,11000]
[null,"","","(UPL-2)","",1,11000,11000]
[null,"5255000000-N","PORTABLE LIGHTING","","",4,133968.9,535875.6]
[null,"5270000000-N","GENERIC LIGHTING ITEM (EA)","LIGHT STANDARD, 45' SA, 15'   ARM","",17,4575,77775]
[null,"5325000000-E","**\" WATER LINE","(36\")","",1303,917.59,1195619.77]
[null,"5325200000-E","2\" WATER LINE","","",560,41.102803571428602,23017.57]
[null,"5325600000-E","6\" WATER LINE","","",6300,123.60316666666699,778699.95]
[null,"5325800000-E","8\" WATER LINE","","",1377,87.329346405228804,120252.51]
[null,"5326200000-E","12\" WATER LINE","","",1883,113.03275092936801,212840.67]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",53010,15.9036200716846,843050.9]
[null,"5536000000-E","2\" VALVE","","",2,738.57,1477.14]
[null,"5540000000-E","6\" VALVE","","",50,2080.1149999999998,104005.75]
[null,"5546000000-E","8\" VALVE","","",2,2640.76,5281.52]
[null,"5558000000-E","12\" VALVE","","",3,3993.8933333333298,11981.68]
[null,"5571600000-E","6\" TAPPING SLEEVE & VALVE","","",1,4992.96,4992.96]
[null,"5600000000-E","**\" BLOW OFF","(3/4\")","",1,1715.58,1715.58]
[null,"5606000000-E","2\" BLOW OFF","","",1,1604.33,1604.33]
[null,"5648000000-N","RELOCATE WATER METER","","",53,1748.1630188679201,92652.64]
[null,"5649000000-N","RECONNECT WATER METER","","",5,1417.46,7087.3]
[null,"5666000000-N","FIRE HYDRANT","","",27,4610.19888888889,124475.37]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",2,3270.7350000000001,6541.47]
[null,"5673000000-E","FIRE HYDRANT LEG","","",620,77.738709677419394,48198]
[null,"5678400000-E","6\" LINE STOP","","",1,18090.45,18090.45]
[null,"5679000000-E","12\" LINE STOP","","",1,25351.759999999998,25351.759999999998]
[null,"5686500000-E","WATER SERVICE LINE","","",2698,35.671100815418797,96240.63]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",9424,189.960596349745,1790188.66]
[null,"5691600000-E","16\" SANITARY GRAVITY SEWER","","",1586,427.44,677919.84]
[null,"5768000000-N","SANITARY SEWER CLEAN-OUT","","",21,1167.8399999999999,24524.639999999999]
[null,"5768500000-E","SEWER SERVICE LINE","","",1240,89.05,110422]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",44,4968.0990909090897,218596.36]
[null,"5776000000-E","5' DIA UTILITY MANHOLE","","",21,9431.0914285714298,198052.92]
[null,"5777000000-E","6' DIA UTILITY MANHOLE","","",4,11758.8,47035.199999999997]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",227,583.19748898678404,132385.82999999999]
[null,"5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",198,836.08525252525203,165544.88]
[null,"5783000000-E","UTILITY MANHOLE WALL 6' DIA","","",12,1326.63,15919.56]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(15\")","",1565,18.09,28310.85]
[null,"","","(36\")","",410,77.39,31729.9]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",915,0.01,9.15]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",5930,12.0478583473862,71443.8]
[null,"5811000000-E","ABANDON 18\" UTILITY PIPE","","",391,28.14,11002.74]
[null,"5815000000-N","REMOVE WATER METER","","",373,160.80000000000001,59978.400000000001]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",49,387.94,19009.060000000001]
[null,"5816000000-N","ABANDON UTILITY MANHOLE","","",105,752.19571428571396,78980.55]
[null,"5828000000-N","REMOVE UTILITY MANHOLE","","",5,954.77,4773.8500000000004]
[null,"5835000000-E","**\" ENCASEMENT PIPE","(54\")","",330,884.42,291858.59999999998]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",80,287.38,22990.400000000001]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",1340,88.44,118509.6]
[null,"5836000000-E","24\" ENCASEMENT PIPE","","",229,141.244716157205,32345.040000000001]
[null,"5836200000-E","30\" ENCASEMENT PIPE","","",360,349.75,125910]
[null,"5872500000-E","BORE & JACK **\"","(18\")","",885,631.16,558576.6]
[null,"","","(24\")","",160,564.47,90315.199999999997]
[null,"5882000000-N","GENERIC UTILITY ITEM (EA)","36\" X 6\" TAPPING SLEEVE AND   VALVE","",1,13567.84,13567.84]
[null,"","","4\" COMBINATION AIR VALVE IN   MH","",1,80804.02,80804.02]
[null,"","","STEEL PILE PIER","",3,10653.27,31959.81]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",319601,2.33692569797967,746883.79]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",10890,57.164049586776898,622516.5]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",50900,53.1694106090373,2706323]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",30930,46.513790817976101,1438671.55]
[null,"6015000000-E","TEMPORARY MULCHING","","",1450,823.52447586206904,1194110.49]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",56700,6.9642680776014103,394874]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",286.5,827.63445026177999,237117.27]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",27630,11.396523706116501,314885.95]
[null,"6029000000-E","SAFETY FENCE","","",15010,2.2816122584943401,34247]
[null,"6030000000-E","SILT EXCAVATION","","",218930,11.990887955054101,2625165.1]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",885040,1.44414896501853,1278129.6000000001]
[null,"6037000000-E","COIR FIBER MAT","","",30800,3.56612987012987,109836.8]
[null,"6038000000-E","PERM SOIL REINF MAT","","",20105,5.0166625217607601,100860]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",50440,4.8731363996827897,245801]
[null,"6045000000-E","**\" TEMPORARY PIPE","(15\")","",165,154.18181818181799,25440]
[null,"","","(36\")","",265,80,21200]
[null,"6046000000-E","TEMP PIPE FOR STREAM CROSS","","",100,50.56,5056]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",790,10.0660759493671,7952.2]
[null,"6069000000-E","STILLING BASINS","","",1016,22.5,22860]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",20,1058,21160]
[null,"6071010000-E","WATTLE","","",6671,6.3393134462599301,42289.56]
[null,"6071012000-E","COIR FIBER WATTLE","","",11390,11.513696224758601,131141]
[null,"6071013000-E","WATTLE BARRIER","","",28978,11.3097453240389,327733.8]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",16795,5.1067222387615399,85767.4]
[null,"6071030000-E","COIR FIBER BAFFLE","","",32860,5.8307273280584297,191597.7]
[null,"6071050000-E","**\" SKIMMER","(1\")","",1,900,900]
[null,"","","(1-1/2\")","",65,1471.11907692308,95622.74]
[null,"","","(2\")","",31,1745.62387096774,54114.34]
[null,"","","(2-1/2\")","",9,2424.7199999999998,21822.48]
[null,"","","(3\")","",5,3033.37,15166.85]
[null,"","","(4\")","",1,4044.49,4044.49]
[null,"6084000000-E","SEEDING AND MULCHING","","",803.3,2266.3890202912999,1820590.3]
[null,"6087000000-E","MOWING","","",904.5,180.094593698176,162895.56]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",14800,6.2168918918918896,92010]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",38.75,1837.41496774194,71199.83]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",19550,4.22056265984655,82512]
[null,"6102000000-E","SODDING","","",3700,9,33300]
[null,"6105000000-E","WATER","","",25,900,22500]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",586.25,992.460895522388,581830.19999999995]
[null,"6111000000-E","IMPERVIOUS DIKE","","",1410,103.22695035461,145550]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",370,171.471081081081,63444.3]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",325,108.316923076923,35203]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",85,649.70588235294099,55225]
[null,"6120000000-E","CULVERT DIVERSION CHANNEL","","",2650,14,37100]
[null,"6123000000-E","REFORESTATION","","",15.1,1789.4284768211901,27020.37]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",9,2400,21600]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",197,396.11370558375597,78034.399999999994]
[null,"","","","DEVICE CLEANOUT",569,202.10249560632701,114996.32]
[null,"6133000000-N","GENERIC EROSION CONTROL ITEM (LS)","CONSTRUCTION, MAINTENANCE, &  REMOVAL OF","TEMP ACCESS AT STA 66+62-Y4-RT",1,275000,275000]
[null,"","","PUMP-AROUND OPERATION","",1,50900,50900]
[null,"","","STREAM INTAKE VAULT","",1,53429.41,53429.41]
[null,"","","SURVEYING FOR MITIGATION","",1,19095,19095]
[null,"6135000000-E","GENERIC EROSION CONTROL ITEM (ACR)","COMPOST BLANKET","",5,20335,101675]
[null,"6138000000-E","GENERIC EROSION CONTROL ITEM (CY)","BLANKET DRAIN","",1350,66.400000000000006,89640]
[null,"","","BORROW FOR STREAM RELOCATION","",25000,18.100000000000001,452500]
[null,"","","DAM EMBANKMENT EARTH FILL","",4850,22.45,108882.5]
[null,"","","IMPERVIOUS SELECT MATERIAL","",700,58.15,40705]
[null,"","","UNCLASSIFIED FOR STREAM","RELOCATION",34000,13.35,453900]
[null,"","","UNDERCUT FOR STREAM RELOCATION","",13000,27.2,353600]
[null,"6141000000-E","GENERIC EROSION CONTROL ITEM (SY)","TYPE 2 GEOTEXTILE","",1050,2.23,2341.5]
[null,"6147000000-E","GENERIC EROSION CONTROL ITEM (LF)","TOE WOOD PROTECTION","",400,111.36,44544]
[null,"6900000000-E","TOPSOIL","","",3600,24.75,89100]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",16,777.78,12444.48]
[null,"7060000000-E","SIGNAL CABLE","","",15050,2.78,41839]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",72,811.11,58399.92]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",7,1030.3,7212.1]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",10,1414.14,14141.4]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",4600,2.78,12788]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",2925,4.55,13308.75]
[null,"7279000000-E","TRACER WIRE","","",35406,0.86,30449.16]
[null,"7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",25,45.45,1136.25]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",4271,6.57,28060.47]
[null,"","","(2, 2\")","",28788,7.58,218213.04]
[null,"","","(3, 2\")","",2530,9.34,23630.2]
[null,"","","(4, 2\")","",440,11.62,5112.8]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",1375,16.16,22220]
[null,"","","(2, 2\")","",2354,17.93,42207.22]
[null,"","","(3, 2\")","",594,20.2,11998.8]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",98,363.64,35636.720000000001]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",75,690.07,51755.25]
[null,"7360000000-N","WOOD POLE","","",23,1060.6099999999999,24394.03]
[null,"7372000000-N","GUY ASSEMBLY","","",23,606.05999999999995,13939.38]
[null,"7384000000-E","***\" RISER WITH **************","(1-1/2\", WEATHERHEAD)","",11,429.29,4722.1899999999996]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",2,404.04,808.08]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",2,858.59,1717.18]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",5625,7.93,44606.25]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",13700,1.77,24249]
[null,"7481000000-N","SITE SURVEY","","",2,1262.6300000000001,2525.2600000000002]
[null,"7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",4,606.05999999999995,2424.2399999999998]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",8,3232.32,25858.560000000001]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",2,6262.63,12525.26]
[null,"7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",8,303.02999999999997,2424.2399999999998]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(144)","",21534,3.79,81613.86]
[null,"","","(24)","",830,3.28,2722.4]
[null,"","","(36)","",5425,3.03,16437.75]
[null,"","","(72)","",21055,3.28,69060.399999999994]
[null,"7528000000-E","DROP CABLE","","",5271,3.03,15971.13]
[null,"7540000000-N","SPLICE ENCLOSURE","","",19,1919.19,36464.61]
[null,"7552000000-N","INTERCONNECT CENTER","","",21,2893.94,60772.74]
[null,"7566000000-N","DELINEATOR MARKER","","",87,122.22,10633.14]
[null,"7575160000-E","REM EXT COMM CABLE","","",4900,0.91,4459]
[null,"7576000000-N","METAL STRAIN SIGNAL POLE","","",8,16666.669999999998,133333.35999999999]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",6,21212.12,127272.72]
[null,"7613000000-N","SOIL TEST","","",21,833.33,17499.93]
[null,"7614100000-E","DRILLED PIER FOUND","","",95,1060.6099999999999,100757.95]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",6,252.53,1515.18]
[null,"7636000000-N","SIGN FOR SIGNALS","","",25,555.55999999999995,13889]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",18,2020.2,36363.599999999999]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",4,2525.25,10101]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(TYPE 2070E, BASE MOUNTED)","",4,16464.650000000001,65858.600000000006]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",32,121.21,3878.72]
[null,"7901000000-N","CABINET BASE EXTENDER","","",4,590.91,2363.64]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,4545.45,4545.45]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","5/8\" X 10' GROUNDING ELECTRODE","",66,252.53,16666.98]
[null,"","","CCTV METAL POLE (60')","",7,14848.48,103939.36]
[null,"","","DIGITAL CCTV CAMERA ASSEMBLY","",8,4141.41,33131.279999999999]
[null,"","","DMS ACCESS LADDER","",5,8585.86,42929.3]
[null,"","","DMS PEDESTAL STRUCTURE","",5,66666.67,333333.34999999998]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE-2C)","",5,75757.58,378787.9]
[null,"","","EQUIPMENT CABINET DISCONNECT","",11,1313.13,14444.43]
[null,"","","ETHERNET EDGE SWITCH","",17,1515.15,25757.55]
[null,"","","FIELD EQUIPMENT CABINET","",8,5454.55,43636.4]
[null,"","","HUB CABINET","",1,24747.47,24747.47]
[null,"","","HUB CABINET BASE EXTENDER","",1,1262.6300000000001,1262.6300000000001]
[null,"","","HUB CABINET FOUNDATION","",1,2525.25,2525.25]
[null,"","","JUNCTION BOX (SPECIAL OVER-   SIZED)","",12,1515.15,18181.8]
[null,"","","METER BASE/DISCONNECT COMBINA-TION PANEL","",11,2323.23,25555.53]
[null,"","","SOLAR POWER ASSEMBLY","",1,11919.19,11919.19]
[null,"","","WOOD PEDESTAL","",11,227.27,2499.9699999999998]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","#4 SOLID BARE COPPER GROUNDINGCONDUCTOR","",660,10.61,7002.6]
[null,"","","3-WIRE COPPER FEEDER CONDUC-  TORS","",1675,5.56,9313]
[null,"","","4-WIRE COPPER FEEDER CONDUC-  TORS","",3570,6.06,21634.2]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(45+22.65 -EBL-)","",1,1,1]
[null,"8021000000-N","REMV EXIST STR **********","(18+27.98 -L-)","",1,145457.97,145457.97]
[null,"8035000000-N","REMV EXIST STR **********","(45+22.65 -EBL-)","",1,4105318.81,4105318.81]
[null,"8056000000-N","REMV EXIST STR **********","(30+13.47 -Y115REV-)","",1,30332.48,30332.48]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",3,2833.3333333333298,8500]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 18+27.98 -L-)","",1,8600,8600]
[null,"","","(1, 22+26.35 -Y1B-)","",1,15082.44,15082.44]
[null,"","","(1, 58+33.94 -Y15FLYCA-)","",1,35948.28,35948.28]
[null,"","","(1, 60+66.06 -Y15FLYAC-)","",1,27643.26,27643.26]
[null,"","","(2, 47+63.62 -Y15FLYBD-)","",1,17732.189999999999,17732.189999999999]
[null,"","","(2, 60+66.06 -Y15FLYAC-)","",1,15528.2,15528.2]
[null,"","","(3, 47+63.62 -Y15FLYBD-)","",1,23622.65,23622.65]
[null,"","","(3, 58+33.94 -Y15FLYCA-)","",1,27245.15,27245.15]
[null,"","","(3, 60+66.06 -Y15FLYAC-)","",1,13683.43,13683.43]
[null,"","","(4, 47+63.62 -Y15FLYBD-)","",1,18719.59,18719.59]
[null,"","","(4, 58+33.94 -Y15FLYCA-)","",1,33346.97,33346.97]
[null,"","","(4, 60+66.06 -Y15FLYAC-)","",1,13681.42,13681.42]
[null,"","","(5, 47+63.62 -Y15FLYBD-)","",1,27212.12,27212.12]
[null,"","","(5, 58+33.94 -Y15FLYCA-)","",1,15879.52,15879.52]
[null,"","","(5, 60+66.06 -Y15FLYAC-)","",1,21367.7,21367.7]
[null,"","","(6, 47+63.62 -Y15FLYBD-)","",1,19829.21,19829.21]
[null,"","","(6, 58+33.94 -Y15FLYCA-)","",1,37299.519999999997,37299.519999999997]
[null,"","","(6, 60+66.06 -Y15FLYAC-)","",1,19923.3,19923.3]
[null,"","","(7, 58+33.94 -Y15FLYCA-)","",1,14083.78,14083.78]
[null,"","","(8, 60+66.06 -Y15FLYAC-)","",1,6194.44,6194.44]
[null,"","","(9, 60+66.06-Y15FLYAC-)","",1,22168.42,22168.42]
[null,"8096000000-E","PILE EXCAVATION IN SOIL","","",115,127.21,14629.15]
[null,"8097000000-E","PILE EXCAVATION NOT IN SOIL","","",281,273.40516014234902,76826.850000000006]
[null,"8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",56,1072.18,60042.080000000002]
[null,"","","(6'-0\")","",47,1272.93,59827.71]
[null,"8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",98.5,1086.93005076142,107062.61]
[null,"8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",56,1072.18,60042.080000000002]
[null,"","","(5'-6\")","",140,1279.33,179106.2]
[null,"8105640000-E","3'-6\" DRILLD PIER NO SOIL","","",67.599999999999994,2387.1800295858002,161373.37]
[null,"8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",212,1063.46,225453.52]
[null,"8112730000-N","PDA TESTING","","",4,1388,5552]
[null,"8113000000-N","SID INSPECTIONS","","",5,510.2,2551]
[null,"8114000000-N","SPT TESTING","","",8,816.33,6530.64]
[null,"8115000000-N","CSL TESTING","","",6,2784.0133333333301,16704.080000000002]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(45+22.65 -EBL-)","",1,2300,2300]
[null,"8126000000-N","CULV EXCAV @ ************","(18+22.67 -Y5B-)","",1,91946.9,91946.9]
[null,"","","(19+75.11 -Y5B-)","",1,34773.54,34773.54]
[null,"","","(30+13.47 -Y115REV-)","",1,127508.06,127508.06]
[null,"","","(35+53.70 -Y15RPDREV-)","",1,74937.38,74937.38]
[null,"","","(43+66.60 -Y15FLYCA-)","",1,63865.88,63865.88]
[null,"","","(45+66.21 -Y4-)","",1,150000,150000]
[null,"","","(768+62.23 -L-)","",1,268837.09999999998,268837.09999999998]
[null,"","","(792+88.12 -L-)","",1,96061.66,96061.66]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",6284,66.941857097390198,420662.63]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",368372,42.8085646846123,15769476.59]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",370000,0.54875421621622,203039.06]
[null,"8175000000-E","CLASS AA CONC (BRIDGE)","","",9485.2999999999993,1200,11382360]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",3098.5,1016.7625980313099,3150438.91]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",4767.5,604.69446040901903,2882880.84]
[null,"8210000000-N","BRG APPR SLAB ***********","(18+27.98 -L-)","",1,58550,58550]
[null,"","","(22+26.35 -Y1B-)","",1,40455.980000000003,40455.980000000003]
[null,"","","(23+43.03 -Y16-)","",1,38428.32,38428.32]
[null,"","","(30+67.66 -Y4-)","",1,144311.93,144311.93]
[null,"","","(45+22.65 -EBL-)","",1,58850,58850]
[null,"","","(47+28.33 -Y15REV-)","",1,233807.08,233807.08]
[null,"","","(47+63.62 -Y15FLYBD-)","",1,55192.76,55192.76]
[null,"","","(58+33.94 -Y15FLYCA-)","",1,55355.53,55355.53]
[null,"","","(60+66.06 -Y15FLYAC-)","",1,55871.19,55871.19]
[null,"","","(61+02.86 -L- LT)","",1,65155,65155]
[null,"","","(61+02.86 -L- RT)","",1,65155,65155]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",2249712,1.29804646994815,2920230.72]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",34843,3.5768877536377501,124629.5]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",823706,1.82995899022224,1507348.2]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",1763.7,273.95000283494898,483165.62]
[null,"8274000000-E","63\" MOD PRESTR CONC GIRDR","","",2195.42,370.38999826912402,813161.61]
[null,"8280000000-E","STRUCTURAL STEEL","","",13568341,2.6121321685532499,35442300]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",126,1973.7642857142901,248694.3]
[null,"","","(HP 14 X 73)","",841,2257.2206896551702,1898322.6]
[null,"","","(HP12X53)","",44,477.44,21007.360000000001]
[null,"8364000000-E","HP12X53 PILES","","",6610,51.505052950075601,340448.4]
[null,"8384000000-E","HP14X73 PILES","","",41469,68.448402662229597,2838486.81]
[null,"8391000000-N","STEEL PILE POINTS","","",45,357.39666666666699,16082.85]
[null,"8392500000-E","PREDRILLING FOR PILES","","",96,315.04000000000002,30243.84]
[null,"8475000000-E","TWO BAR METAL RAIL","","",2014.2,114.33760798331799,230298.81]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",14139.44,72.193516857810494,1020775.9]
[null,"8504000000-E","CONC BARR RAIL MOMENT SLAB","","",2390,377.15,901388.5]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",423.5,112.690011806375,47724.22]
[null,"8510000000-E","CONCRETE MEDIAN BARRIER","","",309.7,95.429996771068801,29554.67]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-3 1/2\")","",354.1,77.160011296243994,27322.36]
[null,"","","(1'-2\" X 2'-6\")","",1040.4100000000001,83.764861929431703,87149.8]
[null,"","","(1'-2\" X 2'-8 1/2\")","",207.43,120.699995179097,25036.799999999999]
[null,"","","(1'-2\" X 3'-3 3/4\")","",481.4,99.490008309098499,47894.49]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",4943.2,73.094788800776797,361322.16]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",65.8,264.96003039513698,17434.37]
[null,"8590000000-E","RIP RAP, CLASS **","(A)","",85,81.92,6963.2]
[null,"8594000000-E","RIP RAP B","","",85,81.92,6963.2]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",740,51.86,38376.400000000001]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",3815,6.5823066841415496,25111.5]
[null,"8654000000-N","DISC BEARINGS","","",2,556961.85499999998,1113923.71]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",4,71178.014999999999,284712.06]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",119.1,1339.20999160369,159499.91]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",7,607.42999999999995,4252.01]
[null,"8692000000-N","FOAM JOINT SEALS","","",1,31200,31200]
[null,"8706000000-N","EXPANSION JOINT SEALS","","",1,438267.27,438267.27]
[null,"8713000000-N","MODULAR EXP JOINT SEALS","","",1,400140.2,400140.2]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",7940,84.9083249370277,674172.1]
[null,"","","(2)","",26683,64.705019675448796,1726524.04]
[null,"","","(3)","",10842,58.8,637509.6]
[null,"8802010000-E","SOIL NAIL RETAINING WALLS","","",2672,123.1,328923.2]
[null,"8802015100-N","SOIL NAIL VERIFICATION TESTS","","",2,1670,3340]
[null,"8802015110-N","SOIL NAIL PROOF TESTS","","",10,725,7250]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL CONCRETE SURFACE","TREATMENT (WALL)",33833,5.0999999999999996,172548.3]
[null,"","","ARCHITECTURAL SURFACE TREAT-  MENT","",555368,2.1,1166272.8]
[null,"","","SOUND BARRIER WALL 1","",56818,29.41,1671017.38]
[null,"","","SOUND BARRIER WALL 2","",85427,29.37,2508990.9900000002]
[null,"","","SOUND BARRIER WALL 3","",87297,29.53,2577880.41]
[null,"","","SOUND BARRIER WALL 4","",108020,29.63,3200632.6]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","FIELD MEASURING","",1,8450,8450]
[null,"","","POST TENSIONING ENCASEMENT","",1,62639.48,62639.48]
[null,"","","POST TENSIONING TENDONS","",1,41963.519999999997,41963.519999999997]
[null,"","","STRIP SEAL EXPANSION JOINTS","",1,129350,129350]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","63\" PRESTRESSED CONCRETE","FLORIDA I-BEAM GIRDERS",4566.33,338.03000002189901,1543556.53]
[null,"","","CLEAN BRIDGE DECK DRAINAGE    SYSTEM","",900,36.729999999999997,33057]
[null,"","","FOAM JOINT SEALS FOR PRESERVA-TION","",69.5,422.22,29344.29]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","6000 PSI CONCRETE","",95.2,1637.66995798319,155906.18]
[null,"","","EPOXY POLYMER CONCRETE        MATERIALS","",119,4616.25,549333.75]
[null,"","","POLYESTER POLYMER CONCRETE    MATERIALS","",null,null,0]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","ARCHITECTURAL CONCRETE SURFACE","TREATMENT (BRIDGE)",1246.4000000000001,45.990003209242602,57321.94]
[null,"","","TOP OF CAP EPOXY COATINGS","",494,20.27,10013.379999999999]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","CONCRETE DECK REPAIR FOR","POLYMER CONCRETE OVERLAY",7.3,1013.32054794521,7397.24]
[null,"","","PLACING & FINISHING POLYMER","CONCRETE OVERLAY",3959,67.55,267430.45]
[null,"","","SCARIFYING BRIDGE DECK","",3959,22.52,89156.68]
[null,"","","SHOTBLASTING BRIDGE DECK","",3959,5.63,22289.17]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","9-5/8\" DIA MICROPILES","",196,10765.31,2110000.7599999998]
[null,"","","BEAM END EPOXY COATINGS","",30,1125,33750]
[null,"","","BEARING KEEPER PLATE","",10,5515,55150]
[null,"","","DEMONSTRATION MICROPILES","",1,26734.69,26734.69]
[null,"","","MICROPILE PROOF TESTS","",8,4591.84,36734.720000000001]
[null,"","","MICROPILE VERIFICATION TESTS","",1,20408.16,20408.16]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  NO 790008","",10,7881.41,78814.100000000006]

{"sheet":"ITEMS - DIV 10","index":12,"n_rows":296,"n_cols":8,"rows_kept":296,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 10"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",8,521290,4170320]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",2,28125,56250]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(27+79.00 -L-)","",1,28959,28959]
[null,"","","(32+31.61 -L-)","",1,25000,25000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",1400,1,1400]
[null,"0043000000-N","GRADING","","",3,587666.66666666698,1763000]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",2,1,2]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",1633,16.1390079608083,26355]
[null,"0106000000-E","BORROW EXCAVATION","","",6319,30.221870549137499,190972]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",220,7.6363636363636402,1680]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",1400,1,1400]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",3750,1,3750]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",6130,1,6130]
[null,"0199000000-E","TEMPORARY SHORING","","",5920,39.677364864864899,234890]
[null,"0241000000-E","GENERIC GRADING ITEM (SY)","SOIL CEMENT BASE (FULL DEPTH","RECLAMATION)",161471,3.3717575911463999,544441.06999999995]
[null,"","","SOIL CEMENT BASE FULL DEPTH","RECLAMATION",8840,4.7,41548]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",110,1,110]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",320,1,320]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",224,42.553571428571402,9532]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",2,1,2]
[null,"0366000000-E","15\" RC PIPE CULV III","","",396,36.545454545454497,14472]
[null,"0372000000-E","18\" RC PIPE CULV III","","",68,42,2856]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",56,32,1792]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",28,39,1092]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",136,48,6528]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",52,38,1976]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",2,1,2]
[null,"0995000000-E","PIPE REMOVAL","","",238,8.6974789915966397,2070]
[null,"1099500000-E","SHALLOW UNDERCUT","","",100,14,1400]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",200,23,4600]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",2769,23,63687]
[null,"1187000000-E","PC FOR SOIL CEMENT BASE","","",5154,174.406476523089,898890.98]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",4758,37.095418242959198,176500]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",90.66,2909.96029119788,263817]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1\")","",245,17,4165]
[null,"","","(1-1/2\")","",491927,2.1917933961746399,1078202.3500000001]
[null,"","","(1-1/4\")","",80668,1.85,149235.79999999999]
[null,"","","(2\")","",499042,1.8,898275.6]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",14122,3.7738988811783001,53295]
[null,"","","(0\" TO 1-1/4\")","",55,6,330]
[null,"","","(0\" TO 3\")","",204,26,5304]
[null,"1330000000-E","INCIDENTAL MILLING","","",28534,4.1798818952828203,119268.75]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",11459,61.847560869185799,708711.2]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",6063,59.513607125185601,360831]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",22058,50.501499682654803,1113962.08]
[null,"1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",797,53.246675031367602,42437.599999999999]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",81559,51.996411186993498,4240775.3]
[null,"1524000000-E","ASP CONC SURF CRS S9.5C LEVEL","","",9072,54.333815035273403,492916.37]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",77935,72,5611320]
[null,"1575000000-E","ASP FOR PLANT MIX","","",7816,487.47824974411498,3810130]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",5450,605.11926605504595,3297900]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",79,41.506329113924103,3279]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",25538,103.953050356332,2654753]
[null,"1735000000-E","REP JNT CONC PVT SLABS","","",2210,490,1082900]
[null,"1736000000-E","SELECT MATERIAL, CLASS IV","","",4473,40,178920]
[null,"1737000000-E","PATCHING CONC PVMT SPALLS","","",1000,95,95000]
[null,"1775000000-E","AST, MAT COAT, #78M STONE","","",50316,1.0887729549248699,54782.7]
[null,"1803500000-E","AST, DOUBLE SEAL","","",159849,1.6554169872817499,264616.75]
[null,"1838000000-E","EMULSION FOR AST","","",104550,2.1750502152080302,227401.5]
[null,"1838500000-N","VACUUM TRUCK","","",13,3846.1538461538498,50000]
[null,"1839140000-E","ULTRATHIN BOND WEAR CRS","","",19397,106.896169510749,2073465]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",141811,0.33277919202319001,47191.75]
[null,"1858000000-E","******\"PCC PVMT RAMPS","(11\")","",2836,212,601232]
[null,"1881000000-E","GENERIC PAVING ITEM (LF)","JOINT CONSTRUCTION, REPAIR ANDSEALING","",113544,3,340632]
[null,"1882000000-E","GENERIC PAVING ITEM (GAL)","STRUCTURAL FOAM VOID FILL/","STABILIZATION",400,150,60000]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","FINE MILLING 5/8\" DEPTH","",43591,11,479501]
[null,"2000000000-N","RIGHT-OF-WAY MARKERS","","",38,200,7600]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",145.6,1,145.6]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",450,1,450]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",33.6,1,33.6]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",75.599999999999994,1,75.599999999999994]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",650,1,650]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",2,1,2]
[null,"2077000000-E","6\" OUTLET PIPE","","",12,1,12]
[null,"2253000000-E","PIPE COLLARS","","",0.44700000000000001,5033.5570469798704,2250]
[null,"2275000000-E","FLOWABLE FILL","","",13,175,2275]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",12,1566.6666666666699,18800]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",0.74,325,240.5]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",2,330,660]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",1,360,360]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",9,377.222222222222,3395]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",548,38.6131386861314,21160]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",63,29,1827]
[null,"2600000000-N","RETROFIT EXT CURB RAMPS","","",50,3145.03,157251.5]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",4,2086.25,8345]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",4760,87.626050420168099,417100]
[null,"2613000000-N","REM & REP CURB RAMPS","","",4,2700,10800]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","2'-6\" CONCRETE CURB & GUTTER","(11\" THICK)",143,60,8580]
[null,"2830000000-N","ADJ MANHOLES","","",112,380.81428571428597,42651.199999999997]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",150,367.19133333333298,55078.7]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",14087,25.080712713849699,353312]
[null,"3045000000-E","SBGR SHOP CURVED","","",137.5,20,2750]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",10,6,60]
[null,"3195000000-N","GR END TYPE AT-1","","",1,550,550]
[null,"3210000000-N","GR END TYPE CAT-1","","",6,1200,7200]
[null,"3287000000-N","GR END TYPE TL-3","","",19,3134.21052631579,59550]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",28,2171.4285714285702,60800]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",13570,1,13570]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",212.5,7,1487.5]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-3)","",1,2000,2000]
[null,"3500000000-E","WOVEN WIRE FENCE **\" FAB","(48\")","",220,8.5,1870]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",10,30,300]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",10,35,350]
[null,"3533000000-E","CHN LK FENCE **\" FABRIC","(60\")","",9460,14.5,137170]
[null,"3539000000-E","MET LINE PST **\" CL FEN","(60\")","",946,75,70950]
[null,"3545000000-E","MET TERM PST **\" CL FEN","(60\")","",237,250,59250]
[null,"3578000000-N","GENERIC FENCING ITEM (EA)","RESET EXISTING GATE","",1,1800,1800]
[null,"3628000000-E","RIP RAP, CLASS I","","",270,35,9450]
[null,"3635000000-E","RIP RAP, CLASS II","","",55,36,1980]
[null,"3649000000-E","RIP RAP, CLASS B","","",495,32.121212121212103,15900]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",2835,1.5873015873015901,4500]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",1,100,100]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(E)","",9,75,675]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",1,1,1]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",3275,5.7443511450381699,18812.75]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",351,13.1538461538461,4617]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",93,5,465]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",6748,5.5190574985180803,37242.6]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",30,150,4500]
[null,"4424000000-N","WZ PRESENCE LIGHTING","","",22,1109.0909090909099,24400]
[null,"4430000000-N","DRUMS","","",136,64.867647058823493,8822]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",72,105,7560]
[null,"4445000000-E","BARRICADES (TYPE III)","","",80,22,1760]
[null,"4447000000-E","PED CHANNEL DEVICES","","",260,32.507692307692302,8452]
[null,"4455000000-N","FLAGGER","","",75,335.33333333333297,25150]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",4,111500,446000]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",6,11500,69000]
[null,"4485000000-E","PORT CONC BARRIER","","",1380,36.700000000000003,50646]
[null,"4510000000-N","LAW ENFORCEMENT","","",10324,59.1460674157303,610624]
[null,"4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","PROTECTIVE CANOPY","",1,5000,5000]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICE","",3,395,1185]
[null,"","","DOUBLE LANE CLOSURE","",150,2000,300000]
[null,"","","INTERSTATE LANE CLOSURE","",612,1800,1101600]
[null,"","","RAMP / LOOP CLOSURE DETOUR    (TYPE A)","",80,1000,80000]
[null,"","","RAMP / LOOP CLOSURE DETOUR    (TYPE B)","",8,1000,8000]
[null,"","","RAMP/LOOP CLOSURE","",120,1400,168000]
[null,"","","SINGLE LANE CLOSURE","",74,1750,129500]
[null,"","","STREET LANE CLOSURE","",62,1300,80600]
[null,"","","TRIPLE LANE CLOSURE","",50,2200,110000]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",129,10.2325581395349,1320]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",753982,0.44003656585966,331779.65000000002]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",222592,0.53,117973.75999999999]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",28979,1.95130956899824,56547]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",16952,1.0144525719679101,17197]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",210,86.988095238095198,18267.5]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",738,81.653116531165296,60260]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",3364,3.7575802615933398,12640.5]
[null,"","","(IV)","",520,2,1040]
[null,"4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",3282,6.75,22153.5]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",105,9,945]
[null,"4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",136,13.5,1836]
[null,"4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(II)","",30,27.5,825]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(II)","",11,250,2750]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",863291,9.9090561583520004E-2,85543.99]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",464109,0.22709320439809999,105396]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",2747,0.84125591554422996,2310.9299999999998]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",47245,0.59198327865383005,27968.25]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",548,3.5742335766423401,1958.68]
[null,"4840000000-N","PAINT PVT MKG CHARACTER","","",172,51.046511627907002,8780]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",317,59.801261829653001,18957]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",1654,4.5,7443]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",1268,5,6340]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",35,16,560]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","CONTRAST COLD APPLIED PLASTIC","PAVEMENT MARKING LINES, TYPE  II (9\")",2873,9,25857]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 12\"","30 MILS (STANDARD GLASS BEADS)",4977,2,9954]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",640,8,5120]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","30 MILS (STANDARD GLASS BEADS)",33705,1.8,60669]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",40,6,240]
[null,"","","","LINES (24\", 90 MILS)",4947,10.554821103699201,52214.7]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",5010,41.849800399201598,209667.5]
[null,"","","","PAVEMENT MARKERS",1663,36.337943475646398,60430]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",40,8.5250000000000004,341]
[null,"5255000000-N","PORTABLE LIGHTING","","",5,63100,315500]
[null,"5325800000-E","8\" WATER LINE","","",2434,113.38,275966.92]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",1820,10.85,19747]
[null,"5546000000-E","8\" VALVE","","",2,4761.08,9522.16]
[null,"5648000000-N","RELOCATE WATER METER","","",2,1469.15,2938.3]
[null,"5686500000-E","WATER SERVICE LINE","","",73,24.29,1773.17]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",2408,9.41,22659.279999999999]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",63.3,99.4,6292.02]
[null,"5872500000-E","BORE & JACK **\"","(18\")","",63.3,3063.1300157977898,193896.13]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",19261,3.5515419760137101,68406.25]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",415,1,415]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",3904,6.4421106557377001,25150]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",1675,6.6388059701492503,11120]
[null,"6015000000-E","TEMPORARY MULCHING","","",12,21.7916666666667,261.5]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",1000,1.05,1050]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",8.5,94.882352941176507,806.5]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",725,4.8275862068965498,3500]
[null,"6029000000-E","SAFETY FENCE","","",3012,5.1657370517928296,15559.2]
[null,"6030000000-E","SILT EXCAVATION","","",5910,2.5,14775]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",32140,1.18817672682016,38188]
[null,"6037000000-E","COIR FIBER MAT","","",1675,2.7522388059701499,4610]
[null,"6038000000-E","PERM SOIL REINF MAT","","",4275,3.2654970760233901,13960]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",770,2.84935064935065,2194]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",250,26.4,6600]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",10,810,8100]
[null,"6071010000-E","WATTLE","","",10468,7.7193781047000396,80806.45]
[null,"6071012000-E","COIR FIBER WATTLE","","",510,7.0176470588235302,3579]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",774,1.87998708010336,1455.11]
[null,"6071030000-E","COIR FIBER BAFFLE","","",770,5.6103896103896096,4320]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",5,769,3845]
[null,"","","(2\")","",2,935,1870]
[null,"6084000000-E","SEEDING AND MULCHING","","",30.3,1246.3696369637,37765]
[null,"6087000000-E","MOWING","","",12,12,144]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",200,1.125,225]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",0.5,500,250]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",375,1.37,513.75]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",11,82.681818181818201,909.5]
[null,"6111000000-E","IMPERVIOUS DIKE","","",104,40,4160]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",20,14.5,290]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",38,9.2105263157894708,350]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",20,1326,26520]
[null,"6123000000-E","REFORESTATION","","",2.4300000000000002,443.20987654320999,1077]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",0.21,5200,1092]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",10335,8.2350024189646795,85108.75]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(32+31.61 -L-)","",1,260000,260000]
[null,"8035000000-N","REMV EXIST STR **********","(27+79.00 -L-)","",1,87550,87550]
[null,"","","(32+31.61 -L-)","",1,275000,275000]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",2,1512.5,3025]
[null,"8105500000-E","**'-**\" DRILLD PIER IN SOIL","(4'-6\")","",136.80000000000001,450,61560]
[null,"8105600000-E","**'-**\" DRILLD PIER NO SOIL","(4'-6\")","",208,1600,332800]
[null,"8111000000-E","PERM STL CASING FOR ** PIER","(4'-6\")","",35.4,480,16992]
[null,"8112730000-N","PDA TESTING","","",2,2500,5000]
[null,"8113000000-N","SID INSPECTIONS","","",12,500,6000]
[null,"8115000000-N","CSL TESTING","","",4,3000,12000]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(32+31.61 -L-)","",1,52000,52000]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",23993,37.453100487642203,898612.24]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",286992,1.1299479427998,324286.02]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",409.4,804.23622374206195,329254.31]
[null,"8210000000-N","BRG APPR SLAB ***********","(27+79.00 -L-)","",1,30175,30175]
[null,"","","(32+31.61 -L-)","",1,51354.93,51354.93]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",82174,1.0688159271789099,87828.88]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",19733,2,39466]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",2604.17,300,781251]
[null,"8277000000-E","72\" MOD PRESTR CONC GIRDR","","",512.66999999999996,380.209998634599,194922.26]
[null,"8296000000-N","POLLUTION CONTROL","","",1,91599.5,91599.5]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",12,350,4200]
[null,"","","(HP 14 X 73)","",14,587.96,8231.44]
[null,"8355000000-E","HP**X** PILES","(HP 14 X 73)","",355,68.59,24349.45]
[null,"8364000000-E","HP12X53 PILES","","",390,58,22620]
[null,"8391000000-N","STEEL PILE POINTS","","",14,293,4102]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",1303.3699999999999,95.370339964860307,124302.84]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",98.2,325,31915]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",2360,12.065423728813601,28474.400000000001]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",2622,3.0814607170099202,8079.59]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",2,8937.5,17875]
[null,"8660000000-E","CONCRETE REPAIRS","","",589.6,850,501160]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",3668.6,625,2292875]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",908.8,90,81792]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","CLEANING & REPAINTING OF","BRIDGE #320",1,400000,400000]
[null,"","","","BRIDGE #330",1,600000,600000]
[null,"","","CONTAINMENT OVER CHARLOTTE","AREA TRANSIT SYSTEM RAIL LINE",1,67000,67000]
[null,"","","MURAL PAINT REPAIR","",1,50000,50000]
[null,"","","PAINTING CONTAINMENT FOR","BRIDGE #320",1,60000,60000]
[null,"","","","BRIDGE #322",1,25000,25000]
[null,"","","","BRIDGE #326",1,40000,40000]
[null,"","","","BRIDGE #327",1,40000,40000]
[null,"","","","BRIDGE #328",1,40000,40000]
[null,"","","","BRIDGE #330",1,75000,75000]
[null,"","","","BRIDGE #332",1,30000,30000]
[null,"","","SPOT PAINTING OF STEEL STRUC-","TURE REPAIR AREAS",1,475000,475000]
[null,"","","STRIP SEAL EXPANSION JOINTS","",1,45000,45000]
[null,"","","VOLUMETRIC MIXER","",1,5000,5000]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FOAM JOINT SEALS FOR","PRESERVATION",3936.9,52.895501536742103,208244.3]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","EPOXY POLYMER CONCRETE","MATERIALS",null,null,0]
[null,"","","LATEX MODIFIED CONCRETE OVER-","LAY - EARLY STRENGTH",43.1,2200,94820]
[null,"","","POLYESTER POLYMER CONCRETE    MATERIALS","",1997.9,2600,5194540]
[null,"8882000000-E","GENERIC STRUCTURE ITEM (CF)","CONCRETE FOR DECK REPAIR","",21.3,95,2023.5]
[null,"","","ELASTOMERIC CONCRETE FOR","PRESERVATION",180.5,460.38781163434902,83100]
[null,"8889000000-E","GENERIC STRUCTURE ITEM (LB)","BEAM REPAIR CUT-OUT","",5040,110,554400]
[null,"","","BEAM REPAIR PLATING","",4016,70,281120]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","BRIDGE JOINT DEMOLITION","",630.79999999999995,103.887127457197,65532]
[null,"","","EPOXY COATING","",22690,6.6403702071397097,150670]
[null,"","","SILANE BARRIER RAIL TREATMENT","",2557,2.5,6392.5]
[null,"","","SURFACE PREPARATION FOR","CONCRETE BARRIER",2557,5,12785]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","CONCRETE DECK REPAIR FOR POLY-","MER CONCRETE OVERLAY",82.8,85,7038]
[null,"","","HYDRO-DEMOLITION OF BRIDGE    DECK","",1035,130,134550]
[null,"","","PLACING & FINISHING LATEX MOD-","IFIED CONCRETE OVERLAY - EARLYSTRENGTH",1035,140,144900]
[null,"","","PLACING & FINISHING POLYMER","CONCRETE OVERLAY",30199,87,2627313]
[null,"","","SCARIFYING BRIDGE DECK","",31234,30,937020]
[null,"","","SHOTBLASTING BRIDGE DECK","",36233,6.5726271630833804,238146]
[null,"","","SILANE DECK TREATMENT","",4999,19.185837167433501,95910]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","BEARING PLATE REPOSITIONING","",1,4000,4000]
[null,"","","BEARING REPLACEMENT","",2,4500,9000]
[null,"","","CLEANING AND PAINTING EXISTINGBEARINGS","WITH HIGH RATIO CALCIUM       SULFONATE",1336,800,1068800]
[null,"","","STEEL BEARING KEEPER ANGLE    ASSEMBLY","",37,1800,66600]
[null,"","","TYPE I BRIDGE JACKING","BRIDGE #138",1,15000,15000]
[null,"","","","BRIDGE #320",1,15000,15000]
[null,"","","","BRIDGE #326",1,15000,15000]
[null,"","","","BRIDGE #327",1,15000,15000]
[null,"","","","BRIDGE #328",1,15000,15000]
[null,"","","","BRIDGE #330",1,15000,15000]
[null,"","","","BRIDGE #332",7,15000,105000]

{"sheet":"ITEMS - DIV 11","index":13,"n_rows":343,"n_cols":8,"rows_kept":343,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 11"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",7,316341.42857142899,2214390]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",6,41333.333333333299,248000]
[null,"0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","DESIGN & CONSTRUCTION OF      BRIDGES","",1,2004595,2004595]
[null,"0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","END BENTS STRUCTURE #020035","",2,110000,220000]
[null,"","","END BENTS STRUCTURE #020133","",2,40000,80000]
[null,"","","END BENTS STRUCTURE #960733","",2,85000,170000]
[null,"","","INTERIOR BENT CAPS STRUCTURE  #020133","",2,30000,60000]
[null,"","","RIGHT OF WAY ACQUISITION","",6,6000,36000]
[null,"0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT #1 STRUCTURE #020035",21,600,12600]
[null,"","","","BENT #1 STRUCTURE #020133",13,750,9750]
[null,"","","","BENT #1 STRUCTURE #960733",22.5,640,14400]
[null,"","","","BENT #2 STRUCTURE #020035",12,1650,19800]
[null,"","","","BENT #2 STRUCTURE #020133",11,815,8965]
[null,"","","","BENT #2 STRUCTURE #960733",20.5,615,12607.5]
[null,"","","AVE FOUNDATION LENGTH AT INT","BENT STRUCTURE #020133",29,6000,174000]
[null,"","","BRIDGE LENGTH STRUCTURE       #020035","",100,4250,425000]
[null,"","","BRIDGE LENGTH STRUCTURE       #020133","",150,3000,450000]
[null,"","","BRIDGE LENGTH STRUCTURE       #960733","",70,3000,210000]
[null,"0001000000-E","CLEARING & GRUBBING","","",5,267000,1335000]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",1,11000,11000]
[null,"0015000000-N","SEALING ABANDONED WELLS","","",3,3972.99,11918.97]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",225920,24.260357648725201,5480900]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(164+30.00 -L-)","",1,100000,100000]
[null,"","","(23+80.00 -L-)","",1,27320,27320]
[null,"","","(34+65.50 -L-)","",1,43756.35,43756.35]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(15+23 -L-)","",1,11800,11800]
[null,"","","(16+62.00 -L-)","",1,11000,11000]
[null,"","","(18+28.00 -L- )","",1,8400,8400]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",1000,17.065000000000001,17065]
[null,"0043000000-N","GRADING","","",3,361388.96333333303,1084166.8899999999]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",5,2646.6,13233]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",2200,9.7329545454545503,21412.5]
[null,"0063000000-N","GRADING","","",2,239075,478150]
[null,"0098000000-E","PRE-SPLITTING OF ROCK","","",16300,41.618098159509202,678375]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",4823,8.6618494712834302,41776.1]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",2400,6.8,16320]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",2750,22.072727272727299,60700]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",5050,2.5260396039603998,12756.5]
[null,"0199000000-E","TEMPORARY SHORING","","",11842,43.542475933119398,515630]
[null,"0223000000-E","ROCK PLATING","","",1315,54.6994676806084,71929.8]
[null,"0241000000-E","GENERIC GRADING ITEM (SY)","TYPE 2 WIRE MESH","",400,210,84000]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING & DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",50,100,5000]
[null,"","","HAULING AND DISPOSAL OF","PETROLEUM CONTAMINATED SOIL",50,49.92,2496]
[null,"0257000000-E","GENERIC GRADING ITEM (LF)","ANCHOR FOR WIRE MESH","",600,190,114000]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",731,28.845417236662101,21086]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",2570,2.0313229571984399,5220.5]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",348,59.678160919540197,20768]
[null,"0335600000-E","36\" DRAINAGE PIPE","","",660,113.41818181818201,74856]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",3,340,1020]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",116,52.3,6066.8]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",148,69.25,10249]
[null,"0354000000-E","***\" RC PIPE CULV *****","(24\", V)","",64,72,4608]
[null,"0366000000-E","15\" RC PIPE CULV III","","",52,47.763076923076902,2483.6799999999998]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",1248,61.105641025640999,76259.839999999997]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",548,93.719416058394202,51358.239999999998]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",464,101.344137931034,47023.68]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",68,140.38,9545.84]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",664,56.507891566265101,37521.24]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",144,66.209999999999994,9534.24]
[null,"0594000000-E","24\" CS PIPE CULV 0.064\"","","",104,121.684615384615,12655.2]
[null,"0600000000-E","30\" CS PIPE CULV 0.079\"","","",88,98,8624]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",18,612.951111111111,11033.12]
[null,"","","(24\", 0.064\")","",3,1300,3900]
[null,"","","(30\", 0.079\")","",1,670,670]
[null,"0926000000-E","***\"CS STR PL PIPE ** GA","(60\", 12)","",152,402,61104]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(24\", 0.500\")","",60,1005.54,60332.4]
[null,"","","(36\", 0.500\")","",60,920.84,55250.400000000001]
[null,"","","(42\", 0.625\")","",90,1072.3499999999999,96511.5]
[null,"","","(60\", 0.875\")","",88,2900,255200]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(24\", 0.500\")","",60,1846.11,110766.6]
[null,"","","(36\", 0.500\")","",60,1882.41,112944.6]
[null,"","","(42\", 0.625\")","",90,1995.74,179616.6]
[null,"","","(60\", 0.875\")","",88,5100,448800]
[null,"0995000000-E","PIPE REMOVAL","","",1176,29.893520408163301,35154.78]
[null,"0996000000-N","PIPE CLEAN OUT","","",1,1000,1000]
[null,"1011000000-N","FINE GRADING","","",1,195500,195500]
[null,"1099500000-E","SHALLOW UNDERCUT","","",700,16.3071428571429,11415]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",1400,29.985714285714302,41980]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",1609,34.676817899316298,55795]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",575,41.4673913043478,23843.75]
[null,"1231000000-E","SHOULDER BORROW","","",550,37.4,20570]
[null,"1275000000-E","PRIME COAT","","",215,5,1075]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",1650,10,16500]
[null,"1330000000-E","INCIDENTAL MILLING","","",2410,18.594813278008299,44813.5]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",10100,81.286693069306907,820995.6]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",5010,74.570858283433097,373600]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",6795,81.194481236203103,551716.5]
[null,"1575000000-E","ASP FOR PLANT MIX","","",1160,566.62534482758599,657285.4]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",150,150.273333333333,22541]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",292.39999999999998,18.9464090287278,5539.93]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",1200,3.1933333333333298,3832]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",17,93,1581]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",202.8,52.574408284023697,10662.09]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",1300,7.95,10335]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",7,350.1,2450.6999999999998]
[null,"2077000000-E","6\" OUTLET PIPE","","",42,31.214285714285701,1311]
[null,"2209000000-E","ENDWALLS","","",14.7,1136.32653061224,16704]
[null,"2220000000-E","REINFORCED ENDWALLS","","",13.4,2000,26800]
[null,"2275000000-E","FLOWABLE FILL","","",132,460.11363636363598,60735]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",59,2862.32966101695,168877.45]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",38,3220,122360]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",46,473.09239130434798,21762.25]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",4,990,3960]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",4,719.96,2879.84]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",23,828.53478260869599,19056.3]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",22,732.89318181818203,16123.65]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(F)","",2,1030,2060]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",2,657.36500000000001,1314.73]
[null,"2538000000-E","**'-**\" CONCRETE CURB & GUTTER","(2'-9\")","",770,39.200000000000003,30184]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",920,32.799999999999997,30176]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",1946,33.2059352517986,64618.75]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",130,70,9100]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",115,83.75,9631.25]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",190,97,18430]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",3987.5,22.556739811912198,89945]
[null,"3045000000-E","SBGR SHOP CURVED","","",362.5,26.237931034482799,9511.25]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",40,11.9625,478.5]
[null,"3180000000-N","GR ANCHOR TYPE **********","(III SHOP CURVED)","",1,2810,2810]
[null,"3195000000-N","GR END TYPE AT-1","","",4,1025,4100]
[null,"3210000000-N","GR END TYPE CAT-1","","",1,1230,1230]
[null,"3215000000-N","GR ANCHOR TYPE III","","",15,1912,28680]
[null,"3287000000-N","GR END TYPE TL-3","","",19,2867.3684210526299,54480]
[null,"3288000000-N","GR END TYPE TL-2","","",8,2762.5,22100]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",12,2376.6666666666702,28520]
[null,"3345000000-E","REMOVE & RESET GUARDRAIL","","",82,8.75,717.5]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",1809,1.1000000000000001,1989.9]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",87.5,7.85005714285714,686.88]
[null,"3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",56.25,11.2,630]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",1,900,900]
[null,"","","(III MODIFIED)","",1,2360,2360]
[null,"","","(THRIE-BEAM)","",2,2300,4600]
[null,"","","(W-BEAM)","",1,1680,1680]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",1,2240,2240]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNITS,TYPE AT-1","",2,393,786]
[null,"3559000000-E","** STRAND BW FENCE W/ POSTS","(4)","",500,10,5000]
[null,"","","(5)","",200,8,1600]
[null,"","","(6)","",200,15,3000]
[null,"3572000000-E","CHAIN LINK FENCE RESET","","",300,10,3000]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","TEMPORARY 3 STRAND BARBED WIRE","FENCE WITH POSTS",500,5,2500]
[null,"3628000000-E","RIP RAP, CLASS I","","",2576,42.0208656832298,108245.75]
[null,"3635000000-E","RIP RAP, CLASS II","","",1106,24.897830018083202,27537]
[null,"3649000000-E","RIP RAP, CLASS B","","",432,52.639236111111103,22740.15]
[null,"3651000000-E","BOULDERS","","",119,175,20825]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",11891,3.1920317887477898,37956.449999999997]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",742,8.3696765498652308,6210.3]
[null,"4082000000-E","SUPPORT, WOOD","","",50,15,750]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",6,181.666666666667,1090]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",26,127.19230769230801,3307]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",3,140.666666666667,422]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",1,257,257]
[null,"","","(WOOD)","",6,250,1500]
[null,"4141000000-N","DISPOSE SUPPORT, WOOD","","",2,10,20]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",44,6.8375000000000004,300.85000000000002]
[null,"4158000000-N","DISPOSE SIGN SYST WOOD","","",1,28.5,28.5]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",6,3.9166666666666701,23.5]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",1283,8.3858144972720208,10759]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",1144,21.143356643356601,24188]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",746,7.1963806970509401,5368.5]
[null,"4415000000-N","FLASHING ARROW BOARD","","",2,3000,6000]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",7,11384.285714285699,79690]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",80,85.4375,6835]
[null,"4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",2,45625,91250]
[null,"4430000000-N","DRUMS","","",522,36.931034482758598,19278]
[null,"4435000000-N","CONES","","",136,1.70588235294118,232]
[null,"4445000000-E","BARRICADES (TYPE III)","","",528,25.186363636363598,13298.4]
[null,"4455000000-N","FLAGGER","","",930,349.93548387096803,325440]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",9,8706.6666666666697,78360]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",10,2723,27230]
[null,"4480000000-N","TMA","","",2,39300,78600]
[null,"4485000000-E","PORT CONC BARRIER","","",2119,42.831760264275601,90760.5]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",2060,64.410194174757294,132685]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",40,41.5,1660]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",1875,20.1264,37737]
[null,"4510000000-N","LAW ENFORCEMENT","","",1800,60.75,109350]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",390,5,1950]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",18579,1.2161973195543401,22595.73]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",650,3.35,2177.5]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",27,156,4212]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(IV)","",560,3,1680]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",130881,0.32276839266203999,42244.25]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",468,4.2510683760683801,1989.5]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",20,89.25,1785]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",32660,0.64246785058175004,20983]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",111,5.9765765765765799,663.4]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",10,90,900]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES,","(4\", 20MILS) (STANDARD GLASS  BEADS)",21440,1,21440]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\"","20 MILS (STANDARD GLASS BEADS)",8228,1.8,14810.4]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",4460,1.55,6913]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (24\", 90 MILS)",75,14.7,1102.5]
[null,"","","","LINES (24\", 90MILS)",130,10.35,1345.5]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",50,74,3700]
[null,"","","","PAVEMENT MARKERS",30,109,3270]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",100,11.15,1115]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",75,87.3333333333333,6550]
[null,"5255000000-N","PORTABLE LIGHTING","","",1,85000,85000]
[null,"5325200000-E","2\" WATER LINE","","",40,72.64,2905.6]
[null,"5326200000-E","12\" WATER LINE","","",1743,83.99,146394.57]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",1380,8.5399999999999991,11785.2]
[null,"5536000000-E","2\" VALVE","","",1,1080.55,1080.55]
[null,"5558000000-E","12\" VALVE","","",1,3631.95,3631.95]
[null,"5648000000-N","RELOCATE WATER METER","","",6,1166.48,6998.88]
[null,"5649000000-N","RECONNECT WATER METER","","",2,592.94000000000005,1185.8800000000001]
[null,"5686500000-E","WATER SERVICE LINE","","",241,21.32,5138.12]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",1777,11.83,21021.91]
[null,"5815000000-N","REMOVE WATER METER","","",1,426.47,426.47]
[null,"5836000000-E","24\" ENCASEMENT PIPE","","",100,155.91,15591]
[null,"5872500000-E","BORE & JACK **\"","(24\")","",40,661.62,26464.799999999999]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",33035,2.05401846526411,67854.5]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",1740,36.399281609195398,63334.75]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",7505,25.334110592938,190132.5]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",4645,26.259418729817,121975]
[null,"6015000000-E","TEMPORARY MULCHING","","",39.6,1117.42424242424,44250]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",2500,2.12,5300]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",14.5,1077.58620689655,15625]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",2355,10.12983014862,23855.75]
[null,"6029000000-E","SAFETY FENCE","","",6520,2.5412576687116601,16569]
[null,"6030000000-E","SILT EXCAVATION","","",10630,7.8451552210724396,83394]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",72720,1.60527365236524,116735.5]
[null,"6037000000-E","COIR FIBER MAT","","",6655,5.8029301277235197,38618.5]
[null,"6038000000-E","PERM SOIL REINF MAT","","",390,7.1551282051282099,2790.5]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",4090,4.3913202933985298,17960.5]
[null,"6045000000-E","**\" TEMPORARY PIPE","(18\")","",725,41,29725]
[null,"6046000000-E","TEMP PIPE FOR STREAM CROSS","","",25,59,1475]
[null,"6048000000-E","FLOAT TURBIDITY CURTAIN","","",325,5,1625]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",47,281.276595744681,13220]
[null,"6071010000-E","WATTLE","","",90,10,900]
[null,"6071012000-E","COIR FIBER WATTLE","","",850,6.4705882352941204,5500]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",3500,8,28000]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",1435,3.5210801393728199,5052.75]
[null,"6071030000-E","COIR FIBER BAFFLE","","",1615,7.5232198142414903,12150]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",2,1000,2000]
[null,"","","(2-1/2\")","",1,1031,1031]
[null,"6084000000-E","SEEDING AND MULCHING","","",47.1,2253.1847133758001,106125]
[null,"6087000000-E","MOWING","","",34.299999999999997,82.507288629737602,2830]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",600,3.2625000000000002,1957.5]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",2.5,773,1932.5]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",1300,4.3846153846153797,5700]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",35.75,929.16083916083903,33217.5]
[null,"6111000000-E","IMPERVIOUS DIKE","","",615,79.016260162601597,48595]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",60,54,3240]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",226,58.6194690265487,13248]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",18,1063.3333333333301,19140]
[null,"6123000000-E","REFORESTATION","","",2.1,2199.5238095238101,4619]
[null,"6138000000-E","GENERIC EROSION CONTROL ITEM (CY)","ASTM C-33 FINE AGGREGATE","",36,155,5580]
[null,"","","SHREDDED HARDWOOD MULCH","",9,135,1215]
[null,"6141000000-E","GENERIC EROSION CONTROL ITEM (SY)","EXCELSIOR NATURAL FIBER MAT-  TING","",3722,2.5,9305]
[null,"7060000000-E","SIGNAL CABLE","","",2200,5.2,11440]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",18,935,16830]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",7,1560,10920]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",850,4.4000000000000004,3740]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",11,430,4730]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",1,680,680]
[null,"7360000000-N","WOOD POLE","","",4,1380,5520]
[null,"7372000000-N","GUY ASSEMBLY","","",10,440,4400]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",3,740,2220]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",2250,2.7,6075]
[null,"7481000000-N","SITE SURVEY","","",5,1700,8500]
[null,"7481200000-N","LUMINAIRE ARM FOR VIDEO SYSTEM","","",5,680,3400]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",3,5550,16650]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",1,7820,7820]
[null,"7481280000-N","RELOCATE CAMERA SENSOR UNIT","","",8,570,4560]
[null,"7576000000-N","METAL STRAIN SIGNAL POLE","","",3,15600,46800]
[null,"7613000000-N","SOIL TEST","","",3,1930,5790]
[null,"7614100000-E","DRILLED PIER FOUND","","",18,1250,22500]
[null,"7636000000-N","SIGN FOR SIGNALS","","",5,430,2150]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",1,1250,1250]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",5,125,625]
[null,"7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",1,15900,15900]
[null,"7901000000-N","CABINET BASE EXTENDER","","",1,430,430]
[null,"8017000000-N","CM&R TEMP ACCESS ***********","(164+30.00 -L-)","",1,326500,326500]
[null,"","","(23+80.00 -L-)","",1,37700,37700]
[null,"","","(34+65.50 -L-)","",1,472950,472950]
[null,"8021000000-N","REMV EXIST STR **********","(23+80.00 -L-)","",1,88330,88330]
[null,"","","(34+65.50 -L-)","",1,608438.31000000006,608438.31000000006]
[null,"8035000000-N","REMV EXIST STR **********","(15+23.00 -L-)","",1,33750,33750]
[null,"","","(16+62.00-L-)","",1,50000,50000]
[null,"","","(164+30.00 -L-)","",1,250000,250000]
[null,"","","(18+28.00 -L-)","",1,52350,52350]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",6,1384.1666666666699,8305]
[null,"8096000000-E","PILE EXCAVATION IN SOIL","","",78,312,24336]
[null,"8097000000-E","PILE EXCAVATION NOT IN SOIL","","",25,312,7800]
[null,"8105500000-E","**'-**\" DRILLD PIER IN SOIL","(5'-0\")","",320.32,1401.3437812187799,448878.44]
[null,"8105520000-E","3'-0\" DRILLD PIER IN SOIL","","",81,1313.46913580247,106391]
[null,"8105600000-E","**'-**\" DRILLD PIER NO SOIL","(5'-0\")","",317,1361.78567823344,431686.06]
[null,"8105620000-E","3'-0\" DRILLD PIER NO SOIL","","",91,1289.16483516484,117314]
[null,"8111000000-E","PERM STL CASING FOR ** PIER","(5'-0\")","",146.32,574.15848824494299,84010.87]
[null,"8111200000-E","PERM STL CASING FOR 3' PIER","","",26,240,6240]
[null,"8113000000-N","SID INSPECTIONS","","",2,1465,2930]
[null,"8114000000-N","SPT TESTING","","",4,1465,5860]
[null,"8115000000-N","CSL TESTING","","",5,3185,15925]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(15+23.00 -L-)","",1,2700,2700]
[null,"","","(16+62.00-L-)","",1,5000,5000]
[null,"","","(164+30.00 -L-)","",1,14900,14900]
[null,"","","(18+28.00 -L-)","",1,2500,2500]
[null,"","","(23+80.00 -L-)","",1,6790,6790]
[null,"8126000000-N","CULV EXCAV @ ************","(19+90.69 -Y2-)","",1,19250,19250]
[null,"","","(46+80.60 -L-)","",1,13400,13400]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",263,58.79,15461.77]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",74709,36.293227857420099,2711430.76]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",71509,0.54290676698037998,38822.720000000001]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",1336,904.97005239521002,1209039.99]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",413.8,681.06000483325295,281822.63]
[null,"8210000000-N","BRG APPR SLAB ***********","(15+23.00 -L-)","",1,27350,27350]
[null,"","","(16+62.00-L-)","",1,25000,25000]
[null,"","","(164+30.00 -L-)","",1,204500,204500]
[null,"","","(18+28.00 -L-)","",1,25150,25150]
[null,"","","(23+80.00 -L-)","",1,36770,36770]
[null,"","","(34+65.50 -L-)","",1,42525,42525]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",277262,1.2919701942566999,358214.24]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",42581,2.5217195462765098,107377.34]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",56423,1.57,88584.11]
[null,"8274000000-E","63\" MOD PRESTR CONC GIRDR","","",1377.92,381,524987.52]
[null,"8277000000-E","72\" MOD PRESTR CONC GIRDR","","",4246.04,307.16000084784901,1304213.6499999999]
[null,"8280000000-E","STRUCTURAL STEEL","","",1437000,2.7313848295059202,3925000]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",18,1130,20340]
[null,"","","(HP 14 X 73)","",28,393,11004]
[null,"","","(HP12 X 53)","",24,521.09166666666704,12506.2]
[null,"","","(HP12X53)","",35,490.52,17168.2]
[null,"8364000000-E","HP12X53 PILES","","",2128,44.2399953007519,94142.71]
[null,"8384000000-E","HP14X73 PILES","","",815,126,102690]
[null,"8391000000-N","STEEL PILE POINTS","","",42,170.142857142857,7146]
[null,"8392500000-E","PREDRILLING FOR PILES","","",250,40,10000]
[null,"8475000000-E","TWO BAR METAL RAIL","","",518.99,132,68506.679999999993]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",2684.88,104.109211584875,279520.74]
[null,"8504000000-E","CONC BARR RAIL MOMENT SLAB","","",500,342,171000]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",500.88,123.57003673534599,61893.760000000002]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",551.16,119,65588.039999999994]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",3543,20.185345752187398,71516.679999999993]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",3936,3.3797510162601601,13302.7]
[null,"8654000000-N","DISC BEARINGS","","",1,59000,59000]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",6,12271.666666666701,73630]
[null,"8692000000-N","FOAM JOINT SEALS","","",2,20395,40790]
[null,"8762000000-E","3'-0\"X 1'-9\"PRESTR SLABS","","",520,143,74360]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",2310,164.839393939394,380779]
[null,"8802014000-E","SOLDIER PILE RETAINING WALLS","","",1955,200,391000]
[null,"8802016000-E","ANCHORED RETAINING WALLS","","",6330,271,1715430]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL SURFACE TREAT-  MENT","",1955,15.05,29422.75]
[null,"","","SHEET PILE CUTOFF WALL","",5730,53,303690]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","BRIDGE DECK DE-ICING SYSTEM","",1,795000,795000]
[null,"","","STRIP SEAL EXPANSION JOINTS","",1,115000,115000]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FIBER OPTIC CONDUIT SYSTEM","",488.3,36.248699569936498,17700.240000000002]

{"sheet":"ITEMS - DIV 12","index":14,"n_rows":99,"n_cols":8,"rows_kept":99,"cut":false,"hidden":false,"merged":[[7,1,7,7]]}
[null,"Information"]
[null,"Author","PHIGGINS",null,"Last Refreshed","3/9/2022 14:05:49"]
[null,"Current User","HLUCAS",null,"Key Date","3/9/2022"]
[null,"Last Changed by","PHIGGINS",null,"Changed At","8/23/2013 10:16:36"]
[null,"InfoProvider","ZSPCI_C01",null,"Status of Data","3/1/2022 23:17:51"]
[null,"Query Technical Name","Y_SPX_ITEMLISTSUPPDESCSDIV",null,"Relevance of Data (Date)","3/1/2022"]
[null,"Query Description","Item List with Supplemental Descriptions (Bid Averages)",null,"Relevance of Data (Time)","23:17:51"]
[null,"2019 BID AVERAGES - DIVISION 12"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",1,27700,27700]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",1,8500,8500]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(17+68.00 -L-)","",1,5275,5275]
[null,"0043000000-N","GRADING","","",1,98800,98800]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",1,1,1]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",450,1,450]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",400,1,400]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",700,2.25,1575]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",20,30,600]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",40,2.25,90]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",12,38,456]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",88,41,3608]
[null,"1099500000-E","SHALLOW UNDERCUT","","",100,15,1500]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",200,28,5600]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",110,28,3080]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",25,28,700]
[null,"1275000000-E","PRIME COAT","","",50,50,2500]
[null,"1330000000-E","INCIDENTAL MILLING","","",210,22,4620]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",90,91.32,8218.7999999999993]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",110,86.32,9495.2000000000007]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",230,79.97,18393.099999999999]
[null,"1575000000-E","ASP FOR PLANT MIX","","",25,534.09,13352.25]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",10,1,10]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",45,1,45]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",200,0.01,2]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",34,1,34]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",200,1,200]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",1,1,1]
[null,"2077000000-E","6\" OUTLET PIPE","","",6,1,6]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",2,1500,3000]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",1,1200,1200]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",1,700,700]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",40,75,3000]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",50,22,1100]
[null,"3045000000-E","SBGR SHOP CURVED","","",50,23.5,1175]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",5,1,5]
[null,"3180000000-N","GR ANCHOR TYPE **********","(III SHOP CURVED)","",1,1900,1900]
[null,"3195000000-N","GR END TYPE AT-1","","",1,600,600]
[null,"3215000000-N","GR ANCHOR TYPE III","","",3,1800,5400]
[null,"3287000000-N","GR END TYPE TL-3","","",3,3000,9000]
[null,"3635000000-E","RIP RAP, CLASS II","","",100,46,4600]
[null,"3649000000-E","RIP RAP, CLASS B","","",3,38,114]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",570,2.25,1282.5]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",102,10,1020]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",102,6,612]
[null,"4430000000-N","DRUMS","","",50,1,50]
[null,"4435000000-N","CONES","","",50,1,50]
[null,"4445000000-E","BARRICADES (TYPE III)","","",64,18.5,1184]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",1940,2.67,5179.8]
[null,"4905000000-N","SNOWPLB PVMT MRKER","","",6,200,1200]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",1100,2.5,2750]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",100,1,100]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",30,38,1140]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",90,32.5,2925]
[null,"6015000000-E","TEMPORARY MULCHING","","",0.3,800,240]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",100,2,200]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",0.5,100,50]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",200,1,200]
[null,"6029000000-E","SAFETY FENCE","","",380,3,1140]
[null,"6030000000-E","SILT EXCAVATION","","",40,10,400]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",350,2.5,875]
[null,"6037000000-E","COIR FIBER MAT","","",100,7,700]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",130,4,520]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",3,50,150]
[null,"6071010000-E","WATTLE","","",20,20,400]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",5,10,50]
[null,"6084000000-E","SEEDING AND MULCHING","","",0.3,2000,600]
[null,"6087000000-E","MOWING","","",0.15,400,60]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",50,2,100]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",0.25,100,25]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",50,2,100]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",0.25,100,25]
[null,"6111000000-E","IMPERVIOUS DIKE","","",180,35,6300]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",10,5,50]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",13,25,325]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",2,460,920]
[null,"8035000000-N","REMV EXIST STR **********","(17+68.00 -L-)","",1,44850,44850]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",1,1625,1625]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(17+68.00 -L-)","",1,2000,2000]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",26.4,1148.2799242424201,30314.59]
[null,"8210000000-N","BRG APPR SLAB ***********","(17+68.00 -L-)","",1,25200,25200]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",3930,1.57,6170.1]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",10,525,5250]
[null,"8364000000-E","HP12X53 PILES","","",275,54.46,14976.5]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",130.25,137.16,17865.09]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",139,46,6394]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",156,2.25,351]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",1,1950,1950]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",650,173.82,112983]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FIBER OPTIC CONDUIT SYSTEM","",126.25,50.609980198019798,6389.51]

{"sheet":"ITEMS - DIV 13","index":15,"n_rows":483,"n_cols":8,"rows_kept":483,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 13"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",5,1253096,6265480]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",2,906500,1813000]
[null,"0000900000-N","GENERIC MISCELLANEOUS ITEM (LS)","ALETERNATE LUMP SUM BID FOR","BRIDGE #580312",null,null,0]
[null,"","","DESIGN & CONSTRUCTION OF","BRIDGES",1,2082600,2082600]
[null,"","","DESIGN & CONSTRUCTION OF CUL-","VERT #100536",1,809374,809374]
[null,"","","","VERT #110237",1,585301,585301]
[null,"0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","END BENTS STRUCTURE #100142","",2,35000,70000]
[null,"","","END BENTS STRUCTURE #110145","",2,32000,64000]
[null,"","","END BENTS STRUCTURE #580312","",2,47000,94000]
[null,"","","END BENTS STRUCTURE #600207","",2,35000,70000]
[null,"","","INTERIOR BENT CAPS STRUCTURE  #580312","",1,30000,30000]
[null,"","","RIGHT OF WAY ACQUISITION","",12,8166.6666666666697,98000]
[null,"0000930000-E","GENERIC MISCELLANEOUS ITEM (LF)","AVE FOUNDATION LENGTH AT END","BENT #1 STRUCTURE #100142",13,4500,58500]
[null,"","","","BENT #1 STRUCTURE #110145",25,685,17125]
[null,"","","","BENT #1 STRUCTURE #580312",18,1,18]
[null,"","","","BENT #1 STRUCTURE #600207",30,960,28800]
[null,"","","","BENT #2 STRUCTURE #100142",10,5800,58000]
[null,"","","","BENT #2 STRUCTURE #110145",22,780,17160]
[null,"","","","BENT #2 STRUCTURE #580312",16,1,16]
[null,"","","","BENT #2 STRUCTURE #600207",20,1000,20000]
[null,"","","AVE FOUNDATION LENGTH AT INTE-","RIOR BENT #1 STRUCTURE #580312",28,5500,154000]
[null,"","","BRIDGE LENGTH STRUCTURE       #100142","",50,3300,165000]
[null,"","","BRIDGE LENGTH STRUCTURE       #110145","",70,3200,224000]
[null,"","","BRIDGE LENGTH STRUCTURE       #580312","",110,3300,363000]
[null,"","","BRIDGE LENGTH STRUCTURE       #600207","",55,3320,182600]
[null,"0001000000-E","CLEARING & GRUBBING","","",113,44753.185840708,5057110]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",5,8450,42250]
[null,"0015000000-N","SEALING ABANDONED WELLS","","",3,3300,9900]
[null,"0022000000-E","UNCLASSIFIED EXCAVATION","","",2860000,5.3,15158000]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(20+88.94 -Y19-)","",1,43500,43500]
[null,"","","(26+65.52 -Y3-)","",1,67600,67600]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(774+41.49 -L3- LT)","",1,93000,93000]
[null,"","","(774+41.49 -L3- RT)","",1,93000,93000]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(12+94.70 -L-)","",1,25000,25000]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",13500,9.9499999999999993,134325]
[null,"0043000000-N","GRADING","","",1,49300,49300]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",1,1000,1000]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",450,10,4500]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",25650,7,179550]
[null,"0141000000-E","BERM DITCH CONSTRUCTION","","",1810,5.9,10679]
[null,"0156000000-E","REMOVAL OF EXT ASPHALT PVMT","","",47600,3.75,178500]
[null,"0163000000-E","REMOVAL OF EXT CONC PVMT","","",3400,11.25,38250]
[null,"0177000000-E","BREAKING OF EXT ASPH PVMT","","",7500,2,15000]
[null,"0192000000-N","PROOF ROLLING","","",100,248,24800]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",11900,63.382352941176499,754250]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",54200,2.2726014760147599,123175]
[null,"0199000000-E","TEMPORARY SHORING","","",151,40,6040]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",100,102,10200]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",8233,38.1034616786105,313705.8]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",25874,3.8003091906933602,98329.2]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",2500,57.051200000000001,142628]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",1796,67,120332]
[null,"0335400000-E","24\" DRAINAGE PIPE","","",1328,86.75,115204]
[null,"0335500000-E","30\" DRAINAGE PIPE","","",1036,132,136752]
[null,"0335600000-E","36\" DRAINAGE PIPE","","",264,129,34056]
[null,"0335700000-E","42\" DRAINAGE PIPE","","",32,179,5728]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",2,300,600]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",96,65,6240]
[null,"0354000000-E","***\" RC PIPE CULV *****","(54\", V)","",352,488,171776]
[null,"0366000000-E","15\" RC PIPE CULV III","","",14496,59.75,866136]
[null,"0372000000-E","18\" RC PIPE CULV III","","",6076,64.75,393421]
[null,"0378000000-E","24\" RC PIPE CULV III","","",4800,81.25,390000]
[null,"0384000000-E","30\" RC PIPE CULV III","","",3316,108,358128]
[null,"0390000000-E","36\" RC PIPE CULV III","","",1700,129,219300]
[null,"0396000000-E","42\" RC PIPE CULV III","","",1256,164,205984]
[null,"0402000000-E","48\" RC PIPE CULV III","","",544,212,115328]
[null,"0408000000-E","54\" RC PIPE CULV III","","",836,372,310992]
[null,"0426000000-E","72\" RC PIPE CULV III","","",24,650,15600]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",172,75.25,12943]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",272,124,33728]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",36,170,6120]
[null,"0536000000-E","***\" HDPE PIPE CULVTS","(8\")","",44,74.75,3289]
[null,"0576000000-E","**\" CS PIPE CULV *****\"","(36\", 0.079\")","",672,198,133056]
[null,"","","(42\", 0.109\")","",588,275,161700]
[null,"","","(60\", 0.138\")","",56,530,29680]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",2012,114,229368]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",2360,115,271400]
[null,"0594000000-E","24\" CS PIPE CULV 0.064\"","","",784,137,107408]
[null,"0600000000-E","30\" CS PIPE CULV 0.079\"","","",648,166,107568]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",16,780,12480]
[null,"","","(18\". 0.064\")","",14,910,12740]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(36\", 0.500\")","",346,850,294100]
[null,"","","(42\", 0.625\")","",276,960,264960]
[null,"","","(66\", 0.875\")","",122,2040,248880]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(36\", 0.500\")","",346,2150,743900]
[null,"","","(42\", 0.625\")","",276,2380,656880]
[null,"","","(66\", 0.875\")","",122,2620,319640]
[null,"0995000000-E","PIPE REMOVAL","","",4749,30.0495683301748,142705.4]
[null,"0996000000-N","PIPE CLEAN OUT","","",4,1550,6200]
[null,"1000000000-E","6\" SLOPE PROTECTION","","",310,108,33480]
[null,"1011000000-N","FINE GRADING","","",1,1000000,1000000]
[null,"1044000000-E","LIME TRTD SOIL (SLURRY)","","",184940,3.35,619549]
[null,"1066000000-E","LIME FOR LIME TREATED SOIL","","",2220,279,619380]
[null,"1099500000-E","SHALLOW UNDERCUT","","",15100,24.9006622516556,376000]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",40000,28.109500000000001,1124380]
[null,"1110000000-E","STABILIZER AGGREGATE","","",1500,38.700000000000003,58050]
[null,"1115000000-E","GEOTEXTILE FOR PVMT STABILIZ","","",129200,4.25,549100]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",92450,30.7718766901028,2844860]
[null,"1176000000-E","SOIL CEMENT BASE","","",184940,3.35,619549]
[null,"1187000000-E","PC FOR SOIL CEMENT BASE","","",5179,240,1242960]
[null,"1209000000-E","ASPHALT CURING SEAL","","",55490,2.75,152597.5]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",10050,36.293532338308502,364750]
[null,"1231000000-E","SHOULDER BORROW","","",38000,13,494000]
[null,"1275000000-E","PRIME COAT","","",317,13.2618927444795,4204.0200000000004]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",6870,9.35,64234.5]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 3\")","",6200,12.35,76570]
[null,"1330000000-E","INCIDENTAL MILLING","","",5939.2,18.715493669181001,111155.06]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",28947,72.565835837910697,2100563.25]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",43600,76,3313600]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",23244,86.880356220960294,2019447]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",34220,70.25,2403955]
[null,"1575000000-E","ASP FOR PLANT MIX","","",7007,803.73911802483201,5631800]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",1000,197,197000]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",92000,0.15,13800]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","7\" CONCRETE TRUCK APRON","",590,110,64900]
[null,"2000000000-N","RIGHT-OF-WAY MARKERS","","",591,412.690355329949,243900]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",1388.8,11.6612903225806,16195.2]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",2200,4.6818181818181799,10300]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",336,71,23856]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",369.6,69.772727272727295,25788]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",4200,12.9047619047619,54200]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",9,682.22222222222194,6140]
[null,"2077000000-E","6\" OUTLET PIPE","","",54,65.7777777777778,3552]
[null,"2099000000-E","SHOULDER DRAIN","","",20800,9.6999999999999993,201760]
[null,"2110000000-E","4\" SHOULDER DRAIN PIPE","","",20832,1.75,36456]
[null,"2121000000-E","4\" OUTLET PIPE FOR SHDR DRN","","",2036,14.7,29929.200000000001]
[null,"2132000000-N","CONC PAD SHLDR DRN OUTLET","","",40,341,13640]
[null,"2143000000-E","BLOTTING SAND","","",20,82.75,1655]
[null,"2209000000-E","ENDWALLS","","",41.4,1770,73278]
[null,"2220000000-E","REINFORCED ENDWALLS","","",24.3,2080,50544]
[null,"2253000000-E","PIPE COLLARS","","",6.4130000000000003,2260,14493.38]
[null,"2264000000-E","PIPE PLUGS","","",1.504,2260,3399.04]
[null,"2275000000-E","FLOWABLE FILL","","",137,413,56581]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",436,3517.6605504587201,1533700]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",24.72,2230,55125.599999999999]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",546.70000000000005,560,306152]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",54,960,51840]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",42,960.95238095238096,40360]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",172,960,165120]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",7,960,6720]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",1,960,960]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",7,960,6720]
[null,"","","(F)","",42,960,40320]
[null,"","","(G)","",31,960,29760]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",41,960,39360]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",15,1240,18600]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",34,1460,49640]
[null,"2462000000-E","**\" SLUICE GATE","(8\")","",2,3080,6160]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","ENERGY DISSIPATOR BASIN","",17,14500,246500]
[null,"2535000000-E","**\"X**\" CONCRETE CURB","(8\" X 12\")","",230,29.3,6739]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",18400,30,552000]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",5326,39.3839654524972,209759]
[null,"2577000000-E","CONC EXPRESSWAY GUTTER","","",750,45.6,34200]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",5480,54,295920]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",6,2250,13500]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",560,78.75,44100]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",177,90,15930]
[null,"2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",8850,73,646050]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",490,74.75,36627.5]
[null,"2703000000-E","CONC BARRIER TYPE ******","(SINGLE SLOPE)","",655,145,94975]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",5350,102,545700]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","2'-0\" MODIFIED VALLEY GUTTER","",360,56.25,20250]
[null,"2759000000-N","GENERIC PAVING ITEM (EA)","VERTICAL CONCRETE BARRIER     TRANSITION","",2,5710,11420]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",2,8130,16260]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",29550,26.8849407783418,794450]
[null,"3045000000-E","SBGR SHOP CURVED","","",1475,28.6,42185]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",40,49.0625,1962.5]
[null,"3195000000-N","GR END TYPE AT-1","","",9,1010,9090]
[null,"3210000000-N","GR END TYPE CAT-1","","",23,1040,23920]
[null,"3215000000-N","GR ANCHOR TYPE III","","",8,1243.25,9946]
[null,"3287000000-N","GR END TYPE TL-3","","",44,3900,171600]
[null,"3288000000-N","GR END TYPE TL-2","","",27,1300.74074074074,35120]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",20,2750,55000]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",7400,1.1000000000000001,8140]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",610,7.8770491803278704,4805]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(III)","",4,750,3000]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",4,2000,8000]
[null,"","","(TL-3)","",2,2470,4940]
[null,"3389400000-E","DBL FACED CABLE GUIDERAIL","","",13200,11.15,147180]
[null,"3389500000-N","ADDITIONAL GUIDERAIL POSTS","","",10,86.25,862.5]
[null,"3389600000-N","CBL GUIDERAIL ANCH UNIT","","",40,1850,74000]
[null,"3435000000-N","GENERIC GUARDRAIL ITEM (EA)","PERMANENT BOLLARDS","",6,500,3000]
[null,"","","REMOVABLE BOLLARDS","",3,1060,3180]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNITS,","TYPE CAT-1",1,300,300]
[null,"3503000000-E","WOVEN WIRE FENCE 47\" FAB","","",60960,3.1,188976]
[null,"3509000000-E","4\" TIMBER POSTS 7'-6\"LONG","","",3730,22.4,83552]
[null,"3515000000-E","5\" TIMBER POSTS 8'-0\"LONG","","",1170,33.6,39312]
[null,"3565000000-E","DBL GATE **HIGH, **WIDE, **OPEN","(47\", 8', 16')","",1,2020,2020]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","BIKE AND PEDESTRIAN SAFETY    RAIL","",810,170,137700]
[null,"","","ORNAMENTAL WOOD FENCE","",100,140,14000]
[null,"3628000000-E","RIP RAP, CLASS I","","",3500,58,203000]
[null,"3635000000-E","RIP RAP, CLASS II","","",6625,60,397500]
[null,"3649000000-E","RIP RAP, CLASS B","","",6480,45.832870370370401,296997]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",44775,5.09262981574539,228022.5]
[null,"4048000000-E","REINF CONC FOUNDTN","","",12,1140,13680]
[null,"4054000000-E","PLN CONC FOUNDTN","","",2,11.4,22.8]
[null,"4057000000-E","OVERHEAD FOOTING","","",30,11.4,342]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",4817,9.1,43834.7]
[null,"4066000000-E","SUPPORTS, SIMPLE STL BM","","",6948,9.1,63226.8]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",6316,9.0737808739708701,57310]
[null,"4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",10,114,1140]
[null,"4082100000-N","SUPPORT, OVRHD SIGN STR STA ****","(861+15 -L3-)","",1,204900,204900]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",5,171,855]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",343,84.780612244897995,29079.75]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",73,171,12483]
[null,"4109000000-N","SIGN ERECTION, TYPE *** (OVRHD)","(A)","",3,1.1499999999999999,3.45]
[null,"","","(B)","",2,1.1499999999999999,2.2999999999999998]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",18,910,16380]
[null,"","","(B)","",9,455,4095]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",9,171,1539]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(D)","",3,228,684]
[null,"","","(E)","",3,228,684]
[null,"","","(F)","",2,228,456]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",103,6.9310679611650503,713.9]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",4,2.2999999999999998,9.1999999999999993]
[null,"4238000000-N","DISPOSE SIGN, D, E, F","","",12,2.2999999999999998,27.6]
[null,"4360000000-N","GENERIC SIGNING ITEM (EA)","ADVANCE WARNING FLASHING BEA-","CON ASSEMBLY",3,8610,25830]
[null,"","","RRFB ASSEMBLY","",4,9380,37520]
[null,"4370000000-N","GENERIC SIGNING ITEM (LS)","DISPOSAL OF FLASHER SYSTEM","",1,1600,1600]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",2880,6.8256249999999996,19657.8]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",1120,19.620044642857099,21974.45]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",616,6.4035714285714302,3944.6]
[null,"4415000000-N","FLASHING ARROW BOARD","","",7,1828.75,12801.25]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",8,6347.4375,50779.5]
[null,"4424500000-N","TEMP PORT TRAF SIGNAL SYS","","",2,12575.5,25151]
[null,"4430000000-N","DRUMS","","",1120,53.491071428571402,59910]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",66,123.454545454545,8148]
[null,"4435000000-N","CONES","","",75,19.066666666666698,1430]
[null,"4445000000-E","BARRICADES (TYPE III)","","",472,27.688135593220299,13068.8]
[null,"4447000000-E","PED CHANNEL DEVICES","","",153,40.2009803921569,6150.75]
[null,"4455000000-N","FLAGGER","","",736,307.59510869565202,226390]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",2,6480,12960]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",2,3300,6600]
[null,"4480000000-N","TMA","","",4,27290.6,109162.4]
[null,"4485000000-E","PORT CONC BARRIER","","",1800,38.700000000000003,69660]
[null,"4500000000-E","REM & RES PORT CONC BARRIER","","",1800,6.9,12420]
[null,"4507000000-E","WATER FILLED BARRIER","","",700,92.5,64750]
[null,"4508000000-E","REM & RES H2O FILL BARR","","",700,17.55,12285]
[null,"4510000000-N","LAW ENFORCEMENT","","",64,66.25,4240]
[null,"4516000000-N","SKINNY DRUM","","",245,45.6,11172]
[null,"4520000000-N","TUBULAR MARKERS (FIXED)","","",68,75,5100]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",1618,8.85,14319.3]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",1687,1.75,2952.25]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",26,154,4004]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",223,191,42593]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",8682,2.5,21705]
[null,"","","(IV)","",8695,3.1608970672800498,27484]
[null,"4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(IV)","",302,8.85,2672.7]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(II)","",1072,5.4,5788.8]
[null,"4785000000-E","12\" COLD PLSTIC LINES TYPE **","(II)","",91,9.5500000000000007,869.05]
[null,"4795000000-E","24\" COLD APPL PLSTIC LINE TYPE **","(IV)","",80,28.35,2268]
[null,"4805000000-N","COLD APPL PLASTIC SYM TYPE **","(I)","",2,1410,2820]
[null,"","","(II)","",14,283.3,3966.2]
[null,"","","(IV)","",10,180.3,1803]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",304296,0.26193558245918003,79705.95]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",23546,0.25,5886.5]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",1400,1.2,1680]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",576,2.0499999999999998,1180.8]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",814,1.91891891891892,1562]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",76,71,5396]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",37650,1.2946879150066399,48745]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",800,2.35,1880]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",110,11.25,1237.5]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",25,104.44,2611]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","POLYUREA PAVEMENT MARKING     LINES, 12\"","20 MILS (STANDARD GLASS BEADS)",10194,2.35,23955.9]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 4\",","20 MILS (STANDARD GLASS BEADS)",88625,0.90641748942171996,80331.25]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",112564,0.9,101307.6]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 8\",","20 MILS (STANDARD GLASS BEADS)",1844,3.25,5993]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (24\", 90 MILS)",430,5.9,2537]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",1606,53.25,85519.5]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",8,29.6,236.8]
[null,"4915000000-E","7' U-CHANNEL POSTS","","",48,74,3552]
[null,"4955000000-N","OBJECT MARKERS (END OF RD)","","",54,96.75,5224.5]
[null,"5325200000-E","2\" WATER LINE","","",1350,67,90450]
[null,"5325600000-E","6\" WATER LINE","","",2515,120,301800]
[null,"5325800000-E","8\" WATER LINE","","",960,116,111360]
[null,"5326000000-E","10\" WATER LINE","","",5790,120,694800]
[null,"5326200000-E","12\" WATER LINE","","",3130,139,435070]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",8349,7.7,64287.3]
[null,"5536000000-E","2\" VALVE","","",5,1500,7500]
[null,"5540000000-E","6\" VALVE","","",35,2060,72100]
[null,"5546000000-E","8\" VALVE","","",4,2870,11480]
[null,"5552000000-E","10\" VALVE","","",22,4250,93500]
[null,"5558000000-E","12\" VALVE","","",6,5370,32220]
[null,"5571600000-E","6\" TAPPING SLEEVE & VALVE","","",1,9250,9250]
[null,"5606000000-E","2\" BLOW OFF","","",5,2510,12550]
[null,"5648000000-N","RELOCATE WATER METER","","",9,1110,9990]
[null,"5649000000-N","RECONNECT WATER METER","","",12,1280,15360]
[null,"5666000000-N","FIRE HYDRANT","","",2,5010,10020]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",15,780,11700]
[null,"5673000000-E","FIRE HYDRANT LEG","","",305.89999999999998,92.5,28295.75]
[null,"5686000000-E","**\" H2O SERVICE LINE","(2\")","",94.7,94.750052798310406,8972.83]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",7698.23,214,1647421.22]
[null,"5691400000-E","10\" SANITARY GRAVITY SEWER","","",1888.1,230,434263]
[null,"5691500000-E","12\" SANITARY GRAVITY SEWER","","",1337.25,260,347685]
[null,"5709200000-E","4\" FORCE MAIN SEWER","","",3117,356,1109652]
[null,"5709400000-E","8\" FORCE MAIN SEWER","","",310,530,164300]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",43,4500,193500]
[null,"5776000000-E","5' DIA UTILITY MANHOLE","","",19,7270,138130]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",139,320,44480]
[null,"5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",215,436,93740]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",4983.8,18.399999999999999,91701.92]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",4827,17.75,85679.25]
[null,"5804000000-E","ABANDON 12\" UTILITY PIPE","","",584,21.7,12672.8]
[null,"5815000000-N","REMOVE WATER METER","","",26,271,7046]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",270,250,67500]
[null,"5835800000-E","18\" ENCASEMENT PIPE","","",1468,309,453612]
[null,"5836000000-E","24\" ENCASEMENT PIPE","","",1386,332,460152]
[null,"5912000000-N","GENERIC UTILITY ITEM (LS)","UTILITY COORDINATOR","",1,745200,745200]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",144400,3.0193905817174498,436000]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",8950,46.191061452513999,413410]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",40950,45.068376068376097,1845550]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",19420,44.374613800205999,861755]
[null,"6015000000-E","TEMPORARY MULCHING","","",712,971.16573033707903,691470]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",27800,3.6086330935251798,100320]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",142,2010.3169014084499,285465]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",28325,16.787290379523402,475500]
[null,"6029000000-E","SAFETY FENCE","","",11720,2.29556313993174,26904]
[null,"6030000000-E","SILT EXCAVATION","","",250980,2.373695115149E-2,5957.5]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",893165,1.45059563462518,1295621.25]
[null,"6037000000-E","COIR FIBER MAT","","",2740,8.0481751824817493,22052]
[null,"6038000000-E","PERM SOIL REINF MAT","","",32000,4.0999999999999996,131200]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",22780,7.5411545215100997,171787.5]
[null,"6045000000-E","**\" TEMPORARY PIPE","(36\")","",135,193,26055]
[null,"6046000000-E","TEMP PIPE FOR STREAM CROSS","","",125,85.5,10687.5]
[null,"6069000000-E","STILLING BASINS","","",210,27.6,5796]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",10,1500,15000]
[null,"6071010000-E","WATTLE","","",40,15,600]
[null,"6071012000-E","COIR FIBER WATTLE","","",14930,11.05,164976.5]
[null,"6071013000-E","WATTLE BARRIER","","",31250,14.35,448437.5]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",17740,13.2524661781285,235098.75]
[null,"6071030000-E","COIR FIBER BAFFLE","","",27845,7.7565990303465604,215982.5]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",75,5770,432750]
[null,"","","(2\")","",18,8630,155340]
[null,"","","(2-1/2\")","",13,11400,148200]
[null,"","","(3\")","",1,14800,14800]
[null,"6084000000-E","SEEDING AND MULCHING","","",366,2181.9672131147499,798600]
[null,"6087000000-E","MOWING","","",251.5,121.95228628230601,30671]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",7300,11.042808219178101,80612.5]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",19.5,1606.41025641026,31325]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",9550,4.4083769633507899,42100]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",284.25,2009.63060686016,571237.5]
[null,"6111000000-E","IMPERVIOUS DIKE","","",880,89.71875,78952.5]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",190,80.763157894736807,15345]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",225,0.34,76.5]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",34,1550,52700]
[null,"6120000000-E","CULVERT DIVERSION CHANNEL","","",1010,14.1,14241]
[null,"6123000000-E","REFORESTATION","","",0.1,4000,400]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",100,166,16600]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",33,204,6732]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",4,1100,4400]
[null,"7060000000-E","SIGNAL CABLE","","",7500,3.3,24750]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",32,1100,35200]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",11,1210,13310]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",3,1660,4980]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",550,6.6,3630]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 2\")","",550,13.25,7287.5]
[null,"","","(2, 2\")","",405,16.55,6702.75]
[null,"","","(4, 2\")","",310,24.3,7533]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",200,17.649999999999999,3530]
[null,"","","(2, 2\")","",575,26.5,15237.5]
[null,"","","(3, 2\")","",100,32,3200]
[null,"","","(4, 2\")","",275,39.700000000000003,10917.5]
[null,"","","(5, 2\")","",150,47.5,7125]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",8,660,5280]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",10,1050,10500]
[null,"7360000000-N","WOOD POLE","","",4,1100,4400]
[null,"7372000000-N","GUY ASSEMBLY","","",7,610,4270]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",2,830,1660]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",3,1050,3150]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",3800,12.331578947368399,46860]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",11100,2.7459459459459499,30480]
[null,"7481000000-N","SITE SURVEY","","",1,1930,1930]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",3,4640,13920]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",1,7180,7180]
[null,"7575142010-N","900MHZ SER/ETH SPEC RADIO","","",10,4860,48600]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",10,20400,204000]
[null,"7590000000-N","DBL MAST ARM WITH METAL POLE","","",2,27500,55000]
[null,"7613000000-N","SOIL TEST","","",12,1600,19200]
[null,"7614100000-E","DRILLED PIER FOUND","","",84,1100,92400]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",12,110,1320]
[null,"7636000000-N","SIGN FOR SIGNALS","","",14,276,3864]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",7,2320,16240]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",4,2210,8840]
[null,"7696000000-N","CONTLRS WITH CBNT (**************)","(2070E, BASE MOUNTED)","",4,17700,70800]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",22,276,6072]
[null,"7901000000-N","CABINET BASE EXTENDER","","",4,610,2440]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,2760,2760]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",1,3860,3860]
[null,"7972000000-N","METAL POLE REMOVAL","","",1,1660,1660]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","2070E CONTROLLER","",6,4640,27840]
[null,"","","PROTECTIVE COATING FOR DUAL","MAST ARM POLE (BLACK)",2,2090,4180]
[null,"","","PROTECTIVE COATING FOR SIGNAL","PEDESTAL (BLACK)",7,110,770]
[null,"","","PROTECTIVE COATING FOR SINGLE","MAST ARM POLE (BLACK)",10,1380,13800]
[null,"8007000000-N","CM&R TEMP STR ***********","(13+24.00 -DET-)","",1,175000,175000]
[null,"8035000000-N","REMV EXIST STR **********","(12+94.70 -L-)","",1,20000,20000]
[null,"8056000000-N","REMV EXIST STR **********","(874+45.00 -L3-)","",1,38600,38600]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",2,5660,11320]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 20+88.94 -Y19-)","",1,22200,22200]
[null,"8105560000-E","4'-0\" DRILLD PIER IN SOIL","","",50,1040,52000]
[null,"8105660000-E","4'-0\" DRILLD PIER NO SOIL","","",50,1040,52000]
[null,"8115000000-N","CSL TESTING","","",1,3860,3860]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(12+94.70 -L-)","",1,10000,10000]
[null,"8126000000-N","CULV EXCAV @ ************","(735+38.59 -L3-)","",1,247200,247200]
[null,"","","(797+66.00 -L3-)","",1,130100,130100]
[null,"","","(830+02.00 -L3-)","",1,278700,278700]
[null,"","","(874+45.00 -L3-)","",1,92100,92100]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",2287,82.75,189249.25]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",38861,42.3,1643820.3]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",120441.4,0.59936873865631002,72188.81]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",656.4,1380.7617306520399,906332]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",5708.1,442,2522980.2000000002]
[null,"8210000000-N","BRG APPR SLAB ***********","(12+94.70 -L-)","",1,38000,38000]
[null,"","","(20+88.94 -Y19-)","",1,55100,55100]
[null,"","","(26+65.52 -Y3-)","",1,110600,110600]
[null,"","","(774+41.49 -L3- LT)","",1,66200,66200]
[null,"","","(774+41.49 -L3- RT)","",1,66200,66200]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",104980,1.3126004953324399,137796.79999999999]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",7072,2.7,19094.400000000001]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",920565,1.55,1426875.75]
[null,"8265000000-E","54\" PRESTR CONCRETE GIRDR","","",2104.67,361,759785.87]
[null,"8277000000-E","72\" MOD PRESTR CONC GIRDR","","",2254.9,399,899705.1]
[null,"8296000000-N","POLLUTION CONTROL","","",1,60000,60000]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",72,484,34848]
[null,"","","(HP 14 X 73)","",30,399,11970]
[null,"","","(HP12X53)","",14,500,7000]
[null,"8364000000-E","HP12X53 PILES","","",4251,71.144142554693005,302433.75]
[null,"8384000000-E","HP14X73 PILES","","",940,97,91180]
[null,"8391000000-N","STEEL PILE POINTS","","",32,301.875,9660]
[null,"8392500000-E","PREDRILLING FOR PILES","","",249,141.64658634538199,35270]
[null,"8475000000-E","TWO BAR METAL RAIL","","",609.92999999999995,121.113176921942,73870.559999999998]
[null,"8482000000-E","THREE BAR METAL RAIL","","",343.92,188,64656.959999999999]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",407.2,154,62708.800000000003]
[null,"8504000000-E","CONC BARR RAIL MOMENT SLAB","","",268,451,120868]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",277.14,130,36028.199999999997]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-2\" X 2'-6\")","",504.55,113,57014.15]
[null,"","","(1'-2\" X 2'-9 1/2\")","",130,200,26000]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",2278,90,205020]
[null,"8559000000-E","SURFACE PREP, CLASS II","","",813.8,44,35807.199999999997]
[null,"8566000000-E","SURFACE PREP, CLASS III","","",14.9,1150,17135]
[null,"8590000000-E","RIP RAP, CLASS **","(II)","",32,72.75,2328]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",140,45,6300]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",1847,5.0094748240389801,9252.5]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",2,12750,25500]
[null,"8660000000-E","CONCRETE REPAIRS","","",11.6,613,7110.8]
[null,"8664000000-E","SHOTCRETE REPAIRS","","",319.5,562.70000000000005,179782.65]
[null,"8678000000-E","EPOXY RESIN INJECTION","","",788.3,77.3,60935.59]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",780,200,156000]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",6350,94.75,601662.5]
[null,"","","(2)","",4335,116,502860]
[null,"","","(6)","",4665,101,471165]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL SURFACE TREAT-  MENT","",149026,2.35,350211.1]
[null,"","","SOUND BARRIER WALL NO -NW11-","",18303,39.1,715647.3]
[null,"","","SOUND BARRIER WALL NO -NW13-","",26005,39.1,1016795.5]
[null,"","","SOUND BARRIER WALL NO -NW15-","",7308,39.299999999999997,287204.40000000002]
[null,"","","SOUND BARRIER WALL NO -NW5A-","",14210,39.1,555611]
[null,"","","SOUND BARRIER WALL NO -NW5B-","",8208,39.1,320932.8]
[null,"","","SOUND BARRIER WALL NO -NW8-","",18010,39.299999999999997,707793]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","CLEANING & PAINTING OF EXIST-","ING WEATHING STEEL FOR BRIDGE 495",1,123000,123000]
[null,"","","CLEANING & REPAINTING OF","BRIDGE #705",1,1025045.4,1025045.4]
[null,"","","MOLDED RUBBER SEGMENTAL EXPAN-SION JOINT","",1,150000,150000]
[null,"","","PAINTING CONTAINMENT FOR","BRIDGE #481",1,10302,10302]
[null,"","","","BRIDGE #495",1,51510,51510]
[null,"","","","BRIDGE 705",1,412080,412080]
[null,"","","SPOT PAINTING OF STEEL STRUC-","TURE REPAIR AREAS",1,30906,30906]
[null,"","","VOLUMETRIC MIXER","",1,80000,80000]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","FOAM JOINT SEALS FOR PRESERVA-TION","",571.29999999999995,55,31421.5]
[null,"","","POURABLE SILICONE JOINT       SEALANT","",284.39999999999998,42,11944.8]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","LATEX MODIFIED CONCRETE OVER-","LAY - EARLY STRENGTH",434.2,1081,469370.2]
[null,"8882000000-E","GENERIC STRUCTURE ITEM (CF)","CONCRETE FOR DECK REPAIR","",1772.3,14.3,25343.89]
[null,"","","ELASTOMERIC CONCRETE FOR PRES-ERVATION","",135.1,280,37828]
[null,"8889000000-E","GENERIC STRUCTURE ITEM (LB)","BEAM REPAIR","",745.1,60,44706]
[null,"","","BOLTED BEAM REPAIR","",226.1,185,41828.5]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","BRIDGE JOINT DEMOLITION","",530.4,45,23868]
[null,"","","EPOXY COATING","",4422.1000000000004,5.1500011306845197,22773.82]
[null,"","","JOINT REPAIR","",373,275,102575]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","HYDRO-DEMOLITION OF BRIDGE    DECK","",9383.2000000000007,53,497309.6]
[null,"","","PLACING & FINISHING LATEX MOD-","IFIED CONCRETE OVERLAY - EARLYSTRENGTH",9383.2000000000007,30,281496]
[null,"","","SCARIFYING BRIDGE DECK","",9383.2000000000007,25,234580]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","TYPE I BRIDGE JACKING BRIDGE  481","",7,3700,25900]
[null,"","","TYPE I BRIDGE JACKING BRIDGE  495","",2,3700,7400]

{"sheet":"ITEMS - DIV 14","index":16,"n_rows":567,"n_cols":8,"rows_kept":567,"cut":false,"hidden":false,"merged":[[0,1,0,7]]}
[null,"2021 BID AVERAGES - DIVISION 14"]
[null,"Item ","Item Description ","Item Supplemental Description","Item Supplemental Description 2","Item Quantity","Average Unit Bid","Extended Amt"]
[null,"0000100000-N","MOBILIZATION","","",12,555312,6663744]
[null,"0000400000-N","CONSTRUCTION SURVEYING","","",6,195962.243333333,1175773.46]
[null,"0000915000-N","GENERIC MISCELLANEOUS ITEM (EA)","WILDLIFE GUARDS","",4,106451,425804]
[null,"","","WILDLIFE JUMP OUTS","",3,14245,42735]
[null,"0008000000-E","SUPP CLEARING & GRUBBING","","",1,10065,10065]
[null,"0015000000-N","SEALING ABANDONED WELLS","","",7,750,5250]
[null,"0028000000-N","TYPE I STANDARD APPR **********","(35+30.22 -L-)","",1,70000,70000]
[null,"0029000000-N","TYPE III REINFORCED APPR **********","(28+62 -L-)","",1,284948,284948]
[null,"0030000000-N","TYPE II MODIFIED APPR **********","(15+45.00 -L-)","",1,23200,23200]
[null,"0036000000-E","UNDERCUT EXCAVATION","","",850,54.705882352941202,46500]
[null,"0043000000-N","GRADING","","",6,1172041.5,7032249]
[null,"0050000000-E","SUPP CLEARING & GRUBBING","","",5,4590.2,22951]
[null,"0057000000-E","UNDERCUT EXCAVATION","","",900,20.3611111111111,18325]
[null,"0134000000-E","DRAINAGE DITCH EXCAVATION","","",3860,10.906735751295299,42100]
[null,"0194000000-E","SELECT GRANULAR MATL, CLASS III","","",450,49,22050]
[null,"0195000000-E","SELECT GRANULAR MATERIAL","","",850,93.352941176470594,79350]
[null,"0196000000-E","GEOTEXTILE SOIL STABILIZATION","","",4105,2.9043848964677199,11922.5]
[null,"0199000000-E","TEMPORARY SHORING","","",10890,62.240404040404002,677798]
[null,"0255000000-E","GENERIC GRADING ITEM (TON)","HAULING AND DISPOSAL OF PETRO-","LEUM CONTAMINATED SOIL",200,100,20000]
[null,"0318000000-E","FND CONDIT MATL MINOR STRS","","",2410,46.518672199170098,112110]
[null,"0320000000-E","FND CONDIT GEOTEXTILE","","",7150,4.6302097902097898,33106]
[null,"0335200000-E","15\" DRAINAGE PIPE","","",228,75.859649122806999,17296]
[null,"0335300000-E","18\" DRAINAGE PIPE","","",140,87.471428571428604,12246]
[null,"0335400000-E","24\" DRAINAGE PIPE","","",76,80,6080]
[null,"0335850000-E","**\" DRAINAGE PIPE ELBOW","(15\")","",4,622,2488]
[null,"0343000000-E","15\" SIDE DRAIN PIPE","","",52,48,2496]
[null,"0344000000-E","18\" SIDE DRAIN PIPE","","",24,66.5,1596]
[null,"0366000000-E","15\" RC PIPE CULV III","","",1188,71.1245791245791,84496]
[null,"0372000000-E","18\" RC PIPE CULV III","","",1168,60,70080]
[null,"0378000000-E","24\" RC PIPE CULV III","","",1544,108.181347150259,167032]
[null,"0384000000-E","30\" RC PIPE CULV III","","",468,189.91452991452999,88880]
[null,"0390000000-E","36\" RC PIPE CULV III","","",116,143,16588]
[null,"0396000000-E","42\" RC PIPE CULV III","","",100,271.68,27168]
[null,"0448000000-E","***\" RCP CULV CLASS IV","(60\")","",12,736,8832]
[null,"0448200000-E","15\" RCP CULV CLASS IV","","",2824,99.328611898017002,280504]
[null,"0448300000-E","18\" RCP CULV CLASS IV","","",2464,187.58279220779201,462204]
[null,"0448400000-E","24\" RCP CULV CLASS IV","","",1496,172.28342245989299,257736]
[null,"0448500000-E","30\" RCP CULV CLASS IV","","",3284,199.79537149817301,656128]
[null,"0448600000-E","36\" RCP CULV CLASS IV","","",480,237,113760]
[null,"0448700000-E","42\" RCP CULV CLASS IV","","",1300,351.89230769230801,457460]
[null,"0536000000-E","***\" HDPE PIPE CULVTS","(18\")","",20,44.5,890]
[null,"0576000000-E","**\" CS PIPE CULV *****\"","(18\", 0.079\")","",340,190,64600]
[null,"","","(24\", 0.109\")","",156,250,39000]
[null,"","","(30\", 0.138\")","",1876,315,590940]
[null,"","","(36\", 0.138\")","",1004,375,376500]
[null,"0582000000-E","15\" CS PIPE CULV 0.064\"","","",680,75,51000]
[null,"0588000000-E","18\" CS PIPE CULV 0.064\"","","",76,164.47368421052599,12500]
[null,"0636000000-E","**\" CS ELBOW *****\" THICK","(15\", 0.064\")","",10,750,7500]
[null,"","","(18\", 0.079\")","",4,2125,8500]
[null,"","","(24\", 0.109\")","",3,2675,8025]
[null,"","","(30\", 0.138\")","",20,4000,80000]
[null,"","","(36\", 0.138')","",15,4925,73875]
[null,"0654000000-E","***X***\"CSP ARCH CULV *****","(95\" X 67\", 0.109\")","",84,922,77448]
[null,"0973100000-E","**\"WLD STL PIPE GRAD B IN SOIL","(18\", 0.500\")","",52,1025,53300]
[null,"","","(42\", 0.625\")","",44,321,14124]
[null,"","","(54\", 0.750\")","",218,2000,436000]
[null,"0973300000-E","**\"WLD STL PIPE GRAD B NOT IN SOIL","(18\", 0.500\")","",52,3400,176800]
[null,"","","(42\", 0.625\")","",44,415,18260]
[null,"","","(54\", 0.750\")","",218,3800,828400]
[null,"0986000000-E","GENERIC PIPE ITEM (LF)","15\" PIPE REHABILITATION CIPP  LINER","",92,245,22540]
[null,"","","18\" PIPE REHABILITATION CIPP  LINER","",688,290,199520]
[null,"","","18\" PIPE REHABILITATION SMOOTH","WALL STEEL SLIP LINER",40,400,16000]
[null,"","","24\" PIPE REHABILITATION CIPP  LINER","",364,400,145600]
[null,"","","30\" PIPE REHABILITATION CIPP  LINER","",262,405,106110]
[null,"","","36\" PIPE REHABILITATION CIPP  LINER","",176,500,88000]
[null,"","","42\" PIPE REHABILITATION","SOLID WALL THERMOPLASTIC SLIP LINER",604,325,196300]
[null,"","","42\" PIPE REHABILITATION CIPP  LINER","",140,850,119000]
[null,"","","42\" PIPE REHABILITATION SMOOTH","WALL STEEL SLIP LINER",88,994,87472]
[null,"","","54\" PIPE REHABILITATION CIPP  LINER","",150,414,62100]
[null,"","","PIPE REHABILITATION CIPP LINER","(15\" ID HOST PIPE)",258,164,42312]
[null,"","","","(18\" ID HOST PIPE)",650,169,109850]
[null,"","","","(24\" ID HOST PIPE)",550,185,101750]
[null,"","","","(8\" ID HOST PIPE)",404,72,29088]
[null,"","","PRE INSTALLATION INSPECTION","",88,5.2,457.6]
[null,"","","PRE-INSTALLATION INSPECTION","",2522,50,126100]
[null,"","","PREINSTALLATION INSPECTION","",1862,7,13034]
[null,"0992000000-E","GENERIC PIPE ITEM (EA)","DE-WATERING","",1,7260,7260]
[null,"","","STANDARD CAST IRON MANHOLE","FRAME AND VENTED MANHOLE GRATE",35,500,17500]
[null,"0995000000-E","PIPE REMOVAL","","",6540,20.205504587156,132144]
[null,"0996000000-N","PIPE CLEAN OUT","","",50,910,45500]
[null,"1077000000-E","#57 STONE","","",6,230,1380]
[null,"1099500000-E","SHALLOW UNDERCUT","","",742,26.450134770889498,19626]
[null,"1099700000-E","CLASS IV SUBGRD STABILIZATION","","",1380,52.898550724637701,73000]
[null,"1121000000-E","AGGREGATE BASE COURSE","","",6953,43.9137063138214,305332]
[null,"1220000000-E","INCIDENTAL STONE BASE","","",1175,42.212765957446798,49600]
[null,"1245000000-E","SHOULDER RECONSTRUCTION","","",89.33,7421.1687003246398,662933]
[null,"1297000000-E","MILL ASP PVMT *****\" DTH","(1-1/2\")","",661276,2.8130157453166298,1860179.8]
[null,"","","(2\")","",273063,1.8781731688291701,512859.6]
[null,"","","(2-1/2\")","",121510,3.05,370605.5]
[null,"","","(3\")","",1500,5,7500]
[null,"","","(3/4\")","",3540,28,99120]
[null,"","","(4\")","",138084,5.4527982966889699,752944.2]
[null,"","","(4-1/2\")","",21589,6.5,140328.5]
[null,"","","(5-1/4\")","",99218,8.5,843353]
[null,"1308000000-E","MILLN ASPHALT PVMT ***** - *****","(0\" TO 1-1/2\")","",31600,3.2,101120]
[null,"","","(0\" TO 2\")","",570,24,13680]
[null,"","","(0\" TO 3\")","",11030,4.8119673617407104,53076]
[null,"1330000000-E","INCIDENTAL MILLING","","",4277,18.1917231704466,77806]
[null,"1491000000-E","ASP CONC BASE CRS B25.0C","","",13290,96.206433408577894,1278583.5]
[null,"1503000000-E","ASP CONC INTR CRS I19.0C","","",70921,78.086264999083497,5537956]
[null,"1519000000-E","ASP CONC SURF CRS S9.5B","","",30955,72.329833629462101,2238970]
[null,"1520000000-E","ASP CONC SURF CRS S9.5B LEVEL","","",2825,75,211875]
[null,"1523000000-E","ASP CONC SURF CRS S9.5C","","",187383,71.798604996184295,13453838]
[null,"1524200000-E","ASP CONC SURF CRS S9.5D","","",28081,98.168868630034495,2756680]
[null,"1575000000-E","ASP FOR PLANT MIX","","",17706,566.70620128769895,10034100]
[null,"1577000000-E","POLYM MOD ASP BNDR FOR PLT MIX","","",3469,806.24243297780299,2796855]
[null,"1662000000-E","OG ASP FRICT FC-1 MOD","","",28584,108.676882171844,3106420]
[null,"1693000000-E","ASPH PLT MIX PVMT REPAIR","","",1181.5999999999999,194.165538253216,229426]
[null,"1704000000-E","PATCHING EXIST PAVEMENT","","",6124,158.61267145656399,971344]
[null,"1839140000-E","ULTRATHIN BOND WEAR CRS","","",7380,125,922500]
[null,"1840000000-E","MILLED RUMBLE STRIPS","","",470898,0.22685753602691,106826.76]
[null,"1891000000-E","GENERIC PAVING ITEM (SY)","4\" CONCRETE PAD FOR PIPES","UNDER FENCE",30,111,3330]
[null,"1925000000-E","MILL RUMBLE STRPS (CONC SHLDR)","","",10661,1,10661]
[null,"2022000000-E","SUBDRAIN EXCAVATION","","",1545.4,18.628769250679401,28788.9]
[null,"2026000000-E","GEOTEXTILE FOR SUBSURF DRNS","","",6500,4.16,27040]
[null,"2033000000-E","SUBDRAIN FINE AGGREGATE","","",33.6,72,2419.1999999999998]
[null,"2036000000-E","SUBDRAIN COARSE AGGREGATE","","",1093.2,103.046103183315,112650]
[null,"2044000000-E","6\" PERF SUBDRN PIPE","","",6700,15.9402985074627,106800]
[null,"2070000000-N","SUBDRN PIPE OUTLET","","",17,752.94117647058795,12800]
[null,"2077000000-E","6\" OUTLET PIPE","","",102,54.588235294117702,5568]
[null,"2190000000-N","TEMP STL PLT COVER FOR MDS","","",8,1301.25,10410]
[null,"2209000000-E","ENDWALLS","","",9.6,2592.8125,24891]
[null,"2220000000-E","REINFORCED ENDWALLS","","",18.399999999999999,2591.0869565217399,47676]
[null,"2253000000-E","PIPE COLLARS","","",2.5499999999999998,3432.8431372548998,8753.75]
[null,"2264000000-E","PIPE PLUGS","","",2.0710000000000002,539.44954128440395,1117.2]
[null,"2275000000-E","FLOWABLE FILL","","",457,310.16411378555802,141745]
[null,"2286000000-N","MASNRY DRAINAGE STRUCT","","",252,5825.5714285714303,1468044]
[null,"2297000000-E","MASNRY DRAINAGE STRUCT","","",46,2035.1739130434801,93618]
[null,"2308000000-E","MASNRY DRAINAGE STRUCT","","",355.2,365.98873873873902,129999.2]
[null,"2352000000-N","FRAME W/GRATE 840.***** STD","(840.36)","",2,900,1800]
[null,"2354200000-N","FRAME W/GRATE 840.24 STD","","",1,540,540]
[null,"2364000000-N","FRAME W/2GRTS 840.16 STD","","",3,1400,4200]
[null,"2364200000-N","FRAME W/2GRTS 840.20 STD","","",37,816.21621621621603,30200]
[null,"2365000000-N","FRAME W/2GRTS 840.22 STD","","",32,877.625,28084]
[null,"2366000000-N","FRAME W/2GRTS 840.24 STD","","",19,783.15789473684197,14880]
[null,"2367000000-N","FRAME W/2GRTS 840.29 STD","","",3,715,2145]
[null,"2374000000-N","FRAME-GRT-HD 840.03 **","(E)","",14,1021.42857142857,14300]
[null,"","","(F)","",36,988.33333333333303,35580]
[null,"","","(G)","",31,943.74193548387098,29256]
[null,"2396000000-N","FRAME W/COVER STD 840.54","","",22,860.68181818181802,18935]
[null,"2407000000-N","STL FRAM W/ 2 GTR, STD 840.37","","",36,2434.1666666666702,87630]
[null,"2451000000-N","CONC TRANS SECT FOR DROP INLET","","",2,1100,2200]
[null,"2473000000-N","GENERIC DRAINAGE ITEM (EA)","DE-WATERING","",16,3200,51200]
[null,"","","HINGED GRATE","",5,2500,12500]
[null,"","","SPECIAL DESIGN PIPE CONNECTION","",85,1800,153000]
[null,"2535000000-E","**\"X**\" CONCRETE CURB","(8\" X 12\")","",50,30,1500]
[null,"","","(8\" X 18\")","",320,29,9280]
[null,"2542000000-E","1'-6\" CONC CURB & GUTTER","","",300,32,9600]
[null,"2549000000-E","2'-6\" CONC CURB & GUTTER","","",11697,30.369838420107701,355236]
[null,"2556000000-E","SHOULDER BERM GUTTER","","",5850,42.677777777777798,249665]
[null,"2591000000-E","4\" CONCRETE SIDEWALK","","",4431,47.7499435793275,211580]
[null,"2605000000-N","CONCRETE CURB RAMPS","","",52,2148.0769230769201,111700]
[null,"2612000000-E","6\" CONCRETE DRIVEWAY","","",290,67.827586206896598,19670]
[null,"2613000000-N","REM & REP CURB RAMPS","","",45,3000,135000]
[null,"2619000000-E","4\" CONCRETE PAVED DITCH","","",5982,108.950852557673,651744]
[null,"2647000000-E","5\" MONO CONC ISLANDS (SURF MTD)","","",420,69,28980]
[null,"2655000000-E","5\" MONO CONC ISLDS (KEY IN)","","",20,71,1420]
[null,"2703000000-E","CONC BARRIER TYPE ******","(SINGLE SLOPE)","",3502,200,700400]
[null,"","","(T)","",392,147,57624]
[null,"","","(TI)","",809,193,156137]
[null,"2724000000-E","PC REINF BARRIER SNGL FC","","",190,273,51870]
[null,"2738000000-E","GENERIC PAVING ITEM (SY)","12\" CONCRETE TRUCK APRON","",445,150,66750]
[null,"","","6\" CONCRETE PAVED DITCH","",1220,175,213500]
[null,"2752000000-E","GENERIC PAVING ITEM (LF)","2'-6\" CONCRETE CURB & GUTTER","(TINTED CONCRETE)",170,52.5,8925]
[null,"2800000000-N","ADJ CATCH BASINS","","",1,1500,1500]
[null,"2815000000-N","ADJ DROP INLETS","","",2,2500,5000]
[null,"2830000000-N","ADJ MANHOLES","","",19,1482.10526315789,28160]
[null,"2845000000-N","ADJ METER OR VALVE BOXES","","",53,993.86792452830196,52675]
[null,"3001000000-N","IMPACT ATTEN TYPE TL-3","","",1,22200,22200]
[null,"3030000000-E","STL BEAM GUARDRAIL","","",15236.5,23.1624749778492,352915.05]
[null,"3045000000-E","SBGR SHOP CURVED","","",150,27.3333333333333,4100]
[null,"3145000000-E","EX LENGTH GR POST ** STL","(8')","",890,100,89000]
[null,"3150000000-N","ADDIT GUARDRAIL POSTS","","",20,74.25,1485]
[null,"3195000000-N","GR END TYPE AT-1","","",2,720,1440]
[null,"3210000000-N","GR END TYPE CAT-1","","",6,828,4968]
[null,"3215000000-N","GR ANCHOR TYPE III","","",4,1890,7560]
[null,"3287000000-N","GR END TYPE TL-3","","",6,3015,18090]
[null,"3288000000-N","GR END TYPE TL-2","","",2,3496,6992]
[null,"3289000000-N","GR END TYPE MEDIAN TL-3","","",3,3607,10821]
[null,"3317000000-N","GR ANCHOR TYPE B-77","","",10,1938.7,19387]
[null,"3360000000-E","REMOVE EXISTING GUARDRAIL","","",18621,1.5120535954030401,28155.95]
[null,"3380000000-E","TEMP STL BM GUARDRAIL","","",362.5,9.3000000000000007,3371.25]
[null,"3382000000-E","TEMP STL BM GDRAIL, SHP CURV","","",37.5,10.5,393.75]
[null,"3387000000-N","TEMP GDRL ANCH UNITS ******","(B-77)","",1,1270,1270]
[null,"","","(III)","",4,1240,4960]
[null,"3389150000-N","TEMP GDRL END UNITS *****","(TL-2)","",2,1660,3320]
[null,"","","(TL-3)","",2,1870,3740]
[null,"3420000000-E","GENERIC GUARDRAIL ITEM (LF)","POWDER COATED GALVANIZED","STEEL BEAM GUARDRAIL",1925,45,86625]
[null,"","","","STEEL BEAM GUARDRAIL, SHOP    CURVED",162.5,47,7637.5]
[null,"3435000000-N","GENERIC GUARDRAIL ITEM (EA)","POWDER COATED GALVANIZED","25' CLEAR SPAN GUARDRAIL      SECTIONS",1,4170,4170]
[null,"","","","ADDITIONAL GUARDRAIL POSTS",10,90,900]
[null,"","","","GUARDRAIL ANCHOR UNITS,       TYPE III",1,3315,3315]
[null,"","","","GUARDRAIL END UNITS, TYPE AT-1",3,1145,3435]
[null,"","","","GUARDRAIL END UNITS, TYPE TL-2",4,4175,16700]
[null,"3436000000-N","GENERIC GUARDRAIL ITEM (EA) 862","TEMPORARY GUARDRAIL END UNIT","TYPE AT-1",2,311,622]
[null,"3566000000-E","WOVEN WIRE FENCE RESET","","",200,18,3600]
[null,"3572000000-E","CHAIN LINK FENCE RESET","","",680,29,19720]
[null,"3575000000-E","GENERIC FENCING ITEM (LF)","WILDLIFE FENCE","",3880,22,85360]
[null,"3578000000-N","GENERIC FENCING ITEM (EA)","WILDLIFE DOUBLE GATES 9' HIGH, 6' WIDE,","12' OPENING",1,5550,5550]
[null,"","","WILDLIFE FENCE POST 4\", 13'","",221,53,11713]
[null,"","","WILDLIFE FENCE POST 5\", 13'","",108,139,15012]
[null,"3628000000-E","RIP RAP, CLASS I","","",1222,79.670212765957402,97357]
[null,"3635000000-E","RIP RAP, CLASS II","","",625,65,40625]
[null,"3642000000-E","RIP RAP, CLASS A","","",57,130.438596491228,7435]
[null,"3649000000-E","RIP RAP, CLASS B","","",878,104.66400911161701,91895]
[null,"3651000000-E","BOULDERS","","",20,220,4400]
[null,"3656000000-E","GEOTEXTILE FOR DRAINGE","","",9184,4.1510779616724696,38123.5]
[null,"3691000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE CLEANOUT",15,444,6660]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",15,222,3330]
[null,"4025000000-E","CONTR FURN, TYPE ***SIGN","(D)","",48,13,624]
[null,"","","(E)","",377.6,13,4908.8]
[null,"","","(F)","",89.5,13,1163.5]
[null,"4048000000-E","REINF CONC FOUNDTN","","",2,1332,2664]
[null,"4057000000-E","OVERHEAD FOOTING","","",8,1520,12160]
[null,"4060000000-E","SUPPORT, BREAKAWAY STL BM","","",1447,19,27493]
[null,"4072000000-E","SUPPORT, 3-LB STL U-CHAN","","",1906,13.223294858342101,25203.599999999999]
[null,"4078000000-E","SUPPORT, 2-LB STL U-CHAN","","",4,3.85,15.4]
[null,"4096000000-N","SIGN ERECTION, TYPE D","","",13,284.230769230769,3695]
[null,"4102000000-N","SIGN ERECTION, TYPE E","","",101,273.97029702970298,27671]
[null,"4108000000-N","SIGN ERECTION, TYPE F","","",14,159.28571428571399,2230]
[null,"4110000000-N","SIGN ERECTION, TYPE *** (GRD MTD)","(A)","",2,3086,6172]
[null,"","","(B)","",2,3086,6172]
[null,"4114000000-N","SIGN ERECTION, MILEMARKERS","","",4,21,84]
[null,"4116100000-N","SIGN ERECT, RELOC ** GRD MTD","(E)","",22,204.09090909090901,4490]
[null,"","","(F)","",7,265,1855]
[null,"4152000000-N","DISPOSE SIGN SYST STL BM","","",3,1221,3663]
[null,"4155000000-N","DISPOSE SIGN SYST U-CHAN","","",60,270.66666666666703,16240]
[null,"4192000000-N","DISPOSE SUPPORT, U-CHAN","","",2,5.5,11]
[null,"4400000000-E","WORK ZONE SIGNS (STAT)","","",3241,5.9892471459426098,19411.150000000001]
[null,"4402000000-E","HIGH VISIBILITY STAT SIGNS","","",1988,11.878772635814901,23615]
[null,"4405000000-E","WORK ZONE SIGNS (PORT)","","",770,28.318441558441599,21805.200000000001]
[null,"4407000000-E","HIGH VISIBILITY PORT SIGNS","","",1340,15.414925373134301,20656]
[null,"4410000000-E","WORK ZONE SIGNS (BARR)","","",1234,7.0703403565640199,8724.7999999999993]
[null,"4413000000-E","WORK ZONE ADV/GEN WARN SIGN","","",8871,7.11475030999887,63114.95]
[null,"4415000000-N","FLASHING ARROW BOARD","","",16,2801.125,44818]
[null,"4420000000-N","PORTABLE CHANGE MSG SIGN","","",15,11399.6,170994]
[null,"4422000000-N","PORT CHANGE MSG SIGN (SHORT TERM)","","",120,110.5,13260]
[null,"4423000000-N","WZ DIGITAL SPD LMT SIGNS","","",9,3860,34740]
[null,"4424000000-N","WZ PRESENCE LIGHTING","","",42,3033.3333333333298,127400]
[null,"4430000000-N","DRUMS","","",336,61.178571428571402,20556]
[null,"4432000000-N","HIGH VISIBILITY DRUMS","","",1372,80.231778425656003,110078]
[null,"4434000000-N","SEQ FLASH WARN LIGHTS","","",256,133.625,34208]
[null,"4435000000-N","CONES","","",61,19.327868852459002,1179]
[null,"4445000000-E","BARRICADES (TYPE III)","","",1140,59.578947368420998,67920]
[null,"4447000000-E","PED CHANNEL DEVICES","","",266,21.289473684210499,5663]
[null,"4455000000-N","FLAGGER","","",266,412.81954887218001,109810]
[null,"4457000000-N","TEMP TRAFFIC CONTROL (SP)","","",5,342158.4,1710792]
[null,"4465000000-N","TEMPORARY CRASH CUSHIONS","","",13,12250.1538461538,159252]
[null,"4470000000-N","REM & RES CRASH CUSHION","","",7,5422.7142857142899,37959]
[null,"4480000000-N","TMA","","",9,31643.111111111099,284788]
[null,"4485000000-E","PORT CONC BARRIER","","",1325,44,58300]
[null,"4490000000-E","PORT CONC BARRIER(ANCHRD)","","",17550,68.387464387464405,1200200]
[null,"4505000000-E","REM & RES PORT CONC BARR, ANCH","","",16260,17.003690036900402,276480]
[null,"4507000000-E","WATER FILLED BARRIER","","",823,61.014580801944099,50215]
[null,"4510000000-N","LAW ENFORCEMENT","","",3564,81.965207631874307,292124]
[null,"4516000000-N","SKINNY DRUM","","",60,37,2220]
[null,"4520000000-N","TUBULAR MARKERS (FIXED)","","",16,80,1280]
[null,"4589000000-N","GENERIC TRAFFIC CONTROL ITEM (LS)","DYNAMIC ZIPPER MERGE SYSTEM   DEPLOYMENT","",3,17690.333333333299,53071]
[null,"4600000000-N","GENERIC TRAFFIC CONTROL ITEM (EA)","AUDIBLE WARNING DEVICES","",5,135,675]
[null,"","","CONNECTED LANE CLOSURE DEVICE","",8,1782.5,14260]
[null,"","","CONNECTED LANE CLOSURE DEVICES","",2,2400,4800]
[null,"","","PORTABLE CCTV CAMERA ASSEMBLY","",16,21821,349136]
[null,"","","RAMP/LOOP CLOSURE","",10,900,9000]
[null,"","","RAMP/LOOP TRAFFIC CONTROL","",12,1300,15600]
[null,"","","SIGNS, COVERING","",4,1625.64,6502.56]
[null,"","","SINGLE LANE CLOSURE","",120,1800,216000]
[null,"","","TEMPORARY CURB RAMPS","",2,1300,2600]
[null,"4609000000-N","GENERIC TRAFFIC CONTROL ITEM (DAY)","DYNAMIC ZIPPER MERGE SYSTEM","",577,130.32928942807601,75200]
[null,"4650000000-N","TEMP RAISED PVMT MRKS","","",859,13.88358556461,11926]
[null,"4685000000-E","THERMO PVT MKG LINES 4\"90","","",254222,1.2190915813737599,309919.90000000002]
[null,"4688000000-E","THERMO PVT MKG LINES,6\"90 MILS","","",357767,1.0010420189676501,358139.8]
[null,"4695000000-E","THERMO PVT MKG LINES 8\"90 MILS","","",10602,2.5793906810035798,27346.7]
[null,"4700000000-E","12\"WIDE THERMO 90 MILS","","",12466,4.1436948499919799,51655.3]
[null,"4720000000-E","THERMO PVT MKG CHARACTER 90","","",18,181.666666666667,3270]
[null,"4725000000-E","THERMO PVT SYMBOL 90MILS","","",630,173.37301587301599,109225]
[null,"4726110000-E","HIP THERMO PVT SYMBOL 90 MILS","","",5,55,275]
[null,"4770000000-E","4\" COLD APPL PLSTIC LINES TYPE **","(II)","",400,4.4000000000000004,1760]
[null,"4775000000-E","6\" COLD APPL PLSTIC LINES TYPE **","(II)","",1400,8,11200]
[null,"4780000000-E","8\" COLD APPL PLSTIC LINES TYPE **","(IV)","",180,11.5,2070]
[null,"4810000000-E","PAINT PVMT MARKINGS 4\"","","",2300200,0.18918847056777999,435171.32]
[null,"4815000000-E","PAINT PVMT MARKINGS 6\"","","",506258,0.51603956875742996,261249.16]
[null,"4820000000-E","PAINT PVMT MARKINGS 8\"","","",660,2.6681818181818202,1761]
[null,"4825000000-E","PAINT PVMT MARKINGS 12\"","","",1630,1.48650306748466,2423]
[null,"4835000000-E","PAINT PVT MKG LINES 24\"","","",1350,2.9029629629629601,3919]
[null,"4845000000-N","PAINT PVT MKG SYMBOL","","",87,98.735632183908095,8590]
[null,"4847500000-E","WZ PERF PVMT MKG LINES 6\"","","",47509,0.9,42758.1]
[null,"4850000000-E","LINE REMOVAL 4\" WIDE","","",5000,0.85,4250]
[null,"4855000000-E","LINE REMOVAL 6\" WIDE","","",25639,1.2470455165958101,31973]
[null,"4860000000-E","LINE REMOVAL 8\" WIDE","","",1000,1.7,1700]
[null,"4870000000-E","LINE REMOVAL 24\" WIDE","","",140,10.064285714285701,1409]
[null,"4875000000-N","REMOVAL OF SYMBL & CHARAC","","",16,92,1472]
[null,"4890000000-E","GENERIC PAVEMENT MARKING ITEM (LF)","HOT SPRAY THERMOPLASTIC","PAVEMENT MARKING LINES, 4\", 50 MILS",186560,0.56000000000000005,104473.60000000001]
[null,"","","HOT SPRAY THERMOPLASTIC PAVE-","MENT MARKING LINES, (4\",      50 MILS)",12504,0.72,9002.8799999999992]
[null,"","","HOT SPRAY THERMOPLASTIC PAVEM-","ENT MARKING LINES (4\", 50MILS)",192780,0.72,138801.60000000001]
[null,"","","POLYUREA PAVEMENT MARKING     LINES, 6\",","20 MILS (STANDARD GLASS BEADS)",4950,2,9900]
[null,"4891000000-E","GENERIC PVMT MARKING ITEM (LF) 1205","THERMOPLASTIC PAVEMENT MARKING","LINES (16\", 90 MILS)",64,9.15,585.6]
[null,"","","","LINES (24\", 90 MILS)",5430,12.1263812154696,65846.25]
[null,"4895000000-N","GENERIC PAVEMENT MARKING ITEM (EA)","NON-CAST IRON SNOW-","PLOWABLE PAVEMENT MARKER",992,40,39680]
[null,"","","NON-CAST IRON SNOWPLOWABLE","PAVEMENT MARKER",2707,43.490579977835203,117729]
[null,"","","","PAVEMENT MARKERS",3607,39.301857499306898,141761.79999999999]
[null,"4900000000-N","PERM RAISED PVMT MARKERS","","",34,21.294117647058801,724]
[null,"4915000000-E","7' U-CHANNEL POSTS","","",7,70,490]
[null,"4955000000-N","OBJECT MARKERS (END OF RD)","","",3,250,750]
[null,"4957000000-N","OBJECT MARKERS (TYPE **)","(I)","",4,300,1200]
[null,"5070000000-N","STD FOUNDAT ***********","(TYPE R1)","",31,2400,74400]
[null,"","","(TYPE R2)","",3,2550,7650]
[null,"5155000000-E","ELECT DUCT BD, SIZE *****","(2\")","",2068,10,20680]
[null,"5160000000-E","ELECT DUCT JA, SIZE *****","(2\")","",486,16.5,8019]
[null,"5170000000-E","**-#8 W/G FEEDER CIRCUIT","(2)","",8665,5.2,45058]
[null,"5180000000-E","**-#4 W/G FEEDER CIRCUIT","(2)","",10924,8,87392]
[null,"5240000000-N","ELEC JB ************","(TYPE IG, 13\"W x 24\"L x 18\"D)","",21,750,15750]
[null,"5255000000-N","PORTABLE LIGHTING","","",4,144500,578000]
[null,"5270000000-N","GENERIC LIGHTING ITEM (EA)","DECORATIVE ROADWAY LUMINAIRE","(118W LED)",5,300,1500]
[null,"","","","(140W LED)",9,300,2700]
[null,"","","","(174W LED)",12,300,3600]
[null,"","","","(57W LED)",11,300,3300]
[null,"","","DECORATIVE ROADWAY POLE (22'","MH, DOUBLE 30\" ARM)",1,1000,1000]
[null,"","","","MH, SINGLE 30\" ARM)",1,950,950]
[null,"","","DECORATIVE ROADWAY POLE (25'","MH, DOUBLE 30\" ARM)",2,1000,2000]
[null,"","","","MH, SINGLE 30\" ARM)",30,950,28500]
[null,"","","LIGHTING CONTROL CENTER","",1,15000,15000]
[null,"5319000000-E","CL B CONC FOR ENCAS LINE","","",6,495,2970]
[null,"5325200000-E","2\" WATER LINE","","",769,46.378933680103998,35665.4]
[null,"5325600000-E","6\" WATER LINE","","",733,98.967257844474801,72543]
[null,"5325800000-E","8\" WATER LINE","","",4544,99.701584507042298,453044]
[null,"5326000000-E","10\" WATER LINE","","",1424,116.582162921348,166013]
[null,"5326200000-E","12\" WATER LINE","","",1441,128,184448]
[null,"5329000000-E","DI H2O PIPE FITTINGS","","",13015,11.3614675374568,147869.5]
[null,"5536000000-E","2\" VALVE","","",5,1427.4,7137]
[null,"5540000000-E","6\" VALVE","","",15,2080.9333333333302,31214]
[null,"5546000000-E","8\" VALVE","","",1,2825,2825]
[null,"5552000000-E","10\" VALVE","","",1,3806,3806]
[null,"5558000000-E","12\" VALVE","","",1,4710,4710]
[null,"5571600000-E","6\" TAPPING SLEEVE & VALVE","","",3,5475,16425]
[null,"5571800000-E","8\" TAPPING SLEEVE & VALVE","","",2,5490,10980]
[null,"5572000000-E","10\" TAPPING SLEEVE & VALVE","","",2,12674,25348]
[null,"5572600000-E","16\" TAPPING SLEEVE & VALVE","","",1,18950,18950]
[null,"5589100000-E","1\" AIR RELEASE VALVE","","",13,4705,61165]
[null,"5648000000-N","RELOCATE WATER METER","","",3,2310,6930]
[null,"5649000000-N","RECONNECT WATER METER","","",16,943.625,15098]
[null,"5666000000-N","FIRE HYDRANT","","",11,4970.8181818181802,54679]
[null,"5672000000-N","RELOCATE FIRE HYDRANT","","",1,2350,2350]
[null,"5673000000-E","FIRE HYDRANT LEG","","",71,97.352112676056294,6912]
[null,"5686500000-E","WATER SERVICE LINE","","",471,16.2,7630.2]
[null,"5691300000-E","8\" SANITARY GRAVITY SEWER","","",1534,174,266916]
[null,"5691700000-E","18\" SANITARY GRAVITY SEWER","","",73,507,37011]
[null,"5709300000-E","6\" FORCE MAIN SEWER","","",745,60,44700]
[null,"5768500000-E","SEWER SERVICE LINE","","",6,200,1200]
[null,"5769000000-E","DI SEWER PIPE FITTINGS","","",1550,16.95,26272.5]
[null,"5775000000-E","4' DIA UTILITY MANHOLE","","",13,3881,50453]
[null,"5776000000-E","5' DIA UTILITY MANHOLE","","",2,4318,8636]
[null,"5781000000-E","UTILITY MANHOLE WALL 4' DIA","","",56.8,307,17437.599999999999]
[null,"5782000000-E","UTILITY MANHOLE WALL 5' DIA","","",1.4,425,595]
[null,"5798000000-E","ABANDON **\" UTILITY PIPE","(2\")","",369,21.7,8007.3]
[null,"5800000000-E","ABANDON 6\" UTILITY PIPE","","",6721.5,10.420203823551301,70039.399999999994]
[null,"5801000000-E","ABANDON 8\" UTILITY PIPE","","",1802.5,18.369570041608899,33111.15]
[null,"5802000000-E","ABANDON 10\" UTILITY PIPE","","",1166,20.7,24136.2]
[null,"5811000000-E","ABANDON 18\" UTILITY PIPE","","",129,44.7,5766.3]
[null,"5815500000-N","REMOVE FIRE HYDRANT","","",4,1375,5500]
[null,"5828000000-N","REMOVE UTILITY MANHOLE","","",1,1080,1080]
[null,"5835700000-E","16\" ENCASEMENT PIPE","","",124,285,35340]
[null,"5872500000-E","BORE & JACK **\"","(16\")","",71,3290,233590]
[null,"","","(2\")","",75,26,1950]
[null,"5872600000-E","DIRECT DRILL **\"","(10\")","",258,52,13416]
[null,"6000000000-E","TEMPORARY SILT FENCE","","",48280,4.6238867025683499,223241.25]
[null,"6006000000-E","EROS CONTRL STONE CL A","","",3715,71.722745625841199,266450]
[null,"6009000000-E","EROS CONTRL STONE CL B","","",4605,74.403908794788293,342630]
[null,"6012000000-E","SEDIMENT CONTROL STONE","","",6715,62.489947877885299,419620]
[null,"6015000000-E","TEMPORARY MULCHING","","",41,1319.5609756097599,54102]
[null,"6018000000-E","SEED FOR TEMP SEEDING","","",2350,4.4170212765957402,10380]
[null,"6021000000-E","FERT FOR TEMP SEEDING","","",13.5,1586.6666666666699,21420]
[null,"6024000000-E","TEMPORARY SLOPE DRAINS","","",1200,31.0833333333333,37300]
[null,"6029000000-E","SAFETY FENCE","","",7510,3.3754993342210402,25350]
[null,"6030000000-E","SILT EXCAVATION","","",6590,17.473444613050098,115150]
[null,"6036000000-E","MATTING FOR EROS CONTROL","","",102000,2.3235294117647101,237000]
[null,"6037000000-E","COIR FIBER MAT","","",1233,9.8057583130575807,12090.5]
[null,"6038000000-E","PERM SOIL REINF MAT","","",835,7.0898203592814397,5920]
[null,"6042000000-E","1/4\" HARDWARE CLOTH","","",9885,9.7966110268083,96839.5]
[null,"6045000000-E","**\" TEMPORARY PIPE","(18\")","",55,75,4125]
[null,"","","(36\")","",835,114.760479041916,95825]
[null,"6046000000-E","TEMP PIPE FOR STREAM CROSS","","",50,125,6250]
[null,"6070000000-N","SPECIAL STILLING BASINS","","",36,1374.55555555556,49484]
[null,"6071010000-E","WATTLE","","",520,15.413461538461499,8015]
[null,"6071012000-E","COIR FIBER WATTLE","","",220,12.818181818181801,2820]
[null,"6071014000-E","COIR FIBER WATTLE BARRIER","","",230,12,2760]
[null,"6071020000-E","POLYACRYLAMIDE (PAM)","","",885,13.1059322033898,11598.75]
[null,"6071030000-E","COIR FIBER BAFFLE","","",450,17.663333333333298,7948.5]
[null,"6071050000-E","**\" SKIMMER","(1-1/2\")","",3,983.33333333333303,2950]
[null,"6084000000-E","SEEDING AND MULCHING","","",53,2725.7547169811301,144465]
[null,"6087000000-E","MOWING","","",44.5,245.61797752808999,10930]
[null,"6090000000-E","SEED FOR REPAIR SEEDING","","",800,10.909375000000001,8727.5]
[null,"6093000000-E","FERT FOR REPAIR SEEDING","","",2.5,1799.5,4498.75]
[null,"6096000000-E","SEED FOR SUPP SEEDING","","",1200,11.091666666666701,13310]
[null,"6108000000-E","FERTILIZER TOPDRESSING","","",35,1355.5,47442.5]
[null,"6111000000-E","IMPERVIOUS DIKE","","",398,236.73869346733699,94222]
[null,"6114500000-N","SPECIALIZED HAND MOWING","","",80,129.25,10340]
[null,"6117000000-N","RESPONSE FOR EROS CONTROL","","",475,294.63157894736798,139950]
[null,"6117500000-N","CONC WASHOUT STRUCTURE","","",28,1866.42857142857,52260]
[null,"6123000000-E","REFORESTATION","","",7.7,6297.0779220779204,48487.5]
[null,"6126000000-E","STREAMBANK REFORESTATION","","",1,8880,8880]
[null,"6132000000-N","GENERIC EROSION CONTROL ITEM (EA)","FABRIC INSERT INLET PROTECTION","DEVICE",112,244.55357142857099,27390]
[null,"","","","DEVICE CLEANOUT",455,225.51648351648399,102610]
[null,"","","FABRIC INSERT INLET PROTECTIONDEVICE","",24,410,9840]
[null,"7048500000-E","16\" PEDEST SIG HEAD 1 SEC W/CD","","",2,1000,2000]
[null,"7060000000-E","SIGNAL CABLE","","",1600,3.75,6000]
[null,"7120000000-E","VEHICLE SIGNAL HD (12\", 3 SECT)","","",9,1030,9270]
[null,"7132000000-E","VEHICLE SIGNAL HD (12\", 4 SECT)","","",2,1150,2300]
[null,"7144000000-E","VEHICLE SIGNAL HD (12\", 5 SECT)","","",1,1570,1570]
[null,"7252000000-E","MESSENGER CABLE (1/4\")","","",80,4.5999999999999996,368]
[null,"7264000000-E","MESSENGER CABLE (3/8\")","","",160,4.9000000000000004,784]
[null,"7279000000-E","TRACER WIRE","","",12295,0.65,7991.75]
[null,"7288000000-E","PAVED TRENCH (***********)","(1, 2\")","",300,30.5,9150]
[null,"7300000000-E","UNPAVED TRENCH (***********)","(1, 1\")","",20,10.3,206]
[null,"","","(1, 2\")","",1920,6.6,12672]
[null,"","","(2, 2\")","",30,15.2,456]
[null,"","","(3, 2\")","",11705,7.6,88958]
[null,"7301000000-E","DIRECT DRILL (***********)","(1, 2\")","",225,21,4725]
[null,"","","(2, 2\")","",125,21,2625]
[null,"","","(3, 2\")","",430,24.488372093023301,10530]
[null,"7324000000-N","JUNCTION BOX (STANDARD SIZE)","","",11,381.81818181818198,4200]
[null,"7348000000-N","JUNCTION BOX (OVER-SIZED, HVY-DUTY)","","",1,660,660]
[null,"7360000000-N","WOOD POLE","","",2,1115,2230]
[null,"7372000000-N","GUY ASSEMBLY","","",4,575,2300]
[null,"7408000000-E","1\" RISER WITH WEATHERHEAD","","",1,745,745]
[null,"7420000000-E","2\" RISER WITH WEATHERHEAD","","",2,750,1500]
[null,"7444000000-E","INDUCTIVE LOOP SAWCUT","","",11046,10.295917074054,113728.7]
[null,"7456000000-E","LEAD-IN CABLE(********)","(14-2)","",7531,2.90705085645997,21893]
[null,"7481000000-N","SITE SURVEY","","",1,1150,1150]
[null,"7481240000-N","CAMERA W/O INT LOOP EMUL PROCESS","","",3,3600,10800]
[null,"7481260000-N","EXT LOOP EMULATOR PROCESS UNIT","","",1,8560,8560]
[null,"7516000000-E","COMMUNICATIONS CABLE (** FIBER)","(144)","",27580,3.3,91014]
[null,"7528000000-E","DROP CABLE","","",670,3.05,2043.5]
[null,"7540000000-N","SPLICE ENCLOSURE","","",4,1215,4860]
[null,"7552000000-N","INTERCONNECT CENTER","","",4,1620,6480]
[null,"7566000000-N","DELINEATOR MARKER","","",29,86,2494]
[null,"7588000000-N","SGNL MAST ARM WITH METAL POLE","","",2,20000,40000]
[null,"7613000000-N","SOIL TEST","","",2,1720,3440]
[null,"7614100000-E","DRILLED PIER FOUND","","",12,1100,13200]
[null,"7631000000-N","MAST ARM W/ MTL POLE DES","","",2,430,860]
[null,"7636000000-N","SIGN FOR SIGNALS","","",2,550,1100]
[null,"7642200000-N","TYPE II PED W/ FOUNDATION","","",4,1800,7200]
[null,"7684000000-N","SIGNAL CABINET FOUNDATION","","",4,2087.5,8350]
[null,"7744000000-N","DETECTOR CARD (TYPE 170)","","",5,135,675]
[null,"7756000000-N","CONTLR WITH CBNT, 2070L BASE MTD","","",1,15500,15500]
[null,"7901000000-N","CABINET BASE EXTENDER","","",1,630,630]
[null,"7948000000-N","TRAFFIC SIGNAL REMOVAL","","",1,2500,2500]
[null,"7960000000-N","METAL POLE FOUND REMVL","","",3,3500,10500]
[null,"7972000000-N","METAL POLE REMOVAL","","",3,1500,4500]
[null,"7980000000-N","GENERIC SIGNAL ITEM (EA)","5/8\" X 10' GROUNDING ELECTRODE","",33,255,8415]
[null,"","","CCTV FIELD EQUIPMENT CABINET","",3,6300,18900]
[null,"","","CCTV WOOD POLE","",3,3400,10200]
[null,"","","DIGITAL CCTV CAMERA  ASSEMBLY","",3,6600,19800]
[null,"","","DMS ACCESS LADDER","",1,7900,7900]
[null,"","","DMS PEDESTAL STRUCTURE","",1,43500,43500]
[null,"","","DYNAMIC MESSAGE SIGN (TYPE 2C)","",3,117000,351000]
[null,"","","ELECTRONIC MARKER BALL","",47,43,2021]
[null,"","","EQUIPMENT CABINET DISCONNECT","",4,859,3436]
[null,"","","ETHERNET EDGE SWITCH","",6,2300,13800]
[null,"","","LIMITED ACCESS FACILITIES - JBW/CONCRETE","COLLAR (OVERSIZED)",22,1860,40920]
[null,"","","","COLLAR (SPECIAL OVERSIZED)",7,2650,18550]
[null,"","","","COLLAR (STANDARD SIZE)",18,930,16740]
[null,"","","METER BASE/DISCONNECT","COMBINATION PANEL",2,1215,2430]
[null,"","","MODIFY EXISTING ELECTRICAL","SERVICE EQUIPMENT",2,455,910]
[null,"","","PCMS (IM)","",3,22100,66300]
[null,"","","PORTABLE CCTV CAMERA  ASSEMBLY","",3,28300,84900]
[null,"","","PROTECTIVE COATING FOR SINGLE","MAST ARM POLE (BROWN)",2,2900,5800]
[null,"","","","PEDESTAL (BROWN)",2,260,520]
[null,"","","SOLAR POWER ASSEMBLY","",2,13200,26400]
[null,"7990000000-E","GENERIC SIGNAL ITEM (LF)","#4 SOLID BARE GROUNDING","CONDUCTOR",750,9.1,6825]
[null,"","","3-WIRE COPPER FEEDER","CONDUCTORS",775,10.1,7827.5]
[null,"","","3-WIRE COPPER SERVICE ENTRANCE","CONDUCTORS",40,23.5,940]
[null,"","","4-WIRE COPPER FEEDER","CONDUCTORS",1390,11,15290]
[null,"","","BRIDGE MOUNTED CONDUIT","",1115,122,136030]
[null,"","","CONDUIT THROUGH ROCK","(1 CONDUIT, 2\")",384,46,17664]
[null,"","","","(2 CONDUITS, 2\")",6,56,336]
[null,"","","","(3 CONDUITS, 2\")",2341,61,142801]
[null,"8007000000-N","CM&R TEMP STR ***********","(53+43.00 -DET-)","",1,124000,124000]
[null,"8035000000-N","REMV EXIST STR **********","(15+45.00 -L-)","",1,48705,48705]
[null,"","","(30+68.60 -L-)","",1,686359,686359]
[null,"","","(35+30.22 -L-)","",1,948000,948000]
[null,"8056000000-N","REMV EXIST STR **********","(14+99.00 -Y4-)","",1,55000,55000]
[null,"","","(22+44.41 -L-)","",1,23300,23300]
[null,"8065000000-N","ASBESTOS ASSESSMENT","","",3,1790,5370]
[null,"8070000000-E","FOUNDATION EXCAVATION BRIDGE","","",629,32.5,20442.5]
[null,"8084000000-N","FND EXCAV EB** STA*******","(1, 35+30.22.-L-)","",1,16000,16000]
[null,"","","(2, 35+30.22-L-)","",1,16000,16000]
[null,"8091000000-N","FND EXCAV B** STA *******","(1, 30+12.56 -L-)","",1,162480,162480]
[null,"8096000000-E","PILE EXCAVATION IN SOIL","","",166,162.915662650602,27044]
[null,"8097000000-E","PILE EXCAVATION NOT IN SOIL","","",98,534.77551020408202,52408]
[null,"8112730000-N","PDA TESTING","","",2,10223,20446]
[null,"8121000000-N","UNCL STR EXCAV STA *****","(15+45.00 -L-)","",1,11500,11500]
[null,"","","(22+44.41 -L-)","",1,140000,140000]
[null,"","","(30+68.60 -L-)","",1,261923,261923]
[null,"8126000000-N","CULV EXCAV @ ************","(14+99.00 -Y4-)","",1,66450,66450]
[null,"8133000000-E","FND CONDIT MAT, BOX CULV","","",176,90,15840]
[null,"8147000000-E","REINF CONCRETE DECK SLAB","","",40009,73.7292859106701,2949835]
[null,"8156000000-E","CONCRETE WEARING SURFACE","","",2789,18.5,51596.5]
[null,"8161000000-E","GROOVING BRIDGE FLOORS","","",106464,0.92945314848212002,98953.3]
[null,"8182000000-E","CLASS A CONCRETE (BRIDGE)","","",463.6,2670.7161345987902,1238144]
[null,"8196000000-E","CLASS A CONCRETE (CULV)","","",502.6,1065.10147234381,535320]
[null,"8210000000-N","BRG APPR SLAB ***********","(15+45.00 -L-)","",1,48700,48700]
[null,"","","(30+68.60 -L-)","",1,267425,267425]
[null,"8217000000-E","REINF STEEL (BRIDGE)","","",86113,2.7968808426137701,240847.8]
[null,"8238000000-E","SPIRAL COL REINF STL BRG","","",3788,8,30304]
[null,"8245000000-E","REINF STEEL (CULVERT)","","",59196,2.30081762281235,136199.20000000001]
[null,"8248000000-E","EPOXY COAT REINF STEEL","","",396,2.8,1108.8]
[null,"8280000000-E","STRUCTURAL STEEL","","",1087000,6.93744250229991,7541000]
[null,"8328200000-E","PILE DRV EQUIP SETUP ** STEEL PILES","(HP 12 X 53)","",22,645.45454545454595,14200]
[null,"","","(HP 14 X 73)","",14,4846,67844]
[null,"","","(HP12 X 53)","",12,5000,60000]
[null,"8364000000-E","HP12X53 PILES","","",777,96.574002574002606,75038]
[null,"8384000000-E","HP14X73 PILES","","",400,362,144800]
[null,"8391000000-N","STEEL PILE POINTS","","",40,318.7,12748]
[null,"8503000000-E","CONCRETE BARRIER RAIL","","",472,197,92984]
[null,"8505000000-E","VERT CONC BARRIER RAIL","","",140.29,180,25252.2]
[null,"8510000000-E","CONCRETE MEDIAN BARRIER","","",266,253,67298]
[null,"8517000000-E","1'-**\"X*****\"CONC PARAPET","(1'-3\" X 2'-6\")","",36,225,8100]
[null,"8531000000-E","4\" SLOPE PROTECTION","","",24,100,2400]
[null,"8608000000-E","RIP RAP II (2'-0\")","","",1706,124.658851113716,212668]
[null,"8622000000-E","GEOTEXTILE FOR DRAINAGE","","",1619,4.0741198270537398,6596]
[null,"8657000000-N","ELASTOMERIC BEARINGS","","",2,85324,170648]
[null,"8706000000-N","EXPANSION JOINT SEALS","","",1,303667,303667]
[null,"8763000000-E","3'-0\" X 2'-0\"PRESTR SLABS","","",980,284,278320]
[null,"8801000000-E","MSE RETAIN WALL NO **","(1)","",3170,194,614980]
[null,"8804000000-N","GENERIC CULVERT ITEM (LS)","CHANNEL SUBSTRATE MATERIALS","",1,35000,35000]
[null,"","","PRECAST REINFORCED CONCRETE   THREE","SIDED CULVERT @ STA 22+44.41 L",1,200000,200000]
[null,"8811000000-E","GENERIC CULVERT ITEM (LF)","ANODIZED TWO BAR METAL RAIL","",28.5,165,4702.5]
[null,"","","GALVANIZED RAILS","",164.88,150,24732]
[null,"8821000000-E","GENERIC CULVERT ITEM (SF)","18\" STEEL SHEET PILES","",440,97,42680]
[null,"","","ARCHITECTURAL SURFACE TREAT-  MENT","",1274,46,58604]
[null,"8839000000-E","GENERIC RET WALL ITEM (LF)","ANODIZED TWO BAR METAL RAIL","",188,165,31020]
[null,"8847000000-E","GENERIC RET WALL ITEM (SF)","ARCHITECTURAL SURFACE TREAT-  MENT","",1990,46,91540]
[null,"","","CIP CANTILEVER RETAINING WALLS","",978,268,262104]
[null,"8860000000-N","GENERIC STRUCTURE ITEM (LS)","ACCESS & FALL PROTECTION","",1,800000,800000]
[null,"","","BEARING REPAIRS","",1,12000,12000]
[null,"","","CLEANING & PAINTING EXISTING","WEATHERING STEEL",1,828000,828000]
[null,"","","GUSSET PLATE RETROFIT","",1,55000,55000]
[null,"","","MOLDED RUBBER SEGMENTAL EXPAN-","SION JOINTS",1,600000,600000]
[null,"","","PAINTING CONTAINMENT","",1,72000,72000]
[null,"","","POLLUTION CONTROL","",1,212000,212000]
[null,"","","POST-TENSIONING ANCHORAGE","",1,750000,750000]
[null,"","","POST-TENSIONING BARS","",1,120000,120000]
[null,"","","WELD REPAIR W1","",1,130,130]
[null,"","","WELD REPAIR W2","",1,210,210]
[null,"","","WELD REPAIR W3","",1,130,130]
[null,"8867000000-E","GENERIC STRUCTURE ITEM (LF)","36\" FLORIDA I-BEAM CONCRETE   GIRDER","",745,651,484995]
[null,"","","54\" FLORIDA I-BEAM CONCRETE   GIRDER","",962,807,776334]
[null,"","","ASPHALT PLUG JOINT REPAIR/RE-","PLACEMENT (18\"-24\" WIDE, W/ PLATE)",1660,185,307100]
[null,"","","","PLACEMENT (18\"-24\" WIDE, WITH PLATE)",250,195,48750]
[null,"","","CONCRETE BARRIER RAIL","(ALL-LIGHTWEIGHT CONCRETE)",2208,149,328992]
[null,"","","CONCRETE MEDIAN BARRIER","(ALL-LIGHTWEIGHT CONCRETE)",1097,170,186490]
[null,"8881000000-E","GENERIC STRUCTURE ITEM (CY)","POLYESTER POLYMER CONCRETE    MATERIALS","",285,3040,866400]
[null,"8892000000-E","GENERIC STRUCTURE ITEM (SF)","FIBER REINFORCED CONCRETE     DECKSLAB","(ALL-LIGHTWEIGHT CONCRETE)",75343,48,3616464]
[null,"","","SILANE TREATMENTS","",3800,16.2,61560]
[null,"","","SURFACE PREPARATION FOR SILANE","",3800,6.75,25650]
[null,"8893000000-E","GENERIC STRUCTURE ITEM (SY)","PLACING & FINISHING POLYESTER","POLYMER CONCRETE OVERLAY",10250,13.5,138375]
[null,"","","SHOTBLASTING BRIDGE DECK","",10250,2.2999999999999998,23575]
[null,"8897000000-N","GENERIC STRUCTURE ITEM (EA)","9-5/8\" DIAMETER MICROPILES","",10,34805,348050]
[null,"","","BRIDGE WASHING","",30,3000,90000]
[null,"","","HOLE REPAIR TYPE I","",12,125,1500]
[null,"","","HOLE REPAIR TYPE II","",3,195,585]
[null,"","","HOLE REPAIR TYPE III","",1,250,250]
[null,"","","PACK RUST REPAIR TYPE I","",17,400,6800]
[null,"","","PACK RUST REPAIR TYPE II","",6,500,3000]
[null,"","","WELD REPAIR W4","",5,500,2500]

{"sheet":"Graph","index":17,"n_rows":48,"n_cols":12,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,null,null,"FEP8Qry3"]
[null,null,null,null,null,null,null,"Author","PHIGGINS",null,"Relevance of Data (Time)","23:17:51"]
[]
[]
[null,null,null,null,null,null,"Information"]
[null,null,null,null,null,null,"Author","PHIGGINS",null,"Last Refreshed","3/16/2022 09:31:37"]
[null,null,null,null,null,null,"Current User","HLUCAS",null,"Key Date","3/16/2022"]
[null,null,null,null,null,null,"Last Changed by","PHIGGINS",null,"Changed At","8/23/2013 09:52:47"]
[null,null,null,null,null,null,"InfoProvider","ZSPCI_C01",null,"Status of Data","3/1/2022 23:17:51"]
[null,null,null,null,null,null,"Query Technical Name","Y_SPX_LBPSR_BW110_VG",null,"Relevance of Data (Date)","3/1/2022"]
[null,null,null,null,null,null,"Query Description","Letting Based Project Summary Report (Bid Averages)",null,"Relevance of Data (Time)","23:17:51"]
[]
[]
[null,null,"Filter",null,null," "]
[null,null,"Area","",null," "]
[null,null,"Beginning Station","",null," "]
[null,null,"Catg #","",null," "]
[null,null,"Contract ID","",null," "]
[null,null,"Cul, O/U, etc. Code","",null," "]
[null,null,"E/M","",null," "]
[null,null,"Fed Work Code","",null," "]
[null,null,"Key Figures","",null," "]
[null,null,"Let Call Order","",null," "]
[null,null,"Letting Date","",null," "]
[null,null,"Primary Div","",null," "]
[null,null,"Project #","",null," "]
[null,null,"Project County","",null," "]
[null,null,"Rdw/Str ID","",null," "]
[null,null,"Substr Code","",null," "]
[null,null,"Supstr Code","",null," "]
[null,null,"TIP","",null," "]
[null,null,"Vendor","",null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]
[null,null,null,null,null," "]