**PEDESTRIAN CHANNELIZATION DEVICES:**

(10/31/2017)

**Description**

Furnish and install Pedestrian Channelization Devices providing a safe and convenient temporary path for existing pedestrian facilities that are disrupted, closed, or relocated by planned work activities.

**Construction Methods**

The Pedestrian Channelization Devices shall be installed in accordance with local governing building codes, and requirements of the Americans with Disabilities Act (ADA). At no time shall materials or equipment be stored within designated walkways during work zone operations.

**Measurement and Payment**

The measurement and payment for the Pedestrian Channelization Devices shall be paid by the linear foot that’s satisfactorily placed and accepted by the Engineer. The linear foot price shall include any costs associated with the installation, maintenance and removal of the devices.

Payment will be made under:

**Pay Item Pay Unit**

Pedestrian Channelization Devices…………………………………………Linear Foot