**WARNING FLAGS:**

(Rev. 10/13/2023)

**General**

Use flags which are orange or fluorescent versions of orange. Each flag must be 16 inches square or larger, and attached to a staff.

**Flag Material**

Use fabric type flags made of an orange or fluorescent orange flexile type of material such as vinyl or nylon.

**Material Certification**

Furnish a Type 3 Certification in accordance with Section 106-3 of the *Standard Specifications* for all warning flags prior to use.

**Approval**

All materials are subject to the approval of the Engineer.

**Payment**

Payment will be made under:

**Pay Item Pay Unit**

Warning Flags Each