**CONSTRUCTION SEQUENCE:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 8-21-12) | 560 | SP1 R34R |

Pave each section of roadway begun in a continuous operation. Do not begin work on another section of roadway unless satisfactory progress is being made toward completion of intersections and all other required incidental work by satisfactorily furnishing additional paving equipment and personnel, except for milling and patching operations.