**BORROW EXCAVATION (In Place or Truck Measurement):**

|  |  |  |
| --- | --- | --- |
| (7-1-95) | 230 | SP2 R58 |

The borrow material used on this project will be measured for payment by in place measurement as provided in Article 230-5 of the *2018* *Standard Specifications*, or by truck measurement as provided in Article 230-5 of the *2018* *Standard Specifications,* as directed by the Engineer.