**THERMOPLASTIC INTERMIXED BEAD TESTING:**

|  |  |  |
| --- | --- | --- |
| 7-19-22 | 1087 | SP10 R04 |

Revise the *2018* *Standard Specifications* as follows:

**Page 10-183, Subarticle 1087-7(B) Thermoplastic Pavement Marking Material Composition,** delete line 34 and 35.

**Page 10-184, Article 1087-8 MATERIAL CERTIFICATION,** delete andreplace with the following after line 34:

|  |  |
| --- | --- |
| Drop-on Glass Beads | Type 3 Material Certification and Type 4 Material Certification |
| Intermix Glass Beads |  Type 2 Material Certification and Type 3 Material Certification |
| Paint |  Type 3 Material Certification |
| Removable Tape |  Type 3 Material Certification |
| Thermoplastic |  Type 3 Material Certification and Type 4 Material Certification |
| Cold Applied Plastic |  Type 2 Material Certification and Type 3 Material Certification |
| Polyurea |  Type 2 Material Certification and Type 3 Material Certification |