**MATERIAL AND EQUIPMENT STORAGE & PARKING OF PERSONAL VEHICLES:**

|  |  |  |
| --- | --- | --- |
| 11-17-21(Rev. 8-16-22) | 1101 | SP11 R03 |

Revise the *2018 Standard Specifications* as follows:

**Page 11-2, Article 1101-8 MATERIAL AND EQUIPMENT STORAGE, line 35-38,** delete and replace with the following:

When work is not in progress, keep all personnel, equipment, machinery, tools, construction debris, materials and supplies away from active travel lanes that meets Table 1101-1.

|  |  |
| --- | --- |
| **TABLE 1101-1**  **MATERIAL AND EQUIPMENT STORAGE FROM ACTIVE TRAVEL LANES** | |
| Posted Speed Limit (mph) | Distance (ft) |
| 40 or less | ≥ 18 |
| 45-50 | ≥ 28 |
| 55 | ≥ 32 |
| 60 or higher | ≥ 40 |

When vehicles, equipment and materials are protected by concrete barrier or guardrail, they shall be offset at least 5 feet from the barrier or guardrail.

**Page 11-2, Article 1101-9 PARKING OF PERSONAL VEHICLES, line 40-41,** delete and replace with the following:

Provide staging areas for personal vehicle parking in accordance with Article 1101-8 or as directed by the Engineer before use.