DITCH MAINTENANCE:
	  (1-18-05)(Rev. 10-20-26)
	SPI 2-02



Description

Clean and grade to drain earth ditches in accordance with the plan, this special provision, and as directed by the Engineer at locations shown on the plans or as directed by the Engineer.

Materials

Furnish all earth material necessary for grading ditches to drain in accordance with Section 1019 of the Standard Specifications.  All soil is subject to test and acceptance or rejection by the Engineer.

Construction Methods

Perform ditching operation in accordance with the plans, applicable requirements of Section 200 and 1660 of the Standard Specifications, this special provision and as directed by the Engineer where existing ditches are excessively overgrown, holding water, or obstructed.  Restore proper drainage by cleaning and grading the ditch to a condition acceptable to the Engineer.  Seeding and mulching shall be incidental to ditch maintenance and in accordance with the Standard Specifications, plans, and the contract unless otherwise specified in the contract.

Traffic control and mobilization for ditch maintenance shall be in accordance with the Standard Specifications, Roadway Standard Drawings, and the contract. 

Protect adjacent traffic, pedestrians, property, and drainage features from cleaning operations.

Material removed from drainage ditches shall be disposed of in waste areas furnished by the Contractor or as directed by the Engineer in accordance with Article 240-3 of the Standard Specifications.

Measurement and Payment

Ditch Maintenance will be measured and paid in linear feet of ditch which has been cleaned, graded and accepted. Measurement will be made along the ditch flow line of each ditch to the nearest foot.  Such price and payment will be full compensation for cleaning, removal and disposal of debris, restoring proper drainage, and any incidentals necessary to satisfactorily complete this work.  Seeding and mulching of the ditch line will be incidental to Ditch Maintenance unless otherwise specified in the contract.

Ditch Maintenance does not include the cost for mobilization and traffic control as these items will be paid for elsewhere in the contract,

Payment will be made under:

	Pay Item
	Pay Unit

	Ditch Maintenance
	Linear Foot



