STEEL PIPE HANDRAIL FOR CONCRETE STEPS:
	(7-25-07)
	SPI 8-05



Description

Furnish and install steel pipe handrail for the concrete steps and wood deck at the location shown in the plans, in accordance with the detail in the plans and as directed by the Engineer. 

Measurement and Payment

Steel Pipe Handrail for Concrete Steps and Deck will measured and paid for as the actual number of linear feet of steel pipe handrail measured along the top of the handrail to the nearest 0.1 of a foot.  Such price and payment shall be full compensation for fabricating, furnishing, installing, painting and all incidentals necessary to satisfactorily install the handrail.

Payment will be made under:

	Pay Item
	Pay Unit

	Steel Pipe Handrail for Concrete Steps and Deck
	Linear Foot



