___" STAMPED CONCRETE SIDEWALK:
	(10-20-15)
	SPI 8-14



Construct the stamped, textured decorative print sidewalk in accordance with Section 848 of the Standard Specification, with the details shown on the plans and as directed by the Engineer.  The Engineer will determine the details related to pattern, depth and dimensions of stamping, color, and sealing.

___" Stamped Concrete Sidewalk will be measured and paid for in square yards measured along the surface of the completed and accepted work. Such price includes, but is not limited to excavating and backfilling, sawing the existing sidewalk, furnishing and placing concrete, constructing and sealing joints, stamping, coloring, and sealing the concrete.

Payment will be made under:

	Pay Item
	Pay Unit

	___" Stamped Concrete Sidewalk
	Square Yards



