TEMPORARY WOVEN WIRE FENCE:
	(12-22-15)
	SPI 8-79



Description

Construct temporary woven wire fence, posts, gates, and barbed wire at locations shown on the plans.

Materials

Use only fabric and posts that have been approved by the Engineer.  Materials shall meet the requirements of Article 866-2 of the Standard Specifications.

Construction Methods

Construct the fence in accordance with Subarticle 866-3(C) of the Standard Specifications and Roadway Standard Drawing No. 866.02.  The fence shall be maintained with fabric taut and securely fastened to the posts at all times.  Barbed wire shall be installed along the top of the posts and at any ditch locations as determined by the Engineer.

After the fence has served its purpose and is no longer needed, as determined by the Engineer, it shall become the property of the Contractor and shall be removed and disposed of by him.

Measurement and Payment

Temporary ________" Woven Wire Fence, Complete with Posts will be measured and paid for as the actual number of linear feet of fence constructed and accepted, measured in place from center of end post to center of end post.  Such price and payment will be full compensation for all materials, labor, fence maintenance, and incidentals, including all barbed wire necessary to satisfactorily complete the work.

Temporary Double Gates, ___" High, ___' Wide, ___' Opening will be measured and paid in units of each as the actual number of gates constructed and accepted in place.  Such price and payment will be full compensation for all materials, labor, fence maintenance, and incidentals necessary to satisfactorily complete the work.

Temporary Single Gates, ___" High, ___' Wide, ___' Opening will be measured and paid in units of each as the actual number of gates constructed and accepted in place.  Such price and payment will be full compensation for all materials, labor, fence maintenance, and incidentals necessary to satisfactorily complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Temporary ________" Woven Wire Fence, Complete with Posts 
	Linear Foot

	Temporary Double Gates, ___" High, ___' Wide, ___' Opening
	Each

	Temporary Single Gates, ___" High, ___' Wide, ___' Opening
	Each



