AGGREGATE BASE COURSE (SUB-BALLAST):
	4-3-08
	SPI 10-03



Description

Place Railroad Sub-Ballast at locations shown in the plans and the Railroad provisions.  Railroad Sub-Ballast shall be placed in accordance with details in the plans and Railroad special provisions/details included elsewhere in the Contract. 

Materials

Provide material in accordance with the Railroad special provisions for Category “B” dense graded aggregate. 

Measurement and Payment

Aggregate Base Course (Sub-Ballast) will be measured and paid for at the contract unit price per ton for the actual number of tons of aggregate which has been incorporated into the completed and accepted work.

The Sub-Ballast will be measured by being weighed in trucks on certified platform scales or other certified weighing devices

Payment will be made under:

	Pay Item
	Pay Unit

	Aggregate Base Course (Sub-Ballast)
	Ton



