DUCTILE IRON PIPE:
	   (12-17-09)
	SPI 10-05



Description

Furnish and install ductile iron pipe at locations indicated on the plans and as directed by the Engineer.  The work includes the construction of joints and connections to other pipes, endwalls, and other drainage structures.

Materials

Refer to Division 10 of the Standard Specifications:

	Item
	Section

	Ductile Iron Pipe 
	1034



Use pipe meeting the requirements for Gravity Flow Sewer Pipe.

Construction Methods

Install pipe in accordance with Section 300 of the Standard Specifications and as directed by the Engineer.

Measurement and Payment

Ductile Iron Pipe will be measured and paid for as the actual number of linear feet of pipe that has been incorporated into the completed and accepted work.

Payment will be made under:

	Pay Item
	Pay Unit

	___ " Ductile Iron Pipe
	Linear Foot



