**BUILDING REMOVAL:**

|  |  |  |
| --- | --- | --- |
| (1-1-02) (Rev. 1-16-24) | 215 | SP2 R15 B |

Remove the buildings, underground storage tanks and appurtenances listed below in accordance with Section 215 of the *Standard Specifications*:

(INSERT BUILDING INFORMATION HERE)

When the description of the work for an item requires a portion of the building to be cut off, that portion of the buildings and appurtenances located within the right of way and/or construction area shall be cut off by the Contractor and disposed of by him. The Engineer will denote on the building, the line where the building is to be cut off. The Contractor will be required to cut the building off on a neat line along the construction line or right of way boundary designated by the Engineer. The Contractor will not be required to do any repairing to that portion of the building located outside the right of way or construction area or to shore it up in any respect. All of the Contractor’s work shall be confined to the right of way and construction area designated by the Engineer.