**GEOTEXTILE FOR SUBGRADE STABILIZATION:**

|  |  |  |
| --- | --- | --- |
|  (5-15-18)(Rev. 4-16-24) | 505, 1056 | SP5 R9 |

**Description**

Provide geotextile for subgrade stabilization in accordance with the contract. Geotextile for subgrade stabilization is required for subgrades to prevent pavement cracking at locations shown in the plans and as directed by the Engineer.

**Materials**

Refer to Article 505-2 of the *Standard Specifications*.

|  |  |
| --- | --- |
|  |  |

**Construction Methods**

Refer to Article 505-3 of the *Standard Specifications*.

**Measurement and Payment**

*Geotextile for Subgrade Stabilization* will be measured and paid in accordance with Article 505-4 of the *Standard Specifications*.