**ASPHALT CONCRETE SURFACE COURSE, TYPE S9.5\_\_ (Leveling Course):**

|  |  |  |
| --- | --- | --- |
| (7-1-95)(Rev. 1-16-24) | 610 | SP6 R85R |

Place a leveling course of *Asphalt Concrete Surface Course, Type S9.5\_\_* at locations shown on the sketch maps and as directed by the Engineer. The rate of this leveling course is not established but will be determined by allowing the screed to drag the high points of the section. It is anticipated that some map numbers will be leveled from beginning to end while others may only require a leveling course for short sections.

The *Asphalt Concrete Surface Course, Type S9.5\_\_ (Leveling Course)* shall meet the requirements of Section 610 of the *Standard Specifications* except payment will be made at the contract unit price per ton for *Asphalt Concrete Surface Course, Type S9.5\_\_* *(Leveling Course).*

**Measurement and Payment**

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Asphalt Concrete Surface Course, Type S9.5\_\_ (Leveling Course) | Ton |