**ADJUSTMENT OF MANHOLES, METER BOXES, AND VALVE BOXES:**

|  |  |  |
| --- | --- | --- |
| (7-1-95)(Rev. 1-16-24) | 858 | SP8 R97R |

The Contractor's attention is directed to Article 858-3 of the *Standard Specifications*. Cast iron or steel fittings will not be permitted for the adjustment of manholes, meter boxes, and valve boxes on this project.