**VINYL COATED CHAIN LINK FENCE:**

|  |  |  |
| --- | --- | --- |
| (1-1-02)(Rev. 6-17-24) | 866 | SP8 R101 |

**Page 8-48, Article 866-4, MEASUREMENT AND PAYMENT,** add the following paragraphs after line 35:

*\_\_\_\_ Vinyl Coated Chain Link Fence, \_\_\_" Fabric* will be measured and paid in linear feet of fence measured in place from center of each post or gate post to center of end post or gate post exclusive of gate sections, that has been completed and accepted.

*\_\_\_\_ Vinyl Coated* *Metal Line Posts for* *\_\_\_" Chain Link Fence* will be measured and paid in units of each for the several sizes and kinds of posts actually installed on the project. For extra length metal posts, the actual length of post in place in excess of the standard pay length for each post shall be measured in linear feet, and half of such length shall be converted to an equivalent number of standard length posts of the same size for which a pay item has been established. In converting to equivalent numbers of standard length posts, any fractional portion of a post remaining from the division of a total number of linear feet by a standard post length shall be considered as equal to one post.

*\_\_\_\_ Vinyl Coated* *Metal Terminal Posts for* *\_\_\_" Chain Link Fence* will be measured and paid in units of each for all end, corner and brace posts installed on the project.

*\_\_\_\_ Vinyl Coated* *Metal Gate Posts for \_\_\_" Chain Link Fence, Double Gate* will be measured and paid in units of each for gateposts installed on the project.

*\_\_\_\_ Vinyl Coated* *Metal Gate Posts for \_\_\_" Chain Link Fence, Single Gate* will be measured and paid in units of each for gate posts installed on the project.

*\_\_\_\_ Vinyl Coated Double Gates, \_\_\_" High, \_\_\_' Wide, \_\_\_' Opening* will be measured and paid in units of each for the number of gates actually erected on the project. Double gates will be measured as one gate.

*\_\_\_\_ Vinyl Coated Single Gates, \_\_\_" High, \_\_\_' Wide, \_\_\_' Opening* will be measured and paid in units of each for the number of gates actually erected on the project.

**Page 8-49, Article 866-4, MEASUREMENT AND PAYMENT,** add the following after line 1:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| *\_\_\_\_* Vinyl Coated Chain Link Fence, \_\_" Fabric | Linear Foot |
| *\_\_\_\_* Vinyl Coated Metal Line Posts for \_\_" Chain Link Fence | Each |
| *\_\_\_\_* Vinyl Coated Metal Terminal Posts for \_\_" Chain Link Fence | Each |
| \_\_\_\_ Vinyl Coated Metal Gate Posts for \_\_" Chain Link Fence, Double Gate | Each |
| \_\_\_\_ Vinyl Coated Metal Gate Posts for \_\_" Chain Link Fence, Single Gate | Each |
| \_\_\_\_ Vinyl Coated Double Gates, \_\_\_" High, \_\_\_' Wide, \_\_\_' Opening | Each |
| \_\_\_\_ Vinyl Coated Single Gates, \_\_\_" High, \_\_\_' Wide, \_\_\_' Opening | Each |