**STEEL FENCE POSTS FOR WOVEN WIRE FENCE:**

|  |  |  |
| --- | --- | --- |
| (11-19-24) | 866 | SP8 R84 |

**Description**

Use steel fence posts to install woven wire fence in accordance with Section 866 of the *Standard Specifications*, Roadway Standard Drawings No. 866.03, the details in the plans and this special provision.

**Materials**

Refer to Division 10 of the *Standard Specifications*.

|  |  |
| --- | --- |
| **Item** | **Section** |
| Metal Posts and Rails | 1050-3(B) |

**Construction Methods**

Woven wire fence shall be constructed using 7.5' or 8' steel fence posts in accordance with the plans, Article 866-3 of the *Standard Specifications* and as directed by the Engineer.

**Measurement and Payment**

*Steel Fence Posts, 7.5' Long* and *Steel Fence Posts, 8' Long* will be measured and paid in units of each for the size and type of post installed on the project, including steel line posts and brace posts.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Steel Fence Posts, 7.5' Long | Each |
| Steel Fence Posts, 8' Long | Each |