**CLEARING AND GRUBBING:**

|  |  |  |
| --- | --- | --- |
| (01-30-14) | 200 | SPD 2-100 |

**Description**

Clear and grub specified areas in order for utility relocations to be performed. Perform clearing and grubbing in accordance with Section 200 of the *2018 Standard Specifications.*

**Notes to Contractor**

The plans provided for this project are for TIP Project TIP #, they are to be used as reference only.

The clearing and grubbing limits will be from the edge of existing pavement (EOP) to the right of way (R/W), easement (E), or permanent utility easement (PUE), as directed by the Engineer. These limits will extend the entire left side (Left of –L-) of the project from STA \_\_\_\_\_–L- to STA \_\_\_\_\_\_–L- and a portion of the right side (Right of –L-) from approximately STA \_\_\_\_\_\_\_\_\_\_to STA \_\_\_\_\_\_\_\_\_\_–L- (End of Project). These limits shall exclude wetland areas at the following locations:

Approx. STA \_\_\_\_\_––L- LT to STA \_\_\_\_\_––L- LT

Approx. STA \_\_\_\_\_––L- RT to STA \_\_\_\_\_––L- RT

The Contractor shall delineate the wetland areas by installing and maintaining an orange safety fence a minimum of 50 ft outside the wetland boundaries. The Contractor shall not perform any land disturbing activities within these boundaries.

The Contractor will be required to complete the clearing and grubbing portion of the project by the completion date as set forth in the Intermediate Completion Time.

**Measurement and Payment**

*Clearing and Grubbing* will be paid on a lump sum basis and no measurement will be made of any clearing and grubbing performed within the limits originally staked and within the right of way or easements.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Clearing and Grubbing | Lump Sum |