## LOCATING EXISTING UNDERGROUND UTILITIES:

|  |  |  |
| --- | --- | --- |
| (3-20-12) | 105 | SP1 G115 |

Revise the *2012* *Standard Specifications* as follows:

**Page 1-43, Article 105-8, line 28, after the first sentence,** add the following:

Identify excavation locations by means of pre-marking with white paint, flags, or stakes or provide a specific written description of the location in the locate request.