**INCIDENTAL STONE BASE:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev.8-21-12) | 545 | SP5 R28R |

**Description**

Place incidental stone base on driveways, mailboxes, etc. immediately after paving and do not have the paving operations exceed stone base placement by more than one week without written permission of the Engineer.

**Materials and Construction**

Provide and place incidental stone base in accordance with Section 545 of the *2012* *Standard Specifications*.

**Measurement and Payment**

*Incidental Stone Base* will be measured and paid in accordance with Article 545-6 of the *2012* *Standard Specifications*.