**PAVING DRIVEWAYS AND MAILBOX TURNOUTS:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 8-21-12) | 610 | SP6 R70AR |

Surface all driveway and mailbox turnouts as directed by the Engineer. The unpaved driveways and mailbox turnouts will be prepared for surfacing by State Forces. Place pavement on driveway and mailbox turnouts of the same material as used on the main line and in depths directed by the Engineer. Widen the pavement on curves as directed by the Engineer.