**GROUT REFERENCES FOR POSITIVE PROTECTION:**

|  |  |  |
| --- | --- | --- |
| (5-19-15) | 1170 | SP11 R20 |

Revise the *2012* *Standard Specifications* as follows:

**Page 11-14, Article 1170-2, Materials,** line 30,in the materials table, replace “Freeze-Thaw Durable Grout, Nonshrink” with “Grout, Type 3”.

**Page 11-14, Article 1170-2, Materials,** lines 31-32, delete the first paragraph after the materials table.