**LONGITUDINAL CHANNELIZING CURB SYSTEM:**

|  |  |  |
| --- | --- | --- |
| 5-13-22 |  |  |

Typically for temporary use during construction.

This provision specifies requirements for a longitudinal channelizing curb system. The

longitudinal channelizing curb system shall consist of three main components: a series of raised

separator units and vertical markers with reflective sheeting.

**See Signing and Delineation Unit for the full provision language and process.**

[**https://apps.ncdot.gov/dot/directory/authenticated/UnitPage.aspx?id=11149**](https://apps.ncdot.gov/dot/directory/authenticated/UnitPage.aspx?id=11149)

**Matt Springer**

**Signing and Delineation Standards Engineer**

**mspringer@ncdot.gov**

**919-814-5025**